(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 87.042 115.5332)
    (grid_origin 87.042 0)
    (pcbplotparams
      (layerselection 0x0001000_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerbers/")
    )
  )
  (net 0 "")
  (net 1 "3_3V_Pico")
  (net 2 "GND")
  (net 3 "Net-(IC1-B0)")
  (net 4 "Net-(IC1-B2)")
  (net 5 "Net-(IC1-B4)")
  (net 6 "Net-(IC1-B6)")
  (net 7 "Net-(IC1-A6)")
  (net 8 "Net-(IC1-A4)")
  (net 9 "Net-(IC1-A2)")
  (net 10 "Net-(IC1-A0)")
  (net 11 "Net-(J2-In)")
  (net 12 "Net-(J3-In)")
  (net 13 "PC3")
  (net 14 "PC1")
  (net 15 "PC2")
  (net 16 "PC0")
  (net 17 "unconnected-(U4-NC-Pad1)")
  (net 18 "Net-(R2-Pad2)")
  (net 19 "Net-(R8-Pad2)")
  (net 20 "unconnected-(U2-NC-Pad1)")
  (net 21 "Net-(U3-GPIO20)")
  (net 22 "unconnected-(U3-SWDIO-Pad43)")
  (net 23 "unconnected-(U3-SWCLK-Pad41)")
  (net 24 "unconnected-(U3-VBUS-Pad40)")
  (net 25 "unconnected-(U3-VSYS-Pad39)")
  (net 26 "unconnected-(U3-3V3_EN-Pad37)")
  (net 27 "unconnected-(U3-ADC_VREF-Pad35)")
  (net 28 "unconnected-(U3-GPIO28_ADC2-Pad34)")
  (net 29 "unconnected-(U3-GPIO27_ADC1-Pad32)")
  (net 30 "unconnected-(U3-GPIO26_ADC0-Pad31)")
  (net 31 "unconnected-(U3-GPIO19-Pad25)")
  (net 32 "unconnected-(U3-GPIO18-Pad24)")
  (net 33 "unconnected-(U3-GPIO17-Pad22)")
  (net 34 "unconnected-(U3-GPIO16-Pad21)")
  (net 35 "unconnected-(U3-GPIO14-Pad19)")
  (net 36 "unconnected-(U3-GPIO12-Pad16)")
  (net 37 "unconnected-(U3-GPIO10-Pad14)")
  (net 38 "unconnected-(U3-GPIO8-Pad11)")
  (net 39 "unconnected-(U3-GPIO7-Pad10)")
  (net 40 "unconnected-(U3-GPIO6-Pad9)")
  (net 41 "unconnected-(U3-GPIO5-Pad7)")
  (net 42 "unconnected-(U3-GPIO4-Pad6)")
  (net 43 "unconnected-(U3-GPIO3-Pad5)")
  (net 44 "unconnected-(U3-GPIO2-Pad4)")
  (net 45 "unconnected-(U3-GPIO1-Pad2)")
  (net 46 "Net-(U3-GPIO0)")
  (net 47 "unconnected-(U3-GPIO22-Pad29)")
  (net 48 "unconnected-(JP1-B-Pad3)")
  (net 49 "Net-(JP1-C)")
  (net 50 "unconnected-(U3-GPIO21-Pad27)")
  (net 51 "Power Supply")
  (net 52 "EXT. PWR")
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 176.9752 107.6444)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J7" (at 0.0388 -1.8472 180) (layer "F.SilkS"))
    (fp_text value "Pseudoclock 0" (at 9.1568 2.4956) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "PC0") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 96.563 92.869 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.82 -90) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.82 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 12 "Net-(J3-In)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 107.945 106.438)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Power_Connections.kicad_sch")
    (property "Sheetname" "Power connections (jumpers)")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "0" (at -4.235 0.1088) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 148.6017 82.5434)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 3.5423 0.0938) (layer "F.SilkS"))
    (fp_text value "100n" (at 6.6343 -0.1134) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 51 "Power Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 148.6017 88.5834)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 3.5423 0.0478) (layer "F.SilkS"))
    (fp_text value "10uF" (at 6.4863 -0.1394) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 51 "Power Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (layer "F.Cu")
    (at 106.4768 98.0488)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Schmitt Buffer Gate, Low-Voltage CMOS")
    (property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS")
    (attr smd)
    (fp_text reference "U4" (at -1.75 -2.63) (layer "F.SilkS"))
    (fp_text value "74LVC1G17" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "unconnected-(U4-NC-Pad1)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "2" smd rect (at -1.35 0) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(R8-Pad2)") (pintype "input"))
    (pad "3" smd rect (at -1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at 1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(U3-GPIO0)") (pintype "output"))
    (pad "5" smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "3_3V_Pico") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 165.842 66.2962 -135)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -0.035 1.895 45) (layer "F.SilkS"))
    (fp_text value "49.9" (at -0.115 -1.785 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 225) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 13 "PC3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 225) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 7 "Net-(IC1-A6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 90.02 98.0468 180)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J3" (at 0.014 -2.1884 180) (layer "F.SilkS"))
    (fp_text value "Ext. Trig." (at 9.018 -2.1432) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "Net-(J3-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 92.742 87.9412)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "mounting_holes.kicad_sch")
    (property "Sheetname" "Mounting Holes")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.85) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0.91 -3.0712) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 98.15055 98.0468)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "500" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 12 "Net-(J3-In)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 19 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 150.5312 62.6354 45)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Power_Connections.kicad_sch")
    (property "Sheetname" "Power connections (jumpers)")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0 -2.28 45) (layer "F.SilkS"))
    (fp_text value "0" (at 2.386627 2.585465 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0 45) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0 45) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 139.696 64.762 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.82 -90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.82 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "Net-(IC1-B6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 148.6017 85.5634)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 3.5423 0.0008) (layer "F.SilkS"))
    (fp_text value "1uF" (at 6.0033 -0.1264) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 51 "Power Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 139.662 77.426 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "Net-(IC1-B2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 176.9752 77.8044)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J6" (at -3.96 -3 90) (layer "F.SilkS"))
    (fp_text value "Pseudoclock 2" (at 8.9168 2.2356) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "PC2") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 166.492 73.0362 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 15 "PC2") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "Net-(IC1-A4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 176.9752 62.8844)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J4" (at 0.0308 -1.8282 180) (layer "F.SilkS"))
    (fp_text value "Pseudoclock 3" (at 9.2068 2.3556) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "PC3") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 109.4022 94.7994)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "3_3V_Pico") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 106.9702 65.3854 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -2.3018 4.7154) (layer "F.SilkS"))
    (fp_text value "PWR SEL" (at 0 7.41) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "3_3V_Pico") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 51 "Power Supply") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 52 "EXT. PWR") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 157.742 111.9522)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "mounting_holes.kicad_sch")
    (property "Sheetname" "Mounting Holes")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at -0.104 -2.415) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0.071 2.5108) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 89.9993 70.1228 180)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J2" (at -0.0547 -2.1624 180) (layer "F.SilkS"))
    (fp_text value "Ext. Clock" (at 8.9973 -2.2772) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(J2-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 139.798 85.12 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "Net-(IC1-B0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 157.742 92.9022)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "mounting_holes.kicad_sch")
    (property "Sheetname" "Mounting Holes")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0.042 -2.669) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at -0.994 2.8288) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 143.036 68.893 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "Net-(IC1-B4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (layer "F.Cu")
    (at 105.6562 72.2104)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Buffef Gate, Low-Voltage CMOS")
    (property "ki_keywords" "Single Gate Buff LVC CMOS")
    (attr smd)
    (fp_text reference "U2" (at -1.1176 -2.6924) (layer "F.SilkS"))
    (fp_text value "74LVC1G34" (at 0.0758 2.2696) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "unconnected-(U2-NC-Pad1)") (pinfunction "NC") (pintype "free"))
    (pad "2" smd rect (at -1.35 0) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(R2-Pad2)") (pintype "input"))
    (pad "3" smd rect (at -1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at 1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(U3-GPIO20)") (pintype "output"))
    (pad "5" smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "3_3V_Pico") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 162.672 83.0162 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at -0.87 -1.86 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 16 "PC0") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "Net-(IC1-A0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MCU_RaspberryPi_and_Boards:RPi_Pico_SMD" (layer "F.Cu")
    (at 125.6246 87.3808 180)
    (descr "Surface Mount header, 2x20, 2.54mm pitch, double rows")
    (tags "Surface Mount header THT 2x20 2.54mm double row")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 0) (layer "F.SilkS"))
    (fp_text value "Pico" (at 0 2.159) (layer "F.Fab"))
    (fp_text user "VBUS" (at 5.998878 -23.4492 45) (layer "F.SilkS"))
    (fp_text user "ADC_VREF" (at 4.4856 -11.4532 180) (layer "F.SilkS"))
    (fp_text user "GND" (at 6.1316 6.5478 45) (layer "F.SilkS"))
    (fp_text user "GP20" (at 5.9076 11.9048 45) (layer "F.SilkS"))
    (fp_text user "GP14" (at -6.0704 20.652 45) (layer "F.SilkS"))
    (fp_text user "GP16" (at 5.7676 24.2658 180) (layer "F.SilkS"))
    (fp_text user "GP26" (at 6.1506 -1.0462 45) (layer "F.SilkS"))
    (fp_text user "AGND" (at 5.8676 -6.3094 180) (layer "F.SilkS"))
    (fp_text user "GP11" (at -6.0704 10.492 45) (layer "F.SilkS"))
    (fp_text user "VSYS" (at 6.066222 -20.7642 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 6.227846 19.5108 45) (layer "F.SilkS"))
    (fp_text user "GP12" (at -6.0704 13.032 45) (layer "F.SilkS"))
    (fp_text user "GP28" (at 6.0986 -8.4612 45) (layer "F.SilkS"))
    (fp_text user "3V3" (at 6.3546 -13.5732 45) (layer "F.SilkS"))
    (fp_text user "GP3" (at -6.339774 -14.908 45) (layer "F.SilkS"))
    (fp_text user "GP13" (at -6.0704 15.572 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 6.227846 -18.0792 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.312837 -7.288 45) (layer "F.SilkS"))
    (fp_text user "GP22" (at 6.0076 4.1828 45) (layer "F.SilkS"))
    (fp_text user "RUN" (at 6.2026 1.4638 45) (layer "F.SilkS"))
    (fp_text user "3V3_EN" (at 5.540942 -15.3942 45) (layer "F.SilkS"))
    (fp_text user "GP17" (at 6.3486 22.1978 45) (layer "F.SilkS"))
    (fp_text user "GP1" (at -6.339774 -22.538 45) (layer "F.SilkS"))
    (fp_text user "GP6" (at -6.339774 -4.748 45) (layer "F.SilkS"))
    (fp_text user "GP21" (at 6.0496 9.2318 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.339725 18.4968 225) (layer "F.SilkS"))
    (fp_text user "GP19" (at 5.9996 14.5308 45) (layer "F.SilkS"))
    (fp_text user "GP0" (at -13.0554 -24.0792 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.312837 5.412 45) (layer "F.SilkS"))
    (fp_text user "GP9" (at -6.339774 2.872 45) (layer "F.SilkS"))
    (fp_text user "SWCLK" (at -5.7 26.2) (layer "F.SilkS"))
    (fp_text user "GP4" (at -6.339774 -12.368 45) (layer "F.SilkS"))
    (fp_text user "GP7" (at -6.339774 -2.238 45) (layer "F.SilkS"))
    (fp_text user "GP8" (at -6.339774 0.332 45) (layer "F.SilkS"))
    (fp_text user "GP27" (at 6.0456 -3.6072 45) (layer "F.SilkS"))
    (fp_text user "SWDIO" (at 5.6 26.2) (layer "F.SilkS"))
    (fp_text user "GP2" (at -6.339774 -17.448 45) (layer "F.SilkS"))
    (fp_text user "GP10" (at -6.0704 7.952 45) (layer "F.SilkS"))
    (fp_text user "GP5" (at -6.339774 -9.828 45) (layer "F.SilkS"))
    (fp_text user "GP18" (at 6.0236 17.1788 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.312837 -19.988 45) (layer "F.SilkS"))
    (fp_text user "GP15" (at -6.0704 23.4378 45) (layer "F.SilkS"))
    (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 -30.2) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -8.89 -24.13 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 46 "Net-(U3-GPIO0)") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "2" smd rect (at -8.89 -21.59 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 45 "unconnected-(U3-GPIO1-Pad2)") (pinfunction "GPIO1") (pintype "bidirectional+no_connect"))
    (pad "3" smd rect (at -8.89 -19.05 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -8.89 -16.51 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 44 "unconnected-(U3-GPIO2-Pad4)") (pinfunction "GPIO2") (pintype "bidirectional+no_connect"))
    (pad "5" smd rect (at -8.89 -13.97 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 43 "unconnected-(U3-GPIO3-Pad5)") (pinfunction "GPIO3") (pintype "bidirectional+no_connect"))
    (pad "6" smd rect (at -8.89 -11.43 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 42 "unconnected-(U3-GPIO4-Pad6)") (pinfunction "GPIO4") (pintype "bidirectional+no_connect"))
    (pad "7" smd rect (at -8.89 -8.89 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 41 "unconnected-(U3-GPIO5-Pad7)") (pinfunction "GPIO5") (pintype "bidirectional+no_connect"))
    (pad "8" smd rect (at -8.89 -6.35 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd rect (at -8.89 -3.81 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 40 "unconnected-(U3-GPIO6-Pad9)") (pinfunction "GPIO6") (pintype "bidirectional+no_connect"))
    (pad "10" smd rect (at -8.89 -1.27 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 39 "unconnected-(U3-GPIO7-Pad10)") (pinfunction "GPIO7") (pintype "bidirectional+no_connect"))
    (pad "11" smd rect (at -8.89 1.27 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 38 "unconnected-(U3-GPIO8-Pad11)") (pinfunction "GPIO8") (pintype "bidirectional+no_connect"))
    (pad "12" smd rect (at -8.89 3.81 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 3 "Net-(IC1-B0)") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd rect (at -8.89 6.35 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd rect (at -8.89 8.89 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 37 "unconnected-(U3-GPIO10-Pad14)") (pinfunction "GPIO10") (pintype "bidirectional+no_connect"))
    (pad "15" smd rect (at -8.89 11.43 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 4 "Net-(IC1-B2)") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "16" smd rect (at -8.89 13.97 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 36 "unconnected-(U3-GPIO12-Pad16)") (pinfunction "GPIO12") (pintype "bidirectional+no_connect"))
    (pad "17" smd rect (at -8.89 16.51 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 5 "Net-(IC1-B4)") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "18" smd rect (at -8.89 19.05 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" smd rect (at -8.89 21.59 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 35 "unconnected-(U3-GPIO14-Pad19)") (pinfunction "GPIO14") (pintype "bidirectional+no_connect"))
    (pad "20" smd rect (at -8.89 24.13 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(IC1-B6)") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "21" smd rect (at 8.89 24.13 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 34 "unconnected-(U3-GPIO16-Pad21)") (pinfunction "GPIO16") (pintype "bidirectional+no_connect"))
    (pad "22" smd rect (at 8.89 21.59 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 33 "unconnected-(U3-GPIO17-Pad22)") (pinfunction "GPIO17") (pintype "bidirectional+no_connect"))
    (pad "23" smd rect (at 8.89 19.05 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "24" smd rect (at 8.89 16.51 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 32 "unconnected-(U3-GPIO18-Pad24)") (pinfunction "GPIO18") (pintype "bidirectional+no_connect"))
    (pad "25" smd rect (at 8.89 13.97 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 31 "unconnected-(U3-GPIO19-Pad25)") (pinfunction "GPIO19") (pintype "bidirectional+no_connect"))
    (pad "26" smd rect (at 8.89 11.43 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 21 "Net-(U3-GPIO20)") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "27" smd rect (at 8.89 8.89 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 50 "unconnected-(U3-GPIO21-Pad27)") (pinfunction "GPIO21") (pintype "bidirectional+no_connect"))
    (pad "28" smd rect (at 8.89 6.35 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "29" smd rect (at 8.89 3.81 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 47 "unconnected-(U3-GPIO22-Pad29)") (pinfunction "GPIO22") (pintype "bidirectional+no_connect"))
    (pad "30" smd rect (at 8.89 1.27 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 49 "Net-(JP1-C)") (pinfunction "RUN") (pintype "input"))
    (pad "31" smd rect (at 8.89 -1.27 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 30 "unconnected-(U3-GPIO26_ADC0-Pad31)") (pinfunction "GPIO26_ADC0") (pintype "bidirectional+no_connect"))
    (pad "32" smd rect (at 8.89 -3.81 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 29 "unconnected-(U3-GPIO27_ADC1-Pad32)") (pinfunction "GPIO27_ADC1") (pintype "bidirectional+no_connect"))
    (pad "33" smd rect (at 8.89 -6.35 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "AGND") (pintype "power_in"))
    (pad "34" smd rect (at 8.89 -8.89 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 28 "unconnected-(U3-GPIO28_ADC2-Pad34)") (pinfunction "GPIO28_ADC2") (pintype "bidirectional+no_connect"))
    (pad "35" smd rect (at 8.89 -11.43 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 27 "unconnected-(U3-ADC_VREF-Pad35)") (pinfunction "ADC_VREF") (pintype "unspecified+no_connect"))
    (pad "36" smd rect (at 8.89 -13.97 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 1 "3_3V_Pico") (pinfunction "3V3") (pintype "power_in"))
    (pad "37" smd rect (at 8.89 -16.51 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 26 "unconnected-(U3-3V3_EN-Pad37)") (pinfunction "3V3_EN") (pintype "input+no_connect"))
    (pad "38" smd rect (at 8.89 -19.05 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "39" smd rect (at 8.89 -21.59 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 25 "unconnected-(U3-VSYS-Pad39)") (pinfunction "VSYS") (pintype "unspecified+no_connect"))
    (pad "40" smd rect (at 8.89 -24.13 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 24 "unconnected-(U3-VBUS-Pad40)") (pinfunction "VBUS") (pintype "unspecified+no_connect"))
    (pad "41" smd rect (at -2.54 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 23 "unconnected-(U3-SWCLK-Pad41)") (pinfunction "SWCLK") (pintype "input+no_connect"))
    (pad "42" smd rect (at 0 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "43" smd rect (at 2.54 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 22 "unconnected-(U3-SWDIO-Pad43)") (pinfunction "SWDIO") (pintype "bidirectional+no_connect"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 166.542 78.2462 135)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.82 135) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 135) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 14 "PC1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 135) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 9 "Net-(IC1-A2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_SL_171971-0002_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 99.5482 62.3094 180)
    (descr "Molex Stackable Linear Connector, 171971-0002 (compatible alternatives: 171971-0102, 171971-0202), 2 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J8" (at -3.7438 -2.2306) (layer "F.SilkS"))
    (fp_text value "EXT PWR" (at 6.1162 1.3594 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 1.85) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 180) (size 1.74 1.74) (drill 1.09) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1436781609)
      (net 52 "EXT. PWR") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.74 1.74) (drill 1.09) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0002_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 176.9752 92.7244)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA")
    (attr smd)
    (fp_text reference "J5" (at 0.1868 -1.8172 180) (layer "F.SilkS"))
    (fp_text value "Pseudoclock 1" (at 9.0068 2.1656) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "PC1") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 90) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 98.3868 70.1228)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "500" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 11 "Net-(J2-In)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 18 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 92.742 108.5412)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "mounting_holes.kicad_sch")
    (property "Sheetname" "Mounting Holes")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 3.121 -0.009) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0 3.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 96.835 75.302 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 11 "Net-(J2-In)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 108.587 68.654)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 1.5628 -2.0544) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "3_3V_Pico") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 105.625 79.071)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "Power_Connections.kicad_sch")
    (property "Sheetname" "Power connections (jumpers)")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "0" (at 4.3098 0.0176) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICs:SOIC127P1032X265-20N" (layer "F.Cu")
    (at 155.572 73.6362 180)
    (descr "SO20")
    (tags "Integrated Circuit")
    (property "Arrow Part Number" "74LVT245D,118")
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/74lvt245d118/nexperia")
    (property "Description" "74LVT245 - 3.3 V octal transceiver with direction pin (3-state)@en-us")
    (property "Height" "2.65")
    (property "Manufacturer_Name" "Nexperia")
    (property "Manufacturer_Part_Number" "74LVT245D,118")
    (property "Mouser Part Number" "")
    (property "Mouser Price/Stock" "")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "74LVT245 - 3.3 V octal transceiver with direction pin (3-state)@en-us")
    (attr smd)
    (fp_text reference "IC1" (at 0 0) (layer "F.SilkS"))
    (fp_text value "74LVT245D,118" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "DIR") (pintype "passive"))
    (pad "2" smd rect (at -4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(IC1-A0)") (pinfunction "A0") (pintype "passive"))
    (pad "3" smd rect (at -4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(IC1-A0)") (pinfunction "A1") (pintype "passive"))
    (pad "4" smd rect (at -4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(IC1-A2)") (pinfunction "A2") (pintype "passive"))
    (pad "5" smd rect (at -4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "Net-(IC1-A2)") (pinfunction "A3") (pintype "passive"))
    (pad "6" smd rect (at -4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(IC1-A4)") (pinfunction "A4") (pintype "passive"))
    (pad "7" smd rect (at -4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "Net-(IC1-A4)") (pinfunction "A5") (pintype "passive"))
    (pad "8" smd rect (at -4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(IC1-A6)") (pinfunction "A6") (pintype "passive"))
    (pad "9" smd rect (at -4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "Net-(IC1-A6)") (pinfunction "A7") (pintype "passive"))
    (pad "10" smd rect (at -4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "11" smd rect (at 4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(IC1-B6)") (pinfunction "B7") (pintype "passive"))
    (pad "12" smd rect (at 4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "Net-(IC1-B6)") (pinfunction "B6") (pintype "passive"))
    (pad "13" smd rect (at 4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(IC1-B4)") (pinfunction "B5") (pintype "passive"))
    (pad "14" smd rect (at 4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(IC1-B4)") (pinfunction "B4") (pintype "passive"))
    (pad "15" smd rect (at 4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(IC1-B2)") (pinfunction "B3") (pintype "passive"))
    (pad "16" smd rect (at 4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(IC1-B2)") (pinfunction "B2") (pintype "passive"))
    (pad "17" smd rect (at 4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(IC1-B0)") (pinfunction "B1") (pintype "passive"))
    (pad "18" smd rect (at 4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(IC1-B0)") (pinfunction "B0") (pintype "passive"))
    (pad "19" smd rect (at 4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "~{OE}") (pintype "passive"))
    (pad "20" smd rect (at 4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Power Supply") (pinfunction "VCC") (pintype "passive"))
    (model "74LVT245D,118.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 110.652 83.538)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "PrawnBlaster_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, both open")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP1" (at 2.3408 0.0166 90) (layer "F.SilkS"))
    (fp_text value "RESET" (at -2.3876 2.54 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(JP1-C)") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(JP1-B-Pad3)") (pinfunction "B") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 87.042 57.1638) (end 180.042 115.5332)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Ext Clk" (at 88.112 77.81) (layer "F.SilkS"))
  (gr_text "Clk 3" (at 177.43 69.1042) (layer "F.SilkS"))
  (gr_text "Clk 0" (at 177.038 114.1942) (layer "F.SilkS"))
  (gr_text "Clk 1" (at 177.117 99.4512) (layer "F.SilkS"))
  (gr_text "Clk 2" (at 177.273 84.4732) (layer "F.SilkS"))
  (gr_text "Ext Trg" (at 87.772 105.26) (layer "F.SilkS"))
  (gr_text "Ext Ref" (at 91.1368 62.1228) (layer "Dwgs.User"))
  (gr_text "Ext Trig" (at 91.54055 104.9368) (layer "Dwgs.User"))
  (gr_text "No" (at 52.07 186.265) (layer "F.Fab"))
  (gr_text "No" (at 108.47 181.75) (layer "F.Fab"))
  (gr_text "None" (at 52.07 181.75) (layer "F.Fab"))
  (gr_text "Castellated pads: " (at 19.512857 186.265) (layer "F.Fab"))
  (gr_text "Impedance Control: " (at 83.627143 181.75) (layer "F.Fab"))
  (gr_text "Copper Layer Count: " (at 19.512857 168.205) (layer "F.Fab"))
  (gr_text "Min track/spacing: " (at 19.512857 177.235) (layer "F.Fab"))
  (gr_text "No" (at 52.07 190.78) (layer "F.Fab"))
  (gr_text "1.6000 mm" (at 108.47 168.205) (layer "F.Fab"))
  (gr_text "0.2000 mm / 0.0000 mm" (at 52.07 177.235) (layer "F.Fab"))
  (gr_text "" (at 108.47 172.72) (layer "F.Fab"))
  (gr_text "0.0000 mm x 0.0000 mm" (at 52.07 172.72) (layer "F.Fab"))
  (gr_text "BOARD CHARACTERISTICS" (at 18.762857 162.035) (layer "F.Fab"))
  (gr_text "Board overall dimensions: " (at 19.512857 172.72) (layer "F.Fab"))
  (gr_text "0.3000 mm" (at 108.47 177.235) (layer "F.Fab"))
  (gr_text "" (at 83.627143 172.72) (layer "F.Fab"))
  (gr_text "2" (at 52.07 168.205) (layer "F.Fab"))
  (gr_text "Min hole diameter: " (at 83.627143 177.235) (layer "F.Fab"))
  (gr_text "No" (at 108.47 186.265) (layer "F.Fab"))
  (gr_text "Board Thickness: " (at 83.627143 168.205) (layer "F.Fab"))
  (gr_text "Plated Board Edge: " (at 83.627143 186.265) (layer "F.Fab"))
  (gr_text "Edge card connectors: " (at 19.512857 190.78) (layer "F.Fab"))
  (gr_text "Copper Finish: " (at 19.512857 181.75) (layer "F.Fab"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.0882 112.7314)
        (xy 121.3382 112.7314)
        (xy 121.3382 98.2314)
        (xy 130.0882 98.2314)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.042 115.54)
        (xy 87.052 115.54)
        (xy 87.052 57.15)
        (xy 180.022 57.17)
      )
    )
  )
)
