(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "Star Tracker Model B PCB Layout")
		(date "2026-02-18")
		(rev "3")
		(company "Univeristy of Idaho")
		(comment 1 "NASA-ASA")
		(comment 2 "Designed by Emmitt Helms")
		(comment 3 "Interdisciplinary Capstone Design, 2025-2026")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_0a000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref yes)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../../../../UIdaho/ECE 4800-4810/Star Tracker/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/+5v")
	(net 3 "/+3.3v")
	(net 4 "Net-(D1-K)")
	(net 5 "Net-(D2-K)")
	(net 6 "/DPHY0_C_P")
	(net 7 "/DPHY0_D2_N")
	(net 8 "/DPHY0_C_N")
	(net 9 "/CAM_GPIO1")
	(net 10 "/DPHY0_D0_P")
	(net 11 "/DPHY0_D1_P")
	(net 12 "/CAM_GPIO0")
	(net 13 "/DPHY0_D2_P")
	(net 14 "/DPHY0_D3_P")
	(net 15 "/SCL0")
	(net 16 "/DPHY0_D0_N")
	(net 17 "/SDA0")
	(net 18 "/DPHY0_D3_N")
	(net 19 "/DPHY0_D1_N")
	(net 20 "/PCIE_nCLKREQ")
	(net 21 "/PCIe_nRST")
	(net 22 "/PCIe_RX_P")
	(net 23 "/PCIE_nWAKE")
	(net 24 "/PCIe_TX_P")
	(net 25 "/PCIe_CLK_P")
	(net 26 "/PCIe_CLK_N")
	(net 27 "/PCIe_TX_N")
	(net 28 "/PCIE_PWR_EN")
	(net 29 "/PCIe_RX_N")
	(net 30 "unconnected-(Module1B-HDMI0_CLK_P-Pad188)")
	(net 31 "unconnected-(Module1B-HDMI1_TX2_P-Pad146)")
	(net 32 "unconnected-(Module1B-HDMI1_TX1_P-Pad152)")
	(net 33 "unconnected-(Module1B-VBUS_EN-Pad111)")
	(net 34 "unconnected-(Module1B-HDMI1_TX0_N-Pad160)")
	(net 35 "unconnected-(Module1B-MIPI1_D2_N-Pad193)")
	(net 36 "unconnected-(Module1B-HDMI0_HOTPLUG-Pad153)")
	(net 37 "unconnected-(Module1B-HDMI1_TX2_N-Pad148)")
	(net 38 "unconnected-(Module1B-HDMI0_TX0_P-Pad182)")
	(net 39 "unconnected-(Module1A-ID_SD-Pad36)")
	(net 40 "unconnected-(Module1A-ID_SC-Pad35)")
	(net 41 "unconnected-(Module1B-HDMI1_HOTPLUG-Pad143)")
	(net 42 "unconnected-(Module1B-USB3-0-TX_N-Pad140)")
	(net 43 "unconnected-(Module1A-Ethernet_Pair3_N-Pad5)")
	(net 44 "unconnected-(Module1A-GPIO19-Pad26)")
	(net 45 "unconnected-(Module1A-SD_DAT7-Pad70)")
	(net 46 "unconnected-(Module1A-Ethernet_SYNC_OUT(3.3v)-Pad18)")
	(net 47 "unconnected-(Module1A-GPIO9-Pad40)")
	(net 48 "unconnected-(Module1B-USB3-1-TX_P-Pad171)")
	(net 49 "unconnected-(Module1A-Ethernet_Pair2_P-Pad11)")
	(net 50 "unconnected-(Module1A-GPIO4-Pad54)")
	(net 51 "unconnected-(Module1A-Ethernet_Pair3_P-Pad3)")
	(net 52 "unconnected-(Module1A-GPIO27-Pad48)")
	(net 53 "unconnected-(Module1B-USB3-0-RX_P-Pad130)")
	(net 54 "unconnected-(Module1B-USB3-1-D_N-Pad165)")
	(net 55 "unconnected-(Module1A-Ethernet_Pair0_P-Pad12)")
	(net 56 "unconnected-(Module1A-GPIO6-Pad30)")
	(net 57 "unconnected-(Module1B-HDMI0_CLK_N-Pad190)")
	(net 58 "unconnected-(Module1A-GPIO12-Pad31)")
	(net 59 "unconnected-(Module1A-GPIO16-Pad29)")
	(net 60 "unconnected-(Module1A-SD_DAT5-Pad64)")
	(net 61 "unconnected-(Module1B-HDMI0_TX2_P-Pad170)")
	(net 62 "unconnected-(Module1B-HDMI0_SDA-Pad199)")
	(net 63 "unconnected-(Module1A-GPIO13-Pad28)")
	(net 64 "unconnected-(Module1B-MIPI1_D1_P-Pad183)")
	(net 65 "unconnected-(Module1B-USB_OTG_ID-Pad101)")
	(net 66 "unconnected-(Module1B-USB3-0-D_P-Pad134)")
	(net 67 "unconnected-(Module1A-GPIO10-Pad44)")
	(net 68 "unconnected-(Module1A-GPIO11-Pad38)")
	(net 69 "unconnected-(Module1A-GPIO14-Pad55)")
	(net 70 "unconnected-(Module1A-Ethernet_nLED2(3.3v)-Pad17)")
	(net 71 "unconnected-(Module1B-HDMI1_SCL-Pad147)")
	(net 72 "unconnected-(Module1A-WiFi_nDisable-Pad89)")
	(net 73 "unconnected-(Module1B-HDMI1_TX1_N-Pad154)")
	(net 74 "unconnected-(Module1A-Ethernet_Pair1_N-Pad6)")
	(net 75 "unconnected-(Module1A-GPIO18-Pad49)")
	(net 76 "unconnected-(Module1B-USB3-1-RX_P-Pad159)")
	(net 77 "unconnected-(Module1B-MIPI1_D3_P-Pad196)")
	(net 78 "unconnected-(Module1B-MIPI1_C_P-Pad189)")
	(net 79 "/VBAT")
	(net 80 "unconnected-(Module1B-HDMI1_CEC-Pad149)")
	(net 81 "unconnected-(Module1B-USB3-1-D_P-Pad163)")
	(net 82 "unconnected-(Module1A-nRPIBOOT-Pad93)")
	(net 83 "unconnected-(Module1B-HDMI0_TX2_N-Pad172)")
	(net 84 "unconnected-(Module1A-GPIO26-Pad24)")
	(net 85 "unconnected-(Module1A-GPIO23-Pad47)")
	(net 86 "unconnected-(Module1A-GPIO3-Pad56)")
	(net 87 "unconnected-(Module1B-USB3-0-RX_N-Pad128)")
	(net 88 "unconnected-(Module1B-USB3-0-TX_P-Pad142)")
	(net 89 "unconnected-(Module1B-HDMI0_TX1_N-Pad178)")
	(net 90 "unconnected-(Module1A-GPIO21-Pad25)")
	(net 91 "unconnected-(Module1A-GPIO25-Pad41)")
	(net 92 "unconnected-(Module1B-HDMI0_TX1_P-Pad176)")
	(net 93 "unconnected-(Module1B-HDMI0_SCL-Pad200)")
	(net 94 "unconnected-(Module1A-Ethernet_Pair0_N-Pad10)")
	(net 95 "unconnected-(Module1B-MIPI1_D1_N-Pad181)")
	(net 96 "Net-(Module1A-+1.8v_(Output)-Pad88)")
	(net 97 "unconnected-(Module1A-Ethernet_Pair2_N-Pad9)")
	(net 98 "unconnected-(Module1B-USB3-0-D_N-Pad136)")
	(net 99 "unconnected-(Module1B-MIPI1_D2_P-Pad195)")
	(net 100 "unconnected-(Module1A-BT_nDisable-Pad91)")
	(net 101 "unconnected-(Module1A-GPIO2-Pad58)")
	(net 102 "unconnected-(Module1A-SD_DAT4-Pad68)")
	(net 103 "unconnected-(Module1B-HDMI1_CLK_N-Pad166)")
	(net 104 "unconnected-(Module1A-GPIO22-Pad46)")
	(net 105 "/GPIO_VREF")
	(net 106 "unconnected-(Module1B-MIPI1_C_N-Pad187)")
	(net 107 "unconnected-(Module1A-GPIO5-Pad34)")
	(net 108 "unconnected-(Module1B-MIPI1_D0_N-Pad175)")
	(net 109 "unconnected-(Module1A-GPIO24-Pad45)")
	(net 110 "unconnected-(Module1B-MIPI1_D3_N-Pad194)")
	(net 111 "unconnected-(Module1B-HDMI0_CEC-Pad151)")
	(net 112 "unconnected-(Module1A-Ethernet_Pair1_P-Pad4)")
	(net 113 "unconnected-(Module1B-HDMI1_CLK_P-Pad164)")
	(net 114 "unconnected-(Module1B-USB3-1-RX_N-Pad157)")
	(net 115 "unconnected-(Module1B-USB3-1-TX_N-Pad169)")
	(net 116 "unconnected-(Module1B-HDMI0_TX0_N-Pad184)")
	(net 117 "unconnected-(Module1A-GPIO15-Pad51)")
	(net 118 "unconnected-(Module1A-GPIO7-Pad37)")
	(net 119 "unconnected-(Module1A-FAN_TACHO-Pad16)")
	(net 120 "unconnected-(Module1A-EEPROM_nWP-Pad20)")
	(net 121 "unconnected-(Module1B-MIPI1_D0_P-Pad177)")
	(net 122 "unconnected-(Module1A-Ethernet_nLED3(3.3v)-Pad15)")
	(net 123 "unconnected-(Module1A-GPIO20-Pad27)")
	(net 124 "unconnected-(Module1A-SD_VDD_Override-Pad73)")
	(net 125 "unconnected-(Module1B-HDMI1_TX0_P-Pad158)")
	(net 126 "unconnected-(Module1A-GPIO17-Pad50)")
	(net 127 "unconnected-(Module1A-SD_DAT6-Pad72)")
	(net 128 "unconnected-(Module1A-FAN_PWM-Pad19)")
	(net 129 "unconnected-(Module1B-HDMI1_SDA-Pad145)")
	(net 130 "unconnected-(Module1A-GPIO8-Pad39)")
	(net 131 "/LED_nPWR")
	(net 132 "/LED_nACT")
	(net 133 "unconnected-(Module1B-USB2_P-Pad105)")
	(net 134 "unconnected-(Module1A-PWR_BUT-Pad92)")
	(net 135 "unconnected-(Module1A-CC1-Pad94)")
	(net 136 "unconnected-(Module1A-CC2-Pad96)")
	(net 137 "unconnected-(Module1A-PMIC_ENABLE-Pad99)")
	(net 138 "unconnected-(Module1B-USB2_N-Pad103)")
	(net 139 "unconnected-(Module1A-SD_PWR_ON-Pad75)")
	(net 140 "unconnected-(Module1A-SD_DAT1-Pad67)")
	(net 141 "unconnected-(Module1A-SD_CLK-Pad57)")
	(net 142 "unconnected-(Module1A-SD_DAT0-Pad63)")
	(net 143 "unconnected-(Module1A-SD_DAT3-Pad61)")
	(net 144 "unconnected-(Module1A-SD_CMD-Pad62)")
	(net 145 "unconnected-(Module1A-SD_DAT2-Pad69)")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 147.65 107.73)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.47 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 3.34 0.475 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Farnell"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "2611911"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" "RM EMK105 B7104KV-F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" "TAIYO YUDEN EUROPE GMBH"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" "110091611"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/+5v")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 90.67254 48.374229)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(thermal_bridge_width 2.54)
			(thermal_bridge_angle 0)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_THTPad_D4.0mm_Drill2.0mm"
		(layer "F.Cu")
		(at 176.39746 52.184389)
		(descr "THT pad as test Point, diameter 4.0mm, hole diameter 2.0mm")
		(tags "test point THT pad")
		(property "Reference" "H2"
			(at 0.1 -4.24 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_THTPad_D0.25in_Drill0.12in"
			(at -0.025 4.325 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 -2.325 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(thermal_bridge_width 2.54)
			(thermal_bridge_angle 0)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 136.38 108.5975 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 2.1375 1.21 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED Green"
			(at 3.4775 -0.82 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS22-2000-226/LTST-S270KGKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Digikey "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "LTST-S270KGKT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" "SML-A12M8TT86N"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" "Rohm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" "650263301"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "	Green 572nm LED Indication - Discrete 2.2V 2-SMD, No Lead"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/+3.3v")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D4.0mm_Drill2.0mm"
		(layer "F.Cu")
		(at 90.67254 48.374229)
		(descr "THT pad as test Point, diameter 4.0mm, hole diameter 2.0mm")
		(tags "test point THT pad")
		(property "Reference" "H1"
			(at 4.83 -0.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_THTPad_D0.25in_Drill0.12in"
			(at -0.025 4.325 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 4.83 -0.02 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "CM5IO:HRS_FH12-16S-0.5SVA_54_"
		(layer "F.Cu")
		(at 98.2962 86.045909 90)
		(tags "FH12-16S-0.5SV55 ")
		(property "Reference" "J4"
			(at -6.9898 -0.0662 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FH12-16S-0.5SVA(54)"
			(at -15 2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x16, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "FH12-16S-0.5SVA(54)"
			(at -15 2 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 1.3462 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 3.75 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 3.250001 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at 2.75 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.250001 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/PCIe_CLK_P")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at 1.749999 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/PCIe_CLK_N")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at 1.25 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at 0.750001 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/PCIe_RX_P")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at 0.25 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/PCIe_RX_N")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at -0.25 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at -0.750001 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/PCIe_TX_P")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at -1.25 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/PCIe_TX_N")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at -1.749999 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at -2.250001 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/PCIE_PWR_EN")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at -2.75 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/PCIE_nWAKE")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd rect
			(at -3.250001 -1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "/PCIE_nCLKREQ")
			(pinfunction "Pin_15")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd rect
			(at -3.75 1.3462 90)
			(size 0.6096 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/PCIe_nRST")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at -4.7498 1.3462 90)
			(size 0.8128 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd rect
			(at 4.7498 1.3462 90)
			(size 0.8128 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd rect
			(at -4.7498 -1.3462 90)
			(size 0.8128 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd rect
			(at 4.7498 -1.3462 90)
			(size 0.8128 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/FH12-16S-0.5SVA-54---3DModel-STEP-1.STEP"
			(offset
				(xyz -16.891 9.017 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
	)
	(footprint "CM5IO:Raspberry-Pi-5-Compute-Module"
		(layer "F.Cu")
		(at 165.11 111.079309 90)
		(descr "Raspberry Pi 5 Compute Module")
		(tags "Raspberry Pi 5 Compute Module")
		(property "Reference" "M2"
			(at 18.38 -5.08 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M2 HAT+ AI Module"
			(at 32.2 0.89 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RaspberryPi M2 HAT+"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "M2 HAT+ mounting holes locations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "" np_thru_hole circle
			(at 0 -58 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 49 -58 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 49 0 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/1-1734839-6.STEP"
			(offset
				(xyz 26.5 56 18.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 180)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/2199230-8.STEP"
			(offset
				(xyz 25.5 39 19.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/m20-7812045.stp"
			(offset
				(xyz 49 4.5 17.79)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/630_thou_Standoff-Body.step"
			(offset
				(xyz 28.9179 24.3205 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/630_thou_Standoff-Body.step"
			(offset
				(xyz 28.9179 82.41792 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/630_thou_Standoff-Body.step"
			(offset
				(xyz 77.8891 82.41792 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/630_thou_Standoff-Body.step"
			(offset
				(xyz 77.8891 24.3205 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/RPi_M2_Board-Body.step"
			(offset
				(xyz 24.4983 28.92552 15.9766)
			)
			(scale
				(xyz 1.001 1.004 0.94)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "CM5IO:Raspberry-Pi-5-Compute-Module"
		(layer "F.Cu")
		(at 160.29 100.479309 90)
		(descr "Raspberry Pi 5 Compute Module")
		(tags "Raspberry Pi 5 Compute Module")
		(property "Reference" "Compute_Module_5"
			(at 18.5 -5 90)
			(layer "F.SilkS")
		)
		(property "Value" "ComputeModule5-CM5"
			(at 16.52 0.19 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RaspberryPi Compute module 5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Amphenol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "2x 10164227-1001A1RLF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" "2x 10164227-1001A1RLF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" "Hirose"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "	100 Position Connector Receptacle, Center Strip Contacts Surface Mount Gold"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "UIdaho_NASA-ASA_Star_Tracker_modB.kicad_sch")
		(attr smd)
		(pad "" np_thru_hole circle
			(at 0 -48 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 33 -48 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "" np_thru_hole circle
			(at 33 0 90)
			(size 2.7 2.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin 1.7)
			(clearance 1.7)
		)
		(pad "1" smd rect
			(at -2.04 -31.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 1.04 -31.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.04 -30.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "unconnected-(Module1A-Ethernet_Pair3_P-Pad3)")
			(pinfunction "Ethernet_Pair3_P")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 1.04 -30.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "unconnected-(Module1A-Ethernet_Pair1_P-Pad4)")
			(pinfunction "Ethernet_Pair1_P")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -2.04 -30.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "unconnected-(Module1A-Ethernet_Pair3_N-Pad5)")
			(pinfunction "Ethernet_Pair3_N")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at 1.04 -30.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "unconnected-(Module1A-Ethernet_Pair1_N-Pad6)")
			(pinfunction "Ethernet_Pair1_N")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at -2.04 -30.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at 1.04 -30.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at -2.04 -29.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "unconnected-(Module1A-Ethernet_Pair2_N-Pad9)")
			(pinfunction "Ethernet_Pair2_N")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at 1.04 -29.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "unconnected-(Module1A-Ethernet_Pair0_N-Pad10)")
			(pinfunction "Ethernet_Pair0_N")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at -2.04 -29.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "unconnected-(Module1A-Ethernet_Pair2_P-Pad11)")
			(pinfunction "Ethernet_Pair2_P")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 1.04 -29.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "unconnected-(Module1A-Ethernet_Pair0_P-Pad12)")
			(pinfunction "Ethernet_Pair0_P")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at -2.04 -28.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at 1.04 -28.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd rect
			(at -2.04 -28.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "unconnected-(Module1A-Ethernet_nLED3(3.3v)-Pad15)")
			(pinfunction "Ethernet_nLED3(3.3v)")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd rect
			(at 1.04 -28.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "unconnected-(Module1A-FAN_TACHO-Pad16)")
			(pinfunction "FAN_TACHO")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at -2.04 -28.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "unconnected-(Module1A-Ethernet_nLED2(3.3v)-Pad17)")
			(pinfunction "Ethernet_nLED2(3.3v)")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd rect
			(at 1.04 -28.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "unconnected-(Module1A-Ethernet_SYNC_OUT(3.3v)-Pad18)")
			(pinfunction "Ethernet_SYNC_OUT(3.3v)")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd rect
			(at -2.04 -27.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "unconnected-(Module1A-FAN_PWM-Pad19)")
			(pinfunction "FAN_PWM")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd rect
			(at 1.04 -27.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "unconnected-(Module1A-EEPROM_nWP-Pad20)")
			(pinfunction "EEPROM_nWP")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd rect
			(at -2.04 -27.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "/LED_nACT")
			(pinfunction "LED_nACT")
			(pintype "open_collector")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd rect
			(at 1.04 -27.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd rect
			(at -2.04 -26.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd rect
			(at 1.04 -26.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "unconnected-(Module1A-GPIO26-Pad24)")
			(pinfunction "GPIO26")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd rect
			(at -2.04 -26.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "unconnected-(Module1A-GPIO21-Pad25)")
			(pinfunction "GPIO21")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd rect
			(at 1.04 -26.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "unconnected-(Module1A-GPIO19-Pad26)")
			(pinfunction "GPIO19")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd rect
			(at -2.04 -26.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "unconnected-(Module1A-GPIO20-Pad27)")
			(pinfunction "GPIO20")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd rect
			(at 1.04 -26.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "unconnected-(Module1A-GPIO13-Pad28)")
			(pinfunction "GPIO13")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd rect
			(at -2.04 -25.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "unconnected-(Module1A-GPIO16-Pad29)")
			(pinfunction "GPIO16")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd rect
			(at 1.04 -25.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "unconnected-(Module1A-GPIO6-Pad30)")
			(pinfunction "GPIO6")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd rect
			(at -2.04 -25.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "unconnected-(Module1A-GPIO12-Pad31)")
			(pinfunction "GPIO12")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd rect
			(at 1.04 -25.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" smd rect
			(at -2.04 -24.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" smd rect
			(at 1.04 -24.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "unconnected-(Module1A-GPIO5-Pad34)")
			(pinfunction "GPIO5")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" smd rect
			(at -2.04 -24.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "unconnected-(Module1A-ID_SC-Pad35)")
			(pinfunction "ID_SC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" smd rect
			(at 1.04 -24.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "unconnected-(Module1A-ID_SD-Pad36)")
			(pinfunction "ID_SD")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" smd rect
			(at -2.04 -24.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "unconnected-(Module1A-GPIO7-Pad37)")
			(pinfunction "GPIO7")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" smd rect
			(at 1.04 -24.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "unconnected-(Module1A-GPIO11-Pad38)")
			(pinfunction "GPIO11")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" smd rect
			(at -2.04 -23.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "unconnected-(Module1A-GPIO8-Pad39)")
			(pinfunction "GPIO8")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" smd rect
			(at 1.04 -23.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "unconnected-(Module1A-GPIO9-Pad40)")
			(pinfunction "GPIO9")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "41" smd rect
			(at -2.04 -23.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "unconnected-(Module1A-GPIO25-Pad41)")
			(pinfunction "GPIO25")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "42" smd rect
			(at 1.04 -23.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "43" smd rect
			(at -2.04 -22.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "44" smd rect
			(at 1.04 -22.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "unconnected-(Module1A-GPIO10-Pad44)")
			(pinfunction "GPIO10")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "45" smd rect
			(at -2.04 -22.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "unconnected-(Module1A-GPIO24-Pad45)")
			(pinfunction "GPIO24")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "46" smd rect
			(at 1.04 -22.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "unconnected-(Module1A-GPIO22-Pad46)")
			(pinfunction "GPIO22")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "47" smd rect
			(at -2.04 -22.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(Module1A-GPIO23-Pad47)")
			(pinfunction "GPIO23")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "48" smd rect
			(at 1.04 -22.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "unconnected-(Module1A-GPIO27-Pad48)")
			(pinfunction "GPIO27")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "49" smd rect
			(at -2.04 -21.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "unconnected-(Module1A-GPIO18-Pad49)")
			(pinfunction "GPIO18")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "50" smd rect
			(at 1.04 -21.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "unconnected-(Module1A-GPIO17-Pad50)")
			(pinfunction "GPIO17")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "51" smd rect
			(at -2.04 -21.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "unconnected-(Module1A-GPIO15-Pad51)")
			(pinfunction "GPIO15")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "52" smd rect
			(at 1.04 -21.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "53" smd rect
			(at -2.04 -20.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "54" smd rect
			(at 1.04 -20.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "unconnected-(Module1A-GPIO4-Pad54)")
			(pinfunction "GPIO4")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "55" smd rect
			(at -2.04 -20.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "unconnected-(Module1A-GPIO14-Pad55)")
			(pinfunction "GPIO14")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "56" smd rect
			(at 1.04 -20.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "unconnected-(Module1A-GPIO3-Pad56)")
			(pinfunction "GPIO3")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "57" smd rect
			(at -2.04 -20.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "unconnected-(Module1A-SD_CLK-Pad57)")
			(pinfunction "SD_CLK")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "58" smd rect
			(at 1.04 -20.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "unconnected-(Module1A-GPIO2-Pad58)")
			(pinfunction "GPIO2")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "59" smd rect
			(at -2.04 -19.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "60" smd rect
			(at 1.04 -19.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "61" smd rect
			(at -2.04 -19.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "unconnected-(Module1A-SD_DAT3-Pad61)")
			(pinfunction "SD_DAT3")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "62" smd rect
			(at 1.04 -19.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "unconnected-(Module1A-SD_CMD-Pad62)")
			(pinfunction "SD_CMD")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "63" smd rect
			(at -2.04 -18.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "unconnected-(Module1A-SD_DAT0-Pad63)")
			(pinfunction "SD_DAT0")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "64" smd rect
			(at 1.04 -18.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "unconnected-(Module1A-SD_DAT5-Pad64)")
			(pinfunction "SD_DAT5")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "65" smd rect
			(at -2.04 -18.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "66" smd rect
			(at 1.04 -18.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "67" smd rect
			(at -2.04 -18.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "unconnected-(Module1A-SD_DAT1-Pad67)")
			(pinfunction "SD_DAT1")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "68" smd rect
			(at 1.04 -18.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "unconnected-(Module1A-SD_DAT4-Pad68)")
			(pinfunction "SD_DAT4")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "69" smd rect
			(at -2.04 -17.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "unconnected-(Module1A-SD_DAT2-Pad69)")
			(pinfunction "SD_DAT2")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "70" smd rect
			(at 1.04 -17.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "unconnected-(Module1A-SD_DAT7-Pad70)")
			(pinfunction "SD_DAT7")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "71" smd rect
			(at -2.04 -17.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "72" smd rect
			(at 1.04 -17.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "unconnected-(Module1A-SD_DAT6-Pad72)")
			(pinfunction "SD_DAT6")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "73" smd rect
			(at -2.04 -16.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "unconnected-(Module1A-SD_VDD_Override-Pad73)")
			(pinfunction "SD_VDD_Override")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "74" smd rect
			(at 1.04 -16.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "75" smd rect
			(at -2.04 -16.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "unconnected-(Module1A-SD_PWR_ON-Pad75)")
			(pinfunction "SD_PWR_ON")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "76" smd rect
			(at 1.04 -16.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "/VBAT")
			(pinfunction "VBAT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "77" smd rect
			(at -2.04 -16.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "78" smd rect
			(at 1.04 -16.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "/GPIO_VREF")
			(pinfunction "GPIO_VREF(1.8v/3.3v_Input)")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "79" smd rect
			(at -2.04 -15.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "80" smd rect
			(at 1.04 -15.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/SCL0")
			(pinfunction "SCL0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "81" smd rect
			(at -2.04 -15.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "82" smd rect
			(at 1.04 -15.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/SDA0")
			(pinfunction "SDA0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "83" smd rect
			(at -2.04 -14.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "84" smd rect
			(at 1.04 -14.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/+3.3v")
			(pinfunction "+3.3v_(Output)")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "85" smd rect
			(at -2.04 -14.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "86" smd rect
			(at 1.04 -14.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/+3.3v")
			(pinfunction "+3.3v_(Output)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "87" smd rect
			(at -2.04 -14.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "+5v_(Input)")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "88" smd rect
			(at 1.04 -14.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "Net-(Module1A-+1.8v_(Output)-Pad88)")
			(pinfunction "+1.8v_(Output)")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "89" smd rect
			(at -2.04 -13.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "unconnected-(Module1A-WiFi_nDisable-Pad89)")
			(pinfunction "WiFi_nDisable")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "90" smd rect
			(at 1.04 -13.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "Net-(Module1A-+1.8v_(Output)-Pad88)")
			(pinfunction "+1.8v_(Output)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "91" smd rect
			(at -2.04 -13.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "unconnected-(Module1A-BT_nDisable-Pad91)")
			(pinfunction "BT_nDisable")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "92" smd rect
			(at 1.04 -13.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "unconnected-(Module1A-PWR_BUT-Pad92)")
			(pinfunction "PWR_BUT")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "93" smd rect
			(at -2.04 -12.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "unconnected-(Module1A-nRPIBOOT-Pad93)")
			(pinfunction "nRPIBOOT")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "94" smd rect
			(at 1.04 -12.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "unconnected-(Module1A-CC1-Pad94)")
			(pinfunction "CC1")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "95" smd rect
			(at -2.04 -12.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "/LED_nPWR")
			(pinfunction "LED_nPWR")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "96" smd rect
			(at 1.04 -12.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "unconnected-(Module1A-CC2-Pad96)")
			(pinfunction "CC2")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "97" smd rect
			(at -2.04 -12.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/CAM_GPIO0")
			(pinfunction "CAM_GPIO0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "98" smd rect
			(at 1.04 -12.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "99" smd rect
			(at -2.04 -11.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "unconnected-(Module1A-PMIC_ENABLE-Pad99)")
			(pinfunction "PMIC_ENABLE")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "100" smd rect
			(at 1.04 -11.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/CAM_GPIO1")
			(pinfunction "CAM_GPIO1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "101" smd rect
			(at 31.96 -31.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "unconnected-(Module1B-USB_OTG_ID-Pad101)")
			(pinfunction "USB_OTG_ID")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "102" smd rect
			(at 35.04 -31.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "/PCIE_nCLKREQ")
			(pinfunction "PCIe_nCLKREQ")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "103" smd rect
			(at 31.96 -30.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "unconnected-(Module1B-USB2_N-Pad103)")
			(pinfunction "USB2_N")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "104" smd rect
			(at 35.04 -30.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/PCIE_nWAKE")
			(pinfunction "PCIE_nWAKE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "105" smd rect
			(at 31.96 -30.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "unconnected-(Module1B-USB2_P-Pad105)")
			(pinfunction "USB2_P")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "106" smd rect
			(at 35.04 -30.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/PCIE_PWR_EN")
			(pinfunction "PCIE_PWR_EN")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "107" smd rect
			(at 31.96 -30.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "108" smd rect
			(at 35.04 -30.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "109" smd rect
			(at 31.96 -29.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/PCIe_nRST")
			(pinfunction "PCIe_nRST")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "110" smd rect
			(at 35.04 -29.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/PCIe_CLK_P")
			(pinfunction "PCIe_CLK_P")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "111" smd rect
			(at 31.96 -29.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(Module1B-VBUS_EN-Pad111)")
			(pinfunction "VBUS_EN")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "112" smd rect
			(at 35.04 -29.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/PCIe_CLK_N")
			(pinfunction "PCIe_CLK_N")
			(pintype "output")
			(die_length 0.01)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "113" smd rect
			(at 31.96 -28.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "114" smd rect
			(at 35.04 -28.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "115" smd rect
			(at 31.96 -28.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/DPHY0_D0_N")
			(pinfunction "MIPI0_D0_N")
			(pintype "input")
			(die_length 0.01)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "116" smd rect
			(at 35.04 -28.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/PCIe_RX_P")
			(pinfunction "PCIe_RX_P")
			(pintype "input")
			(die_length 0.84)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "117" smd rect
			(at 31.96 -28.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/DPHY0_D0_P")
			(pinfunction "MIPI0_D0_P")
			(pintype "input")
			(die_length 0.02)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "118" smd rect
			(at 35.04 -28.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/PCIe_RX_N")
			(pinfunction "PCIe_RX_N")
			(pintype "input")
			(die_length 0.84)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "119" smd rect
			(at 31.96 -27.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "120" smd rect
			(at 35.04 -27.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "121" smd rect
			(at 31.96 -27.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/DPHY0_D1_N")
			(pinfunction "MIPI0_D1_N")
			(pintype "input")
			(die_length 0.4)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "122" smd rect
			(at 35.04 -27.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/PCIe_TX_P")
			(pinfunction "PCIe_TX_P")
			(pintype "output")
			(die_length 3.71)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "123" smd rect
			(at 31.96 -26.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/DPHY0_D1_P")
			(pinfunction "MIPI0_D1_P")
			(pintype "input")
			(die_length 0.4)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "124" smd rect
			(at 35.04 -26.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/PCIe_TX_N")
			(pinfunction "PCIe_TX_N")
			(pintype "output")
			(die_length 3.72)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "125" smd rect
			(at 31.96 -26.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "126" smd rect
			(at 35.04 -26.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "127" smd rect
			(at 31.96 -26.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/DPHY0_C_N")
			(pinfunction "MIPI0_C_N")
			(pintype "input")
			(die_length 0.78)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "128" smd rect
			(at 35.04 -26.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "unconnected-(Module1B-USB3-0-RX_N-Pad128)")
			(pinfunction "USB3-0-RX_N")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "129" smd rect
			(at 31.96 -25.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/DPHY0_C_P")
			(pinfunction "MIPI0_C_P")
			(pintype "input")
			(die_length 0.78)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "130" smd rect
			(at 35.04 -25.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "unconnected-(Module1B-USB3-0-RX_P-Pad130)")
			(pinfunction "USB3-0-RX_P")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "131" smd rect
			(at 31.96 -25.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "132" smd rect
			(at 35.04 -25.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "133" smd rect
			(at 31.96 -24.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/DPHY0_D2_N")
			(pinfunction "MIPI0_D2_N")
			(pintype "input")
			(die_length 0.04)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "134" smd rect
			(at 35.04 -24.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "unconnected-(Module1B-USB3-0-D_P-Pad134)")
			(pinfunction "USB3-0-D_P")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "135" smd rect
			(at 31.96 -24.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/DPHY0_D2_P")
			(pinfunction "MIPI0_D2_P")
			(pintype "input")
			(die_length 0.03)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "136" smd rect
			(at 35.04 -24.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "unconnected-(Module1B-USB3-0-D_N-Pad136)")
			(pinfunction "USB3-0-D_N")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "137" smd rect
			(at 31.96 -24.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "138" smd rect
			(at 35.04 -24.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "139" smd rect
			(at 31.96 -23.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/DPHY0_D3_N")
			(pinfunction "MIPI0_D3_N")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "140" smd rect
			(at 35.04 -23.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "unconnected-(Module1B-USB3-0-TX_N-Pad140)")
			(pinfunction "USB3-0-TX_N")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "141" smd rect
			(at 31.96 -23.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/DPHY0_D3_P")
			(pinfunction "MIPI0_D3_P")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "142" smd rect
			(at 35.04 -23.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(Module1B-USB3-0-TX_P-Pad142)")
			(pinfunction "USB3-0-TX_P")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "143" smd rect
			(at 31.96 -22.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "unconnected-(Module1B-HDMI1_HOTPLUG-Pad143)")
			(pinfunction "HDMI1_HOTPLUG")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "144" smd rect
			(at 35.04 -22.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "145" smd rect
			(at 31.96 -22.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "unconnected-(Module1B-HDMI1_SDA-Pad145)")
			(pinfunction "HDMI1_SDA")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "146" smd rect
			(at 35.04 -22.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(Module1B-HDMI1_TX2_P-Pad146)")
			(pinfunction "HDMI1_TX2_P")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "147" smd rect
			(at 31.96 -22.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "unconnected-(Module1B-HDMI1_SCL-Pad147)")
			(pinfunction "HDMI1_SCL")
			(pintype "open_collector+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "148" smd rect
			(at 35.04 -22.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(Module1B-HDMI1_TX2_N-Pad148)")
			(pinfunction "HDMI1_TX2_N")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "149" smd rect
			(at 31.96 -21.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "unconnected-(Module1B-HDMI1_CEC-Pad149)")
			(pinfunction "HDMI1_CEC")
			(pintype "open_collector+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "150" smd rect
			(at 35.04 -21.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "151" smd rect
			(at 31.96 -21.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "unconnected-(Module1B-HDMI0_CEC-Pad151)")
			(pinfunction "HDMI0_CEC")
			(pintype "open_collector+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "152" smd rect
			(at 35.04 -21.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(Module1B-HDMI1_TX1_P-Pad152)")
			(pinfunction "HDMI1_TX1_P")
			(pintype "output+no_connect")
			(die_length 5.18)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "153" smd rect
			(at 31.96 -20.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(Module1B-HDMI0_HOTPLUG-Pad153)")
			(pinfunction "HDMI0_HOTPLUG")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "154" smd rect
			(at 35.04 -20.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(Module1B-HDMI1_TX1_N-Pad154)")
			(pinfunction "HDMI1_TX1_N")
			(pintype "output+no_connect")
			(die_length 5.18)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "155" smd rect
			(at 31.96 -20.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "156" smd rect
			(at 35.04 -20.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "157" smd rect
			(at 31.96 -20.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "unconnected-(Module1B-USB3-1-RX_N-Pad157)")
			(pinfunction "USB3-1-RX_N")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "158" smd rect
			(at 35.04 -20.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "unconnected-(Module1B-HDMI1_TX0_P-Pad158)")
			(pinfunction "HDMI1_TX0_P")
			(pintype "output+no_connect")
			(die_length 4.75)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "159" smd rect
			(at 31.96 -19.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "unconnected-(Module1B-USB3-1-RX_P-Pad159)")
			(pinfunction "USB3-1-RX_P")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "160" smd rect
			(at 35.04 -19.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(Module1B-HDMI1_TX0_N-Pad160)")
			(pinfunction "HDMI1_TX0_N")
			(pintype "output+no_connect")
			(die_length 4.76)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "161" smd rect
			(at 31.96 -19.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "162" smd rect
			(at 35.04 -19.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "163" smd rect
			(at 31.96 -18.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "unconnected-(Module1B-USB3-1-D_P-Pad163)")
			(pinfunction "USB3-1-D_P")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "164" smd rect
			(at 35.04 -18.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "unconnected-(Module1B-HDMI1_CLK_P-Pad164)")
			(pinfunction "HDMI1_CLK_P")
			(pintype "output+no_connect")
			(die_length 2.99)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "165" smd rect
			(at 31.96 -18.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "unconnected-(Module1B-USB3-1-D_N-Pad165)")
			(pinfunction "USB3-1-D_N")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "166" smd rect
			(at 35.04 -18.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "unconnected-(Module1B-HDMI1_CLK_N-Pad166)")
			(pinfunction "HDMI1_CLK_N")
			(pintype "output+no_connect")
			(die_length 2.99)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "167" smd rect
			(at 31.96 -18.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "168" smd rect
			(at 35.04 -18.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "169" smd rect
			(at 31.96 -17.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "unconnected-(Module1B-USB3-1-TX_N-Pad169)")
			(pinfunction "USB3-1-TX_N")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "170" smd rect
			(at 35.04 -17.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "unconnected-(Module1B-HDMI0_TX2_P-Pad170)")
			(pinfunction "HDMI0_TX2_P")
			(pintype "output+no_connect")
			(die_length 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "171" smd rect
			(at 31.96 -17.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "unconnected-(Module1B-USB3-1-TX_P-Pad171)")
			(pinfunction "USB3-1-TX_P")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "172" smd rect
			(at 35.04 -17.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "unconnected-(Module1B-HDMI0_TX2_N-Pad172)")
			(pinfunction "HDMI0_TX2_N")
			(pintype "output+no_connect")
			(die_length 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "173" smd rect
			(at 31.96 -16.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "174" smd rect
			(at 35.04 -16.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "175" smd rect
			(at 31.96 -16.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "unconnected-(Module1B-MIPI1_D0_N-Pad175)")
			(pinfunction "MIPI1_D0_N")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "176" smd rect
			(at 35.04 -16.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "unconnected-(Module1B-HDMI0_TX1_P-Pad176)")
			(pinfunction "HDMI0_TX1_P")
			(pintype "output+no_connect")
			(die_length 5.18)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "177" smd rect
			(at 31.96 -16.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "unconnected-(Module1B-MIPI1_D0_P-Pad177)")
			(pinfunction "MIPI1_D0_P")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "178" smd rect
			(at 35.04 -16.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "unconnected-(Module1B-HDMI0_TX1_N-Pad178)")
			(pinfunction "HDMI0_TX1_N")
			(pintype "output+no_connect")
			(die_length 5.18)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "179" smd rect
			(at 31.96 -15.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "180" smd rect
			(at 35.04 -15.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "181" smd rect
			(at 31.96 -15.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "unconnected-(Module1B-MIPI1_D1_N-Pad181)")
			(pinfunction "MIPI1_D1_N")
			(pintype "output+no_connect")
			(die_length 1.06)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "182" smd rect
			(at 35.04 -15.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(Module1B-HDMI0_TX0_P-Pad182)")
			(pinfunction "HDMI0_TX0_P")
			(pintype "output+no_connect")
			(die_length 0.18)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "183" smd rect
			(at 31.96 -14.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "unconnected-(Module1B-MIPI1_D1_P-Pad183)")
			(pinfunction "MIPI1_D1_P")
			(pintype "output+no_connect")
			(die_length 1.05)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "184" smd rect
			(at 35.04 -14.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "unconnected-(Module1B-HDMI0_TX0_N-Pad184)")
			(pinfunction "HDMI0_TX0_N")
			(pintype "output+no_connect")
			(die_length 0.18)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "185" smd rect
			(at 31.96 -14.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "186" smd rect
			(at 35.04 -14.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "187" smd rect
			(at 31.96 -14.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "unconnected-(Module1B-MIPI1_C_N-Pad187)")
			(pinfunction "MIPI1_C_N")
			(pintype "output+no_connect")
			(die_length 1.28)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "188" smd rect
			(at 35.04 -14.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(Module1B-HDMI0_CLK_P-Pad188)")
			(pinfunction "HDMI0_CLK_P")
			(pintype "output+no_connect")
			(die_length 0.91)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "189" smd rect
			(at 31.96 -13.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "unconnected-(Module1B-MIPI1_C_P-Pad189)")
			(pinfunction "MIPI1_C_P")
			(pintype "output+no_connect")
			(die_length 1.27)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "190" smd rect
			(at 35.04 -13.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "unconnected-(Module1B-HDMI0_CLK_N-Pad190)")
			(pinfunction "HDMI0_CLK_N")
			(pintype "output+no_connect")
			(die_length 0.91)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "191" smd rect
			(at 31.96 -13.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "192" smd rect
			(at 35.04 -13.3)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "193" smd rect
			(at 31.96 -12.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(Module1B-MIPI1_D2_N-Pad193)")
			(pinfunction "MIPI1_D2_N")
			(pintype "output+no_connect")
			(die_length 0.83)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "194" smd rect
			(at 35.04 -12.9)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "unconnected-(Module1B-MIPI1_D3_N-Pad194)")
			(pinfunction "MIPI1_D3_N")
			(pintype "output+no_connect")
			(die_length 3.79)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "195" smd rect
			(at 31.96 -12.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "unconnected-(Module1B-MIPI1_D2_P-Pad195)")
			(pinfunction "MIPI1_D2_P")
			(pintype "output+no_connect")
			(die_length 0.84)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "196" smd rect
			(at 35.04 -12.5)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "unconnected-(Module1B-MIPI1_D3_P-Pad196)")
			(pinfunction "MIPI1_D3_P")
			(pintype "output+no_connect")
			(die_length 3.79)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "197" smd rect
			(at 31.96 -12.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "198" smd rect
			(at 35.04 -12.1)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "199" smd rect
			(at 31.96 -11.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "unconnected-(Module1B-HDMI0_SDA-Pad199)")
			(pinfunction "HDMI0_SDA")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "200" smd rect
			(at 35.04 -11.7)
			(size 0.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "unconnected-(Module1B-HDMI0_SCL-Pad200)")
			(pinfunction "HDMI0_SCL")
			(pintype "open_collector+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/10164227-1001a1rlf.stp"
			(offset
				(xyz -0.5 21.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/10164227-1001a1rlf.stp"
			(offset
				(xyz 33.5 21.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/CM5R5-3dsteps.step"
			(offset
				(xyz 36.4998 -3.50012 1.4224)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "CM5IO:CON_525592253_MOL"
		(layer "F.Cu")
		(at 134.860012 52.519309)
		(tags "525592253 ")
		(property "Reference" "J2"
			(at 10.609988 -0.28 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "525592253"
			(at -14.220012 -2.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.molex.com/en-us/products/part-detail-pdf/525592253?display=pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "525592253"
			(at 1.450011 3.93 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "525592253"
			(at 1.450011 3.93 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at -10.960012 -1.33 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5.24999 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -4.74999 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/DPHY0_D0_N")
			(pinfunction "2")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -4.249989 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/DPHY0_D0_P")
			(pinfunction "3")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at -3.749989 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "4")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -3.249989 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/DPHY0_D1_N")
			(pinfunction "5")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at -2.74999 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/DPHY0_D1_P")
			(pinfunction "6")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at -2.249989 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "7")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at -1.749989 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/DPHY0_C_N")
			(pinfunction "8")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at -1.249989 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/DPHY0_C_P")
			(pinfunction "9")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at -0.749989 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "10")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at -0.249989 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/DPHY0_D2_N")
			(pinfunction "11")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 0.250011 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/DPHY0_D2_P")
			(pinfunction "12")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at 0.750011 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "13")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at 1.250011 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/DPHY0_D3_N")
			(pinfunction "14")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd rect
			(at 1.750011 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/DPHY0_D3_P")
			(pinfunction "15")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd rect
			(at 2.250011 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "16")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 2.750011 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/CAM_GPIO0")
			(pinfunction "17")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd rect
			(at 3.250011 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/CAM_GPIO1")
			(pinfunction "18")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd rect
			(at 3.750011 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "19")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd rect
			(at 4.250011 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/SCL0")
			(pinfunction "20")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd rect
			(at 4.750011 1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/SDA0")
			(pinfunction "21")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd rect
			(at 5.250011 -1.4)
			(size 0.6 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/+3.3v")
			(pinfunction "22")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "P1" smd rect
			(at -6.249988 1.4)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "P2" smd rect
			(at 6.249988 1.4)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "P3" smd rect
			(at -6.249988 -1.4)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "P4" smd rect
			(at 6.249988 -1.4)
			(size 0.8 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/0525592253.stp"
			(offset
				(xyz 0 -1.143 3.175)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 -0)
			)
		)
	)
	(footprint "CM5IO:CONN_SD-43650-005_02_MOL"
		(layer "F.Cu")
		(at 145.16 118.64)
		(tags "436500213 ")
		(property "Reference" "J1"
			(at -6.270002 6.252691 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "436500213"
			(at -0.890002 8.452691 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.molex.com/en-us/products/part-detail-pdf/436500213?display=pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "436500213"
			(at -1 8.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -6.300002 6.212691 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 1.5 -5.123)
			(size 1.27 2.921)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "1")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -1.5 -5.123)
			(size 1.27 2.921)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/+5v")
			(pinfunction "2")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -5.384998 0.347)
			(size 3.429 1.651)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 5.384998 0.347)
			(size 3.429 1.651)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 139.590799 115.3369) (xy 139.590799 116.9371) (xy 142.029199 116.9371) (xy 142.029199 115.3369)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 148.290801 115.3369) (xy 148.290801 116.9371) (xy 150.729201 116.9371) (xy 150.729201 115.3369)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/CM5IO.3dshapes/0436500213.stp"
			(offset
				(xyz 0 -4.9276 0.5588)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 165.33 92.7 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -0.045 2.769309 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.455 -0.010691 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/+3.3v")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/VBAT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D4.0mm_Drill2.0mm"
		(layer "F.Cu")
		(at 90.67508 128.384389)
		(descr "THT pad as test Point, diameter 4.0mm, hole diameter 2.0mm")
		(tags "test point THT pad")
		(property "Reference" "H4"
			(at -0.06 -4.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_THTPad_D0.25in_Drill0.12in"
			(at -0.025 4.325 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at -0.06 -4.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(thermal_bridge_width 2.54)
			(thermal_bridge_angle 0)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.72 107.73 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.42 -1.59 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 1.97 -3.26 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://search.murata.co.jp/Ceramy/image/img/A01X/G101/ENG/GRM155R71C104KA88-01.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Farnell"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "2611911"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" "RM EMK105 B7104KV-F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" "TAIYO YUDEN EUROPE GMBH"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" "110091611"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "	0.1uF 10% 16V Ceramic Capacitor X7R 0402 (1005 Metric)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/+5v")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 134.32 108.6175 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.74 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Farnell"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "9239235"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" "KOA EUROPE GMBH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" "RK73H1ETTP1001F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Resistor 1K M1005 1% 63mW"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" "125049511"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1-K)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/LED_nACT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 165.21 95.359309 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.300691 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0.820691 -1.63 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/GPIO_VREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/+3.3v")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 176.399968 125.845947)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(thermal_bridge_width 2.54)
			(thermal_bridge_angle 0)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 157.71 110.519309 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -0.03 -1.87 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED Green"
			(at 0.580691 5.38 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS22-2000-226/LTST-S270KGKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Digikey "
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "LTST-S270KGKT"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" "SML-A12M8TT86N"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" "Rohm"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" "650263301"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "	Green 572nm LED Indication - Discrete 2.2V 2-SMD, No Lead"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/+3.3v")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D4.0mm_Drill2.0mm"
		(layer "F.Cu")
		(at 176.399968 125.845947)
		(descr "THT pad as test Point, diameter 4.0mm, hole diameter 2.0mm")
		(tags "test point THT pad")
		(property "Reference" "H3"
			(at 0.03 -4.29 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_THTPad_D0.25in_Drill0.12in"
			(at -0.025 4.325 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0.3 -2.325 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 157.71 107.03 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 1.85 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -0.425 -1.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://fscdn.rohm.com/en/products/databook/datasheet/passive/resistor/chip_resistor/mcr-e.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field4" "Farnell"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" "9239235"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" "KOA EUROPE GMBH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" "RK73H1ETTP1001F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Description" "Resistor 1K M1005 1% 63mW"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" "125049511"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D2-K)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "/LED_nPWR")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 176.39746 52.184389)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 90.67508 128.384389)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.35 6.35)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 177.890423 59.975232)
		(end 180.749957 57.100681)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.396793 47.731603)
		(end 99.971793 47.731603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 89.303164 56.800232)
		(mid 89.650004 57.319309)
		(end 89.771793 57.931603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.528164 129.500232)
		(end 174.377715 132.359767)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 87.571793 132.831603)
		(mid 86.440429 132.362971)
		(end 85.971793 131.231603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 95.96587 132.359767)
		(mid 95.446793 132.706606)
		(end 94.834499 132.828396)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 86.443629 53.95068)
		(mid 86.096793 53.431603)
		(end 85.975 52.819309)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.978164 123.937974)
		(mid 86.099966 123.325686)
		(end 86.446793 122.806603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.221793 131.231603)
		(end 181.218586 120.793897)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.749957 119.662527)
		(end 177.890423 116.787974)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 174.377716 44.403439)
		(mid 174.896793 44.056598)
		(end 175.509087 43.93481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.971793 129.031603)
		(end 170.396793 129.031603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 98.840422 129.500232)
		(mid 99.359499 129.153395)
		(end 99.971793 129.031603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.218586 55.969303)
		(end 181.221793 45.531603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.771793 57.931603)
		(end 89.771793 118.831603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.621793 43.931603)
		(mid 180.753164 44.400232)
		(end 181.221793 45.531603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.421793 61.106603)
		(mid 177.543586 60.49431)
		(end 177.890422 59.975232)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 89.771793 118.831603)
		(mid 89.650002 119.443897)
		(end 89.303164 119.962974)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 170.396793 129.031603)
		(mid 171.009088 129.153393)
		(end 171.528164 129.500232)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 99.971793 47.731603)
		(mid 99.359501 47.609808)
		(end 98.840422 47.262974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.965869 132.359767)
		(end 98.840422 129.500232)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 180.749957 119.662526)
		(mid 181.096793 120.181603)
		(end 181.218586 120.793897)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.221793 131.231603)
		(mid 180.753164 132.362974)
		(end 179.621793 132.831603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.971793 45.531603)
		(end 85.975 52.819309)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.421793 115.656603)
		(end 177.421793 61.106603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 86.44363 53.95068)
		(end 89.303163 56.800232)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 94.8345 43.93481)
		(mid 95.446793 44.056603)
		(end 95.965871 44.403439)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 98.840422 47.262973)
		(end 95.965871 44.403439)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.509093 132.828396)
		(end 179.621793 132.831603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.377716 44.40344)
		(end 171.528164 47.262974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.303164 119.962973)
		(end 86.446793 122.806603)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.571793 132.831603)
		(end 94.834499 132.828396)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.834493 43.93481)
		(end 87.571793 43.931603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.890422 116.787974)
		(mid 177.543586 116.268897)
		(end 177.421793 115.656603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.528164 47.262974)
		(mid 171.009086 47.609809)
		(end 170.396793 47.731603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 175.509086 132.828396)
		(mid 174.896796 132.706598)
		(end 174.377715 132.359767)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.621793 43.931603)
		(end 175.509087 43.93481)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.978164 123.937974)
		(end 85.971793 131.231603)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.218586 55.96931)
		(mid 181.096793 56.581603)
		(end 180.749957 57.100681)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.971793 45.531603)
		(mid 86.440424 44.400234)
		(end 87.571793 43.931603)
		(layer "Edge.Cuts")
	)
	(gr_text "Power LED"
		(at 154.12 113.479309 0)
		(layer "F.SilkS")
	)
	(gr_text "Power In"
		(at 139.76 126.049309 0)
		(layer "F.SilkS")
	)
	(gr_text "Activity\nLED"
		(at 134.87 112.76 0)
		(layer "F.SilkS")
	)
	(gr_text "2026"
		(at 153.26 125.11 0)
		(layer "F.SilkS")
	)
	(gr_text "Camera"
		(at 129.16 50.089309 0)
		(layer "F.SilkS")
	)
	(gr_text "Designed by Emmitt Helms"
		(at 153.17 124.179309 0)
		(layer "F.SilkS")
	)
	(gr_text "Star Tracker Model B Rev 3\nNASA-ASA\nUniversity of Idaho"
		(at 153.05 122.859309 0)
		(layer "F.SilkS")
	)
	(gr_text "RPi AI Kit"
		(at 94.87 91.769309 90)
		(layer "F.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 85.974979 127.584216) (xy 90.67508 128.384389)
		)
		(height 23.705093)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.18504"
			(at 88.32503 153.17 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 150.39 129.039309) (xy 150.39 123.72)
		)
		(height 0)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.2094"
			(at 151.63 126.37946 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 177.566084 132.83) (xy 177.421793 61.106603)
		)
		(height 12.253916)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "2.82376"
			(at 189.87 96.968301 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 91.203146 132.83) (xy 91.204275 43.933207)
		)
		(height -7.133146)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.49987"
			(at 84.34 90.57 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 139.775002 118.987) (xy 139.78 129.03)
		)
		(height -2.395002)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.3954"
			(at 136.28 124.0085 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 91.203146 132.83) (xy 90.67254 48.374229)
		)
		(height -10.553146)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.32503"
			(at 80.53 82.1 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 177.566084 132.83) (xy 176.39746 52.184389)
		)
		(height 8.763916)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.17502"
			(at 186.316321 90.720873 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 85.974978 127.584789) (xy 99.971793 129.031603)
		)
		(height 19.78452)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.55106"
			(at 94.179596 147.372825 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 91.203146 132.83) (xy 90.67508 128.384389)
		)
		(height -20.673146)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.17502"
			(at 68.73 130.607194 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 177.566084 132.83) (xy 177.4218 115.656609)
		)
		(height 15.683916)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.67612"
			(at 193.252244 122.44106 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 91.203146 132.83) (xy 89.771792 118.831603)
		)
		(height -17.033146)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.55112"
			(at 74.183133 125.313133 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 177.566084 132.83) (xy 176.399968 125.845947)
		)
		(height 19.443916)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.27496"
			(at 199.38 129.337973 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 85.974979 127.584216) (xy 181.22019 126.014377)
		)
		(height 9.805093)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.74981"
			(at 140.73 137.29 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 87.49754 48.374229) (xy 93.84754 48.374229)
		)
		(height -8.51492)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.25"
			(at 90.67254 38.709309 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 85.974979 127.584216) (xy 176.399968 125.845947)
		)
		(height 13.155093)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.56004"
			(at 119.69 140.69 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 91.203146 132.83) (xy 89.771793 57.931603)
		)
		(height -14.183146)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "2.94876"
			(at 76.93 97.41 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 174.87346 52.184389) (xy 177.92146 52.184389)
		)
		(height -12.83508)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "0.12"
			(at 176.39746 38.199309 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 85.974978 127.584789) (xy 170.396793 129.031603)
		)
		(height 16.51452)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.32369"
			(at 132.260984 144.06 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 85.973397 49.175456) (xy 176.39746 52.184389)
		)
		(height -7.566147)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 5)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "3.56"
			(at 131.185429 41.6 0)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.04855 68.156152) (xy 127.913848 68.02145) (xy 127.717687 68.474083) (xy 127.949293 68.630016)
				(xy 128.182313 68.474083)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/PCIe_RX_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.96944 85.512673) (xy 97.831144 85.650969) (xy 98.085009 86.031315) (xy 98.296909 85.890907)
				(xy 98.345755 85.641081)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/DPHY0_C_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.313799 68.069309) (xy 134.161399 68.069309) (xy 134.126489 68.169309) (xy 134.19 68.520309)
				(xy 134.29 68.525574)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/DPHY0_D3_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.8064 52.869309) (xy 136.654 52.869309) (xy 136.393941 53.169309) (xy 136.610023 53.920309)
				(xy 136.910023 53.169309)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/PCIE_nWAKE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.7092 88.891159) (xy 100.7092 88.700659) (xy 100.4044 88.491109) (xy 99.6414 88.795909) (xy 100.4044 89.100709)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/DPHY0_D3_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.9936 52.169309) (xy 136.146 52.169309) (xy 136.381501 51.869309) (xy 136.110023 51.118309)
				(xy 135.810023 51.869309)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/CAM_GPIO0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.27475 98.372428) (xy 149.46525 98.372428) (xy 149.619119 97.918862) (xy 149.37 97.868309)
				(xy 149.120881 97.918862)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.28475 105.643431) (xy 136.47525 105.643431) (xy 136.654031 105.144508) (xy 136.38 105.089)
				(xy 136.105969 105.144508)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/DPHY0_D3_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.6662 68.069309) (xy 136.5138 68.069309) (xy 136.49 68.169309) (xy 136.59 68.520309) (xy 136.69 68.169309)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.335 96.089059) (xy 164.335 96.279559) (xy 164.858463 96.569085) (xy 165.211 96.184309) (xy 164.858463 95.799533)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/DPHY0_D1_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.113799 68.069309) (xy 132.961399 68.069309) (xy 132.926489 68.169309) (xy 132.99 68.520309)
				(xy 133.09 68.525574)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/DPHY0_D0_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.066 52.066881) (xy 129.9136 52.066881) (xy 129.740681 52.520447) (xy 129.9898 52.571) (xy 130.238919 52.520447)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PCIe_CLK_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.826881 84.22241) (xy 97.826881 84.41799) (xy 98.280447 84.569319) (xy 98.331 84.3202) (xy 98.280447 84.071081)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/PCIE_nCLKREQ")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.0168 89.39116) (xy 98.0168 89.20066) (xy 97.712 88.99111) (xy 96.949 89.29591) (xy 97.712 89.60071)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.272428 100.80525) (xy 145.272428 100.61475) (xy 144.818862 100.460881) (xy 144.768309 100.71)
				(xy 144.818862 100.959119)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/DPHY0_D1_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.656 52.869309) (xy 131.5036 52.869309) (xy 131.310023 53.169309) (xy 131.610023 53.920309)
				(xy 131.888551 53.169309)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.69475 64.39654) (xy 129.88525 64.39654) (xy 129.824236 63.851473) (xy 129.53 63.909) (xy 129.363329 64.159441)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/CAM_GPIO1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.49475 98.053119) (xy 148.68525 98.053119) (xy 148.849119 97.599553) (xy 148.6 97.549) (xy 148.350881 97.599553)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/SCL0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.73475 97.803119) (xy 144.92525 97.803119) (xy 145.079119 97.349553) (xy 144.83 97.299) (xy 144.580881 97.349553)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.946863 111.041468) (xy 156.812159 111.176172) (xy 157.282134 111.654892) (xy 157.710707 111.307516)
				(xy 157.370038 110.88596)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/DPHY0_D0_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.574 53.073119) (xy 130.7264 53.073119) (xy 130.899319 52.619553) (xy 130.6502 52.569) (xy 130.401081 52.619553)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/DPHY0_D1_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.5036 53.088226) (xy 131.656 53.088226) (xy 131.828919 52.63466) (xy 131.5798 52.584107)
				(xy 131.330681 52.63466)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/DPHY0_C_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.156 52.026881) (xy 133.0036 52.026881) (xy 132.830681 52.480447) (xy 133.0798 52.531) (xy 133.328919 52.480447)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/DPHY0_D1_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.164 52.169309) (xy 132.3164 52.169309) (xy 132.410022 51.869309) (xy 132.110022 51.118309)
				(xy 131.900749 51.869309)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/PCIE_nCLKREQ")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.819255 89.20066) (xy 97.819255 89.39116) (xy 98.299407 89.470116) (xy 98.354915 89.196085)
				(xy 98.198689 88.963772)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.0168 88.39525) (xy 98.0168 88.20475) (xy 97.712 87.99403) (xy 96.949 88.29591) (xy 97.712 88.60071)
			)
		)
	)
	(zone
		(net 105)
		(net_name "/GPIO_VREF")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.335 94.439059) (xy 164.335 94.629559) (xy 164.858463 94.919085) (xy 165.211 94.534309) (xy 164.858463 94.149533)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/PCIe_CLK_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.114385 66.587851) (xy 127.976089 66.449555) (xy 127.56696 66.477394) (xy 127.615806 66.72722)
				(xy 127.757628 66.937706)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PCIe_CLK_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.324114 66.94178) (xy 128.324114 66.7462) (xy 127.942372 66.982294) (xy 128.082487 67.193487)
				(xy 128.332606 67.143934)
			)
		)
	)
	(zone
		(net 132)
		(net_name "/LED_nACT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.617062 107.472358) (xy 133.482358 107.607062) (xy 133.858911 108.062438) (xy 134.320707 107.793207)
				(xy 134.045 107.3925)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.765185 67.364305) (xy 128.765185 67.554805) (xy 129.264108 67.733586) (xy 129.319616 67.459555)
				(xy 129.264108 67.185524)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/SDA0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.194217 98.243538) (xy 145.32892 98.378241) (xy 145.598853 98.001115) (xy 145.388367 97.859293)
				(xy 145.138541 97.909553)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.009693 50.30274) (xy 140.210353 50.30274) (xy 140.394031 49.803817) (xy 140.12 49.748309)
				(xy 139.845969 49.803817)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D2-K)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.61475 108.655) (xy 157.80525 108.655) (xy 158.11 108.207393) (xy 157.71 107.854) (xy 157.31 108.207393)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/DPHY0_D2_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.4536 53.088226) (xy 134.606 53.088226) (xy 134.778919 52.63466) (xy 134.5298 52.584107)
				(xy 134.280681 52.63466)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/DPHY0_D0_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.7264 52.869309) (xy 130.574 52.869309) (xy 130.338513 53.169309) (xy 130.610023 53.920309)
				(xy 130.910023 53.169309)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/DPHY0_C_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.664 53.033119) (xy 133.8164 53.033119) (xy 133.989319 52.579553) (xy 133.7402 52.529) (xy 133.491081 52.579553)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/PCIe_RX_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.732811 85.497289) (xy 98.732811 85.301709) (xy 98.437317 85.018607) (xy 98.295202 85.2298)
				(xy 98.246649 85.478919)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PCIe_CLK_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.0168 84.41799) (xy 98.0168 84.22241) (xy 97.712 84.008387) (xy 96.949 84.29591) (xy 97.712 84.60071)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/DPHY0_D2_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.513799 68.069309) (xy 135.361399 68.069309) (xy 135.326489 68.169309) (xy 135.39 68.520309)
				(xy 135.49 68.525574)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/PCIe_RX_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.319385 84.852851) (xy 104.181089 84.714555) (xy 103.77196 84.742394) (xy 103.820806 84.99222)
				(xy 103.962628 85.202706)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/CAM_GPIO1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.557966 50.224529) (xy 138.423263 50.089826) (xy 138.083939 50.369309) (xy 138.109316 51.120016)
				(xy 138.410023 51.175469)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.09475 93.575) (xy 166.28525 93.575) (xy 166.539776 93.051537) (xy 166.155 92.699) (xy 165.770224 93.051537)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/DPHY0_D1_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.3164 52.081988) (xy 132.164 52.081988) (xy 131.991081 52.535554) (xy 132.2402 52.586107)
				(xy 132.489319 52.535554)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/PCIe_TX_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.0738 85.969902) (xy 101.87822 85.969902) (xy 101.608607 86.278885) (xy 101.8198 86.421)
				(xy 102.068919 86.469553)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/PCIe_TX_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.825097 86.801709) (xy 97.825097 86.997289) (xy 98.309553 86.948919) (xy 98.261 86.6998) (xy 98.048807 86.558685)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/CAM_GPIO0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.626569 57.234059) (xy 146.626569 57.424559) (xy 147.125492 57.60334) (xy 147.181 57.329309)
				(xy 147.125492 57.055278)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/SDA0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.514773 54.969309) (xy 139.705273 54.969309) (xy 139.910023 54.669309) (xy 139.610023 53.918309)
				(xy 139.310023 54.669309)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D2-K)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.80525 108.856809) (xy 157.61475 108.856809) (xy 157.2725 109.398144) (xy 157.71 109.732809)
				(xy 158.1475 109.398144)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/DPHY0_D2_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.114 52.169309) (xy 135.2664 52.169309) (xy 135.410023 51.869309) (xy 135.110023 51.118309)
				(xy 134.866442 51.869309)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/DPHY0_D0_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.9136 52.169309) (xy 130.066 52.169309) (xy 130.326072 51.869309) (xy 130.110022 51.118309)
				(xy 129.810022 51.869309)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.19242 100.421593) (xy 145.057716 100.286889) (xy 144.628194 100.498807) (xy 144.768602 100.710707)
				(xy 144.980502 100.851115)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/DPHY0_D2_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.2664 52.081988) (xy 135.114 52.081988) (xy 134.941081 52.535554) (xy 135.1902 52.586107)
				(xy 135.439319 52.535554)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/PCIE_nCLKREQ")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.793431 65.674559) (xy 128.793431 65.484059) (xy 128.294508 65.305278) (xy 128.239 65.579309)
				(xy 128.294508 65.85334)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.198119 101.13525) (xy 140.198119 100.94475) (xy 139.744553 100.815881) (xy 139.694 101.065)
				(xy 139.744553 101.314119)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/DPHY0_D2_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.606 52.869309) (xy 134.4536 52.869309) (xy 134.310023 53.169309) (xy 134.610023 53.920309)
				(xy 134.853572 53.169309)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/DPHY0_D3_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.654 53.073119) (xy 136.8064 53.073119) (xy 136.979319 52.619553) (xy 136.7302 52.569) (xy 136.481081 52.619553)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/DPHY0_C_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.8164 52.869309) (xy 133.664 52.869309) (xy 133.400749 53.169309) (xy 133.610023 53.920309)
				(xy 133.910023 53.169309)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/DPHY0_C_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.0036 52.169309) (xy 133.156 52.169309) (xy 133.388551 51.869309) (xy 133.110023 51.118309)
				(xy 132.810023 51.869309)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.40288 100.94475) (xy 144.40288 101.13525) (xy 144.910424 100.921193) (xy 144.770309 100.71)
				(xy 144.52019 100.660447)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/PCIe_TX_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.698426 87.290108) (xy 98.698426 87.094528) (xy 98.210447 87.111081) (xy 98.259 87.3602) (xy 98.401115 87.571393)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/PCIe_CLK_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.833119 83.75759) (xy 98.833119 83.56201) (xy 98.379553 83.410681) (xy 98.329 83.6598) (xy 98.379553 83.908919)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/CAM_GPIO1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.023111 91.751593) (xy 148.888407 91.616889) (xy 148.458885 91.828807) (xy 148.599293 92.040707)
				(xy 148.811193 92.181115)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/+5v")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.246)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.055002 114.984808) (xy 147.325002 114.984808) (xy 147.33 104.479309) (xy 146.29 102.869309)
				(xy 146.29 102.169309) (xy 144.09 102.169309) (xy 144.09 102.869309) (xy 143.055002 104.459309)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/DPHY0_C_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.618601 68.069309) (xy 134.466201 68.069309) (xy 134.49 68.525574) (xy 134.59 68.520309)
				(xy 134.653511 68.169309)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/DPHY0_D2_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.818601 68.069309) (xy 135.666201 68.069309) (xy 135.69 68.525574) (xy 135.79 68.520309)
				(xy 135.853511 68.169309)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.20828)
		)
		(min_thickness 0.1778)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.20828)
			(thermal_bridge_width 0.2032)
		)
		(polygon
			(pts
				(xy 85.12 43.009309) (xy 85.12 133.949309) (xy 182.71 133.949309) (xy 182.71 43.159309)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/PCIe_TX_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.42178 85.969902) (xy 102.2262 85.969902) (xy 102.231081 86.469553) (xy 102.4802 86.421)
				(xy 102.691393 86.278885)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/SCL0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.205273 52.025878) (xy 139.014773 52.025878) (xy 138.855969 52.524801) (xy 139.13 52.580309)
				(xy 139.404031 52.524801)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/SCL0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.014773 52.169309) (xy 139.205273 52.169309) (xy 139.410023 51.869309) (xy 139.110023 51.118309)
				(xy 138.810023 51.869309)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/DPHY0_D0_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.2662 68.069309) (xy 132.1138 68.069309) (xy 132.09 68.169309) (xy 132.19 68.520309) (xy 132.29 68.169309)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/PCIe_CLK_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.5756 83.56201) (xy 98.5756 83.75759) (xy 98.8804 84.005918) (xy 99.6434 83.795908) (xy 98.8804 83.491108)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1-K)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.4675 109.34725) (xy 135.4675 109.53775) (xy 136.040038 109.805849) (xy 136.381 109.385)
				(xy 135.96907 109.01157)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.796569 88.20475) (xy 97.796569 88.39525) (xy 98.295492 88.574031) (xy 98.351 88.3) (xy 98.295492 88.025969)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/DPHY0_D0_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.8662 68.069309) (xy 131.7138 68.069309) (xy 131.69 68.169309) (xy 131.79 68.520309) (xy 131.89 68.169309)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/SDA0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.866296 55.550901) (xy 139.731592 55.685605) (xy 140.010556 56.092357) (xy 140.243576 55.937838)
				(xy 140.297377 55.6631)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1-K)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.195 109.53775) (xy 135.195 109.34725) (xy 134.671537 109.057724) (xy 134.319 109.4425) (xy 134.671537 109.827276)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/CAM_GPIO0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.514773 54.969309) (xy 137.705273 54.969309) (xy 137.910023 54.669309) (xy 137.610023 53.918309)
				(xy 137.310023 54.669309)
			)
		)
	)
	(zone
		(net 79)
		(net_name "/VBAT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.705 92.60475) (xy 163.705 92.79525) (xy 164.152607 93.1) (xy 164.506 92.7) (xy 164.152607 92.3)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.418407 110.78242) (xy 156.553111 110.647716) (xy 156.341193 110.218194) (xy 156.129293 110.358602)
				(xy 155.988885 110.570502)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/DPHY0_D1_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.418601 68.069309) (xy 133.266201 68.069309) (xy 133.29 68.525574) (xy 133.39 68.520309)
				(xy 133.453511 68.169309)
			)
		)
	)
	(zone
		(net 131)
		(net_name "/LED_nPWR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.835 106.154059) (xy 156.835 106.344559) (xy 157.358463 106.589776) (xy 157.711 106.205)
				(xy 157.355068 105.822492)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.931656 95.597357) (xy 165.796952 95.462653) (xy 165.044315 95.784309) (xy 165.209293 96.185016)
				(xy 165.685 96.274994)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/PCIe_nRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.7092 89.891159) (xy 100.7092 89.700659) (xy 100.4044 89.491109) (xy 99.6414 89.795909) (xy 100.4044 90.100709)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.47525 106.935) (xy 136.28475 106.935) (xy 135.9425 107.476335) (xy 136.38 107.811) (xy 136.8175 107.476335)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/PCIe_RX_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.565445 85.098911) (xy 104.427149 84.960615) (xy 104.077294 85.317372) (xy 104.28778 85.459194)
				(xy 104.537606 85.50804)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/DPHY0_D3_N")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.146 52.066881) (xy 135.9936 52.066881) (xy 135.820681 52.520447) (xy 136.0698 52.571) (xy 136.318919 52.520447)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/DPHY0_D3_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.0662 68.069309) (xy 136.9138 68.069309) (xy 136.89 68.169309) (xy 136.99 68.520309) (xy 137.09 68.169309)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/PCIe_RX_P")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.858378 85.678203) (xy 97.996674 85.539907) (xy 97.712 85.219803) (xy 96.949293 85.295201)
				(xy 96.903799 85.600708)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.210353 50.069309) (xy 140.009693 50.069309) (xy 139.810023 50.369309) (xy 140.110023 51.120309)
				(xy 140.410023 50.369309)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/PCIe_RX_N")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.746301 85.483799) (xy 98.746301 85.288219) (xy 98.437317 85.018607) (xy 98.295202 85.2298)
				(xy 98.246649 85.478919)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.440391 50.211588) (xy 140.582279 50.0697) (xy 140.352313 49.594083) (xy 140.119293 49.748602)
				(xy 139.964774 49.981622)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PCIe_CLK_N")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.780099 84.261781) (xy 98.780099 84.066201) (xy 98.280447 84.071081) (xy 98.329 84.3202) (xy 98.471115 84.531393)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/PCIe_TX_N")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.710099 86.953799) (xy 98.710099 86.758219) (xy 98.401115 86.488607) (xy 98.259 86.6998) (xy 98.210447 86.948919)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/PCIe_RX_P")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.790615 85.597149) (xy 103.928911 85.735445) (xy 104.33804 85.707606) (xy 104.289194 85.45778)
				(xy 104.147372 85.247294)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.62525 66.993681) (xy 129.43475 66.993681) (xy 129.16339 67.227242) (xy 129.318616 67.460555)
				(xy 129.592647 67.514063)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.43475 64.504236) (xy 129.62525 64.504236) (xy 129.824236 63.968527) (xy 129.53 63.909) (xy 129.235764 63.968527)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/PCIe_TX_P")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.710099 87.301781) (xy 98.710099 87.106201) (xy 98.210447 87.111081) (xy 98.259 87.3602) (xy 98.401115 87.571393)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/CAM_GPIO0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.503983 57.787995) (xy 147.638687 57.653291) (xy 147.412313 57.174083) (xy 147.179293 57.328602)
				(xy 147.024774 57.561622)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.196012 100.425185) (xy 145.054124 100.283297) (xy 144.628194 100.498807) (xy 144.768602 100.710707)
				(xy 144.980502 100.851115)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/CAM_GPIO1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.50475 92.543119) (xy 148.69525 92.543119) (xy 148.849119 92.089553) (xy 148.6 92.039) (xy 148.350881 92.089553)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/CAM_GPIO1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.69525 97.046881) (xy 148.50475 97.046881) (xy 148.350881 97.500447) (xy 148.6 97.551) (xy 148.849119 97.500447)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/SCL0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.03475 53.13274) (xy 139.22525 53.13274) (xy 139.404031 52.633817) (xy 139.13 52.578309)
				(xy 138.855969 52.633817)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/PCIE_nCLKREQ")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.907346 89.28525) (xy 98.907346 89.09475) (xy 98.408423 88.922054) (xy 98.352915 89.196085)
				(xy 98.408423 89.470116)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.20828)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 85.12 43.009309) (xy 85.12 133.949309) (xy 182.71 133.949309) (xy 182.71 43.159309)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.903431 88.394559) (xy 98.903431 88.204059) (xy 98.404508 88.025969) (xy 98.349 88.3) (xy 98.404508 88.574031)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/SDA0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.53525 97.358035) (xy 145.34475 97.358035) (xy 145.176467 97.718885) (xy 145.38766 97.861)
				(xy 145.636779 97.810447)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.272428 100.80525) (xy 145.272428 100.61475) (xy 144.818862 100.460881) (xy 144.768309 100.71)
				(xy 144.818862 100.959119)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/PCIe_RX_N")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.599525 85.288219) (xy 103.599525 85.483799) (xy 103.962628 85.202706) (xy 103.822513 84.991513)
				(xy 103.572394 85.041066)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/SDA0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.558983 56.403687) (xy 140.693687 56.268983) (xy 140.475182 55.781905) (xy 140.242162 55.936424)
				(xy 140.087643 56.169444)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.756655 110.14126) (xy 155.621951 110.275964) (xy 155.988885 110.570502) (xy 156.130707 110.360016)
				(xy 156.080447 110.11019)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/PCIe_RX_P")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.746301 85.831781) (xy 98.746301 85.636201) (xy 98.246649 85.641081) (xy 98.295202 85.8902)
				(xy 98.437317 86.101393)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/SCL0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.92525 96.796881) (xy 144.73475 96.796881) (xy 144.580881 97.250447) (xy 144.83 97.301) (xy 145.079119 97.250447)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/PCIe_CLK_P")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.339555 67.086089) (xy 127.477851 67.224385) (xy 127.827706 66.867628) (xy 127.61722 66.725806)
				(xy 127.367394 66.67696)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/CAM_GPIO0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.793111 97.580902) (xy 149.658407 97.446198) (xy 149.228885 97.658116) (xy 149.369293 97.870016)
				(xy 149.581193 98.010424)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/DPHY0_D3_N")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.324887 66.602379) (xy 137.172487 66.602379) (xy 136.87532 66.905398) (xy 137.086513 67.047513)
				(xy 137.335632 66.99696)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/PCIe_CLK_P")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.780099 83.913799) (xy 98.780099 83.718219) (xy 98.471115 83.448607) (xy 98.329 83.6598) (xy 98.280447 83.908919)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/PCIe_TX_N")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 101.499372 86.770413) (xy 101.637668 86.908709) (xy 101.960915 86.631193) (xy 101.820507 86.419293)
				(xy 101.570681 86.370447)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/PCIe_TX_P")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.084835 86.731116) (xy 102.223131 86.869412) (xy 102.621315 86.631193) (xy 102.480907 86.419293)
				(xy 102.231081 86.370447)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.191881 100.96475) (xy 139.191881 101.15525) (xy 139.645447 101.314119) (xy 139.696 101.065)
				(xy 139.645447 100.815881)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/PCIE_nCLKREQ")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.563983 66.037996) (xy 128.698687 65.903292) (xy 128.472313 65.424083) (xy 128.239293 65.578602)
				(xy 128.084774 65.811622)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/PCIe_CLK_N")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.585615 67.332149) (xy 127.723911 67.470445) (xy 128.13304 67.442606) (xy 128.084194 67.19278)
				(xy 127.942372 66.982294)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/PCIE_PWR_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.491313 68.953292) (xy 127.626017 69.087996) (xy 128.105226 68.861622) (xy 127.950707 68.628602)
				(xy 127.717687 68.474083)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/+3.3v")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.47525 104.536569) (xy 136.28475 104.536569) (xy 136.105969 105.035492) (xy 136.38 105.091)
				(xy 136.654031 105.035492)
			)
		)
	)
	(embedded_fonts no)
)
