(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_575555ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_02000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 5)
			(mirror no)
			(drillshape 2)
			(scaleselection 1)
			(outputdirectory "Artwork, KiCad Export/")
		)
	)
	(net 0 "")
	(net 1 "/BATT+")
	(net 2 "GND")
	(net 3 "/LED+")
	(net 4 "unconnected-(SW1-A-Pad1)")
	(footprint "MountingHole:MountingHole_2mm"
		(layer "F.Cu")
		(at 155.4 67.4)
		(descr "Mounting Hole 2mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "REF**"
			(at 0 -2.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2mm"
			(at 0 2.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2mm"
		(layer "F.Cu")
		(at 145.7 67.4)
		(descr "Mounting Hole 2mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "REF**"
			(at 0 -2.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2mm"
			(at 0 2.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 150.6 54.3)
		(descr "Mounting Hole 3mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "REF**"
			(at 0 -3.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3mm"
			(at 0 3.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "ClaireCad:LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm"
		(layer "B.Cu")
		(at 167 70)
		(descr "LED, diameter 5.0mm, horizontal offset 3.81mm, z-position of LED center 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -5.77 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 6.586037 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Guillotine There U Glow Badge.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 1.27 -3.81 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.27 -3.81 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/LED+")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm.step"
			(offset
				(xyz 1.25 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "oshpark:OSH_small"
		(layer "B.Cu")
		(at 169 141.5 180)
		(descr "Imported from OSHPARK.svg")
		(tags "svg2mod")
		(property "Reference" "OSH_small"
			(at 0 5.49976 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -5.49976 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(embedded_fonts no)
	)
	(footprint "ClaireCad:LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm"
		(layer "B.Cu")
		(at 150.5 63.2)
		(descr "LED, diameter 5.0mm, horizontal offset 3.81mm, z-position of LED center 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -5.77 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 -0.913963 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Guillotine There U Glow Badge.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 1.27 -3.81 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.27 -3.81 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/LED+")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm.step"
			(offset
				(xyz 1.25 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "JumperlessFootprints:CR2032_Holder_Clip_Through_Hole-BS-03-A1AJ001"
		(layer "B.Cu")
		(at 150.603729 134.15)
		(property "Reference" "BT1"
			(at 0 0.5 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Battery_Cell"
			(at 0 -1 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Single-cell battery"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Guillotine There U Glow Badge.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at 11 0.05 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "-"
			(at -3.5 0.05 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" thru_hole circle
			(at 13.55 0)
			(size 2.5 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/BATT+")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -6.25 0)
			(size 2.5 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/BS-3.STEP"
			(offset
				(xyz 0 0 2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "ClaireCad:Claire_SW_CK_JS202011AQN_DPDT_Angled"
		(layer "B.Cu")
		(at 133.7675 127 90)
		(descr "C&K sub miniature slide switch, JS series, DPDT, right angle, http://www.ckswitches.com/media/1422/js.pdf")
		(tags "switch DPDT")
		(property "Reference" "SW1"
			(at 0 2 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "SW_SPDT"
			(at 2.25 -6.75 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Guillotine There U Glow Badge.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -1.75 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 -0.635 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1785714286)
			(net 4 "unconnected-(SW1-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 -0.635 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/BATT+")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5 -0.635 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/LED+")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_CK_JS202011AQN_DPDT_Angled.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/MSK-12D19.step"
			(offset
				(xyz 2.25 -1.2 -1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "ClaireCad:LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm"
		(layer "B.Cu")
		(at 134.005 70)
		(descr "LED, diameter 5.0mm, horizontal offset 3.81mm, z-position of LED center 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 0 -5.77 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 6.141037 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Guillotine There U Glow Badge.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 1.27 -3.81 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -1.27 -3.81 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/LED+")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm.step"
			(offset
				(xyz 1.25 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(gr_line
		(start 124.4 140.6)
		(end 124.4 147)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145 115)
		(end 138.7 115)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.4 147)
		(end 176.6 147)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.8 135.8)
		(end 170.8 55.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.7 113.3)
		(end 138.7 115)
		(layer "Edge.Cuts")
	)
	(gr_poly
		(pts
			(xy 162.2 69.9) (xy 162.2 103.8) (xy 138.8 103.8) (xy 138.8 69.9)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.2 135.8)
		(end 124.4 140.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.2 55.2)
		(end 130.2 135.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.6 140.6)
		(end 170.8 135.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 162.3 113.3)
		(end 162.3 115)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 170.8 55.2)
		(end 173.4 51)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 156 115)
		(mid 150.5 119.93263)
		(end 145 115)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.6 51)
		(end 130.2 55.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.6 147)
		(end 176.6 140.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156 113.3)
		(end 162.3 113.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156 115)
		(end 162.3 115)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 145 113.3)
		(mid 150.499999 108.36737)
		(end 156 113.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.4 51)
		(end 127.6 51)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145 113.3)
		(end 138.7 113.3)
		(layer "Edge.Cuts")
	)
	(gr_text "BATTERY\nHOLDER"
		(at 150.776487 130.339675 0)
		(layer "B.SilkS")
	)
	(gr_text "Created by\nClaire Cassidy"
		(at 133.855477 142.348603 0)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 133.8 65 0)
		(layer "B.SilkS")
	)
	(gr_text "-"
		(at 135.7 64.9 0)
		(layer "B.SilkS")
	)
	(gr_text "SWITCH"
		(at 137.4 120.2 90)
		(layer "B.SilkS")
	)
	(gr_text "-"
		(at 168.7 65 0)
		(layer "B.SilkS")
	)
	(gr_text "LED"
		(at 136 72.8 0)
		(layer "B.SilkS")
	)
	(gr_text "LED"
		(at 169 72.8 0)
		(layer "B.SilkS")
	)
	(gr_text "REPLACE WITH\nCR2032\nCOIN CELL\nBATTERY"
		(at 169.7 126.9 0)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 166.8 65.1 0)
		(layer "B.SilkS")
	)
	(gr_text "www.clairecassidy.info"
		(at 134.75 145.5 0)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 150.3 58.3 0)
		(layer "B.SilkS")
	)
	(gr_text "LED"
		(at 152.5 66.053562 0)
		(layer "B.SilkS")
	)
	(gr_text "-"
		(at 152.2 58.2 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
