(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.5422)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1999)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.9906)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1999)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/DSI_D0_P")
	(net 2 "/DSI_D2_N")
	(net 3 "/DSI_D3_P")
	(net 4 "VDD_3V3")
	(net 5 "/LED_A")
	(net 6 "Net-(D1-A)")
	(net 7 "/DSI_D1_P")
	(net 8 "unconnected-(J1-Pin_21-Pad21)")
	(net 9 "GND")
	(net 10 "unconnected-(J1-Pin_20-Pad20)")
	(net 11 "/DSI_CK_P")
	(net 12 "DSI_3V3")
	(net 13 "/DSI_D2_P")
	(net 14 "/DSI_CK_N")
	(net 15 "/DSI_D3_N")
	(net 16 "/DSI_D0_N")
	(net 17 "/DSI_D1_N")
	(net 18 "/GPIO_TFT_RESET")
	(net 19 "/I2C2_SCL_3V3")
	(net 20 "/I2C2_SDA_3V3")
	(net 21 "+5V")
	(net 22 "unconnected-(J1-Pin_31-Pad31)")
	(net 23 "unconnected-(J1-Pin_40-Pad40)")
	(net 24 "unconnected-(J1-Pin_22-Pad22)")
	(net 25 "unconnected-(J1-Pin_34-Pad34)")
	(net 26 "unconnected-(J1-Pin_26-Pad26)")
	(net 27 "unconnected-(J1-Pin_23-Pad23)")
	(net 28 "unconnected-(J1-Pin_25-Pad25)")
	(net 29 "/TOUCH_RST")
	(net 30 "/TOUCH_VDD")
	(net 31 "/TOUCH_GND")
	(net 32 "/TOUCH_INT")
	(net 33 "/LED_K")
	(net 34 "Net-(U2-EN)")
	(net 35 "/LED_PWM")
	(net 36 "unconnected-(J4-Pin_18-Pad18)")
	(net 37 "unconnected-(J4-Pin_17-Pad17)")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x12_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 63.2 50.04 180)
		(descr "Through hole straight pin header, 1x12, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x12 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x12_Socket"
			(at 0 30.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 13.97 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/GPIO_TFT_RESET")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/LED_PWM")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/I2C2_SCL_3V3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/I2C2_SDA_3V3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/TOUCH_VDD")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/TOUCH_RST")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/TOUCH_INT")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/TOUCH_GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x12_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 39.15 42.2375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -2.2625 -0.05 180)
			(layer "B.SilkS")
		)
		(property "Value" "10kΩ"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 4 "VDD_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 18 "/GPIO_TFT_RESET")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_FFC-FPC:TE_4-1734839-0_1x40-1MP_P0.5mm_Horizontal"
		(layer "B.Cu")
		(at 29.55 46.45 90)
		(descr "TE FPC connector, 40 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0")
		(tags "te fpc 1734839")
		(property "Reference" "J1"
			(at -12.35 2.45 180)
			(layer "B.SilkS")
		)
		(property "Value" "Output to ER-TFT0784-2"
			(at 0 -4.95 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x40, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 -3.25 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.55 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -9.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -9.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/DSI_D0_P")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -8.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "/DSI_D0_N")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -8.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -7.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "/DSI_D1_P")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -7.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "/DSI_D1_N")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -6.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -6.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/DSI_CK_P")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -5.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "/DSI_CK_N")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -5.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -4.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "/DSI_D2_P")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -4.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "/DSI_D2_N")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -3.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -3.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "/DSI_D3_P")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at -2.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "/DSI_D3_N")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -2.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -1.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -1.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "DSI_3V3")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -0.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "DSI_3V3")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -0.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "unconnected-(J1-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
		)
		(pad "21" smd rect
			(at 0.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "unconnected-(J1-Pin_21-Pad21)")
			(pinfunction "Pin_21")
			(pintype "passive+no_connect")
		)
		(pad "22" smd rect
			(at 0.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "unconnected-(J1-Pin_22-Pad22)")
			(pinfunction "Pin_22")
			(pintype "passive+no_connect")
		)
		(pad "23" smd rect
			(at 1.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "unconnected-(J1-Pin_23-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive+no_connect")
		)
		(pad "24" smd rect
			(at 1.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "/GPIO_TFT_RESET")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 2.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "unconnected-(J1-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
		)
		(pad "26" smd rect
			(at 2.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "unconnected-(J1-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
		)
		(pad "27" smd rect
			(at 3.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 3.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "/LED_K")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at 4.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "/LED_K")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at 4.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 5.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "unconnected-(J1-Pin_31-Pad31)")
			(pinfunction "Pin_31")
			(pintype "passive+no_connect")
		)
		(pad "32" smd rect
			(at 5.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 6.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at 6.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "unconnected-(J1-Pin_34-Pad34)")
			(pinfunction "Pin_34")
			(pintype "passive+no_connect")
		)
		(pad "35" smd rect
			(at 7.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/LED_A")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at 7.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/LED_A")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at 8.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at 8.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "VDD_3V3")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at 9.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "VDD_3V3")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at 9.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "unconnected-(J1-Pin_40-Pad40)")
			(pinfunction "Pin_40")
			(pintype "passive+no_connect")
		)
		(pad "MP" smd rect
			(at -11.42 -0.35 90)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "MP" smd rect
			(at 11.42 -0.35 90)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/TE_4-1734839-0_1x40-1MP_P0.5mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "project:SRP7028CC"
		(layer "B.Cu")
		(at 45.525 29.4 180)
		(property "Reference" "L1"
			(at 0.025 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "15 uH"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at -0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at -0.25 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SRP7028CC-150M"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -3.125 0 90)
			(size 3.5 3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "+5V")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 3.125 0 90)
			(size 3.5 3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "Net-(D1-A)")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 35.15 32.6)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.65 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/25V/X7R"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL32B226KAJNNNE"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/LED_A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "B.Cu")
		(at 36.8 29.4)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D1"
			(at 0 -2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "B240A-13-F"
			(at 0 -2.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "B240A-13-F"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net 5 "/LED_A")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0)
			(size 2.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net 6 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 48.5 41.8625 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -2.3375 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "10uf"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ZRB18AC81A106KE01L"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 34.7 43.75 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uf"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ZRB18AC81A106KE01L"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/GPIO_TFT_RESET")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 54 37.0125 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.3125 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" " ERJ-U6QFR56V"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 35 "/LED_PWM")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 34 "Net-(U2-EN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-89-5"
		(layer "B.Cu")
		(at 45.55 35.5 180)
		(descr "SOT-89-5, http://www.e-devices.ricoh.co.jp/en/products/product_power/pkg/sot-89-5.pdf")
		(tags "SOT-89-5")
		(property "Reference" "U2"
			(at 0 -3.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "PT4110"
			(at 0 -3.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.buydisplay.com/download/ic/PT4110.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "LED driver"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.85 1.5 180)
			(size 1.5 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd custom
			(at 0 0 180)
			(size 0.8 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.9 0.5) (xy 2.6 0.5) (xy 2.6 -0.5) (xy 0.9 -0.5) (xy 0.4 -1) (xy -0.4 -1) (xy -0.9 -0.5)
						(xy -2.6 -0.5) (xy -2.6 0.5) (xy -0.9 0.5) (xy -0.4 1) (xy 0.4 1)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd roundrect
			(at -1.85 -1.5 180)
			(size 1.5 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U2-EN)")
			(pinfunction "EN")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 1.85 -1.5 180)
			(size 1.5 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/LED_K")
			(pinfunction "FB")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 1.85 1.5 180)
			(size 1.5 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D1-A)")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 54 33.05 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.25 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "22uF/6V"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL32B226KAJNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 35.15 35)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.65 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/25V/X7R"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL32B226KAJNNNE"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/LED_A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "B.Cu")
		(at 45.05 42.05 90)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at -2.75 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "XC6206P332MR-G"
			(at 0 -2.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc6206/XC6206.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "XC6206P332MR-G"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?3*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VDD_3V3")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "+5V")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 51.7 33.05 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at -2.25 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf/6V"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL32B226KAJNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_FFC-FPC:TE_2-1734839-2_1x22-1MP_P0.5mm_Horizontal"
		(layer "B.Cu")
		(at 54.55 50.95 90)
		(descr "TE FPC connector, 22 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0")
		(tags "te fpc 1734839")
		(property "Reference" "J4"
			(at -7.65 2.65 180)
			(layer "B.SilkS")
		)
		(property "Value" "Breakout DSI Input"
			(at 0 -4.95 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x22, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "FPV-WZB21-22-LF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 -3.25 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.55 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -5.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -4.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "/DSI_D0_N")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -4.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/DSI_D0_P")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -3.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -3.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "/DSI_D1_N")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "/DSI_D1_P")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -2.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -1.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "/DSI_CK_N")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/DSI_CK_P")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -0.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -0.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "/DSI_D2_N")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 0.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "/DSI_D2_P")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 1.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "/DSI_D3_N")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 1.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "/DSI_D3_P")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 2.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "unconnected-(J4-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
		)
		(pad "18" smd rect
			(at 3.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "unconnected-(J4-Pin_18-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
		)
		(pad "19" smd rect
			(at 3.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "GND")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 4.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "/I2C2_SCL_3V3")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 4.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "/I2C2_SDA_3V3")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 5.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "DSI_3V3")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -6.92 -0.35 90)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "MP" smd rect
			(at 6.92 -0.35 90)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/TE_2-1734839-2_1x22-1MP_P0.5mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 35.15 37.4)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.65 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uf/25V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL32B226KAJNNNE"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/LED_A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_FFC-FPC:TE_0-1734839-6_1x06-1MP_P0.5mm_Horizontal"
		(layer "B.Cu")
		(at 29.55 26.45 90)
		(descr "TE FPC connector, 06 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0")
		(tags "te fpc 1734839")
		(property "Reference" "J5"
			(at -3.75 2.25 180)
			(layer "B.SilkS")
		)
		(property "Value" "Touch Input"
			(at 0 -4.95 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 -3.25 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.55 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "/I2C2_SCL_3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "/I2C2_SDA_3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "/TOUCH_VDD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "/TOUCH_RST")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.75 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/TOUCH_INT")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.25 1.35 90)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "/TOUCH_GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -2.92 -0.35 90)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "MP" smd rect
			(at 2.92 -0.35 90)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/TE_0-1734839-6_1x06-1MP_P0.5mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 40.8 36.0875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.3125 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.5Ω/≥1%/0.25 W"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" " ERJ-U6QFR56V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 33 "/LED_K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 41.75 42.2375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -2.3625 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uf"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "ZRB18AC81A106KE01L"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VDD_3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 51.25 37.0125 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.3375 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" " ERJ-U6QFR56V"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "er-tft0784-2-breakout.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 34 "Net-(U2-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 9 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 25 20.25)
		(end 25 60.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 25 60.25)
		(end 65 60.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 65 60.25)
		(end 65 20.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 65 20.25)
		(end 25 20.25)
		(layer "Edge.Cuts")
	)
	(gr_text "RST"
		(at 62.1 29.8 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 62.2 50.04 0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 31.65 57.25 0)
		(layer "B.SilkS")
	)
	(gr_text "40"
		(at 31.45 35.8 0)
		(layer "B.SilkS")
	)
	(gr_text "INT"
		(at 62.1 27.32 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 62.2 22.1 0)
		(layer "B.SilkS")
	)
	(gr_text "D_RST"
		(at 62.2 47.5 0)
		(layer "B.SilkS")
	)
	(gr_text "TOUCH"
		(at 59.025 31.025 90)
		(layer "B.SilkS" knockout)
	)
	(gr_text "GND"
		(at 62.2 39.88 0)
		(layer "B.SilkS")
	)
	(gr_text "D_PWM"
		(at 62.2 44.96 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 62.1 24.72 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "1"
		(at 56.65 57.15 0)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 62.2 42.42 0)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 62.1 37.42 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "VDD"
		(at 62.1 32.34 0)
		(layer "B.SilkS" knockout)
	)
	(gr_text "sndsgd/er-tft0784-2-breakout\nrev1"
		(at 45 24 0)
		(layer "B.SilkS")
	)
	(gr_text "SDA"
		(at 62.1 34.88 0)
		(layer "B.SilkS" knockout)
	)
	(zone
		(net 9)
		(net_name "GND")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 22.5 17.5) (xy 67.5 17.5) (xy 67.5 63) (xy 22.5 63)
			)
		)
	)
	(embedded_fonts no)
)
