(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (gr_line (start -38.1 81.2) (end -35.907 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start -24.093 81.2) (end -24.093 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start 4.482 81.2) (end 6.675 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start 6.675 84.2) (end 4.482 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start -5.935 79.8) (end -5.935 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 75.4) (end 6.675 75.4)
    (layer "Edge.Cuts"))
  (gr_line (start -25.49 81.2) (end -25.49 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start 6.675 88.6) (end 4.482 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start 4.482 76.8) (end 6.675 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 85.6) (end -9.525 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 76.8) (end -7.332 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -5.935 84.2) (end -5.935 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start -34.51 88.6) (end -25.49 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -35.907 84.2) (end -38.1 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start 3.085 76.8) (end 3.085 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 90) (end -9.525 90)
    (layer "Edge.Cuts"))
  (gr_line (start 3.085 81.2) (end -5.935 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start -7.332 79.8) (end -7.332 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -25.49 76.8) (end -25.49 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 85.6) (end -35.907 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 85.6) (end -7.332 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -5.935 88.6) (end 3.085 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -34.51 79.8) (end -34.51 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -35.907 88.6) (end -38.1 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start 6.675 79.8) (end 6.675 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start 6.675 79.8) (end 4.482 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -35.907 88.6) (end -35.907 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -24.093 85.6) (end -24.093 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -34.51 88.6) (end -34.51 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -25.49 81.2) (end -34.51 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start 4.482 76.8) (end 4.482 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -5.935 84.2) (end 3.085 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start 4.482 85.6) (end 6.675 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -5.935 88.6) (end -5.935 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -7.332 84.2) (end -7.332 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start 4.482 85.6) (end 4.482 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -7.332 88.6) (end -7.332 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 75.4) (end -9.525 75.4)
    (layer "Edge.Cuts"))
  (gr_line (start -34.51 79.8) (end -25.49 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start 3.085 81.2) (end 3.085 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start -25.49 76.8) (end -34.51 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -7.332 84.2) (end -9.525 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 76.8) (end -35.907 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -21.9 84.2) (end -21.9 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -24.093 85.6) (end -21.9 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -21.9 79.8) (end -21.9 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start 3.085 85.6) (end -5.935 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -25.49 85.6) (end -25.49 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 88.6) (end -24.093 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -35.907 79.8) (end -35.907 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -35.907 79.8) (end -38.1 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start 4.482 81.2) (end 4.482 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start -24.093 81.2) (end -21.9 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start 3.085 76.8) (end -5.935 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -24.093 76.8) (end -24.093 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start 6.675 75.4) (end 6.675 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start 6.675 84.2) (end 6.675 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -35.907 84.2) (end -35.907 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start 6.675 88.6) (end 6.675 90)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 90) (end -38.1 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 81.2) (end -38.1 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 81.2) (end -9.525 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -24.093 76.8) (end -9.525 76.8)
    (layer "Edge.Cuts"))
  (gr_line (start -21.9 84.2) (end -24.093 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 85.6) (end -38.1 84.2)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 81.2) (end -7.332 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start -25.49 85.6) (end -34.51 85.6)
    (layer "Edge.Cuts"))
  (gr_line (start -34.51 84.2) (end -34.51 81.2)
    (layer "Edge.Cuts"))
  (gr_line (start -7.332 88.6) (end -9.525 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start 3.085 85.6) (end 3.085 88.6)
    (layer "Edge.Cuts"))
  (gr_line (start -7.332 79.8) (end -9.525 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -21.9 79.8) (end -24.093 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -9.525 90) (end 6.675 90)
    (layer "Edge.Cuts"))
  (gr_line (start -38.1 76.8) (end -38.1 75.4)
    (layer "Edge.Cuts"))
  (gr_line (start -5.935 79.8) (end 3.085 79.8)
    (layer "Edge.Cuts"))
  (gr_line (start -34.51 84.2) (end -25.49 84.2)
    (layer "Edge.Cuts"))
  (gr_text "Layer 2 - Track Guides (9.02 Gauge, 28.575 C-C)" (at 25 0) (layer "User.2"))
  (gr_text "Layer 3 - Tracks" (at 25 10) (layer "User.3"))
  (gr_text "Layer 4 - Ties (1.6mm height, 3mm spacing)" (at 25 20) (layer "User.4"))
  (gr_text "Single Track PCB layout" (at 100 45) (layer "User.5"))
  (gr_text "Single Track PCB layout" (at 35 45) (layer "User.5"))
  (gr_text "Layer 5 - Zone definition" (at 25 30) (layer "User.5"))
  (gr_text "Double Track PCB layout (28.575 C-C)\n" (at 50 95) (layer "User.5"))
  (gr_text "Single Track PCB layout" (at -30 45) (layer "User.5"))
  (gr_text "Double Track PCB layout (28.575 C-C)\n" (at -15 95) (layer "User.5"))
  (gr_text "Double Track PCB layout (28.575 C-C)\n" (at 115 95) (layer "User.5"))
)
