(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(A1-3V3-Pad36)")
	(net 2 "unconnected-(A1-GPIO3-Pad5)")
	(net 3 "unconnected-(A1-GPIO17-Pad22)")
	(net 4 "unconnected-(A1-GPIO5-Pad7)")
	(net 5 "unconnected-(A1-GPIO12-Pad16)")
	(net 6 "unconnected-(A1-GPIO22-Pad29)")
	(net 7 "unconnected-(A1-GPIO20-Pad26)")
	(net 8 "unconnected-(A1-GPIO19-Pad25)")
	(net 9 "unconnected-(A1-GPIO28_ADC2-Pad34)")
	(net 10 "unconnected-(A1-GPIO10-Pad14)")
	(net 11 "unconnected-(A1-ADC_VREF-Pad35)")
	(net 12 "unconnected-(A1-VBUS-Pad40)")
	(net 13 "unconnected-(A1-GPIO6-Pad9)")
	(net 14 "unconnected-(A1-GPIO4-Pad6)")
	(net 15 "unconnected-(A1-GPIO2-Pad4)")
	(net 16 "unconnected-(A1-GPIO18-Pad24)")
	(net 17 "unconnected-(A1-GPIO9-Pad12)")
	(net 18 "unconnected-(A1-GPIO27_ADC1-Pad32)")
	(net 19 "unconnected-(A1-GPIO13-Pad17)")
	(net 20 "unconnected-(A1-GPIO7-Pad10)")
	(net 21 "unconnected-(A1-3V3_EN-Pad37)")
	(net 22 "unconnected-(A1-RUN-Pad30)")
	(net 23 "unconnected-(A1-GPIO0-Pad1)")
	(net 24 "unconnected-(A1-GPIO11-Pad15)")
	(net 25 "unconnected-(A1-GPIO21-Pad27)")
	(net 26 "unconnected-(A1-GPIO26_ADC0-Pad31)")
	(net 27 "unconnected-(A1-GPIO1-Pad2)")
	(net 28 "unconnected-(A1-AGND-Pad33)")
	(net 29 "unconnected-(A1-GPIO8-Pad11)")
	(net 30 "unconnected-(A1-GPIO14-Pad19)")
	(net 31 "unconnected-(U1-B5-Pad13)")
	(net 32 "unconnected-(U1-A7-Pad9)")
	(net 33 "unconnected-(U1-B6-Pad12)")
	(net 34 "unconnected-(U1-B7-Pad11)")
	(net 35 "unconnected-(U1-B3-Pad15)")
	(net 36 "unconnected-(U1-A3-Pad5)")
	(net 37 "unconnected-(U1-B2-Pad16)")
	(net 38 "unconnected-(U1-A5-Pad7)")
	(net 39 "unconnected-(U1-CE-Pad19)")
	(net 40 "unconnected-(U1-A6-Pad8)")
	(net 41 "unconnected-(U1-A4-Pad6)")
	(net 42 "unconnected-(U1-B4-Pad14)")
	(net 43 "unconnected-(U1-A2-Pad4)")
	(net 44 "unconnected-(Power_Led_Buzzer_Header1-Pin_6-Pad6)")
	(net 45 "GND")
	(net 46 "/5v_IN")
	(net 47 "/BUZZ_IN")
	(net 48 "/LED_DATA_IN")
	(net 49 "unconnected-(DROK_5V_Module1-Pin_5-Pad5)")
	(net 50 "/BUZZ_OUT")
	(net 51 "/LED_DATA_OUT")
	(net 52 "/BATT_IN_12v")
	(net 53 "Net-(U1-B0)")
	(net 54 "/Net-(A1-VSYS)")
	(net 55 "/Net-(A2-VSYS)")
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 191.5 85.4)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_PH_S5B-PH-K_1x05_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 220.8 78.6 90)
		(descr "JST PH series connector, S5B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "REF**"
			(at 4 -2.55 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JST_PH_S5B-PH-K_1x05_P2.00mm_Horizontal"
			(at 4 7.45 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4 2.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 50 "/BUZZ_OUT")
		)
		(pad "2" thru_hole oval
			(at 2 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
		)
		(pad "3" thru_hole oval
			(at 4 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/LED_DATA_OUT")
		)
		(pad "4" thru_hole oval
			(at 6 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
		)
		(pad "5" thru_hole oval
			(at 8 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/BATT_IN_12v")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S5B-PH-K_1x05_P2.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S8B-PH-K_1x08_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 145.5 75 -90)
		(descr "JST PH series connector, S8B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "Power_Led_Buzzer_Header1"
			(at 7 -2.55 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x08"
			(at 7 7.45 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7 2.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 52 "/BATT_IN_12v")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/BATT_IN_12v")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 6 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 8 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/LED_DATA_OUT")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 10 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(Power_Led_Buzzer_Header1-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 12 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/BUZZ_OUT")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 14 0 270)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S8B-PH-K_1x08_P2.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 142 100.4)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 224.2 50.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 224.2 100.4)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Module:RaspberryPi_Pico_Common_THT"
		(layer "F.Cu")
		(at 197.8 51)
		(descr "Raspberry Pi Pico common (Pico & Pico W) through-hole footprint, supports Raspberry Pi Pico 2, default socketed model has height of 8.51mm, https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
		(tags "module usb pcb antenna")
		(property "Reference" "A1"
			(at 20.6375 48.895 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RaspberryPi_Pico_2W"
			(at 9.28 24.3 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 8.89 24.13 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Versatile and inexpensive microcontroller module (with full pinout for test point and debug connections) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash; also supports Raspberry Pi Pico 2"
			(at 8.89 24.13 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "Possible Antenna"
			(at 8.89 43.815 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep Out"
			(at 8.89 45.72 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "USB Cable"
			(at 8.89 -13.335 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 8.89 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole custom
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole custom
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole custom
			(at 0 30.48)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 0 35.56)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at 0 38.1)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at 0 40.64)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole custom
			(at 0 43.18)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 0.6) (xy 0.8 -0.6) (xy 0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy 0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "19" thru_hole circle
			(at 0 45.72)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at 0 48.26)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 17.78 48.26)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 17.78 45.72)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole custom
			(at 17.78 43.18)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "24" thru_hole circle
			(at 17.78 40.64)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 17.78 38.1)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 17.78 35.56)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 17.78 33.02)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole custom
			(at 17.78 30.48)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "29" thru_hole circle
			(at 17.78 27.94)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at 17.78 25.4)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "RUN")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 17.78 22.86)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 17.78 20.32)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole custom
			(at 17.78 17.78)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "AGND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "34" thru_hole circle
			(at 17.78 15.24)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole circle
			(at 17.78 12.7)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "ADC_VREF")
			(pintype "power_in")
		)
		(pad "36" thru_hole circle
			(at 17.78 10.16)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "37" thru_hole circle
			(at 17.78 7.62)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "3V3_EN")
			(pintype "passive")
		)
		(pad "38" thru_hole custom
			(at 17.78 5.08)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 0 -0.8) (xy 0 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "39" thru_hole circle
			(at 17.78 2.54)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at 17.78 0)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "B.Cu" "F.Paste" "B.Paste")
			(name "Antenna Copper Keep Out")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 204.29 100.119895) (xy 199.59 96.469895) (xy 199.59 92.13) (xy 213.79 92.13) (xy 213.79 96.469895)
					(xy 209.09 100.119895) (xy 209.09 101.13) (xy 204.29 101.13)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.CrtYd")
			(name "USB Cable")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 200.94 47.43) (xy 202.75 47.43) (xy 202.75 47.83) (xy 210.63 47.83) (xy 210.63 47.43) (xy 212.44 47.43)
					(xy 212.44 27.93) (xy 200.94 27.93)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_PinSockets_H8.50mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H.step"
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 191.5 65.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm"
		(layer "F.Cu")
		(at 162.12 97 180)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 10.655954 -2.33 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "SN74HCT245N"
			(at 3.81 25.19 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC245"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?20*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 46 "/5v_IN")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/LED_DATA_IN")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/BUZZ_IN")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(U1-A2-Pad4)")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(U1-A3-Pad5)")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(U1-A4-Pad6)")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" thru_hole circle
			(at 0 15.24 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(U1-A5-Pad7)")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" thru_hole circle
			(at 0 17.78 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(U1-A6-Pad8)")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" thru_hole circle
			(at 0 20.32 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(U1-A7-Pad9)")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" thru_hole circle
			(at 0 22.86 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole circle
			(at 7.62 22.86 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(U1-B7-Pad11)")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" thru_hole circle
			(at 7.62 20.32 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(U1-B6-Pad12)")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" thru_hole circle
			(at 7.62 17.78 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(U1-B5-Pad13)")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" thru_hole circle
			(at 7.62 15.24 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U1-B4-Pad14)")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" thru_hole circle
			(at 7.62 12.7 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(U1-B3-Pad15)")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole circle
			(at 7.62 10.16 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(U1-B2-Pad16)")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" thru_hole circle
			(at 7.62 7.62 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/BUZZ_OUT")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" thru_hole circle
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(U1-B0)")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" thru_hole circle
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(U1-CE-Pad19)")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" thru_hole circle
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/5v_IN")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 142 50.6)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 140.5 56.96)
		(descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x05 2.54mm single row")
		(property "Reference" "DROK_5V_Module1"
			(at 3 5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05"
			(at 0 12.54 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/5v_IN")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/BATT_IN_12v")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(DROK_5V_Module1-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:RaspberryPi_Pico_Common_THT"
		(layer "B.Cu")
		(at 185 51 180)
		(descr "Raspberry Pi Pico common (Pico & Pico W) through-hole footprint, supports Raspberry Pi Pico 2, default socketed model has height of 8.51mm, https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
		(tags "module usb pcb antenna")
		(property "Reference" "A1"
			(at 20.6375 -48.895 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "RaspberryPi_Pico_2W"
			(at 9.28 -24.3 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 8.89 -24.13 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Versatile and inexpensive microcontroller module (with full pinout for test point and debug connections) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash; also supports Raspberry Pi Pico 2"
			(at 8.89 -24.13 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RaspberryPi?Pico?SMD")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr through_hole)
		(fp_text user "USB Cable"
			(at 8.89 13.335 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Possible Antenna"
			(at 8.89 -43.815 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep Out"
			(at 8.89 -45.72 0)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 8.89 -24.13 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 23 "unconnected-(A1-GPIO0-Pad1)")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(A1-GPIO1-Pad2)")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole custom
			(at 0 -5.08 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 -0.6) (xy 0.8 0.6) (xy 0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy 0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(A1-GPIO2-Pad4)")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 0 -10.16 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(A1-GPIO3-Pad5)")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 0 -12.7 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(A1-GPIO4-Pad6)")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole circle
			(at 0 -15.24 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(A1-GPIO5-Pad7)")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole custom
			(at 0 -17.78 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 -0.6) (xy 0.8 0.6) (xy 0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy 0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" thru_hole circle
			(at 0 -20.32 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(A1-GPIO6-Pad9)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 0 -22.86 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(A1-GPIO7-Pad10)")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 0 -25.4 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(A1-GPIO8-Pad11)")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at 0 -27.94 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(A1-GPIO9-Pad12)")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole custom
			(at 0 -30.48 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 -0.6) (xy 0.8 0.6) (xy 0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy 0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "14" thru_hole circle
			(at 0 -33.02 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(A1-GPIO10-Pad14)")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 0 -35.56 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-GPIO11-Pad15)")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole circle
			(at 0 -38.1 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(A1-GPIO12-Pad16)")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at 0 -40.64 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(A1-GPIO13-Pad17)")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole custom
			(at 0 -43.18 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 -0.6) (xy 0.8 0.6) (xy 0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy 0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 -0.6)
					(end 0.8 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0.6 0.6)
					(end 0.8 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "19" thru_hole circle
			(at 0 -45.72 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(A1-GPIO14-Pad19)")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole circle
			(at 0 -48.26 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/BUZZ_IN")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 17.78 -48.26 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/LED_DATA_IN")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 17.78 -45.72 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(A1-GPIO17-Pad22)")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole custom
			(at 17.78 -43.18 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 -0.6) (xy -0.8 0.6) (xy -0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy -0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "24" thru_hole circle
			(at 17.78 -40.64 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-GPIO18-Pad24)")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 17.78 -38.1 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(A1-GPIO19-Pad25)")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 17.78 -35.56 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(A1-GPIO20-Pad26)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 17.78 -33.02 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(A1-GPIO21-Pad27)")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole custom
			(at 17.78 -30.48 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 -0.6) (xy -0.8 0.6) (xy -0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy -0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "29" thru_hole circle
			(at 17.78 -27.94 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(A1-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at 17.78 -25.4 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(A1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 17.78 -22.86 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(A1-GPIO26_ADC0-Pad31)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 17.78 -20.32 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-GPIO27_ADC1-Pad32)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole custom
			(at 17.78 -17.78 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(A1-AGND-Pad33)")
			(pinfunction "AGND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 -0.6) (xy -0.8 0.6) (xy -0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy -0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "34" thru_hole circle
			(at 17.78 -15.24 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(A1-GPIO28_ADC2-Pad34)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole circle
			(at 17.78 -12.7 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(A1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "power_in")
		)
		(pad "36" thru_hole circle
			(at 17.78 -10.16 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(A1-3V3-Pad36)")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "37" thru_hole circle
			(at 17.78 -7.62 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(A1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "passive")
		)
		(pad "38" thru_hole custom
			(at 17.78 -5.08 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 -0.6) (xy -0.8 0.6) (xy -0.6 0.8) (xy 0 0.8) (xy 0 -0.8) (xy -0.6 -0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "39" thru_hole circle
			(at 17.78 -2.54 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/Net-(A1-VSYS)")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "40" thru_hole circle
			(at 17.78 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(A1-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "B.Cu" "F.Paste" "B.Paste")
			(name "Antenna Copper Keep Out")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 178.51 100.119895) (xy 183.21 96.469895) (xy 183.21 92.13) (xy 169.01 92.13) (xy 169.01 96.469895)
					(xy 173.71 100.119895) (xy 173.71 101.13) (xy 178.51 101.13)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.CrtYd")
			(name "USB Cable")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 181.86 47.43) (xy 180.05 47.43) (xy 180.05 47.83) (xy 172.17 47.83) (xy 172.17 47.43) (xy 170.36 47.43)
					(xy 170.36 27.93) (xy 181.86 27.93)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_PinSockets_H8.50mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_H.step"
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_W_AddedHeaders_H2.54mm.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico_WH.step"
			(hide yes)
			(offset
				(xyz 8.89 -24.13 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "B.Cu")
		(at 221.1 58.8 90)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D1"
			(at 0 2.5 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "SS34"
			(at -0.2 2.5 90)
			(layer "B.SilkS")
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "40V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0 90)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net 46 "/5v_IN")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0 90)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net 55 "/Net-(A2-VSYS)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 150.3 91.6 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.43 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Drok 5v Module"
			(at 2.675 29 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Net-(U1-B0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/LED_DATA_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 152.5 97.9)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 1.43 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small_US"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/5v_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 152.5 96.3)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.43 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small_US"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/5v_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA_Handsoldering"
		(layer "B.Cu")
		(at 153.5 51.5)
		(descr "Diode SMA (DO-214AC) Handsoldering")
		(tags "Diode SMA (DO-214AC) Handsoldering")
		(property "Reference" "D1"
			(at 0 2.5 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "SS34"
			(at -0.1 2.6 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" "http://www.vishay.com/docs/88525/1n5817.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "40V 1A Schottky Barrier Rectifier Diode, DO-41"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?41*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5 0)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net 46 "/5v_IN")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5 0)
			(size 3.5 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1388888889)
			(net 54 "/Net-(A1-VSYS)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "B.Cu")
		(at 150.5 77 90)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, diameter=5mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm diameter 5mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at 1 3.75 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small_US"
			(at 1 -4.25 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "rabbit_v3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 270)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 45 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/BATT_IN_12v")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 227.7 47)
		(end 227.7 104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.5 47)
		(end 189 47)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.5 104)
		(end 189 104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189 104)
		(end 194 104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194 47)
		(end 227.7 47)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 194 104)
		(end 227.7 104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 138.5 104)
		(end 138.5 47)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.1 47)
		(end 194.1 47)
		(layer "Edge.Cuts")
	)
	(gr_text "Bz+  Gnd  LD5v Gnd  L12v"
		(at 219.3 79.6 90)
		(layer "F.SilkS")
	)
	(gr_text "Rabbit v4.0"
		(at 202.3 86.3 0)
		(layer "F.SilkS")
	)
	(gr_text "Rabbit v4.0"
		(at 171.6 87 0)
		(layer "F.SilkS")
	)
	(gr_text "Bz+  Gnd  XX  LD5v Gnd  L12v Gnd  12v"
		(at 147.5 90.5 90)
		(layer "F.SilkS")
	)
	(gr_text "JST-PH 2.0, 8-pin"
		(at 140 85.5 90)
		(layer "F.SilkS")
	)
	(gr_text "SN74HCT245N"
		(at 159.5 93.5 90)
		(layer "F.SilkS")
	)
	(gr_text "47 µF electrolytic"
		(at 151.5 86 90)
		(layer "F.SilkS")
	)
	(gr_text "Rabbit v4.0"
		(at 180.3 87 0)
		(layer "B.SilkS")
	)
	(gr_text "4.7 µF ceramic (X5R/X7R\n"
		(at 149.5 98.5 0)
		(layer "B.SilkS")
	)
	(gr_text "Rabbit v4.0"
		(at 211 86.3 0)
		(layer "B.SilkS")
	)
	(gr_text "330 Ω resistor"
		(at 153 93 0)
		(layer "B.SilkS")
	)
	(gr_text "0.1 µF ceramic (100 nF)"
		(at 149.5 97 0)
		(layer "B.SilkS")
	)
	(zone
		(net 45)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.6 47.1) (xy 227.7 47) (xy 227.7 103.9) (xy 138.6 103.9) (xy 138.6 47)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.4 64) (xy 176 64) (xy 176 75.5) (xy 168.4 75.5)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198.991129 75.4) (xy 214.391129 75.3) (xy 214.491129 101) (xy 198.991129 101.15)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.033853 75.3) (xy 168.533853 75.4) (xy 168.433853 101.1) (xy 184.033853 101.05)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 175.995098 63.9) (xy 168.595098 63.9) (xy 168.595098 75.4) (xy 175.995098 75.4)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 214.436966 75.3) (xy 199.036966 75.4) (xy 198.936966 101.1) (xy 214.436966 101.05)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.6 75.4) (xy 183.9 75.4) (xy 184 101.1) (xy 168.6 101.15)
			)
		)
	)
	(zone
		(net 45)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.6 47) (xy 227.7 47) (xy 227.6 103.9) (xy 138.6 103.9)
			)
		)
	)
	(embedded_fonts no)
)
