(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J6-Pin_6)")
	(net 2 "Net-(J4-Pin_3)")
	(net 3 "Net-(J5-Pin_3)")
	(net 4 "Net-(J3-Pin_9)")
	(net 5 "Net-(J4-Pin_8)")
	(net 6 "Net-(J3-Pin_5)")
	(net 7 "Net-(J7-Pin_8)")
	(net 8 "Net-(J5-Pin_5)")
	(net 9 "Net-(J6-Pin_8)")
	(net 10 "Net-(J6-Pin_3)")
	(net 11 "Net-(J3-Pin_4)")
	(net 12 "Net-(J7-Pin_5)")
	(net 13 "Net-(J2-Pin_5)")
	(net 14 "Net-(J2-Pin_2)")
	(net 15 "Net-(J2-Pin_8)")
	(net 16 "Net-(J7-Pin_6)")
	(net 17 "Net-(J2-Pin_7)")
	(net 18 "Net-(J6-Pin_2)")
	(net 19 "Net-(J7-Pin_7)")
	(net 20 "Net-(J7-Pin_3)")
	(net 21 "Net-(J7-Pin_4)")
	(net 22 "Net-(J4-Pin_2)")
	(net 23 "Net-(J2-Pin_9)")
	(net 24 "Net-(J3-Pin_8)")
	(net 25 "Net-(J2-Pin_10)")
	(net 26 "Net-(J4-Pin_9)")
	(net 27 "Net-(J4-Pin_7)")
	(net 28 "Net-(J7-Pin_9)")
	(net 29 "Net-(J2-Pin_4)")
	(net 30 "Net-(J5-Pin_7)")
	(net 31 "Net-(J6-Pin_9)")
	(net 32 "Net-(J5-Pin_4)")
	(net 33 "Net-(J5-Pin_6)")
	(net 34 "Net-(J5-Pin_8)")
	(net 35 "Net-(J6-Pin_5)")
	(net 36 "Net-(J4-Pin_4)")
	(net 37 "Net-(J2-Pin_3)")
	(net 38 "Net-(J5-Pin_9)")
	(net 39 "Net-(J6-Pin_10)")
	(net 40 "Net-(J3-Pin_6)")
	(net 41 "Net-(J3-Pin_2)")
	(net 42 "Net-(J2-Pin_6)")
	(net 43 "Net-(J5-Pin_2)")
	(net 44 "Net-(J6-Pin_4)")
	(net 45 "Net-(J3-Pin_3)")
	(net 46 "Net-(J4-Pin_5)")
	(net 47 "Net-(J7-Pin_2)")
	(net 48 "Net-(J4-Pin_6)")
	(net 49 "Net-(J3-Pin_7)")
	(net 50 "Net-(J6-Pin_7)")
	(net 51 "GND")
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 130.175 76.835)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.19 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Test Header BO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J5-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J5-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J5-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J5-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J5-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 160.655 76.84)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.19 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Test Header BO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J3-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J3-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J3-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J3-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 165.735 76.84)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.19 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Test Header BO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J4-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J4-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J4-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J4-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:PinHeader_1x10_P2.54mm_Vertical - Thin"
		(layer "F.Cu")
		(at 135.255 76.84)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.19 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:PinHeader_1x10_P2.54mm_Vertical - Thin"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Test Header BO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.4224)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J6-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J6-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J6-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J6-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J6-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(J6-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J6-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J6-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J6-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:PinHeader_1x10_P2.54mm_Vertical - Thin"
		(layer "F.Cu")
		(at 155.575 76.84)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.19 0)
			(layer "F.Fab")
		)
		(property "Footprint" "t_connectors:PinHeader_1x10_P2.54mm_Vertical - Thin"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Test Header BO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.4224)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J2-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.3208)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:MOLEX_546840504"
		(layer "F.Cu")
		(at 145.415 88.265)
		(property "Reference" "J1"
			(at -0.635 -8.255 0)
			(layer "F.SilkS")
		)
		(property "Value" "Molex_0546840504"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "t_connectors:MOLEX_546840504"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Test Header BO.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 2.275 -4.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(J2-Pin_2)")
			(pinfunction "1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.275 -4.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(J6-Pin_2)")
			(pinfunction "2")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.275 -4.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "Net-(J3-Pin_2)")
			(pinfunction "3")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.275 -4.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "Net-(J5-Pin_2)")
			(pinfunction "4")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 2.275 -4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(J4-Pin_2)")
			(pinfunction "5")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.275 -4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "Net-(J7-Pin_2)")
			(pinfunction "6")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.275 -3.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "Net-(J2-Pin_3)")
			(pinfunction "7")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -2.275 -3.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "Net-(J6-Pin_3)")
			(pinfunction "8")
			(pintype "input")
		)
		(pad "9" smd rect
			(at 2.275 -3.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "Net-(J3-Pin_3)")
			(pinfunction "9")
			(pintype "input")
		)
		(pad "10" smd rect
			(at -2.275 -3.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(J5-Pin_3)")
			(pinfunction "10")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 2.275 -2.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Net-(J4-Pin_3)")
			(pinfunction "11")
			(pintype "input")
		)
		(pad "12" smd rect
			(at -2.275 -2.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-(J7-Pin_3)")
			(pinfunction "12")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 2.275 -2.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(J2-Pin_4)")
			(pinfunction "13")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -2.275 -2.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "Net-(J6-Pin_4)")
			(pinfunction "14")
			(pintype "input")
		)
		(pad "15" smd rect
			(at 2.275 -2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "Net-(J3-Pin_4)")
			(pinfunction "15")
			(pintype "input")
		)
		(pad "16" smd rect
			(at -2.275 -2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(J5-Pin_4)")
			(pinfunction "16")
			(pintype "input")
		)
		(pad "17" smd rect
			(at 2.275 -1.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "Net-(J4-Pin_4)")
			(pinfunction "17")
			(pintype "input")
		)
		(pad "18" smd rect
			(at -2.275 -1.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(J7-Pin_4)")
			(pinfunction "18")
			(pintype "input")
		)
		(pad "19" smd rect
			(at 2.275 -1.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "Net-(J2-Pin_5)")
			(pinfunction "19")
			(pintype "input")
		)
		(pad "20" smd rect
			(at -2.275 -1.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "Net-(J6-Pin_5)")
			(pinfunction "20")
			(pintype "input")
		)
		(pad "21" smd rect
			(at 2.275 -0.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(J3-Pin_5)")
			(pinfunction "21")
			(pintype "input")
		)
		(pad "22" smd rect
			(at -2.275 -0.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(J5-Pin_5)")
			(pinfunction "22")
			(pintype "input")
		)
		(pad "23" smd rect
			(at 2.275 -0.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "Net-(J4-Pin_5)")
			(pinfunction "23")
			(pintype "input")
		)
		(pad "24" smd rect
			(at -2.275 -0.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "Net-(J7-Pin_5)")
			(pinfunction "24")
			(pintype "input")
		)
		(pad "25" smd rect
			(at 2.275 0)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "Net-(J2-Pin_6)")
			(pinfunction "25")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -2.275 0)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(J6-Pin_6)")
			(pinfunction "26")
			(pintype "input")
		)
		(pad "27" smd rect
			(at 2.275 0.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "Net-(J3-Pin_6)")
			(pinfunction "27")
			(pintype "input")
		)
		(pad "28" smd rect
			(at -2.275 0.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "Net-(J5-Pin_6)")
			(pinfunction "28")
			(pintype "input")
		)
		(pad "29" smd rect
			(at 2.275 0.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "Net-(J4-Pin_6)")
			(pinfunction "29")
			(pintype "input")
		)
		(pad "30" smd rect
			(at -2.275 0.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(J7-Pin_6)")
			(pinfunction "30")
			(pintype "input")
		)
		(pad "31" smd rect
			(at 2.275 1.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(J2-Pin_7)")
			(pinfunction "31")
			(pintype "input")
		)
		(pad "32" smd rect
			(at -2.275 1.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "Net-(J6-Pin_7)")
			(pinfunction "32")
			(pintype "input")
		)
		(pad "33" smd rect
			(at 2.275 1.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "Net-(J3-Pin_7)")
			(pinfunction "33")
			(pintype "input")
		)
		(pad "34" smd rect
			(at -2.275 1.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(J5-Pin_7)")
			(pinfunction "34")
			(pintype "input")
		)
		(pad "35" smd rect
			(at 2.275 2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(J4-Pin_7)")
			(pinfunction "35")
			(pintype "input")
		)
		(pad "36" smd rect
			(at -2.275 2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(J7-Pin_7)")
			(pinfunction "36")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 2.275 2.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "Net-(J2-Pin_8)")
			(pinfunction "37")
			(pintype "input")
		)
		(pad "38" smd rect
			(at -2.275 2.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(J6-Pin_8)")
			(pinfunction "38")
			(pintype "input")
		)
		(pad "39" smd rect
			(at 2.275 2.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "Net-(J3-Pin_8)")
			(pinfunction "39")
			(pintype "input")
		)
		(pad "40" smd rect
			(at -2.275 2.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "Net-(J5-Pin_8)")
			(pinfunction "40")
			(pintype "input")
		)
		(pad "41" smd rect
			(at 2.275 3.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(J4-Pin_8)")
			(pinfunction "41")
			(pintype "input")
		)
		(pad "42" smd rect
			(at -2.275 3.2)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(J7-Pin_8)")
			(pinfunction "42")
			(pintype "input")
		)
		(pad "43" smd rect
			(at 2.275 3.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(J2-Pin_9)")
			(pinfunction "43")
			(pintype "input")
		)
		(pad "44" smd rect
			(at -2.275 3.6)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(J6-Pin_9)")
			(pinfunction "44")
			(pintype "input")
		)
		(pad "45" smd rect
			(at 2.275 4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(J3-Pin_9)")
			(pinfunction "45")
			(pintype "input")
		)
		(pad "46" smd rect
			(at -2.275 4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "Net-(J5-Pin_9)")
			(pinfunction "46")
			(pintype "input")
		)
		(pad "47" smd rect
			(at 2.275 4.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(J4-Pin_9)")
			(pinfunction "47")
			(pintype "input")
		)
		(pad "48" smd rect
			(at -2.275 4.4)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(J7-Pin_9)")
			(pinfunction "48")
			(pintype "input")
		)
		(pad "49" smd rect
			(at 2.275 4.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(J2-Pin_10)")
			(pinfunction "49")
			(pintype "input")
		)
		(pad "50" smd rect
			(at -2.275 4.8)
			(size 1.15 0.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "Net-(J6-Pin_10)")
			(pinfunction "50")
			(pintype "input")
		)
		(model "${T_LIBS}/3d/t_connectors/546840504.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 125.095 76.835)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J7"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.19 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Test Header BO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 14.39 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J7-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J7-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J7-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J7-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J7-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J7-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J7-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 122.555 73.025) (xy 168.275 73.025) (xy 169.545 74.295) (xy 169.545 102.235) (xy 168.275 103.505)
			(xy 122.555 103.505) (xy 121.285 102.235) (xy 121.285 74.295)
		)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "20\n"
		(at 139.065 87.63 -0)
		(layer "B.SilkS")
	)
	(gr_text "26"
		(at 139.065 90.17 -0)
		(layer "B.SilkS")
	)
	(gr_text "15"
		(at 159.385 85.09 -0)
		(layer "B.SilkS")
	)
	(gr_text "39"
		(at 159.385 95.25 -0)
		(layer "B.SilkS")
	)
	(gr_text "Molex 54684-0504\nBreakout Board"
		(at 147.32 80.645 90)
		(layer "B.SilkS")
	)
	(gr_text "18\n"
		(at 128.27 85.09 -0)
		(layer "B.SilkS")
	)
	(gr_text "49"
		(at 153.67 100.33 -0)
		(layer "B.SilkS")
	)
	(gr_text "4"
		(at 133.35 80.01 -0)
		(layer "B.SilkS")
	)
	(gr_text "40\n"
		(at 133.35 95.25 -0)
		(layer "B.SilkS")
	)
	(gr_text "50\n"
		(at 139.065 100.33 -0)
		(layer "B.SilkS")
	)
	(gr_text "16"
		(at 133.35 85.09 -0)
		(layer "B.SilkS")
	)
	(gr_text "37"
		(at 153.67 95.25 -0)
		(layer "B.SilkS")
	)
	(gr_text "17"
		(at 164.465 85.09 -0)
		(layer "B.SilkS")
	)
	(gr_text "11"
		(at 164.465 82.55 -0)
		(layer "B.SilkS")
	)
	(gr_text "24"
		(at 128.27 87.63 -0)
		(layer "B.SilkS")
	)
	(gr_text "14"
		(at 139.065 85.09 -0)
		(layer "B.SilkS")
	)
	(gr_text "46"
		(at 133.35 97.79 -0)
		(layer "B.SilkS")
	)
	(gr_text "29"
		(at 164.405 90.17 -0)
		(layer "B.SilkS")
	)
	(gr_text "38\n"
		(at 139.065 95.25 -0)
		(layer "B.SilkS")
	)
	(gr_text "9"
		(at 158.75 82.55 -0)
		(layer "B.SilkS")
	)
	(gr_text "13"
		(at 153.67 85.09 -0)
		(layer "B.SilkS")
	)
	(gr_text "31"
		(at 153.67 92.71 -0)
		(layer "B.SilkS")
	)
	(gr_text "27"
		(at 159.385 90.17 -0)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 158.75 80.01 -0)
		(layer "B.SilkS")
	)
	(gr_text "8\n"
		(at 138.43 82.55 -0)
		(layer "B.SilkS")
	)
	(gr_text "12"
		(at 128.27 82.55 -0)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 163.83 80.01 -0)
		(layer "B.SilkS")
	)
	(gr_text "48\n"
		(at 128.27 97.79 -0)
		(layer "B.SilkS")
	)
	(gr_text "43"
		(at 153.67 97.79 -0)
		(layer "B.SilkS")
	)
	(gr_text "34"
		(at 133.35 92.71 -0)
		(layer "B.SilkS")
	)
	(gr_text "42"
		(at 128.27 95.25 -0)
		(layer "B.SilkS")
	)
	(gr_text "41"
		(at 164.465 95.25 -0)
		(layer "B.SilkS")
	)
	(gr_text "23"
		(at 164.465 87.63 -0)
		(layer "B.SilkS")
	)
	(gr_text "36"
		(at 128.27 92.71 -0)
		(layer "B.SilkS")
	)
	(gr_text "33"
		(at 159.385 92.71 -0)
		(layer "B.SilkS")
	)
	(gr_text "25"
		(at 153.67 90.17 -0)
		(layer "B.SilkS")
	)
	(gr_text "6"
		(at 128.27 80.01 -0)
		(layer "B.SilkS")
	)
	(gr_text "28\n"
		(at 133.35 90.17 -0)
		(layer "B.SilkS")
	)
	(gr_text "7"
		(at 153.67 82.55 -0)
		(layer "B.SilkS")
	)
	(gr_text "30\n"
		(at 128.27 90.17 -0)
		(layer "B.SilkS")
	)
	(gr_text "44"
		(at 139.065 97.79 -0)
		(layer "B.SilkS")
	)
	(gr_text "10\n"
		(at 133.35 82.55 -0)
		(layer "B.SilkS")
	)
	(gr_text "2"
		(at 138.43 80.01 -0)
		(layer "B.SilkS")
	)
	(gr_text "22"
		(at 133.35 87.63 -0)
		(layer "B.SilkS")
	)
	(gr_text "47"
		(at 164.465 97.79 -0)
		(layer "B.SilkS")
	)
	(gr_text "32"
		(at 139.065 92.71 -0)
		(layer "B.SilkS")
	)
	(gr_text "35"
		(at 164.465 92.71 -0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 153.67 80.01 -0)
		(layer "B.SilkS")
	)
	(gr_text "19"
		(at 153.67 87.63 -0)
		(layer "B.SilkS")
	)
	(gr_text "45"
		(at 159.385 97.79 -0)
		(layer "B.SilkS")
	)
	(gr_text "21"
		(at 159.385 87.63 -0)
		(layer "B.SilkS")
	)
	(gr_text "39"
		(at 157.48 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "27"
		(at 157.48 90.273415 0)
		(layer "F.SilkS")
	)
	(gr_text "26"
		(at 137.16 90.17 0)
		(layer "F.SilkS")
	)
	(gr_text "32"
		(at 137.16 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "38\n"
		(at 137.16 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 153.035 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "18\n"
		(at 126.365 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "33"
		(at 157.48 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "49"
		(at 151.765 100.33 0)
		(layer "F.SilkS")
	)
	(gr_text "35"
		(at 162.56 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "40\n"
		(at 131.445 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "25"
		(at 151.765 90.17 0)
		(layer "F.SilkS")
	)
	(gr_text "28\n"
		(at 131.445 90.17 0)
		(layer "F.SilkS")
	)
	(gr_text "23"
		(at 162.56 87.63 0)
		(layer "F.SilkS")
	)
	(gr_text "29"
		(at 162.56 90.17 0)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 157.48 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "16"
		(at 131.445 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "50\n"
		(at 137.16 100.33 0)
		(layer "F.SilkS")
	)
	(gr_text "46"
		(at 131.445 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "30\n"
		(at 126.365 90.17 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 127 80.01 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 163.195 80.01 0)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 162.56 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "47"
		(at 162.56 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "17"
		(at 162.56 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "20\n"
		(at 137.16 87.63 0)
		(layer "F.SilkS")
	)
	(gr_text "13"
		(at 151.765 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "42"
		(at 126.365 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "45"
		(at 157.48 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 137.16 85.09 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 158.115 80.01 0)
		(layer "F.SilkS")
	)
	(gr_text "8\n"
		(at 137.16 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "36"
		(at 126.365 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "21"
		(at 157.48 87.63 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 132.08 80.01 0)
		(layer "F.SilkS")
	)
	(gr_text "22"
		(at 131.445 87.63 0)
		(layer "F.SilkS")
	)
	(gr_text "43"
		(at 151.765 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 126.365 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "31"
		(at 151.765 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "48\n"
		(at 126.365 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "34"
		(at 131.445 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "10\n"
		(at 131.445 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 137.16 80.01 0)
		(layer "F.SilkS")
	)
	(gr_text "24"
		(at 126.365 87.63 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 153.035 80.01 0)
		(layer "F.SilkS")
	)
	(gr_text "44"
		(at 137.16 97.79 0)
		(layer "F.SilkS")
	)
	(gr_text "37"
		(at 151.765 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 151.765 87.63 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 158.115 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "41"
		(at 162.56 95.25 0)
		(layer "F.SilkS")
	)
	(zone
		(net 51)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.381)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.92 73.66) (xy 168.91 73.66) (xy 168.91 102.87) (xy 121.92 102.87)
			)
		)
	)
)
