(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "/VDD")
	(net 2 "/GND")
	(net 3 "/VCC")
	(net 4 "/VCOIL_N")
	(net 5 "/VCOIL_P")
	(net 6 "Net-(R1-Pad2)")
	(net 7 "/GPIO_1")
	(net 8 "/GPIO_0")
	(net 9 "/GPIO_2")
	(net 10 "/GPIO_3")
	(footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder"
		(layer "F.Cu")
		(at 121.666 90.68 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5975 0 90)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5975 0 90)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/GPIO_0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder"
		(layer "F.Cu")
		(at 127.254 92.712 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.17 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.17 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5975 0 270)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5975 0 270)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_1x02_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 133.63 86.741)
		(descr "Through hole straight pin header, 1x02, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x02 1.27mm single row")
		(property "Reference" "J1"
			(at -0.026 3.175 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 3.015 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x02_P1.27mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 126.746 90.424 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.16 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small_US"
			(at 0 1.16 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 270)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "headstage_footprints:SC-70_SOT323_NEX"
		(layer "F.Cu")
		(at 130.111 86.713)
		(tags "BAT854W_115 ")
		(property "Reference" "U3"
			(at -23.5591 -13.5917 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at -23.5591 -13.5917 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.649999 0.8763)
			(size 0.4572 1.1684)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/GND")
			(pintype "free")
		)
		(pad "2" smd rect
			(at 0.649999 0.8763)
			(size 0.4572 1.1684)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/VCC")
			(pintype "free")
		)
		(pad "3" smd rect
			(at 0 -0.8763)
			(size 0.4572 1.1684)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/VCOIL_P")
			(pintype "free")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder"
		(layer "F.Cu")
		(at 121.666 88.392 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5975 0 90)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/GPIO_0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5975 0 90)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 127.063 86.106)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "J4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/VCOIL_N")
			(pintype "free")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/VCOIL_P")
			(pintype "free")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "headstage_footprints:SC-70_SOT323_NEX"
		(layer "F.Cu")
		(at 124.038 86.713)
		(tags "BAT854W_115 ")
		(property "Reference" "U4"
			(at -23.5591 -13.5917 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at -23.5591 -13.5917 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.649999 0.8763)
			(size 0.4572 1.1684)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/GND")
			(pintype "free")
		)
		(pad "2" smd rect
			(at 0.649999 0.8763)
			(size 0.4572 1.1684)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/VCC")
			(pintype "free")
		)
		(pad "3" smd rect
			(at 0 -0.8763)
			(size 0.4572 1.1684)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/VCOIL_N")
			(pintype "free")
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0402_1005Metric_Pad0.77x0.64mm_HandSolder"
		(layer "F.Cu")
		(at 121.666 86.106 90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5725 0 90)
			(size 0.765 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5725 0 90)
			(size 0.765 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/GPIO_1")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric_Pad0.72x0.64mm_HandSolder"
		(layer "F.Cu")
		(at 128.524 92.712 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5975 0 90)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5975 0 90)
			(size 0.715 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "headstage_footprints:UJ-5_ADI"
		(layer "F.Cu")
		(at 124.280001 91.58205 -90)
		(tags "ADP165AUJZ-3.3-R7 ")
		(property "Reference" "U2"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.37795 -0.950001 270)
			(size 1.0033 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/VCC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.37795 0 270)
			(size 1.0033 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/GND")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.37795 0.950001 270)
			(size 1.0033 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/VCC")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 1.37795 0.950001 270)
			(size 1.0033 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/VDD")
			(pintype "output")
		)
		(pad "5" smd rect
			(at 1.37795 -0.950001 270)
			(size 1.0033 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(R1-Pad2)")
			(pintype "output")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 119.38 86.741)
		(descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x06 1.27mm single row")
		(property "Reference" "J3"
			(at 0 -1.745 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x06_Pin"
			(at 0 8.095 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.175 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/GPIO_1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/GPIO_3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/GPIO_2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3.81)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/GPIO_0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 6.35)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/VDD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric_Pad0.74x0.62mm_HandSolder"
		(layer "F.Cu")
		(at 121.666 92.964 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C_Small_US"
			(at 0 1.16 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "headstage.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.5675 0 90)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.5675 0 90)
			(size 0.735 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 117.496 84.001)
		(end 135.504 95.062)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "FH09"
		(at 130.81 92.202 0)
		(layer "F.SilkS")
	)
	(gr_text "R2\n"
		(at 128.524 92.712 90)
		(layer "F.Fab")
	)
	(gr_text "R1\n"
		(at 127.254 92.712 90)
		(layer "F.Fab")
	)
	(zone
		(net 2)
		(net_name "/GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.856 84.328) (xy 135.128 84.328) (xy 135.128 94.742) (xy 117.856 94.742)
			)
		)
	)
	(embedded_fonts no)
)
