(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(color "Phenolic natural")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+12V")
	(net 2 "GND")
	(net 3 "Net-(U1-PA1)")
	(net 4 "unconnected-(U1-~{RESET}{slash}PA0-Pad6)")
	(net 5 "+5V")
	(net 6 "BATT")
	(net 7 "unconnected-(U1-PA6-Pad2)")
	(net 8 "unconnected-(D1-DOUT-Pad2)")
	(net 9 "Net-(D1-DIN)")
	(net 10 "Net-(Q1-G)")
	(net 11 "Net-(Q1-D)")
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 205.89 138.68 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 2.67 -0.03 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "311-10.0KHRCT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "BATT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 216.78 140.51 -90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U3"
			(at 0 -2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "MCP9700x-ETT"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/20001942g.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low power, analog thermistor temperature sensor, ±4C accuracy, -40C to +125C, in SOT-23-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "MCP9700T-E/TTCT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pinfunction "V_{DD}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-PA1)")
			(pinfunction "V_{OUT}")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 221.885 136.56 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at -2.45 -0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "311-1088-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 214.42 130.2325 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -2.5375 0.19 270)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "311-1445-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-89-3"
		(layer "F.Cu")
		(at 212.89 125.71 90)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "U2"
			(at -4.06 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "L78L05_SOT89"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/15/55/e5/aa/23/5b/43/fd/CD00000446.pdf/files/CD00000446.pdf/jcr:content/translations/en.CD00000446.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 100mA 30V Linear Regulator, Fixed Output 5V, SOT-89"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "497-1181-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?89*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.95 -1.5 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "2" smd custom
			(at -1.8625 0 90)
			(size 1.475 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 3.8625 0.8665) (xy 0.7375 0.8665) (xy 0.7375 -0.8665) (xy 3.8625 -0.8665)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "3" smd roundrect
			(at -1.95 1.5 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+12V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 219.41 131.91 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny412-SS"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001911A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "ATTINY412-SSFRCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "unconnected-(U1-PA6-Pad2)")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D1-DIN)")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-PA1)")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "BATT")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "unconnected-(U1-~{RESET}{slash}PA0-Pad6)")
			(pinfunction "~{RESET}/PA0")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(Q1-G)")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
		(layer "F.Cu")
		(at 219.48 126.26)
		(descr "5.0mm x 5.0mm Addressable RGB LED NeoPixel, https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf")
		(tags "LED RGB NeoPixel PLCC-4 5050")
		(property "Reference" "D1"
			(at -4.06 2.14 270)
			(layer "F.SilkS")
		)
		(property "Value" "WS2812B"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "1568-16347CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 5 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 8 "unconnected-(D1-DOUT-Pad2)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at 2.45 1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at 2.45 -1.65)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 9 "Net-(D1-DIN)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 211.4 130.22 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at -2.63 -0.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "311-1445-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 216.78 136.6 -90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0.28 -2.76 180)
			(layer "F.SilkS")
		)
		(property "Value" "DMN3404L"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.diodes.com/assets/Datasheets/ds31787.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5.8A Id, 30V Vds, N-Channel MOSFET, SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "DMN3404LDICT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(Q1-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 209.63 137.9425 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D2"
			(at -3.3775 0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "BZT52C5V1-TPMSCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "BATT")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "XT30:AMASS_XT30U-F_1x02_P5.0mm_Vertical"
		(layer "F.Cu")
		(at 207.08 126.38 -90)
		(descr "Connector XT30 Vertical Cable Female, https://www.tme.eu/en/Document/3cbfa5cfa544d79584972dd5234a409e/XT30U%20SPEC.pdf")
		(tags "RC Connector XT30")
		(property "Reference" "BT1"
			(at 8.79 0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "Battery"
			(at 2.5 4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "1738-1436-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 5 0 270)
			(size 4 4)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+12V")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 0 0 270)
			(size 3.8 3.8)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/andrew/Downloads/Amass_XT30UPB-M.step"
			(offset
				(xyz 2.5 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 221.87 141.16)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 207.5 138.6625 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -2.7575 0.03 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "311-4.70KHRCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "BATT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric_Pad1.40x3.35mm_HandSolder"
		(layer "F.Cu")
		(at 212.88 137.96 90)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 4.56 0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "15R"
			(at 0 2.63 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey Part" "CPA25Q15.0CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FTCBatteryTester.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.05 0 90)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 1 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.05 0 90)
			(size 1.4 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 11 "Net-(Q1-D)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 205.12 123.18)
		(end 222.32 123.18)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 223.57 141.62)
		(mid 223.203883 142.503883)
		(end 222.32 142.87)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 203.87 124.43)
		(mid 204.236117 123.546117)
		(end 205.12 123.18)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 222.32 123.18)
		(mid 223.203883 123.546117)
		(end 223.57 124.43)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 205.12 142.87)
		(mid 204.236117 142.503883)
		(end 203.87 141.62)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 222.32 142.87)
		(end 205.12 142.87)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 223.57 124.43)
		(end 223.57 141.62)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 203.87 141.62)
		(end 203.87 124.43)
		(layer "Edge.Cuts")
	)
	(gr_text "BattGauge"
		(at 222.64 126.11 0)
		(layer "B.SilkS")
	)
	(gr_text "17097\nProtostars"
		(at 222.47 130.66 0)
		(layer "B.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 223.66 123.13) (xy 223.62 142.91) (xy 203.77 142.87) (xy 203.84 123.13) (xy 223.76 123.17)
			)
		)
	)
	(embedded_fonts no)
)
