(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
			(edge_plating yes)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+3V3")
	(net 2 "+5V")
	(net 3 "unconnected-(J1-Pin_12-Pad12)")
	(net 4 "/CLK1_OUT_TTL")
	(net 5 "unconnected-(J1-Pin_23-Pad23)")
	(net 6 "unconnected-(J1-Pin_15-Pad15)")
	(net 7 "unconnected-(J1-Pin_32-Pad32)")
	(net 8 "/DATA1_OUT_TTL")
	(net 9 "unconnected-(J1-Pin_5-Pad5)")
	(net 10 "GND")
	(net 11 "unconnected-(U3-~{INH}-Pad1)")
	(net 12 "unconnected-(J1-Pin_20-Pad20)")
	(net 13 "unconnected-(J1-Pin_19-Pad19)")
	(net 14 "/EXT_CLK2")
	(net 15 "unconnected-(J1-Pin_26-Pad26)")
	(net 16 "unconnected-(J1-Pin_21-Pad21)")
	(net 17 "unconnected-(J1-Pin_37-Pad37)")
	(net 18 "unconnected-(J1-Pin_18-Pad18)")
	(net 19 "unconnected-(J1-Pin_28-Pad28)")
	(net 20 "unconnected-(J1-Pin_16-Pad16)")
	(net 21 "unconnected-(J1-Pin_29-Pad29)")
	(net 22 "unconnected-(J1-Pin_9-Pad9)")
	(net 23 "unconnected-(J1-Pin_13-Pad13)")
	(net 24 "/EXT_CLK1")
	(net 25 "unconnected-(J1-Pin_39-Pad39)")
	(net 26 "unconnected-(J1-Pin_22-Pad22)")
	(net 27 "unconnected-(J1-Pin_33-Pad33)")
	(net 28 "unconnected-(J1-Pin_7-Pad7)")
	(net 29 "unconnected-(J1-Pin_3-Pad3)")
	(net 30 "unconnected-(J1-Pin_25-Pad25)")
	(net 31 "unconnected-(J1-Pin_30-Pad30)")
	(net 32 "unconnected-(J1-Pin_27-Pad27)")
	(net 33 "unconnected-(J1-Pin_35-Pad35)")
	(net 34 "unconnected-(J1-Pin_31-Pad31)")
	(net 35 "unconnected-(J1-Pin_17-Pad17)")
	(net 36 "unconnected-(J1-Pin_34-Pad34)")
	(net 37 "unconnected-(J1-Pin_11-Pad11)")
	(net 38 "/CLK1_OUT_+")
	(net 39 "/CLK1_OUT_-")
	(net 40 "/DATA1_OUT_+")
	(net 41 "/DATA1_OUT_-")
	(net 42 "/CLK2_OUT_TTL")
	(net 43 "/DATA2_OUT_TTL")
	(net 44 "/DATA2_OUT_+")
	(net 45 "/DATA2_OUT_-")
	(net 46 "/CLK2_OUT_-")
	(net 47 "/CLK2_OUT_+")
	(footprint "footprints:D16"
		(layer "F.Cu")
		(at 52.62 76.95)
		(tags "AM26C31IDR ")
		(property "Reference" "U1"
			(at -3.725 -5.83 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AM26C31IDR"
			(at 0 -7.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/am26c31"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D16 D16-M D16-L")
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.3622 -4.445)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/CLK1_OUT_TTL")
			(pinfunction "1A")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.3622 -3.175)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/CLK1_OUT_+")
			(pinfunction "1Y")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -2.3622 -1.905)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/CLK1_OUT_-")
			(pinfunction "1Z")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -2.3622 -0.635)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "GND")
			(pinfunction "G")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -2.3622 0.635)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/DATA1_OUT_-")
			(pinfunction "2Z")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -2.3622 1.905)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/DATA1_OUT_+")
			(pinfunction "2Y")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -2.3622 3.175)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/DATA1_OUT_TTL")
			(pinfunction "2A")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -2.3622 4.445)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 2.3622 4.445)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/DATA2_OUT_TTL")
			(pinfunction "3A")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 2.3622 3.175)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "/DATA2_OUT_+")
			(pinfunction "3Y")
			(pintype "output")
		)
		(pad "11" smd rect
			(at 2.3622 1.905)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/DATA2_OUT_-")
			(pinfunction "3Z")
			(pintype "output")
		)
		(pad "12" smd rect
			(at 2.3622 0.635)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "GND")
			(pinfunction "*G")
			(pintype "unspecified")
		)
		(pad "13" smd rect
			(at 2.3622 -0.635)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "/CLK2_OUT_-")
			(pinfunction "4Z")
			(pintype "output")
		)
		(pad "14" smd rect
			(at 2.3622 -1.905)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/CLK2_OUT_+")
			(pinfunction "4Y")
			(pintype "output")
		)
		(pad "15" smd rect
			(at 2.3622 -3.175)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/CLK2_OUT_TTL")
			(pinfunction "4A")
			(pintype "input")
		)
		(pad "16" smd rect
			(at 2.3622 -4.445)
			(size 2.1844 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "rsdw:ATXH11F48000MHZG50T"
		(layer "F.Cu")
		(at 44.28 98.768 180)
		(descr "ATX-H11-F-48.000MHZ-G50-T-1")
		(tags "Crystal or Oscillator")
		(property "Reference" "U3"
			(at 3.98 1.308 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ATX-H11-F-48.000MHZ-G50-T"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet_1" "https://abracon.com/datasheets/ATX-H11.pdf"
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_1" "ATXH11F48000MHZG50T"
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.2"
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ABRACON"
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ATX-H11-F-48.000MHZ-G50-T"
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference_1" "Y"
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value_1" "ATX-H11-F-48.000MHZ-G50-T"
			(at 35.56 71.12 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr smd)
		(image
			(at 44.112003 98.738)
			(layer "F.Cu")
			(scale 0.211863)
		)
		(fp_text user "${REFERENCE}"
			(at -1.1 -3.772 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1 0.8 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(U3-~{INH}-Pad1)")
			(pinfunction "~{INH}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.04 0.79 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.03 -1 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/EXT_CLK1")
			(pinfunction "OUTPUT")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.11 -1.01 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+3V3")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "ATX-H11-F-48.000MHZ-G50-T.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x08_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 46.355 129.54)
		(descr "Through hole straight socket strip, 1x08, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x08 2.54mm single row")
		(property "Reference" "J4"
			(at 0 20.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x08_Male"
			(at -7.62 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3V3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/EXT_CLK2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/EXT_CLK1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/DATA2_OUT_TTL")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/CLK2_OUT_TTL")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA1_OUT_TTL")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CLK1_OUT_TTL")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x08_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rsdw:M80-54006YY"
		(layer "F.Cu")
		(at 45 68.06 -90)
		(descr "M80-54006YY")
		(tags "Connector")
		(property "Reference" "J5"
			(at -3.29 -3.895 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M80-5400642"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet_1" "https://content.harwin.com/m/501f35f2e26b8fc5/original/DRG-01248-Technical-Drawing-Datasheet-M80-540-pdf.pdf"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_1" "M80-54006YY"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "6"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Harwin"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "M80-5400642"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "855-M80-5400642"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Harwin/M80-5400642?qs=7jyBjEprRBg3EbeF%2FpszQw%3D%3D"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference_1" "J"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value_1" "M80-5400642"
			(at 81.28 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -7.1 -3.26 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/CLK2_OUT_+")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2 0 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/CLK2_OUT_-")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4 0 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 2 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/DATA2_OUT_+")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -2 2 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/DATA2_OUT_-")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -4 2 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 3.5 1 270)
			(size 3.75 3.75)
			(drill 2.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -7.5 1 270)
			(size 3.75 3.75)
			(drill 2.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "M80-5400642.stp"
			(offset
				(xyz -1.99999997 -4.499999932 3.140000058)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 54.864 102.55 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -2.286 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 5.08 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.05 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 50.1 52.3)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "REF**"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
			(at 0 3.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
		(layer "F.Cu")
		(at 50 161.3)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "REF**"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad_TopOnly"
			(at 0 3.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.6 3.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 5.7 5.7)
			(layers "F.Cu" "F.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 54.864 97.978 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -2.286 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.01uF"
			(at 5.08 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rsdw:M80-54006YY"
		(layer "F.Cu")
		(at 45 88.5 -90)
		(descr "M80-54006YY")
		(tags "Connector")
		(property "Reference" "J3"
			(at 0.4 -3.26 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M80-5400642"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet_1" "https://content.harwin.com/m/501f35f2e26b8fc5/original/DRG-01248-Technical-Drawing-Datasheet-M80-540-pdf.pdf"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint_1" "M80-54006YY"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "6"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Harwin"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "M80-5400642"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "855-M80-5400642"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Harwin/M80-5400642?qs=7jyBjEprRBg3EbeF%2FpszQw%3D%3D"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Reference_1" "J"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Value_1" "M80-5400642"
			(at 40.4 45.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.94 -3.26 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/CLK1_OUT_+")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2 0 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/CLK1_OUT_-")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4 0 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 2 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/DATA1_OUT_+")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -2 2 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/DATA1_OUT_-")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -4 2 270)
			(size 1.15 1.15)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 3.5 1 270)
			(size 3.75 3.75)
			(drill 2.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -7.5 1 270)
			(size 3.75 3.75)
			(drill 2.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "M80-5400642.stp"
			(offset
				(xyz -1.99999997 -4.499999932 3.140000058)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x20_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 49.276 99.06)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "J1"
			(at 1.524 50.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x20_Odd_Even"
			(at 2.54 55.88 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "Toaster_Board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(J1-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(J1-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J1-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CLK1_OUT_TTL")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J1-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA1_OUT_TTL")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(J1-Pin_11-Pad11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(J1-Pin_12-Pad12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J1-Pin_13-Pad13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(J1-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J1-Pin_16-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(J1-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J1-Pin_18-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J1-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J1-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J1-Pin_21-Pad21)")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J1-Pin_22-Pad22)")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(J1-Pin_23-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/EXT_CLK2")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(J1-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at 2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J1-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole circle
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(J1-Pin_27-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole circle
			(at 2.54 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J1-Pin_28-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole circle
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J1-Pin_29-Pad29)")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" thru_hole circle
			(at 2.54 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(J1-Pin_30-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(J1-Pin_31-Pad31)")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole circle
			(at 2.54 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(J1-Pin_32-Pad32)")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole circle
			(at 0 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J1-Pin_33-Pad33)")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at 2.54 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J1-Pin_34-Pad34)")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" thru_hole circle
			(at 0 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(J1-Pin_35-Pad35)")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" thru_hole circle
			(at 2.54 43.18)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/EXT_CLK1")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" thru_hole circle
			(at 0 45.72)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J1-Pin_37-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" thru_hole circle
			(at 2.54 45.72)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/CLK2_OUT_TTL")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" thru_hole circle
			(at 0 48.26)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(J1-Pin_39-Pad39)")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" thru_hole circle
			(at 2.54 48.26)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/DATA2_OUT_TTL")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 60.96 154.94)
		(mid 57.242023 163.918489)
		(end 48.264999 167.64)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 48.26 45.725)
		(mid 57.238489 49.442977)
		(end 60.96 58.420001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 60.96 58.425)
		(end 60.96 154.94)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 48.264999 167.64)
		(mid 39.28651 163.922023)
		(end 35.564999 154.944999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 35.56 154.944999)
		(end 35.56 58.425)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 35.564999 58.425)
		(mid 39.282976 49.446511)
		(end 48.26 45.725)
		(layer "Edge.Cuts")
	)
	(image
		(at 44.330859 98.894815)
		(layer "F.Cu")
		(scale 0.151709)
	)
	(image
		(at 62.289619 104.648001)
		(layer "Edge.Cuts")
		(scale 2.17182)
		(locked yes)
	)
	(gr_text "20260211"
		(at 41.275 156.845 0)
		(layer "F.SilkS")
	)
	(gr_text "BREDSTIC V1 | Tyler Bovenzi"
		(at 59.055 106.045 90)
		(layer "F.SilkS")
	)
	(gr_text "SN___"
		(at 58.42 92.71 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "<GND"
		(at 46.99 128.27 90)
		(layer "F.SilkS")
	)
	(gr_text "Board for RS-422 Encoded Differential Signaling, Timing, and Integrated Clock"
		(at 57.15 153.67 270)
		(layer "B.SilkS")
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 34.29 44.45) (xy 34.29 167.64) (xy 62.23 167.64) (xy 62.289618 44.45)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 34.29 44.45) (xy 34.29 167.64) (xy 62.23 167.64) (xy 62.289618 44.45)
			)
		)
	)
	(embedded_fonts no)
)
