(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerbers/")
		)
	)
	(net 0 "")
	(net 1 "Net-(BT1-PadP)")
	(net 2 "GND")
	(net 3 "VBUS")
	(net 4 "+5V")
	(net 5 "/CAS_0")
	(net 6 "unconnected-(J1-PadB32)")
	(net 7 "unconnected-(J1-PadB31)")
	(net 8 "unconnected-(J1-PadB30)")
	(net 9 "/LWR")
	(net 10 "/VRES")
	(net 11 "unconnected-(J1-PadB29)")
	(net 12 "unconnected-(J1-PadB26)")
	(net 13 "/D3")
	(net 14 "unconnected-(J1-PadB25)")
	(net 15 "unconnected-(J1-PadB24)")
	(net 16 "unconnected-(J1-PadB23)")
	(net 17 "unconnected-(J1-PadB22)")
	(net 18 "unconnected-(J1-PadB21)")
	(net 19 "unconnected-(J1-PadB20)")
	(net 20 "/CEO")
	(net 21 "unconnected-(J1-PadB19)")
	(net 22 "unconnected-(J1-PadB18)")
	(net 23 "unconnected-(J1-PadB15)")
	(net 24 "unconnected-(J1-PadB14)")
	(net 25 "unconnected-(J1-PadB13)")
	(net 26 "/A22")
	(net 27 "/A21")
	(net 28 "/A20")
	(net 29 "/A19")
	(net 30 "/A18")
	(net 31 "/A10")
	(net 32 "/A9")
	(net 33 "unconnected-(J1-PadB12)")
	(net 34 "unconnected-(J1-PadB11)")
	(net 35 "unconnected-(J1-PadB3)")
	(net 36 "unconnected-(J1-PadB2)")
	(net 37 "/D4")
	(net 38 "unconnected-(J1-PadB1)")
	(net 39 "/D2")
	(net 40 "/D5")
	(net 41 "unconnected-(J1-PadA30)")
	(net 42 "/D1")
	(net 43 "/D6")
	(net 44 "unconnected-(J1-PadA27)")
	(net 45 "/D0")
	(net 46 "/D7")
	(net 47 "/A1")
	(net 48 "/A17")
	(net 49 "/A2")
	(net 50 "/A16")
	(net 51 "/A3")
	(net 52 "/A15")
	(net 53 "/A4")
	(net 54 "/A14")
	(net 55 "/A5")
	(net 56 "/A13")
	(net 57 "/A6")
	(net 58 "/A12")
	(net 59 "/A7")
	(net 60 "/A11")
	(net 61 "/A8")
	(net 62 "unconnected-(J1-PadA24)")
	(net 63 "Net-(U1-Pad8)")
	(net 64 "/SRAM_WE")
	(net 65 "/SRCE")
	(net 66 "Net-(U3-Pad8)")
	(net 67 "unconnected-(J1-PadA21)")
	(net 68 "unconnected-(U4-Pad15)")
	(net 69 "unconnected-(U4-Pad14)")
	(net 70 "/TREN")
	(net 71 "unconnected-(U4-Pad13)")
	(net 72 "Net-(U4-Pad7)")
	(net 73 "Net-(U5-Pad9)")
	(net 74 "/SRWE")
	(net 75 "Net-(U5-Pad3)")
	(net 76 "unconnected-(U4-Pad12)")
	(net 77 "unconnected-(U4-Pad10)")
	(net 78 "unconnected-(U5-Pad11)")
	(net 79 "unconnected-(U6-Pad9)")
	(net 80 "Net-(D1-Pad1)")
	(net 81 "unconnected-(U6-Pad8)")
	(net 82 "unconnected-(U6-Pad5)")
	(footprint "Sega CD RAM Cart:Genesis_Card_Edge"
		(layer "F.Cu")
		(at 84.4931 164.7317)
		(descr "Sega Genesis 64-Pin Card Edge Connector")
		(tags "Genesis Edge")
		(property "Reference" "J1"
			(at 34.671 -9.398 0)
			(layer "F.SilkS")
		)
		(property "Value" "Genesis_Edge_Connector"
			(at 35.687 -12.954 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 34.671 -10.922 0)
			(layer "F.Fab")
		)
		(pad "A1" connect rect
			(at 0.889 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A2" connect rect
			(at 3.429 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 4 "+5V")
			(pinfunction "+5V")
			(pintype "power_out")
		)
		(pad "A3" connect rect
			(at 5.969 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 61 "/A8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "A4" connect rect
			(at 8.509 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 60 "/A11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "A5" connect rect
			(at 11.049 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 59 "/A7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "A6" connect rect
			(at 13.589 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 58 "/A12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "A7" connect rect
			(at 16.129 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 57 "/A6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "A8" connect rect
			(at 18.669 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 56 "/A13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "A9" connect rect
			(at 21.209 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 55 "/A5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "A10" connect rect
			(at 23.749 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 54 "/A14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "A11" connect rect
			(at 26.289 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 53 "/A4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "A12" connect rect
			(at 28.829 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 52 "/A15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "A13" connect rect
			(at 31.369 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 51 "/A3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "A14" connect rect
			(at 33.909 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 50 "/A16")
			(pinfunction "A16")
			(pintype "output")
		)
		(pad "A15" connect rect
			(at 36.449 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 49 "/A2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "A16" connect rect
			(at 38.989 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 48 "/A17")
			(pinfunction "A17")
			(pintype "output")
		)
		(pad "A17" connect rect
			(at 41.529 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 47 "/A1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "A18" connect rect
			(at 44.069 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A19" connect rect
			(at 46.609 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 46 "/D7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "A20" connect rect
			(at 49.149 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 45 "/D0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "A21" connect rect
			(at 51.689 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 67 "unconnected-(J1-PadA21)")
			(pinfunction "D8")
			(pintype "tri_state+no_connect")
		)
		(pad "A22" connect rect
			(at 54.229 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 43 "/D6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "A23" connect rect
			(at 56.769 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 42 "/D1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "A24" connect rect
			(at 59.309 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 62 "unconnected-(J1-PadA24)")
			(pinfunction "D9")
			(pintype "tri_state+no_connect")
		)
		(pad "A25" connect rect
			(at 61.849 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 40 "/D5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "A26" connect rect
			(at 64.389 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 39 "/D2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "A27" connect rect
			(at 66.929 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 44 "unconnected-(J1-PadA27)")
			(pinfunction "D10")
			(pintype "tri_state+no_connect")
		)
		(pad "A28" connect rect
			(at 69.469 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "A29" connect rect
			(at 72.009 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 13 "/D3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "A30" connect rect
			(at 74.549 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 41 "unconnected-(J1-PadA30)")
			(pinfunction "D11")
			(pintype "tri_state+no_connect")
		)
		(pad "A31" connect rect
			(at 77.089 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 4 "+5V")
			(pinfunction "+5V")
			(pintype "passive")
		)
		(pad "A32" connect rect
			(at 79.629 -3)
			(size 1.78 6)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B1" connect rect
			(at 0.889 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 38 "unconnected-(J1-PadB1)")
			(pinfunction "Left_Audio")
			(pintype "input+no_connect")
		)
		(pad "B2" connect rect
			(at 3.429 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 36 "unconnected-(J1-PadB2)")
			(pinfunction "/MRES")
			(pintype "output+no_connect")
		)
		(pad "B3" connect rect
			(at 5.969 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 35 "unconnected-(J1-PadB3)")
			(pinfunction "Right_Audio")
			(pintype "output+no_connect")
		)
		(pad "B4" connect rect
			(at 8.509 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 32 "/A9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "B5" connect rect
			(at 11.049 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 31 "/A10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "B6" connect rect
			(at 13.589 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 30 "/A18")
			(pinfunction "A18")
			(pintype "output")
		)
		(pad "B7" connect rect
			(at 16.129 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 29 "/A19")
			(pinfunction "A19")
			(pintype "output")
		)
		(pad "B8" connect rect
			(at 18.669 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 28 "/A20")
			(pinfunction "A20")
			(pintype "output")
		)
		(pad "B9" connect rect
			(at 21.209 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 27 "/A21")
			(pinfunction "A21")
			(pintype "output")
		)
		(pad "B10" connect rect
			(at 23.749 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 26 "/A22")
			(pinfunction "A22")
			(pintype "output")
		)
		(pad "B11" connect rect
			(at 26.289 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 34 "unconnected-(J1-PadB11)")
			(pinfunction "A23")
			(pintype "output+no_connect")
		)
		(pad "B12" connect rect
			(at 28.829 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 33 "unconnected-(J1-PadB12)")
			(pinfunction "/YS")
			(pintype "output+no_connect")
		)
		(pad "B13" connect rect
			(at 31.369 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 25 "unconnected-(J1-PadB13)")
			(pinfunction "/VSYNC")
			(pintype "output+no_connect")
		)
		(pad "B14" connect rect
			(at 33.909 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 24 "unconnected-(J1-PadB14)")
			(pinfunction "/HSYNC")
			(pintype "output+no_connect")
		)
		(pad "B15" connect rect
			(at 36.449 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 23 "unconnected-(J1-PadB15)")
			(pinfunction "EDCLK")
			(pintype "output+no_connect")
		)
		(pad "B16" connect rect
			(at 38.989 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 5 "/CAS_0")
			(pinfunction "/CAS0")
			(pintype "output")
		)
		(pad "B17" connect rect
			(at 41.529 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 20 "/CEO")
			(pinfunction "/CEO")
			(pintype "output")
		)
		(pad "B18" connect rect
			(at 44.069 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 22 "unconnected-(J1-PadB18)")
			(pinfunction "/AS")
			(pintype "output+no_connect")
		)
		(pad "B19" connect rect
			(at 46.609 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 21 "unconnected-(J1-PadB19)")
			(pinfunction "VCLK")
			(pintype "output+no_connect")
		)
		(pad "B20" connect rect
			(at 49.149 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 19 "unconnected-(J1-PadB20)")
			(pinfunction "/DTACK")
			(pintype "output+no_connect")
		)
		(pad "B21" connect rect
			(at 51.689 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 18 "unconnected-(J1-PadB21)")
			(pinfunction "/CAS2")
			(pintype "output+no_connect")
		)
		(pad "B22" connect rect
			(at 54.229 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 17 "unconnected-(J1-PadB22)")
			(pinfunction "D15")
			(pintype "tri_state+no_connect")
		)
		(pad "B23" connect rect
			(at 56.769 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 16 "unconnected-(J1-PadB23)")
			(pinfunction "D14")
			(pintype "tri_state+no_connect")
		)
		(pad "B24" connect rect
			(at 59.309 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 15 "unconnected-(J1-PadB24)")
			(pinfunction "D13")
			(pintype "tri_state+no_connect")
		)
		(pad "B25" connect rect
			(at 61.849 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 14 "unconnected-(J1-PadB25)")
			(pinfunction "D12")
			(pintype "tri_state+no_connect")
		)
		(pad "B26" connect rect
			(at 64.389 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 12 "unconnected-(J1-PadB26)")
			(pinfunction "/ASEL")
			(pintype "output+no_connect")
		)
		(pad "B27" connect rect
			(at 66.929 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 10 "/VRES")
			(pinfunction "/VRES")
			(pintype "output")
		)
		(pad "B28" connect rect
			(at 69.469 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 9 "/LWR")
			(pinfunction "/LWR")
			(pintype "output")
		)
		(pad "B29" connect rect
			(at 72.009 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 11 "unconnected-(J1-PadB29)")
			(pinfunction "/UWR")
			(pintype "output+no_connect")
		)
		(pad "B30" connect rect
			(at 74.549 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 8 "unconnected-(J1-PadB30)")
			(pinfunction "/M3")
			(pintype "input+no_connect")
		)
		(pad "B31" connect rect
			(at 77.089 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 7 "unconnected-(J1-PadB31)")
			(pinfunction "/TIME")
			(pintype "output+no_connect")
		)
		(pad "B32" connect rect
			(at 79.629 -3)
			(size 1.78 6)
			(layers "F.Cu" "F.Mask")
			(net 6 "unconnected-(J1-PadB32)")
			(pinfunction "/CART")
			(pintype "input+no_connect")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 110.0455 114.427 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0.0635 1.651 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "C1206C104K4RACTU"
			(at 220.091 228.854 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 129.032 140.614 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "C1206C104K4RACTU"
			(at -11.582 269.646 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 130.13222 132.76072)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0.03262 -1.78308 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "C1206C104K4RACTU"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 87.9475 152.146 180)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C8"
			(at 1 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF 25v"
			(at 1 3.75 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "25ML22MEFC5X5"
			(at 175.895 304.292 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 90.17 144.5895 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 2.794 -0.0635 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "RMCF0805FT1K00"
			(at 180.34 289.179 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083325)
			(net 80 "Net-(D1-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083325)
			(net 1 "Net-(BT1-PadP)")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:SSOP-20_W5.3mm"
		(layer "F.Cu")
		(at 150.4315 144.9705)
		(descr "http://ww1.microchip.com/downloads/en/DeviceDoc/41606B.pdf")
		(property "Reference" "U7"
			(at 4.7625 0.0127 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS245"
			(at 0 5.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "SN74LS245DBR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.925 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.275 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/D0")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd rect
			(at -1.625 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "/D1")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd rect
			(at -0.975 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "/D2")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd rect
			(at -0.325 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd rect
			(at 0.325 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd rect
			(at 0.975 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd rect
			(at 1.625 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd rect
			(at 2.275 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd rect
			(at 2.925 3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at 2.925 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd rect
			(at 2.275 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd rect
			(at 1.625 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd rect
			(at 0.975 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd rect
			(at 0.325 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd rect
			(at -0.325 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd rect
			(at -0.975 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd rect
			(at -1.625 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd rect
			(at -2.275 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "/TREN")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd rect
			(at -2.925 -3.6)
			(size 0.45 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 143.9545 144.9705 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "C1206C104K4RACTU"
			(at 288.925 1.016 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 4 "+5V")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:SOIC-14_W3.9mm"
		(layer "F.Cu")
		(at 122.7369 130.2169 180)
		(property "Reference" "U5"
			(at -0.0721 5.2489 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LS32"
			(at 0 5.29 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "SN74LS32DR"
			(at 245.4738 260.4338 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "REF**"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(U1-Pad8)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U3-Pad8)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "Net-(U5-Pad3)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(U4-Pad7)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "Net-(U5-Pad3)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "/SRWE")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "/SRAM_WE")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "Net-(U5-Pad9)")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/LWR")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 0 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 78 "unconnected-(U5-Pad11)")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at -1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:SOIC-14_W3.9mm"
		(layer "F.Cu")
		(at 122.682 140.6525 180)
		(property "Reference" "U6"
			(at 0 -4.79 0)
			(layer "F.SilkS")
		)
		(property "Value" "74LS74"
			(at 0 5.29 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "SN74LS74ADR"
			(at 245.364 281.305 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "REF**"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "~{R}")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/D0")
			(pinfunction "D")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "/SRWE")
			(pinfunction "C")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "/VRES")
			(pinfunction "~{S}")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 1.27 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 82 "unconnected-(U6-Pad5)")
			(pinfunction "Q")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 2.54 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 73 "Net-(U5-Pad9)")
			(pinfunction "~{Q}")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.81 2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "unconnected-(U6-Pad8)")
			(pinfunction "~{Q}")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "unconnected-(U6-Pad9)")
			(pinfunction "Q")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "~{S}")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 0 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "C")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at -1.27 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "D")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -2.54 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "~{R}")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -3.81 -2.7 180)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:SOT-23-3"
		(layer "F.Cu")
		(at 90.1065 141.4145 90)
		(property "Reference" "D1"
			(at 0.1905 -2.667 90)
			(layer "F.SilkS")
		)
		(property "Value" "MMBD1204"
			(at 0.254 2.667 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "MMBD1204CT-ND"
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" ""
			(at 231.521 51.308 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.125 0.15 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "Net-(D1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -1.05 0.95 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at 1.05 0 90)
			(size 1.3 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "VBUS")
			(pintype "passive")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:SOIC-16_W3.90mm"
		(locked yes)
		(layer "F.Cu")
		(at 135.8011 139.2428 90)
		(property "Reference" "U4"
			(at 0.5588 5.0419 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS138"
			(at 0 5 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "SN74LS138DR"
			(at 275.0439 3.4417 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "REF**"
			(at -0.0093 -0.0224 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.445 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "/A20")
			(pinfunction "A0")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -3.175 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "/A21")
			(pinfunction "A1")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.905 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "/A22")
			(pinfunction "A2")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at -0.635 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/CEO")
			(pinfunction "E1")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 0.635 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/CEO")
			(pinfunction "E2")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 1.905 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "E3")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.175 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "Net-(U4-Pad7)")
			(pinfunction "O7")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 4.445 2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 4.445 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "/SRCE")
			(pinfunction "O6")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 3.175 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "unconnected-(U4-Pad10)")
			(pinfunction "O5")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 1.905 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "/TREN")
			(pinfunction "O4")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at 0.635 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 76 "unconnected-(U4-Pad12)")
			(pinfunction "O3")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -0.635 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 71 "unconnected-(U4-Pad13)")
			(pinfunction "O2")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -1.905 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 69 "unconnected-(U4-Pad14)")
			(pinfunction "O1")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "15" smd rect
			(at -3.175 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "unconnected-(U4-Pad15)")
			(pinfunction "O0")
			(pintype "output+no_connect")
			(solder_mask_margin 0.07)
		)
		(pad "16" smd rect
			(at -4.445 -2.7 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "Package_SO:SSOP-32_11.305x20.495mm_P1.27mm"
		(layer "F.Cu")
		(at 105.791 136.398 90)
		(descr "SSOP, 32 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SSOP SO")
		(property "Reference" "U2"
			(at 0 -11.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "IS61C5128AS-25QLI"
			(at 0 11.2 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "IS61C5128AS-25QLI"
			(at 242.189 30.607 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -6.55 -9.525 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/A18")
			(pinfunction "A17")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -6.55 -8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "/A17")
			(pinfunction "A16")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -6.55 -6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "/A15")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -6.55 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "/A13")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -6.55 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "/A8")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -6.55 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "/A7")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -6.55 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 57 "/A6")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -6.55 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "/A5")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -6.55 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "/A4")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -6.55 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "/A3")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -6.55 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "/A2")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -6.55 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "/A1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -6.55 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "/D0")
			(pinfunction "I/O0")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -6.55 6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 42 "/D1")
			(pinfunction "I/O1")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -6.55 8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/D2")
			(pinfunction "I/O2")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -6.55 9.525 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "17" smd roundrect
			(at 6.55 9.525 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/D3")
			(pinfunction "I/O3")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 6.55 8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "/D4")
			(pinfunction "I/O4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 6.55 6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "/D5")
			(pinfunction "I/O5")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 6.55 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 43 "/D6")
			(pinfunction "I/O6")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 6.55 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/D7")
			(pinfunction "I/O7")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 6.55 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "/SRCE")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 6.55 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "/A11")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 6.55 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "/CAS_0")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 6.55 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "/A12")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 6.55 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "/A10")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 6.55 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 32 "/A9")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 6.55 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "/A14")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at 6.55 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "/SRAM_WE")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at 6.55 -6.985 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "/A19")
			(pinfunction "A18")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at 6.55 -8.255 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "/A16")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at 6.55 -9.525 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SSOP-32_11.305x20.495mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 89.9795 138.2395 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0.102 1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "C1206C104K4RACTU"
			(at 179.959 276.479 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 3 "VBUS")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:SOIC-14_W3.9mm"
		(layer "F.Cu")
		(at 98.9965 120.4595 -90)
		(property "Reference" "U1"
			(at 0 -4.79 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS30"
			(at 0 5.29 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "SN74LS30DR"
			(at -21.463 219.456 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "REF**"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "/A19")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -2.54 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "/A18")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.27 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "/A17")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "/A16")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 1.27 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/A15")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 2.54 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "/A14")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.81 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 3.81 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "Net-(U1-Pad8)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 2.54 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 1.27 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 0 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "/A13")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at -1.27 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "/A12")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -2.54 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -3.81 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "digikey-footprints:SOIC-14_W3.9mm"
		(layer "F.Cu")
		(at 110.1725 120.523 -90)
		(property "Reference" "U3"
			(at 0 -4.79 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS30"
			(at 0 5.29 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "SN74LS30DR"
			(at -10.3505 230.6955 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "REF**"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "/A11")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "2" smd rect
			(at -2.54 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "/A10")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "3" smd rect
			(at -1.27 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "/A9")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "4" smd rect
			(at 0 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/A8")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "5" smd rect
			(at 1.27 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "/A7")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "6" smd rect
			(at 2.54 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/A6")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "7" smd rect
			(at 3.81 2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
		(pad "8" smd rect
			(at 3.81 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "Net-(U3-Pad8)")
			(pintype "output")
			(solder_mask_margin 0.07)
		)
		(pad "9" smd rect
			(at 2.54 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.07)
		)
		(pad "10" smd rect
			(at 1.27 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.07)
		)
		(pad "11" smd rect
			(at 0 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/A5")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "12" smd rect
			(at -1.27 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/A4")
			(pintype "input")
			(solder_mask_margin 0.07)
		)
		(pad "13" smd rect
			(at -2.54 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(solder_mask_margin 0.07)
		)
		(pad "14" smd rect
			(at -3.81 -2.7 270)
			(size 0.55 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.07)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 98.958 114.4905 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0.0885 1.8415 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "C1206C104K4RACTU"
			(at 197.916 228.981 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 4 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Sega CD RAM Cart:MountingHole_6.2mm"
		(layer "F.Cu")
		(at 90.4611 131.7197)
		(descr "Mounting Hole 6.2mm, no annular")
		(tags "mounting hole 6.2mm no annular")
		(property "Reference" "H1"
			(at 0 -7.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 7.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 6.4)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Sega CD RAM Cart:MountingHole_6.2mm"
		(layer "F.Cu")
		(at 160.3111 131.7197)
		(descr "Mounting Hole 6.2mm, no annular")
		(tags "mounting hole 6.2mm no annular")
		(property "Reference" "H2"
			(at 0 -7.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 7.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 6.4)
			(layers "*.Cu" "*.Mask")
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 143.9037 138.1637 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.85 90)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "C1206C104K4RACTU"
			(at 5.74 282.0674 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.0161 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1886784906)
			(net 4 "+5V")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "BU2450SM:BAT_BU2450SM-JJ-G"
		(layer "F.Cu")
		(at 142.7226 119.1641 180)
		(property "Reference" "BT1"
			(at 16.002 -6.223 0)
			(layer "F.SilkS")
		)
		(property "Value" "Battery_Cell"
			(at 0.0635 0.889 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "BU2450SM-JJ-GTR"
			(at 285.4452 238.3282 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr through_hole)
		(fp_text user "+"
			(at 15.367 0.1905 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at -15.1765 0.0635 0)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at -15.1765 0 0)
			(layer "F.Fab")
		)
		(fp_text user "+"
			(at 15.367 0.127 0)
			(layer "F.Fab")
		)
		(pad "N" smd rect
			(at -19.05 0 180)
			(size 5.08 5.08)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "P" smd rect
			(at 19.05 0 180)
			(size 5.08 5.08)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(BT1-PadP)")
			(pinfunction "+")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 90.17 146.558)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -2.794 0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey PN" "RMCF0805FT10K0"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "C:/Users/WindDrake/Desktop/Sega CD Ram Cart/Sega CD RAM Cart.sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 3 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.2083333333)
			(net 65 "/SRCE")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 166.6611 104.25)
		(end 82.8411 104.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.8411 104.25)
		(end 82.8411 164.4857)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 83.6031 165.7557)
		(end 165.8991 165.7557)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.8411 164.4857)
		(end 83.6031 165.7557)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.6611 164.4857)
		(end 166.6611 104.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.8991 165.7557)
		(end 166.6611 164.4857)
		(layer "Edge.Cuts")
	)
	(gr_text "Sega CD Back-up RAM Cart (4Mbit) v1.2\nDesigned by WindDrake with help from Officer_Skidmark\nBased on l_oliveira's original research\ngithub.com/WindDrake/SegaCD_Ramcart"
		(at 83.4898 108.2802 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 166.37 157.554) (xy 83.058 157.554) (xy 83.058 104.4702) (xy 166.37 104.4702)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
		)
		(polygon
			(pts
				(xy 166.37 157.554) (xy 83.058 157.554) (xy 83.058 129.487) (xy 83.058 104.4702) (xy 166.37 104.4702)
			)
		)
	)
)
