(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(D1-DI)")
	(net 3 "+5V")
	(net 4 "Net-(D1-DO)")
	(net 5 "Net-(D2-DO)")
	(net 6 "Net-(D3-DO)")
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 110.49 53.763333 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm")
		(tags "MeasurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J5"
			(at 0 -2 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DO"
			(at 0 2.54 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "led connector.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D3-DO)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "zia_led:zia_led"
		(layer "F.Cu")
		(at 117.292999 52.705 180)
		(property "Reference" "D1"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "APA-106-F5"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Components/LED/COM-12877.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 5mm Package"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*D5.0mm*RGB*")
		(sheetname "/")
		(sheetfile "led connector.kicad_sch")
		(attr smd)
		(pad "1" thru_hole oval
			(at -2.7 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D1-DO)")
			(pinfunction "DO")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at -0.9 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0.9 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 2.7 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D1-DI)")
			(pinfunction "DI")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "zia_led:zia_led"
		(layer "F.Cu")
		(at 129.292999 52.705 180)
		(property "Reference" "D2"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "APA-106-F5"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Components/LED/COM-12877.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 5mm Package"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*D5.0mm*RGB*")
		(sheetname "/")
		(sheetfile "led connector.kicad_sch")
		(attr smd)
		(pad "1" thru_hole oval
			(at -2.7 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D2-DO)")
			(pinfunction "DO")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at -0.9 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0.9 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 2.7 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D1-DO)")
			(pinfunction "DI")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 110.49 49.53 -90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm")
		(tags "MeasurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J1"
			(at 0 -2 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5V"
			(at 0 2.54 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "led connector.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1 2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 110.49 55.88 90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm")
		(tags "MeasurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J3"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 2.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "led connector.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd roundrect
			(at 0 0 90)
			(size 1 2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Wire:SolderWirePad_1x01_SMD_1x2mm"
		(layer "F.Cu")
		(at 110.49 51.646667 90)
		(descr "Wire Pad, Square, SMD Pad,  1mm x 2mm")
		(tags "MeasurementPoint Square SMDPad 1mmx2mm ")
		(property "Reference" "J2"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DI"
			(at 0 2.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "led connector.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd roundrect
			(at 0 0 90)
			(size 1 2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(D1-DI)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "zia_led:zia_led"
		(layer "F.Cu")
		(at 141.292999 52.705 180)
		(property "Reference" "D3"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "APA-106-F5"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Components/LED/COM-12877.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller, 5mm Package"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*D5.0mm*RGB*")
		(sheetname "/")
		(sheetfile "led connector.kicad_sch")
		(attr smd)
		(pad "1" thru_hole oval
			(at -2.7 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(D3-DO)")
			(pinfunction "DO")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at -0.9 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0.9 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 2.7 0 180)
			(size 1.6 2.5)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D2-DO)")
			(pinfunction "DI")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 108.585 48.26)
		(end 147.955 57.15)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 108.585 48.26) (xy 147.955 48.26) (xy 147.955 57.15) (xy 108.585 57.15)
			)
		)
	)
	(embedded_fonts no)
)
