(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "fab/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+5V")
	(net 3 "+3V3")
	(net 4 "/Temperature Sense/RTD1-")
	(net 5 "/Temperature Sense/RTD1+")
	(net 6 "/Temperature Sense/RTD2+")
	(net 7 "/Temperature Sense/RTD2-")
	(net 8 "/Temperature Sense/RTD3-")
	(net 9 "/Temperature Sense/RTD3+")
	(net 10 "Net-(U1-15_A1_RX3_SPDIF_IN)")
	(net 11 "+24V")
	(net 12 "/Temperature Sense/F1-")
	(net 13 "/Temperature Sense/F1+")
	(net 14 "/Temperature Sense/F2+")
	(net 15 "/Temperature Sense/F2-")
	(net 16 "/Temperature Sense/F3-")
	(net 17 "/Temperature Sense/F3+")
	(net 18 "/Relay_heater")
	(net 19 "/Relay2")
	(net 20 "/Pressure_sense")
	(net 21 "Net-(JP1-A)")
	(net 22 "/MISO")
	(net 23 "/nCS_RTD1")
	(net 24 "/nCS_RTD2")
	(net 25 "/nCS_RTD3")
	(net 26 "Net-(U3-BIAS)")
	(net 27 "Net-(U3-ISENSOR)")
	(net 28 "Net-(U4-BIAS)")
	(net 29 "Net-(U4-ISENSOR)")
	(net 30 "Net-(U2-BIAS)")
	(net 31 "Net-(U2-ISENSOR)")
	(net 32 "unconnected-(U1-VBAT-Pad50)")
	(net 33 "unconnected-(U1-17_A3_TX4_SDA1-Pad39)")
	(net 34 "unconnected-(U1-39_MISO1_OUT1A-Pad31)")
	(net 35 "unconnected-(U1-35_TX8-Pad27)")
	(net 36 "unconnected-(U1-D+-Pad57)")
	(net 37 "/MOSI")
	(net 38 "unconnected-(U1-1_TX1_CTX2_MISO1-Pad3)")
	(net 39 "/nDRDY_RTD3")
	(net 40 "unconnected-(U1-ON_OFF-Pad54)")
	(net 41 "unconnected-(U1-4_BCLK2-Pad6)")
	(net 42 "unconnected-(U1-14_A0_TX3_SPDIF_OUT-Pad36)")
	(net 43 "unconnected-(U1-LED-Pad61)")
	(net 44 "unconnected-(U1-31_CTX3-Pad23)")
	(net 45 "unconnected-(U1-20_A6_TX5_LRCLK1-Pad42)")
	(net 46 "unconnected-(U1-6_OUT1D-Pad8)")
	(net 47 "unconnected-(U1-GND-Pad58)")
	(net 48 "unconnected-(U1-3V3-Pad51)")
	(net 49 "unconnected-(U1-40_A16-Pad32)")
	(net 50 "/nDRDY_RTD2")
	(net 51 "unconnected-(U1-T--Pad62)")
	(net 52 "unconnected-(U1-16_A2_RX4_SCL1-Pad38)")
	(net 53 "unconnected-(U1-8_TX2_IN1-Pad10)")
	(net 54 "unconnected-(U1-VUSB-Pad49)")
	(net 55 "unconnected-(U1-21_A7_RX5_BCLK1-Pad43)")
	(net 56 "unconnected-(U1-5V-Pad55)")
	(net 57 "unconnected-(U1-30_CRX3-Pad22)")
	(net 58 "/nDRDY_RTD1")
	(net 59 "unconnected-(U1-18_A4_SDA-Pad40)")
	(net 60 "unconnected-(U1-22_A8_CTX1-Pad44)")
	(net 61 "unconnected-(U1-41_A17-Pad33)")
	(net 62 "unconnected-(U1-T+-Pad63)")
	(net 63 "unconnected-(U1-GND-Pad52)")
	(net 64 "unconnected-(U1-R--Pad65)")
	(net 65 "unconnected-(U1-GND-Pad64)")
	(net 66 "unconnected-(U1-27_A13_SCK1-Pad19)")
	(net 67 "unconnected-(U1-34_RX8-Pad26)")
	(net 68 "unconnected-(U1-GND-Pad59)")
	(net 69 "unconnected-(U1-28_RX7-Pad20)")
	(net 70 "unconnected-(U1-7_RX2_OUT1A-Pad9)")
	(net 71 "unconnected-(U1-R+-Pad60)")
	(net 72 "unconnected-(U1-D+-Pad67)")
	(net 73 "unconnected-(U1-PROGRAM-Pad53)")
	(net 74 "unconnected-(U1-5_IN2-Pad7)")
	(net 75 "unconnected-(U1-23_A9_CRX1_MCLK1-Pad45)")
	(net 76 "unconnected-(U1-D--Pad66)")
	(net 77 "unconnected-(U1-38_CS1_IN1-Pad30)")
	(net 78 "unconnected-(U1-D--Pad56)")
	(net 79 "unconnected-(U1-19_A5_SCL-Pad41)")
	(net 80 "/SCK")
	(net 81 "unconnected-(U1-3_LRCLK2-Pad5)")
	(net 82 "unconnected-(U1-0_RX1_CRX2_CS1-Pad2)")
	(net 83 "unconnected-(U1-25_A11_RX6_SDA2-Pad17)")
	(net 84 "unconnected-(U1-29_TX7-Pad21)")
	(net 85 "unconnected-(U2-N.C.-Pad20)")
	(net 86 "unconnected-(U3-N.C.-Pad20)")
	(net 87 "unconnected-(U4-N.C.-Pad20)")
	(net 88 "unconnected-(U1-24_A10_TX6_SCL2-Pad16)")
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 133.525 39.445 180)
		(descr "Terminal Block Xinya XY308-2.54-2P, 2 pins, pitch 2.54mm, size 5.58x6.5mm^2, drill diameter 1.2mm, pad diameter 2mm, see http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-2P pitch 2.54mm size 5.58x6.5mm^2 drill 1.2mm pad 2mm")
		(property "Reference" "J1"
			(at 1.27 -4.22 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 1.27 4.52 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.15 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+24V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-2P_1x02_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 79.994998 63.46885 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "Rref1"
			(at -0.01 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k, 0.1%"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U3-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U3-ISENSOR)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 79.448802 48.8038 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "Rref3"
			(at -0.011198 1.4538 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k, 0.1%"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U2-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U2-ISENSOR)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 88.11 70.46 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.74 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 22 "/MISO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 53.32 36.68)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 84.978802 54.8963 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -0.227064 1.851198 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 23 "/nCS_RTD1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-4P_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 68.298802 50.2938 -90)
		(descr "Terminal Block Xinya XY308-2.54-4P, 4 pins, pitch 2.54mm, size 10.7x6.5mm^2, drill diameter 1.2mm, pad diameter 2mm, see http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-4P pitch 2.54mm size 10.7x6.5mm^2 drill 1.2mm pad 2mm")
		(property "Reference" "J2"
			(at -2.7138 -2.661198 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x04"
			(at 3.81 4.52 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.15 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Temperature Sense/F1+")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Temperature Sense/RTD1+")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/Temperature Sense/RTD1-")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 7.62 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Temperature Sense/F1-")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-4P_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 82.254998 62.79885 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 1.01885 1.415002 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.22u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 114.09 37.55 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 3.05 -0.27 270)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 79.62 79.65 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "Rref2"
			(at 0.01 1.26 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k, 0.1%"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U4-BIAS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U4-ISENSOR)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 81.89 78.93 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0.63 1.19 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.22u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 124.17 106.585 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Socket"
			(at 0 7.41 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Relay_heater")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 105.09 178.775 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H2"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 109.64 65.51 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 3.22 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U1-15_A1_RX3_SPDIF_IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 60.84 112.365 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H8"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 139.42 112.195 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H3"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 146.55 186.42)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "PDL_kicad_footprints:21-0056C_20_MXM"
		(layer "F.Cu")
		(at 80.334998 68.92885 -90)
		(tags "MAX31865AAP+ ")
		(property "Reference" "U3"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MAX31865AAP+"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/analog-devices-inc-maxim-integrated/MAX31865AAP/5396622"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "21-0056C_20_MXM 21-0056C_20_MXM-M 21-0056C_20_MXM-L")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.75285 -4.499801 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.75285 -4.499801 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.3114 -3.5941 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.3114 -3.5941 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.49885 -2.925 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/nDRDY_RTD2")
			(pinfunction "*DRDY")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -3.49885 -2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3V3")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -3.49885 -1.625001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -3.49885 -0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(U3-BIAS)")
			(pinfunction "BIAS")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -3.49885 -0.325001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(U3-BIAS)")
			(pinfunction "REFIN+")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -3.49885 0.324998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(U3-ISENSOR)")
			(pinfunction "REFIN-")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at -3.49885 0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(U3-ISENSOR)")
			(pinfunction "ISENSOR")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at -3.49885 1.624998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/Temperature Sense/F2+")
			(pinfunction "FORCE+")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at -3.49885 2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "FORCE2")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -3.49885 2.924998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/Temperature Sense/RTD2+")
			(pinfunction "RTDIN+")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 3.49885 2.925 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/Temperature Sense/RTD2-")
			(pinfunction "RTDIN-")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 3.49885 2.275002 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/Temperature Sense/F2-")
			(pinfunction "FORCE-")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 3.49885 1.625001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND2")
			(pintype "power_out")
		)
		(pad "14" smd rect
			(at 3.49885 0.975002 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/MOSI")
			(pinfunction "SDI")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at 3.49885 0.325001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/SCK")
			(pinfunction "SCLK")
			(pintype "unspecified")
		)
		(pad "16" smd rect
			(at 3.49885 -0.324998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/nCS_RTD2")
			(pinfunction "*CS")
			(pintype "unspecified")
		)
		(pad "17" smd rect
			(at 3.49885 -0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/MISO")
			(pinfunction "SDO")
			(pintype "unspecified")
		)
		(pad "18" smd rect
			(at 3.49885 -1.624998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "DGND")
			(pintype "power_out")
		)
		(pad "19" smd rect
			(at 3.49885 -2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "20" smd rect
			(at 3.49885 -2.924998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "unconnected-(U3-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 79.32 91.11)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.86 0.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 25 "/nCS_RTD3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PDL_kicad_footprints:Teensy41"
		(layer "F.Cu")
		(at 98.71 65.5 -90)
		(property "Reference" "U1"
			(at -4.6 -0.434 180)
			(layer "F.SilkS")
		)
		(property "Value" "Teensy4.1"
			(at 0 10.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/sparkfun-electronics/16996/13158152"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr through_hole)
		(fp_text user "USB Host"
			(at -18.4658 2.4892 90)
			(layer "F.SilkS")
		)
		(fp_text user "Micro SD"
			(at 24.13 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "MIMXRT1062"
			(at -1.27 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "Ethernet"
			(at -12.065 -3.2766 0)
			(layer "F.SilkS")
		)
		(fp_text user "USB"
			(at -26.67 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "DVJ6A"
			(at -2.54 -0.18 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole rect
			(at -29.21 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at -26.67 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "unconnected-(U1-0_RX1_CRX2_CS1-Pad2)")
			(pinfunction "0_RX1_CRX2_CS1")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" thru_hole circle
			(at -24.13 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(U1-1_TX1_CTX2_MISO1-Pad3)")
			(pinfunction "1_TX1_CTX2_MISO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" thru_hole circle
			(at -21.59 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/nDRDY_RTD1")
			(pinfunction "2_OUT2")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at -19.05 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "unconnected-(U1-3_LRCLK2-Pad5)")
			(pinfunction "3_LRCLK2")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole circle
			(at -16.51 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(U1-4_BCLK2-Pad6)")
			(pinfunction "4_BCLK2")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole circle
			(at -13.97 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "unconnected-(U1-5_IN2-Pad7)")
			(pinfunction "5_IN2")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole circle
			(at -11.43 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "unconnected-(U1-6_OUT1D-Pad8)")
			(pinfunction "6_OUT1D")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" thru_hole circle
			(at -8.89 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "unconnected-(U1-7_RX2_OUT1A-Pad9)")
			(pinfunction "7_RX2_OUT1A")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" thru_hole circle
			(at -6.35 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(U1-8_TX2_IN1-Pad10)")
			(pinfunction "8_TX2_IN1")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" thru_hole circle
			(at -3.81 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/nDRDY_RTD2")
			(pinfunction "9_OUT1C")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole circle
			(at -1.27 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/nCS_RTD1")
			(pinfunction "10_CS_MQSR")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole circle
			(at 1.27 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/MOSI")
			(pinfunction "11_MOSI_CTX1")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at 3.81 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/MISO")
			(pinfunction "12_MISO_MQSL")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 6.35 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "16" thru_hole circle
			(at 8.89 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "unconnected-(U1-24_A10_TX6_SCL2-Pad16)")
			(pinfunction "24_A10_TX6_SCL2")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" thru_hole circle
			(at 11.43 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "unconnected-(U1-25_A11_RX6_SDA2-Pad17)")
			(pinfunction "25_A11_RX6_SDA2")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" thru_hole circle
			(at 13.97 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/nDRDY_RTD3")
			(pinfunction "26_A12_MOSI1")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at 16.51 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "unconnected-(U1-27_A13_SCK1-Pad19)")
			(pinfunction "27_A13_SCK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" thru_hole circle
			(at 19.05 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "unconnected-(U1-28_RX7-Pad20)")
			(pinfunction "28_RX7")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" thru_hole circle
			(at 21.59 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "unconnected-(U1-29_TX7-Pad21)")
			(pinfunction "29_TX7")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" thru_hole circle
			(at 24.13 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(U1-30_CRX3-Pad22)")
			(pinfunction "30_CRX3")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" thru_hole circle
			(at 26.67 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(U1-31_CTX3-Pad23)")
			(pinfunction "31_CTX3")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole circle
			(at 29.21 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Relay2")
			(pinfunction "32_OUT1B")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 29.21 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Relay_heater")
			(pinfunction "33_MCLK2")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 26.67 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(U1-34_RX8-Pad26)")
			(pinfunction "34_RX8")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" thru_hole circle
			(at 24.13 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(U1-35_TX8-Pad27)")
			(pinfunction "35_TX8")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" thru_hole circle
			(at 21.59 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/nCS_RTD2")
			(pinfunction "36_CS")
			(pintype "bidirectional")
		)
		(pad "29" thru_hole circle
			(at 19.05 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/nCS_RTD3")
			(pinfunction "37_CS")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole circle
			(at 16.51 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "unconnected-(U1-38_CS1_IN1-Pad30)")
			(pinfunction "38_CS1_IN1")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" thru_hole circle
			(at 13.97 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(U1-39_MISO1_OUT1A-Pad31)")
			(pinfunction "39_MISO1_OUT1A")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" thru_hole circle
			(at 11.43 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(U1-40_A16-Pad32)")
			(pinfunction "40_A16")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" thru_hole circle
			(at 8.89 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(U1-41_A17-Pad33)")
			(pinfunction "41_A17")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" thru_hole circle
			(at 6.35 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "35" thru_hole circle
			(at 3.81 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/SCK")
			(pinfunction "13_SCK_LED")
			(pintype "bidirectional")
		)
		(pad "36" thru_hole circle
			(at 1.27 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U1-14_A0_TX3_SPDIF_OUT-Pad36)")
			(pinfunction "14_A0_TX3_SPDIF_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "37" thru_hole circle
			(at -1.27 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(U1-15_A1_RX3_SPDIF_IN)")
			(pinfunction "15_A1_RX3_SPDIF_IN")
			(pintype "bidirectional")
		)
		(pad "38" thru_hole circle
			(at -3.81 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(U1-16_A2_RX4_SCL1-Pad38)")
			(pinfunction "16_A2_RX4_SCL1")
			(pintype "bidirectional+no_connect")
		)
		(pad "39" thru_hole circle
			(at -6.35 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(U1-17_A3_TX4_SDA1-Pad39)")
			(pinfunction "17_A3_TX4_SDA1")
			(pintype "bidirectional+no_connect")
		)
		(pad "40" thru_hole circle
			(at -8.89 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(U1-18_A4_SDA-Pad40)")
			(pinfunction "18_A4_SDA")
			(pintype "bidirectional+no_connect")
		)
		(pad "41" thru_hole circle
			(at -11.43 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "unconnected-(U1-19_A5_SCL-Pad41)")
			(pinfunction "19_A5_SCL")
			(pintype "bidirectional+no_connect")
		)
		(pad "42" thru_hole circle
			(at -13.97 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(U1-20_A6_TX5_LRCLK1-Pad42)")
			(pinfunction "20_A6_TX5_LRCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "43" thru_hole circle
			(at -16.51 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(U1-21_A7_RX5_BCLK1-Pad43)")
			(pinfunction "21_A7_RX5_BCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "44" thru_hole circle
			(at -19.05 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(U1-22_A8_CTX1-Pad44)")
			(pinfunction "22_A8_CTX1")
			(pintype "bidirectional+no_connect")
		)
		(pad "45" thru_hole circle
			(at -21.59 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "unconnected-(U1-23_A9_CRX1_MCLK1-Pad45)")
			(pinfunction "23_A9_CRX1_MCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "46" thru_hole circle
			(at -24.13 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pinfunction "3V3")
			(pintype "output")
		)
		(pad "47" thru_hole circle
			(at -26.67 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "output")
		)
		(pad "48" thru_hole circle
			(at -29.21 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "49" thru_hole circle
			(at -26.67 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(U1-VUSB-Pad49)")
			(pinfunction "VUSB")
			(pintype "power_out+no_connect")
		)
		(pad "50" thru_hole circle
			(at 16.51 5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(U1-VBAT-Pad50)")
			(pinfunction "VBAT")
			(pintype "power_in+no_connect")
		)
		(pad "51" thru_hole circle
			(at 16.51 2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "unconnected-(U1-3V3-Pad51)")
			(pinfunction "3V3")
			(pintype "power_in+no_connect")
		)
		(pad "52" thru_hole circle
			(at 16.51 0 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "unconnected-(U1-GND-Pad52)")
			(pinfunction "GND")
			(pintype "input+no_connect")
		)
		(pad "53" thru_hole circle
			(at 16.51 -2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "unconnected-(U1-PROGRAM-Pad53)")
			(pinfunction "PROGRAM")
			(pintype "input+no_connect")
		)
		(pad "54" thru_hole circle
			(at 16.51 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(U1-ON_OFF-Pad54)")
			(pinfunction "ON_OFF")
			(pintype "input+no_connect")
		)
		(pad "55" thru_hole rect
			(at -22.9108 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(U1-5V-Pad55)")
			(pinfunction "5V")
			(pintype "power_out+no_connect")
		)
		(pad "56" thru_hole circle
			(at -20.3708 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "unconnected-(U1-D--Pad56)")
			(pinfunction "D-")
			(pintype "bidirectional+no_connect")
		)
		(pad "57" thru_hole circle
			(at -17.8308 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(U1-D+-Pad57)")
			(pinfunction "D+")
			(pintype "bidirectional+no_connect")
		)
		(pad "58" thru_hole circle
			(at -15.2908 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(U1-GND-Pad58)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "59" thru_hole circle
			(at -12.7508 4.5692 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(U1-GND-Pad59)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "60" thru_hole rect
			(at -16.24 -5.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "unconnected-(U1-R+-Pad60)")
			(pinfunction "R+")
			(pintype "bidirectional+no_connect")
		)
		(pad "61" thru_hole circle
			(at -16.24 -3.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(U1-LED-Pad61)")
			(pinfunction "LED")
			(pintype "bidirectional+no_connect")
		)
		(pad "62" thru_hole circle
			(at -16.24 -1.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(U1-T--Pad62)")
			(pinfunction "T-")
			(pintype "bidirectional+no_connect")
		)
		(pad "63" thru_hole circle
			(at -14.24 -1.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "unconnected-(U1-T+-Pad63)")
			(pinfunction "T+")
			(pintype "bidirectional+no_connect")
		)
		(pad "64" thru_hole circle
			(at -14.24 -3.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "unconnected-(U1-GND-Pad64)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "65" thru_hole circle
			(at -14.24 -5.1816 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "unconnected-(U1-R--Pad65)")
			(pinfunction "R-")
			(pintype "bidirectional+no_connect")
		)
		(pad "66" thru_hole circle
			(at -28.48 -1.27 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "unconnected-(U1-D--Pad66)")
			(pinfunction "D-")
			(pintype "bidirectional+no_connect")
		)
		(pad "67" thru_hole circle
			(at -28.48 1.27 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "unconnected-(U1-D+-Pad67)")
			(pinfunction "D+")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.1_Assembly.STEP"
			(offset
				(xyz 0 0 0.762)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 118.62 81.53 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "150 0.1%"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/te-connectivity-passive-product/RA73F2A150RBTD/16031816"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Pressure Sense/")
		(sheetfile "pressure_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 21 "Net-(JP1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 109.07 37.53 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 2.8 -0.06 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 111.56 37.56 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.67 -0.18 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 112.79 64.68)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 10 "Net-(U1-15_A1_RX3_SPDIF_IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 20 "/Pressure_sense")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 118.44 76.255 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP1"
			(at 0 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Jumper_2_Open"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "/Pressure Sense/")
		(sheetfile "pressure_sense.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(JP1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Pressure_sense")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 81.748802 48.1438 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.1938 1.32 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.22u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 53.5 186.32)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 60.84 178.925 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H6"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 74.383802 54.1038 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 1.513802 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/Temperature Sense/RTD1+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/Temperature Sense/RTD1-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 123.25 101.625 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0.01 1.985 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 18 "/Relay_heater")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 139.48 178.775 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H1"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 74.82 85.09 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 1.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/Temperature Sense/RTD3+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/Temperature Sense/RTD3-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 75.114998 68.86885 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 1.554998 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/Temperature Sense/RTD2+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/Temperature Sense/RTD2-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_MetzConnect:TerminalBlock_MetzConnect_Type011_RT05504HBWC_1x04_P5.00mm_Horizontal"
		(layer "F.Cu")
		(at 131.75 82.57 90)
		(descr "terminal block Metz Connect Type011_RT05504HBWC, 4 pins, pitch 5mm, size 20x10.5mm^2, drill diamater 1.4mm, pad diameter 2.8mm, see http://www.metz-connect.com/de/system/files/productfiles/Datenblatt_310111_RT055xxHBLC_OFF-022717S.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_MetzConnect")
		(tags "THT terminal block Metz Connect Type011_RT05504HBWC pitch 5mm size 20x10.5mm^2 drill 1.4mm pad 2.8mm")
		(property "Reference" "J7"
			(at 7.5 -7.56 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x04"
			(at 7.5 5.06 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/Pressure Sense/")
		(sheetfile "pressure_sense.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 3.25 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Pressure_sense")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0 90)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3V3")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15 0 90)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+24V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_MetzConnect.3dshapes/TerminalBlock_MetzConnect_Type011_RT05504HBWC_1x04_P5.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PDL_kicad_footprints:21-0056C_20_MXM"
		(layer "F.Cu")
		(at 79.778802 54.2438 -90)
		(tags "MAX31865AAP+ ")
		(property "Reference" "U2"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MAX31865AAP+"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/analog-devices-inc-maxim-integrated/MAX31865AAP/5396622"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "21-0056C_20_MXM 21-0056C_20_MXM-M 21-0056C_20_MXM-L")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.75285 -4.499801 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.75285 -4.499801 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.3114 -3.5941 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.3114 -3.5941 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.49885 -2.925 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "/nDRDY_RTD1")
			(pinfunction "*DRDY")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -3.49885 -2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3V3")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -3.49885 -1.625001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -3.49885 -0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(U2-BIAS)")
			(pinfunction "BIAS")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -3.49885 -0.325001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(U2-BIAS)")
			(pinfunction "REFIN+")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -3.49885 0.324998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(U2-ISENSOR)")
			(pinfunction "REFIN-")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at -3.49885 0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(U2-ISENSOR)")
			(pinfunction "ISENSOR")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at -3.49885 1.624998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/Temperature Sense/F1+")
			(pinfunction "FORCE+")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at -3.49885 2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "FORCE2")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -3.49885 2.924998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/Temperature Sense/RTD1+")
			(pinfunction "RTDIN+")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 3.49885 2.925 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/Temperature Sense/RTD1-")
			(pinfunction "RTDIN-")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 3.49885 2.275002 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/Temperature Sense/F1-")
			(pinfunction "FORCE-")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 3.49885 1.625001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND2")
			(pintype "power_out")
		)
		(pad "14" smd rect
			(at 3.49885 0.975002 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/MOSI")
			(pinfunction "SDI")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at 3.49885 0.325001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/SCK")
			(pinfunction "SCLK")
			(pintype "unspecified")
		)
		(pad "16" smd rect
			(at 3.49885 -0.324998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "/nCS_RTD1")
			(pinfunction "*CS")
			(pintype "unspecified")
		)
		(pad "17" smd rect
			(at 3.49885 -0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/MISO")
			(pinfunction "SDO")
			(pintype "unspecified")
		)
		(pad "18" smd rect
			(at 3.49885 -1.624998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "DGND")
			(pintype "power_out")
		)
		(pad "19" smd rect
			(at 3.49885 -2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "20" smd rect
			(at 3.49885 -2.924998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(U2-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-4P_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 68.384998 64.52885 -90)
		(descr "Terminal Block Xinya XY308-2.54-4P, 4 pins, pitch 2.54mm, size 10.7x6.5mm^2, drill diameter 1.2mm, pad diameter 2mm, see http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-4P pitch 2.54mm size 10.7x6.5mm^2 drill 1.2mm pad 2mm")
		(property "Reference" "J3"
			(at -2.56885 -2.725002 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x04"
			(at 3.81 4.52 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.15 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Temperature Sense/F2+")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Temperature Sense/RTD2+")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Temperature Sense/RTD2-")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 7.62 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Temperature Sense/F2-")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-4P_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 105.14 112.155 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H4"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 95.14 178.915 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H5"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 132.7 46.57)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "C13"
			(at -0.11 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "+24V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 95.17 112.365 180)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "H7"
			(at 0 -4.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection for relay module board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 79.63 75.06)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.8 0.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 3 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 24 "/nCS_RTD2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PDL_kicad_footprints:21-0056C_20_MXM"
		(layer "F.Cu")
		(at 80.07 85.09 -90)
		(tags "MAX31865AAP+ ")
		(property "Reference" "U4"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MAX31865AAP+"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/analog-devices-inc-maxim-integrated/MAX31865AAP/5396622"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "21-0056C_20_MXM 21-0056C_20_MXM-M 21-0056C_20_MXM-L")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -3.75285 -4.499801 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.75285 -4.499801 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.3114 -3.5941 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.3114 -3.5941 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.49885 -2.925 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/nDRDY_RTD3")
			(pinfunction "*DRDY")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -3.49885 -2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3V3")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -3.49885 -1.625001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -3.49885 -0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U4-BIAS)")
			(pinfunction "BIAS")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -3.49885 -0.325001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(U4-BIAS)")
			(pinfunction "REFIN+")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -3.49885 0.324998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(U4-ISENSOR)")
			(pinfunction "REFIN-")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at -3.49885 0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(U4-ISENSOR)")
			(pinfunction "ISENSOR")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at -3.49885 1.624998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/Temperature Sense/F3+")
			(pinfunction "FORCE+")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at -3.49885 2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "FORCE2")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -3.49885 2.924998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/Temperature Sense/RTD3+")
			(pinfunction "RTDIN+")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at 3.49885 2.925 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/Temperature Sense/RTD3-")
			(pinfunction "RTDIN-")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at 3.49885 2.275002 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/Temperature Sense/F3-")
			(pinfunction "FORCE-")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 3.49885 1.625001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND2")
			(pintype "power_out")
		)
		(pad "14" smd rect
			(at 3.49885 0.975002 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/MOSI")
			(pinfunction "SDI")
			(pintype "unspecified")
		)
		(pad "15" smd rect
			(at 3.49885 0.325001 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/SCK")
			(pinfunction "SCLK")
			(pintype "unspecified")
		)
		(pad "16" smd rect
			(at 3.49885 -0.324998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/nCS_RTD3")
			(pinfunction "*CS")
			(pintype "unspecified")
		)
		(pad "17" smd rect
			(at 3.49885 -0.974999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/MISO")
			(pinfunction "SDO")
			(pintype "unspecified")
		)
		(pad "18" smd rect
			(at 3.49885 -1.624998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "DGND")
			(pintype "power_out")
		)
		(pad "19" smd rect
			(at 3.49885 -2.274999 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "20" smd rect
			(at 3.49885 -2.924998 270)
			(size 1.6129 0.4318)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "unconnected-(U4-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "PDL_kicad_footprints:CONV_R-78K5.0-2.0L"
		(layer "F.Cu")
		(at 121.62 46.9475)
		(property "Reference" "PS1"
			(at 0.2 -2.8075 0)
			(layer "F.SilkS")
		)
		(property "Value" "R-78K5.0-2.0L"
			(at 5.415 -12.225 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/recom-power/R-78K5-0-2-0L/21284879"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "945-R-78K5.0-2.0L-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/R-78K5.0-2.0L/Recom+Power/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "9.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/R-78K5.0-2.0L/Recom+Power/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Recom Power"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "R-78K5.0-2.0L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "2A DC/DC-Converter 'INNOLINE' SIP3 reg"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Recom Power"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 2.54 -9.93)
			(size 2.175 2.175)
			(drill 1.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "+24V")
			(pinfunction "+VIN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 -9.93)
			(size 2.175 2.175)
			(drill 1.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -2.54 -9.93)
			(size 2.175 2.175)
			(drill 1.45)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "+VOUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock:TerminalBlock_Xinya_XY308-2.54-4P_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 68.35 81.14 -90)
		(descr "Terminal Block Xinya XY308-2.54-4P, 4 pins, pitch 2.54mm, size 10.7x6.5mm^2, drill diameter 1.2mm, pad diameter 2mm, see http://www.xinyaelectronic.com/product/xy308-254, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Xinya")
		(tags "THT Terminal Block Xinya XY308-2.54-4P pitch 2.54mm size 10.7x6.5mm^2 drill 1.2mm pad 2mm")
		(property "Reference" "J4"
			(at -2.92 -2.91 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x04"
			(at 3.81 4.52 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/Temperature Sense/")
		(sheetfile "temp_sense.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.15 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/Temperature Sense/F3+")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Temperature Sense/RTD3+")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Temperature Sense/RTD3-")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 7.62 0 270)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Temperature Sense/F3-")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Xinya_XY308-2.54-4P_1x04_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 79.74 106.085 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Socket"
			(at 0 7.41 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Relays/")
		(sheetfile "relays.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Relay2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 146.66 36.68)
		(descr "Mounting Hole 3.2mm, no annular, M3")
		(tags "mounting hole 3.2mm no annular m3")
		(property "Reference" "REF**"
			(at 0 -4.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 78.76 101.195 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 1.585 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Autoclave DAQ.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 19 "/Relay2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PDL_kicad_footprints:calcifer_silkscreen"
		(layer "B.Cu")
		(at 97.99 147.39 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_rect
		(start 49.14 32.32)
		(end 150.83 190.59)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "F+"
		(at 64.05 65.15 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 137.24 83.8 90)
		(layer "F.SilkS")
	)
	(gr_text "Relay"
		(at 78.52 103.96 0)
		(layer "F.SilkS")
	)
	(gr_text "RTD1"
		(at 65.578802 48.4138 0)
		(layer "F.SilkS")
	)
	(gr_text "RTD+"
		(at 64.08 68.51 90)
		(layer "F.SilkS")
	)
	(gr_text "RTD3"
		(at 65.89 78.7 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 117.76 104.89 0)
		(layer "F.SilkS")
	)
	(gr_text "RTD2"
		(at 65.65 62.27 0)
		(layer "F.SilkS")
	)
	(gr_text "Vout"
		(at 137 78.82 90)
		(layer "F.SilkS")
	)
	(gr_text "3v3"
		(at 137.1 73.65 90)
		(layer "F.SilkS")
	)
	(gr_text "RTD+"
		(at 64.2 85.18 90)
		(layer "F.SilkS")
	)
	(gr_text "Relay"
		(at 122.9 104.88 0)
		(layer "F.SilkS")
	)
	(gr_text "RTD-"
		(at 63.91 57.02 90)
		(layer "F.SilkS")
	)
	(gr_text "RTD-"
		(at 64.32 88.25 90)
		(layer "F.SilkS")
	)
	(gr_text "F-"
		(at 64.23 73.72 90)
		(layer "F.SilkS")
	)
	(gr_text "24V"
		(at 131.61 34.37 180)
		(layer "F.SilkS")
	)
	(gr_text "F-"
		(at 63.94 59.16 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 120.81 104.96 0)
		(layer "F.SilkS")
	)
	(gr_text "24V"
		(at 137.29 68.72 90)
		(layer "F.SilkS")
	)
	(gr_text "RTD+"
		(at 63.79 53.95 90)
		(layer "F.SilkS")
	)
	(gr_text "Autoclave pressure and temperature DAQ\nDesigned by Hannah Xiao 2/26/2026\nPlasma and Dielectrics Lab"
		(at 57.97 38.56 0)
		(layer "F.SilkS")
	)
	(gr_text "Heater Power"
		(at 140.65 137.27 270)
		(layer "F.SilkS")
	)
	(gr_text "F-"
		(at 64.35 90.39 90)
		(layer "F.SilkS")
	)
	(gr_text "F+"
		(at 63.76 50.59 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 134.84 34.37 180)
		(layer "F.SilkS")
	)
	(gr_text "F+"
		(at 64.17 81.82 90)
		(layer "F.SilkS")
	)
	(gr_text "Pressure sensor"
		(at 125.19 65.009 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 72.61 104.08 0)
		(layer "F.SilkS")
	)
	(gr_text "RTD-"
		(at 64.2 71.58 90)
		(layer "F.SilkS")
	)
	(gr_text "Relay 2"
		(at 58.81 152.65 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 76.23 104.06 0)
		(layer "F.SilkS")
	)
	(gr_text "Align relay mounting holes to corners"
		(at 121.98 121.305 270)
		(layer "User.1")
	)
	(gr_text "Align relay mounting holes to corners"
		(at 75.84 120.395 270)
		(layer "User.1")
	)
	(zone
		(net 3)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.1)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 83.068802 48.2238) (xy 81.278802 48.2338) (xy 81.168802 51.6238) (xy 82.328802 51.5838) (xy 82.328802 49.7238)
				(xy 83.168802 49.6938)
			)
		)
	)
	(zone
		(net 11)
		(net_name "+24V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.67 34.87) (xy 124.04 70.18) (xy 133.66 70.3) (xy 132.32 46.61) (xy 131.92 34.9)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.1)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 83.674998 62.86885) (xy 81.754998 62.97885) (xy 81.744998 66.34885) (xy 82.844998 66.30885)
				(xy 82.854998 64.21885) (xy 83.824998 64.20885)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.1)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 44.96 31.73) (xy 44.39 188.74) (xy 154.76 189.03) (xy 154.76 30.31)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.1)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 83.08 78.97) (xy 81.49 79.15) (xy 81.47 82.44) (xy 82.59 82.46) (xy 82.57 80.27) (xy 83.46 80.16)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.49 31.69) (xy 104.86 37.67) (xy 116.16 37.62) (xy 117.45 39.09) (xy 120.46 39.07) (xy 120.34 31.51)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 44.74 30.73) (xy 155.07 30.73) (xy 155.07 190.23) (xy 43.74 189.98) (xy 44.49 189.98) (xy 44.49 30.98)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.446051 31.646844) (xy 104.86 37.66) (xy 116.21 37.6) (xy 117.58 39.03) (xy 120.45 39.09)
				(xy 120.52 34.57) (xy 137.59 34.55) (xy 137.01 96.8) (xy 74.91 98.21) (xy 75.31 108.29) (xy 154.95 108.7)
				(xy 154.718523 31.366663)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3V3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 45.23 31.7) (xy 154.72 31.86) (xy 154.11 188.97) (xy 44.63 189.57)
			)
		)
	)
	(zone
		(net 11)
		(net_name "+24V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.535891 35.22) (xy 137.09 35.22) (xy 137.09 70.23479) (xy 124.003184 70.018479)
			)
		)
	)
	(embedded_fonts no)
)
