(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "NES-CPU-11")
		(rev "11")
		(company "Nintendo Co., LTD")
		(comment 4 "Nintendo Entertainment System (NES) Motherboard")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(aux_axis_origin 39.7 143.075)
		(grid_origin 39.7 143.075)
		(pcbplotparams
			(layerselection 0x00010f0_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "ONES-CPU-01 Gerbers/")
		)
	)
	(net 0 "")
	(net 1 "/GND")
	(net 2 "/M2")
	(net 3 "/VCC")
	(net 4 "Net-(P6-Pin_4)")
	(net 5 "Net-(U10-SEED)")
	(net 6 "Net-(P3-Pin_5)")
	(net 7 "Net-(P6-Pin_5)")
	(net 8 "/ALE")
	(net 9 "/PPU-CLK")
	(net 10 "/VIDEO")
	(net 11 "Net-(C6-Pad2)")
	(net 12 "Net-(C7-Pad2)")
	(net 13 "Net-(Q2-B)")
	(net 14 "Net-(Q2-C)")
	(net 15 "/EXP-AUDIO-OUT")
	(net 16 "Net-(C20-Pad1)")
	(net 17 "unconnected-(P2-Pad46)")
	(net 18 "/4017-D0")
	(net 19 "/4017-D3")
	(net 20 "/4017-D4")
	(net 21 "/~{OE1}")
	(net 22 "/4016-D0")
	(net 23 "/4016-D3")
	(net 24 "/4016-D4")
	(net 25 "Net-(C41-Pad1)")
	(net 26 "Net-(Q1-B)")
	(net 27 "/CPU-CLK")
	(net 28 "/SYSTEM-CLK")
	(net 29 "/CIC-TO-MB")
	(net 30 "/CIC-TO-CART")
	(net 31 "Net-(R1-Pad1)")
	(net 32 "/EXP-VIDEO")
	(net 33 "/SOUND-2")
	(net 34 "/SOUND-1")
	(net 35 "Net-(R5-Pad1)")
	(net 36 "/EXP-AUDIO-IN")
	(net 37 "/~{NMI}")
	(net 38 "Net-(U10-DATA_IN)")
	(net 39 "/4016-D2")
	(net 40 "/4016-D1")
	(net 41 "/~{IRQ}")
	(net 42 "/4017-D2")
	(net 43 "/4017-D1")
	(net 44 "/PPU-A13")
	(net 45 "/CPU-A8")
	(net 46 "/CPU-D2")
	(net 47 "/CPU-A9")
	(net 48 "/CPU-D1")
	(net 49 "/CPU-R~{W}")
	(net 50 "/CPU-D0")
	(net 51 "/CPU-A0")
	(net 52 "/CPU-A10")
	(net 53 "/CPU-A1")
	(net 54 "/WRAM-~{CE}")
	(net 55 "/CPU-A2")
	(net 56 "/CPU-D7")
	(net 57 "/CPU-A3")
	(net 58 "/CPU-D6")
	(net 59 "/CPU-A4")
	(net 60 "/CPU-D5")
	(net 61 "/CPU-A5")
	(net 62 "/CPU-D4")
	(net 63 "/CPU-A6")
	(net 64 "/CPU-D3")
	(net 65 "/CPU-A7")
	(net 66 "/PPU-A1")
	(net 67 "/PPU-A0")
	(net 68 "/PPU-D0")
	(net 69 "/PPU-A7")
	(net 70 "/PPU-D2")
	(net 71 "/PPU-D7")
	(net 72 "/PPU-A2")
	(net 73 "/PPU-D5")
	(net 74 "/PPU-A4")
	(net 75 "/PPU-A5")
	(net 76 "/PPU-D4")
	(net 77 "/PPU-A3")
	(net 78 "/PPU-D6")
	(net 79 "/PPU-D3")
	(net 80 "/PPU-A6")
	(net 81 "/PPU-D1")
	(net 82 "/CPU-A15")
	(net 83 "/PPU-~{CE}")
	(net 84 "Net-(U10-DATA_OUT)")
	(net 85 "/CPU-A14")
	(net 86 "/CPU-A13")
	(net 87 "/~{ROMSEL}")
	(net 88 "/PPU-A8")
	(net 89 "/PPU-A9")
	(net 90 "/PPU-~{WE}")
	(net 91 "/PPU-~{RD}")
	(net 92 "/VRAM-A10")
	(net 93 "/VRAM-~{CE}")
	(net 94 "/PPU-A10")
	(net 95 "/PPU-A11")
	(net 96 "/PPU-A12")
	(net 97 "/~{RST}")
	(net 98 "unconnected-(U3B-O0-Pad12)")
	(net 99 "/OUT-1")
	(net 100 "/OUT-2")
	(net 101 "/CPU-A12")
	(net 102 "/CPU-A11")
	(net 103 "unconnected-(U3A-O2-Pad6)")
	(net 104 "unconnected-(U3B-O2-Pad10)")
	(net 105 "/PPU-~{A13}")
	(net 106 "unconnected-(U3A-O3-Pad7)")
	(net 107 "/CIC-CLK")
	(net 108 "Net-(U3A-E)")
	(net 109 "/CIC-RST")
	(net 110 "/+9V")
	(net 111 "/AUDIO")
	(net 112 "/EXP-0")
	(net 113 "/EXP-1")
	(net 114 "/EXP-2")
	(net 115 "/EXP-3")
	(net 116 "/EXP-4")
	(net 117 "/EXP-9")
	(net 118 "/EXP-7")
	(net 119 "/EXP-6")
	(net 120 "/EXP-5")
	(net 121 "/EXP-8")
	(net 122 "unconnected-(U7-~{3Y}-Pad7)")
	(net 123 "/~{OE2}")
	(net 124 "/OUT-0")
	(net 125 "unconnected-(U8-~{3Y}-Pad7)")
	(net 126 "Net-(U10-CLK_IN)")
	(net 127 "unconnected-(U10-NC-Pad5)")
	(net 128 "Net-(C23-Pad2)")
	(net 129 "unconnected-(X1-Pad3)")
	(net 130 "unconnected-(X1-Pad3)_1")
	(net 131 "unconnected-(X1-Pad3)_2")
	(footprint "Capacitor_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 221.275 58.05 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor")
		(property "Reference" "BC1"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "103-25"
			(at 2.375 2.4 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D6.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 194.05 41.475 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor")
		(property "Reference" "BC2"
			(at 2.55 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "103-25"
			(at 2.35 -2.15 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D6.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 192.75 118.575 180)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 1.375 -3.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 1.275 -5.2 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 167.35 122.825 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C2"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at -3.85 0.025 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 69.3799 117.0781 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C3"
			(at 2.5031 0.0701 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 211.45 117.475 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C4"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.55 2.5 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "/AUDIO")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 206.5 114.325 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
		(property "Reference" "C5"
			(at 1.15 -2.075 0)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 1.25 2.25 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/VIDEO")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 196.75 110.325 90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C6"
			(at -3.275 2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at -3.175 4.275 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(C6-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 196.75 100.875 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C7"
			(at -2.525 1.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at -4.1 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 183 112.575 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
		(property "Reference" "C8"
			(at 2.5 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 2.225 2.05 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(P6-Pin_4)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 185.325 118.5 180)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C9"
			(at 1.25 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 1.175 -5.275 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/CIC-TO-MB")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U10-SEED)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 163.45 106.075 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C10"
			(at 2.5 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 224.25 100.825 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C11"
			(at 2.5 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 3.364 -2.515 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(P3-Pin_5)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 224.25 97.825 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C12"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/+9V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 59.7279 82.369 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C13"
			(at 2.5279 0.044 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at -3.7021 0.024 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 217.25 91.325)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C14"
			(at 2.45 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(P3-Pin_5)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 217.25 86.325)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C15"
			(at 2.5 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/+9V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 217.25 81.325)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C16"
			(at 2.45 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.45 -0.075 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 217.3 76.325)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C17"
			(at 2.45 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(P6-Pin_4)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 217.3 71.325)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C18"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(P6-Pin_5)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 212.25 88.325 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C19"
			(at 2.45 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 203.25 80.325)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C20"
			(at -2.464 -0.015 0)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at 1.376 -1.785 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/EXP-AUDIO-OUT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 195.75 80.325)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C21"
			(at -2.274 0.495 0)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at 1.366 -1.785 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 114.45 121.075 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C22"
			(at 2.5 -0.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 191.2 78.325 180)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C23"
			(at 5.524 -0.035 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 1.25 3.75 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(C23-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 187 88.325 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C24"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at -2.955 -0.034 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 59.7279 78.8765 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C25"
			(at 2.5 -0.1985 0)
			(layer "F.SilkS")
		)
		(property "Value" "(Unused)"
			(at 9.7779 0.0015 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 2.5 -0.1985 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 230.975 63.1 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C26"
			(at 2.5 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.45 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 227.2028 57.27634 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C27"
			(at 1.3028 -1.92366 0)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 5.8928 0.00134 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 227.17486 54.77444 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C28"
			(at 4.92486 -0.07556 0)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 6.20486 0.00944 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 227.19772 52.27508 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C29"
			(at 4.89772 0.05008 0)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 6.07772 0.03008 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/4017-D0")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 227.19772 49.77318 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C30"
			(at 4.87272 -0.07682 0)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 1.49772 4.89818 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/4017-D3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 227.19836 47.27636 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C31"
			(at 4.92336 0.20136 0)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 5.84836 0.06136 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27336 -0.02364 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/4017-D4")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 112.7 89.575 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C32"
			(at 2.5 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 2.5 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 212 34.075 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C33"
			(at 1.265 -1.926 90)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 1.25 2.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 209.5 34.075 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C34"
			(at 5.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 1.25 2.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 207 34.075 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C35"
			(at 5.325 0.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 1.25 2.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/4016-D0")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 204.5 34.075 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C36"
			(at 5.25 -0.025 90)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 1.25 2.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/4016-D3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 202 34.075 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C37"
			(at 1.075 2.175 90)
			(layer "F.SilkS")
		)
		(property "Value" "330pF"
			(at 1.025 -15.25 180)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4016-D4")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 200.25 43.825 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C38"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.625 -2.175 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 129.316 101.81 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C39"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 2.5 -2.17 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 185.6 52.725 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C40"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 7.975 0.025 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 87.2 44.075 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3mm width 2mm Capacitor")
		(property "Reference" "C41"
			(at 1.25 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "18pF"
			(at 1.25 2.25 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(C41-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(Q2-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
		(layer "F.Cu")
		(at 63.9 50.075)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
		(property "Reference" "C42"
			(at 4.875 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "15pF"
			(at 5.325 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(Q2-C)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
		(layer "F.Cu")
		(at 74.95 44.425 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
		(property "Reference" "C43"
			(at 1.25 -2.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "51pF"
			(at 1.25 2.3 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(Q2-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 59.05 57.575 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C44"
			(at 4.875 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at 0.95 -2 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/SYSTEM-CLK")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/CPU-CLK")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
		(layer "F.Cu")
		(at 73.2 63.573)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
		(property "Reference" "C45"
			(at -2.725 0.077 0)
			(layer "F.SilkS")
		)
		(property "Value" "51pF"
			(at 5.75 -0.023 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(Q2-C)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/PPU-CLK")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 63.9189 61.8712 180)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
		(property "Reference" "C46"
			(at 2.5189 -0.1038 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 2.6939 -2.0538 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 176.95 116.4 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
		(property "Reference" "D1"
			(at 5.16 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "?"
			(at 5.08 2.12 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at -1.7 0 180)
			(layer "F.SilkS")
		)
		(fp_text user " "
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.38 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 11.9 -0.075 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/CIC-TO-MB")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 171.45 116.4 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
		(property "Reference" "D2"
			(at 5.41 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "?"
			(at 5.08 2.12 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_THT:D_DO-35_SOD27_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user " "
			(at 11.875 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at -1.75 -0.05 180)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at -1.75 -0.05 180)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 5.38 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/CIC-TO-CART")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Array_SIP7"
		(layer "F.Cu")
		(at 210.14 49.925 180)
		(descr "7-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "DA1"
			(at 8.64 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "DAN601"
			(at -4.41 0 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Array_SIP7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/4016-D0")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/4016-D3")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4016-D4")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP7.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Array_SIP7"
		(layer "F.Cu")
		(at 210.14 53.425 180)
		(descr "7-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "DA2"
			(at 8.89 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "UPA64H"
			(at -4.71 -0.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Array_SIP7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/4016-D0")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/4016-D3")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4016-D4")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP7.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Array_SIP7"
		(layer "F.Cu")
		(at 210.15 63.2 180)
		(descr "7-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "DA3"
			(at 18.425 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DAN601"
			(at -4.825 0.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Array_SIP7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/4017-D0")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/4017-D3")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/4017-D4")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP7.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Array_SIP7"
		(layer "F.Cu")
		(at 210.15 66.725 180)
		(descr "7-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "DA4"
			(at 18.45 0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "UPA64H"
			(at -5.025 -0.025 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Array_SIP7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/4017-D0")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/4017-D3")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/4017-D4")
			(pintype "output")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP7.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 211.5 97.865 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "FC1"
			(at 5.06 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "39uH"
			(at 5.07 -2.42 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/EXP-AUDIO-OUT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "/AUDIO")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 208 97.865 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "FC2"
			(at 5.06 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "Ferrite_Coil"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/EXP-VIDEO")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/VIDEO")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NESRE:Mod_RF"
		(layer "F.Cu")
		(at 205.846 122.119)
		(property "Reference" "P3"
			(at 0.01 4.741 0)
			(layer "F.SilkS")
		)
		(property "Value" "MOD RF"
			(at 6.224 -1.314 0)
			(layer "F.Fab")
		)
		(property "Footprint" "NESRE:Mod_RF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 2.156)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/VIDEO")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4 2.156)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "/AUDIO")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 8 2.156)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 12 2.156)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/+9V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 16 2.156)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(P3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -6.23 5.1)
			(size 4.25 9.25)
			(drill oval 1.16 5.12)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at -6.23 15.9)
			(size 4.25 9.25)
			(drill oval 1.16 5.12)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 22.344 -2.275 90)
			(size 4.25 9.25)
			(drill oval 1.16 5.62)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 22.344 16.575 90)
			(size 4.25 9.25)
			(drill oval 1.16 5.62)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
	)
	(footprint "NESRE:TO-126-3_Vertical_Short"
		(layer "F.Cu")
		(at 195.15 71.325)
		(descr "TO-126-3, Vertical, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf")
		(tags "TO-126-3 Vertical RM 2.54mm")
		(property "Reference" "Q1"
			(at -2.814 -0.215 0)
			(layer "F.SilkS")
		)
		(property "Value" "2SA937"
			(at 2.54 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "NESRE:TO-126-3_Vertical_Short"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -3.12 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/EXP-VIDEO")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(model "${KIPRJMOD}/Libraries/TO-126-3_Vertical_short.step"
			(offset
				(xyz 0.1 2 4.5)
			)
			(scale
				(xyz 1.1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "NESRE:TO-126-3_Vertical_Short"
		(layer "F.Cu")
		(at 63.7 44.425)
		(descr "TO-126-3, Vertical, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf")
		(tags "TO-126-3 Vertical RM 2.54mm")
		(property "Reference" "Q2"
			(at 2.54 -3.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "2SC2021"
			(at 2.54 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "NESRE:TO-126-3_Vertical_Short"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -3.12 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(Q2-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/Libraries/TO-126-3_Vertical_short.step"
			(offset
				(xyz 0.1 2 4.5)
			)
			(scale
				(xyz 1.1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "NESRE:TO-126-3_Vertical_Short"
		(layer "F.Cu")
		(at 63.341 55.135)
		(descr "TO-126-3, Vertical, RM 2.54mm, see https://www.diodes.com/assets/Package-Files/TO126.pdf")
		(tags "TO-126-3 Vertical RM 2.54mm")
		(property "Reference" "Q3"
			(at 2.54 -3.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "2SC2021"
			(at 2.54 2.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "NESRE:TO-126-3_Vertical_Short"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 -3.12 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/SYSTEM-CLK")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.8 1.8)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(Q2-C)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KIPRJMOD}/Libraries/TO-126-3_Vertical_short.step"
			(offset
				(xyz 0.1 2 4.5)
			)
			(scale
				(xyz 1.1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 193.05 111.075 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 12.5 0.05 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(R1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 212 94.575 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.1 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "510"
			(at 5.084 2.085 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/EXP-VIDEO")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 60.7 117.035 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.225 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/SOUND-2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 56.6926 117.05 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.225 0.0074 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 4.725 -2.6176 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/SOUND-1")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 209.5 80.325 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.15 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "220"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(R5-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(P6-Pin_5)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 195.59 76.375)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.01 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "47K"
			(at 8.36 -2.325 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(C20-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/EXP-AUDIO-OUT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 97.575 73.65)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 5.08 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "20K"
			(at -3.075 0.05 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/SOUND-1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(C23-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 97.575 76.8)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 5.08 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "12K"
			(at -3.075 0.05 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/SOUND-2")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(C23-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 97.575 70.525)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 5.075 0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "20K"
			(at -3.075 0.025 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/EXP-AUDIO-IN")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(C23-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 77.05 49.9 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at 5.175 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "220K"
			(at 5.075 -2.3 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(Q2-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(Q2-C)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 73.95 60.075 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R11"
			(at 5.1 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.2K"
			(at 5.1 -2.15 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(Q2-C)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 59.75 55.185 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R12"
			(at 5.1 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "510"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/SYSTEM-CLK")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 56.55 55.175 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at 5.1 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "150K"
			(at 5 -2.375 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/CPU-CLK")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 189.2 41.65 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R14"
			(at 5.05 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.6K"
			(at 5.075 -2.15 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 116.29116 47.571)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R16"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 5.08 -2.146 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/~{NMI}")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 186.59 113.725)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R17"
			(at 5.06 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2K"
			(at 0.86 -2.125 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(R1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(C6-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 179.7 126.575 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R18"
			(at 5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at -2.2 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/CIC-TO-MB")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U10-DATA_IN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 174.2 126.575 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R19"
			(at 5.25 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at -2.2 -0.075 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/CIC-TO-CART")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "Net-(U10-DATA_OUT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Array_SIP13"
		(layer "F.Cu")
		(at 156.93 47.575 180)
		(descr "13-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RA1"
			(at 0.98 -2.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "12 x 10K"
			(at 16.51 2.4 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Array_SIP13"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R?Array?SIP*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 15.24 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "common")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/4017-D1")
			(pinfunction "R1")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/4017-D0")
			(pinfunction "R2")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/4017-D4")
			(pinfunction "R3")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/4017-D3")
			(pinfunction "R4")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 12.7 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/4017-D2")
			(pinfunction "R5")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 15.24 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/~{IRQ}")
			(pinfunction "R6")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 17.78 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/4016-D1")
			(pinfunction "R7")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 20.32 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/4016-D0")
			(pinfunction "R8")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 22.86 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/4016-D3")
			(pinfunction "R9")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 25.4 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4016-D4")
			(pinfunction "R10")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 27.94 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/4016-D2")
			(pinfunction "R11")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 30.48 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/~{NMI}")
			(pinfunction "R12")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP13.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Array_SIP5"
		(layer "F.Cu")
		(at 106.11 81.325 180)
		(descr "5-pin Resistor SIP pack")
		(tags "R")
		(property "Reference" "RA2"
			(at 10.585 -2.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "4 x 6.8K"
			(at 5.135 -2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Array_SIP5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.vishay.com/docs/31509/csc.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R?Array?SIP*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "common")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pinfunction "R1")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PPU-A13")
			(pinfunction "R2")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pinfunction "R3")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pinfunction "R4")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NESRE:TrimmerCap-THT"
		(layer "F.Cu")
		(at 80.15 49.925 90)
		(property "Reference" "TC1"
			(at 2.8 1.925 90)
			(layer "F.SilkS")
		)
		(property "Value" "30pF"
			(at 2.925 -1.35 90)
			(layer "F.SilkS")
		)
		(property "Footprint" "NESRE:TrimmerCap-THT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 0 2 90)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(Q2-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.75 2 90)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(C41-Pad1)")
			(pintype "passive")
		)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm"
		(layer "F.Cu")
		(at 134.176 103.578 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "74HC373"
			(at 3.81 25.19 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.cl.cam.ac.uk/teaching//2003/Hardware/datasheets/ht6116.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/PPU-A6")
			(pinfunction "Q0")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/PPU-D6")
			(pinfunction "D0")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/PPU-D4")
			(pinfunction "D1")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/PPU-A4")
			(pinfunction "Q1")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/PPU-A2")
			(pinfunction "Q2")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/PPU-D2")
			(pinfunction "D2")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/PPU-D0")
			(pinfunction "D3")
			(pintype "input")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/PPU-A0")
			(pinfunction "Q3")
			(pintype "output")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/ALE")
			(pinfunction "LE")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/PPU-A1")
			(pinfunction "Q4")
			(pintype "output")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/PPU-D1")
			(pinfunction "D4")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/PPU-D3")
			(pinfunction "D5")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/PPU-A3")
			(pinfunction "Q5")
			(pintype "output")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/PPU-A5")
			(pinfunction "Q6")
			(pintype "output")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/PPU-D5")
			(pinfunction "D6")
			(pintype "input")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/PPU-D7")
			(pinfunction "D7")
			(pintype "input")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/PPU-A7")
			(pinfunction "Q7")
			(pintype "output")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-16_W7.62mm"
		(layer "F.Cu")
		(at 57.9 74.775 90)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "74HC139"
			(at 3.81 20.11 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS139"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(U3A-E)")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/CPU-A13")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/CPU-A14")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/WRAM-~{CE}")
			(pinfunction "O0")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/PPU-~{CE}")
			(pinfunction "O1")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "unconnected-(U3A-O2-Pad6)")
			(pinfunction "O2")
			(pintype "output+no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "unconnected-(U3A-O3-Pad7)")
			(pinfunction "O3")
			(pintype "output+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/~{ROMSEL}")
			(pinfunction "O3")
			(pintype "output")
		)
		(pad "10" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "unconnected-(U3B-O2-Pad10)")
			(pinfunction "O2")
			(pintype "output+no_connect")
		)
		(pad "11" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(U3A-E)")
			(pinfunction "O1")
			(pintype "output")
		)
		(pad "12" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "unconnected-(U3B-O0-Pad12)")
			(pinfunction "O0")
			(pintype "output+no_connect")
		)
		(pad "13" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/CPU-A15")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/M2")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "16" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-40_W15.24mm"
		(layer "F.Cu")
		(at 134.176 88.075 90)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "U5"
			(at 7.62 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "RP2C02 PPU"
			(at 7.625 50.59 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/CPU-R~{W}")
			(pinfunction "R/W")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/CPU-D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/CPU-D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/CPU-D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CPU-D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CPU-D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/CPU-D5")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/CPU-D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/CPU-D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/CPU-A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/CPU-A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/CPU-A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/PPU-~{CE}")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "EXT0")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "EXT1")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "EXT2")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at 0 40.64 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "EXT3")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole oval
			(at 0 43.18 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/PPU-CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "19" thru_hole oval
			(at 0 45.72 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/~{NMI}")
			(pinfunction "~{INT}")
			(pintype "output")
		)
		(pad "20" thru_hole oval
			(at 0 48.26 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 15.24 48.26 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q1-B)")
			(pinfunction "VIDEO_OUT")
			(pintype "output")
		)
		(pad "22" thru_hole oval
			(at 15.24 45.72 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/~{RST}")
			(pinfunction "~{RST}")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 15.24 43.18 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/PPU-~{WE}")
			(pinfunction "~{WR}")
			(pintype "output")
		)
		(pad "24" thru_hole oval
			(at 15.24 40.64 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/PPU-~{RD}")
			(pinfunction "~{RD}")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 15.24 38.1 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PPU-A13")
			(pinfunction "PA13")
			(pintype "output")
		)
		(pad "26" thru_hole oval
			(at 15.24 35.56 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "/PPU-A12")
			(pinfunction "PA12")
			(pintype "output")
		)
		(pad "27" thru_hole oval
			(at 15.24 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "/PPU-A11")
			(pinfunction "PA11")
			(pintype "output")
		)
		(pad "28" thru_hole oval
			(at 15.24 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "/PPU-A10")
			(pinfunction "PA10")
			(pintype "output")
		)
		(pad "29" thru_hole oval
			(at 15.24 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/PPU-A9")
			(pinfunction "PA9")
			(pintype "output")
		)
		(pad "30" thru_hole oval
			(at 15.24 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/PPU-A8")
			(pinfunction "PA8")
			(pintype "output")
		)
		(pad "31" thru_hole oval
			(at 15.24 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/PPU-D7")
			(pinfunction "PD7")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole oval
			(at 15.24 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/PPU-D6")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole oval
			(at 15.24 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/PPU-D5")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole oval
			(at 15.24 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/PPU-D4")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole oval
			(at 15.24 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/PPU-D3")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(pad "36" thru_hole oval
			(at 15.24 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/PPU-D2")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(pad "37" thru_hole oval
			(at 15.24 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/PPU-D1")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "38" thru_hole oval
			(at 15.24 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/PPU-D0")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "39" thru_hole oval
			(at 15.24 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/ALE")
			(pinfunction "ALE")
			(pintype "output")
		)
		(pad "40" thru_hole oval
			(at 15.24 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-40_W15.24mm"
		(layer "F.Cu")
		(at 58.006 100.89 90)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "U6"
			(at 7.62 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "RP2A03 CPU"
			(at 7.62 50.59 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/SOUND-1")
			(pinfunction "AUX_1")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/SOUND-2")
			(pinfunction "AUX_2")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/~{RST}")
			(pinfunction "~{RST}")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/CPU-A0")
			(pinfunction "CPU_A0")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/CPU-A1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/CPU-A2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/CPU-A3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/CPU-A4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/CPU-A5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/CPU-A6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "11" thru_hole oval
			(at 0 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/CPU-A7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "12" thru_hole oval
			(at 0 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/CPU-A8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "13" thru_hole oval
			(at 0 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/CPU-A9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "14" thru_hole oval
			(at 0 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/CPU-A10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "15" thru_hole oval
			(at 0 35.56 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "/CPU-A11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "16" thru_hole oval
			(at 0 38.1 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "/CPU-A12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "17" thru_hole oval
			(at 0 40.64 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/CPU-A13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "18" thru_hole oval
			(at 0 43.18 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/CPU-A14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "19" thru_hole oval
			(at 0 45.72 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/CPU-A15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "20" thru_hole oval
			(at 0 48.26 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 15.24 48.26 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/CPU-D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 15.24 45.72 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/CPU-D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole oval
			(at 15.24 43.18 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/CPU-D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "24" thru_hole oval
			(at 15.24 40.64 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CPU-D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 15.24 38.1 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CPU-D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole oval
			(at 15.24 35.56 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/CPU-D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole oval
			(at 15.24 33.02 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/CPU-D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole oval
			(at 15.24 30.48 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/CPU-D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "29" thru_hole oval
			(at 15.24 27.94 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/CPU-CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "30" thru_hole oval
			(at 15.24 25.4 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "TST/GND")
			(pintype "input")
		)
		(pad "31" thru_hole oval
			(at 15.24 22.86 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/M2")
			(pinfunction "M2")
			(pintype "output")
		)
		(pad "32" thru_hole oval
			(at 15.24 20.32 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/~{IRQ}")
			(pinfunction "~{IRQ}")
			(pintype "input")
		)
		(pad "33" thru_hole oval
			(at 15.24 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/~{NMI}")
			(pinfunction "~{NMI}")
			(pintype "input")
		)
		(pad "34" thru_hole oval
			(at 15.24 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/CPU-R~{W}")
			(pinfunction "R/W")
			(pintype "output")
		)
		(pad "35" thru_hole oval
			(at 15.24 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pinfunction "~{OE2}")
			(pintype "output")
		)
		(pad "36" thru_hole oval
			(at 15.24 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pinfunction "~{OE1}")
			(pintype "output")
		)
		(pad "37" thru_hole oval
			(at 15.24 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/OUT-2")
			(pinfunction "OUT_2")
			(pintype "output")
		)
		(pad "38" thru_hole oval
			(at 15.24 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/OUT-1")
			(pinfunction "OUT_1")
			(pintype "output")
		)
		(pad "39" thru_hole oval
			(at 15.24 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pinfunction "OUT_0")
			(pintype "output")
		)
		(pad "40" thru_hole oval
			(at 15.24 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-16_W7.62mm"
		(layer "F.Cu")
		(at 167.8 50.075 90)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U7"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "40H368 (CI)"
			(at 4.15 -4.425 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.cl.cam.ac.uk/teaching//2003/Hardware/datasheets/ht6116.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pinfunction "~{1OE}")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/4016-D0")
			(pinfunction "1A")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/CPU-D0")
			(pinfunction "~{1Y}")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/4016-D1")
			(pinfunction "2A")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/CPU-D1")
			(pinfunction "~{2Y}")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "3A")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "unconnected-(U7-~{3Y}-Pad7)")
			(pinfunction "~{3Y}")
			(pintype "output+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/CPU-D2")
			(pinfunction "~{4Y}")
			(pintype "output")
		)
		(pad "10" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/4016-D2")
			(pinfunction "4A")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CPU-D3")
			(pinfunction "~{5Y}")
			(pintype "output")
		)
		(pad "12" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/4016-D3")
			(pinfunction "5A")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CPU-D4")
			(pinfunction "~{6Y}")
			(pintype "output")
		)
		(pad "14" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4016-D4")
			(pinfunction "6A")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pinfunction "~{2OE}")
			(pintype "input")
		)
		(pad "16" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-16_W7.62mm"
		(layer "F.Cu")
		(at 167.8 62.975 90)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U8"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "40H368 (CII)"
			(at 3.8 -4.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.cl.cam.ac.uk/teaching//2003/Hardware/datasheets/ht6116.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pinfunction "~{1OE}")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/4017-D0")
			(pinfunction "1A")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/CPU-D0")
			(pinfunction "~{1Y}")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/4017-D1")
			(pinfunction "2A")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/CPU-D1")
			(pinfunction "~{2Y}")
			(pintype "output")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "3A")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "unconnected-(U8-~{3Y}-Pad7)")
			(pinfunction "~{3Y}")
			(pintype "output+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/CPU-D2")
			(pinfunction "~{4Y}")
			(pintype "output")
		)
		(pad "10" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/4017-D2")
			(pinfunction "4A")
			(pintype "input")
		)
		(pad "11" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CPU-D3")
			(pinfunction "~{5Y}")
			(pintype "output")
		)
		(pad "12" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/4017-D3")
			(pinfunction "5A")
			(pintype "input")
		)
		(pad "13" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CPU-D4")
			(pinfunction "~{6Y}")
			(pintype "output")
		)
		(pad "14" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/4017-D4")
			(pinfunction "6A")
			(pintype "input")
		)
		(pad "15" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pinfunction "~{2OE}")
			(pintype "input")
		)
		(pad "16" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-14_W7.62mm"
		(layer "F.Cu")
		(at 192.325 90.85 90)
		(descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U9"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "74LS04"
			(at 3.81 17.57 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS04"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SSOP?14* TSSOP?14*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 7.62 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(C7-Pad2)")
			(pintype "input")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(R1-Pad1)")
			(pintype "output")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(R1-Pad1)")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/CIC-CLK")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PPU-A13")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "/PPU-~{A13}")
			(pintype "output")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(R5-Pad1)")
			(pintype "output")
		)
		(pad "9" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/~{RST}")
			(pintype "input")
		)
		(pad "10" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/EXP-AUDIO-OUT")
			(pintype "output")
		)
		(pad "11" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(C20-Pad1)")
			(pintype "input")
		)
		(pad "12" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(U10-CLK_IN)")
			(pintype "output")
		)
		(pad "13" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(R1-Pad1)")
			(pintype "input")
		)
		(pad "14" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-16_W7.62mm"
		(layer "F.Cu")
		(at 171.7 108.575 90)
		(descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U10"
			(at 3.81 -2.33 90)
			(layer "F.SilkS")
		)
		(property "Value" "CIC"
			(at 3.81 20.11 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "Net-(U10-DATA_OUT)")
			(pinfunction "DATA_OUT")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(U10-DATA_IN)")
			(pinfunction "DATA_IN")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U10-SEED)")
			(pinfunction "SEED")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "LOCK/KEY")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "unconnected-(U10-NC-Pad5)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(U10-CLK_IN)")
			(pinfunction "CLK_IN")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(P6-Pin_4)")
			(pinfunction "RST")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 7.62 17.78 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/~{RST}")
			(pinfunction "~{HOST_RST}")
			(pintype "output")
		)
		(pad "10" thru_hole oval
			(at 7.62 15.24 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "/CIC-RST")
			(pinfunction "CIC-RST")
			(pintype "output")
		)
		(pad "11" thru_hole oval
			(at 7.62 12.7 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 7.62 10.16 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-16_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_HC49-U_Horizontal_1EP_style2"
		(layer "F.Cu")
		(at 98.15 48.8 90)
		(descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystal")
		(property "Reference" "X1"
			(at -2.1 -2.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "21.477272 MHz"
			(at 10.175 8.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Crystal:Crystal_HC49-U_Horizontal_1EP_style2"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Three pin crystal, GND on pin 3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.45 7.625 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(Q2-C)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(C41-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -3.45 9.25 90)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "unconnected-(X1-Pad3)_1")
			(pinfunction "3")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at 2.45 9.25 90)
			(size 11 13.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 131 "unconnected-(X1-Pad3)_2")
			(pinfunction "3")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole rect
			(at 8.35 9.25 90)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "unconnected-(X1-Pad3)")
			(pinfunction "3")
			(pintype "passive+no_connect")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-U_Horizontal_1EP_style2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 213.8 28.825 180)
		(descr "JST PH series connector, S7B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH top entry")
		(property "Reference" "P4"
			(at 6 -2.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Controller Input"
			(at 6 7.45 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6 2.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 1 "/GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 6 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/4016-D0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 8 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 10 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/4016-D3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 12 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4016-D4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 231 58.075 90)
		(descr "JST PH series connector, S7B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH top entry")
		(property "Reference" "P5"
			(at 6 -1.704 90)
			(layer "F.SilkS")
		)
		(property "Value" "Controller Input"
			(at 6 7.45 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_JST:JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6 2.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 1 "/GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 6 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/4017-D0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 8 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 10 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/4017-D3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 12 0 90)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/4017-D4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S7B-PH-K_1x07_P2.00mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NESRE:DIP-24_W15.24-7.62mm"
		(layer "F.Cu")
		(at 78.326 121.075 90)
		(descr "Module Dil 28 pins, pads ronds, e=600 mils")
		(tags "DIL")
		(property "Reference" "U1"
			(at 7.62 -5.08 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6116 (WRAM)"
			(at 11.4935 18.4785 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "NESRE:DIP-24_W15.24-7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.cl.cam.ac.uk/teaching//2003/Hardware/datasheets/ht6116.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/CPU-A7")
			(pinfunction "A7")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/CPU-A6")
			(pinfunction "A6~{}")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/CPU-A5")
			(pinfunction "A5~{}")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/CPU-A4")
			(pinfunction "A4~{}")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/CPU-A3")
			(pinfunction "A3~{}")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/CPU-A2")
			(pinfunction "A2")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/CPU-A1")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/CPU-A0")
			(pinfunction "A0")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/CPU-D0")
			(pinfunction "D0")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/CPU-D1")
			(pinfunction "D1")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/CPU-D2")
			(pinfunction "D2")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND~{}")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 7.62 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CPU-D3")
			(pinfunction "D3")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CPU-D3")
			(pinfunction "D3")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 7.62 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CPU-D4")
			(pinfunction "D4")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CPU-D4")
			(pinfunction "D4")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 7.62 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/CPU-D5")
			(pinfunction "D5")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/CPU-D5")
			(pinfunction "D5")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 7.62 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/CPU-D6")
			(pinfunction "D6")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/CPU-D6")
			(pinfunction "D6")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 7.62 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/CPU-D7")
			(pinfunction "D7")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/CPU-D7")
			(pinfunction "D7")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/WRAM-~{CE}")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/WRAM-~{CE}")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/CPU-A10")
			(pinfunction "A10")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/CPU-A10")
			(pinfunction "A10")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "~{OE}")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "~{OE}")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/CPU-R~{W}")
			(pinfunction "~{WE}")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/CPU-R~{W}")
			(pinfunction "~{WE}")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/CPU-A9")
			(pinfunction "A9")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/CPU-A9")
			(pinfunction "A9")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/CPU-A8")
			(pinfunction "A8")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/CPU-A8")
			(pinfunction "A8")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W15.24mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NESRE:DIP-24_W15.24-7.62mm"
		(layer "F.Cu")
		(at 134.176 123.575 90)
		(descr "Module Dil 28 pins, pads ronds, e=600 mils")
		(tags "DIL")
		(property "Reference" "U4"
			(at 7.62 -5.08 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "6116 (VRAM)"
			(at 11.4935 18.4785 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "NESRE:DIP-24_W15.24-7.62mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.cl.cam.ac.uk/teaching//2003/Hardware/datasheets/ht6116.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/PPU-A7")
			(pinfunction "A7")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/PPU-A6")
			(pinfunction "A6~{}")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/PPU-A5")
			(pinfunction "A5~{}")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/PPU-A4")
			(pinfunction "A4~{}")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/PPU-A3")
			(pinfunction "A3~{}")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/PPU-A2")
			(pinfunction "A2")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/PPU-A1")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/PPU-A0")
			(pinfunction "A0")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/PPU-D0")
			(pinfunction "D0")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/PPU-D1")
			(pinfunction "D1")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/PPU-D2")
			(pinfunction "D2")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND~{}")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 7.62 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/PPU-D3")
			(pinfunction "D3")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/PPU-D3")
			(pinfunction "D3")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 7.62 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/PPU-D4")
			(pinfunction "D4")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/PPU-D4")
			(pinfunction "D4")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 7.62 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/PPU-D5")
			(pinfunction "D5")
			(pintype "passive")
		)
		(pad "15" thru_hole oval
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/PPU-D5")
			(pinfunction "D5")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 7.62 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/PPU-D6")
			(pinfunction "D6")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/PPU-D6")
			(pinfunction "D6")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 7.62 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/PPU-D7")
			(pinfunction "D7")
			(pintype "passive")
		)
		(pad "17" thru_hole oval
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/PPU-D7")
			(pinfunction "D7")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 7.62 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/VRAM-~{CE}")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "/VRAM-~{CE}")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "/VRAM-A10")
			(pinfunction "A10")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "/VRAM-A10")
			(pinfunction "A10")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/PPU-~{RD}")
			(pinfunction "~{OE}")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "/PPU-~{RD}")
			(pinfunction "~{OE}")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/PPU-~{WE}")
			(pinfunction "~{WE}")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/PPU-~{WE}")
			(pinfunction "~{WE}")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/PPU-A9")
			(pinfunction "A9")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "/PPU-A9")
			(pinfunction "A9")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/PPU-A8")
			(pinfunction "A8")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "/PPU-A8")
			(pinfunction "A8")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "24" thru_hole oval
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-24_W15.24mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "NESRE:PowerReset-switch-In"
		(layer "F.Cu")
		(at 226 68.825 -90)
		(property "Reference" "P6"
			(at 3.725 -3.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "PWR/RST IN"
			(at 3.325 -5.6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "NESRE:PowerReset-switch-In"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 22.5 0)
			(size 3.25 3.25)
			(drill 1.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(P3-Pin_5)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 15 0)
			(size 3.25 3.25)
			(drill 1.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/+9V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0)
			(size 3.25 3.25)
			(drill 1.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 5 0)
			(size 3.25 3.25)
			(drill 1.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(P6-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 0)
			(size 3.25 3.25)
			(drill 1.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(P6-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
	)
	(footprint "NESRE:NES_Edge_Connector"
		(layer "F.Cu")
		(at 59.775 131.35)
		(property "Reference" "P1"
			(at 13.525 -0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "72-Pin Connector"
			(at 13.725 -0.825 0)
			(layer "F.Fab")
		)
		(property "Footprint" "NESRE:NES_Edge_Connector"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(pad "1" smd rect
			(at 17.75 6.25)
			(size 3 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "2" smd rect
			(at 20.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 102 "/CPU-A11")
			(pinfunction "CPU_A11")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "3" smd rect
			(at 23.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "/CPU-A10")
			(pinfunction "CPU_A10")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "4" smd rect
			(at 25.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "/CPU-A9")
			(pinfunction "CPU_A9")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "5" smd rect
			(at 28.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "/CPU-A8")
			(pinfunction "CPU_A8")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "6" smd rect
			(at 30.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "/CPU-A7")
			(pinfunction "CPU_A7")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "7" smd rect
			(at 33.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 63 "/CPU-A6")
			(pinfunction "CPU_A6")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "8" smd rect
			(at 35.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "/CPU-A5")
			(pinfunction "CPU_A5")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "9" smd rect
			(at 38.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "/CPU-A4")
			(pinfunction "CPU_A4")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "10" smd rect
			(at 40.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "/CPU-A3")
			(pinfunction "CPU_A3")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "11" smd rect
			(at 43.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "/CPU-A2")
			(pinfunction "CPU_A2")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "12" smd rect
			(at 45.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "/CPU-A1")
			(pinfunction "CPU_A1")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "13" smd rect
			(at 48.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "/CPU-A0")
			(pinfunction "CPU_A0")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "14" smd rect
			(at 50.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "/CPU-R~{W}")
			(pinfunction "CPU_R/W")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "15" smd rect
			(at 53.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "/~{IRQ}")
			(pinfunction "~{IRQ}")
			(pintype "output")
			(solder_mask_margin -0.5)
		)
		(pad "16" smd rect
			(at 55.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 112 "/EXP-0")
			(pinfunction "EXP_0")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "17" smd rect
			(at 58.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 113 "/EXP-1")
			(pinfunction "EXP_1")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "18" smd rect
			(at 60.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 114 "/EXP-2")
			(pinfunction "EXP_2")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "19" smd rect
			(at 63.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 115 "/EXP-3")
			(pinfunction "EXP_3")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "20" smd rect
			(at 65.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 116 "/EXP-4")
			(pinfunction "EXP_4")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "21" smd rect
			(at 68.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 91 "/PPU-~{RD}")
			(pinfunction "PPU_~{RD}")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "22" smd rect
			(at 70.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 92 "/VRAM-A10")
			(pinfunction "VRAM_A10")
			(pintype "output")
			(solder_mask_margin -0.5)
		)
		(pad "23" smd rect
			(at 73.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 80 "/PPU-A6")
			(pinfunction "PPU_A6")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "24" smd rect
			(at 75.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 75 "/PPU-A5")
			(pinfunction "PPU_A5")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "25" smd rect
			(at 78.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 74 "/PPU-A4")
			(pinfunction "PPU_A4")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "26" smd rect
			(at 80.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 77 "/PPU-A3")
			(pinfunction "PPU_A3")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "27" smd rect
			(at 83.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 72 "/PPU-A2")
			(pinfunction "PPU_A2")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "28" smd rect
			(at 85.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 66 "/PPU-A1")
			(pinfunction "PPU_A1")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "29" smd rect
			(at 88.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 67 "/PPU-A0")
			(pinfunction "PPU_A0")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "30" smd rect
			(at 90.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 68 "/PPU-D0")
			(pinfunction "PPU_D0")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "31" smd rect
			(at 93.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 81 "/PPU-D1")
			(pinfunction "PPU_D1")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "32" smd rect
			(at 95.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 70 "/PPU-D2")
			(pinfunction "PPU_D2")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "33" smd rect
			(at 98.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 79 "/PPU-D3")
			(pinfunction "PPU_D3")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "34" smd rect
			(at 100.75 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "/CIC-TO-CART")
			(pinfunction "CIC-TO-CART")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "35" smd rect
			(at 103.25 6.25)
			(size 2 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "/CIC-TO-MB")
			(pinfunction "CIC-TO-MB")
			(pintype "output")
			(solder_mask_margin -0.5)
		)
		(pad "36" smd rect
			(at 106.25 6.25)
			(size 3 9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "37" smd rect
			(at 17.75 6.25)
			(size 3 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 28 "/SYSTEM-CLK")
			(pinfunction "SYSTEM_CLK")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "38" smd rect
			(at 20.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "/M2")
			(pinfunction "M2")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "39" smd rect
			(at 23.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 101 "/CPU-A12")
			(pinfunction "CPU_A12")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "40" smd rect
			(at 25.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 86 "/CPU-A13")
			(pinfunction "CPU_A13")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "41" smd rect
			(at 28.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 85 "/CPU-A14")
			(pinfunction "CPU_A14")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "42" smd rect
			(at 30.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 56 "/CPU-D7")
			(pinfunction "CPU_D7")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "43" smd rect
			(at 33.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 58 "/CPU-D6")
			(pinfunction "CPU_D6")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "44" smd rect
			(at 35.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 60 "/CPU-D5")
			(pinfunction "CPU_D5")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "45" smd rect
			(at 38.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 62 "/CPU-D4")
			(pinfunction "CPU_D4")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "46" smd rect
			(at 40.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 64 "/CPU-D3")
			(pinfunction "CPU_D3")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "47" smd rect
			(at 43.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 46 "/CPU-D2")
			(pinfunction "CPU_D2")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "48" smd rect
			(at 45.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 48 "/CPU-D1")
			(pinfunction "CPU_D1")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "49" smd rect
			(at 48.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 50 "/CPU-D0")
			(pinfunction "CPU_D0")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "50" smd rect
			(at 50.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 87 "/~{ROMSEL}")
			(pinfunction "~{ROMSEL}")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "51" smd rect
			(at 53.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 117 "/EXP-9")
			(pinfunction "EXP_9")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "52" smd rect
			(at 55.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 121 "/EXP-8")
			(pinfunction "EXP_8")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "53" smd rect
			(at 58.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 118 "/EXP-7")
			(pinfunction "EXP_7")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "54" smd rect
			(at 60.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 119 "/EXP-6")
			(pinfunction "EXP_6")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "55" smd rect
			(at 63.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 120 "/EXP-5")
			(pinfunction "EXP_5")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
		(pad "56" smd rect
			(at 65.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 90 "/PPU-~{WE}")
			(pinfunction "PPU_~{WR}")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "57" smd rect
			(at 68.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 93 "/VRAM-~{CE}")
			(pinfunction "VRAM_~{CE}")
			(pintype "output")
			(solder_mask_margin -0.5)
		)
		(pad "58" smd rect
			(at 70.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 105 "/PPU-~{A13}")
			(pinfunction "PPU_~{A13}")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "59" smd rect
			(at 73.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 69 "/PPU-A7")
			(pinfunction "PPU_A7")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "60" smd rect
			(at 75.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 88 "/PPU-A8")
			(pinfunction "PPU_A8")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "61" smd rect
			(at 78.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 89 "/PPU-A9")
			(pinfunction "PPU_A9")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "62" smd rect
			(at 80.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 95 "/PPU-A11")
			(pinfunction "PPU_A11")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "63" smd rect
			(at 83.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 94 "/PPU-A10")
			(pinfunction "PPU_A10")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "64" smd rect
			(at 85.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 96 "/PPU-A12")
			(pinfunction "PPU_A12")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "65" smd rect
			(at 88.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 44 "/PPU-A13")
			(pinfunction "PPU_A13")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "66" smd rect
			(at 90.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 71 "/PPU-D7")
			(pinfunction "PPU_D7")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "67" smd rect
			(at 93.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 78 "/PPU-D6")
			(pinfunction "PPU_D6")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "68" smd rect
			(at 95.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 73 "/PPU-D5")
			(pinfunction "PPU_D5")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "69" smd rect
			(at 98.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 76 "/PPU-D4")
			(pinfunction "PPU_D4")
			(pintype "bidirectional")
			(solder_mask_margin -0.5)
		)
		(pad "70" smd rect
			(at 100.75 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 109 "/CIC-RST")
			(pinfunction "CIC-RST")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "71" smd rect
			(at 103.25 6.25)
			(size 2 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 107 "/CIC-CLK")
			(pinfunction "CIC-CLK")
			(pintype "input")
			(solder_mask_margin -0.5)
		)
		(pad "72" smd rect
			(at 106.25 6.25)
			(size 3 9)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin -0.5)
		)
	)
	(footprint "NESRE:EXP_Header"
		(layer "F.Cu")
		(at 92.508 57.075)
		(property "Reference" "P2"
			(at -5.632 8.535 0)
			(layer "F.SilkS")
		)
		(property "Value" "EXP-Connector"
			(at -2.733 -3.875 0)
			(layer "F.Fab")
		)
		(property "Footprint" "NESRE:EXP_Header"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(image
			(at 138.208 83.025)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at 61 7 0)
			(layer "F.SilkS")
		)
		(fp_text user "48"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -3 7 0)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at 61 0 0)
			(layer "F.SilkS")
		)
		(pad "" np_thru_hole circle
			(at -3.95 3.2)
			(size 4.2 4.2)
			(drill 4.2)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 62.4 3.2)
			(size 3.3 3.3)
			(drill 3.3)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/EXP-AUDIO-IN")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 7.62 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/~{NMI}")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 10.16 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/CPU-A15")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 12.7 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "/EXP-9")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 15.24 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "/EXP-8")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 17.78 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "/EXP-7")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 20.32 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "/EXP-6")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 22.86 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "/EXP-5")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 25.4 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 27.94 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/4016-D1")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 30.48 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/4016-D3")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 33.02 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/~{IRQ}")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 35.56 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/4017-D2")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 38.1 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/4017-D3")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 40.64 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "/~{OE2}")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 43.18 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/4017-D4")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 45.72 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/4017-D0")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 48.26 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/4017-D1")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 50.8 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/EXP-VIDEO")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 53.34 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/EXP-AUDIO-OUT")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 55.88 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "/+9V")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 58.42 6.5)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/CIC-CLK")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 58.42 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/CPU-D7")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at 55.88 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/CPU-D6")
			(pintype "passive")
		)
		(pad "27" thru_hole circle
			(at 53.34 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/CPU-D5")
			(pintype "passive")
		)
		(pad "28" thru_hole circle
			(at 50.8 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CPU-D4")
			(pintype "passive")
		)
		(pad "29" thru_hole circle
			(at 48.26 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CPU-D3")
			(pintype "passive")
		)
		(pad "30" thru_hole circle
			(at 45.72 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/CPU-D2")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 43.18 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/CPU-D1")
			(pintype "passive")
		)
		(pad "32" thru_hole circle
			(at 40.64 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/CPU-D0")
			(pintype "passive")
		)
		(pad "33" thru_hole circle
			(at 38.1 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/4016-D2")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at 35.56 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pintype "passive")
		)
		(pad "35" thru_hole circle
			(at 33.02 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/4016-D0")
			(pintype "passive")
		)
		(pad "36" thru_hole circle
			(at 30.48 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4016-D4")
			(pintype "passive")
		)
		(pad "37" thru_hole circle
			(at 27.94 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pintype "passive")
		)
		(pad "38" thru_hole circle
			(at 25.4 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "/EXP-4")
			(pintype "passive")
		)
		(pad "39" thru_hole circle
			(at 22.86 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/EXP-3")
			(pintype "passive")
		)
		(pad "40" thru_hole circle
			(at 20.32 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "/EXP-2")
			(pintype "passive")
		)
		(pad "41" thru_hole circle
			(at 17.78 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "/EXP-1")
			(pintype "passive")
		)
		(pad "42" thru_hole circle
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "/EXP-0")
			(pintype "passive")
		)
		(pad "43" thru_hole circle
			(at 12.7 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "/OUT-0")
			(pintype "passive")
		)
		(pad "44" thru_hole circle
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/OUT-1")
			(pintype "passive")
		)
		(pad "45" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "/OUT-2")
			(pintype "passive")
		)
		(pad "46" thru_hole circle
			(at 5.08 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(P2-Pad46)")
			(pintype "passive+no_connect")
		)
		(pad "47" thru_hole circle
			(at 2.54 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pintype "passive")
		)
		(pad "48" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
	)
	(footprint "Crystal:Resonator_Murata_CSTLSxxxG-3Pin_W8.0mm_H3.0mm"
		(layer "F.Cu")
		(at 200.75 108.075 90)
		(descr "Ceramic Resomator/Filter Murata CSTLSxxxG, http://www.murata.com/~/media/webrenewal/support/library/catalog/products/timingdevice/ceralock/p17e.ashx, length*width=8.0x3.0mm^2 package, package length=8.0mm, package width=3.0mm, 3 pins")
		(tags "THT ceramic resonator filter CSTLSxxxG")
		(property "Reference" "X2"
			(at 2.5 -2.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "4MHz"
			(at 2.5 2.7 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Crystal:Resonator_Murata_CSTLSxxxG-3Pin_W8.0mm_H3.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(C6-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(C7-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Resonator_Murata_CSTLSxxxG-3Pin_W8.0mm_H3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo2_14.6x12mm_SilkScreen"
		(locked yes)
		(layer "F.Cu")
		(at 119.546 77.43)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo2_14.6x12mm_SilkScreen"
			(at 0.75 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Symbol:OSHW-Logo2_14.6x12mm_SilkScreen"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 116.29116 50.975)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R15"
			(at 5.08 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "5.6K"
			(at 5.05884 2.25 0)
			(layer "F.SilkS")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "Motherboard.kicad_sch")
		(attr through_hole exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{OE1}")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 39.725 143.05)
		(end 64.675 143.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.675 143.05)
		(end 64.675 133.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 64.675 133.05)
		(end 75.075 133.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 75.075 143.05)
		(end 75.075 133.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 75.075 143.05)
		(end 168.475 143.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.475 143.05)
		(end 168.475 133.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.475 133.05)
		(end 179.9 133.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.9 143.05)
		(end 179.9 133.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.9 143.05)
		(end 232.975 143.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.975 143.05)
		(end 232.975 98.225)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 232.975 98.225)
		(end 235.975 98.225)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.675 24.35)
		(end 55.675 27.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.825 24.35)
		(end 187.825 27.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 39.725 46.2)
		(end 39.725 143.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 39.724998 42.450167)
		(end 39.725 24.35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.977296 94.574484)
		(end 235.975 98.225)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.975023 66.074376)
		(end 235.975 93.575)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.975 65.075)
		(end 235.975 24.35)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.975 66.07)
		(end 234.724 66.069)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 223 30.325)
		(end 224.06 30.325)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.724 94.575)
		(mid 234.385204 94.420951)
		(end 234.246681 94.075515)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 44.398 138.174)
		(end 46.458 138.174)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.245456 65.568999)
		(mid 234.38639 65.22971)
		(end 234.721 65.078)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 51.925 30.65)
		(end 53.7 30.65)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.675 24.35)
		(end 39.725 24.35)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 191.799 30.65)
		(end 193.574 30.65)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 55.675 27.3)
		(end 187.825 27.3)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.247 94.078)
		(mid 234.383777 93.732404)
		(end 234.720015 93.574)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.975 93.575)
		(end 234.724 93.575)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 39.724998 42.450167)
		(mid 41.034634 43.008043)
		(end 41.575 44.325)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 41.575166 44.324099)
		(mid 41.035069 45.641754)
		(end 39.725 46.2)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 220.003 138.174)
		(end 222.063 138.174)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.976 65.078)
		(end 234.725 65.078)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 227.95 30.65)
		(end 229.725 30.65)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 228.25 109.3)
		(end 229.850195 109.3)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 51.7 60.325)
		(end 52.7 60.325)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 56.797 138.136)
		(end 58.607 138.136)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.825 24.35)
		(end 235.975 24.35)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 186.857 138.136)
		(end 188.667 138.136)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.720479 66.068375)
		(mid 234.383171 65.913601)
		(end 234.245456 65.568999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 235.977 94.575)
		(end 234.724 94.575)
		(layer "Edge.Cuts")
	)
	(gr_text "72"
		(at 167.325 132.15 0)
		(layer "B.SilkS")
	)
	(gr_text "37"
		(at 76 132.25 0)
		(layer "B.SilkS")
	)
	(gr_text "Redherring32 / Muramasa / Kamoteshake"
		(at 121.718 60.32 -0)
		(layer "B.SilkS")
	)
	(gr_text "1"
		(at 204.34 121.645 0)
		(layer "B.SilkS")
	)
	(gr_text "Cartridge-Connector"
		(at 82.406 130.2 0)
		(layer "F.SilkS")
	)
	(gr_text "RP2A03"
		(at 81.24 93.225 0)
		(layer "F.SilkS")
	)
	(gr_text "21.477272 MHz NTSC"
		(at 130.356 41.04 0)
		(layer "F.SilkS")
	)
	(gr_text "Opentendo NES"
		(at 144.456 69.46 0)
		(layer "F.SilkS")
	)
	(gr_text "40H368"
		(at 176.86 59.255 0)
		(layer "F.SilkS")
	)
	(gr_text "EXP-Connector\n"
		(at 89.775 53.2 0)
		(layer "F.SilkS")
	)
	(gr_text "V1.4\n2024-10-14"
		(at 219.586 119.87 90)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 221.45 121.745 0)
		(layer "F.SilkS")
	)
	(gr_text "ONES-CPU-01"
		(at 146.05 92.425 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 231.025 60.9 0)
		(layer "F.SilkS")
	)
	(gr_text "U5        PPU"
		(at 153.3 90.25 0)
		(layer "F.SilkS")
	)
	(gr_text "E  C  B"
		(at 66.25 46.6 0)
		(layer "F.SilkS")
	)
	(gr_text "40H368"
		(at 176.86 46.555 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 229.286 46.07 0)
		(layer "F.SilkS")
	)
	(gr_text "RP2C02"
		(at 157.38 80.635 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 76.05 132.125 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 228.575 67.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Unused"
		(at 63.85 78.875 0)
		(layer "F.SilkS")
	)
	(gr_text "U1                   SRAM (WRAM)\n"
		(at 94.75 123.7 0)
		(layer "F.SilkS")
	)
	(gr_text "U4                   SRAM (VRAM)\n"
		(at 148.8 125.7 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 201.816 30.74 0)
		(layer "F.SilkS")
	)
	(gr_text "74HCU04"
		(at 199.72 87.195 0)
		(layer "F.SilkS")
	)
	(gr_text "U6      CPU"
		(at 79.875 83.075 0)
		(layer "F.SilkS")
	)
	(gr_text "E  C  B"
		(at 197.69 73.495 0)
		(layer "F.SilkS")
	)
	(gr_text "E  C  B"
		(at 65.45 57.325 0)
		(layer "F.SilkS")
	)
	(gr_text "74HC373"
		(at 146.27 99.915 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 217.1 28.75 0)
		(layer "F.SilkS")
	)
	(gr_text "SRAM (WRAM)"
		(at 92.325 117.3 0)
		(layer "F.SilkS")
	)
	(gr_text "MOD-RF"
		(at 212.01 120.525 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 228.5 93.775 0)
		(layer "F.SilkS")
	)
	(gr_text "26.601712 MHz PAL"
		(at 129.816 42.86 0)
		(layer "F.SilkS")
	)
	(gr_text "SRAM (VRAM)\n"
		(at 148.15 119.825 0)
		(layer "F.SilkS")
	)
	(gr_text "36"
		(at 167.275 132.1 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 204.44 121.765 0)
		(layer "F.SilkS")
	)
	(gr_text "74HC139"
		(at 66.95 70.975 0)
		(layer "F.SilkS")
	)
	(gr_text_box "The Cartridge-Connector footprint has a solder mask expansion of -0.5mm.\nThis will insure that the solder mask overlaps the edge pads a little bit to protect the thin traces.\n\nThe keepout zones are from the OEM NES and are there to prevent any solder mask around the edge connector pads. "
		(start 76.975 145.175)
		(end 113.425 161.8)
		(layer "Cmts.User")
		(border yes)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 165.95 75.025) (xy 161.35 75.05) (xy 161.35 81.65) (xy 165.1 85.35) (xy 165.625 85.475) (xy 165.925 84.675)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(Q2-B)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 68.1 44.35) (xy 73.425 44.35) (xy 73.425 46.3) (xy 77.75 46.3) (xy 79.7 48.25) (xy 84.6 48.25)
				(xy 86.775 46.075) (xy 87.85 47.15) (xy 83.725 51.275) (xy 77.875 51.275) (xy 75 48.225) (xy 68.075 48.225)
				(xy 68.075 44.35)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 211.9 60.85) (xy 226.65 60.85) (xy 226.65 62.775) (xy 226.05 63.775) (xy 225.25 64.225) (xy 211.925 64.225)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 115.972236 45.931413) (xy 115.972236 40.581413) (xy 116.797236 39.756413) (xy 163.747236 39.756413)
				(xy 164.372236 39.131413) (xy 198.122236 39.131413) (xy 199.875 37.45) (xy 200.825 38.125) (xy 201.5 38.6)
				(xy 201.625 39.381413) (xy 201.6 40.575) (xy 198.197236 43.106413) (xy 198.197236 48.181413) (xy 192.322236 48.181413)
				(xy 192.322236 43.731413) (xy 191.097236 42.506413) (xy 187.947236 42.506413) (xy 186.672236 41.231413)
				(xy 168.297236 41.231413) (xy 168.297236 43.056413) (xy 166.397236 45.056413) (xy 166.397236 51.281413)
				(xy 168.297236 53.181413) (xy 168.297236 59.706413) (xy 166.422236 61.581413) (xy 166.422236 71.156413)
				(xy 160.647236 71.156413) (xy 154.775 65.275) (xy 154.772236 64.006413) (xy 163.672236 64.006413)
				(xy 164.922236 62.756413) (xy 164.922236 60.306413) (xy 166.147236 58.956413) (xy 166.147236 56.456413)
				(xy 163.047236 53.356413) (xy 163.047236 50.156413) (xy 161.7 50.025) (xy 161.75 48.775) (xy 162.997236 48.831413)
				(xy 162.997236 45.581413) (xy 162.447236 45.031413) (xy 129.372236 45.106413) (xy 128.747236 44.506413)
				(xy 128.697236 44.506413) (xy 123.847236 44.506413) (xy 119.1153 49.315455) (xy 117.7 52.075) (xy 116 52.075)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 94.3 49.675) (xy 91.0125 49.675) (xy 88.425 52.05) (xy 88.425 55.325) (xy 91.625 58.525) (xy 91.625 63.6)
				(xy 93.075 63.6) (xy 93.075 51.525) (xy 93.65 50.95) (xy 94.3 50.75)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 200.625 100.65) (xy 196.6 102.1) (xy 195.5125 100.6) (xy 195.4375 92) (xy 196.525 92.025) (xy 206.825 92.025)
				(xy 206.775 88.53665) (xy 196.475 88.53665) (xy 196.025 87.725) (xy 196.025 84.475) (xy 207.375 84.51165)
				(xy 208.4 85.1375) (xy 208.4 92.2125) (xy 207.375 93.225) (xy 200.975 93.225) (xy 200.575 93.625)
				(xy 200.375 94.925) (xy 201 95.85) (xy 204.1 95.85) (xy 206.074 97.506) (xy 206.075 98.525) (xy 202.95 98.525)
				(xy 200.925 100.4) (xy 200.675 100.61165)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/EXP-AUDIO-OUT")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 205.103537 80.425) (xy 206.478537 80.425) (xy 208.55 81.625) (xy 203.75 81.625) (xy 204.953537 80.425)
				(xy 205.078537 80.425)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/SYSTEM-CLK")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 59.05 53.725) (xy 63.225 53.775) (xy 63.225 54.6) (xy 63.2 55.15) (xy 60.665568 58.125) (xy 59 58.125)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 165.2 89.975) (xy 165.2 97.625) (xy 166.525 98.95) (xy 166.525 107.825) (xy 167.9 109.2) (xy 168.575 109.2)
				(xy 168.575 95) (xy 167.975 94.4) (xy 167.975 91.325) (xy 166.575 89.925) (xy 165.975 89.2) (xy 165.65 89.2)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(P3-Pin_5)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 223.7 89.45) (xy 224.65 89.45) (xy 226.575 92.85) (xy 223.425 92.85) (xy 220.25 96.025) (xy 220.45 90.625)
				(xy 221.4 89.45) (xy 223.725 89.45) (xy 223.625 89.45)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 164.525 133.475) (xy 164.525 133.1) (xy 164.9 133.1) (xy 165.5 132.5) (xy 165.519 130.786) (xy 166.58825 129.82475)
				(xy 166.72175 129.39325) (xy 166.95 129.05) (xy 166.937 126.369) (xy 167.033 126.211) (xy 167.208 126.115)
				(xy 167.475 126.1) (xy 170.325 122.0125) (xy 170.325 121.525) (xy 166.6375 117.7625) (xy 167.3 116.625)
				(xy 169.15 116.625) (xy 170.075 117.825) (xy 181.025 117.825) (xy 181.025 119.675) (xy 183.7 119.675)
				(xy 183.7 117.125) (xy 180.7 114.125) (xy 180.7 111.25) (xy 179.275 111.25) (xy 178.55 110.525)
				(xy 178.55 106.35) (xy 171.6 106.35) (xy 170.875 105.625) (xy 170.875 94.725) (xy 171.4 94.725)
				(xy 172.675 96) (xy 172.675 102.175) (xy 174.8 104.3) (xy 178.85 104.3) (xy 180.125 105.575) (xy 180.125 109.05)
				(xy 181.25 110.175) (xy 190.475 110.175) (xy 190.475 106.7) (xy 190 106.225) (xy 187.45 106.225)
				(xy 185.425 104.2) (xy 185.425 102.275) (xy 191.375 102.275) (xy 191.375 103.125) (xy 191.15 103.125)
				(xy 191.15 111.45) (xy 192.075 112.375) (xy 195.925 112.375) (xy 195.925 114.375) (xy 197.575 114.375)
				(xy 197.875 112.375) (xy 197.875 105.55) (xy 194.975 105.55) (xy 194.975 104.75) (xy 199.075 104.75)
				(xy 199.075 109.8) (xy 201.1 109.8) (xy 202.6 108.3) (xy 202.6 99.8) (xy 203.35 99.05) (xy 211.875 99.05)
				(xy 212.625 98.3) (xy 212.625 96.15) (xy 211.35 94.875) (xy 211.35 91.275) (xy 213.225 89.4) (xy 213.225 87.025)
				(xy 212 85.8) (xy 212 82.725) (xy 212 82.425) (xy 212 81.725) (xy 214.7 81.725) (xy 214.7 82.425)
				(xy 219.85 82.425) (xy 220.475 82.425) (xy 225.4 77.5) (xy 227.15 79.25) (xy 222.025 84.375) (xy 216.8 84.375)
				(xy 215.775 85.4) (xy 215.775 102.9) (xy 216.221 104.639) (xy 216.285 118.544) (xy 215.04 123.365)
				(xy 215.15 125.175) (xy 212.5 124.975) (xy 213.075 119.225) (xy 213.225 117.775) (xy 213.2 116.025)
				(xy 213.2 107) (xy 211.7 105.5) (xy 206.225 105.5) (xy 205.375 106.35) (xy 205.375 110.15) (xy 201.675 113.85)
				(xy 201.675 116.625) (xy 199.5 118.8) (xy 197.225 118.8) (xy 196.75 119.275) (xy 196.75 119.75)
				(xy 193.125 123.375) (xy 193.125 127.125) (xy 182.975 127.125) (xy 180.95 125.1) (xy 170.85 125.1)
				(xy 170.075 125.875) (xy 170.064 128.426) (xy 168.5 129.975) (xy 168.484 131.628) (xy 167.325 133.45)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(P6-Pin_5)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 221.388232 68.2) (xy 226.013232 68.2) (xy 226.1 70.375) (xy 221.388232 71.55)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 94.289085 39.725) (xy 52.825 39.75) (xy 52.625 67.725) (xy 51.925 68.4) (xy 52.13 124.835) (xy 62.160624 124.773473)
				(xy 62.166764 120.607057) (xy 54.339085 120.608394) (xy 54.339085 103.925) (xy 55.589085 102.675)
				(xy 55.589085 94.475) (xy 58.714085 91.35) (xy 58.714085 84.9) (xy 56.613293 82.9) (xy 56.686708 67.9)
				(xy 58.175 67.95) (xy 58.175 66.35) (xy 56.825 66.35) (xy 56.8 62.65) (xy 59.3 62.65) (xy 59.525 62.5)
				(xy 59.775 62.175) (xy 59.775 61.525) (xy 58.039085 60.1) (xy 56.764085 60.1) (xy 55.539085 58.875)
				(xy 55.55 53.1) (xy 64.975 53.1) (xy 64.975 56.85) (xy 68.839085 60.975) (xy 74.589085 60.975) (xy 74.589085 56.875)
				(xy 66.75 56.925) (xy 66.8 53.175) (xy 65.575 51.6) (xy 65.375 51.35) (xy 65.05 51.175) (xy 61.914085 51.175)
				(xy 61.914085 46.75) (xy 55.589085 46.75) (xy 55.589085 42.45) (xy 94.314085 42.45) (xy 94.314085 39.725)
			)
		)
	)
	(zone
		(net 25)
		(net_name "Net-(C41-Pad1)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 96.0625 43.3) (xy 96.95 43.5) (xy 98.1 43.15) (xy 98.875 44.125) (xy 97.55 44.95) (xy 82.55 44.95)
				(xy 81.675 44.625) (xy 81.675 43.9) (xy 82.075 43.2) (xy 83.025 43.2) (xy 84.1875 43.3)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 95 87.4) (xy 87.65 87.375) (xy 87.65 95.15) (xy 85.85 96.95) (xy 85.85 98.9) (xy 88.525 98.9)
				(xy 88.525 96.625) (xy 89.225 95.925) (xy 90.975 95.925) (xy 90.975 98.9) (xy 93.725 98.9) (xy 93.725 95.75)
				(xy 95 94.475)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 66.75 69.175) (xy 66.75 69.85) (xy 70.725 73.275) (xy 74.025 73.275) (xy 74 71.85) (xy 74.65 71.2)
				(xy 74.65 69.125) (xy 72.125 69.125) (xy 71.875 69.125) (xy 71.875 71.05) (xy 69.55 71.05) (xy 69.55 69.175)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(Q2-C)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 65.35 44.8) (xy 65.3125 49.8625) (xy 67.199413 52.075) (xy 67.325 53.3) (xy 67.325 54.65) (xy 67.575 55.5)
				(xy 68.425 55.5) (xy 75.95 55.35) (xy 76.25 60.475) (xy 77.85 60.325) (xy 77.8 59.6875) (xy 77.525 55.4125)
				(xy 84.125 55.4) (xy 90.5 49.025) (xy 96.675 49.025) (xy 97.8 49.525) (xy 98.85 48.375) (xy 98.25 48)
				(xy 97.125 46.875) (xy 89.8 46.875) (xy 84.65 51.975) (xy 75.225 51.975) (xy 74.65 51.4) (xy 74.65 50.625)
				(xy 74.8 50.025) (xy 74.7 49.525) (xy 74.575 49.325) (xy 74.225 49.05) (xy 73.6625 48.875) (xy 73.25 48.875)
				(xy 67.75 48.875) (xy 67.05 48.5) (xy 67.05 44.8)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 205.325 36.65) (xy 205.325 38.45) (xy 206.925 40.05) (xy 206.925 41.725) (xy 206.15 42.5) (xy 203.525 42.525)
				(xy 203.525 39.875) (xy 203.9 39.5) (xy 203.9 36.65)
			)
		)
	)
	(zone
		(net 110)
		(net_name "/+9V")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 219.75 89.5625) (xy 219.75 98.0875) (xy 219.625 98.5) (xy 218.1 99.225) (xy 217.775 99.875)
				(xy 217.775 101.6) (xy 219.225 103.425) (xy 219.071 120.404) (xy 218.7 122.6) (xy 219.1 125.075)
				(xy 216.6 125.025) (xy 216.2 123.115) (xy 217.2945 119.33375) (xy 217.35 104.35) (xy 216.3 102.15)
				(xy 216.3 101.625) (xy 216.3 94.5) (xy 218.2 92.6) (xy 218.2 86.225) (xy 219.425 85) (xy 221.2 85)
				(xy 221.625 84.875) (xy 222.4 84.875) (xy 224.2 83.125) (xy 226.725 82.3375) (xy 227.325 83.1625)
				(xy 227.7 85.75) (xy 225.375 88.325) (xy 220.925 88.325)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 66.296403 73.728597) (xy 66.296403 71.728597) (xy 63.696403 69.128597) (xy 61.796403 69.128597)
				(xy 61.796403 65.603597) (xy 61.871403 65.478597) (xy 68.721403 65.478597) (xy 69.396403 66.153597)
				(xy 70.046403 65.503597) (xy 71.171403 65.503597) (xy 71.896403 66.228597) (xy 72.596403 65.528597)
				(xy 73.771403 65.528597) (xy 74.471403 66.228597) (xy 75.171403 65.528597) (xy 76.296403 65.528597)
				(xy 76.821403 66.053597) (xy 76.821403 68.578597) (xy 76.15 69.1375) (xy 76.15 71.6125) (xy 74.85 73.075)
				(xy 74.85 75.175) (xy 76.5 75.1375) (xy 77.001799 72.5125) (xy 77.598202 69.853597) (xy 78.371403 68.578597)
				(xy 78.371403 66.053597) (xy 77.021403 64.703597) (xy 68.721403 64.703597) (xy 64.846403 60.828597)
				(xy 62.996403 60.828597) (xy 59.021403 64.803597) (xy 59.021403 73.728597)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(P6-Pin_4)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 225.143429 72.631571) (xy 223.068429 74.706571) (xy 222.018429 76.531571) (xy 222.018429 77.631571)
				(xy 221.343429 78.306571) (xy 221.318429 79.031571) (xy 221.318429 79.056571) (xy 222.768429 79.056571)
				(xy 227.493429 74.331571) (xy 225.493429 72.331571)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 55.324706 27.232551) (xy 187.424706 27.232551) (xy 187.424706 24.232551) (xy 235.649706 24.232551)
				(xy 235.649706 98.207551) (xy 232.699706 98.207551) (xy 232.725 143.075) (xy 179.449706 143.007551)
				(xy 179.449706 133.057551) (xy 169.146 132.973) (xy 169.149706 130.482551) (xy 171.624706 128.007551)
				(xy 194.174706 128.007551) (xy 194.174706 125.807551) (xy 202.399706 117.582551) (xy 203.325 113.825)
				(xy 204.825 113.975) (xy 204.499706 120.607551) (xy 202.1 123.075) (xy 201.9 123.35) (xy 201.725 123.8)
				(xy 201.6 124.225) (xy 201.575 124.425) (xy 201.55 124.65) (xy 201.55 124.8) (xy 201.6 125.3) (xy 201.675 125.6)
				(xy 201.775 125.875) (xy 201.875 126.05) (xy 201.95 126.2) (xy 202.2 126.55) (xy 202.6 126.95) (xy 203.075 127.25)
				(xy 203.5 127.425) (xy 203.775 127.5) (xy 204.1 127.6) (xy 204.349999 127.65011) (xy 221.174706 127.657551)
				(xy 221.475 127.65) (xy 221.649706 127.575) (xy 221.95 127.425) (xy 222.325 127.175) (xy 222.65 126.857551)
				(xy 222.775 126.715956) (xy 223.05 126.320051) (xy 223.275 125.895051) (xy 223.424706 125.326473)
				(xy 223.474706 125.076473) (xy 223.499706 124.882551) (xy 223.499706 124.482551) (xy 223.474706 124.282551)
				(xy 223.449706 124.107551) (xy 223.424706 123.982551) (xy 223.399706 123.882551) (xy 223.374706 123.807551)
				(xy 223.349706 123.707551) (xy 223.199706 123.332551) (xy 223.074706 123.107551) (xy 222.799706 122.707551)
				(xy 222.699706 122.582551) (xy 222.524706 122.407551) (xy 222.424706 122.332551) (xy 222.349706 122.257551)
				(xy 222.249706 122.182551) (xy 221.874706 121.932551) (xy 221.874706 96.157551) (xy 223.349706 94.682551)
				(xy 227.749706 94.682551) (xy 228.324706 94.107551) (xy 228.324706 68.232551) (xy 227.074706 66.982551)
				(xy 212.624706 67.007551) (xy 211.424706 65.432551) (xy 193.974706 65.382551) (xy 193.949706 68.107551)
				(xy 207.024706 68.107551) (xy 207.549706 68.632551) (xy 207.549706 71.232551) (xy 208.174706 71.857551)
				(xy 210.649706 71.857551) (xy 212.524706 69.982551) (xy 219.524706 69.982551) (xy 220.124706 70.582551)
				(xy 220.124706 77.707551) (xy 219.499706 78.332551) (xy 212.499706 78.332551) (xy 211.699706 78.907551)
				(xy 196.874706 78.907551) (xy 196.099706 79.632551) (xy 196.099706 81.732551) (xy 190.099706 81.732551)
				(xy 190.099706 80.582551) (xy 190.949706 80.057551) (xy 192.099706 80.057551) (xy 192.099706 77.657551)
				(xy 190.124706 75.682551) (xy 190.124706 68.182551) (xy 188.424706 68.182551) (xy 186.549706 70.057551)
				(xy 186.549706 74.507551) (xy 185.199706 75.682551) (xy 185.199706 84.707551) (xy 185.999706 85.407551)
				(xy 187.274706 86.682551) (xy 187.274706 96.582551) (xy 190.649706 96.582551) (xy 191.249706 95.982551)
				(xy 191.249706 94.682551) (xy 189.646 93.125) (xy 189.666 80.57) (xy 190.876 80.57) (xy 190.875366 86.74)
				(xy 193.73752 86.74) (xy 193.747651 89.741114) (xy 190.875027 89.765516) (xy 190.874706 92.807551)
				(xy 192.274706 94.207551) (xy 192.274706 97.907551) (xy 190.949706 99.232551) (xy 186.024706 99.23)
				(xy 184.799706 99.645051) (xy 184.799706 106.720051) (xy 183.599706 106.720051) (xy 183.599706 93.945051)
				(xy 184.399706 92.857551) (xy 184.387206 86.245051) (xy 184.2625 80.0125) (xy 183.8375 79.7875)
				(xy 183.025 80.0625) (xy 182.875 80.4875) (xy 182.85 80.75) (xy 183.399706 82.082551) (xy 183.399706 91.632551)
				(xy 182.799706 92.857551) (xy 182.799706 106.707551) (xy 181.249706 106.707551) (xy 181.249706 105.307551)
				(xy 179.224706 103.657551) (xy 175.449706 103.657551) (xy 173.324706 101.607551) (xy 173.324706 95.207551)
				(xy 166.55 88.982551) (xy 166.575 75.025) (xy 171.274706 75.057551) (xy 171.274706 87.107551) (xy 173.649706 87.107551)
				(xy 173.649706 74.732551) (xy 173.799706 74.782551) (xy 175.774706 76.757551) (xy 175.724706 76.857551)
				(xy 175.724706 88.857551) (xy 174.874706 89.707551) (xy 174.874706 91.457551) (xy 177.624706 94.207551)
				(xy 177.624706 99.057551) (xy 179.949706 99.057551) (xy 179.949706 90.907551) (xy 181.324706 89.532551)
				(xy 181.324706 76.932551) (xy 184.549706 73.707551) (xy 184.549706 69.932551) (xy 188.274706 66.207551)
				(xy 188.274706 64.357551) (xy 186.374706 64.357551) (xy 181.349706 69.382551) (xy 178.874706 69.382551)
				(xy 178.874706 71.382551) (xy 167.274706 71.382551) (xy 167.274706 66.707551) (xy 168.574706 65.407551)
				(xy 179.675 65.4) (xy 179.675 61.9) (xy 181.325 61.907551) (xy 181.325 64.282551) (xy 184.424706 64.282551)
				(xy 184.424706 58.607551) (xy 186.349706 56.682551) (xy 186.349706 54.232551) (xy 184.424706 52.307551)
				(xy 184.424706 46.082551) (xy 187.299706 43.207551) (xy 190.474706 43.207551) (xy 191.674706 44.695051)
				(xy 191.724706 48.457551) (xy 192.174706 48.807551) (xy 195.974375 48.798463) (xy 195.974706 51.182551)
				(xy 211.399706 51.257551) (xy 211.799706 36.220051) (xy 213.474706 34.657551) (xy 213.474706 33.457551)
				(xy 213.074706 32.757551) (xy 213.074706 29.157551) (xy 212.499706 27.457551) (xy 201.149706 27.457551)
				(xy 200.349706 28.182551) (xy 200.324706 36.507551) (xy 198.399706 38.270051) (xy 163.524706 38.507551)
				(xy 162.974706 39.207551) (xy 115.874706 39.207551) (xy 115.05 40.125) (xy 114.97593 54.027967)
				(xy 114.843 54.109) (xy 114.672 54.257551) (xy 101.824706 54.257551) (xy 100.424706 55.657551) (xy 96.249706 55.657551)
				(xy 96.2375 58.375) (xy 98.0625 58.375) (xy 98.074706 62.375) (xy 96.199706 62.375) (xy 96.199706 66.907551)
				(xy 94.899706 68.207551) (xy 89.174706 68.207551) (xy 88.499706 67.532551) (xy 85.324706 67.532551)
				(xy 84.674706 68.182551) (xy 84.674706 71.907551) (xy 86.574706 73.807551) (xy 86.574706 81.532551)
				(xy 84.5 84.25) (xy 84.5 93) (xy 83.324706 93.257551) (xy 83.324706 99.257551) (xy 78.799706 99.257551)
				(xy 78.799706 94.032551) (xy 82.7 90.825) (xy 82.7 66.925) (xy 84.074706 64.857551) (xy 89.349706 64.857551)
				(xy 89.999706 65.507551) (xy 92.699706 65.507551) (xy 93.9 64.8625) (xy 93.9 52.9875) (xy 94.799706 51.532551)
				(xy 98.499706 51.532551) (xy 99.75 50.525) (xy 99.7 42.95) (xy 95.574706 39.207551) (xy 51.975 39.15)
				(xy 51.974706 40.332551) (xy 51.974706 67.482551) (xy 51.425 68.075) (xy 51.35 128.125) (xy 51.749706 128.832551)
				(xy 73.349706 128.832551) (xy 75.199706 130.682551) (xy 77.799706 130.682551) (xy 78.724706 131.607551)
				(xy 78.724706 142.082551) (xy 76.032 142.080158) (xy 76.032 132.979842) (xy 64.299706 132.982551)
				(xy 64.299706 142.982551) (xy 39.349706 142.982551) (xy 39.349706 24.232551) (xy 55.324706 24.232551)
			)
		)
		(polygon
			(pts
				(xy 230.45 45) (xy 230 45.275) (xy 226.15 45.275) (xy 225.775 45.65) (xy 225.775 48.125) (xy 220.45 48.125)
				(xy 212.2 55.55) (xy 199.35 55.55) (xy 193.65 61.25) (xy 193.65 64.525) (xy 208.9 64.525) (xy 208.9 61.975)
				(xy 211.3 61.975) (xy 211.275 64.525) (xy 211.75 64.825) (xy 226.375 64.825) (xy 229.95 61.25) (xy 229.95 59.325)
				(xy 229.15 58.525) (xy 229.15 57.8) (xy 229.675 57.275) (xy 232.15 57.275) (xy 232.35 57.075) (xy 232.35 45.825)
				(xy 231.525 45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 193.54298 54.975) (xy 211.49298 54.975) (xy 211.49298 52.325) (xy 203.76798 52.325) (xy 203.76798 54.25)
				(xy 201.26798 54.25) (xy 201.26798 52.325) (xy 193.54298 52.325)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 189.475 60.575) (xy 187.525 58.625) (xy 187.525 51.975) (xy 187.525 49.9) (xy 188.025 49.4)
				(xy 189.8 49.4) (xy 190.6 50.2) (xy 190.6 52.75) (xy 190.95 53.1) (xy 190.95 60.6) (xy 189.5 60.6)
				(xy 189.5 60.625)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 114.375 108.725) (xy 118.875 108.725) (xy 122.825 104.775) (xy 122.825 99.425) (xy 129.296 99.425)
				(xy 131.866 97.325) (xy 133 97.325) (xy 134.9 98.55) (xy 159 98.55) (xy 160.375 97.175) (xy 166.225 97.175)
				(xy 166.925 97.875) (xy 171.375 97.875) (xy 171.375 95.1) (xy 167.6 95.1) (xy 167.15 94.65) (xy 160.525 94.65)
				(xy 157.775 97.4) (xy 136.6125 97.4125) (xy 134.3375 95.1375) (xy 122.3 95.125) (xy 114.375 103.05)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 214.72327 85.775) (xy 213.69827 86.8) (xy 197.27327 86.8) (xy 196.8 87.05) (xy 188.3 87.05)
				(xy 184.29827 83.3) (xy 179.69827 83.3) (xy 178.52327 82.125) (xy 178.52327 80.325) (xy 178.325 79.975)
				(xy 178.125 79.725) (xy 165.07327 79.725) (xy 162.17327 82.625) (xy 131.99827 82.625) (xy 130.6625 81.3)
				(xy 128.5875 81.3) (xy 127.57327 82.325) (xy 116.52327 82.325) (xy 109.92327 88.925) (xy 57.02327 88.925)
				(xy 57.02327 84.825) (xy 58.948412 84.825) (xy 58.94827 87.075) (xy 109.275 87.144755) (xy 111.825 84.719755)
				(xy 111.89827 81.325) (xy 113.32327 79.9) (xy 113.32327 74.075) (xy 114.39827 73) (xy 123.57327 73)
				(xy 125.27327 74.7) (xy 129.925 74.7) (xy 130.29827 75.225) (xy 132.775 75.225) (xy 133.39827 74.7)
				(xy 133.39827 72) (xy 135.02327 72) (xy 135.02327 75.775) (xy 135.025 81.025) (xy 135.425 81.55)
				(xy 160.52327 81.55) (xy 161.19827 80.875) (xy 161.19827 74.6) (xy 161.79827 74) (xy 179.69827 74)
				(xy 182.94827 77.25) (xy 182.94827 81.325) (xy 183.32327 81.7) (xy 186.09827 81.7) (xy 186.42327 82.025)
				(xy 187.82327 82.025) (xy 188.54827 82.75) (xy 188.54827 84.725) (xy 188.77327 84.95) (xy 207.54827 84.95)
				(xy 211.02327 81.475) (xy 211.02327 68.125) (xy 209.37327 66.475) (xy 211.67327 64.175) (xy 211.67327 61.175)
				(xy 210.94827 60.45) (xy 206.84827 60.45) (xy 206.39827 60.25) (xy 202.09827 60.25) (xy 202.09827 58.95)
				(xy 207.54827 58.95) (xy 211.47327 55.025) (xy 211.47327 47.825) (xy 200.14827 47.825) (xy 199.84827 48.125)
				(xy 193.47327 48.125) (xy 192.17327 46.825) (xy 192.175 45.375) (xy 214.4 45.375)
			)
		)
		(polygon
			(pts
				(xy 125.3 78.765) (xy 125.3 80.795) (xy 130.69 80.795) (xy 130.69 78.765)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 53.425 109.875) (xy 60.725 109.875) (xy 62.275 111.425) (xy 70.875 111.425) (xy 74.375 114.825)
				(xy 77.575 114.825) (xy 77.6 112.675) (xy 79.175 112.675) (xy 79.175 114.95) (xy 107.125 114.95)
				(xy 110.275 111.8) (xy 124.45 111.8) (xy 125.7 113.05) (xy 125.7 116.225) (xy 126.875 117.4) (xy 147.625 117.4)
				(xy 148.075 116.95) (xy 168.175 116.95) (xy 168.175 118.625) (xy 148.6 118.625) (xy 148.1 119.125)
				(xy 126.2 119.125) (xy 124.125 117.025) (xy 113.45 117.025) (xy 112.475 116.05) (xy 85.5 116.075)
				(xy 85.175 115.725) (xy 72.475 115.725) (xy 70.725 114.125) (xy 53.475 114.125)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 121.325 39.5) (xy 121.325 44.625) (xy 114.575 44.625) (xy 109.775 49.425) (xy 105.25 49.425)
				(xy 100.95 53.725) (xy 95.075 53.725) (xy 93.35 55.45) (xy 93.35 64.725) (xy 91.3 66.775) (xy 87.5 66.775)
				(xy 83.025 62.3) (xy 79.375 62.3) (xy 79.375 56.475) (xy 80.625 55.225) (xy 88.8 55.225) (xy 90.25 53.775)
				(xy 90.25 40.775) (xy 90.95 40.075) (xy 102.5 40.075) (xy 106.1 43.675) (xy 110.25 43.675) (xy 114.675 39.5)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VCC")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 55.356 120.852591) (xy 62.026 120.85) (xy 62.025 124.05) (xy 92.025 124.05) (xy 92.4 124.45)
				(xy 92.8 124.45) (xy 93.375 124.6) (xy 102.075 124.6) (xy 104.625 127.15) (xy 116.25 127.15) (xy 116.25 123.25)
				(xy 122.475 123.25) (xy 122.875 123.65) (xy 122.875 127.15) (xy 123.725 128) (xy 128.65 128) (xy 129.475 127.175)
				(xy 140.075 127.175) (xy 141.375 128.475) (xy 142.275 128.475) (xy 142.9 127.85) (xy 152.775 127.85)
				(xy 152.775 125.15) (xy 169.625 125.15) (xy 169.625 127.325) (xy 167.75 127.325) (xy 164.85 130.3)
				(xy 132.65 130.3) (xy 132.15 130.8) (xy 87.7 130.8) (xy 86.875 129.975) (xy 80.1 129.975) (xy 77.5 127.375)
				(xy 76.625 126.5) (xy 65.975 126.5) (xy 65.05 127.425) (xy 55.35 127.425)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 55.7 27.275) (xy 187.8 27.275) (xy 187.8 24.325) (xy 236 24.325) (xy 236 98.25) (xy 233 98.25)
				(xy 233 143.075) (xy 179.875 143.075) (xy 179.875 133.075) (xy 167.525 133.075) (xy 167.525 142.1)
				(xy 164.525 142.1) (xy 164.525 133.1) (xy 165.15 133.1) (xy 165.15 130.775) (xy 168.075 127.85)
				(xy 170.2 127.85) (xy 170.2 123.625) (xy 164.3 123.625) (xy 164.3 122.3) (xy 110.3 122.3) (xy 109.875 121.875)
				(xy 105.55 121.875) (xy 105.55 119.75) (xy 85.975 119.75) (xy 83.825 117.6) (xy 68.575 117.6) (xy 67.175 116.2)
				(xy 64.925 116.15) (xy 61.425 117.875) (xy 53.625 117.875) (xy 53.625 129.35) (xy 66.425 129.35)
				(xy 66.775 129.7) (xy 73.975 129.7) (xy 73.975 133.075) (xy 64.7 133.075) (xy 64.7 143.075) (xy 39.7 143.075)
				(xy 39.7 24.325) (xy 55.7 24.325)
			)
		)
		(polygon
			(pts
				(xy 170.6 84.475) (xy 169.8 85.86) (xy 127.575 85.75) (xy 119.075 85.75) (xy 111.9 92.925) (xy 95.95 92.925)
				(xy 94.15 94.725) (xy 87.275 94.725) (xy 85.525 92.975) (xy 77.55 92.975) (xy 77.05 92.475) (xy 72.975 92.475)
				(xy 71.7 93.75) (xy 64.3 93.75) (xy 63.45 92.9) (xy 62.725 92.9) (xy 60.975 94.65) (xy 58.725 94.65)
				(xy 57.35 96.025) (xy 56.0125 96.025) (xy 55.625 96.35) (xy 55.35 96.625) (xy 54.725 96.875) (xy 54.675 107.7)
				(xy 52.5 107.7) (xy 52.5 114.675) (xy 70.35 114.675) (xy 71.95 116.275) (xy 84.875 116.275) (xy 85.25 116.65)
				(xy 112.15 116.65) (xy 113.125 117.625) (xy 123.775 117.625) (xy 126.175 120.025) (xy 148.525 120.025)
				(xy 149.3375 119.65) (xy 172.575 119.675) (xy 172.575 123.3) (xy 172.7 123.625) (xy 172.7 127.875)
				(xy 175.7 127.875) (xy 175.7 125.8) (xy 178.2 125.8) (xy 178.2 127.8) (xy 181.2 127.8) (xy 181.2 119.85)
				(xy 186.325 119.85) (xy 186.325 116.6) (xy 183.3 116.6) (xy 181.75 115.05) (xy 176.525 115.05) (xy 174.625 113.15)
				(xy 163.5 113.15) (xy 163.5 107.025) (xy 163.025 107.025) (xy 160.35 104.35) (xy 156.25 104.35)
				(xy 156.25 102.25) (xy 135.125 102.25) (xy 135.125 104.475) (xy 132.05 104.475) (xy 132.05 106.225)
				(xy 132.25 107.475) (xy 128.625 111.1) (xy 115.775 111.1) (xy 115.775 109.825) (xy 119.375 109.825)
				(xy 123.6 105.6) (xy 123.6 100.575) (xy 123.775 100.375) (xy 123.975 100.175) (xy 131.2 100.175)
				(xy 131.625 100.6) (xy 133.7 100.6) (xy 134.075 100.225) (xy 159.025 100.225) (xy 161.7 102.9) (xy 167.1 102.9)
				(xy 168.3 104.1) (xy 191.125 104.1) (xy 191.125 112.3) (xy 188.45 112.3) (xy 188.45 107.25) (xy 170.3 107.25)
				(xy 168.3 109.25) (xy 168.3 111.65) (xy 175.225 111.65) (xy 177.45 113.875) (xy 182.225 113.85)
				(xy 183.775 115.55) (xy 186.975 115.55) (xy 187.7 114.825) (xy 198.1 114.825) (xy 198.1 111.075)
				(xy 195.9 111.075) (xy 195.9 109.425) (xy 202.075 109.425) (xy 202.075 106.425) (xy 202.025 104.75)
				(xy 202.02983 104.450482) (xy 202.075 101.65) (xy 196.85 101.65) (xy 196.325 101.3) (xy 195.9 100.9)
				(xy 195.9 98.7) (xy 187.646 98.7) (xy 186.95732 98.105) (xy 180.53 98.105) (xy 179.125 96.7) (xy 178.45 96.7)
				(xy 177.175 97.975) (xy 173.275 97.975) (xy 173.275 94.675) (xy 186.546 94.675) (xy 188.806 97.15)
				(xy 206.525 97.225) (xy 206.525 99.65) (xy 217.875 99.65) (xy 217.875 102.4) (xy 221.125 102.4)
				(xy 221.125 94.4) (xy 213.775 94.4) (xy 213.775 92.425) (xy 211.725 90.375) (xy 208.3 90.375) (xy 208.3 91.75)
				(xy 206.725 91.75) (xy 206.725 88.775) (xy 201.025 88.775) (xy 200.6 88.35) (xy 188.95 88.35) (xy 188.15 89.15)
				(xy 186.1 89.15) (xy 186.1 87.65) (xy 184.3 85.85) (xy 179.45 85.85) (xy 177.75 85.825) (xy 176.5 84.475)
			)
		)
		(polygon
			(pts
				(xy 204.3425 122.779) (xy 203.825 122.8) (xy 203.175 123.1) (xy 202.45 124.1) (xy 202.4 124.275)
				(xy 202.35 124.75) (xy 202.45 125.325) (xy 202.5 125.525) (xy 202.65 125.775) (xy 202.825 126.05)
				(xy 203.075 126.275) (xy 203.325 126.475) (xy 203.725 126.65) (xy 204.16 126.803) (xy 220.41 126.803)
				(xy 220.9 126.675) (xy 221.3 126.5) (xy 221.625 126.3) (xy 221.825 126.1) (xy 222 125.875) (xy 222.175 125.625)
				(xy 222.275 125.3) (xy 222.35 124.925) (xy 222.35 124.425) (xy 222.275 124.1) (xy 222.15 123.8)
				(xy 222.025 123.6) (xy 221.9 123.45) (xy 221.65 123.175) (xy 221.35 122.975) (xy 221 122.825) (xy 220.3675 122.779)
			)
		)
		(polygon
			(pts
				(xy 206.7 106.725) (xy 206.7 109.325) (xy 210.2 109.325) (xy 210.2 112.625) (xy 212.8 112.625) (xy 212.8 106.725)
			)
		)
		(polygon
			(pts
				(xy 224.525 89.2) (xy 223.7 90.025) (xy 221.675 90.025) (xy 221.1 90.6) (xy 221.1 91.925) (xy 221.825 92.65)
				(xy 223.725 92.65) (xy 224.625 93.55) (xy 226.7875 93.55) (xy 228.2125 92.125) (xy 228.2375 90.575)
				(xy 226.8625 89.2)
			)
		)
		(polygon
			(pts
				(xy 89.45 38.75) (xy 85.525 42.675) (xy 85.525 47.75) (xy 87.375 49.6) (xy 87.375 54.525) (xy 80.175 54.525)
				(xy 79.275 55.425) (xy 73.2 55.425) (xy 72.375 56.4) (xy 72.375 62.55) (xy 69.1 62.55) (xy 69.1 64.125)
				(xy 58.7 64.125) (xy 56.55 66.275) (xy 56.55 70.95) (xy 59.1 70.95) (xy 60.275 69.775) (xy 67.225 69.775)
				(xy 68.85 71.4) (xy 71.425 71.4) (xy 72.075 70.75) (xy 76.075 70.75) (xy 77.925 72.125) (xy 83.75 72.125)
				(xy 84.55 72.925) (xy 87.075 72.925) (xy 87.075 74.35) (xy 85.825 74.35) (xy 85.175 75) (xy 76.375 75)
				(xy 74.875 73.5) (xy 56.575 73.5) (xy 56.575 77.425) (xy 60.525 77.425) (xy 60.525 83.55) (xy 56.025 83.55)
				(xy 56.025 89.55) (xy 110.25 89.55) (xy 116.9 82.9) (xy 128.825 82.9) (xy 129.675 83.75) (xy 162.875 83.75)
				(xy 165.85 80.775) (xy 175.9 80.775) (xy 178.8 84.05) (xy 184.15 84.05) (xy 188.225 87.75) (xy 189.225 87.75)
				(xy 189.225 87.625) (xy 189.2625 87.75) (xy 196.9875 87.75) (xy 197.425 87.375) (xy 211.85 87.375)
				(xy 214.075 87.4) (xy 215.425 86.05) (xy 215.125 44.675) (xy 193.925 44.775) (xy 191.15 44.75) (xy 190.775 45.525)
				(xy 186.85 45.525) (xy 186.875 41.25) (xy 184.325 41.25) (xy 182.275 39.2) (xy 160.675 39.2) (xy 157.875 42)
				(xy 122.05 42) (xy 122.05 38.875) (xy 114.1 38.875) (xy 109.8 43.175) (xy 106.675 43.175) (xy 102.25 38.75)
			)
		)
		(polygon
			(pts
				(xy 225.075 66.675) (xy 220.95 70.8) (xy 220.95 87.625) (xy 222.6625 87.625) (xy 224.2375 86.05)
				(xy 226.975 86.075) (xy 228.225 84.825) (xy 228.125 68.1) (xy 226.7 66.675)
			)
		)
		(polygon
			(pts
				(xy 230.35 44.975) (xy 229.35 45.975) (xy 226.8 45.975) (xy 225.9 46.875) (xy 225.9 61.725) (xy 224.65 63.1)
				(xy 226.1 64.575) (xy 227.55 62.9) (xy 229.6 60.375) (xy 229.6 57.175) (xy 232.375 57.175) (xy 232.375 45.75)
				(xy 231.6 44.975)
			)
		)
		(polygon
			(pts
				(xy 55.85 53.775) (xy 55.85 58.9) (xy 61.025 58.9) (xy 61.025 56.575) (xy 68.775 56.575) (xy 68.775 53.775)
			)
		)
		(polygon
			(pts
				(xy 72.65 48.6) (xy 72.65 51.225) (xy 78 51.225) (xy 78 48.6)
			)
		)
		(polygon
			(pts
				(xy 64.85 43.025) (xy 64.85 45.825) (xy 70.2 45.825) (xy 70.2 43.025)
			)
		)
		(polygon
			(pts
				(xy 201.2 27.45) (xy 198.4 30.25) (xy 198.4 40.15) (xy 201.575 40.15) (xy 201.575 35.375) (xy 212.3 35.375)
				(xy 213.325 34.35) (xy 213.325 32.775) (xy 207.775 32.775) (xy 207.775 30.25) (xy 212.9 30.25) (xy 212.9 27.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 236.05 44.075) (xy 219.85 44.075) (xy 219.85 55.725) (xy 217.1 55.725) (xy 217.1 24.325) (xy 236 24.325)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 236 98.275) (xy 233.05 98.275) (xy 233.05 143.075) (xy 213.8 143.075) (xy 213.8 126.775) (xy 216.75 126.775)
				(xy 220.35 126.775) (xy 223.05 125.775) (xy 223.95 124.325) (xy 223.25 122.925) (xy 221.95 122.175)
				(xy 216.75 122.175) (xy 216.75 105.025) (xy 227.2 105.025) (xy 227.2 94.575) (xy 236 94.575)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 46.5 143.075) (xy 39.7 143.075) (xy 39.7 24.325) (xy 46.5 24.325)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(locked yes)
		(layer "B.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 168.509835 133.625726) (xy 168.5075 143.090126) (xy 74.99 143.125126) (xy 74.934272 133.595726)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 236 98.225) (xy 233.05 98.225) (xy 233 143.075) (xy 194.6 143.075) (xy 194.6 125.325) (xy 196.15 123.825)
				(xy 197.8 122.225) (xy 203 122.225) (xy 202.1 123.125) (xy 201.65 123.975) (xy 201.8 125.425) (xy 201.85 125.975)
				(xy 202.1 126.425) (xy 202.55 126.875) (xy 203.05 127.175) (xy 203.6 127.425) (xy 204.35 127.625)
				(xy 207.85 127.625) (xy 212.75 127.675) (xy 217.7 127.675) (xy 220.3 127.675) (xy 221.55 127.575)
				(xy 222.4 127.175) (xy 223.3 125.975) (xy 223.95 124.275) (xy 223.15 122.275) (xy 222.754776 102.415)
				(xy 225.9 102.415) (xy 225.9 94.575) (xy 236 94.575)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 236 24.325) (xy 236 43.575) (xy 220.55 43.575) (xy 220.55 48.125) (xy 211.5 48.125) (xy 211.5 38.175)
				(xy 221.35 38.325) (xy 221.35 28.225) (xy 218.05 28.25) (xy 218.05 24.6)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 55.7 27.275) (xy 187.8 27.275) (xy 187.8 24.325) (xy 201.4 24.325) (xy 201.4 27.475) (xy 200.35 28.425)
				(xy 198.4 34.375) (xy 198.4 38.325) (xy 163.6 38.525) (xy 162.95 39.225) (xy 51.95 39.225) (xy 52 67.525)
				(xy 51.45 68.075) (xy 51.403914 116.550003) (xy 51.4 116.625) (xy 51.4 118.825) (xy 51.5 128.525)
				(xy 51.5 128.675) (xy 51.5 128.775) (xy 56.05 128.775) (xy 56.55 128.775) (xy 56.95 128.775) (xy 57.05 128.775)
				(xy 57.205691 128.775046) (xy 64.7 128.775) (xy 64.7 143.075) (xy 39.7 143.075) (xy 39.7 24.325)
				(xy 55.7 24.325)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(locked yes)
		(layer "F.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 168.51 143.095) (xy 168.507661 133.609889) (xy 74.9862 133.574888) (xy 74.93 143.185) (xy 168.48 143.095)
			)
		)
	)
)
