(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "MiniNDP")
		(date "2026-09-09")
		(rev "M10_38")
		(company "Brian K. White - b.kenyon.w@gmail.com")
		(comment 1 "github.com/bkw777/NODE_DATAPAC")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.22)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 177.35 116.025)
		(grid_origin 177.35 116.025)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VMEM")
	(net 3 "VBUS")
	(net 4 "/AD0")
	(net 5 "/AD1")
	(net 6 "/AD2")
	(net 7 "/AD3")
	(net 8 "/AD4")
	(net 9 "/AD5")
	(net 10 "/AD6")
	(net 11 "/AD7")
	(net 12 "/A8")
	(net 13 "/A9")
	(net 14 "/A10")
	(net 15 "/A11")
	(net 16 "/A12")
	(net 17 "/A13")
	(net 18 "/A14")
	(net 19 "/A15")
	(net 20 "/~{RD}")
	(net 21 "/RAMRST")
	(net 22 "/~{Y0}")
	(net 23 "/(A)")
	(net 24 "unconnected-(J1-Pin_39-Pad39)")
	(net 25 "unconnected-(J1-Pin_40-Pad40)")
	(net 26 "unconnected-(J1-Pin_30-Pad30)")
	(net 27 "unconnected-(J1-Pin_31-Pad31)")
	(net 28 "unconnected-(J1-Pin_37-Pad37)")
	(net 29 "/BUS_A11")
	(net 30 "unconnected-(U1-NC-Pad15)")
	(net 31 "unconnected-(U1-NC-Pad37)")
	(net 32 "unconnected-(U1-NC-Pad29)")
	(net 33 "unconnected-(U1-NC-Pad30)")
	(net 34 "/BUS_A10")
	(net 35 "unconnected-(U1-NC-Pad16)")
	(net 36 "unconnected-(U1-NC-Pad38)")
	(net 37 "unconnected-(U1-NC-Pad7)")
	(net 38 "/A5")
	(net 39 "/A6")
	(net 40 "/A19")
	(net 41 "/A18")
	(net 42 "/A7")
	(net 43 "+BATT")
	(net 44 "/BUS_A8")
	(net 45 "/BUS_A9")
	(net 46 "/A16")
	(net 47 "/A17")
	(net 48 "/A0")
	(net 49 "/A1")
	(net 50 "/A2")
	(net 51 "/A3")
	(net 52 "/A4")
	(net 53 "/BYTE")
	(net 54 "unconnected-(U1-NC-Pad8)")
	(net 55 "unconnected-(J1-Pin_17-Pad17)")
	(net 56 "unconnected-(J1-Pin_18-Pad18)")
	(net 57 "unconnected-(J1-Pin_19-Pad19)")
	(net 58 "unconnected-(J1-Pin_20-Pad20)")
	(net 59 "unconnected-(J1-Pin_25-Pad25)")
	(net 60 "unconnected-(J1-Pin_26-Pad26)")
	(net 61 "unconnected-(J1-Pin_27-Pad27)")
	(net 62 "unconnected-(J1-Pin_28-Pad28)")
	(net 63 "unconnected-(J1-Pin_33-Pad33)")
	(net 64 "unconnected-(J1-Pin_34-Pad34)")
	(net 65 "unconnected-(U2-Y0-Pad15)")
	(net 66 "unconnected-(U2-Y7-Pad7)")
	(net 67 "unconnected-(U2-Y5-Pad10)")
	(net 68 "/~{WR}")
	(net 69 "unconnected-(U2-Y2-Pad13)")
	(net 70 "/BLOCK")
	(net 71 "unconnected-(U3-Q10-Pad15)")
	(net 72 "unconnected-(U3-Q11-Pad1)")
	(net 73 "unconnected-(U2-Y4-Pad11)")
	(net 74 "unconnected-(U2-Y6-Pad9)")
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 176.775 97.7 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C2"
			(at 2.575 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 3.775 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.550001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 177.35 94.025 180)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2.000001 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2.000001 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0 180)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 176.775 107.625 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C3"
			(at -3.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at -2.55 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.550001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 144.6 96.897 180)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C1"
			(at 2.025 0.947 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.025 -0.178 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 180)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 180)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 109.35 94.024999)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSOP-II-44"
		(layer "F.Cu")
		(at 157.25 102.025 -90)
		(descr "TSOP-II, 44 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOP-II SO")
		(property "Reference" "U1"
			(at -4.25 -7.6 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AS6C8008_TSOPII"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/AS6C8008.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC SRAM 1Mx8 PARALLEL 5v TSOP-II-44"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AS6C8008-55ZIN"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*11.305x20.495mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.6 -8.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/A5")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -5.6 -7.600001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "/A4")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -5.6 -6.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/A6")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -5.6 -6 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/A3")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -5.6 -5.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/A2")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -5.6 -4.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RAMRST")
			(pinfunction "~{CE1}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -5.6 -3.599999 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "unconnected-(U1-NC-Pad7)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -5.6 -2.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U1-NC-Pad8)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -5.6 -2.000001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -5.6 -1.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -5.6 -0.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -5.6 0.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -5.6 1.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -5.6 2.000001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -5.6 2.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "unconnected-(U1-NC-Pad15)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -5.6 3.599999 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "unconnected-(U1-NC-Pad16)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at -5.6 4.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/~{WR}")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at -5.6 5.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "A19")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at -5.6 6 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "A18")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at -5.6 6.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/A12")
			(pinfunction "A17")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at -5.6 7.600001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/A11")
			(pinfunction "A16")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at -5.6 8.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/A10")
			(pinfunction "A15")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 5.6 8.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/A19")
			(pinfunction "A14")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 5.6 7.600001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/A18")
			(pinfunction "A13")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 5.6 6.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/A17")
			(pinfunction "A12")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 5.6 6 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/A16")
			(pinfunction "A11")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 5.6 5.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 5.6 4.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/A1")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 5.6 3.599999 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "unconnected-(U1-NC-Pad29)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 5.6 2.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "unconnected-(U1-NC-Pad30)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 5.6 2.000001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 5.6 1.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" smd roundrect
			(at 5.6 0.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" smd roundrect
			(at 5.6 -0.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" smd roundrect
			(at 5.6 -1.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" smd roundrect
			(at 5.6 -2.000001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" smd roundrect
			(at 5.6 -2.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "unconnected-(U1-NC-Pad37)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" smd roundrect
			(at 5.6 -3.599999 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "unconnected-(U1-NC-Pad38)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" smd roundrect
			(at 5.6 -4.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/A9")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" smd roundrect
			(at 5.6 -5.2 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/BYTE")
			(pinfunction "CE2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "41" smd roundrect
			(at 5.6 -6 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/~{RD}")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "42" smd roundrect
			(at 5.6 -6.8 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/A7")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "43" smd roundrect
			(at 5.6 -7.600001 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A8")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "44" smd roundrect
			(at 5.6 -8.4 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/A0")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP-II-44_10.16x18.41mm_P0.8mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Keystone_3028_3034_bkw"
		(layer "F.Cu")
		(at 118.35 105.025 -90)
		(descr "Keystone 3034 SMD battery holder for 2020, 2025 and 2032 coincell batteries. http://www.keyelco.com/product-pdf.cfm?p=798")
		(tags "Keystone type 3034 coin cell retainer")
		(property "Reference" "BT1"
			(at -8.75 -5.6 315)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Keystone_3028"
			(at 9.65 0.55 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/Keystone_3028.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMT 20mm x 1.6mm coin cell holder"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "Keystone 3028"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(zone_connect 2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -11.275 -2.75 180)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -11.275 0 180)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -11.275 0 270)
			(size 1.85 7.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -11.275 2.75 180)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 -2.75 180)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 0 180)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at 11.275 0 270)
			(size 1.85 7.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 2.75 180)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 43 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -9.007825 -3.731163 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -9.007825 3.731163 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -3.731163 -9.007825 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -3.731163 9.007825 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd circle
			(at 0 0 270)
			(size 18 18)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 3.731163 -9.007825 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 3.731163 9.007825 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 9.007825 -3.731163 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 9.007825 3.731163 292.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_holder_Keystone_3034.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_holder_BAT-HLD-002-SMT.STEP"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_holder_Keystone_3028.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_blank.step"
			(offset
				(xyz 0 0 1.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_blank.step"
			(hide yes)
			(offset
				(xyz 0 0 1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_blank.step"
			(hide yes)
			(offset
				(xyz 0 0 3.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSSOP-24"
		(layer "F.Cu")
		(at 142.6 102.05)
		(descr "TSSOP, 24 Pin (JEDEC MO-153 Var AD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at -1.3 -2.1 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ABT841"
			(at 1 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/sn54abt841.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC 10BIT LATCH 3-STATE 24-SOIC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "SN74ABT841APW"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*24* *SO*24*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -3.575)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "OE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -2.925)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "D0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "D1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "D2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 -0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "D3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 -0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "D4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "D5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "D6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -2.9 1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "D7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -2.9 2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/BUS_A11")
			(pinfunction "D8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -2.9 2.924997)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/BUS_A10")
			(pinfunction "D9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -2.9 3.575)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 3.575)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/BLOCK")
			(pinfunction "LE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 2.925)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/A19")
			(pinfunction "O9")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/A18")
			(pinfunction "O8")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/A17")
			(pinfunction "O7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 2.9 0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/A16")
			(pinfunction "O6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 2.9 0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "O5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 2.9 -0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "O4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 2.9 -0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "O3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 2.9 -1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/A12")
			(pinfunction "O2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 2.9 -2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/A11")
			(pinfunction "O1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 2.9 -2.925)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/A10")
			(pinfunction "O0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 2.9 -3.575)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-24.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_1206"
		(layer "F.Cu")
		(at 156.499999 94.325001 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.949999 0.500001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47u"
			(at 2.849999 -0.724999 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/TDK_MLCC_Cxxxx.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 47UF 25V X5R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C3216X5R1E476M160DC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475001 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475001 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 160.800001 94.325)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R1"
			(at 2.024999 -0.625 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47k"
			(at 1.849999 0.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/sei-rmcf_rmcp.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RES 47K OHM 1% 1/8W 0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RMCF0805FT47K0"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 21 "/RAMRST")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 109.35 116.025)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:MiniNDP_Cover_M10"
		(layer "F.Cu")
		(at 143.35 105.025)
		(property "Reference" "N1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "MiniNDP_Cover_M10"
			(at 0 1.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "../COVER/MiniNDP_Cover.scad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Snap cover for MiniNDP M10"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MiniNDP_Cover_M10.stl"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Enclosure* Housing*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/MiniNDP_Cover_M10.step"
			(offset
				(xyz 0 0 -1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SOT-23"
		(layer "F.Cu")
		(at 132.1 95.325)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "DA1"
			(at 2 -1.225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BAV70"
			(at 2.025 0.075 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/BAV70.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DIODE ARRAY GP 75V 150MA SOT23-3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "BAV70-7-F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+BATT")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.15 0.95)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 1.15 0)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSSOP-16"
		(layer "F.Cu")
		(at 171.95 98.850001)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at -1.25 -1 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC4040"
			(at 1 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/4040.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC BINARY COUNTER 12-BIT 16SO"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC4040PW,118"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16* SO*16*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "unconnected-(U3-Q11-Pad1)")
			(pinfunction "Q11")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/A5")
			(pinfunction "Q5")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "/A4")
			(pinfunction "Q4")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/A6")
			(pinfunction "Q6")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/A3")
			(pinfunction "Q3")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/A2")
			(pinfunction "Q2")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/A1")
			(pinfunction "Q1")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/A0")
			(pinfunction "Q0")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/BYTE")
			(pinfunction "CLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/BLOCK")
			(pinfunction "Reset")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A8")
			(pinfunction "Q8")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 -0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/A7")
			(pinfunction "Q7")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 -0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/A9")
			(pinfunction "Q9")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 -1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "unconnected-(U3-Q10-Pad15)")
			(pinfunction "Q10")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSSOP-16"
		(layer "F.Cu")
		(at 171.950001 108.775)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at -1.25 -1 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC238"
			(at 1 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/HC238.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC DECODER/DEMUX 1 X 3:8 16SO"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC238PW,118"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/BUS_A8")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/BUS_A9")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{E1}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/~{Y0}")
			(pinfunction "~{E2}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/(A)")
			(pinfunction "E3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "unconnected-(U2-Y7-Pad7)")
			(pinfunction "Y7")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "unconnected-(U2-Y6-Pad9)")
			(pinfunction "Y6")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "unconnected-(U2-Y5-Pad10)")
			(pinfunction "Y5")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "unconnected-(U2-Y4-Pad11)")
			(pinfunction "Y4")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/BYTE")
			(pinfunction "Y3")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 -0.325)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "unconnected-(U2-Y2-Pad13)")
			(pinfunction "Y2")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 -0.975)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/BLOCK")
			(pinfunction "Y1")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 -1.625)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "unconnected-(U2-Y0-Pad15)")
			(pinfunction "Y0")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -2.275)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_1206"
		(layer "F.Cu")
		(at 158.000001 109.725001)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.924999 -0.600001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47u"
			(at 2.924999 0.674999 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/TDK_MLCC_Cxxxx.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 47UF 25V X5R 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C3216X5R1E476M160DC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475001 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475001 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:PinSocket_2x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 129.09 116.025 -90)
		(descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x20 2.54mm double row")
		(property "Reference" "J1"
			(at -1.293 1.67 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x20_Odd_Even"
			(at -4.333 -21.58 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "datasheets/M20-611.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CONN SOCKET VERT THT 02x20 2.54mm pitch 11mm height"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "M20-6112045"
			(at -4.593 -49.68 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "MiniNDP_M10.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.27 -24.13 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1470588235)
			(net 3 "VBUS")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VBUS")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0 -5.079999 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/AD1")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at -2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/AD0")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/AD3")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at -2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/AD2")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/AD5")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at -2.54 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/AD4")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 0 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/AD7")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at -2.54 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/AD6")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 0 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/BUS_A9")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at -2.54 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/BUS_A8")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 0 -17.780001 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/BUS_A11")
			(pinfunction "Pin_15")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at -2.54 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/BUS_A10")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 0 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J1-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at -2.54 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(J1-Pin_18-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at 0 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J1-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at -2.54 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(J1-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole circle
			(at 0 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole circle
			(at -2.54 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole circle
			(at 0 -27.939999 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/~{WR}")
			(pinfunction "Pin_23")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole circle
			(at -2.54 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/~{RD}")
			(pinfunction "Pin_24")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole circle
			(at 0 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(J1-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole circle
			(at -2.54 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(J1-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole circle
			(at 0 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(J1-Pin_27-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole circle
			(at -2.54 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "unconnected-(J1-Pin_28-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" thru_hole circle
			(at 0 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/~{Y0}")
			(pinfunction "Pin_29")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" thru_hole circle
			(at -2.54 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J1-Pin_30-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" thru_hole circle
			(at 0 -38.099999 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J1-Pin_31-Pad31)")
			(pinfunction "Pin_31")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" thru_hole circle
			(at -2.54 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/(A)")
			(pinfunction "Pin_32")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" thru_hole circle
			(at 0 -40.640001 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "unconnected-(J1-Pin_33-Pad33)")
			(pinfunction "Pin_33")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" thru_hole circle
			(at -2.54 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "unconnected-(J1-Pin_34-Pad34)")
			(pinfunction "Pin_34")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" thru_hole circle
			(at 0 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_35")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" thru_hole circle
			(at -2.54 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_36")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" thru_hole circle
			(at 0 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J1-Pin_37-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" thru_hole circle
			(at -2.54 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/RAMRST")
			(pinfunction "Pin_38")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" thru_hole circle
			(at 0 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J1-Pin_39-Pad39)")
			(pinfunction "Pin_39")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" thru_hole circle
			(at -2.54 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(J1-Pin_40-Pad40)")
			(pinfunction "Pin_40")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/M20-6112045.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 107.349999 94.024999)
		(mid 107.935785 92.610785)
		(end 109.349999 92.024999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.349999 116.025)
		(end 107.349999 94.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.349999 92.024999)
		(end 177.35 92.024999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.35 118.025001)
		(mid 107.935786 117.439214)
		(end 107.349999 116.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.349999 92.024999)
		(mid 178.764213 92.610786)
		(end 179.35 94.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.35 118.025)
		(end 109.35 118.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.35 94.025)
		(end 179.35 116.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.35 116.025)
		(mid 178.764213 117.439214)
		(end 177.349999 118.025001)
		(layer "Edge.Cuts")
	)
	(gr_text "CR2012 / CR2016"
		(at 108.35 105.025 270)
		(layer "F.SilkS")
	)
	(gr_text "1M RAM Disk for Olivetti M-10"
		(at 139.92 111.088 0)
		(layer "F.SilkS")
	)
	(gr_text "${TITLE} ${REVISION}"
		(at 139.92 109.183 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 127.185 116.025 0)
		(layer "F.SilkS")
	)
	(gr_text "BASIC to bootstrap\nRAMM10.CO\npreviously saved\nas the first file\nin bank 0"
		(at 170.35 104.875 0)
		(layer "B.SilkS")
	)
	(gr_text "BATTERY\nCR2012\nCR2016"
		(at 108.5 116.775 0)
		(layer "B.SilkS")
	)
	(gr_text "1M RAM DISK\nfor\nOlivetti M-10"
		(at 114.85 96.375 0)
		(layer "B.SilkS")
	)
	(gr_text "${COMMENT1} - ${REVISION}"
		(at 143.35 99.075 0)
		(layer "B.SilkS")
	)
	(gr_text "${TITLE}"
		(at 143.35 95.525 0)
		(layer "B.SilkS")
	)
	(gr_text "bank 0-3:      P=129 '133 137 141\nblock N 0-255: OUT P,N\nread byte:     D=INP(131)\nwrite byte:    OUT 131,D"
		(at 178.45 95.475 0)
		(layer "B.SilkS")
	)
	(gr_text "1 CLEAR0,61558:T=61558:E=62957:OUT129,2\n2 FORA=0TO15:N=INP(131):NEXT:FORA=TTOE\n3 POKEA,INP(131):IFA=T+1007THENOUT129,1\n4 ?{dblquote}.{dblquote};:NEXT:SAVEM{dblquote}RAMDSK{dblquote},T,E,T"
		(at 160.95 101.525 0)
		(layer "B.SilkS")
	)
	(gr_text "Use ENIG copper finish\nfor gold battery contact.\n"
		(at 118.35 91.025 0)
		(layer "Eco1.User")
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.304804 102.475) (xy 140.384336 102.479668) (xy 140.444931 102.492342) (xy 140.547187 102.540561)
				(xy 140.628815 102.583285) (xy 140.751227 102.620196) (xy 140.801 102.375) (xy 140.751227 102.129804)
				(xy 140.614585 102.173094) (xy 140.547186 102.209439) (xy 140.45229 102.255353) (xy 140.389128 102.269681)
				(xy 140.304804 102.275)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.450001 107.975) (xy 169.650001 107.975) (xy 169.650001 108.275) (xy 168.450001 108.275)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.954804 99.225) (xy 141.034336 99.229668) (xy 141.094931 99.242342) (xy 141.197187 99.290561)
				(xy 141.278815 99.333285) (xy 141.401227 99.370196) (xy 141.451 99.125) (xy 141.401227 98.879804)
				(xy 141.264585 98.923094) (xy 141.197186 98.959439) (xy 141.10229 99.005353) (xy 141.039128 99.019681)
				(xy 140.954804 99.025)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.275 99.925001) (xy 168.300352 99.9245) (xy 168.418637 99.930525) (xy 168.471699 99.951167)
				(xy 168.504015 99.99334) (xy 169.051 99.825001) (xy 168.504015 99.656662) (xy 168.471972 99.69865)
				(xy 168.409213 99.721246) (xy 168.300353 99.725502) (xy 168.275 99.725001)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 100.975) (xy 146.249647 100.975501) (xy 146.131363 100.969476) (xy 146.078301 100.948834)
				(xy 146.045985 100.906661) (xy 145.499 101.075) (xy 146.045985 101.243339) (xy 146.078029 101.201351)
				(xy 146.140788 101.178755) (xy 146.249648 101.174499) (xy 146.275 101.175)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.831637 106.858497) (xy 164.801555 106.975776) (xy 164.774443 107.041351) (xy 164.737799 107.099154)
				(xy 164.704676 107.130891) (xy 164.665546 107.150144) (xy 164.648781 107.15348) (xy 164.849794 107.625978)
				(xy 165.090486 107.202165) (xy 165.044857 107.165827) (xy 165.019338 107.098247) (xy 165.015442 106.991216)
				(xy 165.027265 106.900079)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30136)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.132789 99.309202) (xy 174.143509 99.306079) (xy 174.184743 99.295203) (xy 174.23189 99.290523)
				(xy 174.274973 99.302936) (xy 174.304015 99.34334) (xy 174.850866 99.174501) (xy 174.268966 99.035598)
				(xy 174.246127 99.071724) (xy 174.181633 99.102259) (xy 174.085318 99.12462) (xy 174.032788 99.135999)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 100.325) (xy 140.449647 100.325501) (xy 140.331363 100.319476) (xy 140.278301 100.298834)
				(xy 140.245985 100.256661) (xy 139.699 100.425) (xy 140.245985 100.593339) (xy 140.278029 100.551351)
				(xy 140.340788 100.528755) (xy 140.449648 100.524499) (xy 140.475 100.525)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.304804 103.775) (xy 140.384336 103.779668) (xy 140.444931 103.792342) (xy 140.547187 103.840561)
				(xy 140.628815 103.883285) (xy 140.751227 103.920196) (xy 140.801 103.675) (xy 140.751227 103.429804)
				(xy 140.614585 103.473094) (xy 140.547186 103.509439) (xy 140.45229 103.555353) (xy 140.389128 103.569681)
				(xy 140.304804 103.575)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/A6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.275 98.625001) (xy 168.300352 98.6245) (xy 168.418637 98.630525) (xy 168.471699 98.651167)
				(xy 168.504015 98.69334) (xy 169.051 98.525001) (xy 168.504015 98.356662) (xy 168.471972 98.39865)
				(xy 168.409213 98.421246) (xy 168.300353 98.425502) (xy 168.275 98.425001)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.1 108.583888) (xy 173.087281 108.815328) (xy 173.079552 108.95701) (xy 173.105764 109.158527)
				(xy 173.4 109.101) (xy 173.649441 108.933329) (xy 173.574856 108.852459) (xy 173.482783 108.799486)
				(xy 173.450732 108.785868) (xy 173.392008 108.759245) (xy 173.344102 108.724073) (xy 173.311828 108.669304)
				(xy 173.3 108.583888)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30125)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.94313 99.915374) (xy 138.977332 99.911104) (xy 139.09439 99.903448) (xy 139.148788 99.916097)
				(xy 139.1875 99.95) (xy 139.700984 99.774827) (xy 139.122048 99.630985) (xy 139.098553 99.674552)
				(xy 139.04226 99.702123) (xy 138.933338 99.716643) (xy 138.908401 99.718413)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.349992 97.126195) (xy 151.356875 97.043288) (xy 151.385054 96.948305) (xy 151.411936 96.9038)
				(xy 151.449264 96.868132) (xy 151.490485 96.847835) (xy 151.250011 96.424001) (xy 151.009515 96.847835)
				(xy 151.073655 96.887184) (xy 151.119157 96.956918) (xy 151.145618 97.058194) (xy 151.150008 97.123805)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.349999 97.175) (xy 155.356883 97.077484) (xy 155.385073 96.963844) (xy 155.411266 96.912123)
				(xy 155.44742 96.8713) (xy 155.490484 96.847835) (xy 155.249999 96.424) (xy 155.009514 96.847835)
				(xy 155.067879 96.885515) (xy 155.112676 96.958239) (xy 155.142282 97.07171) (xy 155.149999 97.175)
			)
		)
	)
	(zone
		(net 47)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.35001 106.976359) (xy 150.343127 107.043752) (xy 150.31495 107.118611) (xy 150.286805 107.155437)
				(xy 150.247306 107.185716) (xy 150.209515 107.202165) (xy 150.450013 107.625999) (xy 150.690485 107.202165)
				(xy 150.618877 107.160629) (xy 150.573352 107.094561) (xy 150.551584 107.006677) (xy 150.54999 106.973641)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/~{WR}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30122)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.453128 109.997504) (xy 153.490887 109.933987) (xy 153.527837 109.891513) (xy 153.601498 109.846047)
				(xy 153.635046 109.832506) (xy 153.703162 109.803674) (xy 153.786893 109.755867) (xy 153.648454 109.54711)
				(xy 153.402804 109.499227) (xy 153.385668 109.588551) (xy 153.351652 109.736005) (xy 153.27493 109.906702)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.632536 97.149276) (xy 162.618975 97.042251) (xy 162.627069 96.915075) (xy 162.644037 96.863991)
				(xy 162.672285 96.821948) (xy 162.7 96.8) (xy 162.449793 96.424022) (xy 162.252228 96.898822) (xy 162.311572 96.923615)
				(xy 162.364846 96.986029) (xy 162.412028 97.093896) (xy 162.436907 97.190858)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 99.675) (xy 146.249647 99.675501) (xy 146.131363 99.669476) (xy 146.078301 99.648834)
				(xy 146.045985 99.606661) (xy 145.499 99.775) (xy 146.045985 99.943339) (xy 146.078029 99.901351)
				(xy 146.140788 99.878755) (xy 146.249648 99.874499) (xy 146.275 99.875)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.978 111.801333) (xy 133.97292 111.989616) (xy 133.957363 112.142631) (xy 133.936434 112.247788)
				(xy 133.907865 112.339568) (xy 133.828894 112.49822) (xy 133.67996 112.709279) (xy 133.463251 113.012765)
				(xy 134.17 113.486) (xy 134.876749 113.012765) (xy 134.708032 112.790304) (xy 134.508991 112.581981)
				(xy 134.373209 112.441529) (xy 134.316697 112.369127) (xy 134.268772 112.28914) (xy 134.230188 112.196968)
				(xy 134.201696 112.08801) (xy 134.184049 111.957665) (xy 134.178 111.801333)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.35 106.875) (xy 158.343116 106.972519) (xy 158.314925 107.086161) (xy 158.288731 107.137881)
				(xy 158.252577 107.178702) (xy 158.209515 107.202165) (xy 158.45 107.626) (xy 158.690485 107.202165)
				(xy 158.632121 107.164485) (xy 158.587323 107.091762) (xy 158.557717 106.97829) (xy 158.55 106.875)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 175.75 96.750001) (xy 175.816278 96.755346) (xy 175.893528 96.772764) (xy 175.964106 96.799845)
				(xy 176.030789 96.839388) (xy 176.075691 96.879106) (xy 176.112206 96.927662) (xy 176.134368 96.975479)
				(xy 176.147285 97.030295) (xy 176.15 97.072224) (xy 176.776 96.8) (xy 176.23 96.4) (xy 176.197167 96.42753)
				(xy 176.119749 96.438862) (xy 175.963585 96.425791) (xy 175.900679 96.416779) (xy 175.75 96.400001)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30128)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 175.647139 100.408192) (xy 175.605259 100.402919) (xy 175.490268 100.382846) (xy 175.443229 100.359661)
				(xy 175.418592 100.321767) (xy 174.849035 100.474743) (xy 175.395985 100.64334) (xy 175.40879 100.618798)
				(xy 175.427598 100.602258) (xy 175.483378 100.587649) (xy 175.57877 100.598244) (xy 175.595374 100.601376)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.34251 109.937038) (xy 168.488756 109.89122) (xy 168.681294 109.874722) (xy 168.920388 109.896509)
				(xy 169.05871 109.925) (xy 169.050867 109.749501) (xy 168.451956 109.65267) (xy 168.433709 109.686891)
				(xy 168.372295 109.720258) (xy 168.30361 109.742912) (xy 168.242516 109.763831)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30130)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.942865 99.27738) (xy 138.980526 99.271318) (xy 139.09619 99.259045) (xy 139.149542 99.268989)
				(xy 139.1875 99.3) (xy 139.700986 99.124836) (xy 139.115938 98.99013) (xy 139.094048 99.033713)
				(xy 139.039223 99.061751) (xy 138.936264 99.077599) (xy 138.909946 99.080109)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.150008 106.976195) (xy 151.143125 107.04364) (xy 151.114945 107.118565) (xy 151.086804 107.155413)
				(xy 151.047314 107.185706) (xy 151.009515 107.202165) (xy 151.250011 107.625999) (xy 151.490485 107.202165)
				(xy 151.418846 107.16062) (xy 151.373325 107.094567) (xy 151.351577 107.006734) (xy 151.349992 106.973805)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.279446 98.704133) (xy 155.219908 98.757069) (xy 155.168098 98.790954) (xy 155.061697 98.829164)
				(xy 154.973765 98.856674) (xy 154.861107 98.917133) (xy 154.999293 99.125707) (xy 155.207867 99.263893)
				(xy 155.273876 99.136662) (xy 155.295835 99.063304) (xy 155.33047 98.963736) (xy 155.365002 98.908941)
				(xy 155.420867 98.845554)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/~{WR}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.853228 115.029432) (xy 155.947005 115.082731) (xy 156.021667 115.13692) (xy 156.074965 115.18765)
				(xy 156.115552 115.239849) (xy 156.164385 115.348275) (xy 156.182514 115.479608) (xy 156.175846 115.670208)
				(xy 156.167203 115.907813) (xy 156.174537 116.043091) (xy 156.196332 116.190827) (xy 157.030889 116.025454)
				(xy 157.195826 115.191333) (xy 156.765785 115.119399) (xy 156.579775 115.090354) (xy 156.406297 115.049025)
				(xy 156.207125 114.975842) (xy 155.944032 114.851234)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 100.325) (xy 146.249647 100.325501) (xy 146.131363 100.319476) (xy 146.078301 100.298834)
				(xy 146.045985 100.256661) (xy 145.499 100.425) (xy 146.045985 100.593339) (xy 146.078029 100.551351)
				(xy 146.140788 100.528755) (xy 146.249648 100.524499) (xy 146.275 100.525)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.705539 114.848212) (xy 137.652239 114.94199) (xy 137.59805 115.016653) (xy 137.547319 115.069951)
				(xy 137.49512 115.110538) (xy 137.386693 115.159373) (xy 137.255358 115.177504) (xy 137.064768 115.17084)
				(xy 136.827174 115.162202) (xy 136.691902 115.169538) (xy 136.544173 115.191333) (xy 136.709546 116.02589)
				(xy 137.543667 116.190827) (xy 137.615603 115.760722) (xy 137.644638 115.574731) (xy 137.68596 115.401261)
				(xy 137.759138 115.202095) (xy 137.883737 114.939016)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 99.675) (xy 140.449647 99.675501) (xy 140.331363 99.669476) (xy 140.278301 99.648834)
				(xy 140.245985 99.606661) (xy 139.699 99.775) (xy 140.245985 99.943339) (xy 140.278029 99.901351)
				(xy 140.340788 99.878755) (xy 140.449648 99.874499) (xy 140.475 99.875)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.645539 114.848212) (xy 165.592239 114.94199) (xy 165.53805 115.016653) (xy 165.487319 115.069951)
				(xy 165.43512 115.110538) (xy 165.326693 115.159373) (xy 165.195358 115.177504) (xy 165.004768 115.17084)
				(xy 164.767174 115.162202) (xy 164.631902 115.169538) (xy 164.484173 115.191333) (xy 164.649546 116.02589)
				(xy 165.483667 116.190827) (xy 165.555603 115.760722) (xy 165.584638 115.574731) (xy 165.62596 115.401261)
				(xy 165.699138 115.202095) (xy 165.823737 114.939016)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.954804 103.125) (xy 141.034336 103.129668) (xy 141.094931 103.142342) (xy 141.197187 103.190561)
				(xy 141.278815 103.233285) (xy 141.401227 103.270196) (xy 141.451 103.025) (xy 141.401227 102.779804)
				(xy 141.264585 102.823094) (xy 141.197186 102.859439) (xy 141.10229 102.905353) (xy 141.039128 102.919681)
				(xy 140.954804 102.925)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.9 105.65) (xy 139.1 105.65) (xy 139.1 106) (xy 138.9 106)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.6 108.250001) (xy 156.594734 108.328003) (xy 156.577876 108.418138) (xy 156.550309 108.507206)
				(xy 156.509987 108.595555) (xy 156.467144 108.662785) (xy 156.414423 108.723108) (xy 156.362403 108.766056)
				(xy 156.302639 108.800527) (xy 156.242638 108.822718) (xy 156.175913 108.835702) (xy 156.131622 108.838602)
				(xy 156.525 109.726001) (xy 157.1 109.788555) (xy 157.059068 109.557867) (xy 157.044445 109.26308)
				(xy 157.059636 108.879753) (xy 157.076031 108.665182) (xy 157.092707 108.442799) (xy 157.1 108.250001)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.149993 97.126129) (xy 152.156876 97.04324) (xy 152.185056 96.948279) (xy 152.21194 96.903785)
				(xy 152.24927 96.868126) (xy 152.290485 96.847835) (xy 152.050011 96.424001) (xy 151.809515 96.847835)
				(xy 151.873646 96.887181) (xy 151.919147 96.95692) (xy 151.945613 97.058212) (xy 151.950007 97.123871)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.954804 101.825) (xy 141.034336 101.829668) (xy 141.094931 101.842342) (xy 141.197187 101.890561)
				(xy 141.278815 101.933285) (xy 141.401227 101.970196) (xy 141.451 101.725) (xy 141.401227 101.479804)
				(xy 141.264585 101.523094) (xy 141.197186 101.559439) (xy 141.10229 101.605353) (xy 141.039128 101.619681)
				(xy 140.954804 101.625)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30137)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.117303 98.694684) (xy 174.139017 98.687605) (xy 174.246111 98.661576) (xy 174.2986 98.667413)
				(xy 174.3375 98.700001) (xy 174.850939 98.524659) (xy 174.25592 98.40774) (xy 174.236643 98.445502)
				(xy 174.179121 98.475349) (xy 174.095353 98.496028) (xy 174.048895 98.506748)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.825 94.625001) (xy 156.844201 94.624964) (xy 157.003217 94.62884) (xy 157.095239 94.638846)
				(xy 157.186254 94.658579) (xy 157.26925 94.6913) (xy 157.337214 94.74027) (xy 157.383135 94.80875)
				(xy 157.4 94.900001) (xy 157.976 94.325001) (xy 157.4 93.750001) (xy 157.395171 93.801087) (xy 157.381365 93.845432)
				(xy 157.330255 93.916416) (xy 157.245371 93.970181) (xy 157.118572 94.007223) (xy 156.944882 94.024036)
				(xy 156.844201 94.025038) (xy 156.825 94.025001)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 103.575) (xy 140.449647 103.575501) (xy 140.331363 103.569476) (xy 140.278301 103.548834)
				(xy 140.245985 103.506661) (xy 139.699 103.675) (xy 140.245985 103.843339) (xy 140.278029 103.801351)
				(xy 140.340788 103.778755) (xy 140.449648 103.774499) (xy 140.475 103.775)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.65 107.222943) (xy 173.645263 107.351787) (xy 173.632103 107.44266) (xy 173.606455 107.539142)
				(xy 173.555764 107.741473) (xy 173.85 107.801) (xy 174.099441 107.633329) (xy 174.006646 107.521167)
				(xy 173.966191 107.483008) (xy 173.918967 107.437215) (xy 173.882256 107.386712) (xy 173.858465 107.319342)
				(xy 173.85 107.222943)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.2 95.872) (xy 145.210984 95.973122) (xy 145.224578 96.083147) (xy 145.223397 96.191894)
				(xy 145.211749 96.239212) (xy 145.189786 96.27832) (xy 145.155302 96.306588) (xy 145.10609 96.321385)
				(xy 145.5 96.898) (xy 145.89391 96.321385) (xy 145.855821 96.31177) (xy 145.826191 96.294333) (xy 145.788668 96.240306)
				(xy 145.773302 96.152426) (xy 145.783105 96.014685) (xy 145.789016 95.973122) (xy 145.8 95.872)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.615017 106.859229) (xy 161.592937 106.964156) (xy 161.543711 107.080699) (xy 161.511522 107.12172)
				(xy 161.471892 107.150199) (xy 161.438421 107.160403) (xy 161.649817 107.625982) (xy 161.890485 107.202165)
				(xy 161.842438 107.16546) (xy 161.813117 107.096626) (xy 161.803952 106.988056) (xy 161.81161 106.895979)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30132)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.957114 103.828303) (xy 138.981645 103.822759) (xy 139.094027 103.805787) (xy 139.148122 103.815524)
				(xy 139.1875 103.85) (xy 139.700959 103.674719) (xy 139.113985 103.543052) (xy 139.092579 103.583143)
				(xy 139.035145 103.611766) (xy 138.938665 103.630428) (xy 138.900767 103.636405)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.275 97.325001) (xy 168.300352 97.3245) (xy 168.418637 97.330525) (xy 168.471699 97.351167)
				(xy 168.504015 97.39334) (xy 169.051 97.225001) (xy 168.504015 97.056662) (xy 168.471972 97.09865)
				(xy 168.409213 97.121246) (xy 168.300353 97.125502) (xy 168.275 97.125001)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.100028 101.914699) (xy 161.035538 101.963685) (xy 160.980236 101.99456) (xy 160.874865 102.027194)
				(xy 160.781444 102.053572) (xy 160.661107 102.117133) (xy 160.79924 102.325649) (xy 161.007867 102.463893)
				(xy 161.073295 102.338222) (xy 161.09342 102.276174) (xy 161.131943 102.177746) (xy 161.169441 102.125764)
				(xy 161.229919 102.066779)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/BUS_A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.359608 107.344066) (xy 168.488198 107.296143) (xy 168.660637 107.275969) (xy 168.885376 107.291524)
				(xy 169.060202 107.325) (xy 169.050782 107.149377) (xy 168.450001 107.065187) (xy 168.432258 107.098055)
				(xy 168.368058 107.134987) (xy 168.303276 107.159899) (xy 168.234911 107.1877)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.55 95.675) (xy 161.543116 95.772519) (xy 161.514925 95.886161) (xy 161.488731 95.937881)
				(xy 161.452577 95.978702) (xy 161.409515 96.002165) (xy 161.65 96.426) (xy 161.890485 96.002165)
				(xy 161.832121 95.964485) (xy 161.787323 95.891762) (xy 161.757717 95.77829) (xy 161.75 95.675)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.125 94.225) (xy 159.001929 94.205587) (xy 158.920423 94.177495) (xy 158.837041 94.137891)
				(xy 158.759349 94.089571) (xy 158.688252 94.031836) (xy 158.635867 93.975575) (xy 158.593799 93.913274)
				(xy 158.568159 93.856168) (xy 158.553241 93.79524) (xy 158.55 93.75) (xy 157.974 94.325001) (xy 158.55 94.9)
				(xy 158.568673 94.792366) (xy 158.62486 94.688671) (xy 158.721458 94.589183) (xy 158.858375 94.500879)
				(xy 159.018199 94.440085) (xy 159.125 94.425)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 99.025) (xy 140.449647 99.025501) (xy 140.331363 99.019476) (xy 140.278301 98.998834)
				(xy 140.245985 98.956661) (xy 139.699 99.125) (xy 140.245985 99.293339) (xy 140.278029 99.251351)
				(xy 140.340788 99.228755) (xy 140.449648 99.224499) (xy 140.475 99.225)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.429133 99.695554) (xy 163.482069 99.755092) (xy 163.515954 99.806901) (xy 163.554164 99.913303)
				(xy 163.581674 100.001234) (xy 163.642133 100.113893) (xy 163.850707 99.975707) (xy 163.988893 99.767133)
				(xy 163.861662 99.701123) (xy 163.788303 99.679164) (xy 163.688735 99.644529) (xy 163.633941 99.609998)
				(xy 163.570554 99.554133)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.749989 97.126389) (xy 149.756871 97.043429) (xy 149.785048 96.948376) (xy 149.811926 96.90384)
				(xy 149.849249 96.868149) (xy 149.890484 96.847835) (xy 149.650012 96.424001) (xy 149.409514 96.847835)
				(xy 149.47368 96.887191) (xy 149.519184 96.956913) (xy 149.545631 97.058139) (xy 149.550009 97.123611)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.54999 97.126359) (xy 150.556872 97.043408) (xy 150.585049 96.948366) (xy 150.611928 96.903835)
				(xy 150.649251 96.868147) (xy 150.690485 96.847835) (xy 150.450013 96.424001) (xy 150.209515 96.847835)
				(xy 150.273677 96.88719) (xy 150.319181 96.956914) (xy 150.34563 97.058147) (xy 150.35001 97.123641)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.16554 114.848212) (xy 135.112241 114.94199) (xy 135.058051 115.016653) (xy 135.007321 115.069951)
				(xy 134.955122 115.110539) (xy 134.846696 115.159373) (xy 134.715361 115.177504) (xy 134.524769 115.17084)
				(xy 134.287174 115.162202) (xy 134.151902 115.169538) (xy 134.004172 115.191333) (xy 134.169545 116.02589)
				(xy 135.003666 116.190827) (xy 135.075603 115.760725) (xy 135.104639 115.574732) (xy 135.145962 115.401261)
				(xy 135.219139 115.202095) (xy 135.343738 114.939014)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.15 106.875) (xy 159.143116 106.972519) (xy 159.114925 107.086161) (xy 159.088732 107.137881)
				(xy 159.052577 107.178702) (xy 159.009516 107.202165) (xy 159.250001 107.626) (xy 159.490486 107.202165)
				(xy 159.432121 107.164485) (xy 159.387324 107.091762) (xy 159.357717 106.978291) (xy 159.35 106.875)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.304804 101.175) (xy 140.384336 101.179668) (xy 140.444931 101.192342) (xy 140.547187 101.240561)
				(xy 140.628815 101.283285) (xy 140.751227 101.320196) (xy 140.801 101.075) (xy 140.751227 100.829804)
				(xy 140.614585 100.873094) (xy 140.547186 100.909439) (xy 140.45229 100.955353) (xy 140.389128 100.969681)
				(xy 140.304804 100.975)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.950007 106.976129) (xy 151.943124 107.043595) (xy 151.914942 107.118547) (xy 151.886804 107.155404)
				(xy 151.847317 107.185702) (xy 151.809515 107.202165) (xy 152.050011 107.625999) (xy 152.290485 107.202165)
				(xy 152.218834 107.160616) (xy 152.173314 107.09457) (xy 152.151575 107.006757) (xy 152.149993 106.973871)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.608757 112.365178) (xy 145.717208 112.480627) (xy 145.800509 112.584626) (xy 145.856487 112.670241)
				(xy 145.897915 112.751526) (xy 145.947111 112.908917) (xy 145.971684 113.108589) (xy 145.9759 113.166078)
				(xy 145.994556 113.381371) (xy 146.036333 113.650827) (xy 146.870707 113.485707) (xy 147.035827 112.651333)
				(xy 146.724143 112.605087) (xy 146.551078 112.5909) (xy 146.347533 112.571454) (xy 146.255092 112.553329)
				(xy 146.164338 112.524438) (xy 146.071869 112.480908) (xy 145.974287 112.418867) (xy 145.86819 112.334441)
				(xy 145.750178 112.223757)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 100.975) (xy 140.449647 100.975501) (xy 140.331363 100.969476) (xy 140.278301 100.948834)
				(xy 140.245985 100.906661) (xy 139.699 101.075) (xy 140.245985 101.243339) (xy 140.278029 101.201351)
				(xy 140.340788 101.178755) (xy 140.449648 101.174499) (xy 140.475 101.175)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 175.75 106.675) (xy 175.816278 106.680345) (xy 175.893528 106.697763) (xy 175.964106 106.724844)
				(xy 176.030788 106.764387) (xy 176.075691 106.804105) (xy 176.112206 106.852661) (xy 176.134368 106.900478)
				(xy 176.147285 106.955295) (xy 176.15 106.997224) (xy 176.776 106.725) (xy 176.819343 106.325) (xy 176.626239 106.356897)
				(xy 176.369596 106.362639) (xy 176.038598 106.341778) (xy 175.75 106.325)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.275 100.575001) (xy 168.300352 100.5745) (xy 168.418637 100.580525) (xy 168.471699 100.601167)
				(xy 168.504015 100.64334) (xy 169.051 100.475001) (xy 168.504015 100.306662) (xy 168.471972 100.34865)
				(xy 168.409213 100.371246) (xy 168.300353 100.375502) (xy 168.275 100.375001)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.054804 105.725) (xy 146.134336 105.729668) (xy 146.194931 105.742342) (xy 146.297187 105.790561)
				(xy 146.378815 105.833285) (xy 146.501227 105.870196) (xy 146.551 105.625) (xy 146.501227 105.379804)
				(xy 146.364585 105.423094) (xy 146.297186 105.459439) (xy 146.20229 105.505353) (xy 146.139128 105.519681)
				(xy 146.054804 105.525)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.075001 109.25) (xy 174.14158 109.240878) (xy 174.254555 109.228745) (xy 174.303454 109.240592)
				(xy 174.337501 109.275) (xy 174.851001 109.1) (xy 174.337501 108.925) (xy 174.299437 108.961332)
				(xy 174.235857 108.971559) (xy 174.14158 108.959122) (xy 174.075001 108.95)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.83618 97.147357) (xy 161.821582 97.038401) (xy 161.821143 96.973377) (xy 161.829718 96.909383)
				(xy 161.84676 96.859943) (xy 161.874961 96.819502) (xy 161.9 96.8) (xy 161.649778 96.424026) (xy 161.454833 96.900563)
				(xy 161.514106 96.924907) (xy 161.567673 96.986992) (xy 161.615581 97.094786) (xy 161.641196 97.191861)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.15 97.175) (xy 156.156884 97.077484) (xy 156.185074 96.963844) (xy 156.211267 96.912123)
				(xy 156.247421 96.8713) (xy 156.290485 96.847835) (xy 156.05 96.424) (xy 155.809515 96.847835) (xy 155.86788 96.885515)
				(xy 155.912677 96.958239) (xy 155.942283 97.07171) (xy 155.95 97.175)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.958214 111.753273) (xy 128.893612 112.052645) (xy 128.830075 112.269078) (xy 128.785346 112.379469)
				(xy 128.733018 112.482312) (xy 128.577105 112.727212) (xy 128.527013 112.800627) (xy 128.383251 113.012765)
				(xy 129.089808 113.485981) (xy 129.923667 113.319173) (xy 129.854391 113.060745) (xy 129.761892 112.842887)
				(xy 129.680819 112.692904) (xy 129.596058 112.532933) (xy 129.561986 112.450557) (xy 129.535862 112.361718)
				(xy 129.519496 112.262762) (xy 129.514693 112.150037) (xy 129.523263 112.019891) (xy 129.547012 111.86867)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.55 97.175) (xy 158.556884 97.077484) (xy 158.585074 96.963844) (xy 158.611267 96.912123)
				(xy 158.647421 96.8713) (xy 158.690485 96.847835) (xy 158.45 96.424) (xy 158.209515 96.847835) (xy 158.26788 96.885515)
				(xy 158.312677 96.958239) (xy 158.342283 97.07171) (xy 158.35 97.175)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.02257 106.85882) (xy 163.997171 106.968842) (xy 163.973837 107.031334) (xy 163.942009 107.088552)
				(xy 163.909299 107.125731) (xy 163.869774 107.150328) (xy 163.843096 107.157278) (xy 164.049805 107.62598)
				(xy 164.290485 107.202165) (xy 164.243541 107.165624) (xy 164.215955 107.097355) (xy 164.209184 106.989482)
				(xy 164.218726 106.897837)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.397723 111.935019) (xy 141.463159 112.009929) (xy 141.510841 112.080035) (xy 141.540013 112.140247)
				(xy 141.556734 112.197553) (xy 141.557771 112.301975) (xy 141.520765 112.407787) (xy 141.436846 112.534011)
				(xy 141.332482 112.658217) (xy 141.220464 112.791005) (xy 141.111727 112.941285) (xy 141.019331 113.11527)
				(xy 140.983341 113.213093) (xy 140.956333 113.319173) (xy 141.790694 113.485719) (xy 142.496749 113.012765)
				(xy 142.360122 112.807368) (xy 142.172972 112.528736) (xy 142.016422 112.317093) (xy 141.82711 112.097789)
				(xy 141.541672 111.796174)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.75 95.325) (xy 161.770125 95.214474) (xy 161.797523 95.147977) (xy 161.836662 95.084392)
				(xy 161.877402 95.039012) (xy 161.926108 95.003182) (xy 161.971441 94.983507) (xy 162.022075 94.974158)
				(xy 162.036842 94.973639) (xy 161.75 94.324) (xy 161.405328 94.931788) (xy 161.456816 94.959451)
				(xy 161.499953 95.026198) (xy 161.533941 95.145523) (xy 161.55 95.325)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.35 98.629804) (xy 158.345332 98.709336) (xy 158.332658 98.769931) (xy 158.284439 98.872186)
				(xy 158.241714 98.953815) (xy 158.204804 99.076227) (xy 158.45 99.126) (xy 158.695196 99.076227)
				(xy 158.651905 98.939584) (xy 158.615561 98.872187) (xy 158.569647 98.777291) (xy 158.555319 98.714128)
				(xy 158.55 98.629804)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.8 106.425) (xy 177.698878 106.435984) (xy 177.588853 106.449578) (xy 177.480107 106.448397)
				(xy 177.432788 106.436748) (xy 177.39368 106.414786) (xy 177.365412 106.380302) (xy 177.350615 106.33109)
				(xy 176.774 106.725) (xy 177.350615 107.11891) (xy 177.36023 107.080821) (xy 177.377668 107.051191)
				(xy 177.431695 107.013668) (xy 177.519574 106.998302) (xy 177.657316 107.008105) (xy 177.698878 107.014016)
				(xy 177.8 107.025)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.15 105.970196) (xy 156.154668 105.890664) (xy 156.167342 105.830069) (xy 156.215561 105.727813)
				(xy 156.258285 105.646184) (xy 156.295196 105.523773) (xy 156.05 105.474) (xy 155.804804 105.523773)
				(xy 155.848094 105.660415) (xy 155.884439 105.727813) (xy 155.930353 105.822709) (xy 155.944681 105.885872)
				(xy 155.95 105.970196)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.55 105.970196) (xy 158.554668 105.890664) (xy 158.567342 105.830069) (xy 158.615561 105.727813)
				(xy 158.658285 105.646184) (xy 158.695196 105.523773) (xy 158.45 105.474) (xy 158.204804 105.523773)
				(xy 158.248094 105.660415) (xy 158.284439 105.727813) (xy 158.330353 105.822709) (xy 158.344681 105.885872)
				(xy 158.35 105.970196)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.626826 106.85708) (xy 165.59552 106.979702) (xy 165.567063 107.047807) (xy 165.5284 107.106704)
				(xy 165.495493 107.136335) (xy 165.456845 107.153587) (xy 165.445486 107.155682) (xy 165.649778 107.625974)
				(xy 165.890485 107.202165) (xy 165.843252 107.16569) (xy 165.816262 107.098327) (xy 165.81074 106.99261)
				(xy 165.82181 106.901586)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/BUS_A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30135)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.964888 104.478798) (xy 138.983858 104.473831) (xy 139.093571 104.454487) (xy 139.147611 104.463978)
				(xy 139.1875 104.5) (xy 139.700939 104.324658) (xy 139.112628 104.195083) (xy 139.09156 104.233604)
				(xy 139.032819 104.26275) (xy 138.939967 104.282652) (xy 138.896484 104.29086)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30138)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.35 98.125) (xy 145.358916 98.173117) (xy 145.371287 98.257247) (xy 145.35952 98.287933)
				(xy 145.325 98.3) (xy 145.5 98.476) (xy 145.675 98.3) (xy 145.650797 98.295313) (xy 145.636229 98.282502)
				(xy 145.628667 98.239851) (xy 145.641084 98.173117) (xy 145.65 98.125)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/A19")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 104.875) (xy 146.249647 104.875501) (xy 146.131363 104.869476) (xy 146.078301 104.848834)
				(xy 146.045985 104.806661) (xy 145.499 104.975) (xy 146.045985 105.143339) (xy 146.078029 105.101351)
				(xy 146.140788 105.078755) (xy 146.249648 105.074499) (xy 146.275 105.075)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.35 105.970196) (xy 159.354668 105.890664) (xy 159.367342 105.830069) (xy 159.415561 105.727813)
				(xy 159.458285 105.646184) (xy 159.495196 105.523773) (xy 159.25 105.474) (xy 159.004804 105.523773)
				(xy 159.048094 105.660415) (xy 159.084439 105.727813) (xy 159.130353 105.822709) (xy 159.144681 105.885872)
				(xy 159.15 105.970196)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.075001 107.95) (xy 174.14158 107.940878) (xy 174.254555 107.928745) (xy 174.303454 107.940592)
				(xy 174.337501 107.975) (xy 174.851001 107.8) (xy 174.337501 107.625) (xy 174.299437 107.661332)
				(xy 174.235857 107.671559) (xy 174.14158 107.659122) (xy 174.075001 107.65)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 99.025) (xy 146.249647 99.025501) (xy 146.131363 99.019476) (xy 146.078301 98.998834)
				(xy 146.045985 98.956661) (xy 145.499 99.125) (xy 146.045985 99.293339) (xy 146.078029 99.251351)
				(xy 146.140788 99.228755) (xy 146.249648 99.224499) (xy 146.275 99.225)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/A6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.277627 97.125352) (xy 164.246347 96.979703) (xy 164.246825 96.89694) (xy 164.272183 96.82715)
				(xy 164.3 96.8) (xy 164.049618 96.424077) (xy 163.885884 96.917219) (xy 163.944136 96.937292) (xy 164.001374 96.996574)
				(xy 164.058479 97.104819) (xy 164.092852 97.201889)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.150001 98.629804) (xy 159.145333 98.709336) (xy 159.132659 98.769931) (xy 159.08444 98.872186)
				(xy 159.041715 98.953815) (xy 159.004805 99.076227) (xy 159.250001 99.126) (xy 159.495197 99.076227)
				(xy 159.451906 98.939584) (xy 159.415562 98.872187) (xy 159.369648 98.777291) (xy 159.35532 98.714128)
				(xy 159.350001 98.629804)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/BUS_A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30123)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.579231 110.405576) (xy 166.507327 110.60121) (xy 166.402014 110.771325) (xy 166.392133 110.786107)
				(xy 166.599691 110.925951) (xy 166.845196 110.876227) (xy 166.804964 110.748978) (xy 166.786371 110.709201)
				(xy 166.764019 110.659596) (xy 166.75036 110.60865) (xy 166.750475 110.547524) (xy 166.769442 110.467379)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.75 106.875) (xy 152.743116 106.972519) (xy 152.714925 107.086161) (xy 152.688731 107.137881)
				(xy 152.652577 107.178702) (xy 152.609515 107.202165) (xy 152.85 107.626) (xy 153.090485 107.202165)
				(xy 153.032121 107.164485) (xy 152.987323 107.091762) (xy 152.957717 106.97829) (xy 152.95 106.875)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149999 106.875) (xy 155.143115 106.972519) (xy 155.114924 107.086161) (xy 155.08873 107.137881)
				(xy 155.052576 107.178702) (xy 155.009514 107.202165) (xy 155.249999 107.626) (xy 155.490484 107.202165)
				(xy 155.43212 107.164485) (xy 155.387322 107.091762) (xy 155.357716 106.97829) (xy 155.349999 106.875)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.35 108.604804) (xy 162.345332 108.684336) (xy 162.332658 108.744931) (xy 162.284439 108.847186)
				(xy 162.241714 108.928815) (xy 162.204804 109.051227) (xy 162.45 109.101) (xy 162.695196 109.051227)
				(xy 162.651905 108.914584) (xy 162.615561 108.847187) (xy 162.569647 108.752291) (xy 162.555319 108.689128)
				(xy 162.55 108.604804)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30131)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.953611 103.17568) (xy 138.981718 103.170184) (xy 139.094852 103.155866) (xy 139.148597 103.166234)
				(xy 139.1875 103.2) (xy 139.700965 103.024742) (xy 139.115728 102.890443) (xy 139.093875 102.931667)
				(xy 139.036946 102.960106) (xy 138.935491 102.97805) (xy 138.901844 102.982497)
			)
		)
	)
	(zone
		(net 47)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 103.575) (xy 146.249647 103.575501) (xy 146.131363 103.569476) (xy 146.078301 103.548834)
				(xy 146.045985 103.506661) (xy 145.499 103.675) (xy 146.045985 103.843339) (xy 146.078029 103.801351)
				(xy 146.140788 103.778755) (xy 146.249648 103.774499) (xy 146.275 103.775)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/A19")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.750015 106.976694) (xy 148.743133 107.04398) (xy 148.714962 107.118702) (xy 148.686808 107.155484)
				(xy 148.647291 107.185734) (xy 148.609515 107.202165) (xy 148.850016 107.625999) (xy 149.090485 107.202165)
				(xy 149.018939 107.160647) (xy 148.973408 107.094548) (xy 148.951596 107.006561) (xy 148.949985 106.973306)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.063254 97.0091) (xy 165.987596 96.909832) (xy 165.925451 96.760388) (xy 165.904401 96.669875)
				(xy 165.892414 96.572486) (xy 165.890506 96.472387) (xy 165.899291 96.368686) (xy 165.9 96.363639)
				(xy 165.649219 96.424377) (xy 165.631807 96.925) (xy 165.690048 96.940154) (xy 165.775759 97.001551)
				(xy 165.88566 97.111042) (xy 165.938556 97.165467)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.149822 112.223757) (xy 158.034373 112.332208) (xy 157.930373 112.415509) (xy 157.844758 112.471487)
				(xy 157.763473 112.512915) (xy 157.606082 112.562111) (xy 157.40641 112.586684) (xy 157.348922 112.5909)
				(xy 157.133629 112.609556) (xy 156.864173 112.651333) (xy 157.029293 113.485707) (xy 157.863667 113.650827)
				(xy 157.909912 113.339143) (xy 157.924099 113.166079) (xy 157.943545 112.962534) (xy 157.96167 112.870092)
				(xy 157.990561 112.779338) (xy 158.034091 112.68687) (xy 158.096133 112.589287) (xy 158.180559 112.48319)
				(xy 158.291243 112.365178)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 105.525) (xy 146.249647 105.525501) (xy 146.131363 105.519476) (xy 146.078301 105.498834)
				(xy 146.045985 105.456661) (xy 145.499 105.625) (xy 146.045985 105.793339) (xy 146.078029 105.751351)
				(xy 146.140788 105.728755) (xy 146.249648 105.724499) (xy 146.275 105.725)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.61 111.801333) (xy 136.605052 111.959654) (xy 136.590415 112.092095) (xy 136.569459 112.192216)
				(xy 136.541276 112.278987) (xy 136.464771 112.425066) (xy 136.340958 112.583631) (xy 136.303288 112.627263)
				(xy 136.164244 112.79269) (xy 136.003251 113.012765) (xy 136.71 113.486) (xy 137.416749 113.012765)
				(xy 137.229056 112.759671) (xy 137.116712 112.627263) (xy 136.986535 112.469586) (xy 136.933985 112.391403)
				(xy 136.890242 112.306801) (xy 136.855637 112.210636) (xy 136.830506 112.097765) (xy 136.815182 111.963045)
				(xy 136.81 111.801333)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.150002 94.425) (xy 159.272161 94.445663) (xy 159.342705 94.472818) (xy 159.408432 94.511892)
				(xy 159.450009 94.54956) (xy 159.480951 94.594529) (xy 159.49501 94.632657) (xy 159.500002 94.675)
				(xy 159.851002 94.325) (xy 159.500002 93.975) (xy 159.481723 94.053919) (xy 159.42829 94.122003)
				(xy 159.336736 94.179968) (xy 159.212814 94.218716) (xy 159.150002 94.225)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.949985 97.126694) (xy 148.956866 97.043655) (xy 148.985036 96.948496) (xy 149.011908 96.903909)
				(xy 149.049221 96.868179) (xy 149.090485 96.847835) (xy 148.850016 96.424001) (xy 148.609515 96.847835)
				(xy 148.673722 96.887203) (xy 148.719231 96.956906) (xy 148.745656 97.058053) (xy 148.750015 97.123306)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.245569 114.84823) (xy 140.19227 114.942007) (xy 140.138081 115.016669) (xy 140.087351 115.069966)
				(xy 140.035152 115.110553) (xy 139.926726 115.159387) (xy 139.795393 115.177516) (xy 139.604793 115.170847)
				(xy 139.367187 115.162204) (xy 139.231909 115.169538) (xy 139.084173 115.191333) (xy 139.249546 116.02589)
				(xy 140.083667 116.190827) (xy 140.1556 115.760791) (xy 140.184645 115.57478) (xy 140.225975 115.4013)
				(xy 140.299159 115.202127) (xy 140.423767 114.939032)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.275 97.975001) (xy 168.300352 97.9745) (xy 168.418637 97.980525) (xy 168.471699 98.001167)
				(xy 168.504015 98.04334) (xy 169.051 97.875001) (xy 168.504015 97.706662) (xy 168.471972 97.74865)
				(xy 168.409213 97.771246) (xy 168.300353 97.775502) (xy 168.275 97.775001)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 102.275) (xy 140.449647 102.275501) (xy 140.331363 102.269476) (xy 140.278301 102.248834)
				(xy 140.245985 102.206661) (xy 139.699 102.375) (xy 140.245985 102.543339) (xy 140.278029 102.501351)
				(xy 140.340788 102.478755) (xy 140.449648 102.474499) (xy 140.475 102.475)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.336046 106.700109) (xy 168.423617 106.673059) (xy 168.522819 106.653236) (xy 168.633775 106.641692)
				(xy 168.755328 106.639685) (xy 168.884237 106.648053) (xy 169.022213 106.667712) (xy 169.060487 106.675)
				(xy 169.050867 106.4995) (xy 168.450076 106.412122) (xy 168.432305 106.44996) (xy 168.374143 106.484155)
				(xy 168.285165 106.512217) (xy 168.236045 106.526905)
			)
		)
	)
	(zone
		(net 51)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30120)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.275 99.275001) (xy 168.300352 99.2745) (xy 168.418637 99.280525) (xy 168.471699 99.301167)
				(xy 168.504015 99.34334) (xy 169.051 99.175001) (xy 168.504015 99.006662) (xy 168.471972 99.04865)
				(xy 168.409213 99.071246) (xy 168.300353 99.075502) (xy 168.275 99.075001)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.062611 97.1091) (xy 165.040439 97.030439) (xy 165.031987 96.932529) (xy 165.040222 96.8808)
				(xy 165.061547 96.835393) (xy 165.100001 96.8) (xy 164.849501 96.424134) (xy 164.680514 96.91615)
				(xy 164.734354 96.936523) (xy 164.791257 96.998615) (xy 164.852867 97.115668) (xy 164.88721 97.203174)
				(xy 164.889407 97.209099)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30127)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 175.642064 99.753631) (xy 175.603171 99.749508) (xy 175.488354 99.731277) (xy 175.440696 99.708228)
				(xy 175.415028 99.669385) (xy 174.84902 99.824806) (xy 175.395985 99.99334) (xy 175.408686 99.969292)
				(xy 175.42754 99.952862) (xy 175.484673 99.937513) (xy 175.584308 99.94669) (xy 175.603046 99.949787)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.15 111.801333) (xy 139.145052 111.959654) (xy 139.130415 112.092095) (xy 139.109459 112.192216)
				(xy 139.081276 112.278987) (xy 139.004771 112.425066) (xy 138.880958 112.583631) (xy 138.843288 112.627263)
				(xy 138.704244 112.79269) (xy 138.543251 113.012765) (xy 139.25 113.486) (xy 139.956749 113.012765)
				(xy 139.769056 112.759671) (xy 139.656712 112.627263) (xy 139.526535 112.469586) (xy 139.473985 112.391403)
				(xy 139.430242 112.306801) (xy 139.395637 112.210636) (xy 139.370506 112.097765) (xy 139.355182 111.963045)
				(xy 139.35 111.801333)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.65 97.922) (xy 145.655689 97.834702) (xy 145.675513 97.729108) (xy 145.702369 97.64801)
				(xy 145.741425 97.574199) (xy 145.77744 97.530494) (xy 145.8211 97.496979) (xy 145.89391 97.472615)
				(xy 145.5 96.896) (xy 145.10609 97.472615) (xy 145.185846 97.501177) (xy 145.251408 97.564028) (xy 145.304731 97.666045)
				(xy 145.340702 97.80841) (xy 145.35 97.922)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30129)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 175.647139 100.408192) (xy 175.605259 100.402919) (xy 175.490268 100.382846) (xy 175.443229 100.359661)
				(xy 175.418592 100.321767) (xy 174.849035 100.474743) (xy 175.395985 100.64334) (xy 175.40879 100.618798)
				(xy 175.427598 100.602258) (xy 175.483378 100.587649) (xy 175.57877 100.598244) (xy 175.595374 100.601376)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/~{WR}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.95 97.175) (xy 152.956884 97.077484) (xy 152.985074 96.963844) (xy 153.011267 96.912123)
				(xy 153.047421 96.8713) (xy 153.090485 96.847835) (xy 152.85 96.424) (xy 152.609515 96.847835) (xy 152.66788 96.885515)
				(xy 152.712677 96.958239) (xy 152.742283 97.07171) (xy 152.75 97.175)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30124)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.974399 110.492696) (xy 165.937549 110.550062) (xy 165.901186 110.588556) (xy 165.828798 110.628039)
				(xy 165.785255 110.641072) (xy 165.706682 110.666432) (xy 165.611107 110.717133) (xy 165.74952 110.925877)
				(xy 165.995196 110.973773) (xy 166.031962 110.821394) (xy 166.077059 110.719369) (xy 166.106769 110.665995)
				(xy 166.149824 110.588745)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.350001 97.175) (xy 159.356885 97.077484) (xy 159.385075 96.963844) (xy 159.411268 96.912123)
				(xy 159.447422 96.8713) (xy 159.490486 96.847835) (xy 159.250001 96.424) (xy 159.009516 96.847835)
				(xy 159.067881 96.885515) (xy 159.112678 96.958239) (xy 159.142284 97.07171) (xy 159.150001 97.175)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.34251 109.287038) (xy 168.488756 109.24122) (xy 168.681294 109.224722) (xy 168.920388 109.246509)
				(xy 169.05871 109.275) (xy 169.050867 109.099501) (xy 168.451956 109.00267) (xy 168.433709 109.036891)
				(xy 168.372295 109.070258) (xy 168.30361 109.092912) (xy 168.242516 109.113831)
			)
		)
	)
	(zone
		(net 43)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 123.025 94.075) (xy 122.847954 94.054643) (xy 122.740234 94.026783) (xy 122.628657 93.986677)
				(xy 122.526143 93.93861) (xy 122.427357 93.879624) (xy 122.347094 93.819258) (xy 122.274397 93.750277)
				(xy 122.218876 93.682925) (xy 122.172261 93.60878) (xy 122.139205 93.536331) (xy 122.115571 93.458237)
				(xy 122.1 93.318137) (xy 118.349 93.75) (xy 118.287458 94.675) (xy 119.152538 94.625267) (xy 120.077336 94.608342)
				(xy 121.110123 94.623401) (xy 121.827632 94.646237) (xy 122.456001 94.666248) (xy 123.025 94.675)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.55 111.923183) (xy 167.545114 112.03157) (xy 167.53091 112.124923) (xy 167.509628 112.200521)
				(xy 167.481257 112.265525) (xy 167.40591 112.368688) (xy 167.299543 112.451649) (xy 167.138546 112.532726)
				(xy 167.089001 112.554345) (xy 166.937466 112.623149) (xy 166.781573 112.712183) (xy 166.627956 112.836902)
				(xy 166.554075 112.917474) (xy 166.483251 113.012765) (xy 167.19 113.486) (xy 168.023667 113.319173)
				(xy 167.933112 112.943422) (xy 167.874738 112.754211) (xy 167.824581 112.590802) (xy 167.78511 112.419316)
				(xy 167.759268 112.207521) (xy 167.75 111.923183)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/BUS_A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.696233 114.939031) (xy 145.797417 115.148603) (xy 145.865463 115.315084) (xy 145.903668 115.434846)
				(xy 145.930004 115.546819) (xy 145.9644 115.760793) (xy 146.036334 116.190827) (xy 146.870455 116.02589)
				(xy 147.035828 115.191333) (xy 146.811018 115.163977) (xy 146.575493 115.167066) (xy 146.515206 115.170847)
				(xy 146.324793 115.177522) (xy 146.23946 115.169547) (xy 146.159472 115.14842) (xy 146.083903 115.109933)
				(xy 146.011825 115.049878) (xy 145.94231 114.964046) (xy 145.874431 114.848229)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.785569 114.84823) (xy 142.73227 114.942007) (xy 142.678081 115.016669) (xy 142.627351 115.069966)
				(xy 142.575152 115.110553) (xy 142.466726 115.159387) (xy 142.335393 115.177516) (xy 142.144793 115.170847)
				(xy 141.907187 115.162204) (xy 141.771909 115.169538) (xy 141.624173 115.191333) (xy 141.789546 116.02589)
				(xy 142.623667 116.190827) (xy 142.6956 115.760791) (xy 142.724645 115.57478) (xy 142.765975 115.4013)
				(xy 142.839159 115.202127) (xy 142.963767 114.939032)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.349999 105.970196) (xy 155.354667 105.890664) (xy 155.367341 105.830069) (xy 155.41556 105.727813)
				(xy 155.458285 105.646184) (xy 155.495196 105.523773) (xy 155.25 105.474) (xy 155.004804 105.523773)
				(xy 155.048094 105.660415) (xy 155.084438 105.727813) (xy 155.130352 105.822709) (xy 155.14468 105.885872)
				(xy 155.149999 105.970196)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 102.275) (xy 146.249647 102.275501) (xy 146.131363 102.269476) (xy 146.078301 102.248834)
				(xy 146.045985 102.206661) (xy 145.499 102.375) (xy 146.045985 102.543339) (xy 146.078029 102.501351)
				(xy 146.140788 102.478755) (xy 146.249648 102.474499) (xy 146.275 102.475)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 102.925) (xy 146.249647 102.925501) (xy 146.131363 102.919476) (xy 146.078301 102.898834)
				(xy 146.045985 102.856661) (xy 145.499 103.025) (xy 146.045985 103.193339) (xy 146.078029 103.151351)
				(xy 146.140788 103.128755) (xy 146.249648 103.124499) (xy 146.275 103.125)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.55 108.375) (xy 162.556884 108.277484) (xy 162.585074 108.163844) (xy 162.611267 108.112123)
				(xy 162.647421 108.0713) (xy 162.690485 108.047835) (xy 162.45 107.624) (xy 162.209515 108.047835)
				(xy 162.26788 108.085515) (xy 162.312677 108.158239) (xy 162.342283 108.27171) (xy 162.35 108.375)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/A18")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 104.225) (xy 146.249647 104.225501) (xy 146.131363 104.219476) (xy 146.078301 104.198834)
				(xy 146.045985 104.156661) (xy 145.499 104.325) (xy 146.045985 104.493339) (xy 146.078029 104.451351)
				(xy 146.140788 104.428755) (xy 146.249648 104.424499) (xy 146.275 104.425)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.329446 98.704133) (xy 154.269908 98.757069) (xy 154.218098 98.790954) (xy 154.111697 98.829164)
				(xy 154.023765 98.856674) (xy 153.911107 98.917133) (xy 154.049293 99.125707) (xy 154.257867 99.263893)
				(xy 154.323876 99.136662) (xy 154.345835 99.063304) (xy 154.38047 98.963736) (xy 154.415002 98.908941)
				(xy 154.470867 98.845554)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30121)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.237581 101.47884) (xy 174.341982 101.402422) (xy 174.494652 101.341841) (xy 174.699152 101.305504)
				(xy 174.883879 101.300001) (xy 174.850707 101.124294) (xy 174.25 101.18415) (xy 174.244419 101.217399)
				(xy 174.196636 101.264016) (xy 174.150997 101.296282) (xy 174.09616 101.337419)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.444236 107.65) (xy 174.345768 107.645317) (xy 174.270899 107.632538) (xy 174.146106 107.585185)
				(xy 174.049634 107.544237) (xy 173.908527 107.505764) (xy 173.849 107.8) (xy 173.908527 108.094236)
				(xy 174.078017 108.044901) (xy 174.146106 108.014814) (xy 174.264227 107.969151) (xy 174.34144 107.955156)
				(xy 174.444236 107.95)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.275 101.625) (xy 146.249647 101.625501) (xy 146.131363 101.619476) (xy 146.078301 101.598834)
				(xy 146.045985 101.556661) (xy 145.499 101.725) (xy 146.045985 101.893339) (xy 146.078029 101.851351)
				(xy 146.140788 101.828755) (xy 146.249648 101.824499) (xy 146.275 101.825)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.95 102.820196) (xy 152.954668 102.740664) (xy 152.967342 102.680069) (xy 153.015561 102.577813)
				(xy 153.058285 102.496184) (xy 153.095196 102.373773) (xy 152.85 102.324) (xy 152.604804 102.373773)
				(xy 152.648094 102.510415) (xy 152.684439 102.577813) (xy 152.730353 102.672709) (xy 152.744681 102.735872)
				(xy 152.75 102.820196)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/A18")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.550009 106.976389) (xy 149.543126 107.043773) (xy 149.514949 107.118621) (xy 149.486803 107.155442)
				(xy 149.447302 107.185718) (xy 149.409514 107.202165) (xy 149.650012 107.625999) (xy 149.890484 107.202165)
				(xy 149.818882 107.160631) (xy 149.773357 107.09456) (xy 149.751584 107.006667) (xy 149.749989 106.973611)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.95 106.875) (xy 155.943116 106.972519) (xy 155.914925 107.086161) (xy 155.888731 107.137881)
				(xy 155.852577 107.178702) (xy 155.809515 107.202165) (xy 156.05 107.626) (xy 156.290485 107.202165)
				(xy 156.232121 107.164485) (xy 156.187323 107.091762) (xy 156.157717 106.97829) (xy 156.15 106.875)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.954804 100.525) (xy 141.034336 100.529668) (xy 141.094931 100.542342) (xy 141.197187 100.590561)
				(xy 141.278815 100.633285) (xy 141.401227 100.670196) (xy 141.451 100.425) (xy 141.401227 100.179804)
				(xy 141.264585 100.223094) (xy 141.197186 100.259439) (xy 141.10229 100.305353) (xy 141.039128 100.319681)
				(xy 140.954804 100.325)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.85 106.120196) (xy 172.854668 106.040664) (xy 172.867342 105.980069) (xy 172.915561 105.877813)
				(xy 172.958285 105.796184) (xy 172.995196 105.673773) (xy 172.75 105.624) (xy 172.504804 105.673773)
				(xy 172.548094 105.810415) (xy 172.584439 105.877813) (xy 172.630353 105.972709) (xy 172.644681 106.035872)
				(xy 172.65 106.120196)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/~{WR}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.55 106.079804) (xy 153.545332 106.159336) (xy 153.532658 106.219931) (xy 153.484439 106.322186)
				(xy 153.441714 106.403815) (xy 153.404804 106.526227) (xy 153.65 106.576) (xy 153.895196 106.526227)
				(xy 153.851905 106.389584) (xy 153.815561 106.322187) (xy 153.769647 106.227291) (xy 153.755319 106.164128)
				(xy 153.75 106.079804)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.8 96.5) (xy 177.698878 96.510984) (xy 177.588853 96.524578) (xy 177.480107 96.523397) (xy 177.432788 96.511748)
				(xy 177.39368 96.489786) (xy 177.365412 96.455302) (xy 177.350615 96.40609) (xy 176.774 96.8) (xy 177.350615 97.19391)
				(xy 177.36023 97.155821) (xy 177.377668 97.126191) (xy 177.431695 97.088668) (xy 177.519574 97.073302)
				(xy 177.657316 97.083105) (xy 177.698878 97.089016) (xy 177.8 97.1)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30126)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.947004 101.864964) (xy 138.976747 101.860764) (xy 139.093314 101.851955) (xy 139.148204 101.864771)
				(xy 139.1875 101.9) (xy 139.700978 101.724793) (xy 139.121911 101.581189) (xy 139.098444 101.623691)
				(xy 139.041261 101.651356) (xy 138.933881 101.666813) (xy 138.905424 101.669335)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.994236 108.95) (xy 173.895768 108.945317) (xy 173.820899 108.932538) (xy 173.696106 108.885185)
				(xy 173.599634 108.844237) (xy 173.458527 108.805764) (xy 173.399 109.1) (xy 173.458527 109.394236)
				(xy 173.628017 109.344901) (xy 173.696106 109.314814) (xy 173.814227 109.269151) (xy 173.89144 109.255156)
				(xy 173.994236 109.25)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.304804 99.875) (xy 140.384336 99.879668) (xy 140.444931 99.892342) (xy 140.547187 99.940561)
				(xy 140.628815 99.983285) (xy 140.751227 100.020196) (xy 140.801 99.775) (xy 140.751227 99.529804)
				(xy 140.614585 99.573094) (xy 140.547186 99.609439) (xy 140.45229 99.655353) (xy 140.389128 99.669681)
				(xy 140.304804 99.675)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 102.925) (xy 140.449647 102.925501) (xy 140.331363 102.919476) (xy 140.278301 102.898834)
				(xy 140.245985 102.856661) (xy 139.699 103.025) (xy 140.245985 103.193339) (xy 140.278029 103.151351)
				(xy 140.340788 103.128755) (xy 140.449648 103.124499) (xy 140.475 103.125)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30133)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.982919 105.111559) (xy 138.985217 105.110889) (xy 139.032276 105.098696) (xy 139.089321 105.092789)
				(xy 139.144885 105.105708) (xy 139.168528 105.123147) (xy 139.1875 105.149997) (xy 139.700866 104.974497)
				(xy 139.117736 104.837436) (xy 139.095223 104.873345) (xy 139.030888 104.903973) (xy 138.936433 104.926383)
				(xy 138.882919 104.938355)
			)
		)
	)
	(zone
		(net 43)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.872382 94.098118) (xy 121.713442 93.931339) (xy 121.616317 93.807629) (xy 121.53822 93.689279)
				(xy 121.432588 93.527772) (xy 121.099293 93.749293) (xy 120.877772 94.082588) (xy 121.039279 94.18822)
				(xy 121.227813 94.318547) (xy 121.448118 94.522382)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.475 101.625) (xy 140.449647 101.625501) (xy 140.331363 101.619476) (xy 140.278301 101.598834)
				(xy 140.245985 101.556661) (xy 139.699 101.725) (xy 140.245985 101.893339) (xy 140.278029 101.851351)
				(xy 140.340788 101.828755) (xy 140.449648 101.824499) (xy 140.475 101.825)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.9 95.800001) (xy 157.905266 95.721999) (xy 157.922124 95.631864) (xy 157.949691 95.542796)
				(xy 157.990013 95.454447) (xy 158.032856 95.387217) (xy 158.085577 95.326894) (xy 158.137597 95.283946)
				(xy 158.197361 95.249474) (xy 158.257362 95.227283) (xy 158.324087 95.214299) (xy 158.368377 95.211399)
				(xy 157.975 94.324001) (xy 157.4 94.261446) (xy 157.440932 94.492135) (xy 157.455555 94.786922)
				(xy 157.440364 95.170249) (xy 157.423969 95.38482) (xy 157.407293 95.607204) (xy 157.4 95.800001)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30134)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.110466 98.030809) (xy 174.134348 98.025029) (xy 174.244926 98.006748) (xy 174.298364 98.015889)
				(xy 174.3375 98.050001) (xy 174.850951 97.874692) (xy 174.262209 97.745711) (xy 174.241268 97.785378)
				(xy 174.183771 97.814364) (xy 174.088012 97.833884) (xy 174.048665 97.840598)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.35 108.375) (xy 163.356884 108.277484) (xy 163.385074 108.163844) (xy 163.411267 108.112123)
				(xy 163.447421 108.0713) (xy 163.490485 108.047835) (xy 163.25 107.624) (xy 163.009515 108.047835)
				(xy 163.06788 108.085515) (xy 163.112677 108.158239) (xy 163.142283 108.27171) (xy 163.15 108.375)
			)
		)
	)
	(zone
		(net 51)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.448364 97.136184) (xy 163.429855 97.027464) (xy 163.427729 96.962484) (xy 163.435597 96.898956)
				(xy 163.451922 96.853099) (xy 163.479388 96.815725) (xy 163.5 96.8) (xy 163.249761 96.42403) (xy 163.063951 96.906656)
				(xy 163.123519 96.929484) (xy 163.178104 96.989987) (xy 163.228045 97.09585) (xy 163.254177 97.184046)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.869043 112.058732) (xy 173.906269 112.243082) (xy 173.928702 112.400246) (xy 173.940903 112.66264)
				(xy 173.929819 112.867687) (xy 173.920271 113.019982) (xy 173.91914 113.1904) (xy 173.934977 113.395246)
				(xy 173.976333 113.650827) (xy 174.810222 113.485974) (xy 175.282235 112.778251) (xy 175.087483 112.669561)
				(xy 174.882821 112.594721) (xy 174.652669 112.540966) (xy 174.455031 112.494228) (xy 174.367757 112.461311)
				(xy 174.288752 112.415794) (xy 174.218448 112.353003) (xy 174.157272 112.268262) (xy 174.105655 112.156896)
				(xy 174.064028 112.014229)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.2)
			(smoothing fillet)
			(radius 0.1)
		)
		(polygon
			(pts
				(xy 179.35 118.025) (xy 179.35 92.025) (xy 107.35 92.025) (xy 107.35 118.025)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.956557 105.135135) (xy 158.995308 105.174534) (xy 159.017442 105.211256) (xy 159.026433 105.277041)
				(xy 159.01473 105.338394) (xy 158.999541 105.420447) (xy 159.004804 105.523773) (xy 159.25076 105.475649)
				(xy 159.388893 105.267133) (xy 159.307936 105.207589) (xy 159.255534 105.158486) (xy 159.218191 105.116068)
				(xy 159.166641 105.058163) (xy 159.086446 104.983055)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.329133 105.345554) (xy 172.382069 105.405092) (xy 172.415954 105.456901) (xy 172.454164 105.563303)
				(xy 172.481674 105.651234) (xy 172.542133 105.763893) (xy 172.750707 105.625707) (xy 172.888893 105.417133)
				(xy 172.761662 105.351123) (xy 172.688303 105.329164) (xy 172.588735 105.294529) (xy 172.533941 105.259998)
				(xy 172.470554 105.204133)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.39 115.168667) (xy 129.394824 115.01931) (xy 129.408596 114.890235) (xy 129.429837 114.780115)
				(xy 129.457708 114.683695) (xy 129.53465 114.510422) (xy 129.631638 114.351255) (xy 129.711833 114.222594)
				(xy 129.790665 114.073) (xy 129.862991 113.887426) (xy 129.923667 113.650827) (xy 129.09 113.484)
				(xy 128.256333 113.650827) (xy 128.290031 113.795966) (xy 128.328427 113.921594) (xy 128.420874 114.137276)
				(xy 128.548362 114.351256) (xy 128.64023 114.501139) (xy 128.717281 114.669334) (xy 128.747364 114.768736)
				(xy 128.770281 114.882842) (xy 128.784878 115.015027) (xy 128.79 115.168667)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/~{WR}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.75 107.070196) (xy 153.754668 106.990664) (xy 153.767342 106.930069) (xy 153.815561 106.827813)
				(xy 153.858285 106.746184) (xy 153.895196 106.623773) (xy 153.65 106.574) (xy 153.404804 106.623773)
				(xy 153.448094 106.760415) (xy 153.484439 106.827813) (xy 153.530353 106.922709) (xy 153.544681 106.985872)
				(xy 153.55 107.070196)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.295196 103.574997) (xy 141.215663 103.570329) (xy 141.155068 103.557655) (xy 141.052813 103.509437)
				(xy 140.971184 103.466714) (xy 140.848773 103.429804) (xy 140.799 103.675) (xy 140.848773 103.920196)
				(xy 140.985414 103.876905) (xy 141.052813 103.840559) (xy 141.147709 103.794645) (xy 141.210872 103.780316)
				(xy 141.295196 103.774997)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.30324 111.175) (xy 165.502995 111.186037) (xy 165.625091 111.192758) (xy 165.798773 111.170196)
				(xy 165.751 110.925) (xy 165.611107 110.717133) (xy 165.532138 110.789428) (xy 165.485174 110.861787)
				(xy 165.457829 110.90628) (xy 165.42442 110.942219) (xy 165.375905 110.966245) (xy 165.30324 110.975)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.554804 99.225) (xy 153.634336 99.229668) (xy 153.694931 99.242342) (xy 153.797187 99.290561)
				(xy 153.878815 99.333285) (xy 154.001227 99.370196) (xy 154.051 99.125) (xy 154.001227 98.879804)
				(xy 153.864585 98.923094) (xy 153.797186 98.959439) (xy 153.70229 99.005353) (xy 153.639128 99.019681)
				(xy 153.554804 99.025)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.805764 109.2) (xy 172.888989 109.204708) (xy 172.954514 109.217662) (xy 173.05331 109.262022)
				(xy 173.093409 109.288048) (xy 173.191663 109.3462) (xy 173.257406 109.372452) (xy 173.341473 109.394236)
				(xy 173.401 109.1) (xy 173.341473 108.805764) (xy 173.260601 108.826507) (xy 173.196727 108.851418)
				(xy 173.093409 108.911952) (xy 173.040883 108.945383) (xy 172.981776 108.973464) (xy 172.906574 108.9928)
				(xy 172.805764 109)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.073336 105.268545) (xy 158.119241 105.313183) (xy 158.147714 105.353793) (xy 158.173839 105.432259)
				(xy 158.176545 105.446225) (xy 158.195025 105.520951) (xy 158.242133 105.613893) (xy 158.450766 105.475642)
				(xy 158.498773 105.229804) (xy 158.416488 105.215283) (xy 158.312975 105.190391) (xy 158.201898 105.11534)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.304804 102.425) (xy 160.384336 102.429668) (xy 160.444931 102.442342) (xy 160.547187 102.490561)
				(xy 160.628815 102.533285) (xy 160.751227 102.570196) (xy 160.801 102.325) (xy 160.751227 102.079804)
				(xy 160.614585 102.123094) (xy 160.547186 102.159439) (xy 160.45229 102.205353) (xy 160.389128 102.219681)
				(xy 160.304804 102.225)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.945196 101.625) (xy 141.865664 101.620332) (xy 141.805069 101.607658) (xy 141.702813 101.559439)
				(xy 141.621184 101.516714) (xy 141.498773 101.479804) (xy 141.449 101.725) (xy 141.498773 101.970196)
				(xy 141.635415 101.926905) (xy 141.702813 101.890561) (xy 141.797709 101.844647) (xy 141.860872 101.830319)
				(xy 141.945196 101.825)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.720914 105.137335) (xy 155.763477 105.186687) (xy 155.787996 105.230447) (xy 155.800891 105.306592)
				(xy 155.798153 105.353398) (xy 155.794721 105.428237) (xy 155.804804 105.523773) (xy 156.050707 105.475707)
				(xy 156.188893 105.267133) (xy 156.022109 105.148902) (xy 155.884555 105.018151) (xy 155.862335 104.995914)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/~{WR}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.55 109.052804) (xy 153.545331 109.131749) (xy 153.532646 109.191991) (xy 153.483505 109.294822)
				(xy 153.440092 109.3765) (xy 153.402804 109.499227) (xy 153.648 109.549) (xy 153.893196 109.499227)
				(xy 153.84977 109.361609) (xy 153.814627 109.295564) (xy 153.769351 109.200425) (xy 153.755237 109.137191)
				(xy 153.75 109.052804)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.945196 102.925) (xy 141.865664 102.920332) (xy 141.805069 102.907658) (xy 141.702813 102.859439)
				(xy 141.621184 102.816714) (xy 141.498773 102.779804) (xy 141.449 103.025) (xy 141.498773 103.270196)
				(xy 141.635415 103.226905) (xy 141.702813 103.190561) (xy 141.797709 103.144647) (xy 141.860872 103.130319)
				(xy 141.945196 103.125)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.720554 99.545867) (xy 154.780092 99.49293) (xy 154.831901 99.459045) (xy 154.938304 99.420835)
				(xy 155.026235 99.393326) (xy 155.138893 99.332867) (xy 155.000707 99.124293) (xy 154.792133 98.986107)
				(xy 154.726123 99.113338) (xy 154.704164 99.186697) (xy 154.669529 99.286264) (xy 154.634998 99.341059)
				(xy 154.579133 99.404446)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.18548 99.49582) (xy 158.272799 99.431576) (xy 158.341393 99.401331) (xy 158.425219 99.383841)
				(xy 158.498773 99.370196) (xy 158.450773 99.124366) (xy 158.242133 98.986107) (xy 158.187751 99.095652)
				(xy 158.171597 99.157175) (xy 158.142759 99.245138) (xy 158.111264 99.290722) (xy 158.058602 99.341218)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.295196 100.975) (xy 141.215664 100.970332) (xy 141.155069 100.957658) (xy 141.052813 100.909439)
				(xy 140.971184 100.866714) (xy 140.848773 100.829804) (xy 140.799 101.075) (xy 140.848773 101.320196)
				(xy 140.985415 101.276905) (xy 141.052813 101.240561) (xy 141.147709 101.194647) (xy 141.210872 101.180319)
				(xy 141.295196 101.175)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.945196 99.025) (xy 141.865664 99.020332) (xy 141.805069 99.007658) (xy 141.702813 98.959439)
				(xy 141.621184 98.916714) (xy 141.498773 98.879804) (xy 141.449 99.125) (xy 141.498773 99.370196)
				(xy 141.635415 99.326905) (xy 141.702813 99.290561) (xy 141.797709 99.244647) (xy 141.860872 99.230319)
				(xy 141.945196 99.225)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.449822 112.223757) (xy 145.334373 112.332208) (xy 145.230373 112.415509) (xy 145.144758 112.471487)
				(xy 145.063473 112.512915) (xy 144.906082 112.562111) (xy 144.70641 112.586684) (xy 144.648922 112.5909)
				(xy 144.433629 112.609556) (xy 144.164173 112.651333) (xy 144.329293 113.485707) (xy 145.163667 113.650827)
				(xy 145.209912 113.339143) (xy 145.224099 113.166079) (xy 145.243545 112.962534) (xy 145.26167 112.870092)
				(xy 145.290561 112.779338) (xy 145.334091 112.68687) (xy 145.396133 112.589287) (xy 145.480559 112.48319)
				(xy 145.591243 112.365178)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.295196 99.675) (xy 141.215664 99.670332) (xy 141.155069 99.657658) (xy 141.052813 99.609439)
				(xy 140.971184 99.566714) (xy 140.848773 99.529804) (xy 140.799 99.775) (xy 140.848773 100.020196)
				(xy 140.985415 99.976905) (xy 141.052813 99.940561) (xy 141.147709 99.894647) (xy 141.210872 99.880319)
				(xy 141.295196 99.875)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.79 114.325) (xy 128.78468 114.441303) (xy 128.767441 114.57908) (xy 128.73929 114.716989)
				(xy 128.697841 114.857426) (xy 128.654118 114.966453) (xy 128.600156 115.06839) (xy 128.548168 115.143415)
				(xy 128.488478 115.209104) (xy 128.431443 115.255995) (xy 128.368302 115.29338) (xy 128.25903 115.329329)
				(xy 129.09 116.026) (xy 129.92097 115.329329) (xy 129.800403 115.287688) (xy 129.69281 115.21032)
				(xy 129.595908 115.09365) (xy 129.510872 114.932287) (xy 129.442536 114.724343) (xy 129.399409 114.483165)
				(xy 129.39 114.325)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.044688 105.475) (xy 146.940982 105.470339) (xy 146.866797 105.457714) (xy 146.785171 105.431997)
				(xy 146.708137 105.406491) (xy 146.598773 105.379804) (xy 146.549 105.625) (xy 146.688893 105.832867)
				(xy 146.785568 105.762443) (xy 146.838064 105.723675) (xy 146.889339 105.696406) (xy 146.953509 105.680295)
				(xy 147.044688 105.675)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.802945 105.277946) (xy 154.865513 105.315216) (xy 154.907396 105.351825) (xy 154.952009 105.424951)
				(xy 154.965621 105.459767) (xy 154.994064 105.528967) (xy 155.042133 105.613893) (xy 155.25089 105.475454)
				(xy 155.298773 105.229804) (xy 155.224722 105.215393) (xy 155.068371 105.178864) (xy 154.893749 105.099749)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.255764 107.9) (xy 173.338989 107.904708) (xy 173.404514 107.917662) (xy 173.50331 107.962022)
				(xy 173.543409 107.988048) (xy 173.641663 108.0462) (xy 173.707406 108.072452) (xy 173.791473 108.094236)
				(xy 173.851 107.8) (xy 173.791473 107.505764) (xy 173.710601 107.526507) (xy 173.646727 107.551418)
				(xy 173.543409 107.611952) (xy 173.490883 107.645383) (xy 173.431776 107.673464) (xy 173.356574 107.6928)
				(xy 173.255764 107.7)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/BUS_A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.320554 111.345867) (xy 166.380092 111.29293) (xy 166.431901 111.259045) (xy 166.538304 111.220835)
				(xy 166.626235 111.193326) (xy 166.738893 111.132867) (xy 166.600707 110.924293) (xy 166.392133 110.786107)
				(xy 166.326123 110.913338) (xy 166.304164 110.986697) (xy 166.269529 111.086264) (xy 166.234998 111.141059)
				(xy 166.179133 111.204446)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.270867 100.254446) (xy 164.21793 100.194908) (xy 164.184045 100.143098) (xy 164.145835 100.036696)
				(xy 164.118326 99.948765) (xy 164.057867 99.836107) (xy 163.849293 99.974293) (xy 163.711107 100.182867)
				(xy 163.838338 100.248876) (xy 163.911696 100.270835) (xy 164.011264 100.305471) (xy 164.066059 100.340002)
				(xy 164.129446 100.395867)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.295196 102.275) (xy 141.215664 102.270332) (xy 141.155069 102.257658) (xy 141.052813 102.209439)
				(xy 140.971184 102.166714) (xy 140.848773 102.129804) (xy 140.799 102.375) (xy 140.848773 102.620196)
				(xy 140.985415 102.576905) (xy 141.052813 102.540561) (xy 141.147709 102.494647) (xy 141.210872 102.480319)
				(xy 141.295196 102.475)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.945196 109) (xy 162.865664 108.995332) (xy 162.805069 108.982658) (xy 162.702813 108.934439)
				(xy 162.621184 108.891714) (xy 162.498773 108.854804) (xy 162.449 109.1) (xy 162.498773 109.345196)
				(xy 162.635415 109.301905) (xy 162.702813 109.265561) (xy 162.797709 109.219647) (xy 162.860872 109.205319)
				(xy 162.945196 109.2)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.345196 102.225) (xy 153.265664 102.220332) (xy 153.205069 102.207658) (xy 153.102813 102.159439)
				(xy 153.021184 102.116714) (xy 152.898773 102.079804) (xy 152.849 102.325) (xy 152.898773 102.570196)
				(xy 153.035415 102.526905) (xy 153.102813 102.490561) (xy 153.197709 102.444647) (xy 153.260872 102.430319)
				(xy 153.345196 102.425)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/BUS_A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.325569 114.848231) (xy 145.272271 114.942008) (xy 145.218082 115.01667) (xy 145.167352 115.069967)
				(xy 145.115154 115.110554) (xy 145.006728 115.159387) (xy 144.875396 115.177517) (xy 144.684794 115.170848)
				(xy 144.447188 115.162204) (xy 144.311909 115.169538) (xy 144.164173 115.191333) (xy 144.329546 116.02589)
				(xy 145.163667 116.190827) (xy 145.2356 115.760794) (xy 145.264646 115.574782) (xy 145.305976 115.401303)
				(xy 145.379159 115.202129) (xy 145.503767 114.939033)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.087829 99.618184) (xy 159.208325 99.497438) (xy 159.219572 99.484021) (xy 159.28225 99.41544)
				(xy 159.388894 99.332867) (xy 159.250761 99.124351) (xy 159.004805 99.076227) (xy 159 99.182825)
				(xy 159.015401 99.262577) (xy 159.026304 99.314387) (xy 159.02647 99.363228) (xy 159.006736 99.412625)
				(xy 158.95794 99.466103)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.945196 100.325) (xy 141.865664 100.320332) (xy 141.805069 100.307658) (xy 141.702813 100.259439)
				(xy 141.621184 100.216714) (xy 141.498773 100.179804) (xy 141.449 100.425) (xy 141.498773 100.670196)
				(xy 141.635415 100.626905) (xy 141.702813 100.590561) (xy 141.797709 100.544647) (xy 141.860872 100.530319)
				(xy 141.945196 100.525)
			)
		)
	)
	(embedded_fonts yes)
	(embedded_files
		(file
			(name "ProggyVector.ttf")
			(type font)
		)
	)
)
