(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6002)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Front")
		(2 "B.Cu" signal "Back")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.5102)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_57ffffff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 100.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "/COL0")
	(net 2 "/COL1")
	(net 3 "/COL10")
	(net 4 "/COL11")
	(net 5 "/COL4")
	(net 6 "/COL5")
	(net 7 "/COL6")
	(net 8 "/LED_A")
	(net 9 "/LED_B")
	(net 10 "/LED_C")
	(net 11 "/ROW0")
	(net 12 "/ROW1")
	(net 13 "/ROW2")
	(net 14 "/ROW3")
	(net 15 "/ROW4")
	(net 16 "/ROW5")
	(net 17 "/SCLM")
	(net 18 "/SDAM")
	(net 19 "GND")
	(net 20 "VCC")
	(net 21 "Net-(D1:7-Pad1)")
	(net 22 "Net-(D1:8-Pad1)")
	(net 23 "Net-(J1-Pad1)")
	(net 24 "Net-(J1-Pad2)")
	(net 25 "Net-(J1-Pad3)")
	(net 26 "Net-(J1-Pad4)")
	(net 27 "Net-(J1-Pad5)")
	(net 28 "Net-(LED_A1-Pad1)")
	(net 29 "Net-(LED_B1-Pad1)")
	(net 30 "Net-(LED_C1-Pad1)")
	(net 31 "Net-(SW0:7-Pad2)")
	(net 32 "Net-(SW0:8-Pad2)")
	(net 33 "Net-(SW0:9-Pad2)")
	(net 34 "Net-(SW0:10-Pad2)")
	(net 35 "Net-(SW0:11-Pad2)")
	(net 36 "Net-(SW0:12-Pad2)")
	(net 37 "Net-(SW1:9-Pad2)")
	(net 38 "Net-(SW1:10-Pad2)")
	(net 39 "Net-(SW1:11-Pad2)")
	(net 40 "Net-(SW1:12-Pad2)")
	(net 41 "Net-(SW1:13-Pad2)")
	(net 42 "Net-(SW2:7-Pad2)")
	(net 43 "Net-(SW2:8-Pad2)")
	(net 44 "Net-(SW2:9-Pad2)")
	(net 45 "Net-(SW2:10-Pad2)")
	(net 46 "Net-(SW2:11-Pad2)")
	(net 47 "Net-(SW2:12-Pad2)")
	(net 48 "Net-(SW2:13-Pad2)")
	(net 49 "Net-(SW3:8-Pad2)")
	(net 50 "Net-(SW3:9-Pad2)")
	(net 51 "Net-(SW3:10-Pad2)")
	(net 52 "Net-(SW3:11-Pad2)")
	(net 53 "Net-(SW3:12-Pad2)")
	(net 54 "Net-(SW3:13-Pad2)")
	(net 55 "Net-(SW4:7-Pad2)")
	(net 56 "Net-(SW4:8-Pad2)")
	(net 57 "Net-(SW4:9-Pad2)")
	(net 58 "Net-(SW4:10-Pad2)")
	(net 59 "Net-(SW4:11-Pad2)")
	(net 60 "Net-(SW4:12-Pad2)")
	(net 61 "Net-(SW4:13-Pad2)")
	(net 62 "Net-(SW5:7-Pad2)")
	(net 63 "Net-(SW5:8-Pad2)")
	(net 64 "Net-(SW5:9-Pad2)")
	(net 65 "Net-(SW5:10-Pad2)")
	(net 66 "Net-(SW5:11-Pad2)")
	(net 67 "Net-(SW5:12-Pad2)")
	(net 68 "Net-(SW5:13-Pad2)")
	(net 69 "Net-(U1-Pad12)")
	(net 70 "Net-(U1-Pad19)")
	(net 71 "Net-(U2-Pad14)")
	(net 72 "Net-(U2-Pad27)")
	(net 73 "Net-(U2-Pad28)")
	(net 74 "/RST")
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 186.69 143.20266)
		(property "Reference" "SW1:13"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW1:0"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(SW1:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(SW1:13-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(SW1:13-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(SW1:13-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 129.54 138.43)
		(property "Reference" "SW1:10"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW1:3"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(SW1:10-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(SW1:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(SW1:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(SW1:10-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 110.49 140.02766)
		(property "Reference" "SW1:9"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW1:4"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(SW1:9-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(SW1:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(SW1:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(SW1:9-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_XX"
		(layer "F.Cu")
		(at 191.4525 124.15266)
		(property "Reference" "SW2:13"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW2:0"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -9.8425 -2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at -7.3025 -3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.28346 2.28346)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "2" thru_hole circle
			(at -9.8425 2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -7.3025 3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -4.7625 -5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
		)
		(pad "2" thru_hole oval
			(at -2.38252 0)
			(size 8.7503 3.9878)
			(drill oval 8.7503 3.9878)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -4.7625 5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(SW2:13-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 129.54 119.38)
		(property "Reference" "SW2:10"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW2:3"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(SW2:10-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(SW2:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(SW2:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(SW2:10-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 110.49 120.97766)
		(property "Reference" "SW2:9"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW2:4"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(SW2:9-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(SW2:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(SW2:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(SW2:9-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 72.39 117.48516 90)
		(property "Reference" "SW2:7"
			(at 0 3.302 90)
			(layer "F.SilkS")
		)
		(property "Value" "SW2:6"
			(at 0 3.302 90)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(SW2:7-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(SW2:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(SW2:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(SW2:7-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_XX"
		(layer "F.Cu")
		(at 191.4525 105.10266)
		(property "Reference" "SW3:13"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW3:0"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -9.8425 -2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at -7.3025 -3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.28346 2.28346)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "2" thru_hole circle
			(at -9.8425 2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -7.3025 3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -4.7625 -5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
		)
		(pad "2" thru_hole oval
			(at -2.38252 0)
			(size 8.7503 3.9878)
			(drill oval 8.7503 3.9878)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -4.7625 5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(SW3:13-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 148.59 101.92766)
		(property "Reference" "SW3:11"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW3:2"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(SW3:11-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(SW3:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(SW3:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(SW3:11-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 129.54 100.33)
		(property "Reference" "SW3:10"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW3:3"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(SW3:10-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(SW3:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(SW3:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(SW3:10-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 110.49 101.92766)
		(property "Reference" "SW3:9"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW3:4"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(SW3:9-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(SW3:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(SW3:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(SW3:9-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 91.44 103.19766)
		(property "Reference" "SW3:8"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW3:5"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(SW3:8-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(SW3:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(SW3:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(SW3:8-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_XX"
		(layer "F.Cu")
		(at 191.4525 86.05266)
		(property "Reference" "SW4:13"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW4:0"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -9.8425 -2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at -7.3025 -3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.28346 2.28346)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "2" thru_hole circle
			(at -9.8425 2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -7.3025 3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -4.7625 -5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
		)
		(pad "2" thru_hole oval
			(at -2.38252 0)
			(size 8.7503 3.9878)
			(drill oval 8.7503 3.9878)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -4.7625 5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "Net-(SW4:13-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 167.64 86.05266)
		(property "Reference" "SW4:12"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW4:1"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(SW4:12-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(SW4:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(SW4:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(SW4:12-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 148.59 82.87766)
		(property "Reference" "SW4:11"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW4:2"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(SW4:11-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(SW4:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(SW4:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "Net-(SW4:11-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 129.54 81.28)
		(property "Reference" "SW4:10"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW4:3"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(SW4:10-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(SW4:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(SW4:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "Net-(SW4:10-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 110.49 82.87766)
		(property "Reference" "SW4:9"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW4:4"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(SW4:9-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(SW4:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(SW4:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(SW4:9-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 91.44 84.14766)
		(property "Reference" "SW4:8"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW4:5"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(SW4:8-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(SW4:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(SW4:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(SW4:8-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 72.39 88.91016 90)
		(property "Reference" "SW4:7"
			(at 0 3.302 90)
			(layer "F.SilkS")
		)
		(property "Value" "SW4:6"
			(at 0 3.302 90)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(SW4:7-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 90)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(SW4:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(SW4:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(SW4:7-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 90)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 81.30286 153.06548 115)
		(property "Reference" "SW0:10"
			(at 0.000001 3.302 115)
			(layer "F.SilkS")
		)
		(property "Value" "SW0:3"
			(at 0.000001 3.302 115)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 115)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 115)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 115)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(SW0:10-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(SW0:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(SW0:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(SW0:10-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 50.8 177.8 25)
		(property "Reference" "SW0:12"
			(at 0.000001 3.302 25)
			(layer "F.SilkS")
		)
		(property "Value" "SW0:1"
			(at 0.000001 3.302 25)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 25)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(SW0:12-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(SW0:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(SW0:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(SW0:12-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 64.03848 161.11728 115)
		(property "Reference" "SW0:11"
			(at 0.000001 3.302 115)
			(layer "F.SilkS")
		)
		(property "Value" "SW0:2"
			(at 0.000001 3.302 115)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 115)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 115)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 115)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(SW0:11-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 115)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(SW0:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(SW0:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(SW0:11-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 115)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 115)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 42.7482 160.53308 25)
		(property "Reference" "SW0:9"
			(at 0.000001 3.302 25)
			(layer "F.SilkS")
		)
		(property "Value" "SW0:4"
			(at 0.000001 3.302 25)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 25)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(SW0:9-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(SW0:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(SW0:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(SW0:9-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 34.69894 143.2687 25)
		(property "Reference" "SW0:7"
			(at 0.000001 3.302 25)
			(layer "F.SilkS")
		)
		(property "Value" "SW0:6"
			(at 0.000001 3.302 25)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 25)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(SW0:7-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(SW0:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(SW0:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(SW0:7-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 148.59 140.02766)
		(property "Reference" "SW1:11"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW1:2"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(SW1:11-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(SW1:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(SW1:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(SW1:11-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 51.96332 135.21944 25)
		(property "Reference" "SW0:8"
			(at 0.000001 3.302 25)
			(layer "F.SilkS")
		)
		(property "Value" "SW0:5"
			(at 0.000001 3.302 25)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 25)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(SW0:8-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(SW0:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(SW0:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(SW0:8-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "MX_LED"
		(layer "F.Cu")
		(at 72.39 117.48516 90)
		(property "Reference" "LED_C1"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LEDc"
			(at 0 10.16 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -1.27 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(LED_C1-Pad1)")
		)
		(pad "2" thru_hole rect
			(at 1.27 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "MX_LED"
		(layer "F.Cu")
		(at 72.39 88.91016 90)
		(property "Reference" "LED_B1"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LEDb"
			(at 0 10.16 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -1.27 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(LED_B1-Pad1)")
		)
		(pad "2" thru_hole rect
			(at 1.27 5.08 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "MX_LED"
		(layer "F.Cu")
		(at 72.39 65.1002)
		(property "Reference" "LED_A1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LEDa"
			(at 0 10.16 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -1.27 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(LED_A1-Pad1)")
		)
		(pad "2" thru_hole rect
			(at 1.27 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "RESISTOR"
		(layer "F.Cu")
		(at 125.4125 46.99 180)
		(property "Reference" "RC1"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LEDc"
			(at 0 0 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5.08 0 180)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/LED_C")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(LED_C1-Pad1)")
		)
		(embedded_fonts no)
	)
	(footprint "RESISTOR"
		(layer "F.Cu")
		(at 148.9075 45.4025 -135)
		(property "Reference" "RA1"
			(at 0 0 225)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LEDa"
			(at 0 0 225)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5.079999 0 225)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/LED_A")
		)
		(pad "2" thru_hole circle
			(at 5.079999 0 225)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(LED_A1-Pad1)")
		)
		(embedded_fonts no)
	)
	(footprint "RESISTOR"
		(layer "F.Cu")
		(at 147.0025 43.4975 -135)
		(property "Reference" "RB1"
			(at 0 0 225)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LEDb"
			(at 0 0 225)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 225)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 225)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5.079999 0 225)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LED_B")
		)
		(pad "2" thru_hole circle
			(at 5.079999 0 225)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(LED_B1-Pad1)")
		)
		(embedded_fonts no)
	)
	(footprint "RESISTOR"
		(layer "F.Cu")
		(at 105.41 40.3225 -45)
		(property "Reference" "R1"
			(at 0 0 315)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2kΩ"
			(at 0 0 315)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5.079999 0 315)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(pad "2" thru_hole circle
			(at 5.079999 0 315)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SDAM")
		)
		(embedded_fonts no)
	)
	(footprint "4pin35mmAudio"
		(layer "F.Cu")
		(at 86.3092 30.48 -90)
		(property "Reference" "J2"
			(at 1.27 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.5mm"
			(at 5.715 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "3.5mm"
			(at 5.715 0 0)
			(layer "B.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 2.8956 0 270)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
		)
		(pad "" np_thru_hole circle
			(at 7.8994 0 270)
			(size 0.9906 0.9906)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
		)
		(pad "1" thru_hole oval
			(at 2.8956 -4.6482 270)
			(size 1.7526 2.0574)
			(drill oval 1.0922 1.397)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 27 "Net-(J1-Pad5)")
		)
		(pad "2" thru_hole circle
			(at 7.8994 3.6068 270)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 18 "/SDAM")
		)
		(pad "3" thru_hole circle
			(at 10.9982 -1.6002 270)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 17 "/SCLM")
		)
		(pad "4" thru_hole oval
			(at 2.8956 4.6482 270)
			(size 1.7526 2.0574)
			(drill oval 1.0922 1.397)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 23 "Net-(J1-Pad1)")
		)
		(pad "5" thru_hole circle
			(at 10.9982 1.6002 270)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 17 "/SCLM")
		)
		(pad "6" thru_hole circle
			(at 7.8994 -3.6068 270)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 18 "/SDAM")
		)
		(embedded_fonts no)
	)
	(footprint "100PITCH1X3"
		(layer "F.Cu")
		(at 78.74 37.465 90)
		(property "Reference" "J4"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JMP"
			(at 0 3.048 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(pad "2" thru_hole circle
			(at 0 0 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 23 "Net-(J1-Pad1)")
		)
		(pad "3" thru_hole circle
			(at 2.54 0 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "RESISTOR"
		(layer "F.Cu")
		(at 102.235 41.5925 -45)
		(property "Reference" "R2"
			(at 0 0 315)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2kΩ"
			(at 0 0 315)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5.079999 0 315)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(pad "2" thru_hole circle
			(at 5.079999 0 315)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/SCLM")
		)
		(embedded_fonts no)
	)
	(footprint "USBMINImod"
		(layer "F.Cu")
		(at 137.6426 30.48 -90)
		(property "Reference" "J1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole oval
			(at 6.79958 -1.6002 270)
			(size 1.651 1.143)
			(drill 0.762
				(offset 0.27432 0)
			)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 23 "Net-(J1-Pad1)")
		)
		(pad "1" thru_hole circle
			(at 9.779 -2.413 270)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 23 "Net-(J1-Pad1)")
		)
		(pad "2" thru_hole circle
			(at 3.937 -5.715 270)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 24 "Net-(J1-Pad2)")
		)
		(pad "2" thru_hole oval
			(at 5.6007 -0.8001 270)
			(size 1.651 1.143)
			(drill 0.762
				(offset -0.27432 0)
			)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 24 "Net-(J1-Pad2)")
		)
		(pad "3" thru_hole oval
			(at 6.79958 0 270)
			(size 1.651 1.143)
			(drill 0.762
				(offset 0.27432 0)
			)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 25 "Net-(J1-Pad3)")
		)
		(pad "3" thru_hole circle
			(at 9.779 0 270)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 25 "Net-(J1-Pad3)")
		)
		(pad "4" thru_hole circle
			(at 3.937 5.715 270)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 26 "Net-(J1-Pad4)")
		)
		(pad "4" thru_hole oval
			(at 5.6007 0.8001 270)
			(size 1.651 1.143)
			(drill 0.762
				(offset -0.27432 0)
			)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 26 "Net-(J1-Pad4)")
		)
		(pad "5" thru_hole oval
			(at 6.79958 1.6002 270)
			(size 1.651 1.143)
			(drill 0.762
				(offset 0.27432 0)
			)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 27 "Net-(J1-Pad5)")
		)
		(pad "5" thru_hole circle
			(at 9.779 2.413 270)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 27 "Net-(J1-Pad5)")
		)
		(pad "6" thru_hole oval
			(at 1.75006 -3.64744 270)
			(size 2.794 1.7018)
			(drill oval 1.905 0.762)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(pad "6" thru_hole oval
			(at 1.75006 3.64744 270)
			(size 2.794 1.7018)
			(drill oval 1.905 0.762)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_XX"
		(layer "F.Cu")
		(at 191.4525 67.0052)
		(property "Reference" "SW5:13"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW5:0"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -9.8425 -2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at -7.3025 -3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.28346 2.28346)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "2" thru_hole circle
			(at -9.8425 2.54)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -7.3025 3.81)
			(size 2.28092 2.28092)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -4.7625 -5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
		)
		(pad "2" thru_hole oval
			(at -2.38252 0)
			(size 8.7503 3.9878)
			(drill oval 8.7503 3.9878)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -4.7625 5.08 90)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "Net-(SW5:13-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 110.49 63.82766)
		(property "Reference" "SW5:9"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW5:4"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(SW5:9-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(SW5:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(SW5:9-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(SW5:9-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 129.54 62.23)
		(property "Reference" "SW5:10"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW5:3"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(SW5:10-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(SW5:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(SW5:10-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(SW5:10-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 148.59 63.82766)
		(property "Reference" "SW5:11"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW5:2"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(SW5:11-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(SW5:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(SW5:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(SW5:11-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 167.64 67.0052)
		(property "Reference" "SW5:12"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW5:1"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(SW5:12-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(SW5:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(SW5:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(SW5:12-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 91.44 65.1002)
		(property "Reference" "SW5:8"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW5:5"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(SW5:8-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(SW5:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(SW5:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(SW5:8-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 72.39 65.1002)
		(property "Reference" "SW5:7"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW5:6"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(SW5:7-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(SW5:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(SW5:7-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(SW5:7-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 148.59 120.97766)
		(property "Reference" "SW2:11"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW2:2"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(SW2:11-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(SW2:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(SW2:11-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(SW2:11-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 91.44 122.24766)
		(property "Reference" "SW2:8"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW2:5"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(SW2:8-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(SW2:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(SW2:8-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(SW2:8-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 167.64 105.10266)
		(property "Reference" "SW3:12"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW3:1"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(SW3:12-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(SW3:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(SW3:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(SW3:12-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 167.64 124.15266)
		(property "Reference" "SW2:12"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW2:1"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(SW2:12-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(SW2:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(SW2:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(SW2:12-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:MX_FLIP_DIODE"
		(layer "F.Cu")
		(at 167.64 143.20266)
		(property "Reference" "SW1:12"
			(at 0 3.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "SW1:1"
			(at 0 3.302 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(SW1:12-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(SW1:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(SW1:12-Pad2)")
		)
		(pad "3" thru_hole circle
			(at -3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(SW1:12-Pad2)")
		)
		(pad "4" thru_hole rect
			(at 3.81 5.08)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "4" thru_hole rect
			(at 3.81 7.62)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 7.62)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "MX_FLIP"
		(layer "F.Cu")
		(at 77.2795 144.43202 25)
		(property "Reference" "SX1:8"
			(at 0.000001 3.302 25)
			(layer "F.SilkS")
		)
		(property "Value" "SX1:5"
			(at 0.000001 3.302 25)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 25)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D1:8-Pad1)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D1:8-Pad1)")
		)
		(embedded_fonts no)
	)
	(footprint "MX_FLIP"
		(layer "F.Cu")
		(at 60.01512 152.48382 25)
		(property "Reference" "SX1:7"
			(at 0.000001 3.302 25)
			(layer "F.SilkS")
		)
		(property "Value" "SX1:6"
			(at 0.000001 3.302 25)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 25)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 25)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D1:7-Pad1)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 25)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D1:7-Pad1)")
		)
		(embedded_fonts no)
	)
	(footprint "MX_FLIP"
		(layer "F.Cu")
		(at 85.3313 161.69894 -155)
		(property "Reference" "SX0:10"
			(at 0.000001 3.302 205)
			(layer "F.SilkS")
		)
		(property "Value" "SX0:3"
			(at 0.000001 3.302 205)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 205)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 205)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 205)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 205)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 205)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(SW0:10-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(SW0:10-Pad2)")
		)
		(embedded_fonts no)
	)
	(footprint "MX_FLIP"
		(layer "F.Cu")
		(at 68.06438 169.7482 -155)
		(property "Reference" "SX0:11"
			(at 0.000001 3.302 205)
			(layer "F.SilkS")
		)
		(property "Value" "SX0:2"
			(at 0.000001 3.302 205)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 205)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 205)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.08 0 205)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 0 0 205)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 5.08 0 205)
			(size 1.7018 1.7018)
			(drill 1.7018)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.54 -5.08 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "1" thru_hole circle
			(at 3.81 -2.54 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "2" thru_hole circle
			(at -3.81 -2.54 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(SW0:11-Pad2)")
		)
		(pad "2" thru_hole circle
			(at -2.54 -5.08 205)
			(size 2.286 2.286)
			(drill 1.4986)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(SW0:11-Pad2)")
		)
		(embedded_fonts no)
	)
	(footprint "DIODE"
		(layer "F.Cu")
		(at 74.05878 137.52576 25)
		(property "Reference" "D1:8"
			(at 0 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "D"
			(at 0 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.81 0 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(D1:8-Pad1)")
		)
		(pad "2" thru_hole rect
			(at 3.81 0 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "99" smd rect
			(at -1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOXmech"
		(layer "F.Cu")
		(at 50.8 177.8)
		(property "Reference" "H99"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MECHANICAL"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 3.0988 -11.9634)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 8.8646 -56.134)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 16.6116 -140.6652)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 54.6354 -20.0406)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 67.4116 -140.6652)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 88.2396 -86.2076)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 150.3426 -140.6652)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 150.9776 -37.7444)
			(size 6.3754 6.3754)
			(drill 6.3754)
			(layers "*.Cu" "*.Mask")
			(solder_mask_margin -0.254)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "DIODE"
		(layer "F.Cu")
		(at 56.7944 145.57756 25)
		(property "Reference" "D1:7"
			(at 0 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "D"
			(at 0 0 25)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 25)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -3.81 0 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(D1:7-Pad1)")
		)
		(pad "2" thru_hole rect
			(at 3.81 0 25)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "99" smd rect
			(at -1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at -1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "99" smd rect
			(at 1.6637 0 25)
			(size 0.8382 0.8382)
			(layers "B.Cu" "B.Mask" "B.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:TEENSY_2.0_WITH_RESET"
		(layer "F.Cu")
		(at 175.895 42.545)
		(property "Reference" "U1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ItsyBitsy"
			(at -0.825 -0.935 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -13.97 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(pad "2" thru_hole circle
			(at -11.43 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "3" thru_hole circle
			(at -8.89 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "4" thru_hole circle
			(at -6.35 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "5" thru_hole circle
			(at -3.81 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "6" thru_hole circle
			(at -1.27 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/LED_C")
		)
		(pad "7" thru_hole circle
			(at 1.27 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/SCLM")
		)
		(pad "8" thru_hole circle
			(at 3.81 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SDAM")
		)
		(pad "9" thru_hole circle
			(at 6.35 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "10" thru_hole circle
			(at 8.89 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "11" thru_hole circle
			(at 11.43 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "12" thru_hole circle
			(at 13.97 7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(U1-Pad12)")
		)
		(pad "16" thru_hole circle
			(at 13.97 -2.54)
			(size 1.7526 1.7526)
			(drill 1.08966)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/RST")
		)
		(pad "18" thru_hole circle
			(at 13.97 -7.62)
			(size 1.7526 1.7526)
			(drill 1.08966)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 0)
		)
		(pad "19" thru_hole circle
			(at 11.43 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(U1-Pad19)")
		)
		(pad "20" thru_hole circle
			(at 8.89 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(pad "21" thru_hole circle
			(at 6.35 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/LED_A")
		)
		(pad "22" thru_hole circle
			(at 3.81 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LED_B")
		)
		(pad "23" thru_hole circle
			(at 1.27 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "24" thru_hole circle
			(at -1.27 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "25" thru_hole circle
			(at -3.81 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "26" thru_hole circle
			(at -6.35 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "27" thru_hole circle
			(at -8.89 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "28" thru_hole circle
			(at -11.43 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "29" thru_hole circle
			(at -13.97 -7.62)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint "GAP"
		(layer "F.Cu")
		(at 186.13 40.89)
		(property "Reference" "JP1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JUMPER"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 0 -0.635)
			(size 2.032 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "VCC")
		)
		(pad "1" smd rect
			(at 0 0.635)
			(size 2.032 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "VCC")
		)
		(embedded_fonts no)
	)
	(footprint "STAB_PCB940"
		(layer "F.Cu")
		(at 64.03848 161.11728 115)
		(property "Reference" "S1"
			(at 0 0 115)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "STAB200"
			(at 0 0 115)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 115)
			(layer "F.Fab")
			(hide yes)
		)
		(solder_mask_margin -0.254)
		(zone_connect 2)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -11.938 -8.255 115)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at -11.938 6.985 115)
			(size 3.048 3.048)
			(drill 3.048)
			(layers "*.Cu")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 11.938 6.985 115)
			(size 3.048 3.048)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 11.938001 -8.255 115)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "STAB_PCB940"
		(layer "F.Cu")
		(at 81.30286 153.06548 -65)
		(property "Reference" "S2"
			(at 0 0 295)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "STAB200"
			(at 0 0 295)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 295)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 295)
			(layer "F.Fab")
			(hide yes)
		)
		(solder_mask_margin -0.254)
		(zone_connect 2)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -11.938 -8.255 295)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at -11.938 6.985 295)
			(size 3.048 3.048)
			(drill 3.048)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 11.938 6.985 295)
			(size 3.048 3.048)
			(drill 3.048)
			(layers "*.Cu")
			(zone_connect 2)
		)
		(pad "" np_thru_hole circle
			(at 11.938001 -8.255 295)
			(size 3.9878 3.9878)
			(drill 3.9878)
			(layers "*.Cu" "*.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:STAR"
		(layer "F.Cu")
		(at 95.9325 140.5575)
		(property "Reference" "STAR_1"
			(at 0 5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STAR_FRONT"
			(at 0 3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "0" smd circle
			(at -2.8448 0)
			(size 1.27 1.27)
			(layers "F.Cu")
		)
		(pad "0" smd circle
			(at -1.4224 -2.46126)
			(size 1.27 1.27)
			(layers "F.Cu")
		)
		(pad "0" smd circle
			(at -1.41986 2.46126)
			(size 1.27 1.27)
			(layers "F.Cu")
		)
		(pad "0" smd circle
			(at 1.41986 -2.46126)
			(size 1.27 1.27)
			(layers "F.Cu")
		)
		(pad "0" smd circle
			(at 1.4224 2.46126)
			(size 1.27 1.27)
			(layers "F.Cu")
		)
		(pad "0" smd circle
			(at 2.8448 0)
			(size 1.27 1.27)
			(layers "F.Cu")
		)
		(pad "1" smd circle
			(at -5.08 -1.75768)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "1" smd circle
			(at -4.06146 3.5179)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "1" smd circle
			(at -1.016 -5.27812)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "1" smd circle
			(at 1.016 5.27812)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "1" smd circle
			(at 4.06146 -3.5179)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "1" smd circle
			(at 5.08 1.75768)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "2" smd circle
			(at -5.08 1.75768)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "2" smd circle
			(at -4.064 -3.5179)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "2" smd circle
			(at -1.01346 5.27812)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "2" smd circle
			(at 1.01346 -5.27812)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "2" smd circle
			(at 4.064 3.5179)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "2" smd circle
			(at 5.07746 -1.75768)
			(size 0.508 0.508)
			(layers "F.Cu")
		)
		(pad "3" smd circle
			(at -7.112 -1.75768)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "3" smd circle
			(at -5.07746 5.27812)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "3" smd circle
			(at -2.032 -7.03834)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "3" smd circle
			(at 2.032 7.03834)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "3" smd circle
			(at 5.07746 -5.27812)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "3" smd circle
			(at 7.112 1.75768)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "4" smd circle
			(at -7.112 1.75768)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "4" smd circle
			(at -5.08 -5.27812)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "4" smd circle
			(at -2.02946 7.03834)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "4" smd circle
			(at 2.02946 -7.03834)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "4" smd circle
			(at 5.08 5.27812)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "4" smd circle
			(at 7.10946 -1.75768)
			(size 0.3048 0.3048)
			(layers "F.Cu")
		)
		(pad "5" smd circle
			(at -8.128 -3.5179)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "5" smd circle
			(at -7.10946 5.27812)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "5" smd circle
			(at -1.016 -8.79856)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "5" smd circle
			(at 1.016 8.79856)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "5" smd circle
			(at 7.10946 -5.27812)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "5" smd circle
			(at 8.128 3.5179)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "6" smd circle
			(at -8.128 3.5179)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "6" smd circle
			(at -7.112 -5.27812)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "6" smd circle
			(at -1.01346 8.79856)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "6" smd circle
			(at 1.01346 -8.79856)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "6" smd circle
			(at 7.112 5.27812)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(pad "6" smd circle
			(at 8.128 -3.5179)
			(size 0.2032 0.2032)
			(layers "F.Cu")
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 138.75 64.4)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 78.13 55.02)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 174.46 54.43)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 155.3 37.14)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 101.49 129.46)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 59.87 171.84)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 119.94 134)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 138.67 134.08)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 157.79 132.51)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 177.24 132.59)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "lib_footprints:STITCHING_VIA"
		(layer "F.Cu")
		(at 100.19 58.53)
		(property "Reference" "STITCHING_VIA"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Value" "~"
			(at 0 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "GND" thru_hole circle
			(at 0 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 19 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Buttons_Switches_SMD:SW_SPST_B3U-1000P"
		(layer "F.Cu")
		(at 194.5 41.45 -90)
		(descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
		(tags "Tactile Switch")
		(property "Reference" "SW_RST1"
			(at 0 -2.5 270)
			(layer "F.SilkS")
		)
		(property "Value" "SWITCH_PUSH"
			(at 0 2.5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/RST")
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "DIP28_300"
		(layer "B.Cu")
		(at 178.435 41.275)
		(property "Reference" "U2"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MCP23018"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at 6.35 3.81)
			(size 1.0922 1.0922)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 8.89 3.81)
			(size 1.0922 1.0922)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 11.43 3.81)
			(size 1.0922 1.0922)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at -16.51 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(pad "2" thru_hole circle
			(at -13.97 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "3" thru_hole circle
			(at -11.43 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/ROW5")
		)
		(pad "4" thru_hole circle
			(at -8.89 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/ROW4")
		)
		(pad "5" thru_hole circle
			(at -6.35 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/ROW3")
		)
		(pad "6" thru_hole circle
			(at -3.81 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/ROW2")
		)
		(pad "7" thru_hole circle
			(at -1.27 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/ROW1")
		)
		(pad "8" thru_hole circle
			(at 1.27 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/ROW0")
		)
		(pad "9" thru_hole circle
			(at 3.81 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/LED_B")
		)
		(pad "10" thru_hole circle
			(at 6.35 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/LED_A")
		)
		(pad "11" thru_hole circle
			(at 8.89 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(pad "12" thru_hole circle
			(at 11.43 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/SCLM")
		)
		(pad "13" thru_hole circle
			(at 13.97 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/SDAM")
		)
		(pad "14" thru_hole circle
			(at 16.51 -3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(U2-Pad14)")
		)
		(pad "15" thru_hole circle
			(at 16.51 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(pad "16" thru_hole circle
			(at 13.97 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(pad "20" thru_hole circle
			(at 3.81 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/COL0")
		)
		(pad "21" thru_hole circle
			(at 1.27 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COL1")
		)
		(pad "22" thru_hole circle
			(at -1.27 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/COL11")
		)
		(pad "23" thru_hole circle
			(at -3.81 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COL10")
		)
		(pad "24" thru_hole circle
			(at -6.35 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/COL4")
		)
		(pad "25" thru_hole circle
			(at -8.89 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/COL5")
		)
		(pad "26" thru_hole circle
			(at -11.43 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/COL6")
		)
		(pad "27" thru_hole circle
			(at -13.97 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 72 "Net-(U2-Pad27)")
		)
		(pad "28" thru_hole circle
			(at -16.51 3.81)
			(size 1.7526 1.7526)
			(drill 1.0922)
			(layers "*.Cu" "*.SilkS" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(U2-Pad28)")
		)
		(embedded_fonts no)
	)
	(footprint "100PITCH1X3"
		(layer "B.Cu")
		(at 93.98 37.465 90)
		(property "Reference" "J3"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "JMP"
			(at 0 -3.048 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "B.SilkS")
			(remove_unused_layers no)
			(net 20 "VCC")
		)
		(pad "2" thru_hole circle
			(at 0 0 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "B.SilkS")
			(remove_unused_layers no)
			(net 27 "Net-(J1-Pad5)")
		)
		(pad "3" thru_hole circle
			(at 2.54 0 90)
			(size 1.651 1.651)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask" "B.SilkS")
			(remove_unused_layers no)
			(net 19 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "GAP"
		(layer "B.Cu")
		(at 192.7225 34.925 -90)
		(property "Reference" "JP2"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "JUMPER"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" smd rect
			(at 0 -0.635 270)
			(size 2.032 1.016)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "GND")
		)
		(pad "1" smd rect
			(at 0 0.635 270)
			(size 2.032 1.016)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "GND")
			(zone_connect 0)
		)
		(embedded_fonts no)
	)
	(footprint "ErgoDOX pcb:STAR"
		(layer "B.Cu")
		(at 95.9325 140.5575 180)
		(property "Reference" "STAR_2"
			(at 0 5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "STAR_BACK"
			(at 0 3 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "0" smd circle
			(at -2.8448 0 180)
			(size 1.27 1.27)
			(layers "B.Cu")
		)
		(pad "0" smd circle
			(at -1.4224 2.46126 180)
			(size 1.27 1.27)
			(layers "B.Cu")
		)
		(pad "0" smd circle
			(at -1.41986 -2.46126 180)
			(size 1.27 1.27)
			(layers "B.Cu")
		)
		(pad "0" smd circle
			(at 1.41986 2.46126 180)
			(size 1.27 1.27)
			(layers "B.Cu")
		)
		(pad "0" smd circle
			(at 1.4224 -2.46126 180)
			(size 1.27 1.27)
			(layers "B.Cu")
		)
		(pad "0" smd circle
			(at 2.8448 0 180)
			(size 1.27 1.27)
			(layers "B.Cu")
		)
		(pad "1" smd circle
			(at -5.08 1.75768 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "1" smd circle
			(at -4.06146 -3.5179 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "1" smd circle
			(at -1.016 5.27812 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "1" smd circle
			(at 1.016 -5.27812 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "1" smd circle
			(at 4.06146 3.5179 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "1" smd circle
			(at 5.08 -1.75768 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "2" smd circle
			(at -5.08 -1.75768 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "2" smd circle
			(at -4.064 3.5179 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "2" smd circle
			(at -1.01346 -5.27812 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "2" smd circle
			(at 1.01346 5.27812 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "2" smd circle
			(at 4.064 -3.5179 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "2" smd circle
			(at 5.07746 1.75768 180)
			(size 0.508 0.508)
			(layers "B.Cu")
		)
		(pad "3" smd circle
			(at -7.112 1.75768 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "3" smd circle
			(at -5.07746 -5.27812 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "3" smd circle
			(at -2.032 7.03834 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "3" smd circle
			(at 2.032 -7.03834 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "3" smd circle
			(at 5.07746 5.27812 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "3" smd circle
			(at 7.112 -1.75768 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "4" smd circle
			(at -7.112 -1.75768 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "4" smd circle
			(at -5.08 5.27812 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "4" smd circle
			(at -2.02946 -7.03834 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "4" smd circle
			(at 2.02946 7.03834 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "4" smd circle
			(at 5.08 -5.27812 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "4" smd circle
			(at 7.10946 1.75768 180)
			(size 0.3048 0.3048)
			(layers "B.Cu")
		)
		(pad "5" smd circle
			(at -8.128 3.5179 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "5" smd circle
			(at -7.10946 -5.27812 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "5" smd circle
			(at -1.016 8.79856 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "5" smd circle
			(at 1.016 -8.79856 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "5" smd circle
			(at 7.10946 5.27812 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "5" smd circle
			(at 8.128 -3.5179 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "6" smd circle
			(at -8.128 -3.5179 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "6" smd circle
			(at -7.112 5.27812 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "6" smd circle
			(at -1.01346 -8.79856 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "6" smd circle
			(at 1.01346 8.79856 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "6" smd circle
			(at 7.112 -5.27812 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(pad "6" smd circle
			(at 8.128 3.5179 180)
			(size 0.2032 0.2032)
			(layers "B.Cu")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 23.08098 141.31544)
		(end 44.76496 187.81776)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 24.61768 137.0965)
		(end 23.08098 141.31544)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 44.76496 187.81776)
		(end 48.9839 189.35192)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 48.9839 189.35192)
		(end 127.1524 152.908)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 57.7088 121.666)
		(end 24.61768 137.0965)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.611 35.433)
		(end 62.611 121.666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.611 121.666)
		(end 57.7088 121.666)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 65.8114 32.258)
		(end 62.611 35.433)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77.8764 30.48)
		(end 77.8764 32.258)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 77.8764 32.258)
		(end 65.8114 32.258)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.2137 30.48)
		(end 77.8764 30.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 84.2137 31.75)
		(end 84.2137 30.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.7095 30.48)
		(end 88.7095 31.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 88.7095 31.75)
		(end 84.2137 31.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.0468 30.48)
		(end 88.7095 30.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 95.0468 32.258)
		(end 95.0468 30.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.1524 152.908)
		(end 196.3928 152.908)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.9022 30.48)
		(end 131.9022 32.258)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.9022 32.258)
		(end 95.0468 32.258)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.3328 32)
		(end 202.6672 32)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4084 30.48)
		(end 131.9022 30.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4084 32.258)
		(end 143.4084 30.48)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.3928 152.9125)
		(end 205.9178 143.3875)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.9178 35.433)
		(end 202.7428 32.258)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 205.9178 143.383)
		(end 205.9178 35.433)
		(layer "Edge.Cuts")
	)
	(gr_text "ID"
		(at 129.794 34.544 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 132.207 40.386 0)
		(layer "F.SilkS")
	)
	(gr_text "D+"
		(at 137.668 42.164 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 142.494 40.386 0)
		(layer "F.SilkS")
	)
	(gr_text "D-"
		(at 146.30146 34.544 0)
		(layer "F.SilkS")
	)
	(gr_text "Components are intended to be\nplaced on the side they are drawn. It is however possible to\ninvert the design. See the webpage for further instructions.\nwww.ergodox.io"
		(at 65.7 51.12 0)
		(layer "F.SilkS")
	)
	(gr_text "FR4 Tg170° Laminate\n24mil traces on 1oz copper "
		(at 160.655 54.61 0)
		(layer "F.SilkS")
	)
	(gr_text ""
		(at 70.86 129.7 0)
		(layer "F.SilkS")
	)
	(gr_text ""
		(at 201.93 127 90)
		(layer "F.SilkS")
	)
	(gr_text ""
		(at 202.5 111.5 90)
		(layer "F.SilkS")
	)
	(gr_text "RIGHT\nHAND"
		(at 67.31 100.965 0)
		(layer "F.SilkS")
	)
	(gr_text "FR4 Tg170° Laminate\n24mil traces on 1oz copper "
		(at 191.77 54.61 0)
		(layer "B.SilkS")
	)
	(gr_text ""
		(at 70.83 129.73 0)
		(layer "B.SilkS")
	)
	(gr_text ""
		(at 201.93 91.44 270)
		(layer "B.SilkS")
	)
	(gr_text "LEFT\nHAND"
		(at 78.105 100.965 0)
		(layer "B.SilkS")
	)
	(gr_text "ErgoDox"
		(at 113.03 48.895 0)
		(layer "B.SilkS")
	)
	(zone
		(net 19)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.3048)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3048)
			(thermal_bridge_width 0.6096)
		)
		(polygon
			(pts
				(xy 48.9839 189.35192) (xy 127.1524 152.908) (xy 196.3928 152.908) (xy 205.9178 143.383) (xy 205.9178 35.433)
				(xy 202.7428 32.258) (xy 143.4084 32.258) (xy 143.4084 30.48) (xy 131.9022 30.48) (xy 131.9022 32.258)
				(xy 95.0468 32.258) (xy 95.0468 30.48) (xy 88.7095 30.48) (xy 88.7095 31.75) (xy 84.2137 31.75)
				(xy 84.2137 30.48) (xy 77.8764 30.48) (xy 77.8764 32.258) (xy 65.8114 32.258) (xy 62.611 35.433)
				(xy 62.611 121.666) (xy 57.7088 121.666) (xy 24.61768 137.0965) (xy 23.08098 141.31544) (xy 44.76496 187.81776)
			)
		)
	)
	(zone
		(net 19)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.3048)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3048)
			(thermal_bridge_width 0.6096)
		)
		(polygon
			(pts
				(xy 48.9839 189.35192) (xy 127.1524 152.908) (xy 196.3928 152.908) (xy 205.9178 143.383) (xy 205.9178 35.433)
				(xy 202.7428 32.258) (xy 143.4084 32.258) (xy 143.4084 30.48) (xy 131.9022 30.48) (xy 131.9022 32.258)
				(xy 95.0468 32.258) (xy 95.0468 30.48) (xy 88.7095 30.48) (xy 88.7095 31.75) (xy 84.2137 31.75)
				(xy 84.2137 30.48) (xy 77.8764 30.48) (xy 77.8764 32.258) (xy 65.8114 32.258) (xy 62.611 35.433)
				(xy 62.611 121.666) (xy 57.7088 121.666) (xy 24.61768 137.0965) (xy 23.08098 141.31544) (xy 44.76496 187.81776)
			)
		)
	)
	(embedded_fonts no)
)
