(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A")
	(title_block
		(title "KENWOOD CD AUTOCHANGER BREAKOUT BOARD")
		(date "2026-03-14")
		(rev "-")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 102 67)
		(grid_origin 102 67)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_02000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab no)
			(crossoutdnponfab no)
			(subtractmaskfromsilk no)
			(outputformat 5)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/MUTE")
	(net 2 "/~{REQ_H}")
	(net 3 "/~{CLK}")
	(net 4 "/DATA C")
	(net 5 "/ON")
	(net 6 "/RESET")
	(net 7 "/~{REQ_C}")
	(net 8 "/DATA H")
	(net 9 "/D. GND")
	(net 10 "/B.U.")
	(net 11 "/GND")
	(net 12 "GND1")
	(net 13 "/L_ch_H")
	(net 14 "/R_ch_H")
	(net 15 "/R_ch_C")
	(net 16 "/L_ch_C")
	(footprint "Library:Jack_3.5mm_CUI_SJ1-3523N_Horizontal"
		(layer "F.Cu")
		(at 108.5 95 90)
		(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
		(tags "TRS audio jack stereo horizontal")
		(property "Reference" "J4"
			(at -6.9 2.6 180)
			(layer "F.SilkS")
		)
		(property "Value" "AudioJack3"
			(at 0 -10 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/")
		(sheetfile "changer cable breakout.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(fp_line
			(start 1.8 3.1)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.2 3.5)
			(end 2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 3.5)
			(end -2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.2 4.5)
			(end 6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 4.5)
			(end -6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 1.8 3.1)
			(mid 2.082843 3.217157)
			(end 2.2 3.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -2.2 3.5)
			(mid -2.082843 3.217158)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_text user "PCB edge"
			(at 0 3.65 90)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5 0 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -5 2.5 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 0 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 2.5 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "R" thru_hole oval
			(at -5 -5 90)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/L_ch_H")
			(pintype "passive")
		)
		(pad "S" thru_hole oval
			(at 0 0 90)
			(size 2.2 1.2)
			(drill oval 1.4 0.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 5 -5 270)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/R_ch_H")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3523N_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:Jack_3.5mm_CUI_SJ1-3523N_Horizontal"
		(layer "F.Cu")
		(at 108.5 113 90)
		(descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
		(tags "TRS audio jack stereo horizontal")
		(property "Reference" "J5"
			(at 6.8 2.6 180)
			(layer "F.SilkS")
		)
		(property "Value" "AudioJack3"
			(at 0 -10 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/")
		(sheetfile "changer cable breakout.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(fp_line
			(start 1.8 3.1)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.2 3.5)
			(end 2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 3.5)
			(end -2.2 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 2.2 4.5)
			(end 6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -2.2 4.5)
			(end -6.5 4.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 1.8 3.1)
			(mid 2.082843 3.217157)
			(end 2.2 3.5)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -2.2 3.5)
			(mid -2.082843 3.217158)
			(end -1.8 3.1)
			(layer "Edge.Cuts")
		)
		(fp_text user "PCB edge"
			(at 0 3.65 90)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -5 0 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -5 2.5 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 -5 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 0 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 5 2.5 90)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
		)
		(pad "R" thru_hole oval
			(at -5 -5 90)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/L_ch_C")
			(pintype "passive")
		)
		(pad "S" thru_hole oval
			(at 0 0 90)
			(size 2.2 1.2)
			(drill oval 1.4 0.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 5 -5 270)
			(size 1.2 2.2)
			(drill oval 0.4 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/R_ch_C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3523N_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:CUI_SDD-130J"
		(layer "F.Cu")
		(at 102 67 180)
		(property "Reference" "J1"
			(at -6.425 -18.335 180)
			(layer "F.SilkS")
		)
		(property "Value" "SDD-130J"
			(at -1.98 3.935 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.sameskydevices.com/product/resource/sds-j.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.06/02-13-2020"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "19.80mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "CUI Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "changer cable breakout.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 3.3 -15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/~{REQ_H}")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0.8 -15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -1.6 -15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/B.U.")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -4 -15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ON")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 4.5 -13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/MUTE")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 2.1 -13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D. GND")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at -0.4 -13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/RESET")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -2.8 -13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/R_ch_H")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 3.3 -11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/~{REQ_C}")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 0.8 -11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DATA C")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at -1.6 -11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA H")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at -4 -11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/L_ch_H")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at -0.4 -9.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/~{CLK}")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "E1" thru_hole circle
			(at -5 0 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND1")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "E2" thru_hole circle
			(at 5 0 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND1")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "F:/Cloud/Dropbox/Documents/KiCAD/kenwood_cd_changer_emulator/hardware/kicad/lib/Library.pretty/SDD-130J.step"
			(offset
				(xyz 0 -2.8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Library:PinSocket_1x11_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 93 104)
		(descr "Through hole straight socket strip, 1x11, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x11 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -14.87 0)
			(layer "F.SilkS")
		)
		(property "Value" "Test Points"
			(at -2.1 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x11, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "changer cable breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${NET_NAME(8)}"
			(at 1.524 5.08 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(1)}"
			(at 1.524 -12.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(3)}"
			(at 1.524 -7.62 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(4)}"
			(at 1.524 -5.08 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(5)}"
			(at 1.524 -2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(2)}"
			(at 1.524 -10.16 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(11)}"
			(at 1.524 12.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(7)}"
			(at 1.524 2.54 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(9)}"
			(at 1.524 7.62 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(10)}"
			(at 1.524 10.16 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${NET_NAME(6)}"
			(at 1.524 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ON")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/B.U.")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/RESET")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D. GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/~{REQ_H}")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/~{REQ_C}")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/MUTE")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DATA C")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA H")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/~{CLK}")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x11_P2.54mm_Vertical.step"
			(offset
				(xyz 0 12.7 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Library:CUI_SDD-130J"
		(layer "B.Cu")
		(at 102 141 180)
		(property "Reference" "J2"
			(at -6.425 18.335 0)
			(layer "B.SilkS")
		)
		(property "Value" "SDD-130J"
			(at -1.98 -3.935 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.sameskydevices.com/product/resource/sds-j.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.06/02-13-2020"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "19.80mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "CUI Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "changer cable breakout.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at 3.3 15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/~{REQ_H}")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0.8 15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -1.6 15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/B.U.")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -4 15.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/ON")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 4.5 13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/MUTE")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 2.1 13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D. GND")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at -0.4 13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/RESET")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -2.8 13.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/R_ch_C")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 3.3 11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/~{REQ_C}")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 0.8 11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DATA C")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at -1.6 11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA H")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at -4 11.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/L_ch_C")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at -0.4 9.7 180)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/~{CLK}")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "E1" thru_hole circle
			(at -5 0 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND1")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "E2" thru_hole circle
			(at 5 0 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND1")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "F:/Cloud/Dropbox/Documents/KiCAD/kenwood_cd_changer_emulator/hardware/kicad/lib/Library.pretty/SDD-130J.step"
			(offset
				(xyz 0 -2.8 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(gr_line
		(start 113 101.5)
		(end 113 106.499999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113 88.5)
		(end 113 66)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 91 66)
		(mid 91.585786 64.585786)
		(end 93 64)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91 142)
		(end 91 66)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 111 64)
		(mid 112.414214 64.585786)
		(end 113 66)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 113 142)
		(mid 112.414214 143.414214)
		(end 111 144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111 144)
		(end 93 144)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 93 144)
		(mid 91.585786 143.414214)
		(end 91 142)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 113 119.500001)
		(end 113 142)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 93 64)
		(end 111 64)
		(layer "Edge.Cuts")
	)
	(gr_text "CHANGER SIDE"
		(at 102 121 0)
		(layer "F.SilkS")
	)
	(gr_text "HEAD UNIT SIDE"
		(at 102 86 0)
		(layer "F.SilkS")
	)
	(gr_text "13 PIN MINI DIN\nPASSTHROUGH BREAKOUT\nCD CHANGER PROTOCOL\nREVERSE ENGINEERING\nPROJECT"
		(at 102 132.5 0)
		(layer "F.SilkS")
	)
	(gr_text "ALLEN KREAGER\n${ISSUE_DATE}\nREV. ${REVISION}"
		(at 102 69.5 0)
		(layer "B.SilkS")
	)
	(gr_text "https://github.com/akreager/cd_changer_emulator"
		(at 95 123 90)
		(layer "B.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 91 66) (xy 113 66)
		)
		(height -8.2)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "22"
			(at 102 56.65 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 93 64) (xy 93 144)
		)
		(height -15.4)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "80"
			(at 76.45 104 90)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 11)
		(net_name "/GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 90.5 72.1) (xy 113.5 72.1) (xy 113.5 136.1) (xy 90.5 136.1)
			)
		)
	)
	(zone
		(net 12)
		(net_name "GND1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 90.5 136.1) (xy 113.5 136.1) (xy 113.5 143.95) (xy 90.5 143.95)
			)
		)
	)
	(zone
		(net 12)
		(net_name "GND1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 90.5 64.05) (xy 113.5 64.05) (xy 113.5 72.05) (xy 90.5 72.05)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.5)
		)
		(polygon
			(pts
				(xy 90.5 72.118174) (xy 113.5 72.118174) (xy 113.5 136.118174) (xy 90.5 136.118174)
			)
		)
	)
	(embedded_fonts no)
)
