Altium Designer Pick and Place Locations
C:\Users\brand\AppData\Local\TempReleases\Snapshot\1\Assembly\Pick Place\Pick Place for 2.4 GHz Radio Transmitter.txt

========================================================================================================================
File Design Information:

Date:       15/04/26
Time:       09:22
Revision:   Not in VersionControl
Variant:    No variations
Units used: mil

Center-X(mil) Center-Y(mil) Comment              Description                                                                                                    Designator Footprint                    Layer    Rotation 
5153.000      52.500        LTC1563-2CGN#PBF     "Active Filter Dual Low Pass 8th Order 256kHz 16-Pin SSOP N"                                                   U11        LTC1563-2CGN#PBF-Footprint-1 TopLayer 0        
2785.000      850.000       10k                  "RES SMD 100 OHM 1% 1/8W 0603"                                                                                 R38        FP-MCT0603-IPC_B             TopLayer 0        
2150.000      1470.000      51                   "RES Thick Film, 51O, 5%, 0.1W, 200ppm/°C, 0603"                                                               R35        FP-CRCW0603-e3-IPC_B         TopLayer 270      
3054.999      1430.000      10pF                 ""                                                                                                             C84        CAPC1608X92X38LL15T08        TopLayer 180      
3260.000      1265.000      1.5pF                "Cap Ceramic 1.5pF 50V C0G 0.25pF Pad SMD 0402 +125°C Automotive T/R"                                          C82        FP-CGA2B-MFG                 TopLayer 90       
4820.000      1025.000      "15 nH"              "Wire Wound Ferrite type RF Inductor 15nH ±5% 2200mA 0.025O 0603 (1608)"                                       L12        FP-LQW18CA_00-MFG            TopLayer 90       
3445.000      1160.000      TSW-102-07-L-S       "CONN HEADER VERT 2POS 2.54MM"                                                                                 J4         FP-TSW-102-07-L-S-MFG        TopLayer 90       
3805.788      1161.772      TRF3705IRGET         "TRF3705IRGET, Modulator Quadrature 3.1dB 3.15  3.6 V 24-Pin VQFN"                                             IQM1       QFN50P400X400X100-25N-D      TopLayer 0        
845.590       987.717       ""                   "Chip Ferrite Bead, 0603, 180O @ 100MHz, 0.09O, 25%, 1.5A"                                                     FB7        FP-BLM18-0_15-t0_8-IPC_B     TopLayer 90       
5058.504      920.000       "1 pF"               ""                                                                                                             C106       CAPC1608X95X40LL15T15        TopLayer 180      
4955.000      1085.000      "1.2 pF"             ""                                                                                                             C105       CAPC1608X92X38NL15T08        TopLayer 90       
5070.000      860.000       "2.2 pF"             "CAP 2.2pF 16V ±0.5pF 0603 (1608 Metric) Thickness 1mm SMD"                                                    C104       CAPC0603(1608)100_N          TopLayer 0        
4630.000      1180.000      "12 pF"              ""                                                                                                             C103       CAPC1608X95X40ML15T15        TopLayer 0        
4960.000      1545.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C102       FP-GCM21B-0_15-IPC_A         TopLayer 0        
4955.000      1345.000      "12 pF"              ""                                                                                                             C101       CAPC1608X95X40ML15T15        TopLayer 180      
4955.000      1430.000      "10 nF"              "Chip Multilayer Ceramic Capacitors for General Purpose, 0603, 10000pF, C0G, 30ppm/°C, 5%, 50V"                C100       FP-GRM188-0_1-e0_2_0_5-IPC_B TopLayer 0        
4070.000      1145.000      "0.2 pF"             "Ceramic Capacitor 0.2pF ±0.1pF 250VDC C0G 0603 Paper T/R"                                                     C99        FP-GQM187-0_15-IPC_C         TopLayer 270      
3975.001      1170.000      "6.8 pF"             "CAP 6.8pF 16V ±0.5pF 0603 (1608 Metric) Thickness 1mm SMD"                                                    C97        CAPC0603(1608)100_L          TopLayer 0        
3575.000      1060.000      "12 pF"              ""                                                                                                             C96        CAPC1608X95X40ML15T15        TopLayer 0        
3975.000      1360.000      "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C95        CAPC1608X95X40LL15T15        TopLayer 270      
4055.000      1376.466      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C94        FP-GCM21B-0_15-IPC_A         TopLayer 270      
3590.000      1365.000      "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C92        CAPC1608X95X40LL15T15        TopLayer 0        
2838.150      1555.000      100nF                "Cap Ceramic 100nF 100V C0G 5% Pad SMD 1206 +125°C Automotive T/R"                                             C91        FP-CGA5L-0_3-0_1-IPC_A       TopLayer 180      
2885.000      1455.000      10pF                 ""                                                                                                             C90        CAPC1608X92X38LL15T08        TopLayer 0        
3020.000      995.000       1.2nF                "Multilayer Ceramic Capacitors 1.2nF ±5% 100V C0G SMD 0603"                                                    C89        FP-C1608-080-0_1-IPC_C       TopLayer 270      
4350.000      1170.020      DEA142450BT-3028A1   "Signal Conditioning LTCC BAND PASS FLTR 2400-2500MHz"                                                         BPF1       DEA142450BT3028A1            TopLayer 0        
4315.000      47.500        LTC1563-2CGN#PBF     "Active Filter Dual Low Pass 8th Order 256kHz 16-Pin SSOP N"                                                   U13        LTC1563-2CGN#PBF-Footprint-1 TopLayer 0        
3495.000      42.500        LTC1563-2CGN#PBF     "Active Filter Dual Low Pass 8th Order 256kHz 16-Pin SSOP N"                                                   U12        LTC1563-2CGN#PBF-Footprint-1 TopLayer 0        
2570.000      47.500        LTC1563-2CGN#PBF     "Active Filter Dual Low Pass 8th Order 256kHz 16-Pin SSOP N"                                                   U10        LTC1563-2CGN#PBF-Footprint-1 TopLayer 0        
2880.102      -575.158      ADA4940              "ROHS3Compliant EAR99 ADA4940 Tape & Reel (TR) op amp amplifier circuit 3mm 1.1muA 60muV 90dB"                 U9         ADA4940-Footprint-1          TopLayer 180      
1094.528      -515.255      AD5689RTCPZ-EP-RL7   "IC DAC 16BIT V-OUT 16LFCSP"                                                                                   U8         FP-CP-16-22-IPC_C            TopLayer 180      
1300.000      1105.000      LDL1117S33R          "LDL1117 Series 1.2 A 3.3 V High PSRR LDO Linear Voltage Regulator-SOT-223"                                    U7         FP-SOT223-0046067-IPC_A      TopLayer 0        
1300.000      1710.000      LDL1117S33R          "LDL1117 Series 1.2 A 3.3 V High PSRR LDO Linear Voltage Regulator-SOT-223"                                    U6         FP-SOT223-0046067-IPC_A      TopLayer 0        
5340.000      -881.172      LDL1117S33R          "LDL1117 Series 1.2 A 3.3 V High PSRR LDO Linear Voltage Regulator-SOT-223"                                    U5         FP-SOT223-0046067-IPC_A      TopLayer 90       
-49.685       -780.000      LDL1117S33R          "LDL1117 Series 1.2 A 3.3 V High PSRR LDO Linear Voltage Regulator-SOT-223"                                    U4         FP-SOT223-0046067-IPC_A      TopLayer 90       
4343.820      -1388.126     LDL1117S33R          "LDL1117 Series 1.2 A 3.3 V High PSRR LDO Linear Voltage Regulator-SOT-223"                                    U3         FP-SOT223-0046067-IPC_A      TopLayer 0        
2758.820      -1363.126     LDL1117S33R          "LDL1117 Series 1.2 A 3.3 V High PSRR LDO Linear Voltage Regulator-SOT-223"                                    U2         FP-SOT223-0046067-IPC_A      TopLayer 0        
1288.821      -1418.126     LDL1117S33R          "LDL1117 Series 1.2 A 3.3 V High PSRR LDO Linear Voltage Regulator-SOT-223"                                    U1         FP-SOT223-0046067-IPC_A      TopLayer 0        
3035.000      -885.000      CR0603-FX-52R3ELF    "Resistor, thick film, SMD 0603 (1608), 52.3 ?, 0.1 W, ±1 %, CR0603-FX-52R3ELF"                                RT4        FP-CR0603-IPC_A              TopLayer 90       
2760.000      -895.772      CR0603-FX-52R3ELF    "Resistor, thick film, SMD 0603 (1608), 52.3 ?, 0.1 W, ±1 %, CR0603-FX-52R3ELF"                                RT3        FP-CR0603-IPC_A              TopLayer 90       
2170.000      -412.441      CR0603-FX-52R3ELF    "Resistor, thick film, SMD 0603 (1608), 52.3 ?, 0.1 W, ±1 %, CR0603-FX-52R3ELF"                                RT2        FP-CR0603-IPC_A              TopLayer 270      
2170.000      -747.559      CR0603-FX-52R3ELF    "Resistor, thick film, SMD 0603 (1608), 52.3 ?, 0.1 W, ±1 %, CR0603-FX-52R3ELF"                                RT1        FP-CR0603-IPC_A              TopLayer 90       
3125.000      -883.330      CRCW060350R0FKEA     "Res Thick Film 0603 50 Ohm 1% 0.1W(1/10W) ±100ppm/C Pad SMD Automotive T/R"                                   RS4        FP-CRCW0603-e3-IPC_C         TopLayer 90       
2845.000      -890.000      CRCW060350R0FKEA     "Res Thick Film 0603 50 Ohm 1% 0.1W(1/10W) ±100ppm/C Pad SMD Automotive T/R"                                   RS3        FP-CRCW0603-e3-IPC_C         TopLayer 90       
2120.772      -535.000      CRCW060350R0FKEA     "Res Thick Film 0603 50 Ohm 1% 0.1W(1/10W) ±100ppm/C Pad SMD Automotive T/R"                                   RS2        FP-CRCW0603-e3-IPC_C         TopLayer 180      
2120.000      -620.000      CRCW060350R0FKEA     "Res Thick Film 0603 50 Ohm 1% 0.1W(1/10W) ±100ppm/C Pad SMD Automotive T/R"                                   RS1        FP-CRCW0603-e3-IPC_C         TopLayer 0        
3035.000      -740.000      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RG4        FP-CPF0603-MFG               TopLayer 90       
2795.000      -775.772      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RG3        FP-CPF0603-MFG               TopLayer 0        
2260.000      -535.000      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RG2        FP-CPF0603-MFG               TopLayer 180      
2260.000      -620.000      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RG1        FP-CPF0603-MFG               TopLayer 0        
3090.000      -515.000      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RF4        FP-CPF0603-MFG               TopLayer 0        
2890.000      -335.000      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RF3        FP-CPF0603-MFG               TopLayer 90       
2910.000      -750.000      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RF2        FP-CPF0603-MFG               TopLayer 270      
2765.000      -380.000      6-1879336-2          "Fixed Resistor, Thin Film, 0.063W, 1000ohm, 50V, 1% +/-Tol, 50ppm/Cel, Surface Mount, 0603"                   RF1        FP-CPF0603-MFG               TopLayer 0        
3870.000      970.000       "49.9 Ohms"          "Res Thin Film 0603 49.9 Ohm 0.1% 1/8W ±25ppm/°C Molded SMD SMD Paper T/R"                                     R47        RESC1609X55X30NL10T20        TopLayer 180      
3753.543      970.000       "49.9 Ohms"          "Res Thin Film 0603 49.9 Ohm 0.1% 1/8W ±25ppm/°C Molded SMD SMD Paper T/R"                                     R46        RESC1609X55X30NL10T20        TopLayer 180      
3745.000      1400.000      "49.9 Ohm"           "Res Thin Film 0603 49.9 Ohm 0.1% 1/8W ±25ppm/°C Molded SMD SMD Paper T/R"                                     R45        RESC1609X55X30NL10T20        TopLayer 180      
3870.000      1400.000      "49.9 Ohm"           "Res Thin Film 0603 49.9 Ohm 0.1% 1/8W ±25ppm/°C Molded SMD SMD Paper T/R"                                     R44        RESC1609X55X30NL10T20        TopLayer 0        
2920.000      685.000       360                  "RES Thick Film, 360O, 1%, 0.063W, 100ppm/°C, 0402"                                                            R43        FP-CRCW0402-e3-IPC_C         TopLayer 90       
2920.000      775.000       360                  "RES Thick Film, 360O, 1%, 0.063W, 100ppm/°C, 0402"                                                            R42        FP-CRCW0402-e3-IPC_C         TopLayer 90       
2995.000      670.000       360                  "RES Thick Film, 360O, 1%, 0.063W, 100ppm/°C, 0402"                                                            R41        FP-CRCW0402-e3-IPC_C         TopLayer 180      
3100.000      675.000       360                  "RES Thick Film, 360O, 1%, 0.063W, 100ppm/°C, 0402"                                                            R40        FP-CRCW0402-e3-IPC_C         TopLayer 180      
2575.000      1275.000      100                  "RES SMD 0603 1/4W 1% 100 OHM"                                                                                 R39        FP-SR0603-MFG                TopLayer 90       
3114.999      965.000       680                  "RES SMD 680 OHM 0.1% 1/16W 0402"                                                                              R37        FP-RT0402-MFG                TopLayer 180      
2935.000      1370.000      4.7k                 ""                                                                                                             R36        RESC1609X50X30NL10T20        TopLayer 0        
1800.000      1410.000      10k                  "RES SMD 10K OHM 1% 1/16W 0402"                                                                                R34        FP-CRG0402-IPC_B             TopLayer 0        
3050.000      1170.000      100                  ""                                                                                                             R33        RESC1609X50X30LL10T20        TopLayer 270      
4380.000      -160.000      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R32        FP-CPF0603-MFG               TopLayer 0        
4025.002      -155.432      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R31        FP-CPF0603-MFG               TopLayer 90       
3560.000      -165.000      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R30        FP-CPF0603-MFG               TopLayer 0        
3205.002      -160.432      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R29        FP-CPF0603-MFG               TopLayer 90       
4060.000      -25.000       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R28        FP-CPF0603-MFG               TopLayer 0        
3240.000      -30.000       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R27        FP-CPF0603-MFG               TopLayer 0        
4650.001      10.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R26        FP-CPF0603-MFG               TopLayer 0        
4059.999      60.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R25        FP-CPF0603-MFG               TopLayer 0        
3830.001      10.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R24        FP-CPF0603-MFG               TopLayer 0        
3239.999      55.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R23        FP-CPF0603-MFG               TopLayer 0        
4645.000      110.000       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R22        FP-CPF0603-MFG               TopLayer 0        
3825.000      105.000       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R21        FP-CPF0603-MFG               TopLayer 0        
5215.001      -155.000      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R20        FP-CPF0603-MFG               TopLayer 0        
4860.000      -150.433      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R19        FP-CPF0603-MFG               TopLayer 90       
2635.000      -159.998      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R18        FP-CPF0603-MFG               TopLayer 0        
2280.002      -155.433      CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R17        FP-CPF0603-MFG               TopLayer 90       
4895.000      -20.000       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R16        FP-CPF0603-MFG               TopLayer 0        
2315.000      -25.000       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R15        FP-CPF0603-MFG               TopLayer 0        
5485.000      15.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R14        FP-CPF0603-MFG               TopLayer 0        
4895.000      65.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R13        FP-CPF0603-MFG               TopLayer 0        
2905.001      10.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R12        FP-CPF0603-MFG               TopLayer 0        
2314.999      60.000        CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R11        FP-CPF0603-MFG               TopLayer 0        
5480.000      115.001       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R10        FP-CPF0603-MFG               TopLayer 0        
2900.001      110.000       CPF0603B120KE1       "Res Thin Film 0603 120K Ohm 0.1% 1/16W ±25ppm/°C Molded SMD SMD Paper T/R"                                    R9         FP-CPF0603-MFG               TopLayer 0        
1085.001      -345.000      10K                  "CRGCQ 0603 10K 5%"                                                                                            R8         FP-CRGCQ0603-IPC_C           TopLayer 270      
1015.000      -650.000      10K                  "CRGCQ 0603 10K 5%"                                                                                            R7         FP-CRGCQ0603-IPC_C           TopLayer 270      
1215.000      -430.000      0                    "0O ±0 0.1W 0603 Thick Film Chip Resistor AEC-Q200 compliant"                                                  R6         FP-RMCF0603-IPC_B            TopLayer 90       
890.000       -345.000      0                    "0O ±0 0.1W 0603 Thick Film Chip Resistor AEC-Q200 compliant"                                                  R5         FP-RMCF0603-IPC_B            TopLayer 0        
910.000       -525.000      10K                  "CRGCQ 0603 10K 5%"                                                                                            R4         FP-CRGCQ0603-IPC_C           TopLayer 0        
1850.000      -651.379      ""                   "Thick Film Chip Resistors 0603 2kO 0.1W 5% 200ppm/°C"                                                         R3         FP-CR0603-IPC_B              TopLayer 90       
1840.000      -505.001      ""                   "Thick Film Chip Resistors 0603 2kO 0.1W 5% 200ppm/°C"                                                         R2         FP-CR0603-IPC_B              TopLayer 270      
895.000       -440.000      CRGCQ0603F22R        "Res Thick Film 0603 22 Ohm 1% 0.1W(1/10W) ±200ppm/C Pad SMD Automotive T/R"                                   R1         FP-CRGCQ0603-IPC_A           TopLayer 0        
2895.000      1170.000      ADF4350BCPZ-RL7      "Wideband Synthesizer with Integrated VCO, CP-32-2, Pb-Free, 1500 Reel"                                        PLL1       ADI-CP-32-2_L                TopLayer 90       
5083.658      1054.567      ADL5320ARKZ-R7       "IC RF AMP 400MHZ-2.7GHZ SOT89-3"                                                                              PA1        FP-RK-3-MFG                  TopLayer 270      
1920.000      1470.000      LMK6CE10000DDLFT     "IC 100 MHz LVCMOS Oscillator 1.8V Enable/Disable 4-VDFN"                                                      OSC1       DLF0004A_MFG                 TopLayer 90       
3195.001      1250.000      3.6nH                "Multilayer type RF Inductor 3.6nH ±0.2nH 0.14O 750mA 0402"                                                    L11        FP-LQG15HH_02-MFG            TopLayer 0        
3120.000      1190.000      7.5nH                "Multilayer type Inductor for Automotive 7.5nH ±3% 0.16O 600mA 0402"                                           L10        FP-LQG15WH_02-MFG            TopLayer 180      
3120.000      1115.000      7.5nH                "Multilayer type Inductor for Automotive 7.5nH ±3% 0.16O 600mA 0402"                                           L9         FP-LQG15WH_02-MFG            TopLayer 180      
3195.748      1060.000      3.6nH                "Multilayer type RF Inductor 3.6nH ±0.2nH 0.14O 750mA 0402"                                                    L8         FP-LQG15HH_02-MFG            TopLayer 0        
560.000       999.262       ""                   "Common Mode Chokes Dual 500Ohm 100MHz 1A 0.23Ohm DCR SMD T/R"                                                 L7         FP-DLW5BS-MFG                TopLayer 270      
560.000       1609.262      ""                   "Common Mode Chokes Dual 500Ohm 100MHz 1A 0.23Ohm DCR SMD T/R"                                                 L6         FP-DLW5BS-MFG                TopLayer 270      
5355.334      -1498.032     ""                   "Common Mode Chokes Dual 500Ohm 100MHz 1A 0.23Ohm DCR SMD T/R"                                                 L5         FP-DLW5BS-MFG                TopLayer 90       
-29.095       -1391.860     ""                   "Common Mode Chokes Dual 500Ohm 100MHz 1A 0.23Ohm DCR SMD T/R"                                                 L4         FP-DLW5BS-MFG                TopLayer 90       
3694.558      -1413.126     ""                   "Common Mode Chokes Dual 500Ohm 100MHz 1A 0.23Ohm DCR SMD T/R"                                                 L3         FP-DLW5BS-MFG                TopLayer 0        
2174.558      -1388.126     ""                   "Common Mode Chokes Dual 500Ohm 100MHz 1A 0.23Ohm DCR SMD T/R"                                                 L2         FP-DLW5BS-MFG                TopLayer 0        
696.714       -1444.632     ""                   "Common Mode Chokes Dual 500Ohm 100MHz 1A 0.23Ohm DCR SMD T/R"                                                 L1         FP-DLW5BS-MFG                TopLayer 0        
950.000       0.000         61302011821          "THT Vertical Socket Header WR-PHD, Pitch 2.54 mm, Single Row, 20 pins"                                        J9         61302011821                  TopLayer 0        
950.000       700.000       61302011821          "THT Vertical Socket Header WR-PHD, Pitch 2.54 mm, Single Row, 20 pins"                                        J8         61302011821                  TopLayer 180      
4460.000      1130.000      TSW-102-07-G-S       "CONN HEADER VERT 2POS 2.54MM"                                                                                 J7         FP-TSW-102-07-G-S-MFG        TopLayer 270      
4210.000      1120.000      TSW-102-07-G-S       "CONN HEADER VERT 2POS 2.54MM"                                                                                 J6         FP-TSW-102-07-G-S-MFG        TopLayer 270      
5400.000      860.000       SMA-J-P-H-RA-TH1     Description                                                                                                    J5         CONN_SMA-J-P-H-RA-TH1_SAI    TopLayer 270      
3700.000      670.000       TSW-106-07-S-S       "Male Header, Pitch 2.54 mm, 1 x 6 Position, Height 8.38 mm, Tail Length 2.54 mm, -55 to 125 degC, RoHS, Bulk" J3         SMTC-TSW-106-07-S-S_V        TopLayer 0        
3425.000      -710.000      TSW-106-07-S-S       "Male Header, Pitch 2.54 mm, 1 x 6 Position, Height 8.38 mm, Tail Length 2.54 mm, -55 to 125 degC, RoHS, Bulk" J2         SMTC-TSW-106-07-S-S_V        TopLayer 90       
1625.000      -570.000      TSW-102-07-G-S       "CONN HEADER VERT 2POS 2.54MM"                                                                                 J1         FP-TSW-102-07-G-S-MFG        TopLayer 270      
850.000       1595.000      ""                   "Chip Ferrite Bead, 0603, 180O @ 100MHz, 0.09O, 25%, 1.5A"                                                     FB6        FP-BLM18-0_15-t0_8-IPC_B     TopLayer 90       
5285.000      -1190.000     ""                   "Chip Ferrite Bead, 0603, 180O @ 100MHz, 0.09O, 25%, 1.5A"                                                     FB5        FP-BLM18-0_15-t0_8-IPC_B     TopLayer 90       
-99.685       -1065.000     ""                   "Chip Ferrite Bead, 0603, 180O @ 100MHz, 0.09O, 25%, 1.5A"                                                     FB4        FP-BLM18-0_15-t0_8-IPC_B     TopLayer 90       
4068.820      -1338.125     ""                   "Chip Ferrite Bead, 0603, 180O @ 100MHz, 0.09O, 25%, 1.5A"                                                     FB3        FP-BLM18-0_15-t0_8-IPC_B     TopLayer 0        
2498.820      -1318.126     ""                   "Chip Ferrite Bead, 0603, 180O @ 100MHz, 0.09O, 25%, 1.5A"                                                     FB2        FP-BLM18-0_15-t0_8-IPC_B     TopLayer 0        
1008.820      -1368.125     ""                   "Chip Ferrite Bead, 0603, 180O @ 100MHz, 0.09O, 25%, 1.5A"                                                     FB1        FP-BLM18-0_15-t0_8-IPC_B     TopLayer 0        
3569.999      1250.000      "12 pF"              ""                                                                                                             C98        CAPC1608X95X40ML15T15        TopLayer 0        
3575.000      1450.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C93        FP-GCM21B-0_15-IPC_A         TopLayer 180      
3195.000      729.999       39nF                 "C1206 39,000 pF C0G 5.00% 50 V"                                                                               C88        FP-C1206C-EB-MFG             TopLayer 270      
3100.000      870.000       2.7nF                "Multilayer Ceramic Capacitors 2.7nF ±5% 250V C0G SMD 0805"                                                    C87        FP-C2012-125-0_2-IPC_A       TopLayer 180      
2740.000      1385.000      10pF                 ""                                                                                                             C86        CAPC1608X92X38LL15T08        TopLayer 90       
2645.000      1465.000      100nF                "Chip Multilayer Ceramic Capacitors for General Purpose, 1206, 0.10uF, C0G, 30ppm/°C, 5%, 50V"                 C85        FP-GRM31C-0_2-e0_3_0_8-IPC_B TopLayer 90       
3080.836      1510.000      100nF                "Chip Multilayer Ceramic Capacitors for General Purpose, 1206, 0.10uF, C0G, 30ppm/°C, 5%, 50V"                 C83        FP-GRM31C-0_2-e0_3_0_8-IPC_B TopLayer 0        
3105.000      1273.346      2.2pF                "Cap Ceramic 2.2pF 50V C0G 0.25pF Pad SMD 0402 +125°C Automotive T/R"                                          C81        FP-CGA2B-IPC_B               TopLayer 90       
1739.999      1500.000      1nF                  "Cap Ceramic 1nF 250V C0G 5% Pad SMD 0603 +125°C Automotive T/R"                                               C80        FP-CGA3E-0_3-0_1-IPC_A       TopLayer 180      
1739.646      1600.000      1nF                  "Cap Ceramic 1nF 250V C0G 5% Pad SMD 0603 +125°C Automotive T/R"                                               C79        FP-CGA3E-0_3-0_1-IPC_A       TopLayer 180      
2270.000      1500.000      1nF                  ""                                                                                                             C78        CAPC1608X95X40NL15T15        TopLayer 0        
2045.000      1500.000      1nF                  ""                                                                                                             C77        CAPC1608X95X40NL15T15        TopLayer 0        
3335.001      1250.000      1nF                  "CAP CER 1000PF 16V X7R 0402"                                                                                  C76        FP-C0402C102K4RAC7411-MFG    TopLayer 0        
3265.000      1039.999      1.5pF                "Ceramic Capacitor for Automotive 1.5pF ±5% 50VDC C0G 0402 Paper T/R"                                          C75        FP-GCM155-0_05-IPC_A         TopLayer 270      
3120.000      1045.000      2.2pF                "Cap Ceramic 2.2pF 50V C0G 0.25pF Pad SMD 0402 +125°C Automotive T/R"                                          C74        FP-CGA2B-IPC_B               TopLayer 270      
3334.999      1060.000      1nF                  "CAP CER 1000PF 16V X7R 0402"                                                                                  C73        FP-C0402C102K4RAC7411-MFG    TopLayer 0        
2655.000      -625.000      0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C72        CAPC1608X87X35LL15T15        TopLayer 90       
2585.000      -635.433      10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C71        CAPC0603(1608)100_M          TopLayer 90       
3135.000      -630.394      0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C70        CAPC1608X87X35LL15T15        TopLayer 90       
3205.000      -640.000      10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C69        CAPC0603(1608)100_M          TopLayer 90       
4190.000      -145.000      CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C68        FP-CGA5L-MFG                 TopLayer 0        
3370.001      -150.000      CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C67        FP-CGA5L-MFG                 TopLayer 0        
2655.000      -456.300      0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C66        CAPC1608X87X35LL15T15        TopLayer 270      
2585.000      -446.300      10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C65        CAPC0603(1608)100_M          TopLayer 270      
2611.300      -810.000      0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C64        CAPC1608X87X35LL15T15        TopLayer 0        
2601.301      -880.000      10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C63        CAPC0603(1608)100_M          TopLayer 0        
4310.000      305.000       CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C62        FP-CGA5L-MFG                 TopLayer 180      
3490.000      300.000       CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C61        FP-CGA5L-MFG                 TopLayer 180      
4350.000      225.000       0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C60        CAPC1608X87X35LL15T15        TopLayer 0        
3530.000      220.000       0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C59        CAPC1608X87X35LL15T15        TopLayer 0        
4340.001      395.000       10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C58        CAPC0603(1608)100_M          TopLayer 0        
3520.001      390.000       10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C57        CAPC0603(1608)100_M          TopLayer 0        
5025.000      -140.000      CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C56        FP-CGA5L-MFG                 TopLayer 0        
2445.000      -145.000      CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C55        FP-CGA5L-MFG                 TopLayer 0        
5145.000      310.000       CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C54        FP-CGA5L-MFG                 TopLayer 180      
2565.000      305.000       CGA5L2C0G1H104J160AA "CGA Series 1206 100 nF 50 V ±5 % Tolerance C0G SMT Multilayer Ceramic Capacitor"                              C53        FP-CGA5L-MFG                 TopLayer 180      
5185.000      230.000       0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C52        CAPC1608X87X35LL15T15        TopLayer 0        
2605.000      225.000       0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C51        CAPC1608X87X35LL15T15        TopLayer 0        
5175.001      400.000       10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C50        CAPC0603(1608)100_M          TopLayer 0        
2595.001      395.000       10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C49        CAPC0603(1608)100_M          TopLayer 0        
1770.001      -646.380      ""                   200pF                                                                                                          C48        CAPC1608X90X35LL15T15        TopLayer 90       
1770.000      -510.000      ""                   200pF                                                                                                          C47        CAPC1608X90X35LL15T15        TopLayer 270      
1205.000      -765.001      0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C46        CAPC1608X87X35LL15T15        TopLayer 180      
1215.000      -945.000      10uF                 "CAP 10uF 6.3V ±10% 0603 (1608 Metric) Thickness 1mm SMD"                                                      C45        CAPC0603(1608)100_M          TopLayer 180      
1205.000      -820.000      0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C44        CAPC1608X87X35LL15T15        TopLayer 180      
1204.607      -875.000      0.1uF                "Ceramic Capacitor, Multilayer, Ceramic, 25V, 10% +Tol, 10% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C43        CAPC1608X87X35LL15T15        TopLayer 180      
1645.000      1128.622      "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C42        CAPC1608X95X40LL15T15        TopLayer 270      
1730.000      1145.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C41        FP-GCM21B-0_15-IPC_A         TopLayer 90       
1560.000      1140.000      "4.7 uF"             "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0805 4.7uF 10%, 16VDC,  X7R 15%"                                 C40        FP-GCJ21B-0_3-IPC_A          TopLayer 90       
970.000       985.000       "1 uF"               "VJ0603Y105KXJCW1BC Multilayer Ceramic Capacitor, 1 uF, 16 V, ± 10%, X7R, 0603 [1608 Metric]"                  C39        FP-VJ0603Y105KXJCW1BC-MFG    TopLayer 270      
739.999       1000.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C38        FP-GCM21B-0_15-IPC_A         TopLayer 90       
1040.000      990.001       "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C37        CAPC1608X95X40LL15T15        TopLayer 90       
1675.000      1739.999      "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C36        CAPC1608X95X40LL15T15        TopLayer 270      
1780.000      1755.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C35        FP-GCM21B-0_15-IPC_A         TopLayer 90       
1580.000      1748.569      "4.7 uF"             "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0805 4.7uF 10%, 16VDC,  X7R 15%"                                 C34        FP-GCJ21B-0_3-IPC_A          TopLayer 90       
1039.999      1590.000      "1 uF"               "VJ0603Y105KXJCW1BC Multilayer Ceramic Capacitor, 1 uF, 16 V, ± 10%, X7R, 0603 [1608 Metric]"                  C33        FP-VJ0603Y105KXJCW1BC-MFG    TopLayer 270      
740.000       1605.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C32        FP-GCM21B-0_15-IPC_A         TopLayer 90       
960.000       1598.622      "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C31        CAPC1608X95X40LL15T15        TopLayer 90       
5310.001      -530.000      "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C30        CAPC1608X95X40LL15T15        TopLayer 0        
5295.000      -435.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C29        FP-GCM21B-0_15-IPC_A         TopLayer 180      
5300.000      -620.000      "4.7 uF"             "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0805 4.7uF 10%, 16VDC,  X7R 15%"                                 C28        FP-GCJ21B-0_3-IPC_A          TopLayer 180      
5430.000      -1189.528     "1 uF"               "VJ0603Y105KXJCW1BC Multilayer Ceramic Capacitor, 1 uF, 16 V, ± 10%, X7R, 0603 [1608 Metric]"                  C27        FP-VJ0603Y105KXJCW1BC-MFG    TopLayer 270      
5320.000      -1316.172     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C26        FP-GCM21B-0_15-IPC_A         TopLayer 0        
5355.000      -1185.000     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C25        CAPC1608X95X40LL15T15        TopLayer 90       
-74.685       -430.000      "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C24        CAPC1608X95X40LL15T15        TopLayer 0        
4723.820      -1418.126     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C23        CAPC1608X95X40LL15T15        TopLayer 90       
-88.219       -340.000      "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C22        FP-GCM21B-0_15-IPC_A         TopLayer 180      
-88.253       -520.000      "4.7 uF"             "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0805 4.7uF 10%, 16VDC,  X7R 15%"                                 C21        FP-GCJ21B-0_3-IPC_A          TopLayer 180      
40.315        -1070.000     "1 uF"               "VJ0603Y105KXJCW1BC Multilayer Ceramic Capacitor, 1 uF, 16 V, ± 10%, X7R, 0603 [1608 Metric]"                  C20        FP-VJ0603Y105KXJCW1BC-MFG    TopLayer 270      
-64.685       -1205.000     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C19        FP-GCM21B-0_15-IPC_A         TopLayer 0        
4823.820      -1433.126     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C18        FP-GCM21B-0_15-IPC_A         TopLayer 270      
4618.820      -1428.126     "4.7 uF"             "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0805 4.7uF 10%, 16VDC,  X7R 15%"                                 C17        FP-GCJ21B-0_3-IPC_A          TopLayer 270      
4068.820      -1478.126     "1 uF"               "VJ0603Y105KXJCW1BC Multilayer Ceramic Capacitor, 1 uF, 16 V, ± 10%, X7R, 0603 [1608 Metric]"                  C16        FP-VJ0603Y105KXJCW1BC-MFG    TopLayer 180      
3888.820      -1374.592     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C15        FP-GCM21B-0_15-IPC_A         TopLayer 270      
-24.685       -1065.000     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C14        CAPC1608X95X40LL15T15        TopLayer 90       
4068.820      -1408.126     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C13        CAPC1608X95X40LL15T15        TopLayer 0        
3103.820      -1388.126     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C12        CAPC1608X95X40LL15T15        TopLayer 90       
3193.820      -1403.126     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C11        FP-GCM21B-0_15-IPC_A         TopLayer 270      
3013.820      -1398.126     "4.7 uF"             "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0805 4.7uF 10%, 16VDC,  X7R 15%"                                 C10        FP-GCJ21B-0_3-IPC_A          TopLayer 270      
2498.348      -1453.126     "1 uF"               "VJ0603Y105KXJCW1BC Multilayer Ceramic Capacitor, 1 uF, 16 V, ± 10%, X7R, 0603 [1608 Metric]"                  C9         FP-VJ0603Y105KXJCW1BC-MFG    TopLayer 180      
2368.820      -1353.126     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C8         FP-GCM21B-0_15-IPC_A         TopLayer 270      
2503.348      -1388.126     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C7         CAPC1608X95X40LL15T15        TopLayer 0        
1653.820      -1393.126     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C6         CAPC1608X95X40LL15T15        TopLayer 270      
1763.820      -1374.592     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C5         FP-GCM21B-0_15-IPC_A         TopLayer 90       
1553.820      -1383.126     "4.7 uF"             "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0805 4.7uF 10%, 16VDC,  X7R 15%"                                 C4         FP-GCJ21B-0_3-IPC_A          TopLayer 90       
1009.292      -1508.126     "1 uF"               "VJ0603Y105KXJCW1BC Multilayer Ceramic Capacitor, 1 uF, 16 V, ± 10%, X7R, 0603 [1608 Metric]"                  C3         FP-VJ0603Y105KXJCW1BC-MFG    TopLayer 180      
873.820       -1403.126     "10 uF"              "0805 10 uF 6.3 V ±10% Tolerance X7R Multilayer Ceramic Chip Capacitor"                                        C2         FP-GCM21B-0_15-IPC_A         TopLayer 270      
1013.820      -1438.126     "0.1 uF"             "Ceramic Capacitor, Multilayer, Ceramic, 16V, 20% +Tol, 20% -Tol, X7R, 15% TC, 0.1uF, Surface Mount, 0603"     C1         CAPC1608X95X40LL15T15        TopLayer 0        
