(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(aux_axis_origin 42.672 157.988)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5f1)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_a20000a5)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab yes)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 4)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 168 46 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R42"
			(at 5.08 2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1001FS / 5905-00-432-6410"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "5%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1001FS / 5905-00-197-4289"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1k 1/4W 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.78"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q5-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 88 93.5 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J15"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "B2P-VH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J15-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 157.347945 127.006193 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J23"
			(at -4.5 1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J22-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J23-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 145.886976 78.261953 90)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "Q2"
			(at 5.75 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Q_NPN_EBC"
			(at 1.27 4.02 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, emitter/base/collector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "1086-3052-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "494-JANTXV2N2222A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Transistor 2N2222A TO-18 NPN"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Microchip Technology"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.78"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 -4.02 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27 90)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 90)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q1-E)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm_Pad"
		(locked yes)
		(layer "F.Cu")
		(at 176.87 143.4)
		(descr "Mounting Hole 3mm")
		(tags "mounting hole 3mm")
		(property "Reference" "H4"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Test Indication")
		(sheetfile "Test Circuit.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.5 121.5)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J21"
			(at 4.75 3.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0 7.41 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J21-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J21-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 103.5 76.2)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R21"
			(at 11.2 -4.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "51k"
			(at 11.2 4.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "MMFR6518B51K0V9"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "RESI"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 51k Ohm 1W 0.1% 5ppm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "4.65"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "25V Reference")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5B--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 117 143)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J5"
			(at 4.5 1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J4-Pin_1)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal"
		(layer "F.Cu")
		(at 146.17586 49.064465 -90)
		(descr "Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=20.32mm, 1.5W, length*diameter=14.3*5.7mm^2")
		(tags "Resistor Axial_DIN0614 series Axial Horizontal pin pitch 20.32mm 1.5W length 14.3mm diameter 5.7mm")
		(property "Reference" "R36"
			(at 10.16 -3.97 90)
			(layer "F.SilkS")
		)
		(property "Value" "3k"
			(at 10.16 3.97 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Watts" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K3700FHEB"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.37k Ohm 1/2W"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.66"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(R36-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 20.32 0 270)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J27-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 145.446465 103.433811 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R31"
			(at 5.08 2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1001FS / 5905-00-432-6410"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "5%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1001FS / 5905-00-197-4289"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1k 1/4W 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.78"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q3-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 144.975232 119.109945)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R16"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.74k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K7400FHEB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.74k Ohm 1/2W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J22-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J23-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm_Pad"
		(locked yes)
		(layer "F.Cu")
		(at 89.5 27.45)
		(descr "Mounting Hole 3mm")
		(tags "mounting hole 3mm")
		(property "Reference" "H1"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Test Indication")
		(sheetfile "Test Circuit.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 160.535581 55.154457 90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C9"
			(at 5.6 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 1.25 4.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 135 134.5)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R15"
			(at 11.2 -4.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J21-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 129 122 180)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C6"
			(at 1.5 4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 1.25 4.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "106CKH100M"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "ECEA1HKS100"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Capacitor Electrolytic 10uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.27"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 96.5 46.5 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R11"
			(at 11 4.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "TBD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "250 mW"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J19-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 112 93)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R19"
			(at 11.2 -4.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "TBD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5B--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 138 57 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R24"
			(at 11.2 4.32 180)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "TBD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5A-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "25V Reference")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 168.9091 27.3273 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J27"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J27-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J27-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 82.5 112 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.74k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K7400FHEB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.74k Ohm 1/2W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J8-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J11-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 135 144 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -3 270)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J6-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp"
		(layer "F.Cu")
		(at 102 50 90)
		(descr "Diode, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
		(property "Reference" "D2"
			(at 1.170645 2.798861 90)
			(layer "F.SilkS")
		)
		(property "Value" "25V"
			(at 1.27 3.215371 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Irev" "2mA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "JAN1N4117-1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Diode Zener 25 V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Microchip Technology"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.84"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "A"
			(at 4.500618 0.142454 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 -2.326371 90)
			(layer "F.Fab")
		)
		(fp_text user "A"
			(at 4.34 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 126.5 146 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "845"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF55845R00FHEB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 845 Ohm 1/2W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.7"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J6-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 112 102.4)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R18"
			(at 11.2 -4.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J21-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 135 80 180)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "Q1"
			(at 1 4 180)
			(layer "F.SilkS")
		)
		(property "Value" "Q_NPN_EBC"
			(at 1.27 4.02 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, emitter/base/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "1086-3052-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "494-JANTXV2N2222A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Transistor 2N2222A TO-18 NPN"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Microchip Technology"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.78"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 -4.02 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q1-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27 180)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 180)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J24-Pin_1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 139 38 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R26"
			(at 11.2 4.32 180)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "TBD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5A-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 107 120.5 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 5.086769 -2.609069 90)
			(layer "F.SilkS")
		)
		(property "Value" "SAT (3.6k to 5.7k)"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "125 mW"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "TBD"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-DIS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 168 35 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R44"
			(at 5.08 2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "365"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Watts" "250 mW"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K3650FS / 5905-00-346-8875"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H3650FS / 5905-00-194-8391"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 365 Ohm 1/4W, 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.59"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J27-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 102.5 55.3 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R23"
			(at 5 2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1001FS / 5905-00-432-6410"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "5%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1001FS / 5905-00-197-4289"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1k 1/4W 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.78"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -0.42 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.58 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 76.8 75 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J18"
			(at 0 5.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J18-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 99 123 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J7"
			(at -4.567682 1.312396 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J7-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 139.5 47.6 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R25"
			(at 11.2 4.32 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "MMFR6518B2K20V9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "RESI"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 2.2k Ohm 1W 0.1% 5PPM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "4.65"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5A-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "25V Reference")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 74 100 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J11"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J11-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 176.630465 81.060116 90)
		(descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
		(tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
		(property "Reference" "R40"
			(at 6.35 -2.92 90)
			(layer "F.SilkS")
		)
		(property "Value" "27.4k"
			(at 6.35 2.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Watts" "250 mW"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RN60D2742FB14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 27.4k Ohm 1/4W 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.93"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q6-C)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 90)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q4-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm"
		(layer "F.Cu")
		(at 129 131.5 90)
		(descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
		(tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
		(property "Reference" "C5"
			(at 1.25 -2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "5n"
			(at 1.25 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "SR155C502KART"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Capacitor Ceramic 5nF 50V"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Kyocera AVX"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.47"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 89.5 84 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J17"
			(at 0 5.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J17-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 74 83)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 5.08 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.74k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K7400FHEB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.74k Ohm 1/2W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.73"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J18-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J20-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 110 34.5 -90)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.8 -3 0)
			(layer "F.SilkS")
		)
		(property "Value" "TL072"
			(at 3.81 9.95 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3A--)")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J19-Pin_1)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D2-K)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "25V Reference")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "25V Reference")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 125.1 25.4)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R29"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1002FS / 5905-00-426-7095"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1002FS / 5905-00-138-1283"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 10k 1/4W 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.30"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3A--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q7-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 139.914061 113.627341 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R30"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.74k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K7400FHEB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.74k Ohm 1/2W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J24-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 74 136 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J2"
			(at -0.009412 6.035646 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-A)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 106 137 180)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at -2.333434 1.870458 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.47u"
			(at 1.25 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "UVR2AR33MDD1TD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Capacitor Electrolytic 0.33uF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Nichicon"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.25"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 141.988775 88.925271 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J25"
			(at 4.5 1 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J25-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 89 122)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C4"
			(at 5.635646 0.009412 90)
			(layer "F.SilkS")
		)
		(property "Value" "27u"
			(at 1.25 4.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "860160673012"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Capacitor Electrolytic 27uF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Wurth Eletronik"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.18"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J7-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 96.8 90 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 5.08 2.35 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.74k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K7400FHEB"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.74k Ohm 1/2W"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.73"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J15-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J13-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Horizontal_TabDown"
		(layer "F.Cu")
		(at 114.5 137.6)
		(descr "TO-220-3, Horizontal, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Horizontal RM 2.54mm")
		(property "Reference" "U2"
			(at 2.5 -20.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM340T15"
			(at 2.54 2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 15V, TO-220/TO-263/TO-252"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "LM340T-15/NOPB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Regulator Linear 15V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.74"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 2.54 -20.58 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at 2.54 -16.66)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Horizontal_TabDown.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 161.632984 60.900875)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.75 -2.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "TL072"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4A--)")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4B-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4B--)")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 82 129)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U1"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM555"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/icm7/icm7555-56.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CMOS General Purpose Timer, 555 compatible, PDIP-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "SE555P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "555 Timer 8 pin DIP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.35"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-A)")
			(pinfunction "TR")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_2)")
			(pinfunction "Q")
			(pintype "output")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pinfunction "R")
			(pintype "input")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-CV)")
			(pinfunction "CV")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-DIS)")
			(pinfunction "THR")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-DIS)")
			(pinfunction "DIS")
			(pintype "input")
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm_Pad"
		(locked yes)
		(layer "F.Cu")
		(at 176.7103 28.0034)
		(descr "Mounting Hole 3mm")
		(tags "mounting hole 3mm")
		(property "Reference" "H2"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Test Indication")
		(sheetfile "Test Circuit.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 159.297542 82.625813 -90)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "Q3"
			(at -2.8 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Q_PNP_BCE"
			(at 1.27 4.02 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PNP transistor, base/collector/emitter"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "2N2907 (TO-18) / 5961-00-925-3777"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Transistor 2N2907 TO-18  PNP"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.40"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 -4.02 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27 270)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 270)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J26-Pin_1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 82 97.5 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.74k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K7400FHEB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.74k Ohm 1/2W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J14-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J17-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 153.493721 48.009022 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R38"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1002FS / 5905-00-426-7095"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1002FS / 5905-00-138-1283"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 10k 1/4W 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.30"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(R36-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4A-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 107.89 58.2824)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C7"
			(at 1.25 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 96.5 37 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R12"
			(at 11.2 4.32 180)
			(layer "F.SilkS")
		)
		(property "Value" "3k"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "MMFR6518B3K00V9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.05%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "250 mW"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "RESI"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 3k Ohm 1W 0.1% 5ppm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "4.65"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J19-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 157.954041 40.288185)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R43"
			(at 5.08 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1002FS / 5905-00-426-7095"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1002FS / 5905-00-138-1283"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 10k 1/4W 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.30"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(R34-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4B-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 77 145.8 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at -4.6 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 103 113 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J10"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "B2P-VH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 74 91 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J14"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J14-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 176.444312 62.961257 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R41"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "698"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "125 mW"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H6980FS / 5905-00-169-9453"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K6980FS / 5905-00-192-3461"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 698 Ohm 1/4W 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.20"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q4-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 96.5 65.3 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R9"
			(at 11 4.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "3k"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "MMFR6518B3K00V9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.05%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "250 mW"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "RESI"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 3k Ohm 1W 0.1% 5ppm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "4.65"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J19-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J18-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 74 109 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J8"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "B2P-VH"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J8-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 95 75 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J20"
			(at 0 5.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J20-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 147.347945 127.006193 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J22"
			(at -4.5 1.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J22-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J22-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 107.5 143)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J4"
			(at 4.5 1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm_Pad"
		(locked yes)
		(layer "F.Cu")
		(at 88.8 143.9)
		(descr "Mounting Hole 3mm")
		(tags "mounting hole 3mm")
		(property "Reference" "H3"
			(at 0 -4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "Test Indication")
		(sheetfile "Test Circuit.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6 6)
			(drill 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 154.638232 63.990558 -90)
		(descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
		(tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
		(property "Reference" "R37"
			(at 6.35 2.92 90)
			(layer "F.SilkS")
		)
		(property "Value" "27.4k"
			(at 6.35 2.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Watts" "250 mW"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RN60D2742FB14"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 27.4k Ohm 1/4W 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.93"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q5-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 270)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J25-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal"
		(layer "F.Cu")
		(at 101 84.85)
		(descr "Resistor, Axial_DIN0414 series, Axial, Horizontal, pin pitch=15.24mm, 2W, length*diameter=11.9*4.5mm^2, http://www.vishay.com/docs/20128/wkxwrx.pdf")
		(tags "Resistor Axial_DIN0414 series Axial Horizontal pin pitch 15.24mm 2W length 11.9mm diameter 4.5mm")
		(property "Reference" "R20"
			(at 7.62 -3.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "40k"
			(at 7.62 3.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "UPF50B40KV"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "TE Connectivity Passive Product"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 40k Ohm 1/2W 1% 5ppm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "5.09"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15.24 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5B--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0414_L11.9mm_D4.5mm_P15.24mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 170.46269 74.320271 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R39"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1002FS / 5905-00-426-7095"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1002FS / 5905-00-138-1283"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 10k 1/4W 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.30"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4B--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q2-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 158.29772 105.704953 -90)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "Q6"
			(at 5.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "Q_PNP_BCE"
			(at 1.27 4.02 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PNP transistor, base/collector/emitter"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "2N2907 (TO-18) / 5961-00-925-3777"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Transistor 2N2907 TO-18  PNP"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.40"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 -4.02 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 270)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27 270)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J26-Pin_2)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 270)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q6-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 109.5 48.5 -90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C8"
			(at -3.4 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 1.25 4.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field5" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field6" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field7" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field9" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field10" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field11" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 169.135953 55.104162 90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C10"
			(at 5.2 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 3.75 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 96.5 55.8 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R10"
			(at 11 4.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "TBD"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "250 mW"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J19-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J18-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 119.8 27.5 180)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R27"
			(at 11.2 4.32 180)
			(layer "F.SilkS")
		)
		(property "Value" "3.3k"
			(at 11.2 4.32 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.05%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "MMFR6518B3K30V9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "RESI"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 3.3k Ohm 1W 0.1% 5ppm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "4.65"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5A-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 150.542982 112.722038 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R32"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "365"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Watts" "250 mW"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K3650FS / 5905-00-346-8875"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H3650FS / 5905-00-194-8391"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 365 Ohm 1/4W, 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.59"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J26-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 88 103 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J12"
			(at 0 5.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J11-Pin_2)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/Users/namlun/Documents/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp"
		(layer "F.Cu")
		(at 74.3 128.5)
		(descr "Diode, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
		(tags "Diode DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
		(property "Reference" "D1"
			(at 1.27 -2.750635 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N4001"
			(at 1.27 3.639635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "4878-1N4001CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Diode Generic Rectifier"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "673-1N4001"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Diotec Semiconductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.11"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "A"
			(at 4.64 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 1.27 -2.750635 0)
			(layer "F.Fab")
		)
		(fp_text user "A"
			(at 4.64 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 2.2 2.2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 73.2 122.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.33k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60H1331FS / 5905-00-459-2840"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "250 mW"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60K1331FS / 5905-00-721-2376"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.33k Ohm 1/4W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.29"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 103 103 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J13"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J13-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 83 75 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J19"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J19-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J19-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 105.5 93 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J16"
			(at 0 5.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J13-Pin_1)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm"
		(layer "F.Cu")
		(at 144.9 34.8)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U5"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "TL072"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tl071.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(R36-Pad1)")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q7-C)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q4-C)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(R34-Pad1)")
			(pintype "output")
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 109 66.85)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R22"
			(at 11.2 -4.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "SAT"
			(at 11.2 4.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.25W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PPM" "5ppm/C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Toll" "0.1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "TBD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "25V Reference")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U5B--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 141.5 144)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R14"
			(at 11.2 -4.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "13k"
			(at 11.2 4.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J21-Pin_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 96.8 115 90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.74k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "CMF551K7400FHEB"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "0.5W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 1.74k Ohm 1/2W"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.73"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J9-Pin_2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 98 143)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at 4.5 1.7 270)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 125.1 30.7)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R28"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1002FS / 5905-00-426-7095"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1002FS / 5905-00-138-1283"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 10k 1/4W 1%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.30"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U3A--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q4-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 175.221845 37.716968)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "Q5"
			(at 1 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "Q_PNP_BCE"
			(at 1.27 4.02 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PNP transistor, base/collector/emitter"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "2N2907 (TO-18) / 5961-00-925-3777"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Transistor 2N2907 TO-18  PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.40"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 -4.02 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q5-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J27-Pin_1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Rect_L4.0mm_W2.5mm_P2.50mm"
		(layer "F.Cu")
		(at 97 137.5 180)
		(descr "C, Rect series, Radial, pin pitch=2.50mm, , length*width=4*2.5mm^2, Capacitor")
		(tags "C Rect series Radial pin pitch 2.50mm  length 4mm width 2.5mm Capacitor")
		(property "Reference" "C1"
			(at 1.25 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 1.25 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" "R82EC2100AA50J"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "K103K15X7RF53K2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Capacitor Ceramic 10nF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Beyschlang/Draloric/BC Components"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.20"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-CV)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L4.0mm_W2.5mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 88 112 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J9-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 141.954934 95.733495)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J24"
			(at -4.5 1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J24-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J24-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm"
		(layer "F.Cu")
		(at 149.6 27)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C11"
			(at 1.25 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.25 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal"
		(layer "F.Cu")
		(at 176.605441 97.758534 180)
		(descr "Resistor, Axial_DIN0614 series, Axial, Horizontal, pin pitch=20.32mm, 1.5W, length*diameter=14.3*5.7mm^2")
		(tags "Resistor Axial_DIN0614 series Axial Horizontal pin pitch 20.32mm 1.5W length 14.3mm diameter 5.7mm")
		(property "Reference" "R34"
			(at 10.16 4 0)
			(layer "F.SilkS")
		)
		(property "Value" "3k"
			(at 10.16 3.97 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Watts" "250mW"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K8660FS / 5905-00-428-7161"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H8660FS / 5905-00-024-7657"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 866 Ohm 1/4W 1%"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.34"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 10.16 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(R34-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 20.32 0 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J26-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0614_L14.3mm_D5.7mm_P20.32mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_2pin 2.54mm HWS4548:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 167.407356 82.487565 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J26"
			(at 0 5.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.87 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "Talk with Russell about Tooling"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J26-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J26-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/2pin.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_Power_L20.0mm_W6.4mm_P22.40mm"
		(layer "F.Cu")
		(at 112 111.8)
		(descr "Resistor, Axial_Power series, Box, pin pitch=22.4mm, 4W, length*width*height=20*6.4*6.4mm^3, http://cdn-reichelt.de/documents/datenblatt/B400/5WAXIAL_9WAXIAL_11WAXIAL_17WAXIAL%23YAG.pdf")
		(tags "Resistor Axial_Power series Box pin pitch 22.4mm 4W length 20mm width 6.4mm height 6.4mm")
		(property "Reference" "R17"
			(at 11.2 -4.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.8k"
			(at 11.2 4.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 11.2 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 22.4 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J21-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_Power_L20.0mm_W6.4mm_P22.40mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 139.039728 63.475224 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R35"
			(at 5.08 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Wattage" "0.125W"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1002FS / 5905-00-426-7095"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1002FS / 5905-00-138-1283"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 10k 1/4W 1%"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "1.30"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U4A--)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 176.378744 47.977557 90)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "Q4"
			(at 5.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "Q_NPN_EBC"
			(at 1.27 4.02 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, emitter/base/collector"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "1086-3052-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "494-JANTXV2N2222A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Transistor 2N2222A TO-18 NPN"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey / Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Microchip Technology"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.78"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 -4.02 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 90)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27 90)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 90)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q4-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal"
		(layer "F.Cu")
		(at 150.381651 97.482162 90)
		(descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
		(tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
		(property "Reference" "R33"
			(at 6.35 3.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "27.4k"
			(at 6.35 2.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Watts" "250 mW"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RN60D2742FB14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tol" "1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 27.4k Ohm 1/4W 1%"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.93"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 6.35 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q3-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 12.7 0 90)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J25-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 73.2 117)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 5.08 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 5.08 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "RNC60K1003FS / 5905-00-137-0804 (DLA)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Power" "125 mW"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "RNC60H1003FS / 5905-00-407-2160"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Resistor 100k Ohm 1/4W"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Vishay Dale"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.44"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+15V")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J7-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-18-3"
		(layer "F.Cu")
		(at 143.4 27 180)
		(descr "TO-18-3")
		(tags "TO-18-3")
		(property "Reference" "Q7"
			(at 1.15 4 180)
			(layer "F.SilkS")
		)
		(property "Value" "Q_PNP_BCE"
			(at 1.27 4.02 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PNP transistor, base/collector/emitter"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "2N2907 (TO-18) / 5961-00-925-3777"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Transistor 2N2907 TO-18  PNP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "DLA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "3.40"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 -4.02 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0 180)
			(size 1.6 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 1.27 180)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J27-Pin_2)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 180)
			(size 1.2 1.2)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q7-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-18-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 95.5 130)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 5.8623 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 1.25 4.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Tollerance" "20%"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number / NSN" "106CKH100M"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part Number / NSN" "ECEA1HKS100"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternate Part Number /  NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Alternte Part Number / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartNumber / NSN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Nomenclature" "Capacitor Electrolytic 10uF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Panasonic Electronic Components"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price (EA)" "0.27"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Source" "Digikey, Mouser"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Ic" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Pulse Load Circuit")
		(sheetfile "PulseLoadCircuit.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-DIS)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm"
		(layer "F.Cu")
		(at 157.8 27)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
		(property "Reference" "C12"
			(at 1.2 -4.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 1.25 4.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Over Under Voltage Detectors")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+28")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 69.033933 20.835995)
		(end 182.918904 150.379157)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Pulse Load Tester"
		(at 170.815 135.89 90)
		(layer "F.SilkS")
	)
	(gr_text "Ver:"
		(at 176.53 135.755551 90)
		(layer "F.SilkS")
	)
	(zone
		(net "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 69.85 21.59) (xy 182.245 21.59) (xy 182.245 149.86) (xy 69.85 149.86)
			)
		)
	)
	(embedded_fonts no)
)
