(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "cryo_pdk_arduino_board_v1_gerbers/")
		)
	)
	(net 0 "")
	(net 1 "/Supdate_HV")
	(net 2 "/Sclkn_HV")
	(net 3 "unconnected-(A1-PadA3)")
	(net 4 "unconnected-(A1-A5{slash}SCL-PadA5)")
	(net 5 "unconnected-(A1-D1{slash}TX-PadD1)")
	(net 6 "unconnected-(A1-PadD10)")
	(net 7 "unconnected-(A1-PadAREF)")
	(net 8 "unconnected-(A1-PadA2)")
	(net 9 "/Sclkp_HV")
	(net 10 "unconnected-(A1-PadD8)")
	(net 11 "unconnected-(A1-RESET-PadRST1)")
	(net 12 "GND")
	(net 13 "unconnected-(A1-D11_MOSI-PadD11)")
	(net 14 "unconnected-(A1-RESET-PadRST2)")
	(net 15 "unconnected-(A1-D13_SCK-PadD13)")
	(net 16 "unconnected-(A1-D0{slash}RX-PadD0)")
	(net 17 "/Senable_HV")
	(net 18 "unconnected-(A1-A4{slash}SDA-PadA4)")
	(net 19 "/Sin_HV")
	(net 20 "unconnected-(A1-PadA6)")
	(net 21 "/Sout_Chip1_HV")
	(net 22 "/Sreset_HV")
	(net 23 "unconnected-(A1-PadVIN)")
	(net 24 "unconnected-(A1-D12_MISO-PadD12)")
	(net 25 "+5V")
	(net 26 "unconnected-(A1-PadA7)")
	(net 27 "unconnected-(A1-PadD9)")
	(net 28 "/DIR Sin")
	(net 29 "unconnected-(A1-GND-PadGND1)")
	(net 30 "/Sout_Chip2_HV")
	(net 31 "/VSSA")
	(net 32 "/1V8")
	(net 33 "/Sin_0V9")
	(net 34 "/Sclkn_0V9")
	(net 35 "/Chip1_Sout_0V9")
	(net 36 "/Sreset_0V9")
	(net 37 "/Supdate_0V9")
	(net 38 "/Chip1_vd_sense")
	(net 39 "/vb")
	(net 40 "/Chip1_vs_sense")
	(net 41 "/Chip1_vd_force")
	(net 42 "/vgxp")
	(net 43 "/Chip2_vd_sense")
	(net 44 "/Chip2_Sout_0V9")
	(net 45 "/Chip2_vs_sense")
	(net 46 "/0V9")
	(net 47 "/Senable_0V9")
	(net 48 "/Sclkp_0V9")
	(net 49 "/VDDA")
	(net 50 "/vgxn")
	(net 51 "/Chip1_vs_force")
	(net 52 "/vg")
	(net 53 "/Chip2_vd_force")
	(net 54 "/Chip2_vs_force")
	(net 55 "VCC")
	(net 56 "/DIR Sreset")
	(net 57 "/DIR Sclk")
	(net 58 "/DIR Sout")
	(footprint "Connector_Coaxial:SMA_Amphenol_132134-16_Vertical"
		(layer "F.Cu")
		(at 187.246 109.3)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/598157/parent/132134-16/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J8"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/vgxn")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-16_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 171.9365 96.52 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 42 "/vgxp")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "/VSSA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 157.48 98.9095 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/0V9")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/VDDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 128.7565 96.266 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 32 "/1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "arduino-library:lbl_logo"
		(layer "F.Cu")
		(at 142.494 57.15)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 122.682 96.266)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 55 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.15 88.9 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J13"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0 7.46 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "/DIR Sout")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "VCC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 143.375589 96.385589 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 46 "/0V9")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134-16_Vertical"
		(layer "F.Cu")
		(at 144.502 109.3)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/598157/parent/132134-16/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J5"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/0V9")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-16_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "arduino footprints:TE_5747846-6"
		(layer "F.Cu")
		(at 201.3712 66.27 90)
		(descr "<b>SUB-D</b>")
		(property "Reference" "J1"
			(at -38.7915 -3.7026 90)
			(layer "F.SilkS")
		)
		(property "Value" "TE 5747846-6"
			(at -25.49062 19.054235 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Cinch Connectivity Solutions"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "Commercial PCB Mount Connector | Socket | 25 Positions | Yellow Chromate over Cadmium | Thermoset, Glass-Reinforced, Diallyl Phthalate | Female | 90 PCB | Narrow Profile | Jackpost"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "DCCM25SCBRP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "Unavailable"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "25"
			(at -34.4081 3.18017 90)
			(layer "F.SilkS")
		)
		(fp_text user "14"
			(at 0.992 3.08357 90)
			(layer "F.SilkS")
		)
		(fp_text user "13"
			(at -35.6494 0.682733 90)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at -34.3909 3.17858 90)
			(layer "F.Fab")
		)
		(fp_text user "13"
			(at -35.6694 0.683116 90)
			(layer "F.Fab")
		)
		(fp_text user "14"
			(at -0.209045 3.07907 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/vg")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -2.76 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/vgxn")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -5.52 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/vgxp")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -8.28 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/Chip1_vd_sense")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at -11.04 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/Chip1_vs_sense")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at -13.8 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/Chip1_vd_force")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at -16.56 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/Chip1_vs_force")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -19.32 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/Supdate_0V9")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at -22.08 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/Sreset_0V9")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at -24.84 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/Sclkp_0V9")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at -27.6 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/Sclkn_0V9")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at -30.36 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/Senable_0V9")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at -33.12 0 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/Sin_0V9")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at -1.38 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/0V9")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at -4.14 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at -6.9 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/Chip2_vd_sense")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at -9.66 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/Chip2_vs_sense")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at -12.42 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/Chip2_vd_force")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at -15.18 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/Chip2_vs_force")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at -17.94 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/vb")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "21" thru_hole circle
			(at -20.7 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/1V8")
			(pinfunction "21")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "22" thru_hole circle
			(at -23.46 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/VDDA")
			(pinfunction "22")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "23" thru_hole circle
			(at -26.22 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "23")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "24" thru_hole circle
			(at -28.98 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/Chip2_Sout_0V9")
			(pinfunction "24")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "25" thru_hole circle
			(at -31.74 2.8448 90)
			(size 1.5621 1.5621)
			(drill 1.0414)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/Chip1_Sout_0V9")
			(pinfunction "25")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "G1" thru_hole circle
			(at -40.0804 1.4224 90)
			(size 4.191 4.191)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(pad "G2" thru_hole circle
			(at 6.9604 1.4224 90)
			(size 4.191 4.191)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/5747846_6/5747846-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 158.75 53.848)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -2.794 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/Chip1_vs_force")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/Chip1_vs_sense")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 185.6525 101.6 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 1.778 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 50 "/vgxn")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "/VSSA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 122.682 91.186)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 55 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 162.306 64.516)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at -3.048 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/Chip1_vd_force")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/Chip1_vd_sense")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.15 70.104 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J11"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 13.6385 15.09 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/DIR Sreset")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "VCC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 143.354089 100.703589 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 46 "/0V9")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 122.522 52.006)
		(descr "Mounting Hole 3mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H4"
			(at 0 -3.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.15 82.55 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 13.6385 15.09 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/DIR Sin")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "VCC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 171.9365 101.346 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 42 "/vgxp")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "/VSSA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 173.228 56.642 90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0 10 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/Chip2_vs_force")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/Chip2_vd_force")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/Chip2_vs_sense")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/Chip2_vd_sense")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "arduino-library:Arduino_Nano_Socket"
		(layer "F.Cu")
		(at 118.966 77.724 -90)
		(descr "https://docs.arduino.cc/hardware/nano")
		(property "Reference" "A1"
			(at 0 -44.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "Arduino_Nano_Socket"
			(at 0 -21.082 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://docs.arduino.cc/hardware/nano"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Socket for Arduino Nano"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Arduino_Nano_Socket")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "D0"
			(at -10.16 -36.736 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "D0"
			(at -10.16 -36.736 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "USB"
			(at 0 0.9525 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -7.62 -41.91 270)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -7.62 -1.27 270)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 7.62 -41.91 270)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 7.62 -1.27 270)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "3V3" thru_hole circle
			(at 7.62 -6.35 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "VCC")
			(pinfunction "3.3V")
			(pintype "power_out")
		)
		(pad "5V" thru_hole circle
			(at 7.62 -31.75 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "+5V")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "A0" thru_hole circle
			(at 7.62 -11.43 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/Sout_Chip1_HV")
			(pinfunction "A0")
			(pintype "bidirectional")
		)
		(pad "A1" thru_hole circle
			(at 7.62 -13.97 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/Sout_Chip2_HV")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "A2" thru_hole circle
			(at 7.62 -16.51 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(A1-PadA2)")
			(pinfunction "A2")
			(pintype "bidirectional+no_connect")
		)
		(pad "A3" thru_hole circle
			(at 7.62 -19.05 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(A1-PadA3)")
			(pinfunction "A3")
			(pintype "bidirectional+no_connect")
		)
		(pad "A4" thru_hole circle
			(at 7.62 -21.59 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A1-A4{slash}SDA-PadA4)")
			(pinfunction "A4/SDA")
			(pintype "bidirectional+no_connect")
		)
		(pad "A5" thru_hole circle
			(at 7.62 -24.13 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(A1-A5{slash}SCL-PadA5)")
			(pinfunction "A5/SCL")
			(pintype "bidirectional+no_connect")
		)
		(pad "A6" thru_hole circle
			(at 7.62 -26.67 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(A1-PadA6)")
			(pinfunction "A6")
			(pintype "input+no_connect")
		)
		(pad "A7" thru_hole circle
			(at 7.62 -29.21 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(A1-PadA7)")
			(pinfunction "A7")
			(pintype "input+no_connect")
		)
		(pad "AREF" thru_hole circle
			(at 7.62 -8.89 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(A1-PadAREF)")
			(pinfunction "AREF")
			(pintype "input+no_connect")
		)
		(pad "D0" thru_hole circle
			(at -7.62 -36.83 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A1-D0{slash}RX-PadD0)")
			(pinfunction "D0/RX")
			(pintype "bidirectional+no_connect")
		)
		(pad "D1" thru_hole circle
			(at -7.62 -39.37 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(A1-D1{slash}TX-PadD1)")
			(pinfunction "D1/TX")
			(pintype "bidirectional+no_connect")
		)
		(pad "D2" thru_hole circle
			(at -7.62 -29.21 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Supdate_HV")
			(pinfunction "D2_INT0")
			(pintype "bidirectional")
		)
		(pad "D3" thru_hole circle
			(at -7.62 -26.67 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/Sreset_HV")
			(pinfunction "D3_INT1")
			(pintype "bidirectional")
		)
		(pad "D4" thru_hole circle
			(at -7.62 -24.13 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Sclkp_HV")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "D5" thru_hole circle
			(at -7.62 -21.59 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/Sclkn_HV")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "D6" thru_hole circle
			(at -7.62 -19.05 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/Senable_HV")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "D7" thru_hole circle
			(at -7.62 -16.51 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Sin_HV")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "D8" thru_hole circle
			(at -7.62 -13.97 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(A1-PadD8)")
			(pinfunction "D8")
			(pintype "bidirectional+no_connect")
		)
		(pad "D9" thru_hole circle
			(at -7.62 -11.43 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(A1-PadD9)")
			(pinfunction "D9")
			(pintype "bidirectional+no_connect")
		)
		(pad "D10" thru_hole circle
			(at -7.62 -8.89 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(A1-PadD10)")
			(pinfunction "D10")
			(pintype "bidirectional+no_connect")
		)
		(pad "D11" thru_hole circle
			(at -7.62 -6.35 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(A1-D11_MOSI-PadD11)")
			(pinfunction "D11_MOSI")
			(pintype "bidirectional+no_connect")
		)
		(pad "D12" thru_hole circle
			(at -7.62 -3.81 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A1-D12_MISO-PadD12)")
			(pinfunction "D12_MISO")
			(pintype "bidirectional+no_connect")
		)
		(pad "D13" thru_hole circle
			(at 7.62 -3.81 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(A1-D13_SCK-PadD13)")
			(pinfunction "D13_SCK")
			(pintype "bidirectional+no_connect")
		)
		(pad "GND1" thru_hole rect
			(at -7.62 -31.75 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(A1-GND-PadGND1)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "GND2" thru_hole rect
			(at 7.62 -36.83 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "RST1" thru_hole circle
			(at -7.62 -34.29 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(A1-RESET-PadRST1)")
			(pinfunction "RESET")
			(pintype "open_collector+no_connect")
		)
		(pad "RST2" thru_hole circle
			(at 7.62 -34.29 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(A1-RESET-PadRST2)")
			(pinfunction "RESET")
			(pintype "open_collector+no_connect")
		)
		(pad "VIN" thru_hole circle
			(at 7.62 -39.37 270)
			(size 1.7272 1.7272)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(A1-PadVIN)")
			(pinfunction "VIN")
			(pintype "power_in+no_connect")
		)
		(embedded_fonts no)
		(model "C:/Users/bglen/OneDrive/Documents/KiCad/9.0/kicad-lib-arduino-main/Arduino.3dshapes/arduino_nano.x3d"
			(offset
				(xyz -7.5 39.5 2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134-16_Vertical"
		(layer "F.Cu")
		(at 172.998 109.3)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/598157/parent/132134-16/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J7"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/vgxp")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-16_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 176.022 63.246)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -2.8975 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/Chip2_vs_force")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/Chip2_vs_sense")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134-16_Vertical"
		(layer "F.Cu")
		(at 158.75 109.3)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/598157/parent/132134-16/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J10"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/VDDA")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/VSSA")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-16_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 202.522 113.006)
		(descr "Mounting Hole 3mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H2"
			(at 0 -3.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "arduino-library:slac_logo"
		(layer "F.Cu")
		(at 128.524 59.436)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 156.718 57.15 90)
		(descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x04 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 0 10 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/Chip1_vs_force")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/Chip1_vd_force")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/Chip1_vs_sense")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/Chip1_vd_sense")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 122.522 113.006)
		(descr "Mounting Hole 3mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H1"
			(at 0 -3.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 178.562 53.594)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 2.794 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/Chip2_vd_force")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/Chip2_vd_sense")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3mm"
		(layer "F.Cu")
		(at 202.522 52.006)
		(descr "Mounting Hole 3mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H3"
			(at 0 -3.95 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 189.987 56.642 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J9"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 4.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/vb")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/vg")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 164.0625 101.346 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 49 "/VDDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "/VSSA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 184.15 76.2 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J12"
			(at 0 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Pin"
			(at 13.6385 15.09 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/DIR Sclk")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "VCC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 185.674 96.774 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 50 "/vgxn")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "/VSSA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 128.7565 100.838 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 32 "/1V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 164.0625 96.52 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 49 "/VDDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "/VSSA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132134-16_Vertical"
		(layer "F.Cu")
		(at 130.254 109.3)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/598157/parent/132134-16/")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J6"
			(at 0 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/1V8")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132134-16_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 151.638 102.362)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 2.032 180)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.43 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/VSSA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-8_3x3mm_P0.65mm"
		(layer "B.Cu")
		(at 173.482 91.948)
		(descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U4"
			(at 0 2.54 180)
			(layer "B.SilkS")
		)
		(property "Value" "SN74AXC2T45DCTR"
			(at 0 -2.45 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/sn74axc2t45"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP_T45DCTR_TEX SSOP_T45DCTR_TEX-M SSOP_T45DCTR_TEX-L")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.762 0.762 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "VCC")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/Sout_Chip1_HV")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/Sout_Chip2_HV")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "5" smd roundrect
			(at 2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/DIR Sout")
			(pinfunction "DIR")
			(pintype "unspecified")
		)
		(pad "6" smd roundrect
			(at 2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/Chip2_Sout_0V9")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Chip1_Sout_0V9")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/0V9")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-8_3x3mm_P0.65mm"
		(layer "B.Cu")
		(at 173.482 85.598)
		(descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U2"
			(at 0 2.45 180)
			(layer "B.SilkS")
		)
		(property "Value" "SN74AXC2T45DCTR"
			(at 0 -2.45 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/sn74axc2t45"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP_T45DCTR_TEX SSOP_T45DCTR_TEX-M SSOP_T45DCTR_TEX-L")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "VCC")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/Sin_HV")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/Senable_HV")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "5" smd roundrect
			(at 2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/DIR Sin")
			(pinfunction "DIR")
			(pintype "unspecified")
		)
		(pad "6" smd roundrect
			(at 2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/Senable_0V9")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Sin_0V9")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/0V9")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-8_3x3mm_P0.65mm"
		(layer "B.Cu")
		(at 173.482 79.248)
		(descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U9"
			(at 0 2.45 180)
			(layer "B.SilkS")
		)
		(property "Value" "SN74AXC2T45DCTR"
			(at 0 -2.45 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/sn74axc2t45"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP_T45DCTR_TEX SSOP_T45DCTR_TEX-M SSOP_T45DCTR_TEX-L")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "VCC")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/Sclkn_HV")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/Sclkp_HV")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "5" smd roundrect
			(at 2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/DIR Sclk")
			(pinfunction "DIR")
			(pintype "unspecified")
		)
		(pad "6" smd roundrect
			(at 2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/Sclkp_0V9")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Sclkn_0V9")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/0V9")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:MSOP-8_3x3mm_P0.65mm"
		(layer "B.Cu")
		(at 173.482 72.898)
		(descr "MSOP, 8 Pin (https://www.jedec.org/system/files/docs/mo-187F.pdf variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "MSOP SO")
		(property "Reference" "U3"
			(at 0 2.45 180)
			(layer "B.SilkS")
		)
		(property "Value" "SN74AXC2T45DCTR"
			(at 0 -2.45 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/sn74axc2t45"
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP_T45DCTR_TEX SSOP_T45DCTR_TEX-M SSOP_T45DCTR_TEX-L")
		(sheetname "/")
		(sheetfile "cryo_pdk_arduino_board_v5.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "VCC")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/Sreset_HV")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/Supdate_HV")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "5" smd roundrect
			(at 2.1125 -0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/DIR Sreset")
			(pinfunction "DIR")
			(pintype "unspecified")
		)
		(pad "6" smd roundrect
			(at 2.1125 -0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/Supdate_0V9")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.1125 0.325)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Sreset_0V9")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.1125 0.975)
			(size 1.625 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/0V9")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8_3x3mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 117.696 47.926)
		(end 209.042 117.428)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "vs_s"
		(at 178.816 61.722 90)
		(layer "F.SilkS")
	)
	(gr_text "vd_f"
		(at 176.276 61.722 90)
		(layer "F.SilkS")
	)
	(gr_text "vg"
		(at 193.04 60.706 90)
		(layer "F.SilkS")
	)
	(gr_text "vs_f"
		(at 157.226 61.976 90)
		(layer "F.SilkS")
	)
	(gr_text "Hi"
		(at 179.578 85.598 0)
		(layer "F.SilkS")
	)
	(gr_text "Chip 1"
		(at 157.226 51.816 0)
		(layer "F.SilkS")
	)
	(gr_text "Lo\n"
		(at 182.118 73.152 0)
		(layer "F.SilkS")
	)
	(gr_text "28nm CRYO PDK DAQ board, v5\nB.L. 2026-06-03\n\n"
		(at 121.92 67.056 0)
		(layer "F.SilkS")
	)
	(gr_text "vb"
		(at 190.246 60.706 90)
		(layer "F.SilkS")
	)
	(gr_text "Supdate / Sreset"
		(at 163.576 70.612 0)
		(layer "F.SilkS")
	)
	(gr_text "Chip 2"
		(at 172.974 51.816 0)
		(layer "F.SilkS")
	)
	(gr_text "Hi"
		(at 179.578 73.152 0)
		(layer "F.SilkS")
	)
	(gr_text "vgxn"
		(at 184.404 115.824 0)
		(layer "F.SilkS")
	)
	(gr_text "Sclk"
		(at 173.482 76.962 0)
		(layer "F.SilkS")
	)
	(gr_text "vs_f"
		(at 173.736 61.722 90)
		(layer "F.SilkS")
	)
	(gr_text "vd_s"
		(at 164.846 61.976 90)
		(layer "F.SilkS")
	)
	(gr_text "Sin / Senable"
		(at 165.862 83.312 0)
		(layer "F.SilkS")
	)
	(gr_text "VDDA"
		(at 155.906429 115.824 0)
		(layer "F.SilkS")
	)
	(gr_text "Lo\n"
		(at 182.118 79.248 0)
		(layer "F.SilkS")
	)
	(gr_text "Lo\n"
		(at 182.118 91.948 0)
		(layer "F.SilkS")
	)
	(gr_text "Hi"
		(at 179.578 91.948 0)
		(layer "F.SilkS")
	)
	(gr_text "vgxp"
		(at 170.280214 115.824 0)
		(layer "F.SilkS")
	)
	(gr_text "Sout"
		(at 173.482 89.408 0)
		(layer "F.SilkS")
	)
	(gr_text "1.8V"
		(at 128.016 115.824 0)
		(layer "F.SilkS")
	)
	(gr_text "vs_s"
		(at 162.306 61.976 90)
		(layer "F.SilkS")
	)
	(gr_text "0.9V"
		(at 142.139786 115.824 0)
		(layer "F.SilkS")
	)
	(gr_text "Lo\n"
		(at 182.372 85.598 0)
		(layer "F.SilkS")
	)
	(gr_text "vd_f"
		(at 159.766 61.976 90)
		(layer "F.SilkS")
	)
	(gr_text "Hi"
		(at 179.578 79.248 0)
		(layer "F.SilkS")
	)
	(gr_text "Shared"
		(at 187.452 51.816 0)
		(layer "F.SilkS")
	)
	(gr_text "vd_s"
		(at 181.356 61.722 90)
		(layer "F.SilkS")
	)
	(zone
		(net 32)
		(net_name "/1V8")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.73 88.138) (xy 139.192 88.138) (xy 139.192 116.84) (xy 125.73 116.84)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/1V8")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.73 88.138) (xy 176.276 88.138) (xy 176.276 92.202) (xy 125.73 92.202)
			)
		)
	)
	(zone
		(net 12)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 208.28 90.424) (xy 201.93 90.424) (xy 201.93 98.552) (xy 151.384 98.552) (xy 151.384 116.84)
				(xy 118.11 117.094) (xy 118.618 48.768) (xy 208.28 48.768)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/VSSA")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 202.692 91.186) (xy 208.28 91.186) (xy 208.28 116.84) (xy 152.146 116.84) (xy 152.146 99.314)
				(xy 202.692 99.314)
			)
		)
	)
	(zone
		(net 55)
		(net_name "VCC")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.736 71.374) (xy 123.952 71.374) (xy 123.952 93.98) (xy 173.736 93.98)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/0V9")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.384 116.84) (xy 151.384 98.552) (xy 201.93 98.806) (xy 201.93 90.424) (xy 208.534 90.424)
				(xy 208.534 48.514) (xy 140.208 48.514) (xy 139.954 116.84)
			)
		)
	)
	(embedded_fonts no)
)
