(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/COMPLOW")
	(net 3 "/COMPHIGH")
	(net 4 "/RING")
	(footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount"
		(layer "F.Cu")
		(at 132.88 59.1 90)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/595984/parent/132289/")
		(tags "SMA")
		(property "Reference" "RING1"
			(at -4.5 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_Coaxial"
			(at 5 6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "middle board v2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.79 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 180)
			(size 1.5 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/RING")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -4.25 180)
			(size 1.5 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -4.25 180)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 4.25 180)
			(size 1.5 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 4.25 180)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2_Pad_TopBottom"
		(layer "F.Cu")
		(at 133 73.678)
		(descr "Mounting Hole 2.2mm, M2, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "ringendcap1"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "middle board v2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.6 2.6)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/RING")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.4 4.4)
			(layers "F.Cu" "F.Mask")
			(net 4 "/RING")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.4 4.4)
			(layers "B.Cu" "B.Mask")
			(net 4 "/RING")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "mine:single sided 1.2m holes for DC"
		(layer "B.Cu")
		(at 122.1 75.15 180)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 ISO14580")
		(property "Reference" "complower1"
			(at 0 3.2 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 -3.2 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "middle board v2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/COMPLOW")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "B.Cu" "B.Mask")
			(net 2 "/COMPLOW")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount"
		(layer "B.Cu")
		(at 155.35 59.1125 90)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/595984/parent/132289/")
		(tags "SMA")
		(property "Reference" "COMPHIGH1"
			(at -4.5 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_Coaxial"
			(at 5 -6 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "middle board v2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.79 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "/COMPHIGH")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -4.25)
			(size 1.5 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -4.25)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 4.25)
			(size 1.5 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 4.25)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "mine:single sided 1.2m holes for DC"
		(layer "B.Cu")
		(at 143.9 75.15 180)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 ISO14580")
		(property "Reference" "compupper1"
			(at 0 3.2 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_Pad"
			(at 0 -3.2 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "middle board v2.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/COMPHIGH")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "B.Cu" "B.Mask")
			(net 3 "/COMPHIGH")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount"
		(layer "B.Cu")
		(at 110.75 59.1 90)
		(descr "https://www.amphenolrf.com/library/download/link/link_id/595984/parent/132289/")
		(tags "SMA")
		(property "Reference" "COMPLOW1"
			(at -4.5 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_Coaxial"
			(at 5 -6 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "middle board v2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 4.79 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "/COMPLOW")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -4.25)
			(size 1.5 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -4.25)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 4.25)
			(size 1.5 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 4.25)
			(size 1.5 5.08)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 143.772205 77.75)
		(end 121.94 77.75)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 146.35 67.7)
		(end 148.65 67.7)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 139.3 74.4)
		(end 141.6 74.4)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 126.7 74.4)
		(end 129 74.4)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161 56.05)
		(end 105 56.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161 61.55)
		(end 161 56.05)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.772205 77.75)
		(end 161 61.55)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105 61.55)
		(end 121.934139 77.75)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 137.45 67.7)
		(end 139.75 67.7)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105 56.05)
		(end 105 61.55)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 119.65 67.7)
		(end 121.95 67.7)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 128.55 67.7)
		(end 130.85 67.7)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "RING"
		(at 131.15 64.36 0)
		(layer "F.SilkS")
	)
	(gr_text "COMP 1"
		(at 157.76 64.31 0)
		(layer "B.SilkS")
	)
	(gr_text "COMP 2"
		(at 114.31 64.37 0)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch none 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105 56) (xy 104.95 61.5) (xy 122.35 78.25) (xy 143.4 78.15) (xy 161 61.5) (xy 161 60.5) (xy 161 56.05)
				(xy 105 56.05)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(locked yes)
		(layer "B.Cu")
		(hatch none 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105 56.05) (xy 161 56.05) (xy 161 61.5) (xy 140.5 81.45) (xy 140.55 87.2) (xy 137 90.7) (xy 128.95 90.7)
				(xy 125.1 87.15) (xy 125.15 81.45) (xy 104.95 61.5)
			)
		)
	)
	(embedded_fonts no)
)
