(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/GND")
	(net 2 "Net-(D1-K)")
	(net 3 "Net-(U2-VC)")
	(net 4 "Net-(C5-Pad2)")
	(net 5 "/SCLK")
	(net 6 "/SYNC_1")
	(net 7 "/SYNC")
	(net 8 "/SDI_1")
	(net 9 "/SDI")
	(net 10 "/SCLK_1")
	(net 11 "/SDO")
	(net 12 "unconnected-(A2-D0-Pad19)")
	(net 13 "unconnected-(A2-EN-Pad27)")
	(net 14 "unconnected-(A2-A0-Pad5)")
	(net 15 "unconnected-(A2-A4-Pad9)")
	(net 16 "unconnected-(A2-A3-Pad8)")
	(net 17 "unconnected-(A2-D5-Pad24)")
	(net 18 "unconnected-(A2-A2-Pad7)")
	(net 19 "unconnected-(A2-~{RESET}-Pad1)")
	(net 20 "unconnected-(A2-MISO-Pad13)")
	(net 21 "unconnected-(A2-A1-Pad6)")
	(net 22 "unconnected-(A2-VBAT-Pad28)")
	(net 23 "unconnected-(A2-D4-Pad23)")
	(net 24 "unconnected-(A2-USB-Pad26)")
	(net 25 "unconnected-(A2-SDA-Pad17)")
	(net 26 "unconnected-(A2-D3-Pad22)")
	(net 27 "/AVDD_3V3")
	(net 28 "unconnected-(A2-AREF-Pad3)")
	(net 29 "unconnected-(A2-SPARE-Pad16)")
	(net 30 "unconnected-(A2-TX-Pad15)")
	(net 31 "unconnected-(A2-D6-Pad25)")
	(net 32 "Net-(U2-FB)")
	(net 33 "unconnected-(U2-NFB-Pad6)")
	(net 34 "Net-(D1-A)")
	(net 35 "Net-(J3-Pin_1)")
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 174.9845 98.806)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at -2.3315 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small_US"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "Net-(U2-VC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 180.915 105.952)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 2.219 6.824 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small_US"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_PowerDI-5"
		(layer "F.Cu")
		(at 186.249 105.698 90)
		(descr "PowerDI,Diode,Vishay,https://www.diodes.com/assets/Package-Files/PowerDI5.pdf")
		(tags "PowerDI diode vishay")
		(property "Reference" "D1"
			(at 0.542 3.235 180)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky_AAK"
			(at 0 3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.12 0 270)
			(size 4.86 3.36)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.862 -0.92 270)
			(size 1.4 1.39)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.862 0.92 270)
			(size 1.4 1.39)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_PowerDI-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 195.139 101.1475 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0.1985 -1.965 180)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small_US"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 35 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 180.915 108.238)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0.441 4.538 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small_US"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 193.107 101.1475 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0.261252 2.099 180)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small_US"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 35 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Wurth_60312002114503_Vertical"
		(layer "F.Cu")
		(at 191.329 125.51)
		(descr "https://www.we-online.de/katalog/datasheet/60312002114503.pdf")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J2"
			(at 0 2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D1-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Wurth_60312002114503_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "control:DDPAK-7_R_LIT"
		(layer "F.Cu")
		(at 179.832 84.709)
		(tags "LT1370CR-TRPBF ")
		(property "Reference" "U2"
			(at -7.112 -7.747 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -7.112 -6.477 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -3.81 5.0165 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -3.81 5.0165 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.81 8.8011)
			(size 0.9398 2.286)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(U2-VC)")
			(pinfunction "VC")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.54 8.8011)
			(size 0.9398 2.286)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "Net-(U2-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -1.27 8.8011)
			(size 0.9398 2.286)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(J3-Pin_1)")
			(pinfunction "S/S")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0 8.8011)
			(size 0.9398 2.286)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 1.27 8.8011)
			(size 0.9398 2.286)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(D1-A)")
			(pinfunction "Vsw")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.54 8.8011)
			(size 0.9398 2.286)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(U2-NFB-Pad6)")
			(pinfunction "NFB")
			(pintype "input+no_connect")
		)
		(pad "7" smd rect
			(at 3.81 8.8011)
			(size 0.9398 2.286)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "Net-(J3-Pin_1)")
			(pinfunction "VIN")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 0 0)
			(size 9.4488 11.2522)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "control:SOIC8-N_MC_MCH"
		(layer "F.Cu")
		(at 175.581 106.714 90)
		(tags "MCP4162-103E/SN ")
		(property "Reference" "U3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at 0.034 -1.337 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.5748 -2.3749 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.5748 -2.3749 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.3622 -1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/SYNC")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.3622 -0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/SCLK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.3622 0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/SDI")
			(pinfunction "SDI")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.3622 1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/GND")
			(pinfunction "VSS")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 2.3622 1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/GND")
			(pinfunction "P0W")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.3622 0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "Net-(U2-FB)")
			(pinfunction "P0B")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.3622 -0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/SDO")
			(pinfunction "SDO")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 2.3622 -1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/AVDD_3V3")
			(pinfunction "VDD")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 182.455 99.348 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -2.711 -0.474 180)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(U2-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_APV_ANR5040"
		(layer "F.Cu")
		(at 189.043 98.078)
		(descr "Inductor, APV, ANR5040, 5.0x5.0x4.0mm, (http://en.apvind.com/public/upload/20240407/3375c395e460caa8519b4d637d9113ce.pdf), generated with kicad-footprint-generator gen_inductor.py")
		(tags "wirewound power shielded")
		(property "Reference" "L1"
			(at -0.067 -0.034 0)
			(layer "F.SilkS")
		)
		(property "Value" "L"
			(at 0 3.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.85 0)
			(size 1.4 4.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 34 "Net-(D1-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.85 0)
			(size 1.4 4.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 35 "Net-(J3-Pin_1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_APV_ANR5040.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 174.9845 96.774)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -2.3315 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small_US"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "Net-(U2-VC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:Adafruit_Feather"
		(layer "F.Cu")
		(at 147.765 84.695)
		(descr "Common footprint for the Adafruit Feather series of boards, https://learn.adafruit.com/adafruit-feather/feather-specification")
		(tags "Adafruit Feather")
		(property "Reference" "A2"
			(at 9.969 -3.923 0)
			(layer "F.SilkS")
		)
		(property "Value" "Adafruit_Feather_Generic"
			(at 10.435 42.63 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microcontroller module in various flavor, generic symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Adafruit*Feather*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(clearance 0.2)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 19.05 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 19 "unconnected-(A2-~{RESET}-Pad1)")
			(pinfunction "~{RESET}")
			(pintype "input+no_connect")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/AVDD_3V3")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(A2-AREF-Pad3)")
			(pinfunction "AREF")
			(pintype "input+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(A2-A0-Pad5)")
			(pinfunction "A0")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(A2-A1-Pad6)")
			(pinfunction "A1")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(A2-A2-Pad7)")
			(pinfunction "A2")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(A2-A3-Pad8)")
			(pinfunction "A3")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(A2-A4-Pad9)")
			(pinfunction "A4")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/SDI")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/SCLK_1")
			(pinfunction "SCK")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/SDI_1")
			(pinfunction "MOSI")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(A2-MISO-Pad13)")
			(pinfunction "MISO")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SYNC_1")
			(pinfunction "RX")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole oval
			(at 0 35.56)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(A2-TX-Pad15)")
			(pinfunction "TX")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" thru_hole oval
			(at 0 38.1)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(A2-SPARE-Pad16)")
			(pinfunction "SPARE")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" thru_hole oval
			(at 20.32 38.1 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(A2-SDA-Pad17)")
			(pinfunction "SDA")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" thru_hole oval
			(at 20.32 35.56 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/SCLK")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole oval
			(at 20.32 33.02 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(A2-D0-Pad19)")
			(pinfunction "D0")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" thru_hole oval
			(at 20.32 30.48 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/SDO")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 20.32 27.94 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SYNC")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 20.32 25.4 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(A2-D3-Pad22)")
			(pinfunction "D3")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" thru_hole oval
			(at 20.32 22.86 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(A2-D4-Pad23)")
			(pinfunction "D4")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole oval
			(at 20.32 20.32 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(A2-D5-Pad24)")
			(pinfunction "D5")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole oval
			(at 20.32 17.78 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(A2-D6-Pad25)")
			(pinfunction "D6")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" thru_hole oval
			(at 20.32 15.24 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(A2-USB-Pad26)")
			(pinfunction "USB")
			(pintype "power_in+no_connect")
		)
		(pad "27" thru_hole oval
			(at 20.32 12.7 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(A2-EN-Pad27)")
			(pinfunction "EN")
			(pintype "input+no_connect")
		)
		(pad "28" thru_hole oval
			(at 20.32 10.16 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(A2-VBAT-Pad28)")
			(pinfunction "VBAT")
			(pintype "power_in+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 182.455 97.316 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -2.711 -0.982 180)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(U2-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Wurth_60312002114503_Vertical"
		(layer "F.Cu")
		(at 191.329 80.806)
		(descr "https://www.we-online.de/katalog/datasheet/60312002114503.pdf")
		(tags "SMA THT Female Jack Vertical ExtendedLegs")
		(property "Reference" "J3"
			(at 0 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.05 2.05)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 -2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 2.25 2.25)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Wurth_60312002114503_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 180.915 103.666)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at -1.337 9.11 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small_US"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 175.022 100.91 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 2.302 0.072 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "control.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(C5-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "/GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 142.767 74.684)
		(end 199.496 131.945)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "FH09"
		(at 176.403 129.54 0)
		(layer "F.SilkS")
	)
	(gr_text "*"
		(at 177.803 99.8572 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.9)
		)
		(polygon
			(pts
				(xy 143.3 75.192) (xy 198.938 75.192) (xy 198.938 131.462) (xy 143.3 131.462)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 7.5)
		)
		(polygon
			(pts
				(xy 173.736 77.724) (xy 185.928 77.724) (xy 185.928 90.678) (xy 173.736 90.678)
			)
		)
	)
	(embedded_fonts no)
)
