(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Exports/")
		)
	)
	(net 0 "")
	(net 1 "Net-(D3-K)")
	(net 2 "/BAT")
	(net 3 "GND")
	(net 4 "/VBUS")
	(net 5 "/EN2")
	(net 6 "Net-(U2-VCC)")
	(net 7 "Net-(D1-A)")
	(net 8 "Net-(D1-K)")
	(net 9 "Net-(D2-A)")
	(net 10 "Net-(D2-K)")
	(net 11 "Net-(D3-A)")
	(net 12 "Net-(J1-CC2)")
	(net 13 "unconnected-(J1-DN2-PadB7)")
	(net 14 "unconnected-(J1-DP2-PadB6)")
	(net 15 "Net-(J1-CC1)")
	(net 16 "unconnected-(J1-DP1-PadA6)")
	(net 17 "unconnected-(J1-SBU1-PadA8)")
	(net 18 "unconnected-(J1-SBU2-PadB8)")
	(net 19 "unconnected-(J1-DN1-PadA7)")
	(net 20 "Net-(U1-TMR)")
	(net 21 "Net-(U1-ILIM)")
	(net 22 "Net-(U1-ISET)")
	(net 23 "Net-(U2-CS)")
	(net 24 "Net-(U3-FB)")
	(net 25 "/TS")
	(net 26 "unconnected-(U2-TD-Pad4)")
	(net 27 "Net-(U2-OD)")
	(net 28 "unconnected-(Q1-Pad1)")
	(net 29 "Net-(U2-OC)")
	(net 30 "Net-(Q2-D)")
	(net 31 "/P-")
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 152.15 91)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "GREEN"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/liteon/LTST-S270KGKT/386893"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6_Handsoldering"
		(layer "F.Cu")
		(at 139.9 87.7 180)
		(descr "6-pin SOT-23 package, Handsoldering")
		(tags "SOT-23-6 Handsoldering")
		(property "Reference" "U2"
			(at -0.45 -2.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "DW01A"
			(at 0 2.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://hmsemi.com/downfile/DW01A.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Overcharge, overcurrent and overdischarge protection IC for single cell lithium-ion/polymer battery"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.35 -0.95 180)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-OD)")
			(pinfunction "OD")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -1.35 0 180)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U2-CS)")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.35 0.95 180)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U2-OC)")
			(pinfunction "OC")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at 1.35 0.95 180)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "unconnected-(U2-TD-Pad4)")
			(pinfunction "TD")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 1.35 0 180)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-VCC)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 1.35 -0.95 180)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 152.15 92.75)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0.02125 1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "RED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/liteon/LTST-S270KRKT/386895"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1008_2520Metric_Pad1.43x2.20mm_HandSolder"
		(layer "F.Cu")
		(at 137.75 93.25 180)
		(descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
		(tags "inductor handsolder")
		(property "Reference" "L1"
			(at 3 -0.75 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uH"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1625 0 180)
			(size 1.425 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.175439)
			(net 2 "/BAT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1625 0 180)
			(size 1.425 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.175439)
			(net 11 "Net-(D3-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5_HandSoldering"
		(layer "F.Cu")
		(at 137.79 96.45)
		(descr "5-pin TSOT23 package, http://cds.linear.com/docs/en/packaging/SOT_5_05-08-1635.pdf")
		(tags "TSOT-23-5 Hand-soldering")
		(property "Reference" "U3"
			(at -2.29 2.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "MIC2295YD5-TR"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "MIC2295YD5-TR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT-23-5_D5_MCH TSOT-23-5_D5_MCH-M TSOT-23-5_D5_MCH-L")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.71 -0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D3-A)")
			(pinfunction "SW")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.71 0)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/P-")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.71 0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U3-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.71 0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(Q2-D)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.71 -0.95)
			(size 2 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BAT")
			(pinfunction "VIN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 141.75 96.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10A475KO8NNNC/3887442"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BAT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/P-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 158.65 92.4)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0.01 -1.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "OUT"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${NET_NAME(1)}"
			(at 0 2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 5 "/EN2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm_ThermalVias"
		(layer "F.Cu")
		(at 153.1875 98 180)
		(descr "VQFN, 16 Pin (http://www.ti.com/lit/ds/symlink/cdclvp1102.pdf#page=28), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "VQFN NoLead")
		(property "Reference" "U1"
			(at 0.6375 2.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "BQ24074RGT"
			(at 0 2.83 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24074.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB-Friendly Li-Ion Battery Charger and Power-Path Management, VQFN-16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VQFN*1EP*3x3mm*P0.5mm*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.4 -0.4 180)
			(size 0.69 0.69)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.4 0.4 180)
			(size 0.69 0.69)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.4 -0.4 180)
			(size 0.69 0.69)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.4 0.4 180)
			(size 0.69 0.69)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.4375 -0.75 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/TS")
			(pinfunction "TS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.4375 -0.25 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BAT")
			(pinfunction "BAT")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at -1.4375 0.25 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BAT")
			(pinfunction "BAT")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.4375 0.75 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -0.75 1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/EN2")
			(pinfunction "EN2")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -0.25 1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "EN1")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 0.25 1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D1-K)")
			(pinfunction "~{PGOOD}")
			(pintype "open_collector")
		)
		(pad "8" smd roundrect
			(at 0.75 1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 1.4375 0.75 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D2-K)")
			(pinfunction "~{CHG}")
			(pintype "open_collector")
		)
		(pad "10" smd roundrect
			(at 1.4375 0.25 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/EN2")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(pad "11" smd roundrect
			(at 1.4375 -0.25 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/EN2")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 1.4375 -0.75 180)
			(size 0.875 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-ILIM)")
			(pinfunction "ILIM")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 0.75 -1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/VBUS")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at 0.25 -1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-TMR)")
			(pinfunction "TMR")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -0.25 -1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "ITERM")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at -0.75 -1.4375 180)
			(size 0.25 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U1-ISET)")
			(pinfunction "ISET")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -0.5 -0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -0.5 0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 1.6 1.6)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "17" smd rect
			(at 0 0 180)
			(size 1.6 1.6)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "17" thru_hole circle
			(at 0.5 -0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0.5 0.5 180)
			(size 0.508 0.508)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/Downloaded/BQ24074RGTR/BQ24074RGTR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 149.5 92.45 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at -3 -1.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603FR-0710KL/726880"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BAT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(Q2-D)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 155.5 102.4)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0.7 -2.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "VBUS"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${NET_NAME(1)}"
			(at -0.6 2.3 45)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "/VBUS")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 143.56 84.52 30)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 2.23875 0.022372 120)
			(layer "F.SilkS")
		)
		(property "Value" "2kΩ"
			(at 0.000001 1.43 30)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB202V/1465861"
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 30)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.912501 0 30)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U2-CS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.912501 0 30)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/P-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 149.5 96.75 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 1.95 -1.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10B105KP8NNNC/3887604"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "F.Cu")
		(at 145.8 92.5875 180)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q2"
			(at 0.05 -2.9125 0)
			(layer "F.SilkS")
		)
		(property "Value" "Q_NMOS_GSD"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/diodes-incorporated/BSS138K-7-W/27803573"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-MOSFET transistor, gate/source/drain"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 -0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/VBUS")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 0.95 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/P-")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 180)
			(size 1.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(Q2-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6_Handsoldering"
		(layer "F.Cu")
		(at 139.62 82.86 -60)
		(descr "6-pin SOT-23 package, Handsoldering")
		(tags "SOT-23-6 Handsoldering")
		(property "Reference" "Q1"
			(at 0.806692 2.682769 120)
			(layer "F.SilkS")
		)
		(property "Value" "FS8205A"
			(at 0 2.9 120)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Fortune Semiconductor"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.2mm"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "Package"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/FS8205A/Fortune+Semiconductor/view-part/?ref=eda"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.7"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/FS8205A/Fortune+Semiconductor/view-part/?ref=snap"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "FS8205A"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" ""
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Fortune Semiconductor"
			(at 0 0 300)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 30)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.35 -0.95 300)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "unconnected-(Q1-Pad1)")
			(pintype "passive+no_connect")
		)
		(pad "2" smd roundrect
			(at -1.35 0 300)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.35 0.95 300)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.35 0.95 300)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-OD)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.35 0 300)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U2-OC)")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.35 -0.95 300)
			(size 1.56 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/P-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 155.65 92.75)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0.75 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "120Ω"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB121V/1465832"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/EN2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123F"
		(layer "F.Cu")
		(at 133.25 96.75 90)
		(descr "D_SOD-123F")
		(tags "D_SOD-123F")
		(property "Reference" "D3"
			(at 2.75 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/onsemi/SS24FL/5305066"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.127 -1.905 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.399999 0 90)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 1 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.399999 0 90)
			(size 1.1 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2272727273)
			(net 11 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123F.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 141.75 93 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -0.7 1.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10A475KO8NNNC/3887442"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BAT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 155.65 91)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at -1.25 -1.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "120Ω"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERA-3AEB121V/1465832"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/EN2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pads:4mm_by_4mm_pad"
		(layer "F.Cu")
		(at 138 102.75)
		(property "Reference" "9V4+"
			(at -3.7 -1.4 315)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "9V"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "9V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0)
			(size 4 4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 1 "Net-(D3-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 144.35 89.4)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.648 0)
			(layer "F.SilkS")
		)
		(property "Value" "BST EN"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "BST_EN"
			(at -1 1.9 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "Net-(Q2-D)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 151.7 101.95 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 2.7 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "51k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603FR-0751KL/727282"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U1-TMR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 133.25 92.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at -1 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "28k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603FR-0728KL/727108"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U3-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 134.79 88 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "470Ω"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603JR-07470RL/726791"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BAT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-VCC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 153.4 102.05 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 2.6 0.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "590Ω"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603FR-07590RL/727314"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U1-ISET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 138.25 99.5)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at -2.65 0.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL21B106KOQNNNE/3888530"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 31 "/P-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pads:3mm_by_4mm_pad"
		(layer "F.Cu")
		(at 147.5 88 90)
		(property "Reference" "BT-"
			(at 2.8 -1.55 45)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BATT-"
			(at 0 3.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 135)
			(size 3 4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 3 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 143.2 82)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 1.45 -0.75 300)
			(layer "F.SilkS")
		)
		(property "Value" "P+ & BATT+"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${NET_NAME(1)}"
			(at -0.4 -1.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 31 "/P-")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 136.54 88 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -2.1 -0.26 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/kemet/C0603C104K5RACTU/1465594"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U2-VCC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 157.2 95.6)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at -0.1 1.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/samsung-electro-mechanics/CL10A475KO8NNNC/3887442"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/EN2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "USB4105_GF_A:GCT_USB4105-GF-A"
		(layer "F.Cu")
		(at 145.5 104.5)
		(property "Reference" "J1"
			(at 0 -1.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "USB4105-GF-A"
			(at 5.16 -7.135 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "B4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.31 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "GCT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "PCB EDGE"
			(at 5.4 2.5 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -3.68)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -3.68)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1_B12" smd rect
			(at -3.2 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A4_B9" smd rect
			(at -2.4 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 4 "/VBUS")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "A5" smd rect
			(at -1.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 15 "Net-(J1-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 16 "unconnected-(J1-DP1-PadA6)")
			(pinfunction "DP1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A7" smd rect
			(at 0.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 19 "unconnected-(J1-DN1-PadA7)")
			(pinfunction "DN1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A8" smd rect
			(at 1.25 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 17 "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
		)
		(pad "B1_A12" smd rect
			(at 3.2 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 3 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
		)
		(pad "B4_A9" smd rect
			(at 2.4 -4.755)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 4 "/VBUS")
			(pinfunction "VBUS__1")
			(pintype "power_in")
		)
		(pad "B5" smd rect
			(at 1.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 12 "Net-(J1-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 14 "unconnected-(J1-DP2-PadB6)")
			(pinfunction "DP2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B7" smd rect
			(at -0.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 13 "unconnected-(J1-DN2-PadB7)")
			(pinfunction "DN2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B8" smd rect
			(at -1.75 -4.755)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 18 "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
		)
		(pad "SH1" thru_hole oval
			(at -4.32 -4.18)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "SHELL_GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH2" thru_hole oval
			(at 4.32 -4.18)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "SHELL_GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH3" thru_hole oval
			(at -4.32 0)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "SHELL_GND__2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH4" thru_hole oval
			(at 4.32 0)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "SHELL_GND__3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Downloaded/USB4105_GF_A/USB4105-GF-A.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 137.75 91)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at -2.75 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.3k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/panasonic-electronic-components/ERJ-3EKF4301V/1746409"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U3-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/P-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 157.75 100.25 60)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at -1.544615 -1.475352 150)
			(layer "F.SilkS")
		)
		(property "Value" "1.1kΩ"
			(at 0.000001 1.429999 60)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/vishay-dale/CRCW06031K10FKEAC/7924830"
			(at 0 0 60)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 60)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 60)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 60)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-ILIM)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 60)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "pads:4mm_by_4mm_pad"
		(layer "B.Cu")
		(at 145.75 91.75)
		(property "Reference" "BT+1"
			(at 0 -2.95 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "BATT+"
			(at 0 -1 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0)
			(size 4 4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net 2 "/BAT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 143.75 102.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603FR-0710KL/726880"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(J1-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 142.7 81.7 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 147.4 97 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "TH1"
			(at -1.75 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -4.92 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~https://www.semitec-global.com/uploads/2022/01/P12-13-AT-Thermistor.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Temperature dependent resistor, negative temperature coefficient"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*NTC* *Thermistor* PIN?ARRAY* bornier* *Terminal?Block* R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/TS")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "B.Cu")
		(at 147.25 102.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.digikey.com/en/products/detail/yageo/RC0603FR-0710KL/726880"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "flashlight adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J1-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 135.6 93.3 135)
		(property "Reference" "G***"
			(at 0 0 135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 135)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_arc
		(start 136.01 84.11)
		(mid 136.206465 85.48806)
		(end 134.834324 85.72232)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 134.67 83.06)
		(mid 139.293967 79.797167)
		(end 144.796313 78.473781)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.01 84.11)
		(end 134.67 83.06)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 139.730425 107.398976)
		(mid 131.006492 97.546067)
		(end 133.37 84.6)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 160.248489 90.483086)
		(mid 158.800426 100.551123)
		(end 151.280111 107.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.833246 85.723887)
		(end 133.37 84.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 151.280111 107.4)
		(end 139.730425 107.398975)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 160.248481 90.483086)
		(mid 150.512821 87.059539)
		(end 144.796022 78.467568)
		(layer "Edge.Cuts")
	)
	(gr_text "9V li-ion flashlight Adapter V1\nMade with <3 by\nSiwen Long"
		(at 138.7 104.8 315)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "Net-(D3-K)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 132.6 92.1) (xy 128.8 92.5) (xy 130.1 105.5) (xy 136.6 104.5) (xy 139.8 101.2) (xy 138.2 100.2)
				(xy 137.7 98.9) (xy 133.6 97.8) (xy 132.7 96.2)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/BAT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.25 97.5) (xy 138.5 97.75) (xy 140.5 97.75) (xy 142.5 97.75) (xy 142.5 96.25) (xy 142.5 95)
				(xy 142.5 92.25) (xy 138 92)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/EN2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 156 90.8) (xy 156 93.1) (xy 153.6 95.1) (xy 153.6 95.8) (xy 156.1 96) (xy 156.7 96) (xy 159.3 92.6)
				(xy 156.7 90.6)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(D3-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137 95.8) (xy 137.3 92.2) (xy 135.1 92.2) (xy 132.8 95.2) (xy 132.8 95.8)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.75 77.5) (xy 126.25 78.5) (xy 125.75 113.25) (xy 172.75 110.25) (xy 169 78.25)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/BAT")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.1 94.7) (xy 154.5 94.6) (xy 151.567732 91.75) (xy 143.8 91.75) (xy 143.7 93.1) (xy 140.2 93.05)
				(xy 140.15 94.7) (xy 141.15 94.7)
			)
		)
	)
	(embedded_fonts no)
)
