(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-K)")
  (net 2 "Net-(D2-K)")
  (net 3 "Net-(D1-A)")
  (net 4 "Net-(D3-K)")
  (net 5 "Net-(D4-K)")
  (net 6 "Net-(C1-Pad2)")
  (net 7 "Net-(D5-K)")
  (net 8 "Net-(D6-K)")
  (net 9 "Net-(D7-K)")
  (net 10 "Net-(D8-K)")
  (net 11 "Net-(P6-P1)")
  (net 12 "Net-(P7-P1)")
  (net 13 "Net-(P1-P1)")
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 149.92 79.756)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 3.496 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 149.92 54.864)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 3.75 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D2-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 134.74 79.756)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 3.944 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D3-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 134.74 54.864)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C4" (at 3.944 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D4-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D2-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 119.56 79.756)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C5" (at 3.75 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D5-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D3-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 119.56 54.864)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C6" (at 3.75 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D6-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D4-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 104.38 79.756)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at 3.75 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D7-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D5-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D14.5mm_W5.0mm_P7.50mm" (layer "F.Cu")
    (at 104.38 54.864)
    (descr "C, Disc series, Radial, pin pitch=7.50mm, , diameter*width=14.5*5.0mm^2, Capacitor, http://www.vishay.com/docs/28535/vy2series.pdf")
    (tags "C Disc series Radial pin pitch 7.50mm  diameter 14.5mm width 5.0mm Capacitor")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at 3.316 0) (layer "F.SilkS"))
    (fp_text value "0.01uf" (at 3.75 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.75 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D8-K)") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.5 0) (size 2 2) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D6-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D14.5mm_W5.0mm_P7.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 157.286 73.66 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D1" (at 6.604 0.194 180) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 149.738568 60.96 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D2" (at 6.604 0.132568) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D2-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(D1-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 142.19114 73.66 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D3" (at 6.604 0.04886 180) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D2-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 134.643712 60.96 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D4" (at 6.604 0.023712) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(D3-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 127.096284 73.66 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D5" (at 6.604 -0.096284 180) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D4-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 119.548856 60.96 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D6" (at 6.604 0.168856) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D6-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D5-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 112.001428 73.66 90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D7" (at 6.35 0.012572 180) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.74 0 90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D7-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 90) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D6-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-41_SOD81_P12.70mm_Horizontal" (layer "F.Cu")
    (at 104.454 60.96 -90)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=12.7mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 12.7mm  length 5.2mm diameter 2.7mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr through_hole)
    (fp_text reference "D8" (at 6.858 0.06) (layer "F.SilkS"))
    (fp_text value "D" (at 6.35 2.47 -90) (layer "F.Fab"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.SilkS"))
    (fp_text user "K" (at 0 -2.1 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.74 0 -90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D8-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 12.7 0 270) (size 2.2 2.2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D7-K)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-41_SOD81_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm" (layer "F.Cu")
    (at 109.328 89.408)
    (descr "Soldered wire connection, for a single 0.1 mm² wire, basic insulation, conductor diameter 0.4mm, outer diameter 1mm, size source Multi-Contact FLEXI-E 0.1 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.1sqmm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P1" (at -3.664 -0.254) (layer "F.SilkS"))
    (fp_text value "IN" (at -0.362 3.048) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4 4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(P1-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.1sqmm_1x01_D0.4mm_OD1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 151.384 89.154)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P2" (at 3.556 0.254) (layer "F.SilkS"))
    (fp_text value "GND" (at 0 3.556) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4 4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-A)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 157.48 47.244 90)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P3" (at 0 -4.064 180) (layer "F.SilkS"))
    (fp_text value "GND" (at -1.524 -4.318 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4 4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-A)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 142.24 47.244 90)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P4" (at 0 -4.064 180) (layer "F.SilkS"))
    (fp_text value "Treble" (at -1.524 -4.826 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4 4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(D2-K)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 104.648 47.244 90)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P5" (at 0 4.064 180) (layer "F.SilkS"))
    (fp_text value "Bass" (at -1.524 4.826 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4 4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D8-K)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 127 87.63 180)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 6.096 -0.254 180) (layer "F.SilkS"))
    (fp_text value "330K" (at 6.35 2.72 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.35 0 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.54 2.54) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 12.7 0 180) (size 2.54 2.54) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(P1-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal" (layer "F.Cu")
    (at 133.35 87.63)
    (descr "Resistor, Axial_DIN0309 series, Axial, Horizontal, pin pitch=12.7mm, 0.5W = 1/2W, length*diameter=9*3.2mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0309 series Axial Horizontal pin pitch 12.7mm 0.5W = 1/2W length 9mm diameter 3.2mm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 6.35 0.254) (layer "F.SilkS"))
    (fp_text value "2.2M" (at 6.35 -2.794) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.54 2.54) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole circle (at 12.7 0) (size 2.54 2.54) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(D1-A)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0309_L9.0mm_D3.2mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "sdsLogos:sdsLabs-large-fSilk" (layer "F.Cu")
    (at 124.206 47.244)
    (attr through_hole)
    (fp_text reference "G***" (at 0 -7.62) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0 -5.08) (layer "F.SilkS") hide)
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 147.574 105.156 90)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P7" (at 0 3.556 180) (layer "F.SilkS"))
    (fp_text value "AC" (at -3.302 0.254 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4 4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(P7-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Wire:SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm" (layer "F.Cu")
    (at 113.538 105.156 90)
    (descr "Soldered wire connection, for a single 0.5 mm² wire, basic insulation, conductor diameter 0.9mm, outer diameter 2.1mm, size source Multi-Contact FLEXI-E 0.5 (https://ec.staubli.com/AcroFiles/Catalogues/TM_Cab-Main-11014119_(en)_hi.pdf), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
    (tags "connector wire 0.5sqmm")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "P6" (at 0 -3.556 180) (layer "F.SilkS"))
    (fp_text value "AC" (at -3.556 -0.254 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4 4) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(P6-P1)") (pinfunction "P1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.5sqmm_1x01_D0.9mm_OD2.1mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuseholder_Clip-5x20mm_Keystone_3512P_Inline_P23.62x7.27mm_D1.02x2.41x1.02x1.57mm_Horizontal" (layer "F.Cu")
    (at 118.46 105.156)
    (descr "Fuseholder Clips, 5x20mm Cylinder Fuse, Pins Inline, Horizontal, Keystone 3512P, http://www.keyelco.com/product-pdf.cfm?p=1386")
    (tags "fuse clip open")
    (property "Sheetfile" "/Users/stokes/Audio folder/Circuit Boards/Quad57-Rectifier-v2.0/Quad57-Rectifier-v2.0.sch")
    (property "Sheetname" "")
    (property "ki_description" "Fuse")
    (property "ki_keywords" "fuse")
    (attr through_hole)
    (fp_text reference "F1" (at 11.81 0) (layer "F.SilkS"))
    (fp_text value "100mA" (at 11.555 4.5) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 11.81 0) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0) (size 2 3.7) (drill oval 1.02 2.71) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(P6-P1)") (pintype "passive"))
    (pad "1" thru_hole roundrect (at 7.27 0) (size 2 2.8) (drill oval 1.02 1.87) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(P6-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 16.35 0) (size 2 2.8) (drill oval 1.02 1.87) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(P7-P1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 23.62 0) (size 2 3.7) (drill oval 1.02 2.71) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(P7-P1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Clip-5x20mm_Keystone_3512P_Inline_P23.62x7.27mm_D1.02x2.41x1.02x1.57mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 98.806 112.014) (end 162.306 112.014)
    (layer "Edge.Cuts"))
  (gr_circle (center 158.496 98.044) (end 160.041022 98.044)
    (fill none) (layer "Edge.Cuts"))
  (gr_circle (center 102.616 98.044) (end 104.161022 98.044)
    (fill none) (layer "Edge.Cuts"))
  (gr_line (start 98.806 42.164) (end 162.306 42.164)
    (layer "Edge.Cuts"))
  (gr_line (start 162.306 112.014) (end 162.306 42.164)
    (layer "Edge.Cuts"))
  (gr_line (start 98.806 42.164) (end 98.806 112.014)
    (layer "Edge.Cuts"))
  (gr_text "Quad ESL Rectifier" (at 129.794 98.044) (layer "F.SilkS"))
  (gr_text "GP02-30" (at 154.492 67.31 90) (layer "F.SilkS"))
  (gr_text "IN" (at 109.22 90.424) (layer "F.SilkS"))
  (gr_text "IN" (at 151.384 89.916) (layer "F.SilkS"))
)
