(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A1")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 207.5 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 332.5 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 207.5 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 520 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 82.5 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 145 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 395 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 332.5 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 145 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 270 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 395 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 270 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 457.5 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 457.5 135)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 520 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(footprint "probeHoles:MountingHole_1.2mm"
		(locked yes)
		(layer "F.Cu")
		(at 82.5 142.5)
		(descr "Mounting Hole 2.1mm, no annular")
		(tags "mounting hole 2.1mm no annular")
		(property "Reference" ""
			(at 0 -3.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_1.2mm"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "probeHoles:MountingHole_1.2mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.1 2.1)
			(drill 1.3)
			(layers "F.Cu" "B.Mask")
			(solder_mask_margin 10)
			(clearance 1.1)
		)
	)
	(gr_rect
		(start 22 90)
		(end 580.5 180)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "TM010 Impedance bandwidth sim: 2.384 GHz - 2.440 GHz\n					  Measured: "
		(at 579.475 100.025 0)
		(layer "B.SilkS")
	)
	(gr_text "TM020 Impedance bandwidth sim: 4.748 GHz - 4.874 GHz\n					  Measured: "
		(at 407.15 100.3 0)
		(layer "B.SilkS")
	)
	(gr_text "Designed by Samuel Robbins, Dec 2025"
		(at 22.9 93.75 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 188.5 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 313.5 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 376 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "TM010 Mode"
		(at 227.225 125.05 -90)
		(layer "F.SilkS")
	)
	(gr_text "E-plane TM020\nradiation pattern"
		(at 275.3 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "Elements are spaced at .5λ for 2.4 GHZ"
		(at 23.175 178.575 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 438.5 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 251 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "2\n"
		(at 126 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 501 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "Huff Research Group"
		(at 262.225 175.775 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 63.5 148.875 0)
		(layer "F.SilkS")
	)
	(gr_text "TM020 Mode"
		(at 289.925 126.95 270)
		(layer "F.SilkS")
	)
	(gr_text "E-plane TM010\nradiation pattern"
		(at 211.475 95.15 0)
		(layer "F.SilkS")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 145 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 82.5 135 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 395 135 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 457.5 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 332.5 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 520 135 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 520 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 207.5 135 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 82.5 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 457.5 135 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 270 135 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 145 135 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 207.5 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 395 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 270 142.5 0)
		(layer "F.Fab")
	)
	(gr_text "${REFERENCE}"
		(locked yes)
		(at 332.5 135 0)
		(layer "F.Fab")
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 82.5 148.875) (xy 145 148.875)
		)
		(height 6.525)
		(gr_text "62.5000 mm"
			(at 113.75 154.3 0)
			(layer "F.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 63.5 148.875) (xy 63.5 121.125)
		)
		(height -3.2)
		(gr_text "27.75 mm"
			(at 59.2 135 90)
			(layer "F.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 82.5 135) (xy 82.5 142.5)
		)
		(height 5.35)
		(gr_text "7.5000 mm"
			(at 76.05 138.75 90)
			(layer "F.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "F.SilkS")
		(pts
			(xy 63.5 121.125) (xy 101.5 121.125)
		)
		(height -3.625)
		(gr_text "38.00 mm"
			(at 82.5 116.4 0)
			(layer "F.SilkS")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 2)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 22 180) (xy 580.5 180) (xy 580.5 90) (xy 22 90)
			)
		)
	)
)