(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "A2DVI.v2.4")
	)
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 128.143 114.03205)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "A2DVI.v2.4-gerbers")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "3.3V")
	(net 3 "VSYS")
	(net 4 "5V")
	(net 5 "PHI0")
	(net 6 "RW")
	(net 7 "DevSel")
	(net 8 "D0")
	(net 9 "D1")
	(net 10 "D2")
	(net 11 "D3")
	(net 12 "D4")
	(net 13 "D5")
	(net 14 "D6")
	(net 15 "D7")
	(net 16 "A8")
	(net 17 "A9")
	(net 18 "A15")
	(net 19 "A14")
	(net 20 "A10")
	(net 21 "A11")
	(net 22 "A12")
	(net 23 "A13")
	(net 24 "A0")
	(net 25 "A1")
	(net 26 "A2")
	(net 27 "A3")
	(net 28 "A4")
	(net 29 "A5")
	(net 30 "A6")
	(net 31 "A7")
	(net 32 "DATAOE")
	(net 33 "LSBOE")
	(net 34 "MSBOE")
	(net 35 "L-PHI0")
	(net 36 "L-RW")
	(net 37 "D2_N")
	(net 38 "D2_P")
	(net 39 "D1_P")
	(net 40 "D1_N")
	(net 41 "D0_P")
	(net 42 "D0_N")
	(net 43 "CK_P")
	(net 44 "CK_N")
	(net 45 "SYNC")
	(net 46 "L-DevSel")
	(net 47 "AD0")
	(net 48 "AD1")
	(net 49 "AD2")
	(net 50 "AD3")
	(net 51 "AD4")
	(net 52 "AD5")
	(net 53 "AD6")
	(net 54 "AD7")
	(net 55 "IOSel")
	(net 56 "AltChr")
	(net 57 "5Vout")
	(net 58 "L-AltChr")
	(footprint "Package_DIP:DIP-20_W7.62mm_Socket"
		(layer "F.Cu")
		(at 140.081 125.97005 -90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U2"
			(at -0.8382 25.5778 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC244"
			(at 3.8 11.425 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "LSBOE")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "A7")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "AD6")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "A5")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "AD4")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "A3")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "AD2")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "A1")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "AD0")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "A0")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "AD1")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "A2")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "AD3")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "A4")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "AD5")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "A6")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "AD7")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "LSBOE")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 119.761 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "3" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 25 "A1")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 132.461 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "43" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 14 "D6")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.001 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "9" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 31 "A7")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 145.161 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "38" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 140.081 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "40" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 5 "PHI0")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 106.15805 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R8"
			(at 6.9342 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "D1_N")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "D1_N")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 129.921 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "7" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 29 "A5")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 110.998 145.14705 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R4"
			(at 6.604 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "AltChr")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 113.06685 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R11"
			(at 7.366 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "CK_P")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "CK_P")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RaspberryPI PicoW:RPi_PicoW_SMD_TH"
		(layer "F.Cu")
		(at 94.53955 109.66325 90)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "U1"
			(at -12.43205 -24.638 180)
			(layer "F.SilkS")
		)
		(property "Value" "Pico"
			(at -0.127 0.127 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "pico_vga_sd_aud.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -8.89 -24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "AD0")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "1" smd rect
			(at -8.89 -24.13 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 47 "AD0")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at -8.89 -21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "AD1")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -8.89 -21.59 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 48 "AD1")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole rect
			(at -8.89 -19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -8.89 -19.05 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at -8.89 -16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "AD2")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -8.89 -16.51 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 49 "AD2")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole oval
			(at -8.89 -13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "AD3")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -8.89 -13.97 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 50 "AD3")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at -8.89 -11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "AD4")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -8.89 -11.43 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 51 "AD4")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at -8.89 -8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "AD5")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.89 -8.89 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 52 "AD5")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole rect
			(at -8.89 -6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at -8.89 -6.35 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" thru_hole oval
			(at -8.89 -3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "AD6")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -8.89 -3.81 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 53 "AD6")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole oval
			(at -8.89 -1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "AD7")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -8.89 -1.27 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 54 "AD7")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole oval
			(at -8.89 1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "L-DevSel")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -8.89 1.27 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 46 "L-DevSel")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" thru_hole oval
			(at -8.89 3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "L-RW")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -8.89 3.81 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 36 "L-RW")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole rect
			(at -8.89 6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -8.89 6.35 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at -8.89 8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "L-AltChr")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -8.89 8.89 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 58 "L-AltChr")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole oval
			(at -8.89 11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "DATAOE")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -8.89 11.43 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 32 "DATAOE")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at -8.89 13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "LSBOE")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -8.89 13.97 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 33 "LSBOE")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at -8.89 16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "MSBOE")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -8.89 16.51 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 34 "MSBOE")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole rect
			(at -8.89 19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at -8.89 19.05 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" thru_hole oval
			(at -8.89 21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "CK_P")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at -8.89 21.59 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 43 "CK_P")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at -8.89 24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "CK_N")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -8.89 24.13 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 44 "CK_N")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 8.89 24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "D2_P")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 8.89 24.13 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 38 "D2_P")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 8.89 21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "D2_N")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 8.89 21.59 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 37 "D2_N")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole rect
			(at 8.89 19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" smd rect
			(at 8.89 19.05 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "24" thru_hole oval
			(at 8.89 16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "D1_P")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 8.89 16.51 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 39 "D1_P")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 8.89 13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "D1_N")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 8.89 13.97 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 40 "D1_N")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole oval
			(at 8.89 11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "D0_P")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 8.89 11.43 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 41 "D0_P")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole oval
			(at 8.89 8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "D0_N")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 8.89 8.89 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 42 "D0_N")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "28" thru_hole rect
			(at 8.89 6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "28" smd rect
			(at 8.89 6.35 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" thru_hole oval
			(at 8.89 3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at 8.89 3.81 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "30" thru_hole oval
			(at 8.89 1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "30" smd rect
			(at 8.89 1.27 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "31" thru_hole oval
			(at 8.89 -1.27 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "L-PHI0")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 8.89 -1.27 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 35 "L-PHI0")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole oval
			(at 8.89 -3.81 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 8.89 -3.81 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "33" thru_hole rect
			(at 8.89 -6.35 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "33" smd rect
			(at 8.89 -6.35 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "34" thru_hole oval
			(at 8.89 -8.89 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 8.89 -8.89 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole oval
			(at 8.89 -11.43 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "ADC_VREF")
			(pintype "unspecified+no_connect")
		)
		(pad "35" smd rect
			(at 8.89 -11.43 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(pinfunction "ADC_VREF")
			(pintype "unspecified+no_connect")
		)
		(pad "36" thru_hole oval
			(at 8.89 -13.97 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
			(pinfunction "3V3")
			(pintype "unspecified")
		)
		(pad "36" smd rect
			(at 8.89 -13.97 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "3.3V")
			(pinfunction "3V3")
			(pintype "unspecified")
		)
		(pad "37" thru_hole oval
			(at 8.89 -16.51 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "3V3_EN")
			(pintype "input+no_connect")
		)
		(pad "37" smd rect
			(at 8.89 -16.51 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(pinfunction "3V3_EN")
			(pintype "input+no_connect")
		)
		(pad "38" thru_hole rect
			(at 8.89 -19.05 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 8.89 -19.05 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
		)
		(pad "39" thru_hole oval
			(at 8.89 -21.59 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VSYS")
			(pinfunction "VSYS")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at 8.89 -21.59 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 3 "VSYS")
			(pinfunction "VSYS")
			(pintype "unspecified")
		)
		(pad "40" thru_hole oval
			(at 8.89 -24.13 90)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "VBUS")
			(pintype "unspecified")
		)
		(pad "40" smd rect
			(at 8.89 -24.13 90)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(pinfunction "VBUS")
			(pintype "unspecified")
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 171.323 143.77545 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C5"
			(at 6.604 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 168.021 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "29" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 174.498 138.79705 -90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C1"
			(at -1.651 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.627 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "5V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 171.323 133.59005 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C3"
			(at 6.691 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.627 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 155.321 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "34" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm_Socket"
		(layer "F.Cu")
		(at 168.021 137.40005 -90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U5"
			(at -0.762 25.395 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC244"
			(at 3.546 11.933 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "MSBOE")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "A10")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "AD1")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "A8")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "AD7")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "A14")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "AD5")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "A12")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "AD3")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "A11")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "AD4")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "A13")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "AD6")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "A15")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "AD0")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "A9")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "AD2")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "MSBOE")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 114.681 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 55 "IOSel")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 175.641 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "25" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 4 "5V")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 132.461 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "8" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 30 "A6")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 152.781 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "35" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 137.541 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "10" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 16 "A8")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 168.021 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "22" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 165.481 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "30" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 103.99905 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R7"
			(at 6.9342 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "D1_P")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "D1_P")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 157.861 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "18" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 6 "RW")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 115.22585 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R12"
			(at 7.3914 -0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "CK_N")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "CK_N")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 119.761 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "48" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 9 "D1")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 147.701 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "37" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 173.101 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "27" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 123.103 118.73105)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C6"
			(at -1.905 0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.627 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "5Vout")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 147.701 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "14" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 22 "A12")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 129.921 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "44" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 13 "D5")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 134.0104 99.07145)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "H1"
			(at 5.1308 0.0254 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_2x10_P2.54mm_Vertical"
			(at 1.27 25.19 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "D2_P")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "D2_N")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "D1_P")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "D1_N")
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "D0_P")
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "D0_N")
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "CK_P")
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "CK_N")
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "5Vout")
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.621 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "12" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 20 "A10")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 122.301 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "4" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 26 "A2")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 117.221 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "2" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 24 "A0")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 110.73005 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R10"
			(at 7.4168 -0.0762 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "D0_N")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "D0_N")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 99.37625 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R5"
			(at 6.9342 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "D2_P")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "D2_P")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 165.481 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "21" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 162.941 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "31" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 124.841 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "46" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 11 "D3")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 108.458 128.51005 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at -1.524 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "LSBOE")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 173.101 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "24" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 177.292 139.94005 90)
		(descr "Diode, DO-34_SOD68 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=3.04*1.6mm^2, , https://www.nxp.com/docs/en/data-sheet/KTY83_SER.pdf")
		(tags "Diode DO-34_SOD68 series Axial Horizontal pin pitch 7.62mm  length 3.04mm diameter 1.6mm")
		(property "Reference" "D1"
			(at -1.9 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_DO-34_SOD68_P7.62mm_Horizontal"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_THT:D_DO-34_SOD68_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.038 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VSYS")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "5V")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-34_SOD68_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 114.046 133.59005 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C2"
			(at 6.604 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.627 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm_Socket"
		(layer "F.Cu")
		(at 140.081 137.40005 -90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U4"
			(at -0.635 25.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC244"
			(at 3.556 11.684 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "DATAOE")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "D7")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "AD6")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "D5")
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "AD4")
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "D3")
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "AD2")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "D1")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "AD0")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "D0")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "AD1")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "D2")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "AD3")
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "D4")
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "AD5")
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "D6")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "AD7")
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "DATAOE")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 122.301 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "47" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 10 "D2")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 127.381 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "6" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 28 "A4")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 160.401 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "32" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 108.57105 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R9"
			(at 6.9342 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "D0_P")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "D0_P")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 150.241 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "36" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 108.458 145.14705 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R2"
			(at 6.604 -0.381 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "DATAOE")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 137.541 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "41" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 7 "DevSel")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 127.381 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "45" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 12 "D4")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.621 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "39" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 140.081 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "11" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 17 "A9")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 150.241 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "15" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 23 "A13")
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 114.046 145.02005 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "C4"
			(at 6.604 -0.127 0)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 110.998 128.51005 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R3"
			(at -1.524 -0.127 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.54 0 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "MSBOE")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 145.161 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "13" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 21 "A11")
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.5146 101.53525 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R6"
			(at 6.9342 -0.0508 180)
			(layer "F.SilkS")
		)
		(property "Value" "270"
			(at 2.54 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "D2_N")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "D2_N")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 114.681 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "50" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Package_DIP:DIP-20_W7.62mm_Socket"
		(layer "F.Cu")
		(at 168.021 125.97005 -90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "U3"
			(at -0.762 25.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC244"
			(at 3.546 11.933 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 8.89 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "3" thru_hole oval
			(at 0 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "L-RW")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "5" thru_hole oval
			(at 0 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "6" thru_hole oval
			(at 0 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "7" thru_hole oval
			(at 0 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "L-AltChr")
		)
		(pad "8" thru_hole oval
			(at 0 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "PHI0")
		)
		(pad "9" thru_hole oval
			(at 0 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "L-DevSel")
		)
		(pad "10" thru_hole oval
			(at 0 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "11" thru_hole oval
			(at 7.62 22.86 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "DevSel")
		)
		(pad "12" thru_hole oval
			(at 7.62 20.32 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "L-PHI0")
		)
		(pad "13" thru_hole oval
			(at 7.62 17.78 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "AltChr")
		)
		(pad "14" thru_hole oval
			(at 7.62 15.24 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole oval
			(at 7.62 12.7 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole oval
			(at 7.62 10.16 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole oval
			(at 7.62 7.62 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "RW")
		)
		(pad "18" thru_hole oval
			(at 7.62 5.08 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "19" thru_hole oval
			(at 7.62 2.54 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "20" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "3.3V")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 170.561 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "23" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 160.401 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "19" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 45 "SYNC")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 124.841 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "5" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 27 "A3")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 152.781 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "16" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 19 "A14")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 175.641 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "26" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 155.321 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "17" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
			(net 18 "A15")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 162.941 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "20" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 157.861 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "33" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.001 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "42" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 15 "D7")
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 170.561 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "28" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
		)
	)
	(footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 174.498 133.59005 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
		(property "Reference" "Fu1"
			(at 6.731 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100mA"
			(at 2.5 0.127 90)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "5V")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "5Vout")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 117.221 150.98905)
		(property "Reference" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "49" connect rect
			(at 0 0)
			(size 1.524 6.35)
			(layers "B.Cu" "B.Mask")
			(net 8 "D0")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 93.021 140.82905 180)
		(descr "Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x01 2.54mm single row")
		(property "Reference" "H2"
			(at -0.07 -2.52605 180)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_1x01_P2.54mm_Horizontal"
			(at 4.385 2.27 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "AltChr")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo2_7.3x6mm_SilkScreen"
		(layer "B.Cu")
		(at 144.0688 111.54285 180)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo2_7.3x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_line
		(start 112.395 154.03705)
		(end 112.395 146.925)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.927 154.03705)
		(end 177.927 146.925)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.927 154.03705)
		(end 177.673 154.29105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.4924 122.7951)
		(end 180.4924 146.92505)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.8848 97.26805)
		(end 68.8848 146.925)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.649 154.280243)
		(end 112.395 154.03705)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.395 146.925)
		(end 68.8848 146.925)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 112.649 154.280243)
		(end 177.673 154.29105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.4924 146.92505)
		(end 177.927 146.925)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.4924 122.7951)
		(end 153.162 122.79505)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.162 97.26805)
		(end 68.8848 97.26805)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 153.162 97.26805)
		(end 153.162 122.79505)
		(layer "Edge.Cuts")
	)
	(gr_text "A2DVI"
		(at 97.1804 135.085788 0)
		(layer "B.SilkS")
	)
	(gr_text "KIT"
		(at 84.328 134.86005 0)
		(layer "B.SilkS")
	)
	(gr_text "ALTCHR"
		(at 83.115 143.87705 0)
		(layer "F.SilkS")
	)
	(gr_text ""
		(at 152.781 153.328713 0)
		(layer "F.SilkS")
	)
	(gr_text "A2DVI.v2.4 (c) 2024 by Ralle Palaveev, https://apple2.co.uk/"
		(at 144.907 147.05205 0)
		(layer "F.SilkS")
	)
	(gr_text "RPI Pico"
		(at 90.7034 109.96805 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 132.207 99.90965 90)
		(layer "F.SilkS")
	)
	(gr_text "A2DVI"
		(at 80.6196 134.958788 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 132.1816 123.02365 90)
		(layer "F.SilkS")
	)
	(gr_text "KIT"
		(at 93.472 134.86005 0)
		(layer "F.SilkS")
	)
	(gr_text "HDMI break-out board"
		(at 145.2626 119.03585 90)
		(layer "F.SilkS")
	)
	(gr_text ""
		(at 152.781 153.328713 0)
		(layer "F.SilkS")
	)
	(gr_text "A2DVI.v2.4\nBoard design by R. Palaveev, (c) 2025\nFirmware by Thorsten Brehm, (c) 2025"
		(at 94.6912 108.92665 0)
		(layer "B.Mask")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.4924 146.92505) (xy 180.4924 122.79505) (xy 153.162 122.76965) (xy 153.162 97.26805) (xy 68.9102 97.29345)
				(xy 68.8848 146.92505)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Mask")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.575)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.395 147.803243) (xy 112.395 154.026243) (xy 112.649 154.280243) (xy 177.673 154.280243)
				(xy 177.927 154.026243) (xy 177.927 147.803243)
			)
		)
	)
)
