(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "ATF150x_uDEV")
		(date "2026-09-05")
		(rev "014")
		(company "Brian K. White")
		(comment 1 "CC-BY-SA")
		(comment 2 "github.com/bkw777/ATF150x_uDEV")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "HAL lead-free")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 144.78 100.33)
		(grid_origin 144.78 100.33)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin yes)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(LED1-A)")
	(net 3 "Net-(LED2-A)")
	(net 4 "/1{slash}TDI")
	(net 5 "/7{slash}TMS")
	(net 6 "/32{slash}TDO")
	(net 7 "/26{slash}TCK")
	(net 8 "/3")
	(net 9 "/13")
	(net 10 "/6")
	(net 11 "/12")
	(net 12 "/8")
	(net 13 "/15")
	(net 14 "/5{slash}PD1")
	(net 15 "/18")
	(net 16 "/14")
	(net 17 "/10")
	(net 18 "/19{slash}PD2")
	(net 19 "/20")
	(net 20 "/11")
	(net 21 "/2")
	(net 22 "/37{slash}GCLK1")
	(net 23 "/38{slash}OE1{slash}Vpp")
	(net 24 "/25")
	(net 25 "/44")
	(net 26 "/39{slash}GCLR")
	(net 27 "/43")
	(net 28 "/28")
	(net 29 "/34")
	(net 30 "/33")
	(net 31 "/27")
	(net 32 "/31")
	(net 33 "/30")
	(net 34 "/35{slash}GCLK3")
	(net 35 "/40{slash}OE2{slash}GCLK2")
	(net 36 "/42")
	(net 37 "/21")
	(net 38 "unconnected-(J1-nc-Pad7)")
	(net 39 "unconnected-(J1-nc-Pad8)")
	(net 40 "Net-(J1-VPP)")
	(net 41 "VCCIO")
	(net 42 "VCCINT")
	(net 43 "/22")
	(net 44 "/23")
	(footprint "000_LOCAL:IDC-Header_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 120.650003 101.599999 90)
		(descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
		(property "Reference" "J1"
			(at 0 -2.159001 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Altera JTAG-A+VPP"
			(at 1.27 16.26 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "datasheets/JTAG-A.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 7 "/26{slash}TCK")
			(pinfunction "TCK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/32{slash}TDO")
			(pinfunction "TDO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "VCCIO")
			(pinfunction "VREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/7{slash}TMS")
			(pinfunction "TMS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J1-VPP)")
			(pinfunction "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(J1-nc-Pad7)")
			(pinfunction "nc")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(J1-nc-Pad8)")
			(pinfunction "nc")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0 10.16 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/1{slash}TDI")
			(pinfunction "TDI")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/IDC-Header_2x05_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SolderJumper_1mm_2p_open"
		(layer "F.Cu")
		(at 139.922513 94.637487 45)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at -1.262893 -1.161069 45)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "VPP"
			(at -0.81388 0.006364 45)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" smd custom
			(at -0.349999 0 45)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(net 40 "Net-(J1-VPP)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.25 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.25 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.25 0.5) (xy 0 0.5) (xy 0 -0.5) (xy 0.25 -0.5)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.349999 0 225)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(net 23 "/38{slash}OE1{slash}Vpp")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.25 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.25 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.25 0.5) (xy 0 0.5) (xy 0 -0.5) (xy 0.25 -0.5)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/SolderJumper_1.2x1.0.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "F.Cu")
		(at 163.83 96.139 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED2"
			(at 0.014 1.651 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GRN"
			(at 0 1.778 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "150060GS75000"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfg" "Wurth"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.397 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(LED2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:VQFP44"
		(layer "F.Cu")
		(at 144.780003 100.329999 45)
		(property "Reference" "U1"
			(at -1.796054 -3.771709 45)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATF150x-xAx44"
			(at -0.459622 0.459618 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/ATF1502AS.pdf"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microchip CPLD, 32 Macrocell, 5 V, TQFP-44"
			(at 0 0 45)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*10x10mm*P0.8mm*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -5.75 -4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/1{slash}TDI")
			(pinfunction "I/O/TDI")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -5.75 -3.2 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/2")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -5.75 -2.4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/3")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -5.75 -1.6 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -5.75 -0.799999 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/5{slash}PD1")
			(pinfunction "I/O/PD1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -5.75 0 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/6")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -5.75 0.799999 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/7{slash}TMS")
			(pinfunction "I/O/TMS")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -5.75 1.6 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/8")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -5.75 2.4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "VCCIO")
			(pinfunction "VCCIO")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -5.75 3.2 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/10")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -5.75 4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/11")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -4 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/12")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -3.2 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/13")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -2.4 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/14")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -1.6 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/15")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -0.799999 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 0 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "VCCINT")
			(pinfunction "VCCINT")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 0.799999 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/18")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 1.6 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/19{slash}PD2")
			(pinfunction "I/O/PD2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 2.4 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/20")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 3.2 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/21")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 4 5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/22")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 5.75 4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/23")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 5.75 3.2 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 5.75 2.4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/25")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 5.75 1.6 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/26{slash}TCK")
			(pinfunction "I/O/TCK")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 5.75 0.799999 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/27")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 5.75 0 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/28")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 5.75 -0.799999 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "VCCIO")
			(pinfunction "VCCIO")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 5.75 -1.6 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/30")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 5.75 -2.4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/31")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 5.75 -3.2 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/32{slash}TDO")
			(pinfunction "I/O/TDO")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" smd roundrect
			(at 5.75 -4 135)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/33")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" smd roundrect
			(at 4 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/34")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" smd roundrect
			(at 3.2 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/35{slash}GCLK3")
			(pinfunction "I/O/GCLK3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" smd roundrect
			(at 2.4 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" smd roundrect
			(at 1.6 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/37{slash}GCLK1")
			(pinfunction "I/GCLK1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" smd roundrect
			(at 0.799999 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/38{slash}OE1{slash}Vpp")
			(pinfunction "I/OE1/Vpp")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" smd roundrect
			(at 0 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/39{slash}GCLR")
			(pinfunction "I/GCLR")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" smd roundrect
			(at -0.799999 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/40{slash}OE2{slash}GCLK2")
			(pinfunction "I/OE2/GCLK2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "41" smd roundrect
			(at -1.6 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "VCCINT")
			(pinfunction "VCCINT")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "42" smd roundrect
			(at -2.4 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/42")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "43" smd roundrect
			(at -3.2 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/43")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "44" smd roundrect
			(at -4 -5.75 45)
			(size 0.4572 0.8636)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/44")
			(pinfunction "I/O")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/TQFP-44_10x10mm_P0.8mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "F.Cu")
		(at 163.83 104.521 180)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at 0.014 -1.777999 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GRN"
			(at 0.014 -1.651 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "150060GS75000"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mfg" "Wurth"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.397 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0 180)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:PinHeader_1x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 116.840003 91.439999 -90)
		(descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x20 2.54mm single row")
		(property "Reference" "J3"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "1x20x2.54mm"
			(at 0 -50.59 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -24.130001 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "VCCINT")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/44")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/43")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0 -10.16 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/42")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at 0 -12.7 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/40{slash}OE2{slash}GCLK2")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 0 -15.24 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/39{slash}GCLR")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at 0 -17.78 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/38{slash}OE1{slash}Vpp")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0 -20.32 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/37{slash}GCLK1")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 0 -22.86 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/35{slash}GCLK3")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 0 -25.4 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/34")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at 0 -27.94 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/33")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 0 -30.48 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/32{slash}TDO")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at 0 -33.02 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/31")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 0 -35.56 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/30")
			(pinfunction "Pin_15")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 0 -38.1 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/28")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 0 -40.64 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/27")
			(pinfunction "Pin_17")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at 0 -43.18 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/26{slash}TCK")
			(pinfunction "Pin_18")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at 0 -45.72 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/25")
			(pinfunction "Pin_19")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at 0 -48.26 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/23")
			(pinfunction "Pin_20")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_1x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "B.Cu")
		(at 148.479818 96.398814)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C2"
			(at -1.999817 -0.468814 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at -1.999817 0.756186 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.270001 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 41 "VCCIO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "B.Cu")
		(at 149.18 103.63)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C3"
			(at -2.025 -0.35 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at -2.05 0.825 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.270001 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 42 "VCCINT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "B.Cu")
		(at 154.94 101.6)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "JP1"
			(at 0 -5.08 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VCC"
			(at 4.385 -4.81 180)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 -1.27 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "VCCIO")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "VCCINT")
			(pinfunction "B")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/Jumper.step"
			(offset
				(xyz 4.064 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -0 90)
			)
		)
	)
	(footprint "000_LOCAL:PinHeader_1x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 116.840001 109.219999 -90)
		(descr "Through hole straight pin header, 1x20, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x20 2.54mm single row")
		(property "Reference" "J2"
			(at 0 2.33 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "1x20x2.54mm"
			(at 0 -50.59 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -24.130001 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "VCCIO")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/1{slash}TDI")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/2")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0 -10.16 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/3")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at 0 -12.7 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/5{slash}PD1")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 0 -15.24 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/6")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at 0 -17.78 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/7{slash}TMS")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0 -20.32 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/8")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 0 -22.86 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/10")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 0 -25.4 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/11")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at 0 -27.94 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/12")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 0 -30.48 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/13")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at 0 -33.02 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/14")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 0 -35.56 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/15")
			(pinfunction "Pin_15")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 0 -38.1 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/18")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 0 -40.64 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/19{slash}PD2")
			(pinfunction "Pin_17")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at 0 -43.18 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/20")
			(pinfunction "Pin_18")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at 0 -45.72 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/21")
			(pinfunction "Pin_19")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at 0 -48.26 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/22")
			(pinfunction "Pin_20")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/PinHeader_1x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "B.Cu")
		(at 157.353 104.521)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R1"
			(at -1.773 -0.508 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at -1.773 0.635 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.270001 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 0.7 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 41 "VCCIO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 0.7 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "Net-(LED1-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "B.Cu")
		(at 139.383131 98.095869 180)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C4"
			(at 1.928132 0.625 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at 2.003132 -0.55 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.270001 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 180)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 42 "VCCINT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 180)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "B.Cu")
		(at 157.353 96.139)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R2"
			(at -1.773 -0.635 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at -1.773 0.508 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.270001 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 0.7 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 42 "VCCINT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 0.7 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 3 "Net-(LED2-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "B.Cu")
		(at 142.13 105.28 180)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C1"
			(at 1.931558 0.612555 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at 1.931558 -0.612445 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ATF150x_uDEV.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.270001 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 180)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 41 "VCCIO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 180)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 115.569999 91.439999)
		(mid 115.941973 90.541974)
		(end 116.839998 90.169999)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.569999 109.22)
		(end 115.569999 91.440001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.84 90.169999)
		(end 165.099998 90.169999)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116.84 110.490001)
		(mid 115.941972 110.118027)
		(end 115.569999 109.22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 165.099998 90.169999)
		(mid 165.998024 90.541974)
		(end 166.369999 91.440001)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 165.099999 110.49)
		(end 116.839999 110.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 166.369999 91.440001)
		(end 166.369999 109.22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 166.370001 109.22)
		(mid 165.998026 110.118027)
		(end 165.099998 110.490001)
		(layer "Edge.Cuts")
	)
	(gr_text "JTAG-A+VPP"
		(at 125.73 105.918 0)
		(layer "F.SilkS")
	)
	(gr_text "1V8"
		(at 158.242 102.295 0)
		(layer "F.SilkS")
	)
	(gr_text "ATF1502"
		(at 161.29 98.485 0)
		(layer "F.SilkS")
	)
	(gr_text "ATF1504"
		(at 161.29 100.39 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 161.29 102.295 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 164.338 102.295 0)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 144.7038 107.823 0)
		(layer "F.SilkS")
	)
	(gr_text "33"
		(at 144.82 92.964 0)
		(layer "F.SilkS")
	)
	(gr_text "VIO"
		(at 116.84 108.077 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 119.38 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 121.92 108.077 90)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 124.460002 108.204001 90)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 127 108.204001 90)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 129.54 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 132.080002 108.204001 90)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 134.62 108.0262 90)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 137.16 108.204001 90)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 139.700002 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "11"
		(at 141.859 108.585 90)
		(layer "F.SilkS")
	)
	(gr_text "13"
		(at 147.886606 108.592577 90)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 149.86 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 152.4 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "18"
		(at 154.94 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 157.48 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "20"
		(at 160.02 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "21"
		(at 162.560002 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "22"
		(at 165.1 108.204 90)
		(layer "F.SilkS")
	)
	(gr_text "VINT"
		(at 116.840003 92.239999 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 119.38 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "44"
		(at 121.92 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "43"
		(at 124.46 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "42"
		(at 127 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "40"
		(at 129.540001 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "39"
		(at 132.08 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "38"
		(at 134.62 92.4814 90)
		(layer "F.SilkS")
	)
	(gr_text "37"
		(at 137.033 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "35"
		(at 138.78 92.13 90)
		(layer "F.SilkS")
	)
	(gr_text "34"
		(at 141.43 92.13 90)
		(layer "F.SilkS")
	)
	(gr_text "32"
		(at 148.3868 92.5322 90)
		(layer "F.SilkS")
	)
	(gr_text "31"
		(at 150.241 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "30"
		(at 152.400001 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "28"
		(at 154.94 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "27"
		(at 157.48 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "26"
		(at 160.02 92.6084 90)
		(layer "F.SilkS")
	)
	(gr_text "25"
		(at 162.56 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "23"
		(at 165.1 92.456 90)
		(layer "F.SilkS")
	)
	(gr_text "VCCINT"
		(at 161.925 96.145606 0)
		(layer "F.SilkS")
	)
	(gr_text "VCCIO"
		(at 161.925 104.521 0)
		(layer "F.SilkS")
	)
	(gr_text "OE2\nGCLK2"
		(at 129.285999 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "OE1\nVPP"
		(at 134.62 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "v${REVISION}"
		(at 134.28 100.33 0)
		(layer "B.SilkS")
	)
	(gr_text "${COMMENT2}"
		(at 142.875 101.98 0)
		(layer "B.SilkS")
	)
	(gr_text "VCCINT"
		(at 116.84 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 119.38 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "TCK"
		(at 120.649998 102.616 90)
		(layer "B.SilkS")
	)
	(gr_text "TDO"
		(at 123.19 102.615999 90)
		(layer "B.SilkS")
	)
	(gr_text "TMS"
		(at 125.856998 102.616 90)
		(layer "B.SilkS")
	)
	(gr_text "TDI"
		(at 130.809998 102.616 90)
		(layer "B.SilkS")
	)
	(gr_text "GCLR"
		(at 132.079999 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "GCLK1"
		(at 137.159999 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "GCLK3"
		(at 139.7 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "TDO"
		(at 147.319999 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "TCK"
		(at 160.019998 92.837 90)
		(layer "B.SilkS")
	)
	(gr_text "VCCIO"
		(at 116.840002 107.823 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 119.38 107.823 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 120.65 98.044 90)
		(layer "B.SilkS")
	)
	(gr_text "TDI"
		(at 121.92 107.823 90)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 123.19 98.044 90)
		(layer "B.SilkS")
	)
	(gr_text "VPP"
		(at 125.73 98.044 90)
		(layer "B.SilkS")
	)
	(gr_text "PD1"
		(at 129.54 107.823 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 130.81 98.044 90)
		(layer "B.SilkS")
	)
	(gr_text "TMS"
		(at 134.62 107.823 90)
		(layer "B.SilkS")
	)
	(gr_text "PD2"
		(at 157.48 107.8992 90)
		(layer "B.SilkS")
	)
	(gr_text "VCCINT"
		(at 166.116 96.901 0)
		(layer "B.SilkS")
	)
	(gr_text "VCCIO"
		(at 166.116 103.886 0)
		(layer "B.SilkS")
	)
	(gr_text "${TITLE}"
		(at 144.78 100.33 0)
		(layer "B.SilkS")
	)
	(zone
		(net 22)
		(net_name "/37{slash}GCLK1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.326372 92.464977) (xy 138.225709 92.361478) (xy 138.148928 92.267599) (xy 138.097537 92.189297)
				(xy 138.060122 92.114544) (xy 138.017245 91.967512) (xy 137.996746 91.742689) (xy 137.982521 91.539025)
				(xy 137.944631 91.283927) (xy 137.159282 91.439307) (xy 137.003931 92.224627) (xy 137.301844 92.268312)
				(xy 137.451968 92.280338) (xy 137.636819 92.297748) (xy 137.721116 92.313987) (xy 137.804212 92.339873)
				(xy 137.88927 92.378873) (xy 137.979453 92.434455) (xy 138.077925 92.510087) (xy 138.18785 92.609237)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.78 104.685764) (xy 142.780271 104.77972) (xy 142.775392 104.982418) (xy 142.735764 105.221473)
				(xy 143.03 105.281) (xy 143.324236 105.221473) (xy 143.284608 104.98242) (xy 143.279729 104.779727)
				(xy 143.28 104.685764)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/33")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.805405 92.623117) (xy 145.722441 92.533242) (xy 145.658692 92.449402) (xy 145.614476 92.375291)
				(xy 145.583356 92.304359) (xy 145.553097 92.167153) (xy 145.555527 92.010846) (xy 145.56992 91.891908)
				(xy 145.585387 91.765689) (xy 145.594678 91.625113) (xy 145.590267 91.46594) (xy 145.564631 91.283927)
				(xy 144.779296 91.439292) (xy 144.335547 92.105175) (xy 144.459974 92.182645) (xy 144.57319 92.242663)
				(xy 144.785697 92.327171) (xy 144.975115 92.378141) (xy 145.131863 92.419662) (xy 145.290887 92.482263)
				(xy 145.464242 92.589403) (xy 145.560061 92.667006) (xy 145.663983 92.764539)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/22")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.908789 108.170208) (xy 164.014609 108.28303) (xy 164.095074 108.384225) (xy 164.148255 108.466919)
				(xy 164.187166 108.545512) (xy 164.232749 108.699644) (xy 164.257877 108.925871) (xy 164.27616 109.126004)
				(xy 164.315373 109.376071) (xy 165.100708 109.220706) (xy 165.256073 108.435371) (xy 164.951851 108.390333)
				(xy 164.805875 108.377875) (xy 164.613379 108.358483) (xy 164.526181 108.340966) (xy 164.440666 108.313355)
				(xy 164.353573 108.271991) (xy 164.261641 108.213214) (xy 164.161608 108.133366) (xy 164.050211 108.028786)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/1{slash}TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.237707 101.81) (xy 137.283272 101.809035) (xy 137.448859 101.812781) (xy 137.524961 101.831059)
				(xy 137.577113 101.869494) (xy 137.886712 101.567436) (xy 137.771071 101.358787) (xy 137.655496 101.464078)
				(xy 137.510912 101.546613) (xy 137.349529 101.598011) (xy 137.237707 101.61)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/38{slash}OE1{slash}Vpp")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.671727 94.948932) (xy 140.635217 94.90506) (xy 140.60039 94.846983) (xy 140.574479 94.783142)
				(xy 140.560255 94.713933) (xy 140.560399 94.658961) (xy 140.572766 94.604481) (xy 140.591973 94.564014)
				(xy 140.169293 94.389293) (xy 140.346777 94.92033) (xy 140.374495 94.917934) (xy 140.421969 94.957739)
				(xy 140.483014 95.03268) (xy 140.530306 95.090353)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/43")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.913713 98.130615) (xy 138.000118 98.232823) (xy 138.037069 98.299351) (xy 138.053328 98.368369)
				(xy 138.040469 98.426933) (xy 138.452104 98.527584) (xy 138.351453 98.115949) (xy 138.287623 98.128574)
				(xy 138.210387 98.106517) (xy 138.116172 98.044701) (xy 138.055135 97.989193)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.518695 103.183282) (xy 138.532702 103.175963) (xy 138.604501 103.139848) (xy 138.690243 103.105603)
				(xy 138.77437 103.09056) (xy 138.810967 103.095657) (xy 138.841325 103.112055) (xy 139.018034 102.698498)
				(xy 138.630932 102.761669) (xy 138.629964 102.826735) (xy 138.592988 102.891329) (xy 138.516638 102.957569)
				(xy 138.456886 102.993074)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/38{slash}OE1{slash}Vpp")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.46896 94.030381) (xy 139.527363 94.078105) (xy 139.617209 94.153213) (xy 139.642531 94.187168)
				(xy 139.63967 94.213223) (xy 140.170707 94.390707) (xy 139.995137 93.968027) (xy 139.909499 93.99863)
				(xy 139.812018 93.995157) (xy 139.70498 93.956431) (xy 139.610381 93.88896)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/37{slash}GCLK1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.307826 94.736502) (xy 141.394231 94.83871) (xy 141.431182 94.905238) (xy 141.447441 94.974256)
				(xy 141.434582 95.03282) (xy 141.846217 95.133471) (xy 141.745566 94.721836) (xy 141.681736 94.734461)
				(xy 141.6045 94.712404) (xy 141.510285 94.650588) (xy 141.449248 94.59508)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.051527 98.447974) (xy 140.90602 98.29508) (xy 140.815878 98.181513) (xy 140.733683 98.05592)
				(xy 140.615719 97.873641) (xy 140.282424 98.095162) (xy 140.060903 98.428457) (xy 140.246727 98.533612)
				(xy 140.356275 98.578427) (xy 140.432819 98.609036) (xy 140.510174 98.648668) (xy 140.596004 98.708954)
				(xy 140.697974 98.801527)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VPP)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.015241 94.73) (xy 139.129867 94.749621) (xy 139.266313 94.814678) (xy 139.336732 94.865223)
				(xy 139.404544 94.926742) (xy 139.466007 94.996494) (xy 139.521465 95.075794) (xy 139.535035 95.098536)
				(xy 139.676026 94.884974) (xy 139.358433 94.49446) (xy 139.317131 94.522805) (xy 139.228407 94.537015)
				(xy 139.085176 94.533152) (xy 139.015241 94.53)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.219541 107.837353) (xy 147.231402 107.943553) (xy 147.231297 108.034132) (xy 147.221515 108.105622)
				(xy 147.203262 108.167751) (xy 147.144005 108.27186) (xy 147.043454 108.375206) (xy 146.980052 108.4294)
				(xy 146.82179 108.571701) (xy 146.738332 108.663436) (xy 146.654825 108.775543) (xy 147.320157 109.220986)
				(xy 147.985177 108.775543) (xy 147.815729 108.549861) (xy 147.713164 108.433804) (xy 147.613608 108.319438)
				(xy 147.532214 108.1968) (xy 147.467273 108.035731) (xy 147.417079 107.806073)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/1{slash}TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.872066 103.151815) (xy 130.959905 102.898432) (xy 131.036876 102.715374) (xy 131.159387 102.500491)
				(xy 131.272855 102.336973) (xy 131.475179 102.044455) (xy 130.810312 101.599048) (xy 130.144827 102.044455)
				(xy 130.2868 102.226776) (xy 130.471123 102.409976) (xy 130.604818 102.541917) (xy 130.656919 102.608348)
				(xy 130.696252 102.679916) (xy 130.720615 102.760243) (xy 130.727806 102.852952) (xy 130.715621 102.961666)
				(xy 130.681858 103.090007)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.233633 108.195022) (xy 151.334296 108.298523) (xy 151.411077 108.392402) (xy 151.462467 108.470705)
				(xy 151.499882 108.545458) (xy 151.542758 108.692491) (xy 151.563257 108.917308) (xy 151.577482 109.120973)
				(xy 151.615373 109.376071) (xy 152.400722 109.220691) (xy 152.556073 108.435371) (xy 152.258164 108.391687)
				(xy 152.108032 108.37966) (xy 151.923182 108.362251) (xy 151.838886 108.346012) (xy 151.755791 108.320126)
				(xy 151.670733 108.281127) (xy 151.580551 108.225545) (xy 151.48208 108.149913) (xy 151.372157 108.050764)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/44")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.348028 98.6963) (xy 137.434433 98.798508) (xy 137.471384 98.865036) (xy 137.487643 98.934054)
				(xy 137.474784 98.992618) (xy 137.886419 99.093269) (xy 137.785768 98.681634) (xy 137.721938 98.694259)
				(xy 137.644702 98.672202) (xy 137.550487 98.610386) (xy 137.48945 98.554878)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.710703 99.90285) (xy 153.78906 99.831395) (xy 153.863179 99.777308) (xy 153.929701 99.740716)
				(xy 153.993732 99.716498) (xy 154.117092 99.699369) (xy 154.251697 99.717677) (xy 154.420288 99.77017)
				(xy 154.560364 99.815897) (xy 154.716059 99.852179) (xy 154.892814 99.866072) (xy 154.99079 99.860576)
				(xy 155.096072 99.844628) (xy 154.940707 99.059293) (xy 154.274824 98.615544) (xy 154.154944 98.786281)
				(xy 154.05184 98.915859) (xy 153.880727 99.089096) (xy 153.752301 99.196165) (xy 153.580838 99.339385)
				(xy 153.35715 99.549297)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/7{slash}TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.669792 108.028788) (xy 135.55697 108.134608) (xy 135.455775 108.215072) (xy 135.373081 108.268253)
				(xy 135.294488 108.307165) (xy 135.140356 108.352748) (xy 134.914129 108.377875) (xy 134.713996 108.396158)
				(xy 134.463929 108.435371) (xy 134.619294 109.220706) (xy 135.404629 109.376071) (xy 135.449666 109.071849)
				(xy 135.462124 108.925876) (xy 135.481515 108.733379) (xy 135.499033 108.64618) (xy 135.526644 108.560666)
				(xy 135.568008 108.473573) (xy 135.626785 108.381641) (xy 135.706634 108.281607) (xy 135.811214 108.17021)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/26{slash}TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.970213 92.631211) (xy 159.083035 92.52539) (xy 159.18423 92.444926) (xy 159.266924 92.391744)
				(xy 159.345517 92.352833) (xy 159.499648 92.30725) (xy 159.725877 92.282123) (xy 159.926009 92.26384)
				(xy 160.176075 92.224627) (xy 160.02071 91.439292) (xy 159.235375 91.283927) (xy 159.190337 91.588147)
				(xy 159.177879 91.734126) (xy 159.158487 91.926621) (xy 159.14097 92.013819) (xy 159.113359 92.099334)
				(xy 159.071995 92.186427) (xy 159.013219 92.278359) (xy 158.933371 92.378392) (xy 158.828791 92.489789)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/44")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 123.068679 92.446404) (xy 122.97221 92.370233) (xy 122.89681 92.297622) (xy 122.844248 92.23346)
				(xy 122.805099 92.170253) (xy 122.759423 92.043816) (xy 122.742921 91.890126) (xy 122.742334 91.769925)
				(xy 122.738592 91.551791) (xy 122.727291 91.425006) (xy 122.704631 91.283927) (xy 121.919194 91.439412)
				(xy 121.763931 92.224627) (xy 122.123356 92.282621) (xy 122.165052 92.28801) (xy 122.355336 92.315912)
				(xy 122.526457 92.361887) (xy 122.713392 92.450972) (xy 122.951119 92.608204)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.635087 107.883491) (xy 145.52511 107.986664) (xy 145.424588 108.067846) (xy 145.333196 108.129587)
				(xy 145.247265 108.17684) (xy 145.06997 108.24579) (xy 144.957097 108.278015) (xy 144.827515 108.3152)
				(xy 144.684981 108.365913) (xy 144.523117 108.441879) (xy 144.335545 108.554823) (xy 144.779294 109.220706)
				(xy 145.564629 109.376071) (xy 145.592119 109.147491) (xy 145.584214 108.932329) (xy 145.558119 108.753196)
				(xy 145.533676 108.575075) (xy 145.532066 108.489901) (xy 145.54241 108.404719) (xy 145.568367 108.317579)
				(xy 145.613596 108.226532) (xy 145.681757 108.129626) (xy 145.776509 108.024913)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/7{slash}TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.63 105.041804) (xy 125.625332 105.121336) (xy 125.612658 105.181931) (xy 125.564439 105.284186)
				(xy 125.521714 105.365815) (xy 125.484804 105.488227) (xy 125.73 105.538) (xy 125.975196 105.488227)
				(xy 125.931905 105.351584) (xy 125.895561 105.284187) (xy 125.849647 105.189291) (xy 125.835319 105.126128)
				(xy 125.83 105.041804)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.098328 107.036495) (xy 147.024988 106.946955) (xy 146.994002 106.88815) (xy 146.97974 106.825442)
				(xy 146.994053 106.758549) (xy 146.582538 106.657796) (xy 146.683069 107.069533) (xy 146.753078 107.053455)
				(xy 146.827091 107.072369) (xy 146.90638 107.125603) (xy 146.936524 107.154047)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.491098 108.051772) (xy 125.332895 108.160524) (xy 125.20018 108.2383) (xy 125.101678 108.284432)
				(xy 125.009667 108.316888) (xy 124.814771 108.357285) (xy 124.705009 108.371989) (xy 124.527414 108.396312)
				(xy 124.303929 108.435371) (xy 124.459193 109.220586) (xy 125.244629 109.376071) (xy 125.277446 109.126709)
				(xy 125.282327 108.89005) (xy 125.286351 108.705908) (xy 125.298099 108.622314) (xy 125.321486 108.541853)
				(xy 125.360374 108.462636) (xy 125.418624 108.382776) (xy 125.500098 108.300383) (xy 125.608658 108.21357)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/32{slash}TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.417081 92.853923) (xy 147.445224 92.707488) (xy 147.478329 92.589591) (xy 147.512961 92.502006)
				(xy 147.552241 92.427979) (xy 147.652856 92.293551) (xy 147.713165 92.226195) (xy 147.837518 92.083964)
				(xy 147.985179 91.884455) (xy 147.320159 91.439012) (xy 146.654827 91.884455) (xy 146.78775 92.052866)
				(xy 146.942723 92.199027) (xy 146.980053 92.230597) (xy 147.098294 92.336262) (xy 147.146409 92.391264)
				(xy 147.185274 92.452202) (xy 147.213455 92.522443) (xy 147.229517 92.605352) (xy 147.232024 92.704296)
				(xy 147.219543 92.822643)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/19{slash}PD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.331443 108.21347) (xy 156.427897 108.289622) (xy 156.503286 108.362217) (xy 156.555842 108.42637)
				(xy 156.594987 108.489569) (xy 156.640653 108.615991) (xy 156.65714 108.769649) (xy 156.657708 108.88993)
				(xy 156.661418 109.108127) (xy 156.672711 109.23495) (xy 156.695373 109.376071) (xy 157.48081 109.220586)
				(xy 157.636073 108.435371) (xy 157.276433 108.377322) (xy 157.23524 108.371992) (xy 157.044884 108.344045)
				(xy 156.873733 108.298039) (xy 156.686775 108.208927) (xy 156.448995 108.051664)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/34")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.004882 93.039446) (xy 143.091287 93.141654) (xy 143.128238 93.208182) (xy 143.144497 93.2772)
				(xy 143.131638 93.335764) (xy 143.543273 93.436415) (xy 143.442622 93.02478) (xy 143.378792 93.037405)
				(xy 143.301556 93.015348) (xy 143.207341 92.953532) (xy 143.146304 92.898024)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.187838 108.05077) (xy 138.074354 108.152908) (xy 137.973006 108.230003) (xy 137.890233 108.280635)
				(xy 137.811825 108.317196) (xy 137.657276 108.359075) (xy 137.451994 108.379668) (xy 137.25349 108.396711)
				(xy 137.003929 108.435371) (xy 137.15928 109.220691) (xy 137.944629 109.376071) (xy 137.985283 109.091528)
				(xy 137.996752 108.91733) (xy 138.011027 108.732994) (xy 138.02628 108.648895) (xy 138.051699 108.566373)
				(xy 138.090852 108.482575) (xy 138.147304 108.394651) (xy 138.224622 108.299749) (xy 138.326374 108.195016)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.546104 97.712395) (xy 139.644326 97.817326) (xy 139.710891 97.902573) (xy 139.79961 98.05744)
				(xy 139.858784 98.169392) (xy 139.950543 98.318097) (xy 140.283838 98.096576) (xy 140.505359 97.763281)
				(xy 140.286341 97.633643) (xy 140.244702 97.612348) (xy 140.091379 97.5247) (xy 140.005504 97.45785)
				(xy 139.899657 97.358842)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/30")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.110757 94.59508) (xy 148.008544 94.681489) (xy 147.942014 94.718439) (xy 147.872994 94.734695)
				(xy 147.81444 94.721836) (xy 147.713789 95.133471) (xy 148.125424 95.03282) (xy 148.112799 94.96899)
				(xy 148.134856 94.891753) (xy 148.196671 94.797538) (xy 148.252179 94.736502)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.574236 93.73) (xy 129.48028 93.730271) (xy 129.277582 93.725392) (xy 129.038527 93.685764)
				(xy 128.979 93.98) (xy 129.038527 94.274236) (xy 129.27758 94.234608) (xy 129.480273 94.229729)
				(xy 129.574236 94.23)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.973997 107.827425) (xy 146.02498 107.763833) (xy 146.097868 107.674114) (xy 146.132311 107.646621)
				(xy 146.161446 107.643853) (xy 146.018147 107.223583) (xy 145.768196 107.298335) (xy 145.812433 107.349312)
				(xy 145.845111 107.400878) (xy 145.880191 107.505808) (xy 145.876331 107.603973) (xy 145.860991 107.645982)
				(xy 145.838387 107.679812) (xy 145.832575 107.686003)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/27")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.430212 92.631211) (xy 156.543034 92.52539) (xy 156.644229 92.444926) (xy 156.726923 92.391745)
				(xy 156.805516 92.352833) (xy 156.959647 92.30725) (xy 157.185876 92.282123) (xy 157.386009 92.26384)
				(xy 157.636075 92.224627) (xy 157.48071 91.439292) (xy 156.695375 91.283927) (xy 156.650337 91.588148)
				(xy 156.637879 91.734125) (xy 156.618487 91.92662) (xy 156.60097 92.013819) (xy 156.573359 92.099334)
				(xy 156.531995 92.186426) (xy 156.473218 92.278359) (xy 156.39337 92.378392) (xy 156.28879 92.489789)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/38{slash}OE1{slash}Vpp")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.950652 92.30923) (xy 135.848892 92.200664) (xy 135.768701 92.101113) (xy 135.707637 92.010328)
				(xy 135.660948 91.924836) (xy 135.593713 91.749225) (xy 135.560161 91.625978) (xy 135.524318 91.494206)
				(xy 135.474641 91.349493) (xy 135.398977 91.185414) (xy 135.285179 90.995543) (xy 134.619296 91.439292)
				(xy 134.463931 92.224627) (xy 134.69576 92.252835) (xy 134.914203 92.245875) (xy 135.079635 92.223963)
				(xy 135.25825 92.202339) (xy 135.343517 92.201994) (xy 135.42875 92.213483) (xy 135.515943 92.24045)
				(xy 135.607091 92.286539) (xy 135.704189 92.355392) (xy 135.80923 92.450652)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.972672 102.618415) (xy 137.986028 102.611058) (xy 138.05384 102.575142) (xy 138.135066 102.541217)
				(xy 138.215816 102.526367) (xy 138.251673 102.531433) (xy 138.282201 102.547674) (xy 138.452288 102.132668)
				(xy 138.065246 102.195983) (xy 138.064614 102.260656) (xy 138.027627 102.327097) (xy 137.949749 102.397689)
				(xy 137.881877 102.440213)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.146303 107.761973) (xy 143.248503 107.675574) (xy 143.315025 107.638624) (xy 143.384039 107.62236)
				(xy 143.442622 107.635218) (xy 143.543273 107.223583) (xy 143.131638 107.324234) (xy 143.144263 107.388064)
				(xy 143.122206 107.4653) (xy 143.06039 107.559514) (xy 143.004882 107.620551)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.580619 107.196289) (xy 142.682823 107.109887) (xy 142.749348 107.072936) (xy 142.818364 107.056675)
				(xy 142.876937 107.069533) (xy 142.977588 106.657898) (xy 142.565953 106.758549) (xy 142.578578 106.822379)
				(xy 142.556521 106.899616) (xy 142.494705 106.99383) (xy 142.439197 107.054867)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.686495 106.489181) (xy 147.60009 106.386973) (xy 147.563139 106.320445) (xy 147.546881 106.251427)
				(xy 147.559739 106.192863) (xy 147.148104 106.092212) (xy 147.248755 106.503847) (xy 147.312585 106.491223)
				(xy 147.389823 106.51328) (xy 147.484038 106.575096) (xy 147.545073 106.630603)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/43")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.651213 92.489791) (xy 125.545393 92.376968) (xy 125.464929 92.275774) (xy 125.411747 92.19308)
				(xy 125.372836 92.114487) (xy 125.327253 91.960355) (xy 125.302126 91.734127) (xy 125.283844 91.533994)
				(xy 125.244631 91.283927) (xy 124.459296 91.439292) (xy 124.303931 92.224627) (xy 124.608152 92.269664)
				(xy 124.754126 92.282122) (xy 124.946622 92.301513) (xy 125.03382 92.319031) (xy 125.119335 92.346642)
				(xy 125.206428 92.388006) (xy 125.29836 92.446783) (xy 125.398394 92.526632) (xy 125.509791 92.631212)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/39{slash}GCLR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.228659 92.446428) (xy 133.132192 92.370258) (xy 133.056794 92.297649) (xy 133.004233 92.233488)
				(xy 132.965085 92.170281) (xy 132.919411 92.043845) (xy 132.902911 91.890159) (xy 132.902328 91.769948)
				(xy 132.898591 91.551804) (xy 132.887291 91.425013) (xy 132.864631 91.283927) (xy 132.079194 91.439412)
				(xy 131.923931 92.224627) (xy 132.283389 92.28263) (xy 132.325005 92.288009) (xy 132.515301 92.315918)
				(xy 132.686426 92.361898) (xy 132.873365 92.450989) (xy 133.111099 92.608228)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/26{slash}TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.3735 96.857822) (xy 150.271287 96.944231) (xy 150.204757 96.981181) (xy 150.135736 96.997437)
				(xy 150.077182 96.984578) (xy 149.976531 97.396213) (xy 150.388166 97.295562) (xy 150.375542 97.231732)
				(xy 150.397599 97.154495) (xy 150.459415 97.06028) (xy 150.514922 96.999244)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/32{slash}TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.186861 94.539075) (xy 146.289057 94.452679) (xy 146.355576 94.415729) (xy 146.424588 94.399463)
				(xy 146.483181 94.412321) (xy 146.583832 94.000686) (xy 146.172197 94.101337) (xy 146.184821 94.165167)
				(xy 146.162763 94.242403) (xy 146.100947 94.336617) (xy 146.045439 94.397653)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/20")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.828789 108.170208) (xy 158.934609 108.28303) (xy 159.015074 108.384225) (xy 159.068255 108.466919)
				(xy 159.107166 108.545512) (xy 159.152749 108.699644) (xy 159.177877 108.925871) (xy 159.19616 109.126004)
				(xy 159.235373 109.376071) (xy 160.020708 109.220706) (xy 160.176073 108.435371) (xy 159.871851 108.390333)
				(xy 159.725875 108.377875) (xy 159.533379 108.358483) (xy 159.446181 108.340966) (xy 159.360666 108.313355)
				(xy 159.273573 108.271991) (xy 159.181641 108.213214) (xy 159.081608 108.133366) (xy 158.970211 108.028786)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.917155 108.002685) (xy 148.994276 108.08671) (xy 149.053255 108.165738) (xy 149.093901 108.236339)
				(xy 149.121826 108.304131) (xy 149.145989 108.435017) (xy 149.135852 108.580234) (xy 149.105123 108.727758)
				(xy 149.076078 108.862297) (xy 149.054734 109.011947) (xy 149.051148 109.18158) (xy 149.075373 109.376071)
				(xy 149.860708 109.220706) (xy 150.304457 108.554823) (xy 150.168859 108.46982) (xy 150.048156 108.404319)
				(xy 149.82137 108.307872) (xy 149.71806 108.27231) (xy 149.569656 108.219482) (xy 149.419328 108.148246)
				(xy 149.253494 108.036281) (xy 149.058577 107.861263)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/23")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.070556 98.554878) (xy 151.968343 98.641287) (xy 151.901813 98.678237) (xy 151.832792 98.694493)
				(xy 151.774238 98.681634) (xy 151.673587 99.093269) (xy 152.085222 98.992618) (xy 152.072598 98.928788)
				(xy 152.094655 98.851551) (xy 152.156471 98.757336) (xy 152.211978 98.6963)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(LED1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.9175 104.621) (xy 162.038401 104.640563) (xy 162.117676 104.668609) (xy 162.197426 104.708315)
				(xy 162.265192 104.753805) (xy 162.324598 104.808058) (xy 162.364127 104.858783) (xy 162.392975 104.914953)
				(xy 162.411216 105.0085) (xy 162.8935 104.521) (xy 162.411216 104.0335) (xy 162.391414 104.130995)
				(xy 162.334651 104.22261) (xy 162.23793 104.3081) (xy 162.102815 104.37947) (xy 161.955179 104.418639)
				(xy 161.9175 104.421)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.552702 103.749145) (xy 148.486054 103.682881) (xy 148.346187 103.536116) (xy 148.205177 103.339065)
				(xy 147.955029 103.505029) (xy 147.789065 103.755177) (xy 147.986129 103.896196) (xy 148.132918 104.036084)
				(xy 148.199149 104.102698)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/18")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.949235 104.22644) (xy 149.86283 104.124232) (xy 149.82588 104.057704) (xy 149.809621 103.988686)
				(xy 149.82248 103.930122) (xy 149.410845 103.829471) (xy 149.511496 104.241106) (xy 149.575326 104.228482)
				(xy 149.652563 104.250539) (xy 149.746778 104.312355) (xy 149.807813 104.367862)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/34")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.967881 92.719601) (xy 142.89728 92.642044) (xy 142.84512 92.569477) (xy 142.81221 92.506949)
				(xy 142.791693 92.4468) (xy 142.782299 92.332256) (xy 142.809533 92.20429) (xy 142.878354 92.031169)
				(xy 142.95753 91.835408) (xy 142.994114 91.722123) (xy 143.024631 91.596071) (xy 142.239296 91.439292)
				(xy 141.795547 92.105175) (xy 142.173962 92.343703) (xy 142.324836 92.436424) (xy 142.465405 92.53464)
				(xy 142.623377 92.666718) (xy 142.826459 92.861023)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.749791 108.028787) (xy 140.636968 108.134607) (xy 140.535774 108.215072) (xy 140.453079 108.268253)
				(xy 140.374486 108.307164) (xy 140.220355 108.352747) (xy 139.994128 108.377875) (xy 139.793995 108.396158)
				(xy 139.543929 108.435371) (xy 139.699294 109.220706) (xy 140.484629 109.376071) (xy 140.529666 109.07185)
				(xy 140.542125 108.925873) (xy 140.561516 108.733377) (xy 140.579033 108.646179) (xy 140.606644 108.560664)
				(xy 140.648008 108.473571) (xy 140.706784 108.381639) (xy 140.786633 108.281606) (xy 140.891213 108.170209)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/5{slash}PD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.589791 108.028787) (xy 130.476968 108.134607) (xy 130.375774 108.215072) (xy 130.293079 108.268253)
				(xy 130.214486 108.307164) (xy 130.060355 108.352747) (xy 129.834128 108.377875) (xy 129.633995 108.396158)
				(xy 129.383929 108.435371) (xy 129.539294 109.220706) (xy 130.324629 109.376071) (xy 130.369666 109.07185)
				(xy 130.382125 108.925873) (xy 130.401516 108.733377) (xy 130.419033 108.646179) (xy 130.446644 108.560664)
				(xy 130.488008 108.473571) (xy 130.546784 108.381639) (xy 130.626633 108.281606) (xy 130.731213 108.170209)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/25")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.510213 92.631211) (xy 161.623035 92.52539) (xy 161.72423 92.444926) (xy 161.806924 92.391744)
				(xy 161.885517 92.352833) (xy 162.039648 92.30725) (xy 162.265877 92.282123) (xy 162.466009 92.26384)
				(xy 162.716075 92.224627) (xy 162.56071 91.439292) (xy 161.775375 91.283927) (xy 161.730337 91.588147)
				(xy 161.717879 91.734126) (xy 161.698487 91.926621) (xy 161.68097 92.013819) (xy 161.653359 92.099334)
				(xy 161.611995 92.186427) (xy 161.553219 92.278359) (xy 161.473371 92.378392) (xy 161.368791 92.489789)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/21")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.368789 108.170209) (xy 161.474609 108.283031) (xy 161.555074 108.384226) (xy 161.608255 108.46692)
				(xy 161.647166 108.545513) (xy 161.692749 108.699644) (xy 161.717877 108.925872) (xy 161.73616 109.126004)
				(xy 161.775373 109.376071) (xy 162.560708 109.220706) (xy 162.716073 108.435371) (xy 162.411852 108.390333)
				(xy 162.265874 108.377875) (xy 162.073378 108.358484) (xy 161.98618 108.340966) (xy 161.900665 108.313355)
				(xy 161.813573 108.271991) (xy 161.721641 108.213215) (xy 161.621607 108.133367) (xy 161.510211 108.028787)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.96329 95.661786) (xy 147.858357 95.760009) (xy 147.773109 95.826574) (xy 147.618245 95.915293)
				(xy 147.506294 95.974467) (xy 147.35759 96.066226) (xy 147.579111 96.399521) (xy 147.912406 96.621042)
				(xy 148.042043 96.402025) (xy 148.063337 96.360385) (xy 148.150985 96.207061) (xy 148.217835 96.121186)
				(xy 148.316844 96.015339)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.552701 103.262324) (xy 148.572598 103.235641) (xy 148.579975 103.209043) (xy 148.564369 103.160199)
				(xy 148.505632 103.107464) (xy 148.38996 103.055513) (xy 148.313663 103.036754) (xy 148.238905 103.028732)
				(xy 148.178284 103.032206) (xy 148.128985 103.047202) (xy 148.102863 103.066216) (xy 148.087199 103.092614)
				(xy 148.085764 103.139999) (xy 148.380707 103.080765) (xy 148.085764 103.139999) (xy 148.094472 103.159786)
				(xy 148.107753 103.161112) (xy 148.13897 103.127899) (xy 148.195949 103.013533) (xy 148.220866 102.936952)
				(xy 148.220881 102.897311) (xy 148.199148 102.908771)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/42")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.100003 93.024627) (xy 127.104954 92.870023) (xy 127.119613 92.741571) (xy 127.140481 92.645492)
				(xy 127.168541 92.562404) (xy 127.245296 92.421184) (xy 127.387496 92.243449) (xy 127.516083 92.089006)
				(xy 127.665179 91.884455) (xy 127.000003 91.438999) (xy 126.334827 91.884455) (xy 126.518097 92.131417)
				(xy 126.61251 92.24345) (xy 126.734914 92.393276) (xy 126.784186 92.467321) (xy 126.82513 92.547313)
				(xy 126.857465 92.638145) (xy 126.88091 92.744713) (xy 126.895183 92.871908) (xy 126.900003 93.024627)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/22")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.211978 101.963698) (xy 152.125573 101.86149) (xy 152.088622 101.794962) (xy 152.072364 101.725944)
				(xy 152.085222 101.66738) (xy 151.673587 101.566729) (xy 151.774238 101.978364) (xy 151.838068 101.96574)
				(xy 151.915306 101.987797) (xy 152.009521 102.049613) (xy 152.070556 102.10512)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/31")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.545073 94.029395) (xy 147.44286 94.115804) (xy 147.37633 94.152754) (xy 147.307309 94.16901)
				(xy 147.248755 94.156151) (xy 147.148104 94.567786) (xy 147.559739 94.467135) (xy 147.547115 94.403305)
				(xy 147.569172 94.326068) (xy 147.630988 94.231853) (xy 147.686495 94.170817)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.317877 104.933547) (xy 140.420081 104.847145) (xy 140.486606 104.810194) (xy 140.555622 104.793933)
				(xy 140.614195 104.806791) (xy 140.714846 104.395156) (xy 140.303211 104.495807) (xy 140.315836 104.559637)
				(xy 140.293779 104.636874) (xy 140.231963 104.731088) (xy 140.176455 104.792125)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.449248 106.064918) (xy 141.551452 105.978516) (xy 141.617977 105.941565) (xy 141.686993 105.925304)
				(xy 141.745566 105.938162) (xy 141.846217 105.526527) (xy 141.434582 105.627178) (xy 141.447207 105.691008)
				(xy 141.42515 105.768245) (xy 141.363334 105.862459) (xy 141.307826 105.923496)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VPP)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.938975 97.780397) (xy 125.009338 97.857665) (xy 125.062571 97.930951) (xy 125.098476 97.99682)
				(xy 125.122056 98.060285) (xy 125.137721 98.182046) (xy 125.117375 98.312921) (xy 125.047618 98.506038)
				(xy 124.991013 98.653013) (xy 124.945127 98.816396) (xy 124.924926 99.002109) (xy 124.929134 99.105189)
				(xy 124.945375 99.216071) (xy 125.73071 99.060706) (xy 126.174459 98.394823) (xy 125.839463 98.188718)
				(xy 125.721315 98.123815) (xy 125.577426 98.043613) (xy 125.436912 97.952385) (xy 125.278371 97.825662)
				(xy 125.080397 97.638975)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/1{slash}TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.394631 101.61) (xy 132.259638 101.605098) (xy 132.145343 101.590787) (xy 132.05546 101.569757)
				(xy 131.977849 101.541687) (xy 131.84863 101.465853) (xy 131.719582 101.348664) (xy 131.666227 101.292981)
				(xy 131.496554 101.123813) (xy 131.387417 101.031279) (xy 131.254459 100.934823) (xy 130.809003 101.599999)
				(xy 130.966075 102.384627) (xy 131.096901 102.353753) (xy 131.2106 102.317569) (xy 131.404473 102.228731)
				(xy 131.579401 102.113025) (xy 131.634482 102.071492) (xy 131.771168 101.972584) (xy 131.926488 101.889146)
				(xy 132.019073 101.856457) (xy 132.125842 101.831508) (xy 132.24997 101.815592) (xy 132.394631 101.81)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.25218 105.923496) (xy 148.165775 105.821288) (xy 148.128824 105.75476) (xy 148.112566 105.685742)
				(xy 148.125424 105.627178) (xy 147.713789 105.526527) (xy 147.81444 105.938162) (xy 147.87827 105.925538)
				(xy 147.955508 105.947595) (xy 148.049723 106.009411) (xy 148.110758 106.064918)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/39{slash}GCLR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.176508 95.917399) (xy 140.246871 95.976842) (xy 140.281643 96.01822) (xy 140.306996 96.064871)
				(xy 140.315817 96.103718) (xy 140.311474 96.143745) (xy 140.303211 96.164191) (xy 140.715005 96.264634)
				(xy 140.590747 95.848543) (xy 140.531478 95.863457) (xy 140.450232 95.845606) (xy 140.340718 95.787888)
				(xy 140.280924 95.7473) (xy 140.276502 95.744192)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/32{slash}TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.936529 93.50595) (xy 146.860873 93.568834) (xy 146.810331 93.594704) (xy 146.754598 93.606494)
				(xy 146.719062 93.60344) (xy 146.683069 93.590465) (xy 146.582538 94.002202) (xy 146.994053 93.901449)
				(xy 146.97974 93.834578) (xy 147.000018 93.757792) (xy 147.057371 93.669012) (xy 147.098333 93.623502)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/27")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.807814 96.292136) (xy 149.705601 96.378545) (xy 149.639071 96.415495) (xy 149.57005 96.431751)
				(xy 149.511496 96.418892) (xy 149.410845 96.830527) (xy 149.82248 96.729876) (xy 149.809856 96.666046)
				(xy 149.831913 96.588809) (xy 149.893729 96.494594) (xy 149.949236 96.433558)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/18")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.679474 108.239524) (xy 153.770544 108.337424) (xy 153.842843 108.429248) (xy 153.898059 108.514673)
				(xy 153.939818 108.596157) (xy 153.994451 108.760071) (xy 154.027198 108.965046) (xy 154.0482 109.114439)
				(xy 154.085864 109.276436) (xy 154.156101 109.457591) (xy 154.274825 109.664455) (xy 154.940708 109.220706)
				(xy 155.096073 108.435371) (xy 154.83023 108.399461) (xy 154.560458 108.394676) (xy 154.37685 108.392504)
				(xy 154.291057 108.382334) (xy 154.205894 108.361356) (xy 154.118828 108.326007) (xy 154.027328 108.272724)
				(xy 153.928862 108.197943) (xy 153.820896 108.098102)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.28 105.249236) (xy 143.279729 105.155273) (xy 143.284608 104.95258) (xy 143.324236 104.713527)
				(xy 143.03 104.654) (xy 142.735764 104.713527) (xy 142.775392 104.952582) (xy 142.780271 105.15528)
				(xy 142.78 105.249236)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/23")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.050213 92.631211) (xy 164.163035 92.52539) (xy 164.26423 92.444926) (xy 164.346924 92.391744)
				(xy 164.425517 92.352833) (xy 164.579648 92.30725) (xy 164.805877 92.282123) (xy 165.006009 92.26384)
				(xy 165.256075 92.224627) (xy 165.10071 91.439292) (xy 164.315375 91.283927) (xy 164.270337 91.588147)
				(xy 164.257879 91.734126) (xy 164.238487 91.926621) (xy 164.22097 92.013819) (xy 164.193359 92.099334)
				(xy 164.151995 92.186427) (xy 164.093219 92.278359) (xy 164.013371 92.378392) (xy 163.908791 92.489789)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.199147 102.908772) (xy 148.132898 102.975404) (xy 147.986122 103.11528) (xy 147.789065 103.256295)
				(xy 147.955029 103.506443) (xy 148.205177 103.672407) (xy 148.346192 103.475348) (xy 148.48607 103.328571)
				(xy 148.5527 103.262325)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/28")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.908904 92.608228) (xy 154.067107 92.499475) (xy 154.199823 92.421698) (xy 154.298325 92.375567)
				(xy 154.390336 92.343109) (xy 154.585231 92.302713) (xy 154.694997 92.288009) (xy 154.872591 92.263685)
				(xy 155.096075 92.224627) (xy 154.940811 91.439412) (xy 154.155375 91.283927) (xy 154.122557 91.533289)
				(xy 154.117676 91.769949) (xy 154.113651 91.95409) (xy 154.101903 92.037685) (xy 154.078516 92.118146)
				(xy 154.039628 92.197363) (xy 153.981378 92.277223) (xy 153.899904 92.359616) (xy 153.791344 92.44643)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/32{slash}TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.709446 95.309133) (xy 144.649908 95.362069) (xy 144.598098 95.395954) (xy 144.491697 95.434164)
				(xy 144.403765 95.461674) (xy 144.291107 95.522133) (xy 144.429293 95.730707) (xy 144.637867 95.868893)
				(xy 144.703876 95.741662) (xy 144.725835 95.668304) (xy 144.76047 95.568736) (xy 144.795002 95.513941)
				(xy 144.850867 95.450554)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/35{slash}GCLK3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.439197 93.605131) (xy 142.525602 93.707339) (xy 142.562553 93.773867) (xy 142.578812 93.842885)
				(xy 142.565953 93.901449) (xy 142.977588 94.0021) (xy 142.876937 93.590465) (xy 142.813107 93.60309)
				(xy 142.735871 93.581033) (xy 142.641656 93.519217) (xy 142.580619 93.463709)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/1{slash}TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.969792 108.028788) (xy 122.85697 108.134608) (xy 122.755775 108.215072) (xy 122.673081 108.268253)
				(xy 122.594488 108.307165) (xy 122.440356 108.352748) (xy 122.214129 108.377875) (xy 122.013996 108.396158)
				(xy 121.763929 108.435371) (xy 121.919294 109.220706) (xy 122.704629 109.376071) (xy 122.749666 109.071849)
				(xy 122.762124 108.925876) (xy 122.781515 108.733379) (xy 122.799033 108.64618) (xy 122.826644 108.560666)
				(xy 122.868008 108.473573) (xy 122.926785 108.381641) (xy 123.006634 108.281607) (xy 123.111214 108.17021)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/5{slash}PD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.752192 104.367862) (xy 139.854396 104.28146) (xy 139.920921 104.244509) (xy 139.989937 104.228248)
				(xy 140.04851 104.241106) (xy 140.149161 103.829471) (xy 139.737526 103.930122) (xy 139.750151 103.993952)
				(xy 139.728094 104.071189) (xy 139.666278 104.165403) (xy 139.61077 104.22644)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/31")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.058578 92.798734) (xy 149.175076 92.689029) (xy 149.280035 92.60334) (xy 149.374111 92.538616)
				(xy 149.462034 92.488845) (xy 149.647891 92.411571) (xy 149.718062 92.387687) (xy 149.973045 92.291321)
				(xy 150.126135 92.214506) (xy 150.304459 92.105175) (xy 149.86071 91.439292) (xy 149.075375 91.283927)
				(xy 149.050259 91.501733) (xy 149.061198 91.706241) (xy 149.105125 91.932238) (xy 149.1402 92.109028)
				(xy 149.146567 92.194013) (xy 149.140502 92.27914) (xy 149.118267 92.366221) (xy 149.076123 92.457069)
				(xy 149.010333 92.553495) (xy 148.917156 92.657312)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/25")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.939183 97.423506) (xy 150.836966 97.509918) (xy 150.770433 97.546868) (xy 150.701411 97.563122)
				(xy 150.642867 97.550263) (xy 150.542216 97.961898) (xy 150.953851 97.861247) (xy 150.941226 97.797416)
				(xy 150.963283 97.720179) (xy 151.025098 97.625964) (xy 151.080605 97.564928)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.049792 108.028787) (xy 127.936969 108.134607) (xy 127.835775 108.215072) (xy 127.75308 108.268253)
				(xy 127.674487 108.307164) (xy 127.520356 108.352747) (xy 127.294128 108.377875) (xy 127.093996 108.396158)
				(xy 126.843929 108.435371) (xy 126.999294 109.220706) (xy 127.784629 109.376071) (xy 127.829666 109.071849)
				(xy 127.842125 108.925874) (xy 127.861516 108.733378) (xy 127.879033 108.646179) (xy 127.906644 108.560664)
				(xy 127.948008 108.473572) (xy 128.006785 108.381639) (xy 128.086634 108.281606) (xy 128.191214 108.170209)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/26{slash}TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.411204 97.800071) (xy 149.462596 97.786828) (xy 149.620321 97.752536) (xy 149.693831 97.752261)
				(xy 149.747046 97.775971) (xy 149.978231 97.395395) (xy 149.839114 97.21034) (xy 149.747132 97.354881)
				(xy 149.62604 97.477351) (xy 149.488101 97.565811) (xy 149.388816 97.601329)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/35{slash}GCLK3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.121027 92.004117) (xy 140.928917 91.804853) (xy 140.796729 91.650867) (xy 140.637744 91.42276)
				(xy 140.584049 91.336816) (xy 140.365179 90.995543) (xy 139.699296 91.439292) (xy 139.856075 92.224627)
				(xy 140.071339 92.164751) (xy 140.302599 92.067604) (xy 140.474475 91.994955) (xy 140.554471 91.972718)
				(xy 140.633325 91.964643) (xy 140.713151 91.97431) (xy 140.796064 92.005296) (xy 140.884177 92.061179)
				(xy 140.979605 92.145539)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VPP)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.903977 94.53) (xy 138.837408 94.525192) (xy 138.788065 94.511538) (xy 138.72352 94.466691)
				(xy 138.692902 94.433729) (xy 138.642401 94.380666) (xy 138.568893 94.322133) (xy 138.429 94.53)
				(xy 138.478773 94.775196) (xy 138.519046 94.767157) (xy 138.700817 94.735779) (xy 138.903977 94.73)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.129791 108.028787) (xy 133.016968 108.134607) (xy 132.915774 108.215072) (xy 132.833079 108.268253)
				(xy 132.754486 108.307164) (xy 132.600355 108.352747) (xy 132.374128 108.377875) (xy 132.173995 108.396158)
				(xy 131.923929 108.435371) (xy 132.079294 109.220706) (xy 132.864629 109.376071) (xy 132.909666 109.07185)
				(xy 132.922125 108.925873) (xy 132.941516 108.733377) (xy 132.959033 108.646179) (xy 132.986644 108.560664)
				(xy 133.028008 108.473571) (xy 133.086784 108.381639) (xy 133.166633 108.281606) (xy 133.271213 108.170209)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VPP)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.750867 97.309446) (xy 124.69793 97.249908) (xy 124.664045 97.198098) (xy 124.625835 97.091696)
				(xy 124.598326 97.003765) (xy 124.537867 96.891107) (xy 124.329293 97.029293) (xy 124.191107 97.237867)
				(xy 124.318338 97.303876) (xy 124.391696 97.325835) (xy 124.491264 97.360471) (xy 124.546059 97.395002)
				(xy 124.609446 97.450867)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.974089 100.314464) (xy 147.167806 100.139862) (xy 147.288119 100.030911) (xy 147.35225 99.955046)
				(xy 147.429441 99.846671) (xy 147.180707 99.679293) (xy 146.930559 99.513329) (xy 146.819815 99.698054)
				(xy 146.749232 99.814693) (xy 146.620536 99.960911)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/26{slash}TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.862121 95.771828) (xy 145.665538 95.647003) (xy 145.468893 95.522133) (xy 145.329169 95.729445)
				(xy 145.378773 95.975196) (xy 145.497504 95.937237) (xy 145.524452 95.925285) (xy 145.576842 95.903499)
				(xy 145.627167 95.893407) (xy 145.682775 95.902463) (xy 145.751015 95.938125)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/30")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.372157 92.609236) (xy 151.485664 92.507093) (xy 151.58703 92.429997) (xy 151.669813 92.379367)
				(xy 151.748228 92.342807) (xy 151.902795 92.30093) (xy 152.108035 92.280337) (xy 152.306527 92.263288)
				(xy 152.556075 92.224627) (xy 152.400724 91.439307) (xy 151.615375 91.283927) (xy 151.574726 91.568445)
				(xy 151.563259 91.74269) (xy 151.548989 91.927025) (xy 151.533738 92.011124) (xy 151.508319 92.093646)
				(xy 151.469166 92.177441) (xy 151.412712 92.26536) (xy 151.33539 92.360256) (xy 151.233633 92.464978)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/38{slash}OE1{slash}Vpp")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.74214 95.302188) (xy 140.828545 95.404396) (xy 140.865496 95.470924) (xy 140.881755 95.539942)
				(xy 140.868896 95.598506) (xy 141.280531 95.699157) (xy 141.17988 95.287522) (xy 141.11605 95.300147)
				(xy 141.038814 95.27809) (xy 140.944599 95.216274) (xy 140.883562 95.160766)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/28")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.242129 95.726451) (xy 149.139916 95.81286) (xy 149.073386 95.84981) (xy 149.004365 95.866066)
				(xy 148.945811 95.853207) (xy 148.84516 96.264842) (xy 149.256795 96.164191) (xy 149.244171 96.100361)
				(xy 149.266228 96.023124) (xy 149.328044 95.928909) (xy 149.383551 95.867873)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/7{slash}TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.830002 103.184627) (xy 125.834953 103.030023) (xy 125.849612 102.901571) (xy 125.87048 102.805492)
				(xy 125.89854 102.722404) (xy 125.975295 102.581185) (xy 126.117495 102.403449) (xy 126.246083 102.249007)
				(xy 126.395179 102.044455) (xy 125.730003 101.598999) (xy 125.064827 102.044455) (xy 125.248097 102.291418)
				(xy 125.34251 102.403449) (xy 125.464913 102.553276) (xy 125.514185 102.627321) (xy 125.555129 102.707313)
				(xy 125.587464 102.798145) (xy 125.610909 102.904713) (xy 125.625182 103.031909) (xy 125.630002 103.184627)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(LED2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.785196 96.039) (xy 161.705664 96.034332) (xy 161.645069 96.021658) (xy 161.542813 95.973439)
				(xy 161.461184 95.930714) (xy 161.338773 95.893804) (xy 161.289 96.139) (xy 161.338773 96.384196)
				(xy 161.475415 96.340905) (xy 161.542813 96.304561) (xy 161.637709 96.258647) (xy 161.700872 96.244319)
				(xy 161.785196 96.239)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(LED1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.785196 104.421) (xy 161.705664 104.416332) (xy 161.645069 104.403658) (xy 161.542813 104.355439)
				(xy 161.461184 104.312714) (xy 161.338773 104.275804) (xy 161.289 104.521) (xy 161.338773 104.766196)
				(xy 161.475415 104.722905) (xy 161.542813 104.686561) (xy 161.637709 104.640647) (xy 161.700872 104.626319)
				(xy 161.785196 104.621)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/20")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.080606 103.09507) (xy 150.994204 102.992866) (xy 150.957254 102.926341) (xy 150.940992 102.857325)
				(xy 150.953851 102.798751) (xy 150.542216 102.6981) (xy 150.642867 103.109735) (xy 150.706697 103.097111)
				(xy 150.783934 103.119168) (xy 150.878148 103.180984) (xy 150.939184 103.236492)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.131454 103.974993) (xy 143.037366 104.075787) (xy 142.976127 104.155691) (xy 142.908163 104.272831)
				(xy 142.780559 104.488329) (xy 143.029293 104.655707) (xy 143.279441 104.821671) (xy 143.317226 104.756848)
				(xy 143.34097 104.699398) (xy 143.364939 104.579582) (xy 143.373428 104.521591) (xy 143.390388 104.462837)
				(xy 143.424641 104.399696) (xy 143.485007 104.328546)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/21")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.646293 102.529383) (xy 151.559888 102.427175) (xy 151.522937 102.360647) (xy 151.506679 102.291629)
				(xy 151.519537 102.233065) (xy 151.107902 102.132414) (xy 151.208553 102.544049) (xy 151.272383 102.531425)
				(xy 151.349621 102.553482) (xy 151.443836 102.615298) (xy 151.504871 102.670805)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.826458 107.798976) (xy 142.642647 107.975794) (xy 142.497108 108.100664) (xy 142.277757 108.253256)
				(xy 142.173965 108.316291) (xy 141.795545 108.554823) (xy 142.239294 109.220706) (xy 143.024629 109.063927)
				(xy 142.963609 108.841778) (xy 142.878352 108.628828) (xy 142.808662 108.45302) (xy 142.787894 108.371541)
				(xy 142.781278 108.29141) (xy 142.792393 108.210431) (xy 142.824813 108.126402) (xy 142.882116 108.037123)
				(xy 142.967879 107.940397)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/40{slash}OE2{slash}GCLK2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.528991 96.515813) (xy 139.597758 96.574909) (xy 139.707284 96.671403) (xy 139.746715 96.720743)
				(xy 139.762303 96.766958) (xy 140.149161 96.830527) (xy 139.960712 96.419103) (xy 139.928913 96.442527)
				(xy 139.895463 96.455937) (xy 139.821339 96.457317) (xy 139.737161 96.424671) (xy 139.670413 96.374391)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/42")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.479399 97.564929) (xy 138.565804 97.667137) (xy 138.602755 97.733665) (xy 138.619014 97.802683)
				(xy 138.606155 97.861247) (xy 139.01779 97.961898) (xy 138.917139 97.550263) (xy 138.853309 97.562888)
				(xy 138.776073 97.540831) (xy 138.681858 97.479015) (xy 138.620821 97.423507)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/33")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.854014 92.95457) (xy 145.892459 93.020916) (xy 145.901105 93.066369) (xy 145.900339 93.117226)
				(xy 145.889081 93.172268) (xy 145.866277 93.229978) (xy 145.832312 93.286947) (xy 145.785665 93.343863)
				(xy 145.772873 93.356985) (xy 146.018147 93.436415) (xy 146.179543 93.019743) (xy 146.1493 93.009542)
				(xy 146.094499 92.94802) (xy 146.056577 92.894243) (xy 145.995436 92.813148)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(LED2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.9175 96.239) (xy 162.038401 96.258563) (xy 162.117676 96.286609) (xy 162.197426 96.326315)
				(xy 162.265192 96.371805) (xy 162.324598 96.426058) (xy 162.364127 96.476783) (xy 162.392975 96.532953)
				(xy 162.411216 96.6265) (xy 162.8935 96.139) (xy 162.411216 95.6515) (xy 162.391414 95.748995) (xy 162.334651 95.84061)
				(xy 162.23793 95.9261) (xy 162.102815 95.99747) (xy 161.955179 96.036639) (xy 161.9175 96.039)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/7{slash}TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.883562 105.499232) (xy 140.985766 105.41283) (xy 141.052291 105.375879) (xy 141.121307 105.359618)
				(xy 141.17988 105.372476) (xy 141.280531 104.960841) (xy 140.868896 105.061492) (xy 140.881521 105.125322)
				(xy 140.859464 105.202559) (xy 140.797648 105.296773) (xy 140.74214 105.35781)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/19{slash}PD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.514922 103.660754) (xy 150.428517 103.558546) (xy 150.391566 103.492018) (xy 150.375308 103.423)
				(xy 150.388166 103.364436) (xy 149.976531 103.263785) (xy 150.077182 103.67542) (xy 150.141012 103.662796)
				(xy 150.21825 103.684853) (xy 150.312465 103.746669) (xy 150.3735 103.802176)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/40{slash}OE2{slash}GCLK2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.731215 92.489789) (xy 130.625394 92.376966) (xy 130.54493 92.275772) (xy 130.491748 92.193077)
				(xy 130.452837 92.114484) (xy 130.407254 91.960353) (xy 130.382127 91.734125) (xy 130.363844 91.533993)
				(xy 130.324631 91.283927) (xy 129.539296 91.439292) (xy 129.383931 92.224627) (xy 129.688152 92.269664)
				(xy 129.834129 92.282123) (xy 130.026624 92.301514) (xy 130.113823 92.319031) (xy 130.199337 92.346642)
				(xy 130.28643 92.388006) (xy 130.378363 92.446782) (xy 130.478396 92.526631) (xy 130.589793 92.631211)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.3)
			(smoothing fillet)
			(radius 0.1)
		)
		(polygon
			(pts
				(xy 115.57 90.17) (xy 166.369998 90.17) (xy 166.369999 110.49) (xy 115.569999 110.49)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.174236 99.945) (xy 147.2009 99.940271) (xy 147.211856 99.927169) (xy 147.201263 99.891657)
				(xy 147.136518 99.819665) (xy 147.000849 99.723128) (xy 146.943226 99.697993) (xy 146.901299 99.694791)
				(xy 146.888465 99.704463) (xy 146.884045 99.72342) (xy 146.885764 99.738527) (xy 147.181 99.68)
				(xy 146.885764 99.738527) (xy 146.896078 99.765873) (xy 146.91293 99.781577) (xy 146.957476 99.784102)
				(xy 147.030798 99.747601) (xy 147.134632 99.653904) (xy 147.183976 99.591087) (xy 147.217153 99.531297)
				(xy 147.227306 99.492595) (xy 147.221092 99.463444) (xy 147.206695 99.451145) (xy 147.183123 99.445336)
				(xy 147.174236 99.445)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.539637 104.34319) (xy 142.596361 104.406547) (xy 142.633836 104.462169) (xy 142.673709 104.563898)
				(xy 142.680948 104.591822) (xy 142.711723 104.692679) (xy 142.780559 104.821671) (xy 143.030707 104.655707)
				(xy 143.279441 104.488329) (xy 143.1905 104.352704) (xy 143.07375 104.184392) (xy 142.89319 103.989637)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.596545 100.567009) (xy 122.855918 100.311216) (xy 123.043952 100.141175) (xy 123.228813 99.999597)
				(xy 123.478665 99.829194) (xy 123.553538 99.779202) (xy 123.634459 99.725175) (xy 123.19071 99.059292)
				(xy 122.405375 98.903927) (xy 122.380772 99.11868) (xy 122.391887 99.320335) (xy 122.428954 99.519231)
				(xy 122.460342 99.688601) (xy 122.465464 99.769936) (xy 122.458792 99.851384) (xy 122.436767 99.934701)
				(xy 122.395831 100.021646) (xy 122.332426 100.113978) (xy 122.242991 100.213455)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/32{slash}TDO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 123.707603 100.178975) (xy 123.44553 100.432492) (xy 123.253725 100.592697) (xy 122.965989 100.789155)
				(xy 122.745547 100.934823) (xy 123.189296 101.600706) (xy 123.974631 101.443927) (xy 123.916828 101.240993)
				(xy 123.825347 101.036286) (xy 123.794556 100.976356) (xy 123.715492 100.811696) (xy 123.690144 100.734472)
				(xy 123.679045 100.658018) (xy 123.685789 100.580359) (xy 123.713971 100.49952) (xy 123.767185 100.413524)
				(xy 123.849025 100.320397)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(LED2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.794804 96.239) (xy 160.874336 96.243668) (xy 160.934931 96.256342) (xy 161.037187 96.304561)
				(xy 161.118815 96.347285) (xy 161.241227 96.384196) (xy 161.291 96.139) (xy 161.241227 95.893804)
				(xy 161.104585 95.937094) (xy 161.037186 95.973439) (xy 160.94229 96.019353) (xy 160.879128 96.033681)
				(xy 160.794804 96.039)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(LED2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.003 96.039) (xy 158.880841 96.018337) (xy 158.810297 95.991182) (xy 158.74457 95.952108)
				(xy 158.702993 95.91444) (xy 158.672051 95.869471) (xy 158.657992 95.831343) (xy 158.653 95.789)
				(xy 158.302 96.139) (xy 158.653 96.489) (xy 158.671279 96.410081) (xy 158.724712 96.341997) (xy 158.816266 96.284032)
				(xy 158.940188 96.245284) (xy 159.003 96.239)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.635764 94.23) (xy 127.729727 94.229729) (xy 127.93242 94.234608) (xy 128.171473 94.274236)
				(xy 128.231 93.98) (xy 128.171473 93.685764) (xy 127.932418 93.725392) (xy 127.72972 93.730271)
				(xy 127.635764 93.73)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.785764 103.331472) (xy 147.879727 103.331201) (xy 148.08242 103.33608) (xy 148.321473 103.375708)
				(xy 148.381 103.081472) (xy 148.321473 102.787236) (xy 148.082418 102.826864) (xy 147.87972 102.831743)
				(xy 147.785764 102.831472)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/32{slash}TDO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.98324 95.68) (xy 144.039218 95.68478) (xy 144.080934 95.698239) (xy 144.133251 95.742471)
				(xy 144.165174 95.793212) (xy 144.2118 95.865144) (xy 144.291107 95.937867) (xy 144.431 95.73) (xy 144.478773 95.484804)
				(xy 144.359987 95.465977) (xy 144.274257 95.462144) (xy 144.182995 95.468963) (xy 143.98324 95.48)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.174236 99.445) (xy 146.925408 99.43745) (xy 146.712773 99.400661) (xy 146.638527 99.385764)
				(xy 146.579 99.68) (xy 146.638527 99.974236) (xy 146.803533 99.946614) (xy 146.917669 99.939923)
				(xy 147.002422 99.941825) (xy 147.174236 99.945)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.819911 99.079536) (xy 146.729708 99.170992) (xy 146.599702 99.295995) (xy 146.413329 99.430559)
				(xy 146.579293 99.680707) (xy 146.829441 99.846671) (xy 146.978536 99.636495) (xy 147.141799 99.464722)
				(xy 147.173464 99.433089)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(LED1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.794804 104.621) (xy 160.874336 104.625668) (xy 160.934931 104.638342) (xy 161.037187 104.686561)
				(xy 161.118815 104.729285) (xy 161.241227 104.766196) (xy 161.291 104.521) (xy 161.241227 104.275804)
				(xy 161.104585 104.319094) (xy 161.037186 104.355439) (xy 160.94229 104.401353) (xy 160.879128 104.415681)
				(xy 160.794804 104.421)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.829818 97.191128) (xy 147.834562 97.047476) (xy 147.847773 96.940128) (xy 147.894545 96.767886)
				(xy 147.931865 96.646882) (xy 147.972132 96.47685) (xy 147.579818 96.397814) (xy 147.187504 96.47685)
				(xy 147.250705 96.723386) (xy 147.265091 96.767888) (xy 147.31153 96.93828) (xy 147.324983 97.046273)
				(xy 147.329818 97.191128)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.078474 107.579362) (xy 116.942819 107.786551) (xy 116.828611 107.945032) (xy 116.615239 108.202326)
				(xy 116.424941 108.428428) (xy 116.174825 108.775543) (xy 116.839469 109.220845) (xy 117.624629 109.063927)
				(xy 117.560499 108.826885) (xy 117.464408 108.589777) (xy 117.394762 108.419486) (xy 117.372382 108.338166)
				(xy 117.362195 108.255248) (xy 117.367123 108.167622) (xy 117.390089 108.072177) (xy 117.434017 107.965803)
				(xy 117.501829 107.845388)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/26{slash}TCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.477313 100.341265) (xy 121.400767 100.44946) (xy 121.277635 100.554277) (xy 121.101792 100.651278)
				(xy 120.872535 100.73187) (xy 120.599767 100.78508) (xy 120.453638 100.798252) (xy 120.304973 100.801396)
				(xy 120.251756 100.799999) (xy 120.649296 101.600706) (xy 121.450003 101.868152) (xy 121.428923 101.523051)
				(xy 121.445484 101.163905) (xy 121.467922 100.992496) (xy 121.499224 100.831427) (xy 121.536571 100.691336)
				(xy 121.581078 100.565629) (xy 121.618735 100.482687)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.829818 97.423814) (xy 147.827158 97.357735) (xy 147.823355 97.241918) (xy 147.835036 97.121595)
				(xy 147.852065 97.068103) (xy 147.879421 97.023515) (xy 147.919258 96.991176) (xy 147.973728 96.974429)
				(xy 147.579818 96.397814) (xy 147.185908 96.974429) (xy 147.225266 96.984203) (xy 147.257296 97.001939)
				(xy 147.303193 97.058762) (xy 147.329969 97.151012) (xy 147.335645 97.290551) (xy 147.332478 97.357735)
				(xy 147.329818 97.423814)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.339925 103.54239) (xy 156.320179 103.655855) (xy 156.293261 103.722701) (xy 156.25452 103.786141)
				(xy 156.214894 103.829945) (xy 156.167363 103.864071) (xy 156.124001 103.882029) (xy 156.075493 103.890173)
				(xy 156.403156 104.521987) (xy 156.747672 103.914212) (xy 156.680929 103.886319) (xy 156.622263 103.821067)
				(xy 156.572142 103.710835) (xy 156.540663 103.562977) (xy 156.537461 103.511096)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(LED1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.003 104.421) (xy 158.880841 104.400337) (xy 158.810297 104.373182) (xy 158.74457 104.334108)
				(xy 158.702993 104.29644) (xy 158.672051 104.251471) (xy 158.657992 104.213343) (xy 158.653 104.171)
				(xy 158.302 104.521) (xy 158.653 104.871) (xy 158.671279 104.792081) (xy 158.724712 104.723997)
				(xy 158.816266 104.666032) (xy 158.940188 104.627284) (xy 159.003 104.621)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.131212 102.64979) (xy 156.025391 102.536967) (xy 155.944927 102.435773) (xy 155.891745 102.353078)
				(xy 155.852834 102.274485) (xy 155.807251 102.120354) (xy 155.782124 101.894126) (xy 155.763841 101.693994)
				(xy 155.724628 101.443928) (xy 154.939293 101.599293) (xy 154.783928 102.384628) (xy 155.088149 102.429665)
				(xy 155.234126 102.442124) (xy 155.426621 102.461515) (xy 155.51382 102.479032) (xy 155.599334 102.506643)
				(xy 155.686427 102.548007) (xy 155.77836 102.606783) (xy 155.878393 102.686632) (xy 155.98979 102.791212)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.913584 92.541028) (xy 117.826853 92.447378) (xy 117.760518 92.360894) (xy 117.714985 92.285631)
				(xy 117.682763 92.213805) (xy 117.649943 92.073958) (xy 117.647296 91.906658) (xy 117.651576 91.831761)
				(xy 117.658837 91.590998) (xy 117.649656 91.447514) (xy 117.624631 91.283927) (xy 116.839296 91.439292)
				(xy 116.395547 92.105175) (xy 116.728552 92.309256) (xy 116.889054 92.395109) (xy 117.039149 92.475959)
				(xy 117.18695 92.569523) (xy 117.353548 92.700748) (xy 117.56003 92.894582)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/26{slash}TCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.909133 95.450554) (xy 144.962069 95.510092) (xy 144.995954 95.561901) (xy 145.034164 95.668303)
				(xy 145.061674 95.756234) (xy 145.122133 95.868893) (xy 145.330707 95.730707) (xy 145.468893 95.522133)
				(xy 145.341662 95.456123) (xy 145.268303 95.434164) (xy 145.168735 95.399529) (xy 145.113941 95.364998)
				(xy 145.050554 95.309133)
			)
		)
	)
	(zone
		(net 41)
		(net_name "VCCIO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.500368 101.38) (xy 153.605664 101.384878) (xy 153.695519 101.399028) (xy 153.767575 101.42014)
				(xy 153.829139 101.448199) (xy 153.927421 101.523253) (xy 154.010262 101.632396) (xy 154.083463 101.766064)
				(xy 154.149489 101.888987) (xy 154.232202 102.016303) (xy 154.343566 102.143278) (xy 154.495544 102.265176)
				(xy 154.941 101.6) (xy 154.783928 100.815372) (xy 154.517751 100.86321) (xy 154.318682 100.887449)
				(xy 154.043203 100.893216) (xy 153.928025 100.889209) (xy 153.500368 100.88)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.199147 102.908772) (xy 148.132898 102.975404) (xy 147.986122 103.11528) (xy 147.789065 103.256295)
				(xy 147.955029 103.506443) (xy 148.205177 103.672407) (xy 148.346192 103.475348) (xy 148.48607 103.328571)
				(xy 148.5527 103.262325)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VPP)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.956023 94.73) (xy 138.159182 94.735779) (xy 138.340954 94.767157) (xy 138.381227 94.775196)
				(xy 138.431 94.53) (xy 138.291107 94.322133) (xy 138.193597 94.404716) (xy 138.167097 94.433729)
				(xy 138.130245 94.472731) (xy 138.08935 94.503162) (xy 138.03456 94.522944) (xy 137.956023 94.53)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/7{slash}TMS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.150867 105.816446) (xy 126.09793 105.756908) (xy 126.064045 105.705098) (xy 126.025835 105.598696)
				(xy 125.998326 105.510765) (xy 125.937867 105.398107) (xy 125.729293 105.536293) (xy 125.591107 105.744867)
				(xy 125.718338 105.810876) (xy 125.791696 105.832835) (xy 125.891264 105.867471) (xy 125.946059 105.902002)
				(xy 126.009446 105.957867)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.480702 103.331472) (xy 147.538252 103.336649) (xy 147.598942 103.352885) (xy 147.656499 103.379241)
				(xy 147.712082 103.417234) (xy 147.758416 103.462) (xy 147.799625 103.517506) (xy 147.831604 103.57868)
				(xy 147.856512 103.650008) (xy 147.872536 103.728346) (xy 147.87972 103.816908) (xy 147.88 103.84009)
				(xy 148.281 103.63) (xy 148.07665 103.005) (xy 148.020429 103.007351) (xy 147.901122 102.972617)
				(xy 147.781834 102.925057) (xy 147.61692 102.861019) (xy 147.543064 102.839627) (xy 147.480702 102.831472)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.136589 103.678436) (xy 148.202835 103.611806) (xy 148.349612 103.471928) (xy 148.546671 103.330913)
				(xy 148.380707 103.080765) (xy 148.130559 102.914801) (xy 147.989544 103.111858) (xy 147.849668 103.258634)
				(xy 147.783036 103.324883)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.537495 97.148907) (xy 156.543099 97.077371) (xy 156.560196 96.99041) (xy 156.587282 96.907679)
				(xy 156.626321 96.832738) (xy 156.661039 96.790551) (xy 156.702391 96.760317) (xy 156.747672 96.745788)
				(xy 156.403156 96.138013) (xy 156.075514 96.769841) (xy 156.161067 96.792618) (xy 156.23486 96.850033)
				(xy 156.296201 96.943313) (xy 156.334893 97.063473) (xy 156.339959 97.117613)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/7{slash}TMS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.428789 108.170209) (xy 133.534609 108.283031) (xy 133.615074 108.384226) (xy 133.668255 108.46692)
				(xy 133.707166 108.545513) (xy 133.752749 108.699644) (xy 133.777877 108.925872) (xy 133.79616 109.126004)
				(xy 133.835373 109.376071) (xy 134.620708 109.220706) (xy 134.776073 108.435371) (xy 134.471852 108.390333)
				(xy 134.325874 108.377875) (xy 134.133378 108.358484) (xy 134.04618 108.340966) (xy 133.960665 108.313355)
				(xy 133.873573 108.271991) (xy 133.781641 108.213215) (xy 133.681607 108.133367) (xy 133.570211 108.028787)
			)
		)
	)
	(zone
		(net 42)
		(net_name "VCCINT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.98979 97.868788) (xy 155.876967 97.974608) (xy 155.775773 98.055073) (xy 155.693078 98.108254)
				(xy 155.614485 98.147165) (xy 155.460354 98.192748) (xy 155.234127 98.217876) (xy 155.033994 98.236159)
				(xy 154.783928 98.275372) (xy 154.939293 99.060707) (xy 155.724628 99.216072) (xy 155.769665 98.911851)
				(xy 155.782124 98.765874) (xy 155.801515 98.573378) (xy 155.819032 98.48618) (xy 155.846643 98.400665)
				(xy 155.888007 98.313572) (xy 155.946783 98.22164) (xy 156.026632 98.121607) (xy 156.131212 98.01021)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VPP)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.609446 96.609133) (xy 124.549908 96.662069) (xy 124.498098 96.695954) (xy 124.391697 96.734164)
				(xy 124.303765 96.761674) (xy 124.191107 96.822133) (xy 124.329293 97.030707) (xy 124.537867 97.168893)
				(xy 124.603876 97.041662) (xy 124.625835 96.968304) (xy 124.66047 96.868736) (xy 124.695002 96.813941)
				(xy 124.750867 96.750554)
			)
		)
	)
	(embedded_fonts no)
)
