(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "Net-(D1-Pad1)")
  (net 4 "/AT_CLK")
  (net 5 "/XT_CLK")
  (net 6 "/XT_DATA")
  (net 7 "unconnected-(J1-Pad3)")
  (net 8 "unconnected-(J2-Pad2)")
  (net 9 "/AT_DATA")
  (net 10 "unconnected-(J2-Pad6)")
  (net 11 "unconnected-(SW1-Pad1)")
  (net 12 "Net-(R3-Pad2)")
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 147.6375 92.3925 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text value "47k" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 129.8575 102.872612 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 4.447612 -1.5875 180) (layer "F.SilkS"))
    (fp_text value "47uF" (at 4.447612 1.5875 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 134.9475 106.9875 90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -1.915 -1.915 180) (layer "F.SilkS"))
    (fp_text value "PIC12F629-IP" (at -1.915 5.07 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "VDD") (pintype "power_in"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "/XT_CLK") (pinfunction "GP5") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "/XT_DATA") (pinfunction "GP4") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad2)") (pinfunction "GP3") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/AT_CLK") (pinfunction "GP2") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/AT_DATA") (pinfunction "GP1") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)") (pinfunction "GP0") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE50CD5)
    (at 129.8575 92.3925)
    (descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 0.9525 -4.1275 90) (layer "F.SilkS"))
    (fp_text user "K" (at -0.9525 -1.8) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 4.11 0) (layer "F.Fab"))
    (fp_text user "K" (at 0 -1.8) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/AT_CLK") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 147.955 88.265 90)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 3.4925 90) (layer "F.Fab"))
    (fp_text value "M2" (at 0 4.7625 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "MountingHole:MountingHole_2.2mm_M2_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 129.54 107.315 90)
    (descr "Mounting Hole 2.2mm, M2")
    (tags "mounting hole 2.2mm m2")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.445 90) (layer "F.Fab"))
    (fp_text value "M2" (at 0 -3.175 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 4.4 4.4) (drill 2.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "input"))
  )
  (footprint "Button_Switch_THT:SW_CuK_OS102011MA1QN1_SPDT_Angled" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 147.955 105.1875 90)
    (descr "CuK miniature slide switch, OS series, SPDT, right angle, http://www.ckswitches.com/media/1428/os.pdf")
    (tags "switch SPDT")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at -0.8575 -3.175 90) (layer "F.SilkS"))
    (fp_text value "E0 PASS" (at 4.54 -3.175 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 2.3 1.7 90) (layer "F.Fab"))
    (pad "" thru_hole oval (at -2.1 0 90) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "" thru_hole oval (at 6.1 0 90) (size 2.2 3.5) (drill 1.5) (layers *.Cu *.Mask))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "unconnected-(SW1-Pad1)") (pinfunction "A") (pintype "passive+no_connect"))
    (pad "2" thru_hole oval (at 2 0 90) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(R3-Pad2)") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 4 0 90) (size 1.5 2.5) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_CuK_OS102011MA1QN1_SPDT_Angled.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_Mini_DIN_6pin" (layer "F.Cu")
    (tedit 692DEAF7)
    (at 138.7475 77.29328)
    (descr "Connector, Mini-DIN, 6 pin")
    (tags "MINI DIN CONN 6PIN")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -10.16 10.65422 90) (layer "F.SilkS"))
    (fp_text value "PS/2 KBD" (at -10.16 4.93922 90) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at -1.3 8.5 180) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 "/AT_DATA") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.3 8.5 180) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 "unconnected-(J2-Pad2)") (pintype "passive+no_connect"))
    (pad "3" thru_hole circle (at -3.4 8.5 180) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "4" thru_hole circle (at 3.4 8.5 180) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "5" thru_hole circle (at -3.4 11 180) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask)
      (net 4 "/AT_CLK") (pintype "passive"))
    (pad "6" thru_hole circle (at 3.4 11 180) (size 1.3716 1.3716) (drill 0.889) (layers *.Cu *.Mask)
      (net 10 "unconnected-(J2-Pad6)") (pintype "passive+no_connect"))
    (pad "~" thru_hole circle (at 6.75 5.5 180) (size 4.0005 4.0005) (drill 2.29108) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "~" thru_hole circle (at 0 4.7 180) (size 4.0005 4.0005) (drill 2.29108) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "~" thru_hole circle (at -6.75 5.5 180) (size 4.0005 4.0005) (drill 2.29108) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "r_mini_dins/minidin_6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 147.6375 95.5675 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 3.81 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "/AT_DATA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "My_Components:Conn_DIN_5pin" (layer "F.Cu")
    (tedit 692DEB1B)
    (at 138.7475 128.3675 180)
    (descr "Connector, Mini-DIN, 8 pin")
    (tags "MINI DIN CONN 8PIN")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 10.9855 3.8059 90) (layer "F.SilkS"))
    (fp_text value "XT KBD" (at 11.0363 8.67 270) (layer "F.SilkS"))
    (pad "0" thru_hole circle (at 2.5 2.7) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "0" thru_hole circle (at -2.5 2.7) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "1" thru_hole circle (at -7.5 12.7) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "/XT_CLK") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 12.7) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "/XT_DATA") (pintype "passive"))
    (pad "3" thru_hole circle (at 7.5 12.7) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "unconnected-(J1-Pad3)") (pintype "passive+no_connect"))
    (pad "4" thru_hole circle (at -5 15.2) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "5" thru_hole circle (at 5 15.2) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "~" thru_hole circle (at -7.5 7.7) (size 4 4) (drill 2.4) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (pad "~" thru_hole circle (at 7.5 7.7) (size 4 4) (drill 2.4) (layers *.Cu *.Mask)
      (net 2 "GND"))
    (model "r_mini_dins/minidin_6.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 129.8575 95.5675)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "ps2-xt.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text value "4.7k" (at 3.81 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "/AT_CLK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 149.225 127) (end 128.27 127) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 128.27 127) (mid 127.371974 126.628026) (end 127 125.73) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 149.225 78.105) (mid 150.123026 78.476974) (end 150.495 79.375) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 149.225 78.105) (end 128.27 78.105) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 127 79.375) (mid 127.371974 78.476974) (end 128.27 78.105) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 127 125.73) (end 127 79.375) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 150.495 125.73) (mid 150.123026 126.628026) (end 149.225 127) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150.495 125.73) (end 150.495 79.375) (layer "Edge.Cuts") (width 0.1))
  (gr_text "PCB Design:\n(C) 2025 Sergey Kiselev\n" (at 138.7475 109.855) (layer "B.SilkS"))
  (gr_text "github.com/skiselev/ps2-xt/" (at 136.8425 90.17) (layer "B.SilkS"))
  (gr_text "Firmware:\n(C) 2011 Charles P. Guzis\n{dblquote}Gone, but never forgotten.{dblquote}\n" (at 138.7475 102.87) (layer "B.SilkS"))
  (gr_text "V1.0" (at 138.7475 88.265) (layer "B.SilkS"))
  (gr_text "V1.0" (at 138.7475 97.4725) (layer "F.SilkS"))
  (gr_text "www.malinov.com" (at 149.8092 118.2624 90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.495 78.105)
        (xy 150.495 127)
        (xy 127 127)
        (xy 127 78.105)
      )
    )
  )
)
