(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A3")
  (title_block
    (date "15 nov 2012")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100 100)
    (grid_origin 136.449 102.159)
    (pcbplotparams
      (layerselection 0x0000030_80000001)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 6)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "SDA")
  (net 3 "SCL")
  (net 4 "/GPIO4{slash}GPCLK0")
  (net 5 "/GPIO14{slash}TXD0")
  (net 6 "/GPIO15{slash}RXD0")
  (net 7 "/GPIO17")
  (net 8 "/GPIO18{slash}PCM.CLK")
  (net 9 "/GPIO27")
  (net 10 "/GPIO22")
  (net 11 "/GPIO23")
  (net 12 "/GPIO26")
  (net 13 "/GPIO24")
  (net 14 "MOSI")
  (net 15 "MISO")
  (net 16 "CSZ")
  (net 17 "SCLK")
  (net 18 "/GPIO25")
  (net 19 "/ID_SDA")
  (net 20 "/ID_SCL")
  (net 21 "/GPIO12{slash}PWM0")
  (net 22 "/GPIO16")
  (net 23 "/GPIO20{slash}PCM.DIN")
  (net 24 "/GPIO21{slash}PCM.DOUT")
  (net 25 "+5V")
  (net 26 "+3V3")
  (net 27 "HOST_IRQ")
  (net 28 "PRINT")
  (net 29 "SYS_RDY")
  (net 30 "PROJ_ON")
  (net 31 "SPI_RDY")
  (net 32 "/5V_raw")
  (net 33 "+12V")
  (net 34 "Net-(JP2-B)")
  (footprint "TestPoint:TestPoint_Pad_D1.5mm" (layer "F.Cu")
    (at 125.2984 91.1608)
    (descr "SMD pad as test Point, diameter 1.5mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "test point")
    (property "ki_keywords" "test point tp")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.648) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65) (layer "F.Fab"))
    (pad "1" smd circle (at 0 0) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 33 "+12V") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" locked (layer "F.Cu")
    (at 161.5 73.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH2" (at 0 4) (layer "F.Fab") hide)
    (fp_text value "MountingHole_2.7mm_M2.5" (at 0 3.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "F&B.Cu" "*.Mask")
      (clearance 0.3))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 155.8292 83.7948)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Pin" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal" (layer "F.Cu")
    (at 161.5234 88.8808 90)
    (descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST SH top entry")
    (property "Mouser" "485-4208")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J8" (at 0 -3.98 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 0 3.98 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5 -2 90) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -0.5 -2 90) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at 0.5 -2 90) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at 1.5 -2 90) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "SCL") (pinfunction "Pin_4") (pintype "passive"))
    (pad "MP" smd roundrect (at -2.8 1.875 90) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (pad "MP" smd roundrect (at 2.8 1.875 90) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (model "${KIPRJMOD}/board-assets/PRT-14417--3DModel-STEP-SnapEDA.STEP"
      (offset (xyz 0 1.3 -0.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical" (layer "F.Cu")
    (at 102.7432 78.664)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x01, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J9" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x01_Pin" (at 0 2.33) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_Pico-Clasp_501331-1207_1x12-1MP_P1.00mm_Vertical" (layer "F.Cu")
    (at 149.712 95.627)
    (descr "Molex Pico-Clasp series connector, 501331-1207 (http://www.molex.com/pdm_docs/sd/5013310207_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Pico-Clasp side entry")
    (property "Field5" "")
    (property "Mouser" "538-501331-1207")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x12, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J2" (at 0 -4.52) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x12_Pin" (at 0 3.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.15) (layer "F.Fab"))
    (pad "1" smd roundrect (at -5.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -4.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "MOSI") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -3.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "CSZ") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at -2.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "SCLK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at -1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at -0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "SPI_RDY") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect (at 0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "SCL") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd roundrect (at 1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "SDA") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd roundrect (at 2.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "PROJ_ON") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd roundrect (at 3.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "SYS_RDY") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd roundrect (at 4.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "PRINT") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd roundrect (at 5.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "HOST_IRQ") (pinfunction "Pin_12") (pintype "passive"))
    (pad "MP" smd roundrect (at -6.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (pad "MP" smd roundrect (at 6.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (model "${KIPRJMOD}/board-assets/molex_5013311207.stp"
      (offset (xyz 0 -1.1 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 180 180))
    )
  )
  (footprint "Converter_DCDC:Converter_DCDC_RECOM_R-78E-0.5_THT" (layer "F.Cu")
    (at 121.717 81.331 -90)
    (descr "DCDC-Converter, RECOM, RECOM_R-78E-0.5, SIP-3, pitch 2.54mm, package size 11.6x8.5x10.4mm^3, https://www.recom-power.com/pdf/Innoline/R-78Exx-0.5.pdf")
    (tags "dc-dc recom buck sip-3 pitch 2.54mm")
    (property "Field5" "")
    (property "Mouser" "490-P78E05-1000")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "1.5A Step-Down DC/DC-Regulator, 7-36V input, 3.3V fixed Output Voltage, LM78xx replacement, -40°C to +85°C, OKI-78SR_Vertical")
    (property "ki_keywords" "dc-dc murata Step-Down DC/DC-Regulator")
    (attr through_hole)
    (fp_text reference "U2" (at 2.54 -7.56 90) (layer "F.SilkS") hide)
    (fp_text value "CUI P78E05-1000" (at 2.54 3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.5 2.3) (drill 1) (layers "*.Cu" "*.Mask")
      (net 34 "Net-(JP2-B)") (pinfunction "IN") (pintype "power_in"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.5 2.3) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval (at 5.08 0 270) (size 1.5 2.3) (drill 1) (layers "*.Cu" "*.Mask")
      (net 32 "/5V_raw") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Converter_DCDC.3dshapes/Converter_DCDC_RECOM_R-78E-0.5_THT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" locked (layer "F.Cu")
    (at 103.5 96.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH3" (at 0 -4) (layer "F.Fab") hide)
    (fp_text value "MountingHole_2.7mm_M2.5" (at 0 3.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "F&B.Cu" "*.Mask")
      (clearance 0.3))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" locked (layer "F.Cu")
    (at 103.5 73.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH1" (at 0 4) (layer "F.Fab") hide)
    (fp_text value "MountingHole_2.7mm_M2.5" (at 0 3.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "F&B.Cu" "*.Mask")
      (clearance 0.3))
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "F.Cu")
    (at 109.144 78.41)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Field5" "")
    (property "Mouser" "771-PMEG1020EJ-T/R")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Schottky diode")
    (property "ki_keywords" "diode Schottky")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "D_Schottky" (at 0.1 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.25 0) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "+5V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/5V_raw") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_GCT_DCJ200-10-A_Horizontal" (layer "F.Cu")
    (at 114.965 88.342 -90)
    (descr "Barrel jack connector (5.5 mm outer diameter, 2.05 inner diameter ), https://gct.co/files/drawings/dcj200-10.pdf")
    (tags "connector barrel jack")
    (property "Field5" "")
    (property "Mouser" "490-PJ-002B")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "DC Barrel Jack")
    (property "ki_keywords" "DC power barrel jack connector")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.5 90) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack" (at 0 15.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 4.6 2) (drill oval 3.6 1) (layers "*.Cu" "*.Mask")
      (net 33 "+12V") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 6.3 270) (size 4.2 2) (drill oval 3.2 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "3" thru_hole oval (at 4.8 2.9 270) (size 2 4.2) (drill oval 1 3.2) (layers "*.Cu" "*.Mask"))
    (model "${KIPRJMOD}/board-assets/barreljack_DCJ200-10-A-K1-K-740395.STEP"
      (offset (xyz 0 -6.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm" (layer "F.Cu")
    (at 115.023 81.331)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Solder Jumper, 2-pole, closed/bridged")
    (property "ki_keywords" "solder jumper SPST")
    (attr exclude_from_pos_files)
    (fp_text reference "JP2" (at 0 -1.8) (layer "F.SilkS") hide)
    (fp_text value "SolderJumper_2_Bridged" (at 0 1.9) (layer "F.Fab"))
    (pad "1" smd custom (at -0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 33 "+12V") (pinfunction "A") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy 1 0)
            (xy 0.5 0.75)
            (xy -0.5 0.75)
            (xy -0.5 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
    (pad "2" smd custom (at 0.725 0) (size 0.3 0.3) (layers "F.Cu" "F.Mask")
      (net 34 "Net-(JP2-B)") (pinfunction "B") (pintype "passive") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy 0.5 0.75)
            (xy -0.65 0.75)
            (xy -0.15 0)
            (xy -0.65 -0.75)
            (xy 0.5 -0.75)
          )
          (width 0) (fill yes))
      ))
  )
  (footprint "MountingHole:MountingHole_2.7mm_M2.5" locked (layer "F.Cu")
    (at 161.5 96.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "MH4" (at 0 -4) (layer "F.Fab") hide)
    (fp_text value "MountingHole_2.7mm_M2.5" (at 0 3.7) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle locked (at 0 0) (size 2.7 2.7) (drill 2.7) (layers "F&B.Cu" "*.Mask")
      (clearance 0.3))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 148.26 83.998 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Pin" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "SCLK") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "CSZ") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "MOSI") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "MISO") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_Pico-Clasp_501331-0807_1x08-1MP_P1.00mm_Vertical" (layer "F.Cu")
    (at 133.401 95.403)
    (descr "Molex Pico-Clasp series connector, 501331-0807 (http://www.molex.com/pdm_docs/sd/5013310207_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex Pico-Clasp side entry")
    (property "Field5" "")
    (property "Mouser" "538-501331-0807")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x08, script generated")
    (property "ki_keywords" "connector")
    (attr smd)
    (fp_text reference "J3" (at 0 -4.52) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x08_Pin" (at 0 3.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.15) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "+12V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd roundrect (at -2.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "+12V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd roundrect (at -1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "+12V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd roundrect (at -0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "+12V") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd roundrect (at 0.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd roundrect (at 1.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd roundrect (at 2.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd roundrect (at 3.5 1.325) (size 0.6 1.55) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "MP" smd roundrect (at -4.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (pad "MP" smd roundrect (at 4.8 -1.2) (size 1.2 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.208333))
    (model "${KIPRJMOD}/board-assets/molex_5013310807.stp"
      (offset (xyz 0 -1.1 6.3))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x7.7" (layer "F.Cu")
    (at 121.049 95.047 180)
    (descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
    (tags "capacitor electrolytic")
    (property "Field5" "")
    (property "Mouser" "667-EEE-FN1E101UP")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -4.35) (layer "F.SilkS"))
    (fp_text value "100uF" (at 0 4.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.7 0 180) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 33 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.7 0 180) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 159.7916 81.2548 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x04_Pin" (at 1.27 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/GPIO26") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/GPIO20{slash}PCM.DIN") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/GPIO16") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/GPIO21{slash}PCM.DOUT") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical" (layer "B.Cu")
    (at 108.37 74.77 -90)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (property "Sheetfile" "elegoo-dlp-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x20, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 2.5 0) (layer "B.SilkS"))
    (fp_text value "GPIO" (at -5.77 -24.13) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -24.13 180) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "SDA") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 25 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "SCL") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "/GPIO4{slash}GPCLK0") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/GPIO14{slash}TXD0") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/GPIO15{slash}RXD0") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/GPIO17") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/GPIO18{slash}PCM.CLK") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "/GPIO27") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "/GPIO22") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "/GPIO23") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 26 "+3V3") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 13 "/GPIO24") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 14 "MOSI") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 15 "MISO") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 18 "/GPIO25") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "SCLK") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 16 "CSZ") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 31 "SPI_RDY") (pinfunction "Pin_26") (pintype "passive"))
    (pad "27" thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 19 "/ID_SDA") (pinfunction "Pin_27") (pintype "passive"))
    (pad "28" thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 20 "/ID_SCL") (pinfunction "Pin_28") (pintype "passive"))
    (pad "29" thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 30 "PROJ_ON") (pinfunction "Pin_29") (pintype "passive"))
    (pad "30" thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_30") (pintype "passive"))
    (pad "31" thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "SYS_RDY") (pinfunction "Pin_31") (pintype "passive"))
    (pad "32" thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 21 "/GPIO12{slash}PWM0") (pinfunction "Pin_32") (pintype "passive"))
    (pad "33" thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 28 "PRINT") (pinfunction "Pin_33") (pintype "passive"))
    (pad "34" thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_34") (pintype "passive"))
    (pad "35" thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 27 "HOST_IRQ") (pinfunction "Pin_35") (pintype "passive"))
    (pad "36" thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 22 "/GPIO16") (pinfunction "Pin_36") (pintype "passive"))
    (pad "37" thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "/GPIO26") (pinfunction "Pin_37") (pintype "passive"))
    (pad "38" thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 23 "/GPIO20{slash}PCM.DIN") (pinfunction "Pin_38") (pintype "passive"))
    (pad "39" thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "Pin_39") (pintype "passive"))
    (pad "40" thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 24 "/GPIO21{slash}PCM.DOUT") (pinfunction "Pin_40") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "board-assets:openmla-logo" (layer "B.Cu")
    (at 133.981076 88.384939 90)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 180) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 90) (layer "B.SilkS") hide)
  )
  (gr_arc (start 162 70) (mid 164.12132 70.87868) (end 165 73)
    (layer "Edge.Cuts"))
  (gr_line (start 165 97) (end 165 73)
    (layer "Edge.Cuts"))
  (gr_line (start 100 73) (end 100 97)
    (layer "Edge.Cuts"))
  (gr_arc (start 103 100) (mid 100.87868 99.12132) (end 100 97)
    (layer "Edge.Cuts"))
  (gr_line (start 103 100) (end 162 100)
    (layer "Edge.Cuts"))
  (gr_arc (start 165 97) (mid 164.12132 99.12132) (end 162 100)
    (layer "Edge.Cuts"))
  (gr_arc (start 100 73) (mid 100.87868 70.87868) (end 103 70)
    (layer "Edge.Cuts"))
  (gr_line (start 162 70) (end 103 70)
    (layer "Edge.Cuts"))
  (gr_text "12V" (at 126.797 91.745) (layer "F.SilkS"))
  (gr_text "5V" (at 104.318 79.3752) (layer "F.SilkS"))
  (gr_text "SPI" (at 143.8912 81.7628) (layer "F.SilkS" knockout))
  (gr_text "Enable 5V" (at 111.811 79.426) (layer "F.SilkS" knockout))
  (gr_text "Stemma \nQT" (at 163.1444 88.7224 90) (layer "F.SilkS"))
  (gr_text "openMLA\nProject" (at 131.369 82.855) (layer "F.SilkS" knockout))
  (gr_text "3.3V" (at 154.356 82.1692) (layer "F.SilkS"))
  (gr_text "Pico-Clasp 12 pin" (at 149.911 95.428) (layer "F.SilkS"))
  (gr_text "8 pin\nPico-Clasp " (at 133.655 95.047) (layer "F.SilkS"))
  (gr_text "I2C" (at 163.8048 93.4468) (layer "F.SilkS"))
  (gr_text "GPIO\n20\n" (at 159.5884 77.1908) (layer "F.SilkS"))
  (gr_text "SCLK" (at 149.3776 88.3668 90) (layer "F.SilkS"))
  (gr_text "Anhua DMD\ncontroller" (at 131.369 85.903) (layer "F.SilkS"))
  (gr_text "GPIO\n21" (at 162.6364 77.1908) (layer "F.SilkS"))
  (gr_text "GPIO\n26\n" (at 159.182 84.8616) (layer "F.SilkS"))
  (gr_text "Center Positive\n5.5mm OD 2.5mm ID" (at 100.5588 82.982) (layer "F.SilkS"))
  (gr_text "Board\nRev 0.1" (at 107.9248 98.4252) (layer "F.SilkS"))
  (gr_text "GND\n" (at 134.544 99.238) (layer "F.SilkS"))
  (gr_text "CSZ" (at 146.8884 88.316 90) (layer "F.SilkS"))
  (gr_text "12V" (at 129.337 99.238) (layer "F.SilkS"))
  (gr_text "GPIO\n16" (at 162.6364 84.9632) (layer "F.SilkS"))
  (gr_text "CUI \nP78E05-1000" (at 126.289 88.951 90) (layer "F.SilkS"))
  (gr_text "MOSI\n" (at 144.3484 88.2144 90) (layer "F.SilkS"))
  (gr_text "GND\n" (at 154.3052 89.1796) (layer "F.SilkS"))
  (gr_text "MISO" (at 141.8084 88.2144 90) (layer "F.SilkS"))
  (gr_text "PoE" (at 161.5 79.64) (layer "Dwgs.User"))
  (zone (net 33) (net_name "+12V") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 113.8176 86.03)
        (xy 113.8176 90.7544)
        (xy 116.9164 90.7544)
        (xy 121.9456 95.0216)
        (xy 121.9964 95.9868)
        (xy 125.7048 95.9868)
        (xy 127.94 96.063)
        (xy 129.337 97.46)
        (xy 133.2232 97.333)
        (xy 133.2232 91.1608)
        (xy 131.8008 89.6876)
        (xy 120.828 89.6876)
        (xy 118.3896 87.4016)
        (xy 116.1544 87.4016)
        (xy 116.1544 83.7948)
        (xy 115.0876 82.3216)
        (xy 113.8176 80.5944)
      )
    )
  )
  (zone (net 34) (net_name "Net-(JP2-B)") (layer "F.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 120.828 82.093)
        (xy 120.955 80.569)
        (xy 117.399 80.569)
        (xy 115.099008 80.581652)
        (xy 115.851546 81.4326)
        (xy 115.371016 82.078278)
      )
    )
  )
  (zone (net 25) (net_name "+5V") (layer "F.Cu") (hatch edge 0.5)
    (priority 4)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 108.8392 77.394)
        (xy 108.8392 79.4514)
        (xy 100.4064 79.4768)
        (xy 100.4064 72.4664)
        (xy 102.5908 70.3836)
        (xy 112.1412 70.3836)
        (xy 112.1412 73.3808)
        (xy 107.1628 73.3808)
        (xy 107.1628 75.8192)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 110.541 89.84)
        (xy 110.541 86.538)
        (xy 109.652 85.649)
        (xy 107.62 85.649)
        (xy 106.731 86.538)
        (xy 106.731 96.063)
        (xy 107.493 96.952)
        (xy 116.891 96.952)
        (xy 117.7292 96.063)
        (xy 117.7292 93.8532)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.5)
    (priority 3)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 134.163 89.586)
        (xy 138.862 89.586)
        (xy 138.862 92.38)
        (xy 137.211 93.142)
        (xy 137.211 97.46)
        (xy 133.6296 97.46)
        (xy 133.6296 90.094)
      )
    )
  )
  (zone (net 32) (net_name "/5V_raw") (layer "F.Cu") (hatch edge 0.5)
    (priority 5)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 109.652 77.648)
        (xy 109.652 79.426)
        (xy 123.368 79.426)
        (xy 123.7744 79.7816)
        (xy 123.7236 84.9632)
        (xy 123.1648 85.4712)
        (xy 120.6756 85.4712)
        (xy 120.3708 85.7252)
        (xy 120.3708 86.8936)
        (xy 120.6756 87.2492)
        (xy 123.7744 87.2492)
        (xy 125.5016 85.8268)
        (xy 125.5016 78.5624)
        (xy 124.5364 77.648)
        (xy 112.2428 77.648)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (priority 2)
    (connect_pads yes (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 83.8964 57.7344)
        (xy 173.5076 57.7344)
        (xy 173.5076 107.5692)
        (xy 83.8964 107.5692)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (name "PoE") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks allowed) (vias allowed) (pads allowed) (copperpour allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164 82.14)
        (xy 159 82.14)
        (xy 159 77.14)
        (xy 164 77.14)
      )
    )
  )
)
