(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "User" 185 135)
	(title_block
		(title "Smoker PCB")
		(date "2026-03-10")
		(rev "V2.2")
		(company "Smoke Sense")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/CS1")
	(net 3 "3V3")
	(net 4 "/CS2")
	(net 5 "/SCK")
	(net 6 "/SCL")
	(net 7 "/SDA")
	(net 8 "unconnected-(U2-ALERT-Pad6)")
	(net 9 "/CS3")
	(net 10 "/CS4")
	(net 11 "5V")
	(net 12 "/SO")
	(net 13 "Net-(J3-Pin_2)")
	(net 14 "unconnected-(U3-GPIO10{slash}SPI_MOSI-Pad19)")
	(net 15 "Net-(J7-Pin_1)")
	(net 16 "Net-(U2-A0)")
	(net 17 "Net-(U5-VIN-)")
	(net 18 "/Signal Low")
	(net 19 "Net-(J4-Pin_2)")
	(net 20 "Net-(J4-Pin_1)")
	(net 21 "Net-(J4-Pin_4)")
	(net 22 "Net-(J4-Pin_3)")
	(net 23 "Net-(J4-Pin_5)")
	(net 24 "Net-(J5-Pin_1)")
	(net 25 "Net-(J5-Pin_4)")
	(net 26 "Net-(J5-Pin_3)")
	(net 27 "Net-(J5-Pin_2)")
	(net 28 "Net-(IC1-VCC)")
	(net 29 "unconnected-(U2-ALERT-Pad6)_1")
	(net 30 "Net-(J20-Pin_7)")
	(net 31 "Net-(J20-Pin_2)")
	(net 32 "Net-(J20-Pin_5)")
	(net 33 "Net-(J20-Pin_8)")
	(net 34 "Net-(J20-Pin_4)")
	(net 35 "Net-(J20-Pin_6)")
	(net 36 "Net-(J20-Pin_3)")
	(net 37 "Net-(J1-Pin_2)")
	(net 38 "Net-(J1-Pin_1)")
	(net 39 "Net-(J20-Pin_1)")
	(footprint "CL32B226MOJNNNE:CAPC3225X270N"
		(layer "F.Cu")
		(at 152.46 17 180)
		(property "Reference" "C6"
			(at -1.11 -1.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF-CL32B226MOJNNNE"
			(at 0.89 1.95 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "E_max" "2.7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "L_max" "0.9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "A_max" "2.7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "L1_nom" "0.6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "D_max" "3.5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "A_nom" "2.7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "L1_max" "0.9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "L1_min" "0.3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "A_min" "2.7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "E_min" "2.3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "D_min" "2.9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "D_nom" "3.2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "E_nom" "2.5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "L_min" "0.3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "L_nom" "0.6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samsung Electro-Mechanics"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.421 0 180)
			(size 1.37 2.72)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 28 "Net-(IC1-VCC)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at 1.421 0 180)
			(size 1.37 2.72)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 153.5 111.5)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "REF**"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Adafruit_MAX31855 v2:Max31855_Module"
		(layer "F.Cu")
		(at 70.617 41.945626)
		(property "Reference" "IC3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MAX31855"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(pad "1" thru_hole circle
			(at 8.223549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(IC1-VCC)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1" thru_hole circle
			(at 16.373549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 10.763549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 12.873549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 13.303549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "T+")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 15.843549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SO")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 18.383549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/CS3")
			(pinfunction "SCK")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 20.923549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/SCK")
			(pinfunction "/CS")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 6.953549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 22.193549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 166.5 118.08 90)
		(descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J1"
			(at 2.54 -6.32 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 3.08 1.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 38 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Adafruit_MAX31855 v2:Max31855_Module"
		(layer "F.Cu")
		(at 124.290446 42.24066)
		(property "Reference" "IC1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MAX31855"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(pad "1" thru_hole circle
			(at 8.223549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(IC1-VCC)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1" thru_hole circle
			(at 16.373549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 10.763549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 12.873549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 13.303549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "T+")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 15.843549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SO")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 18.383549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/CS1")
			(pinfunction "SCK")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 20.923549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/SCK")
			(pinfunction "/CS")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 6.953549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 22.193549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Harwin:Harwin_M20-89005xx_1x05_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 35.5 20.5 90)
		(descr "Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89005xx, 5 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator")
		(tags "connector Harwin M20-890 horizontal")
		(property "Reference" "J4"
			(at -0.48 -7.55 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x05_Pin"
			(at -0.5 8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.48 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.525 -5.08 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -5.525 -2.54 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -5.525 0 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -5.525 2.54 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -5.525 5.08 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_M20-89005xx_1x05_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 51 82.6284)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "Ri1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 2.5 0.8716 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 17 "Net-(U5-VIN-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 27.5 41.5)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "Mount"
			(at 0 -3.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 152 42.5)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "REF**"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380_Pad"
		(layer "F.Cu")
		(at 16.5 107)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "REF**"
			(at 0 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO7380_Pad"
			(at 0 3.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.7 5.7)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-16-5.08_1x16_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 16.18 116.5)
		(descr "Terminal Block Phoenix MKDS-1,5-16-5.08, 16 pins, pitch 5.08mm, size 81.3x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-16-5.08 pitch 5.08mm size 81.3x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J16"
			(at 38.1 -6.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x16"
			(at 38.1 5.72 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x16, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 38.1 3.2 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 7 "/SDA")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SDA")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.16 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SDA")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.24 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SDA")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.32 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCL")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25.4 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCL")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 30.48 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCL")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 35.56 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCL")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 40.64 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3V3")
			(pinfunction "Power")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 45.72 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3V3")
			(pinfunction "Power")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 50.8 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3V3")
			(pinfunction "Power")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 55.88 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3V3")
			(pinfunction "Power")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 60.96 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pi-GND")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 66.04 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pi-GND")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 71.12 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pi-GND")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 76.2 0)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pi-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-16-5.08_1x16_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "N7803-1C:N78031C"
		(layer "F.Cu")
		(at 160.16 22.16 90)
		(descr "N7803-1C-4")
		(tags "Power Supply")
		(property "Reference" "PS2"
			(at 2.54 3.965 90)
			(layer "F.SilkS")
		)
		(property "Value" "N7803-1C"
			(at 2.54 3.965 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.meanwell.com/webapp/product/search.aspx?prod=N78"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Switching Voltage Regulators 6-36Vin 3.3Vout 0-1000mA Encapsulated Non-Isolated DC-DC Switching Regulator"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "17.5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Mean Well"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "N7803-1C"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "709-N7803-1C"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/MEAN-WELL/N7803-1C?qs=7D1LtPJG0i1K0F21XTLD8Q%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.965 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J7-Pin_1)")
			(pinfunction "+VIN")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(IC1-VCC)")
			(pinfunction "+VOUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "N7803-1C.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MCP6001:SOT95P270X145-5N"
		(layer "F.Cu")
		(at 57.5 80.6284 -90)
		(property "Reference" "U5"
			(at -0.09329 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "MCP6001UT-I_OT"
			(at 8.45727 9.395455 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.3716 -0.9398 270)
			(size 1.3208 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(U2-A0)")
			(pinfunction "VOUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -1.3716 0 270)
			(size 1.3208 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -1.3716 0.9398 270)
			(size 1.3208 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(J3-Pin_2)")
			(pinfunction "VIN+")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 1.3716 0.9398 270)
			(size 1.3208 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U5-VIN-)")
			(pinfunction "VIN-")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at 1.3716 -0.9398 270)
			(size 1.3208 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "5V")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Adafruit_MAX31855 v2:Max31855_Module"
		(layer "F.Cu")
		(at 45.394451 41.563451)
		(property "Reference" "IC4"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MAX31855"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(fp_text user "Yellow +"
			(at 18.918549 -19.186151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "CS"
			(at 18.878549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at 11.258549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "CLK"
			(at 21.418549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin"
			(at 8.718549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 13.798549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "DO"
			(at 16.338549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Red -"
			(at 11.418549 -20.186151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 8.223549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(IC1-VCC)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1" thru_hole circle
			(at 16.373549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 10.763549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 12.873549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 13.303549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "T+")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 15.843549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SO")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 18.383549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/CS4")
			(pinfunction "SCK")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 20.923549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/SCK")
			(pinfunction "/CS")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 6.953549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 22.193549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 48.4125 97.5875 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7k"
			(at 0.5 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 3 "3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 6 "/SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 18.6325 70.455 -90)
		(descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J3"
			(at 2.54 -6.32 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.54 5.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 18 "/Signal Low")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Custom:ADS1115"
		(layer "F.Cu")
		(at 29.133 94.487)
		(property "Reference" "U2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115_ADC_Module"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(fp_text user "A1"
			(at -7.984 -0.597 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A-"
			(at -7.984 -5.804 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A0"
			(at -7.984 -3.264 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A2"
			(at -7.984 1.816 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A3"
			(at -7.984 4.483 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A+"
			(at -7.984 7.15 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -6.333 7.023 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "1" thru_hole circle
			(at 6.367 7.023 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3V3")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -6.333 4.483 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 6.367 4.483 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -6.333 1.943 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "SCL")
			(pintype "input")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 6.367 1.943 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -6.333 -0.597 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Signal Low")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 6.367 -0.597 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -6.333 -3.137 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U2-A0)")
			(pinfunction "ADDR")
			(pintype "input")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 6.367 -3.137 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "ADDR")
			(pintype "input")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at -6.333 -5.677 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(U2-ALERT-Pad6)_1")
			(pinfunction "ALERT")
			(pintype "output+no_connect")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 6.367 -5.677 180)
			(size 1.778 1.778)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(U2-ALERT-Pad6)")
			(pinfunction "ALERT")
			(pintype "output+no_connect")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at -6.333 -9.487 90)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at -6.333 10.833 90)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 6.367 -9.487 90)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 6.367 10.833 90)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 22.8 82.984) (xy 22.519427 83.00362) (xy 22.244315 83.062096) (xy 21.980019 83.158292) (xy 21.731683 83.290335)
					(xy 21.50414 83.455654) (xy 21.30182 83.651033) (xy 21.12866 83.872667) (xy 20.988031 84.116244)
					(xy 20.88267 84.377022) (xy 20.814628 84.649925) (xy 20.785228 84.929643) (xy 20.795044 85.210729)
					(xy 20.843884 85.487715) (xy 20.930797 85.755207) (xy 21.054093 86.008) (xy 21.21137 86.241174)
					(xy 21.399569 86.450189) (xy 21.615025 86.630978) (xy 21.853545 86.780022) (xy 22.110487 86.89442)
					(xy 22.38085 86.971946) (xy 22.659371 87.011089) (xy 22.940629 87.011089) (xy 23.21915 86.971946)
					(xy 23.489513 86.89442) (xy 23.746455 86.780022) (xy 23.984975 86.630978) (xy 24.200431 86.450189)
					(xy 24.38863 86.241174) (xy 24.545907 86.008) (xy 24.669203 85.755207) (xy 24.756116 85.487715)
					(xy 24.804956 85.210729) (xy 24.814772 84.929643) (xy 24.785372 84.649925) (xy 24.71733 84.377022)
					(xy 24.611969 84.116244) (xy 24.47134 83.872667) (xy 24.29818 83.651033) (xy 24.09586 83.455654)
					(xy 23.868317 83.290335) (xy 23.619981 83.158292) (xy 23.355685 83.062096) (xy 23.080573 83.00362)
				)
			)
			(polygon
				(pts
					(xy 22.8 85.016) (xy 22.811314 85.011314) (xy 22.816 85) (xy 22.811314 84.988686) (xy 22.8 84.984)
					(xy 22.788686 84.988686) (xy 22.784 85) (xy 22.788686 85.011314)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 22.8 103.304) (xy 22.519427 103.32362) (xy 22.244315 103.382096) (xy 21.980019 103.478292)
					(xy 21.731683 103.610335) (xy 21.50414 103.775654) (xy 21.30182 103.971033) (xy 21.12866 104.192667)
					(xy 20.988031 104.436244) (xy 20.88267 104.697022) (xy 20.814628 104.969925) (xy 20.785228 105.249643)
					(xy 20.795044 105.530729) (xy 20.843884 105.807715) (xy 20.930797 106.075207) (xy 21.054093 106.328)
					(xy 21.21137 106.561174) (xy 21.399569 106.770189) (xy 21.615025 106.950978) (xy 21.853545 107.100022)
					(xy 22.110487 107.21442) (xy 22.38085 107.291946) (xy 22.659371 107.331089) (xy 22.940629 107.331089)
					(xy 23.21915 107.291946) (xy 23.489513 107.21442) (xy 23.746455 107.100022) (xy 23.984975 106.950978)
					(xy 24.200431 106.770189) (xy 24.38863 106.561174) (xy 24.545907 106.328) (xy 24.669203 106.075207)
					(xy 24.756116 105.807715) (xy 24.804956 105.530729) (xy 24.814772 105.249643) (xy 24.785372 104.969925)
					(xy 24.71733 104.697022) (xy 24.611969 104.436244) (xy 24.47134 104.192667) (xy 24.29818 103.971033)
					(xy 24.09586 103.775654) (xy 23.868317 103.610335) (xy 23.619981 103.478292) (xy 23.355685 103.382096)
					(xy 23.080573 103.32362)
				)
			)
			(polygon
				(pts
					(xy 22.8 105.336) (xy 22.811314 105.331314) (xy 22.816 105.32) (xy 22.811314 105.308686) (xy 22.8 105.304)
					(xy 22.788686 105.308686) (xy 22.784 105.32) (xy 22.788686 105.331314)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 35.5 82.984) (xy 35.219427 83.00362) (xy 34.944315 83.062096) (xy 34.680019 83.158292) (xy 34.431683 83.290335)
					(xy 34.20414 83.455654) (xy 34.00182 83.651033) (xy 33.82866 83.872667) (xy 33.688031 84.116244)
					(xy 33.58267 84.377022) (xy 33.514628 84.649925) (xy 33.485228 84.929643) (xy 33.495044 85.210729)
					(xy 33.543884 85.487715) (xy 33.630797 85.755207) (xy 33.754093 86.008) (xy 33.91137 86.241174)
					(xy 34.099569 86.450189) (xy 34.315025 86.630978) (xy 34.553545 86.780022) (xy 34.810487 86.89442)
					(xy 35.08085 86.971946) (xy 35.359371 87.011089) (xy 35.640629 87.011089) (xy 35.91915 86.971946)
					(xy 36.189513 86.89442) (xy 36.446455 86.780022) (xy 36.684975 86.630978) (xy 36.900431 86.450189)
					(xy 37.08863 86.241174) (xy 37.245907 86.008) (xy 37.369203 85.755207) (xy 37.456116 85.487715)
					(xy 37.504956 85.210729) (xy 37.514772 84.929643) (xy 37.485372 84.649925) (xy 37.41733 84.377022)
					(xy 37.311969 84.116244) (xy 37.17134 83.872667) (xy 36.99818 83.651033) (xy 36.79586 83.455654)
					(xy 36.568317 83.290335) (xy 36.319981 83.158292) (xy 36.055685 83.062096) (xy 35.780573 83.00362)
				)
			)
			(polygon
				(pts
					(xy 35.5 85.016) (xy 35.511314 85.011314) (xy 35.516 85) (xy 35.511314 84.988686) (xy 35.5 84.984)
					(xy 35.488686 84.988686) (xy 35.484 85) (xy 35.488686 85.011314)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 35.5 103.304) (xy 35.219427 103.32362) (xy 34.944315 103.382096) (xy 34.680019 103.478292)
					(xy 34.431683 103.610335) (xy 34.20414 103.775654) (xy 34.00182 103.971033) (xy 33.82866 104.192667)
					(xy 33.688031 104.436244) (xy 33.58267 104.697022) (xy 33.514628 104.969925) (xy 33.485228 105.249643)
					(xy 33.495044 105.530729) (xy 33.543884 105.807715) (xy 33.630797 106.075207) (xy 33.754093 106.328)
					(xy 33.91137 106.561174) (xy 34.099569 106.770189) (xy 34.315025 106.950978) (xy 34.553545 107.100022)
					(xy 34.810487 107.21442) (xy 35.08085 107.291946) (xy 35.359371 107.331089) (xy 35.640629 107.331089)
					(xy 35.91915 107.291946) (xy 36.189513 107.21442) (xy 36.446455 107.100022) (xy 36.684975 106.950978)
					(xy 36.900431 106.770189) (xy 37.08863 106.561174) (xy 37.245907 106.328) (xy 37.369203 106.075207)
					(xy 37.456116 105.807715) (xy 37.504956 105.530729) (xy 37.514772 105.249643) (xy 37.485372 104.969925)
					(xy 37.41733 104.697022) (xy 37.311969 104.436244) (xy 37.17134 104.192667) (xy 36.99818 103.971033)
					(xy 36.79586 103.775654) (xy 36.568317 103.610335) (xy 36.319981 103.478292) (xy 36.055685 103.382096)
					(xy 35.780573 103.32362)
				)
			)
			(polygon
				(pts
					(xy 35.5 105.336) (xy 35.511314 105.331314) (xy 35.516 105.32) (xy 35.511314 105.308686) (xy 35.5 105.304)
					(xy 35.488686 105.308686) (xy 35.484 105.32) (xy 35.488686 105.331314)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 22.8 82.984) (xy 22.519427 83.00362) (xy 22.244315 83.062096) (xy 21.980019 83.158292) (xy 21.731683 83.290335)
					(xy 21.50414 83.455654) (xy 21.30182 83.651033) (xy 21.12866 83.872667) (xy 20.988031 84.116244)
					(xy 20.88267 84.377022) (xy 20.814628 84.649925) (xy 20.785228 84.929643) (xy 20.795044 85.210729)
					(xy 20.843884 85.487715) (xy 20.930797 85.755207) (xy 21.054093 86.008) (xy 21.21137 86.241174)
					(xy 21.399569 86.450189) (xy 21.615025 86.630978) (xy 21.853545 86.780022) (xy 22.110487 86.89442)
					(xy 22.38085 86.971946) (xy 22.659371 87.011089) (xy 22.940629 87.011089) (xy 23.21915 86.971946)
					(xy 23.489513 86.89442) (xy 23.746455 86.780022) (xy 23.984975 86.630978) (xy 24.200431 86.450189)
					(xy 24.38863 86.241174) (xy 24.545907 86.008) (xy 24.669203 85.755207) (xy 24.756116 85.487715)
					(xy 24.804956 85.210729) (xy 24.814772 84.929643) (xy 24.785372 84.649925) (xy 24.71733 84.377022)
					(xy 24.611969 84.116244) (xy 24.47134 83.872667) (xy 24.29818 83.651033) (xy 24.09586 83.455654)
					(xy 23.868317 83.290335) (xy 23.619981 83.158292) (xy 23.355685 83.062096) (xy 23.080573 83.00362)
				)
			)
			(polygon
				(pts
					(xy 22.8 85.016) (xy 22.811314 85.011314) (xy 22.816 85) (xy 22.811314 84.988686) (xy 22.8 84.984)
					(xy 22.788686 84.988686) (xy 22.784 85) (xy 22.788686 85.011314)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 22.8 103.304) (xy 22.519427 103.32362) (xy 22.244315 103.382096) (xy 21.980019 103.478292)
					(xy 21.731683 103.610335) (xy 21.50414 103.775654) (xy 21.30182 103.971033) (xy 21.12866 104.192667)
					(xy 20.988031 104.436244) (xy 20.88267 104.697022) (xy 20.814628 104.969925) (xy 20.785228 105.249643)
					(xy 20.795044 105.530729) (xy 20.843884 105.807715) (xy 20.930797 106.075207) (xy 21.054093 106.328)
					(xy 21.21137 106.561174) (xy 21.399569 106.770189) (xy 21.615025 106.950978) (xy 21.853545 107.100022)
					(xy 22.110487 107.21442) (xy 22.38085 107.291946) (xy 22.659371 107.331089) (xy 22.940629 107.331089)
					(xy 23.21915 107.291946) (xy 23.489513 107.21442) (xy 23.746455 107.100022) (xy 23.984975 106.950978)
					(xy 24.200431 106.770189) (xy 24.38863 106.561174) (xy 24.545907 106.328) (xy 24.669203 106.075207)
					(xy 24.756116 105.807715) (xy 24.804956 105.530729) (xy 24.814772 105.249643) (xy 24.785372 104.969925)
					(xy 24.71733 104.697022) (xy 24.611969 104.436244) (xy 24.47134 104.192667) (xy 24.29818 103.971033)
					(xy 24.09586 103.775654) (xy 23.868317 103.610335) (xy 23.619981 103.478292) (xy 23.355685 103.382096)
					(xy 23.080573 103.32362)
				)
			)
			(polygon
				(pts
					(xy 22.8 105.336) (xy 22.811314 105.331314) (xy 22.816 105.32) (xy 22.811314 105.308686) (xy 22.8 105.304)
					(xy 22.788686 105.308686) (xy 22.784 105.32) (xy 22.788686 105.331314)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 35.5 82.984) (xy 35.219427 83.00362) (xy 34.944315 83.062096) (xy 34.680019 83.158292) (xy 34.431683 83.290335)
					(xy 34.20414 83.455654) (xy 34.00182 83.651033) (xy 33.82866 83.872667) (xy 33.688031 84.116244)
					(xy 33.58267 84.377022) (xy 33.514628 84.649925) (xy 33.485228 84.929643) (xy 33.495044 85.210729)
					(xy 33.543884 85.487715) (xy 33.630797 85.755207) (xy 33.754093 86.008) (xy 33.91137 86.241174)
					(xy 34.099569 86.450189) (xy 34.315025 86.630978) (xy 34.553545 86.780022) (xy 34.810487 86.89442)
					(xy 35.08085 86.971946) (xy 35.359371 87.011089) (xy 35.640629 87.011089) (xy 35.91915 86.971946)
					(xy 36.189513 86.89442) (xy 36.446455 86.780022) (xy 36.684975 86.630978) (xy 36.900431 86.450189)
					(xy 37.08863 86.241174) (xy 37.245907 86.008) (xy 37.369203 85.755207) (xy 37.456116 85.487715)
					(xy 37.504956 85.210729) (xy 37.514772 84.929643) (xy 37.485372 84.649925) (xy 37.41733 84.377022)
					(xy 37.311969 84.116244) (xy 37.17134 83.872667) (xy 36.99818 83.651033) (xy 36.79586 83.455654)
					(xy 36.568317 83.290335) (xy 36.319981 83.158292) (xy 36.055685 83.062096) (xy 35.780573 83.00362)
				)
			)
			(polygon
				(pts
					(xy 35.5 85.016) (xy 35.511314 85.011314) (xy 35.516 85) (xy 35.511314 84.988686) (xy 35.5 84.984)
					(xy 35.488686 84.988686) (xy 35.484 85) (xy 35.488686 85.011314)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 35.5 103.304) (xy 35.219427 103.32362) (xy 34.944315 103.382096) (xy 34.680019 103.478292)
					(xy 34.431683 103.610335) (xy 34.20414 103.775654) (xy 34.00182 103.971033) (xy 33.82866 104.192667)
					(xy 33.688031 104.436244) (xy 33.58267 104.697022) (xy 33.514628 104.969925) (xy 33.485228 105.249643)
					(xy 33.495044 105.530729) (xy 33.543884 105.807715) (xy 33.630797 106.075207) (xy 33.754093 106.328)
					(xy 33.91137 106.561174) (xy 34.099569 106.770189) (xy 34.315025 106.950978) (xy 34.553545 107.100022)
					(xy 34.810487 107.21442) (xy 35.08085 107.291946) (xy 35.359371 107.331089) (xy 35.640629 107.331089)
					(xy 35.91915 107.291946) (xy 36.189513 107.21442) (xy 36.446455 107.100022) (xy 36.684975 106.950978)
					(xy 36.900431 106.770189) (xy 37.08863 106.561174) (xy 37.245907 106.328) (xy 37.369203 106.075207)
					(xy 37.456116 105.807715) (xy 37.504956 105.530729) (xy 37.514772 105.249643) (xy 37.485372 104.969925)
					(xy 37.41733 104.697022) (xy 37.311969 104.436244) (xy 37.17134 104.192667) (xy 36.99818 103.971033)
					(xy 36.79586 103.775654) (xy 36.568317 103.610335) (xy 36.319981 103.478292) (xy 36.055685 103.382096)
					(xy 35.780573 103.32362)
				)
			)
			(polygon
				(pts
					(xy 35.5 105.336) (xy 35.511314 105.331314) (xy 35.516 105.32) (xy 35.511314 105.308686) (xy 35.5 105.304)
					(xy 35.488686 105.308686) (xy 35.484 105.32) (xy 35.488686 105.331314)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "GRM21BR61H106KE43L:CAPC2012X145N"
		(layer "F.Cu")
		(at 152.16 24.66 180)
		(property "Reference" "C5"
			(at -0.46 -1.32 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF-GRM21BR61H106KE43L"
			(at -1.34 1.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.9 0 180)
			(size 1.11 1.47)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(J7-Pin_1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.9 0 180)
			(size 1.11 1.47)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 57.5875 86.6284)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "Rf1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k"
			(at 1.9125 -1.6284 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 17 "Net-(U5-VIN-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 16 "Net-(U2-A0)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 164 36.42 -90)
		(descr "Terminal Block Phoenix MKDS-1,5-2-5.08, 2 pins, pitch 5.08mm, size 10.2x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-2-5.08 pitch 5.08mm size 10.2x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J7"
			(at 2.54 -6.32 270)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.54 5.72 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.2 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 15 "Net-(J7-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-2-5.08_1x02_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Harwin:Harwin_M20-89004xx_1x04_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 20 20.5 90)
		(descr "Harwin Male Horizontal Surface Mount Single Row 2.54mm (0.1 inch) Pitch PCB Connector, M20-89004xx, 4 Pins per row (https://cdn.harwin.com/pdfs/M20-890.pdf), generated with kicad-footprint-generator")
		(tags "connector Harwin M20-890 horizontal")
		(property "Reference" "J5"
			(at -0.48 -6.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at -0.48 6.28 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.48 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.525 -3.81 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(J5-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -5.525 -1.27 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(J5-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -5.525 1.27 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -5.525 3.81 90)
			(size 2.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Harwin.3dshapes/Harwin_M20-89004xx_1x04_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-8-5.08_1x08_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 166.5 96.32 90)
		(descr "Terminal Block Phoenix MKDS-1,5-8-5.08, 8 pins, pitch 5.08mm, size 40.6x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-8-5.08 pitch 5.08mm size 40.6x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J20"
			(at 17.78 -6.32 90)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x08"
			(at 14.82 -3.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 17.78 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 39 "Net-(J20-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J20-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.16 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J20-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.24 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J20-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.32 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J20-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25.4 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J20-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 30.48 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J20-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 35.56 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J20-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-8-5.08_1x08_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RASPBERRY_PI_4B_4GB:MODULE_RASPBERRY_PI_4B_4GB"
		(layer "F.Cu")
		(at 134.77 143.27)
		(property "Reference" "U3"
			(at -39.575 -29.635 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RASPBERRY_PI_4B_4GB"
			(at 1.20625 109.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Raspberry Pi"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "16 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RASPBERRY%20PI%204B/4GB/Raspberry+Pi/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RASPBERRY%20PI%204B/4GB/Raspberry+Pi/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RASPBERRY PI 4B/4GB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "BCM2711 Raspberry Pi 4 Model B 4GB - ARM® Cortex®-A72 MPU Embedded Evaluation Board"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Raspberry Pi"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "Not in stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "RASPBERRY PI 4B/4GB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -34.13 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3V3")
			(pinfunction "3V-PI")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -34.13 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "5V")
			(pinfunction "5V")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -31.59 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SDA")
			(pinfunction "GPIO2/SDA1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -31.59 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "5V")
			(pinfunction "5V")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at -29.05 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/SCL")
			(pinfunction "GPIO3/SCL1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at -29.05 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at -26.51 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J20-Pin_4)")
			(pinfunction "GPIO4/GPIO_GCKL")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -26.51 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J4-Pin_4)")
			(pinfunction "GPIO14/TXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at -23.97 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at -23.97 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J4-Pin_5)")
			(pinfunction "GPIO15/RXD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at -21.43 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J20-Pin_2)")
			(pinfunction "GPIO17/GPIO_GEN0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at -21.43 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J4-Pin_1)")
			(pinfunction "GPIO18/GPIO_GEN1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at -18.89 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J20-Pin_3)")
			(pinfunction "GPIO27/GPIO_GEN2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at -18.89 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at -16.35 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J20-Pin_6)")
			(pinfunction "GPIO22/GPIO_GEN3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at -16.35 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J4-Pin_2)")
			(pinfunction "GPIO23/GPIO_GEN4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at -13.81 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "3V3")
			(pinfunction "3V3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at -13.81 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J4-Pin_3)")
			(pinfunction "GPIO24/GPIO_GEN5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at -11.27 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(U3-GPIO10{slash}SPI_MOSI-Pad19)")
			(pinfunction "GPIO10/SPI_MOSI")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at -11.27 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "21" thru_hole circle
			(at -8.73 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SO")
			(pinfunction "GPIO9/SPI_MISO")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" thru_hole circle
			(at -8.73 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/CS1")
			(pinfunction "GPIO25/GPIO_GEN6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "23" thru_hole circle
			(at -6.19 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/SCK")
			(pinfunction "GPIO11/SPI_SCLK")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" thru_hole circle
			(at -6.19 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CS2")
			(pinfunction "GPIO8/~{SPI_CE0}")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "25" thru_hole circle
			(at -3.65 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "26" thru_hole circle
			(at -3.65 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/CS3")
			(pinfunction "GPIO7/~{SPI_CE1}")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "27" thru_hole circle
			(at -1.11 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J5-Pin_4)")
			(pinfunction "ID_SD")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "28" thru_hole circle
			(at -1.11 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/CS4")
			(pinfunction "ID_SC")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "29" thru_hole circle
			(at 1.43 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J5-Pin_1)")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "30" thru_hole circle
			(at 1.43 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "31" thru_hole circle
			(at 3.97 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J5-Pin_2)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "32" thru_hole circle
			(at 3.97 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J20-Pin_5)")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "33" thru_hole circle
			(at 6.51 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J5-Pin_3)")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "34" thru_hole circle
			(at 6.51 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "35" thru_hole circle
			(at 9.05 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J1-Pin_2)")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "36" thru_hole circle
			(at 9.05 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J20-Pin_8)")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "37" thru_hole circle
			(at 11.59 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J20-Pin_7)")
			(pinfunction "GPIO26")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "38" thru_hole circle
			(at 11.59 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J20-Pin_1)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "39" thru_hole circle
			(at 14.13 -23.23)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "40" thru_hole circle
			(at 14.13 -25.77)
			(size 1.524 1.524)
			(drill 1.016)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J1-Pin_1)")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 48.5 92 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7k"
			(at 1.5 -10.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 3 "3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 7 "/SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Adafruit_MAX31855 v2:Max31855_Module"
		(layer "F.Cu")
		(at 97.351 41.945626)
		(property "Reference" "IC2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MAX31855"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Schematic V2.4.kicad_sch")
		(fp_text user "CS"
			(at 18.878549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "CLK"
			(at 21.418549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Yellow +"
			(at 18.918549 -19.186151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3Vo"
			(at 11.258549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "DO"
			(at 16.338549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Red -"
			(at 11.418549 -20.186151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin"
			(at 8.718549 -8.686151 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at 8.223549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(IC1-VCC)")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1" thru_hole circle
			(at 16.373549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 10.763549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at 12.873549 -24.293451)
			(size 2.1844 2.1844)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "T-")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at 13.303549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "T+")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at 15.843549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SO")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at 18.383549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CS2")
			(pinfunction "SCK")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 20.923549 -7.275451 90)
			(size 1.9304 1.9304)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/SCK")
			(pinfunction "/CS")
			(pintype "input")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 6.953549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "P$1" thru_hole circle
			(at 22.193549 -25.563451)
			(size 3 3)
			(drill 2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 175 125)
		(end 10 125)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 10 10)
		(end 175 10)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175 10)
		(end 175 125)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 10 125)
		(end 10 10)
		(layer "Edge.Cuts")
	)
	(gr_text "Amplifier"
		(at 45.5 77 0)
		(layer "F.SilkS")
	)
	(gr_text "Thermocouple 4\n"
		(at 133.5 13.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Thermocouple 3\n"
		(at 106.5 13.5 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIO"
		(at 20 29.5 90)
		(layer "F.SilkS")
	)
	(gr_text "CS"
		(at 89.54 33 90)
		(layer "F.SilkS")
	)
	(gr_text "Thermocouple 2\n"
		(at 80 13.5 0)
		(layer "F.SilkS")
	)
	(gr_text "MCP6001UT\n"
		(at 50.5 75 0)
		(layer "F.SilkS")
	)
	(gr_text "CLK"
		(at 145.708995 33.554509 90)
		(layer "F.SilkS")
	)
	(gr_text "3Vo"
		(at 81.875549 33.259475 90)
		(layer "F.SilkS")
	)
	(gr_text "3.3V"
		(at 65 122 0)
		(layer "F.SilkS")
	)
	(gr_text "10uF"
		(at 154 27 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 111.149549 33.259475 90)
		(layer "F.SilkS")
	)
	(gr_text "High"
		(at 25 77.6284 0)
		(layer "F.SilkS")
	)
	(gr_text "CLK"
		(at 92.035549 33.259475 90)
		(layer "F.SilkS")
	)
	(gr_text "SSR1"
		(at 172.5 118 90)
		(layer "F.SilkS")
	)
	(gr_text "Red -"
		(at 135.708995 22.054509 90)
		(layer "F.SilkS")
	)
	(gr_text "PWM"
		(at 29 29.5 90)
		(layer "F.SilkS")
	)
	(gr_text "22uF"
		(at 156.5682 17.470118 0)
		(layer "F.SilkS")
	)
	(gr_text "Mount"
		(at 153.5 107.5 0)
		(layer "F.SilkS")
	)
	(gr_text "CS"
		(at 143.168995 33.554509 90)
		(layer "F.SilkS")
	)
	(gr_text "Oxygen Sensor"
		(at 13 67 0)
		(layer "F.SilkS")
	)
	(gr_text "Pin29\n"
		(at 12 31.5 90)
		(layer "F.SilkS")
	)
	(gr_text "1115ADC"
		(at 24.5 81.5 0)
		(layer "F.SilkS")
	)
	(gr_text "4.7k"
		(at 48.5 90 0)
		(layer "F.SilkS")
	)
	(gr_text "Mount"
		(at 152 38.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Pull"
		(at 48.4125 94 0)
		(layer "F.SilkS")
	)
	(gr_text "Yellow +"
		(at 89.535549 22.759475 90)
		(layer "F.SilkS")
	)
	(gr_text "DO"
		(at 87 33 90)
		(layer "F.SilkS")
	)
	(gr_text "Yellow +"
		(at 143.208995 23.054509 90)
		(layer "F.SilkS")
	)
	(gr_text "GPIO"
		(at 37 30 90)
		(layer "F.SilkS")
	)
	(gr_text "1k"
		(at 48 82.5 0)
		(layer "F.SilkS")
	)
	(gr_text "GPIOx1   x2   x3    x4     x5    x6     x7    x8\n"
		(at 172.207738 79.446372 90)
		(layer "F.SilkS")
	)
	(gr_text "4k"
		(at 58.5 88.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Low"
		(at 25 70 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 85 122.5 0)
		(layer "F.SilkS")
	)
	(gr_text "4.7k"
		(at 48.5 100 0)
		(layer "F.SilkS")
	)
	(gr_text "Thermocouple\n"
		(at 107.258549 25.652175 0)
		(layer "F.SilkS")
	)
	(gr_text "Pin8\n"
		(at 19.223 75.3927 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 138.088995 33.554509 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 84.415549 33.259475 90)
		(layer "F.SilkS")
	)
	(gr_text "DO"
		(at 140.628995 33.554509 90)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 23.5 122.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Vin"
		(at 79.335549 33.259475 90)
		(layer "F.SilkS")
	)
	(gr_text "SSR2\n"
		(at 172.5 113.5 90)
		(layer "F.SilkS")
	)
	(gr_text "12V"
		(at 172 40.5 90)
		(layer "F.SilkS")
	)
	(gr_text "Thermocouple\n"
		(at 134.258549 25.652175 0)
		(layer "F.SilkS")
	)
	(gr_text "Mount"
		(at 16.5 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Down\n"
		(at 48.5 95.5 0)
		(layer "F.SilkS")
	)
	(gr_text "Thermocouple 1\n"
		(at 54.5 13.5 0)
		(layer "F.SilkS")
	)
	(gr_text "3Vo"
		(at 135.548995 33.554509 90)
		(layer "F.SilkS")
	)
	(gr_text "Vin"
		(at 133.008995 33.554509 90)
		(layer "F.SilkS")
	)
	(gr_text "Red -"
		(at 82.035549 21.759475 90)
		(layer "F.SilkS")
	)
	(gr_text "Smoke Sense PCB\nV4.0\n3/20/2026\n"
		(at 96.5 61.5 0)
		(layer "F.SilkS")
	)
	(gr_text "12V - 5V DC/DC Convert"
		(at 172 32 90)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 44.5 122.5 0)
		(layer "F.SilkS")
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 12 12) (xy 173 12) (xy 173 123) (xy 12 123)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 12 12) (xy 173 12) (xy 173 123) (xy 12 123)
			)
		)
	)
	(embedded_fonts no)
)
