(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(plotinvisibletext no)
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "HIGHVOLTAGE")
	(net 3 "Net-(D1-A)")
	(net 4 "Net-(D2-A)")
	(net 5 "Net-(D2-K)")
	(net 6 "Net-(D3-A)")
	(net 7 "Net-(D3-K)")
	(net 8 "Net-(IC1-DHL)")
	(net 9 "Net-(IC1-DLH)")
	(net 10 "Net-(IC1-EN{slash}HI)")
	(net 11 "Net-(IC1-HO)")
	(net 12 "Net-(IC1-HS_1)")
	(net 13 "Net-(IC1-LO)")
	(net 14 "Net-(IC1-PWM{slash}LI)")
	(net 15 "Net-(IC1-VDD)")
	(net 16 "Net-(J1-In)")
	(net 17 "Net-(Q2-D)")
	(net 18 "Net-(Q3-G)")
	(net 19 "VBOOST (80V)")
	(net 20 "VDropOff (~12 or 15V)")
	(net 21 "unconnected-(HIGHVOLTAGE1-Pad2)")
	(net 22 "unconnected-(HIGHVOLTAGE1-Pad3)")
	(net 23 "unconnected-(HIGHVOLTAGE1-Pad4)")
	(net 24 "unconnected-(HIGHVOLTAGE1-Pad5)")
	(net 25 "unconnected-(IC1-NC1-Pad14)")
	(net 26 "unconnected-(IC1-NC_1-Pad1)")
	(net 27 "unconnected-(IC1-NC_2-Pad11)")
	(net 28 "unconnected-(IC1-NC_3-Pad15)")
	(net 29 "unconnected-(J-1-Pad2)")
	(net 30 "unconnected-(J-1-Pad3)")
	(net 31 "unconnected-(J-1-Pad4)")
	(net 32 "unconnected-(J-1-Pad5)")
	(footprint "1_KICADPULSERFootPrint:DIO_RB160VAM_ROM"
		(layer "F.Cu")
		(at 118.364 47.8028 -90)
		(tags "RB578VAM100TR ")
		(property "Reference" "D1"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.9304 0 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.9304 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -0.7493 0 90)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.7493 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3208 0 270)
			(size 0.4572 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "VDropOff (~12 or 15V)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3208 0 270)
			(size 0.4572 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(D1-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(filled_areas_thickness no)
			(polygon
				(pts (xy 119.0117 46.7614) (xy 119.0117 48.8442) (xy 117.7163 48.8442) (xy 117.7163 46.7614))
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 63.5 59 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "RPullup1"
			(at 0.182 3.048 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(IC1-EN{slash}HI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(IC1-VDD)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:CONN_73099-2_POM"
		(layer "F.Cu")
		(at 145.796 49.022)
		(tags "73099-2 ")
		(property "Reference" "HIGHVOLTAGE1"
			(at -9.398 -0.762 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "73099-2"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "73099-2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_73099-2_POM")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.7178 2.7178)
			(drill 2.2098)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "HIGHVOLTAGE")
			(pinfunction "1_1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at -5.08 -6.35)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(HIGHVOLTAGE1-Pad2)")
			(pinfunction "2_2")
			(pintype "unspecified+no_connect")
		)
		(pad "3" thru_hole circle
			(at -5.08 3.81)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(HIGHVOLTAGE1-Pad3)")
			(pinfunction "3_3")
			(pintype "unspecified+no_connect")
		)
		(pad "4" thru_hole circle
			(at 5.08 3.81)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(HIGHVOLTAGE1-Pad4)")
			(pinfunction "4_4")
			(pintype "unspecified+no_connect")
		)
		(pad "5" thru_hole circle
			(at 5.08 -6.35)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(HIGHVOLTAGE1-Pad5)")
			(pinfunction "5_5")
			(pintype "unspecified+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 97.282 57.658)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "CBoost1"
			(at 9.3765 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 9.3765 1.27 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.254 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 19 "VBOOST (80V)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 113.932 72.644)
		(descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -2.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.4 0)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 5 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.4 0)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 4 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_3640_9110Metric_Pad2.10x10.45mm_HandSolder"
		(layer "F.Cu")
		(at 162.195 48.26 180)
		(descr "Capacitor SMD 3640 (9110 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size from: http://datasheets.avx.com/AVX-HV_MLCC.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0.143 -7.874 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 6.18 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.175 0 180)
			(size 2.1 10.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 16 "Net-(J1-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.175 0 180)
			(size 2.1 10.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 2 "HIGHVOLTAGE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_3640_9110Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 118.364 54.47 -90)
		(descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -2.28 270)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.28 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.4 0 270)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 3 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.4 0 270)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 4 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 90 54.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "CB1"
			(at 0 2.176 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(IC1-HS_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D3-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 68.0875 66 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "RHL1"
			(at 5.6035 -0.294 180)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(IC1-DHL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:DIO_RB160VAM_ROM"
		(layer "F.Cu")
		(at 113.5888 61.722)
		(tags "RB578VAM100TR ")
		(property "Reference" "D2"
			(at 0.0508 -2.286 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -0.7493 0 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.7493 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3208 0)
			(size 0.4572 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D2-K)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3208 0)
			(size 0.4572 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D2-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(filled_areas_thickness no)
			(polygon
				(pts (xy 112.5474 61.0743) (xy 114.6302 61.0743) (xy 114.6302 62.3697) (xy 112.5474 62.3697))
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 68 68.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "RLH1"
			(at -5.516 0.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(IC1-DLH)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 113.6385 67.056)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "CC1"
			(at 0.022 -1.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 1 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:TO544P521X1594X2574-3P"
		(layer "F.Cu")
		(at 129.54 54.864 90)
		(descr "TO-247-3L")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q3"
			(at -0.254 3.81 90)
			(layer "F.SilkS")
		)
		(property "Value" "C2M0025120D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://assets.wolfspeed.com/uploads/2024/01/Wolfspeed_C2M0025120D_data_sheet.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1200 V, 25 m, TO-247-3 package, Industrial qualified, Discrete SiC MOSFET"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "5.21"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "941-C2M0025120D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Wolfspeed/C2M0025120D?qs=EIEdgivfP%2FgDvLbUe6yqrg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Wolfspeed"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "C2M0025120D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.58 2.58)
			(drill 1.72)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 18 "Net-(Q3-G)")
			(pinfunction "G_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole circle
			(at 5.44 0 180)
			(size 2.58 2.58)
			(drill 1.72)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 2 "HIGHVOLTAGE")
			(pinfunction "D_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.88 0 180)
			(size 2.58 2.58)
			(drill 1.72)
			(layers "*.Cu" "*.Mask" "F.SilkS")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock:TerminalBlock_MaiXu_MX126-5.0-02P_1x02_P5.00mm"
		(layer "F.Cu")
		(at 58.928 49.276 180)
		(descr "terminal block MaiXu MX126-5.0-02P, 2 pins, pitch 5mm, size 10.5x7.8mm, drill diameter 1.3mm, pad diameter 2.8mm, https://www.lcsc.com/datasheet/lcsc_datasheet_2309150913_MAX-MX126-5-0-03P-GN01-Cu-S-A_C5188435.pdf")
		(tags "THT terminal block MaiXu MX126-5.0-02P pitch 5mm size 10.5x7.8mm drill 1.3mm pad 2.8mm")
		(property "Reference" "VDropOff1"
			(at 2.25 -5.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 1.016 5.08 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "terminal_block/MaiXu"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.25 2.65 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.089286)
			(net 20 "VDropOff (~12 or 15V)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_MaiXu_MX126-5.0-02P_1x02_P5.00mm.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:CONN_73099-2_POM"
		(layer "F.Cu")
		(at 146.05 61.976 180)
		(tags "73099-2 ")
		(property "Reference" "Ground"
			(at 9.398 -0.762 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "73099-0"
			(at 0 -1.27 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "73099-2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_73099-2_POM")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr through_hole dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 2.7178 2.7178)
			(drill 2.2098)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1_1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at -5.08 -6.35 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(J-1-Pad2)")
			(pinfunction "2_2")
			(pintype "unspecified+no_connect")
		)
		(pad "3" thru_hole circle
			(at -5.08 3.81 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(J-1-Pad3)")
			(pinfunction "3_3")
			(pintype "unspecified+no_connect")
		)
		(pad "4" thru_hole circle
			(at 5.08 3.81 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(J-1-Pad4)")
			(pinfunction "4_4")
			(pintype "unspecified+no_connect")
		)
		(pad "5" thru_hole circle
			(at 5.08 -6.35 180)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(J-1-Pad5)")
			(pinfunction "5_5")
			(pintype "unspecified+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 103.886 74.054 90)
		(descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "RD2"
			(at 0 -2.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.4 0 90)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 17 "Net-(Q2-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.4 0 90)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 5 "Net-(D2-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:NTypeRightAngle"
		(layer "F.Cu")
		(at 168.91 71.628 180)
		(property "Reference" "J1"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_Coaxial"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3 3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J1-In)")
			(pinfunction "In_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -5.1 -5.1 180)
			(size 3 3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -5.1 5.1 180)
			(size 3 3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.1 -5.1 180)
			(size 3 3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.1 5.1 180)
			(size 3 3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Ext_2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "1_KICADPULSERFootPrint:DIO_RB160VAM_ROM"
		(layer "F.Cu")
		(at 84 54.5 180)
		(tags "RB578VAM100TR ")
		(property "Reference" "D3"
			(at 0 2.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "D_Schottky"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.9304 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.9304 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.7493 0 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.7493 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3208 0 180)
			(size 0.4572 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D3-K)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.3208 0 180)
			(size 0.4572 0.8382)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D3-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(filled_areas_thickness no)
			(polygon
				(pts (xy 85.0414 55.1477) (xy 82.9586 55.1477) (xy 82.9586 53.8523) (xy 85.0414 53.8523))
			)
		)
		(embedded_fonts no)
	)
	(footprint "1_KICADPULSERFootPrint:IGD70R500D2SAUMA1"
		(layer "F.Cu")
		(at 92 62 90)
		(descr "PG‑TO252‑3_2026")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q1"
			(at 5.866 1.472 90)
			(layer "F.SilkS")
		)
		(property "Value" "IGD70R500D2SAUMA1"
			(at 0 0.01 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.infineon.com/assets/row/public/documents/24/49/infineon-igd70r500d2s-datasheet-en.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 700 V 3.4A (Tc) 11W (Tc) Surface Mount PG-TO252-3-U03 , -40C ~ 150C (TJ)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Infineon"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "IGD70R500D2SAUMA1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.01 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.28 4.21 90)
			(size 1.2 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(IC1-HO)")
			(pinfunction "G_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.09 90)
			(size 5.8 6.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC1-HS_1)")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.28 4.21 90)
			(size 1.2 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "VBOOST (80V)")
			(pinfunction "D_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "IGD70R500D2SAUMA1.stp"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:LMG1210RVRR"
		(layer "F.Cu")
		(at 79.1 63)
		(descr "RVR0019A")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 2.434 -3.818 0)
			(layer "F.SilkS")
		)
		(property "Value" "LMG1210RVRR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/lmg1210.pdf?ts=1777810937454"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Half-Bridge Gate Driver IC Non-Inverting 19-WQFN (3x4) -40C ~ 125C ,3A,200 V"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-LMG1210RVRR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LMG1210RVRR?qs=r5DSvlrkXmKqI241KOY62g%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LMG1210RVRR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.9 -1 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(IC1-NC_1-Pad1)")
			(pinfunction "NC_1_1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -1.9 -0.5 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "VDropOff (~12 or 15V)")
			(pinfunction "VIN_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.9 0 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS_1_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.9 0.5 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(IC1-VDD)")
			(pinfunction "VDD_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.9 1 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(IC1-DHL)")
			(pinfunction "DHL_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -1.25 1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(IC1-DLH)")
			(pinfunction "DLH_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -0.75 1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS_2_7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.25 1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(IC1-LO)")
			(pinfunction "LO_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0.75 1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC1-HS_1)")
			(pinfunction "HS_1_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.25 1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(IC1-HO)")
			(pinfunction "HO_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 1.9 1 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(IC1-NC_2-Pad11)")
			(pinfunction "NC_2_11")
			(pintype "passive+no_connect")
		)
		(pad "12" smd rect
			(at 1.9 0.5 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D3-K)")
			(pinfunction "HB_12")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 1.9 0 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC1-HS_1)")
			(pinfunction "HS_2_13")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 1.9 -0.5 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(IC1-NC1-Pad14)")
			(pinfunction "NC1_14")
			(pintype "passive+no_connect")
		)
		(pad "15" smd rect
			(at 1.9 -1 90)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(IC1-NC_3-Pad15)")
			(pinfunction "NC_3_15")
			(pintype "passive+no_connect")
		)
		(pad "16" smd rect
			(at 1.25 -1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC1-HS_1)")
			(pinfunction "HS_3_16")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at -0.25 -1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D3-A)")
			(pinfunction "BST_17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -0.75 -1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC1-EN{slash}HI)")
			(pinfunction "EN/HI_18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -1.25 -1.4)
			(size 0.25 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(IC1-PWM{slash}LI)")
			(pinfunction "PWM/LI_19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -0.75 0)
			(size 1.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS_3_20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 0.975 0)
			(size 0.75 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC1-HS_1)")
			(pinfunction "HS_4_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "LMG1210RVRR.stp"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:IGD70R500D2SAUMA1"
		(layer "F.Cu")
		(at 90.72 74.29)
		(descr "PG‑TO252‑3_2026")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q2"
			(at -6.138 0.132 0)
			(layer "F.SilkS")
		)
		(property "Value" "IGD70R500D2SAUMA1"
			(at 0 0.01 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.infineon.com/assets/row/public/documents/24/49/infineon-igd70r500d2s-datasheet-en.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 700 V 3.4A (Tc) 11W (Tc) Surface Mount PG-TO252-3-U03 , -40C ~ 150C (TJ)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Infineon"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "IGD70R500D2SAUMA1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.01 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.28 4.21)
			(size 1.2 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(IC1-LO)")
			(pinfunction "G_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.09)
			(size 5.8 6.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.28 4.21)
			(size 1.2 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(Q2-D)")
			(pinfunction "D_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "IGD70R500D2SAUMA1.stp"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 122.936 62.992)
		(descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "RD3"
			(at 0 -2.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.4 0)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 4 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.4 0)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 18 "Net-(Q3-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "1_KICADPULSERFootPrint:COAX4_CONBNC001_TEC"
		(layer "F.Cu")
		(at 71.2724 52.4764)
		(tags "CONBNC001 ")
		(property "Reference" "J5"
			(at 0.1016 -6.7564 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CONBNC001"
			(at 0.3556 -8.2804 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=CONBNC001&DocType=Data+Sheet&DocLang=English&PartCntxt=CONBNC001&DocFormat=pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "COAX4_CONBNC001_TEC")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.7018 1.7018)
			(drill 1.1938)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(IC1-PWM{slash}LI)")
			(pinfunction "SIGNAL_1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at -3.1496 -3.1496)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at -3.1496 3.1496)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND_3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 3.1496 3.1496)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND_4")
			(pintype "unspecified")
		)
		(pad "5" thru_hole circle
			(at 3.1496 -3.1496)
			(size 2.1082 2.1082)
			(drill 1.6002)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND_5")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 63.5 63.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "CDD1"
			(at -6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(IC1-VDD)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "F.Cu")
		(at 97.7515 54.864)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "Cboost2"
			(at 8.89 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 8.89 1.27 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 19 "VBOOST (80V)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 71.1375 61.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "CIN1"
			(at -2.8115 -1.302 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "VDropOff (~12 or 15V)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 103.886 63.64 -90)
		(descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "RD1"
			(at 0 -2.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.4 0 270)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 12 "Net-(IC1-HS_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.4 0 270)
			(size 1.4 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.178571)
			(net 5 "Net-(D2-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_MaiXu_MX126-5.0-02P_1x02_P5.00mm"
		(layer "F.Cu")
		(at 96.992 47.244 180)
		(descr "terminal block MaiXu MX126-5.0-02P, 2 pins, pitch 5mm, size 10.5x7.8mm, drill diameter 1.3mm, pad diameter 2.8mm, https://www.lcsc.com/datasheet/lcsc_datasheet_2309150913_MAX-MX126-5-0-03P-GN01-Cu-S-A_C5188435.pdf")
		(tags "THT terminal block MaiXu MX126-5.0-02P pitch 5mm size 10.5x7.8mm drill 1.3mm pad 2.8mm")
		(property "Reference" "Vboost1"
			(at 2.25 -5.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 2.25 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "terminal_block/MaiXu"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "KICADPULSER.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.25 2.65 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.089286)
			(net 19 "VBOOST (80V)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_MaiXu_MX126-5.0-02P_1x02_P5.00mm.step"
			(offset (xyz 0 0 0))
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts (xy 48.541562 40.386) (xy 180.086 40.386) (xy 180.114566 83.987798) (xy 48.541562 84.074))
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 126.871306 51.801126)
		(end 132.882075 51.839226)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 126.891203 46.736)
		(end 132.842 46.7741)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Gate Boosted Driver Circuit"
		(at 102.616 82.296 0)
		(layer "F.SilkS")
	)
	(zone
		(net 19)
		(net_name "VBOOST (80V)")
		(layer "F.Cu")
		(name "VBOOSTPAD")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(filled_areas_thickness no)
		(polygon
			(pts (xy 94.952158 60.445925) (xy 97.028 60.452) (xy 97.100099 45.47613) (xy 94.996 45.466))
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(filled_areas_thickness no)
		(polygon
			(pts
				(xy 49.531837 40.912995)
				(xy 179.794346 40.979896)
				(xy 179.772911 82.716396)
				(xy 49.23506 83.317459)
				(xy 49.276 40.922182)
			)
		)
	)
	(embedded_fonts no)
)
