(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 102.84 108.775)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Pad12)")
	(net 2 "Net-(J1-P25)")
	(net 3 "Net-(J1-Pad3)")
	(net 4 "Net-(J1-P15)")
	(net 5 "Net-(J1-Pad13)")
	(net 6 "Net-(J1-P16)")
	(net 7 "Net-(J1-Pad4)")
	(net 8 "Net-(J1-P24)")
	(net 9 "unconnected-(J2-Pad10)")
	(net 10 "unconnected-(J2-Pad28)")
	(net 11 "unconnected-(J2-Pad30)")
	(net 12 "unconnected-(J2-Pad29)")
	(net 13 "unconnected-(J2-Pad27)")
	(net 14 "Net-(J1-Pad6)")
	(net 15 "Net-(J1-Pad9)")
	(net 16 "Net-(J1-P22)")
	(net 17 "Net-(J1-Pad10)")
	(net 18 "Net-(J1-P18)")
	(net 19 "Net-(J1-P21)")
	(net 20 "Net-(J1-Pad7)")
	(net 21 "Net-(J1-P19)")
	(net 22 "Net-(J2-Pad2)")
	(net 23 "Net-(J3-P15)")
	(net 24 "Net-(J2-Pad25)")
	(net 25 "Net-(J2-Pad23)")
	(net 26 "Net-(J2-Pad6)")
	(net 27 "Net-(J3-P16)")
	(net 28 "Net-(J3-P25)")
	(net 29 "Net-(J2-Pad4)")
	(net 30 "Net-(J2-Pad9)")
	(net 31 "Net-(J3-P24)")
	(net 32 "Net-(J3-P18)")
	(net 33 "Net-(J3-P19)")
	(net 34 "Net-(J2-Pad21)")
	(net 35 "Net-(J3-P21)")
	(net 36 "Net-(J2-Pad8)")
	(net 37 "Net-(J3-P22)")
	(net 38 "GND")
	(footprint "Connector_Dsub:DSUB-25_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm"
		(layer "F.Cu")
		(at 153.16 94.495 90)
		(descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, socket (female), pitch 2.77x2.84mm, pin-PCB-offset 4.94mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 4.94mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "25-pin D-Sub connector horizontal angled 90deg THT socket pitch 2.77x2.84mm pin-PCB-offset 4.94mm mounting-holes-distance 47.1mm mounting-hole-offset 4.94mm")
		(property "Reference" "J3"
			(at -16.62 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "DB25_Socket_MountingHoles"
			(at -16.62 15.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "25-pin D-SUB connector, socket (female), Mounting Hole"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Socket*")
		(sheetname "/")
		(sheetfile "OVC_to_3726_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -16.62 11.265 90)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -40.17 2.84 90)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 6.93 2.84 90)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J2-Pad8)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J2-Pad9)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -13.85 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J2-Pad6)")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -16.62 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J2-Pad25)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -19.39 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -22.16 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J2-Pad4)")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -24.93 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J2-Pad23)")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -27.7 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -30.47 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pad2)")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -33.24 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J2-Pad21)")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -1.385 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -4.155 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J3-P15)")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at -6.925 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J3-P16)")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -9.695 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -12.465 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J3-P18)")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at -15.235 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J3-P19)")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at -18.005 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at -20.775 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J3-P21)")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at -23.545 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J3-P22)")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at -26.315 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at -29.085 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J3-P24)")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at -31.855 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J3-P25)")
			(pinfunction "P25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 154.84 144.775)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "M3"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Dsub:DSUB-25_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm"
		(layer "F.Cu")
		(at 153.16 39.495 90)
		(descr "25-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, socket (female), pitch 2.77x2.84mm, pin-PCB-offset 4.94mm, distance of mounting holes 47.1mm, distance of mounting holes to PCB edge 4.94mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "25-pin D-Sub connector horizontal angled 90deg THT socket pitch 2.77x2.84mm pin-PCB-offset 4.94mm mounting-holes-distance 47.1mm mounting-hole-offset 4.94mm")
		(property "Reference" "J1"
			(at -16.62 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "DB25_Socket_MountingHoles"
			(at -16.62 15.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "25-pin D-SUB connector, socket (female), Mounting Hole"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Socket*")
		(sheetname "/")
		(sheetfile "OVC_to_3726_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -16.62 11.265 90)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -40.17 2.84 90)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 6.93 2.84 90)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pad3)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -13.85 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J1-Pad6)")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -16.62 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J1-Pad7)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -19.39 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -22.16 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J1-Pad9)")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -24.93 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J1-Pad10)")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -27.7 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -30.47 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pad12)")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -33.24 0 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pad13)")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -1.385 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -4.155 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-P15)")
			(pinfunction "P15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at -6.925 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-P16)")
			(pinfunction "P16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -9.695 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -12.465 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J1-P18)")
			(pinfunction "P18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at -15.235 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J1-P19)")
			(pinfunction "P19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at -18.005 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at -20.775 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J1-P21)")
			(pinfunction "P21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at -23.545 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J1-P22)")
			(pinfunction "P22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at -26.315 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "P23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at -29.085 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-P24)")
			(pinfunction "P24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at -31.855 2.84 90)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-P25)")
			(pinfunction "P25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-25_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 100.84 21.775)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "M3"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_Dsub:DSUB-37_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm"
		(layer "F.Cu")
		(at 102.84 108.775 -90)
		(descr "37-pin D-Sub connector, horizontal/angled (90 deg), THT-mount, socket (female), pitch 2.77x2.84mm, pin-PCB-offset 4.94mm, distance of mounting holes 63.5mm, distance of mounting holes to PCB edge 4.94mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "37-pin D-Sub connector horizontal angled 90deg THT socket pitch 2.77x2.84mm pin-PCB-offset 4.94mm mounting-holes-distance 63.5mm mounting-hole-offset 4.94mm")
		(property "Reference" "J2"
			(at -24.93 -2.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "DC37_Socket_MountingHoles"
			(at -24.93 15.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "37-pin D-SUB connector, socket (female), Mounting Hole"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Socket*")
		(sheetname "/")
		(sheetfile "OVC_to_3726_breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -24.93 11.265 90)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -56.68 2.84 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 6.82 2.84 270)
			(size 4 4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "GND")
			(pinfunction "PAD")
			(pintype "passive")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J3-P24)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.77 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J2-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.54 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(J3-P21)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -8.31 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J2-Pad4)")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -11.08 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J3-P18)")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -13.85 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J2-Pad6)")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -16.62 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J3-P15)")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -19.39 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J2-Pad8)")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -22.16 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J2-Pad9)")
			(pinfunction "9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -24.93 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(J2-Pad10)")
			(pinfunction "10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at -27.7 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-P25)")
			(pinfunction "11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -30.47 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J1-P24)")
			(pinfunction "12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at -33.24 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J1-Pad12)")
			(pinfunction "13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -36.01 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J1-P21)")
			(pinfunction "14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at -38.78 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J1-Pad9)")
			(pinfunction "15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at -41.55 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J1-P18)")
			(pinfunction "16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at -44.32 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J1-Pad6)")
			(pinfunction "17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -47.09 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-P15)")
			(pinfunction "18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at -49.86 0 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J1-Pad3)")
			(pinfunction "19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at -1.385 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J3-P25)")
			(pinfunction "20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at -4.155 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J2-Pad21)")
			(pinfunction "21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at -6.925 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(J3-P22)")
			(pinfunction "22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at -9.695 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J2-Pad23)")
			(pinfunction "23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at -12.465 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J3-P19)")
			(pinfunction "24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at -15.235 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J2-Pad25)")
			(pinfunction "25")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at -18.005 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J3-P16)")
			(pinfunction "26")
			(pintype "passive")
		)
		(pad "27" thru_hole circle
			(at -20.775 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J2-Pad27)")
			(pinfunction "27")
			(pintype "passive")
		)
		(pad "28" thru_hole circle
			(at -23.545 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(J2-Pad28)")
			(pinfunction "28")
			(pintype "passive")
		)
		(pad "29" thru_hole circle
			(at -26.315 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J2-Pad29)")
			(pinfunction "29")
			(pintype "passive")
		)
		(pad "30" thru_hole circle
			(at -29.085 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J2-Pad30)")
			(pinfunction "30")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at -31.855 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-Pad13)")
			(pinfunction "31")
			(pintype "passive")
		)
		(pad "32" thru_hole circle
			(at -34.625 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J1-P22)")
			(pinfunction "32")
			(pintype "passive")
		)
		(pad "33" thru_hole circle
			(at -37.395 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J1-Pad10)")
			(pinfunction "33")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at -40.165 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J1-P19)")
			(pinfunction "34")
			(pintype "passive")
		)
		(pad "35" thru_hole circle
			(at -42.935 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J1-Pad7)")
			(pinfunction "35")
			(pintype "passive")
		)
		(pad "36" thru_hole circle
			(at -45.705 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-P16)")
			(pinfunction "36")
			(pintype "passive")
		)
		(pad "37" thru_hole circle
			(at -48.475 2.84 270)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pad4)")
			(pinfunction "37")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-37_Socket_Horizontal_P2.77x2.84mm_EdgePinOffset4.94mm_Housed_MountingHolesOffset4.94mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 154.84 21.775)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "M3"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 100.84 144.775)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "M3"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_DIN965_Pad"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 95 16.13)
		(end 161.34 151)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "LS 3726\nInput 1"
		(at 147.84 58.775 90)
		(layer "F.SilkS")
	)
	(gr_text "ISOLATE FROM\nOTHER GROUNDS"
		(at 141.84 83.775 90)
		(layer "F.SilkS")
	)
	(gr_text "Lower OVC\nFeedthrough"
		(at 106.84 49.775 270)
		(layer "F.SilkS")
	)
	(gr_text "Taj Dyson\n2-18-2026\nSLAC National Accelerator Laboratory"
		(at 127.84 139.775 0)
		(layer "F.SilkS")
	)
	(gr_text "LS 3726\nInput 2"
		(at 147.84 113.775 90)
		(layer "F.SilkS")
	)
	(gr_text "GROUNDED TO FRIDGE\nVIA CABLE SHIELD"
		(at 126.84 83.775 90)
		(layer "F.SilkS")
	)
	(gr_text "J1"
		(at 84.9125 134.21 90)
		(layer "F.Fab")
	)
	(zone
		(net 38)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 159 149) (xy 97 149) (xy 97 18) (xy 159 18)
			)
		)
	)
	(embedded_fonts no)
)
