(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Floppy-80 Model 1k")
		(date "2025-11-15")
		(rev "1.0")
		(company "kiwisincebirth")
		(comment 2 "with standard 40pin IDC pin header")
		(comment 3 "Floppy-80 supporting TRS-80 Model 1k")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3V3")
	(net 3 "/D7")
	(net 4 "/D6")
	(net 5 "/D5")
	(net 6 "/D4")
	(net 7 "/D3")
	(net 8 "/D2")
	(net 9 "/D1")
	(net 10 "/D0")
	(net 11 "/A1")
	(net 12 "/A0")
	(net 13 "/DIR")
	(net 14 "/MREQ'")
	(net 15 "/~{IN}")
	(net 16 "/~{RAS}")
	(net 17 "/~{WR}")
	(net 18 "/~{WAIT}")
	(net 19 "/~{RD}")
	(net 20 "unconnected-(J2-Pin_3-Pad3)")
	(net 21 "unconnected-(J2-Pin_14-Pad14)")
	(net 22 "/~{INT}")
	(net 23 "/~{OUT}")
	(net 24 "unconnected-(J2-Pin_23-Pad23)")
	(net 25 "/~{SYSRES}")
	(net 26 "/A10")
	(net 27 "/A12")
	(net 28 "/A13")
	(net 29 "/A15")
	(net 30 "/A11")
	(net 31 "/A14")
	(net 32 "/A8")
	(net 33 "/CD")
	(net 34 "/WAIT'")
	(net 35 "+5V")
	(net 36 "unconnected-(J2-Pin_16-Pad16)")
	(net 37 "Net-(D1-K)")
	(net 38 "/PD5")
	(net 39 "/PD4")
	(net 40 "/PD6")
	(net 41 "/PD3")
	(net 42 "/A9")
	(net 43 "/PD2")
	(net 44 "/PD1")
	(net 45 "/PD7")
	(net 46 "/A4")
	(net 47 "/PD0")
	(net 48 "/A3")
	(net 49 "/A5")
	(net 50 "/A7")
	(net 51 "/A6")
	(net 52 "/A2")
	(net 53 "Net-(J3-DAT2)")
	(net 54 "Net-(J3-DAT1)")
	(net 55 "unconnected-(U1-B3-Pad19)")
	(net 56 "unconnected-(U1-A2-Pad4)")
	(net 57 "unconnected-(U1-B2-Pad20)")
	(net 58 "unconnected-(U1-A3-Pad5)")
	(net 59 "/INT'")
	(net 60 "unconnected-(U2-VBUS-Pad40)")
	(net 61 "/IN'")
	(net 62 "/RD'")
	(net 63 "/WR'")
	(net 64 "/ADDRL_OE")
	(net 65 "/DATAB_OE")
	(net 66 "/OUT'")
	(net 67 "/ADDRH_OE")
	(net 68 "unconnected-(U2-ADC_VREF-Pad35)")
	(net 69 "unconnected-(U2-RUN-Pad30)")
	(net 70 "/SYSRES'")
	(net 71 "unconnected-(U2-3V3_EN-Pad37)")
	(net 72 "Net-(U2-GPIO6)")
	(net 73 "unconnected-(J3-WRITE_PROTECT-Pad11)")
	(net 74 "/MOSI")
	(net 75 "/CS_CD")
	(net 76 "/SCLK")
	(net 77 "/MISO")
	(net 78 "unconnected-(U2-SWDIO-PadD3)")
	(net 79 "unconnected-(U2-SWCLK-PadD1)")
	(footprint "Connector_Card:SD_Hirose_DM1AA_SF_PEJ82"
		(layer "F.Cu")
		(at 157.75 106.34)
		(descr "SD, SMD, top-mount, push-push (https://www.hirose.com/product/document?clcode=CL0609-0004-8-82&productname=DM1AA-SF-PEJ(82)&series=DM1&documenttype=2DDrawing&lang=en&documentid=0000915301)")
		(tags "SD card connector")
		(property "Reference" "J3"
			(at 0 -0.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "SD_Card_Receptacle"
			(at -0.6 10.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://portal.fciconnect.com/Comergent//fci/drawing/10067847.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SD card receptacle"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SD*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -11.9 -12.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 10.5 -12.75)
			(size 1.3 1.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at 6.075 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "/CS_CD")
			(pinfunction "CD/DAT3")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at 3.575 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/MOSI")
			(pinfunction "CMD")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at 1.075 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -1.425 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3V3")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -3.925 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "/SCLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -6.425 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at -8.85 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "/MISO")
			(pinfunction "DAT0")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -10.55 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(J3-DAT1)")
			(pinfunction "DAT1")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at 8.575 -14.95)
			(size 1.1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "Net-(J3-DAT2)")
			(pinfunction "DAT2")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -13.6 -3.55)
			(size 2 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/CD")
			(pinfunction "CARD_DETECT")
			(pintype "output")
		)
		(pad "11" smd rect
			(at -13.6 5.4)
			(size 2 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "unconnected-(J3-WRITE_PROTECT-Pad11)")
			(pinfunction "WRITE_PROTECT")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at -13.6 8)
			(size 2 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHELL1")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -14.5 -8.2)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -14.5 10.45)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 14.5 -8.2)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 14.5 10.45)
			(size 2 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHELL2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3AT-SF-PEJM5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 2 2 1.5)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 166.34 84.08 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -2.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "A106056CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Cost" "0.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 53 "Net-(J3-DAT2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 152.77 84.79)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 3.97 0.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "A106056CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Cost" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 54 "Net-(J3-DAT1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "FDC:PinHeader_2x20_P2.54mm_Even_Odd_Vertical"
		(layer "F.Cu")
		(at 123.635 54.115 90)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "J2"
			(at 5.015 3.825 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x20_Odd_Even"
			(at 1.27 50.59 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "A31723-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "A31723-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Cost" "3.69"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 24.13 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/~{RAS}")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/~{SYSRES}")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J2-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole oval
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/A10")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/A12")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/A13")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/A15")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "9" thru_hole oval
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/A11")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/A14")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "/A8")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole oval
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/~{OUT}")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole oval
			(at 2.54 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/~{WR}")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole oval
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J2-Pin_14-Pad14)")
			(pinfunction "Pin_14")
			(pintype "passive+no_connect")
		)
		(pad "15" thru_hole oval
			(at 2.54 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/~{RD}")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole oval
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(J2-Pin_16-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
		)
		(pad "17" thru_hole oval
			(at 2.54 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/A9")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole oval
			(at 0 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/D4")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole oval
			(at 2.54 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/~{IN}")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole oval
			(at 0 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/D7")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole oval
			(at 2.54 25.4 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/~{INT}")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole oval
			(at 0 25.4 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/D1")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole oval
			(at 2.54 27.94 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J2-Pin_23-Pad23)")
			(pinfunction "Pin_23")
			(pintype "passive+no_connect")
		)
		(pad "24" thru_hole oval
			(at 0 27.94 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/D6")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole oval
			(at 2.54 30.48 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/A0")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole oval
			(at 0 30.48 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/D3")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole oval
			(at 2.54 33.02 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/A1")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole oval
			(at 0 33.02 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/D5")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole oval
			(at 2.54 35.56 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_29")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "30" thru_hole oval
			(at 0 35.56 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/D0")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole oval
			(at 2.54 38.1 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "/A4")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole oval
			(at 0 38.1 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/D2")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole oval
			(at 2.54 40.64 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/~{WAIT}")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole oval
			(at 0 40.64 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/A3")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" thru_hole oval
			(at 2.54 43.18 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/A5")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" thru_hole oval
			(at 0 43.18 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/A7")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" thru_hole oval
			(at 2.54 45.72 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_37")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "38" thru_hole oval
			(at 0 45.72 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/A6")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" thru_hole oval
			(at 2.54 48.26 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_39")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "40" thru_hole oval
			(at 0 48.26 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "/A2")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x20_P2.54mm_Vertical.wrl"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -180 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 152.71 87.495 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at -3.66 -0.085 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 116.015 54.115 90)
		(descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x02 2.54mm double row")
		(property "Reference" "J1"
			(at 5.065 -0.575 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Odd_Even"
			(at 1.27 4.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "+5V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -180 -0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 112.21 91.13)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H1"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
		(layer "B.Cu")
		(at 154.02 71.45 -90)
		(descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U3"
			(at 0.01 8.61 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SN74LVCC4245ADWR"
			(at 0 -8.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74avc8t245.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "1.83"
			(at 66.5226 -211.3026 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "296-26634-1-ND"
			(at 66.5226 -211.3026 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 66.5226 -211.3026 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x7.8mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/DIR")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/D4")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/D7")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/D1")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/D6")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/D3")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/D5")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/D0")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/D2")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/PD2")
			(pinfunction "B8")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/PD0")
			(pinfunction "B7")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/PD5")
			(pinfunction "B6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/PD3")
			(pinfunction "B5")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/PD6")
			(pinfunction "B4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/PD1")
			(pinfunction "B3")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/PD7")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/PD4")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/DATAB_OE")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
		(layer "B.Cu")
		(at 172.29 71.43 -90)
		(descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U5"
			(at 0.03 8.75 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SN74LVCC4245ADWR"
			(at 0 -8.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74avc8t245.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "1.83"
			(at 48.514 -193.294 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "296-26634-1-ND"
			(at 48.514 -193.294 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 48.514 -193.294 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x7.8mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "+5V")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A0")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/A1")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/A4")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/A5")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/A3")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/A7")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/A6")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 52 "/A2")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/PD2")
			(pinfunction "B8")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/PD6")
			(pinfunction "B7")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/PD7")
			(pinfunction "B6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/PD3")
			(pinfunction "B5")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/PD5")
			(pinfunction "B4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/PD4")
			(pinfunction "B3")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/PD1")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/PD0")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/ADDRL_OE")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 129.09 78.85 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 2.78 -0.05 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 206.3496 53.4924 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 206.3496 53.4924 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 206.3496 53.4924 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 129.12 64.34 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 2.6924 -0.1524 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 61.595 -198.247 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 61.595 -198.247 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 61.595 -198.247 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 35 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 147.12 78.68 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 2.8 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 224.7138 71.2978 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 224.7138 71.2978 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 224.7138 71.2978 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 146.61 64.24 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 2.667 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 79.9084 -216.154 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 79.9084 -216.154 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 79.9084 -216.154 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 35 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:RaspberryPi_Pico_SMD_HandSolder"
		(layer "B.Cu")
		(at 154.98 97.995 90)
		(descr "Raspberry Pi Pico (non-W) surface-mount footprint with debug pads for hand soldering, supports Raspberry Pi Pico 2 (non-W), https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf")
		(tags "module usb pcb swd")
		(property "Reference" "U2"
			(at 1.105 -27.55 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "RaspberryPi_Pico"
			(at 0 -27.94 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Versatile and inexpensive microcontroller module (with debug pins) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash; also supports Raspberry Pi Pico 2"
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "2648-SC0915CT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "4.00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RaspberryPi?Pico?SMD*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "Exposed Copper Keep Out"
			(at -2.5 14.25 180)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Exposed"
			(at 0 24.6175 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep"
			(at 1 5 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Copper"
			(at 0 23.9825 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep"
			(at 0 21.3175 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "USB Cable"
			(at 0 38.735 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Keep Out"
			(at 0 36.195 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Copper"
			(at 1 5.635 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Out"
			(at 0 20.6825 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "Copper Keepouts shown on Dwgs layer"
			(at 0.469 48.413 90)
			(layer "Cmts.User")
		)
		(fp_text user "Out"
			(at 1 4.365 270)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "AGND Plane"
			(at 5.08 7.62 180)
			(unlocked yes)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "" smd rect
			(at -8.89 -24.13 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -21.59 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -19.05 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -16.51 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -13.97 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -11.43 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -8.89 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -6.35 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -3.81 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 -1.27 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 1.27 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 3.81 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 6.35 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 8.89 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 11.43 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 13.97 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 16.51 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 19.05 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 21.59 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at -8.89 24.13 90)
			(size 3.8 2.2)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" np_thru_hole circle
			(at -2.725 24 90)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Mask")
		)
		(pad "" smd rect
			(at -2.54 -23.9 90)
			(size 2.2 3.8)
			(drill
				(offset 0 -0.8)
			)
			(layers "B.Paste")
		)
		(pad "" np_thru_hole circle
			(at -2.425 20.97 90)
			(size 1.85 1.85)
			(drill 1.85)
			(layers "*.Mask")
		)
		(pad "" smd rect
			(at 0 -23.9 90)
			(size 2.2 3.8)
			(drill
				(offset 0 -0.8)
			)
			(layers "B.Paste")
		)
		(pad "" np_thru_hole circle
			(at 2.425 20.97 90)
			(size 1.85 1.85)
			(drill 1.85)
			(layers "*.Mask")
		)
		(pad "" smd rect
			(at 2.54 -23.9 90)
			(size 2.2 3.8)
			(drill
				(offset 0 -0.8)
			)
			(layers "B.Paste")
		)
		(pad "" np_thru_hole circle
			(at 2.725 24 90)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Mask")
		)
		(pad "" smd rect
			(at 8.89 -24.13 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -21.59 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -19.05 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -16.51 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -13.97 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -11.43 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -8.89 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -6.35 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -3.81 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 -1.27 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 1.27 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 3.81 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 6.35 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 8.89 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 11.43 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 13.97 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 16.51 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 19.05 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 21.59 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "" smd rect
			(at 8.89 24.13 90)
			(size 3.8 2.2)
			(drill
				(offset 0.8 0)
			)
			(layers "B.Paste")
		)
		(pad "1" smd custom
			(at -9.69 24.13 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 59 "/INT'")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 0.6) (xy -1.6 -0.6) (xy -1.4 -0.8) (xy 0.8 -0.8) (xy 0.8 0.8) (xy -1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd roundrect
			(at -9.69 21.59 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 34 "/WAIT'")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" smd custom
			(at -9.69 19.05 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 0.6) (xy 1.6 -0.6) (xy 1.4 -0.8) (xy -0.8 -0.8) (xy -0.8 0.8) (xy 1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "4" smd roundrect
			(at -9.69 16.51 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 76 "/SCLK")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -9.69 13.97 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 74 "/MOSI")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -9.69 11.43 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 77 "/MISO")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -9.69 8.89 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 75 "/CS_CD")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" smd custom
			(at -9.69 6.35 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 0.6) (xy 1.6 -0.6) (xy 1.4 -0.8) (xy -0.8 -0.8) (xy -0.8 0.8) (xy 1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "9" smd roundrect
			(at -9.69 3.81 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 72 "Net-(U2-GPIO6)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -9.69 1.27 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 64 "/ADDRL_OE")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -9.69 -1.27 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 65 "/DATAB_OE")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -9.69 -3.81 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 67 "/ADDRH_OE")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" smd custom
			(at -9.69 -6.35 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 0.6) (xy 1.6 -0.6) (xy 1.4 -0.8) (xy -0.8 -0.8) (xy -0.8 0.8) (xy 1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "14" smd roundrect
			(at -9.69 -8.89 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 61 "/IN'")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -9.69 -11.43 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 62 "/RD'")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -9.69 -13.97 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 63 "/WR'")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -9.69 -16.51 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 66 "/OUT'")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "18" smd custom
			(at -9.69 -19.05 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center -0.8 0)
					(end 0 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 1.6 0.6) (xy 1.6 -0.6) (xy 1.4 -0.8) (xy -0.8 -0.8) (xy -0.8 0.8) (xy 1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 0.6)
					(end 1.6 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.4 -0.6)
					(end 1.6 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "19" smd roundrect
			(at -9.69 -21.59 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 14 "/MREQ'")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -9.69 -24.13 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 47 "/PD0")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 9.69 -24.13 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 44 "/PD1")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 9.69 -21.59 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 43 "/PD2")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "23" smd custom
			(at 9.69 -19.05 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 0.6) (xy -1.6 -0.6) (xy -1.4 -0.8) (xy 0.8 -0.8) (xy 0.8 0.8) (xy -1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "24" smd roundrect
			(at 9.69 -16.51 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 41 "/PD3")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at 9.69 -13.97 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 39 "/PD4")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 9.69 -11.43 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 38 "/PD5")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "27" smd roundrect
			(at 9.69 -8.89 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 40 "/PD6")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "28" smd custom
			(at 9.69 -6.35 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 0.6) (xy -1.6 -0.6) (xy -1.4 -0.8) (xy 0.8 -0.8) (xy 0.8 0.8) (xy -1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "29" smd roundrect
			(at 9.69 -3.81 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 45 "/PD7")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 9.69 -1.27 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 69 "unconnected-(U2-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "passive+no_connect")
		)
		(pad "31" smd roundrect
			(at 9.69 1.27 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 13 "/DIR")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 9.69 3.81 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 70 "/SYSRES'")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "33" smd custom
			(at 9.69 6.35 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_out")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 0.6) (xy -1.6 -0.6) (xy -1.4 -0.8) (xy 0.8 -0.8) (xy 0.8 0.8) (xy -1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "34" smd roundrect
			(at 9.69 8.89 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 33 "/CD")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 9.69 11.43 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 68 "unconnected-(U2-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "power_in+no_connect")
		)
		(pad "36" smd roundrect
			(at 9.69 13.97 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 2 "+3V3")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "37" smd roundrect
			(at 9.69 16.51 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 71 "unconnected-(U2-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "passive+no_connect")
		)
		(pad "38" smd custom
			(at 9.69 19.05 90)
			(size 1.6 0.8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0.8 0)
					(end 1.6 0)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy -1.6 0.6) (xy -1.6 -0.6) (xy -1.4 -0.8) (xy 0.8 -0.8) (xy 0.8 0.8) (xy -1.4 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 0.6)
					(end -1.2 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -1.4 -0.6)
					(end -1.2 -0.6)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "39" smd roundrect
			(at 9.69 21.59 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 35 "+5V")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at 9.69 24.13 90)
			(size 3.2 1.6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 60 "unconnected-(U2-VBUS-Pad40)")
			(pinfunction "VBUS")
			(pintype "power_out+no_connect")
		)
		(pad "D1" smd roundrect
			(at -2.54 -23.9)
			(size 3.2 1.6)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 79 "unconnected-(U2-SWCLK-PadD1)")
			(pinfunction "SWCLK")
			(pintype "input+no_connect")
		)
		(pad "D2" smd custom
			(at 0 -23.9 180)
			(size 1.6 1.6)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.8 0.6) (xy -0.8 -0.6) (xy -0.6 -0.8) (xy 1.6 -0.8) (xy 1.6 0.8) (xy -0.6 0.8)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 -0.6)
					(end -0.4 -0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center -0.6 0.6)
					(end -0.4 0.6)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 1.6 0)
					(end 2.4 0)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "D3" smd roundrect
			(at 2.54 -23.9)
			(size 3.2 1.6)
			(drill
				(offset -0.8 0)
			)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.5)
			(net 78 "unconnected-(U2-SWDIO-PadD3)")
			(pinfunction "SWDIO")
			(pintype "bidirectional+no_connect")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP7")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 159.03 96.995) (xy 159.03 96.545) (xy 159.032139 96.479455) (xy 159.066067 96.352833) (xy 159.131612 96.239306)
					(xy 159.224306 96.146612) (xy 159.337833 96.081067) (xy 159.464455 96.047139) (xy 159.53 96.045)
					(xy 160.43 96.045) (xy 160.495545 96.047139) (xy 160.622167 96.081067) (xy 160.735694 96.146612)
					(xy 160.828388 96.239306) (xy 160.893933 96.352833) (xy 160.927861 96.479455) (xy 160.93 96.545)
					(xy 160.93 96.995)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP7")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 160.495545 97.942861) (xy 160.622167 97.908932) (xy 160.735694 97.843388) (xy 160.828388 97.750694)
					(xy 160.893932 97.637167) (xy 160.927861 97.510545) (xy 160.93 97.445) (xy 160.93 96.995) (xy 159.03 96.995)
					(xy 159.03 97.445) (xy 159.032139 97.510545) (xy 159.066068 97.637167) (xy 159.131612 97.750694)
					(xy 159.224306 97.843388) (xy 159.337833 97.908932) (xy 159.464455 97.942861) (xy 159.53 97.945)
					(xy 160.43 97.945)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP6")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 165.032139 101.010545) (xy 165.066068 101.137167) (xy 165.131612 101.250694) (xy 165.224306 101.343388)
					(xy 165.337833 101.408932) (xy 165.464455 101.442861) (xy 165.53 101.445) (xy 169.23 101.445) (xy 169.23 99.545)
					(xy 165.53 99.545) (xy 165.464455 99.547139) (xy 165.337833 99.581068) (xy 165.224306 99.646612)
					(xy 165.131612 99.739306) (xy 165.066068 99.852833) (xy 165.032139 99.979455) (xy 165.03 100.045)
					(xy 165.03 100.945)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP4")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 169.23 99.545) (xy 172.93 99.545) (xy 172.995545 99.547139) (xy 173.122167 99.581067) (xy 173.235694 99.646612)
					(xy 173.328388 99.739306) (xy 173.393933 99.852833) (xy 173.427861 99.979455) (xy 173.43 100.045)
					(xy 173.43 100.945) (xy 173.427861 101.010545) (xy 173.393933 101.137167) (xy 173.328388 101.250694)
					(xy 173.235694 101.343388) (xy 173.122167 101.408933) (xy 172.995545 101.442861) (xy 172.93 101.445)
					(xy 169.23 101.445)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP1")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 175.03 97.995) (xy 175.03 97.545) (xy 175.032139 97.479455) (xy 175.066067 97.352833) (xy 175.131612 97.239306)
					(xy 175.224306 97.146612) (xy 175.337833 97.081067) (xy 175.464455 97.047139) (xy 175.53 97.045)
					(xy 176.43 97.045) (xy 176.495545 97.047139) (xy 176.622167 97.081067) (xy 176.735694 97.146612)
					(xy 176.828388 97.239306) (xy 176.893933 97.352833) (xy 176.927861 97.479455) (xy 176.93 97.545)
					(xy 176.93 97.995)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP1")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 176.495545 98.942861) (xy 176.622167 98.908932) (xy 176.735694 98.843388) (xy 176.828388 98.750694)
					(xy 176.893932 98.637167) (xy 176.927861 98.510545) (xy 176.93 98.445) (xy 176.93 97.995) (xy 175.03 97.995)
					(xy 175.03 98.445) (xy 175.032139 98.510545) (xy 175.066068 98.637167) (xy 175.131612 98.750694)
					(xy 175.224306 98.843388) (xy 175.337833 98.908932) (xy 175.464455 98.942861) (xy 175.53 98.945)
					(xy 176.43 98.945)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP2")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 178.315 96.995) (xy 178.315 96.545) (xy 178.317139 96.479455) (xy 178.351067 96.352833) (xy 178.416612 96.239306)
					(xy 178.509306 96.146612) (xy 178.622833 96.081067) (xy 178.749455 96.047139) (xy 178.815 96.045)
					(xy 179.715 96.045) (xy 179.780545 96.047139) (xy 179.907167 96.081067) (xy 180.020694 96.146612)
					(xy 180.113388 96.239306) (xy 180.178933 96.352833) (xy 180.212861 96.479455) (xy 180.215 96.545)
					(xy 180.215 96.995)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP3")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 178.33 98.995) (xy 178.33 98.545) (xy 178.332139 98.479455) (xy 178.366067 98.352833) (xy 178.431612 98.239306)
					(xy 178.524306 98.146612) (xy 178.637833 98.081067) (xy 178.764455 98.047139) (xy 178.83 98.045)
					(xy 179.73 98.045) (xy 179.795545 98.047139) (xy 179.922167 98.081067) (xy 180.035694 98.146612)
					(xy 180.128388 98.239306) (xy 180.193933 98.352833) (xy 180.227861 98.479455) (xy 180.23 98.545)
					(xy 180.23 98.995)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP2")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 179.780545 97.942861) (xy 179.907167 97.908932) (xy 180.020694 97.843388) (xy 180.113388 97.750694)
					(xy 180.178932 97.637167) (xy 180.212861 97.510545) (xy 180.215 97.445) (xy 180.215 96.995) (xy 178.315 96.995)
					(xy 178.315 97.445) (xy 178.317139 97.510545) (xy 178.351068 97.637167) (xy 178.416612 97.750694)
					(xy 178.509306 97.843388) (xy 178.622833 97.908932) (xy 178.749455 97.942861) (xy 178.815 97.945)
					(xy 179.715 97.945)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "B.Cu" "B.Paste")
			(name "Pad Keep Out TP3")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 179.795545 99.942861) (xy 179.922167 99.908932) (xy 180.035694 99.843388) (xy 180.128388 99.750694)
					(xy 180.193932 99.637167) (xy 180.227861 99.510545) (xy 180.23 99.445) (xy 180.23 98.995) (xy 178.33 98.995)
					(xy 178.33 99.445) (xy 178.332139 99.510545) (xy 178.366068 99.637167) (xy 178.431612 99.750694)
					(xy 178.524306 99.843388) (xy 178.637833 99.908932) (xy 178.764455 99.942861) (xy 178.83 99.945)
					(xy 179.73 99.945)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "Edge.Cuts")
			(name "Board Keep Out USB Cable")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 202.63 104.195) (xy 202.63 91.795) (xy 182.23 91.795) (xy 182.23 104.195)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.CrtYd")
			(name "USB Cable Keep Out")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 182.68 103.745) (xy 182.68 101.935) (xy 182.28 101.935) (xy 182.28 94.055) (xy 182.68 94.055)
					(xy 182.68 92.245) (xy 202.18 92.245) (xy 202.18 103.745)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/RaspberryPi_Pico.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "B.Cu")
		(at 110.6 52.81 180)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 1.27 2.96 0)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 -2.96 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.70"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "754-1519-1-ND"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3V3")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Green.step"
			(offset
				(xyz 0 0 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 111.26 57.99 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 3 0.07 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.1"
			(at 272.3896 48.5648 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "RMCF0805FT100RCT-ND"
			(at 272.3896 48.5648 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 272.3896 48.5648 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 37 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 72 "Net-(U2-GPIO6)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 150.63 48.36 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at -3.43 0.03 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "A106056CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 22 "/~{INT}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 35 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 165.41 78.74 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 2.79 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 242.9002 89.5858 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 242.9002 89.5858 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 242.9002 89.5858 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 165.48 64.14 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 2.7432 -0.1016 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 98.1202 -234.3658 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 98.1202 -234.3658 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 98.1202 -234.3658 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 35 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 109.67 78.78 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -2.93 -0.09 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 109.63 64.28 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at -2.91 0.05 90)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.10"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "732-8080-1-ND"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 35 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 157.71 82.47 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 2.73 -0.11 90)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.1"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "A106056CT-ND"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 13 "/DIR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "B.Cu")
		(at 176.0075 52.77 90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q1"
			(at -3.83 0.0525 180)
			(layer "B.SilkS")
		)
		(property "Value" "SSM3K324RLFCT-ND"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "N-MOSFET transistor, gate/source/drain"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "SSM3K324RLFCT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" ".37"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 0.95 90)
			(size 1.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/WAIT'")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 -0.95 90)
			(size 1.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.5 0 90)
			(size 1.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/~{WAIT}")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
		(layer "B.Cu")
		(at 135.85 71.52 -90)
		(descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0.01 8.73 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SN74LVCC4245ADWR"
			(at 0 -8.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74avc8t245.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "1.83"
			(at 84.709 -229.489 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "296-26634-1-ND"
			(at 84.709 -229.489 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 84.709 -229.489 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x7.8mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "+5V")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/~{SYSRES}")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(U1-A2-Pad4)")
			(pinfunction "A2")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U1-A3-Pad5)")
			(pinfunction "A3")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" smd roundrect
			(at -4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/~{RAS}")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/~{OUT}")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/~{WR}")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/~{RD}")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/~{IN}")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/IN'")
			(pinfunction "B8")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/RD'")
			(pinfunction "B7")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/WR'")
			(pinfunction "B6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/OUT'")
			(pinfunction "B5")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/MREQ'")
			(pinfunction "B4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "unconnected-(U1-B3-Pad19)")
			(pinfunction "B3")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" smd roundrect
			(at 4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U1-B2-Pad20)")
			(pinfunction "B2")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd roundrect
			(at 4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/SYSRES'")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(zone_connect 0)
		)
		(pad "23" smd roundrect
			(at 4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "B.Cu")
		(at 145.09 48.3 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 3.19 0.02 180)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "A106056CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "0.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 18 "/~{WAIT}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
			(net 35 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
		(layer "B.Cu")
		(at 117.72 71.54 -90)
		(descr "SOIC, 24 Pin (JEDEC MS-013AD, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/RW_24.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at -0.16 8.63 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SN74LVCC4245ADWR"
			(at 0 -8.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74avc8t245.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" "1.83"
			(at 103.0224 -247.7516 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "296-26634-1-ND"
			(at 103.0224 -247.7516 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 103.0224 -247.7516 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x7.8mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "+5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "+5V")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/A14")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/A13")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/A10")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/A12")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/A15")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/A11")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "/A8")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/A9")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 4.65 -6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 4.65 -5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/PD1")
			(pinfunction "B8")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/PD0")
			(pinfunction "B7")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/PD3")
			(pinfunction "B6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/PD7")
			(pinfunction "B5")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/PD4")
			(pinfunction "B4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 4.65 0.635 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/PD2")
			(pinfunction "B3")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 4.65 1.905 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/PD5")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 4.65 3.175 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/PD6")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 4.65 4.445 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/ADDRH_OE")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 4.65 5.715 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 4.65 6.985 270)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3V3")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-24W_7.5x15.4mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23_Handsoldering"
		(layer "B.Cu")
		(at 179.8 52.77 90)
		(descr "SOT-23, Handsoldering")
		(tags "SOT-23")
		(property "Reference" "Q2"
			(at -3.87 0.02 180)
			(layer "B.SilkS")
		)
		(property "Value" "SSM3K324RLFCT-ND"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "N-MOSFET transistor, gate/source/drain"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digikey" "SSM3K324RLFCT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Cost" ".37"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "FDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5 0.95 90)
			(size 1.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/INT'")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.5 -0.95 90)
			(size 1.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "passive")
			(zone_connect 0)
		)
		(pad "3" smd roundrect
			(at 1.5 0 90)
			(size 1.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/~{INT}")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 105.8448 46.614)
		(end 182.0234 121.8298)
		(fill no)
		(layer "Edge.Cuts")
	)
	(image
		(at 150.214 87.2)
		(layer "Dwgs.User")
		(scale 0.221072)
		(locked yes)
	)
	(gr_text "40"
		(at 171.15 56.68 0)
		(layer "F.SilkS")
	)
	(gr_text "Floppy-80\n(Model 1k)"
		(at 125.32 115.4 0)
		(layer "F.SilkS")
	)
	(gr_text "39"
		(at 171.15 49.98 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 123.31 49.92 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 123.26 56.74 0)
		(layer "F.SilkS")
	)
	(gr_text "Floppy-80 (Original) GitHub Project:\nhttps://github.com/MichaelM4/Floppy80-M1"
		(at 165.405 114.65 0)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 107.8 55.05 0)
		(layer "B.SilkS")
	)
	(gr_text "V1.0"
		(at 170.125 114.37 0)
		(layer "B.SilkS")
	)
	(gr_text "Board designed for the TRS-80 Model 1k:\nhttps://github.com/kiwisincebirth/TRS-80-MODEL-1-K"
		(at 174.355 118.43 0)
		(layer "B.SilkS")
	)
	(zone
		(net 35)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 10)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 107.877178 62.93889) (xy 114.24 62.974709) (xy 114.24 49.78325) (xy 120.33 49.823405) (xy 120.33 62.979034)
				(xy 181.660183 62.880333) (xy 181.670184 85.81264) (xy 177.848058 85.836679) (xy 177.8281 90.846411)
				(xy 175.37 90.909669) (xy 175.37 83.01) (xy 180.079867 83.01) (xy 180.089867 65.509625) (xy 107.86 65.61)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 10)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 107.877262 77.464327) (xy 168.399863 77.653785) (xy 169.21 78.29) (xy 172.15 78.29) (xy 172.114633 84.368518)
				(xy 170.264881 84.35284) (xy 170.220642 90.767374) (xy 167.72 90.78997) (xy 167.72 82.35) (xy 169.45 82.35)
				(xy 169.45 80.894839) (xy 107.854596 80.988701)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 181.64333 121.110872) (xy 106.384722 121.084549) (xy 106.384802 47.0694) (xy 181.64341 47.0694)
			)
		)
	)
	(embedded_fonts no)
)
