(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_575555ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gt-gerbers-jlc")
		)
	)
	(net 0 "")
	(net 1 "~{RST-OSC}")
	(net 2 "GND")
	(net 3 "+5V")
	(net 4 "Net-(IC702-RGB-)")
	(net 5 "Net-(IC702-OSC)")
	(net 6 "Net-(IC700-OSC)")
	(net 7 "OSC")
	(net 8 "AUDIO-L")
	(net 9 "CESEL")
	(net 10 "A18")
	(net 11 "A14")
	(net 12 "A9")
	(net 13 "A10")
	(net 14 "D6")
	(net 15 "DCK")
	(net 16 "XVSYNC")
	(net 17 "VD8")
	(net 18 "VD7")
	(net 19 "VD5")
	(net 20 "VD4")
	(net 21 "VD3")
	(net 22 "VD2")
	(net 23 "VD1")
	(net 24 "VD0")
	(net 25 "VIDEOR")
	(net 26 "XB")
	(net 27 "HSM")
	(net 28 "~{WR}")
	(net 29 "A8")
	(net 30 "~{RD}")
	(net 31 "D7")
	(net 32 "D4")
	(net 33 "D2")
	(net 34 "XHSYNC")
	(net 35 "A0")
	(net 36 "A2")
	(net 37 "VD6")
	(net 38 "A5")
	(net 39 "A7")
	(net 40 "A12")
	(net 41 "A16")
	(net 42 "A20")
	(net 43 "RDY")
	(net 44 "~{XIRQ2}")
	(net 45 "VIDEOG")
	(net 46 "AUDIO-R")
	(net 47 "~{CEK}")
	(net 48 "A17")
	(net 49 "A13")
	(net 50 "A11")
	(net 51 "D5")
	(net 52 "D3")
	(net 53 "D1")
	(net 54 "D0")
	(net 55 "A1")
	(net 56 "A3")
	(net 57 "A4")
	(net 58 "A6")
	(net 59 "A15")
	(net 60 "A19")
	(net 61 "SYNCV")
	(net 62 "VIDEOB")
	(net 63 "DI0")
	(net 64 "DI1")
	(net 65 "DI2")
	(net 66 "DI3")
	(net 67 "SEL")
	(net 68 "CLR")
	(net 69 "Net-(IC700-O0)")
	(net 70 "Net-(IC700-O1)")
	(net 71 "AGND")
	(net 72 "unconnected-(IC700-N{slash}C-Pad9)")
	(net 73 "unconnected-(IC700-SX-Pad13)")
	(net 74 "unconnected-(IC700-N{slash}C-Pad23)")
	(net 75 "unconnected-(IC700-K4-Pad27)")
	(net 76 "unconnected-(IC700-K5-Pad28)")
	(net 77 "unconnected-(IC700-O2-Pad33)")
	(net 78 "unconnected-(IC700-O3-Pad34)")
	(net 79 "unconnected-(IC700-O4-Pad35)")
	(net 80 "unconnected-(IC700-O5-Pad36)")
	(net 81 "unconnected-(IC700-O6-Pad37)")
	(net 82 "unconnected-(IC700-O7-Pad38)")
	(net 83 "unconnected-(IC700-ERT-Pad39)")
	(net 84 "unconnected-(IC700-ER3-Pad40)")
	(net 85 "unconnected-(IC700-ER2-Pad41)")
	(net 86 "unconnected-(IC700-ER1-Pad42)")
	(net 87 "~{IRQ+PUP}")
	(net 88 "unconnected-(IC700-SYNC-Pad46)")
	(net 89 "~{CE7}")
	(net 90 "~{CER}")
	(net 91 "unconnected-(IC701-D15-Pad4)")
	(net 92 "unconnected-(IC701-D14-Pad5)")
	(net 93 "unconnected-(IC701-D13-Pad6)")
	(net 94 "unconnected-(IC701-D12-Pad7)")
	(net 95 "unconnected-(IC701-D11-Pad8)")
	(net 96 "unconnected-(IC701-D10-Pad9)")
	(net 97 "unconnected-(IC701-D9-Pad10)")
	(net 98 "unconnected-(IC701-D8-Pad12)")
	(net 99 "unconnected-(IC701-DISP-Pad27)")
	(net 100 "Net-(IC701-MWR)")
	(net 101 "Net-(IC701-MRD)")
	(net 102 "/VDC/MD0")
	(net 103 "/VDC/MD1")
	(net 104 "/VDC/MD2")
	(net 105 "/VDC/MD3")
	(net 106 "/VDC/MD4")
	(net 107 "/VDC/MD5")
	(net 108 "/VDC/MD6")
	(net 109 "/VDC/MD7")
	(net 110 "/VDC/MD8")
	(net 111 "/VDC/MD9")
	(net 112 "/VDC/MD10")
	(net 113 "/VDC/MD11")
	(net 114 "/VDC/MD12")
	(net 115 "/VDC/MD13")
	(net 116 "/VDC/MD14")
	(net 117 "/VDC/MD15")
	(net 118 "/VDC/MA0")
	(net 119 "/VDC/MA1")
	(net 120 "/VDC/MA2")
	(net 121 "/VDC/MA3")
	(net 122 "/VDC/MA4")
	(net 123 "/VDC/MA5")
	(net 124 "/VDC/MA6")
	(net 125 "/VDC/MA7")
	(net 126 "/VDC/MA8")
	(net 127 "/VDC/MA9")
	(net 128 "/VDC/MA10")
	(net 129 "/VDC/MA11")
	(net 130 "/VDC/MA12")
	(net 131 "/VDC/MA13")
	(net 132 "/VDC/MA14")
	(net 133 "/VDC/MA15")
	(net 134 "unconnected-(IC702-D8-Pad4)")
	(net 135 "unconnected-(IC702-TEST1-Pad58)")
	(net 136 "unconnected-(IC702-TEST2-Pad59)")
	(net 137 "unconnected-(IC702-TEST3-Pad60)")
	(net 138 "unconnected-(IC703-N{slash}C-Pad1)")
	(net 139 "unconnected-(R708-R1.1-Pad1)")
	(net 140 "unconnected-(R708-R1.2-Pad8)")
	(net 141 "AR12")
	(net 142 "AR7")
	(net 143 "AR6")
	(net 144 "AR5")
	(net 145 "AR4")
	(net 146 "AR3")
	(net 147 "AR2")
	(net 148 "AR1")
	(net 149 "AR0")
	(net 150 "AR10")
	(net 151 "AR11")
	(net 152 "AR9")
	(net 153 "AR8")
	(net 154 "AR14")
	(net 155 "AR13")
	(net 156 "AR18")
	(net 157 "AR17")
	(net 158 "AR16")
	(net 159 "AR15")
	(net 160 "AR19")
	(net 161 "AR20")
	(net 162 "Net-(IC700-RD)")
	(net 163 "Net-(IC700-WR)")
	(net 164 "unconnected-(R707-R1.1-Pad1)")
	(net 165 "unconnected-(R707-R1.2-Pad8)")
	(net 166 "Net-(X700-OUT)")
	(net 167 "Net-(CN0-Pin_21)")
	(net 168 "unconnected-(R200-R4.1-Pad4)")
	(net 169 "unconnected-(R200-R4.2-Pad5)")
	(net 170 "Net-(D204-K)")
	(net 171 "Net-(D205-K)")
	(net 172 "Net-(D206-K)")
	(net 173 "EXT_AUDIO")
	(net 174 "EXT_GREEN")
	(net 175 "unconnected-(R203-R1.1-Pad1)")
	(net 176 "unconnected-(R203-R1.2-Pad8)")
	(net 177 "EXT_RED")
	(net 178 "EXT_BLUE")
	(net 179 "Net-(R203-R3.1)")
	(net 180 "Net-(R203-R2.1)")
	(net 181 "Net-(R203-R4.1)")
	(net 182 "Net-(IC700-K0)")
	(net 183 "Net-(IC700-K1)")
	(net 184 "Net-(IC700-K2)")
	(net 185 "Net-(IC700-K3)")
	(net 186 "Net-(IC700-K6)")
	(net 187 "Net-(C200-Pad2)")
	(net 188 "Net-(Q506-B)")
	(net 189 "EXT_BRIGHT")
	(net 190 "Net-(Q504-Pad1)")
	(net 191 "Net-(VR502-Pin_1)")
	(net 192 "unconnected-(VR502-Pin_4-Pad4)")
	(net 193 "Net-(SW500-A)")
	(net 194 "Net-(D501-A-Pad1)")
	(net 195 "Net-(C507-Pad1)")
	(net 196 "Net-(Q502-B)")
	(net 197 "Net-(R506-Pad1)")
	(net 198 "Net-(D501-K)")
	(net 199 "Net-(D502-common)")
	(net 200 "Net-(Q500-C)")
	(net 201 "Net-(Q500-B)")
	(net 202 "unconnected-(T500-Pad5)")
	(net 203 "Net-(D503-K)")
	(net 204 "Net-(D503-A-Pad1)")
	(net 205 "Net-(ZD500-K)")
	(net 206 "Net-(C501-Pad2)")
	(net 207 "Net-(Q900-B)")
	(net 208 "Net-(Q901-B)")
	(net 209 "unconnected-(T900-Pad8)")
	(net 210 "Net-(L900-Pad1)")
	(net 211 "Net-(C901-Pad2)")
	(net 212 "Net-(CN900-Pin_1)")
	(net 213 "Net-(Q903-E)")
	(net 214 "Net-(C500-Pad2)")
	(net 215 "Net-(Q901-C)")
	(net 216 "BLH")
	(net 217 "Net-(Q900-C)")
	(net 218 "Net-(D901-K)")
	(net 219 "Net-(D901-A-Pad1)")
	(net 220 "SLEEP")
	(net 221 "Net-(D900-common)")
	(net 222 "Net-(D900-A)")
	(net 223 "EAR1")
	(net 224 "Net-(J100-Pin_5)")
	(net 225 "Net-(IC100B--)")
	(net 226 "Net-(IC100A--)")
	(net 227 "Net-(IC100A-+)")
	(net 228 "Net-(J100-Pin_1)")
	(net 229 "Net-(J100-Pin_2)")
	(net 230 "Net-(J100-Pin_3)")
	(net 231 "Net-(J100-Pin_11)")
	(net 232 "Net-(R101-R3.2)")
	(net 233 "Net-(R101-R2.1)")
	(net 234 "Net-(R101-R1.1)")
	(net 235 "Net-(C102-Pad2)")
	(net 236 "Net-(C103-Pad2)")
	(net 237 "HUCARD_AUDIO")
	(net 238 "VOL_IN_R")
	(net 239 "VOL_IN_L")
	(net 240 "Net-(D500-K)")
	(net 241 "Net-(J500-Pad1)")
	(net 242 "Net-(J500-Pad2)")
	(net 243 "Net-(J500-Pad3)")
	(net 244 "Net-(CC101-Pad1)")
	(net 245 "Net-(CC103-Pad1)")
	(net 246 "Net-(CC103-Pad2)")
	(net 247 "Net-(CC102-Pad1)")
	(net 248 "Net-(IC100B-+)")
	(net 249 "Net-(CC104-Pad2)")
	(net 250 "Net-(L101-Pad2)")
	(net 251 "Net-(L100-Pad1)")
	(net 252 "Net-(L102-Pad1)")
	(net 253 "Net-(L102-Pad2)")
	(net 254 "Net-(R502-Pad2)")
	(net 255 "HPOS")
	(net 256 "unconnected-(IC702-BRT--Pad17)")
	(net 257 "unconnected-(IC702-BRTC-Pad18)")
	(net 258 "unconnected-(IC702-BURS-Pad20)")
	(net 259 "unconnected-(IC702-B-Y--Pad23)")
	(net 260 "unconnected-(IC702-B-YC-Pad24)")
	(net 261 "unconnected-(IC702-B-Y-Pad26)")
	(net 262 "unconnected-(IC702-R-Y--Pad30)")
	(net 263 "unconnected-(IC702-R-YC-Pad31)")
	(net 264 "unconnected-(IC702-R-Y-Pad33)")
	(net 265 "unconnected-(IC702-Y--Pad37)")
	(net 266 "unconnected-(IC702-YC-Pad38)")
	(net 267 "unconnected-(IC702-Y-Pad40)")
	(net 268 "Net-(ZD501-K)")
	(net 269 "Net-(Q700-B)")
	(net 270 "N{slash}C")
	(net 271 "Net-(D500-A)")
	(net 272 "PWR3")
	(net 273 "LCD_BRIGHT")
	(net 274 "LCD_SYNC")
	(net 275 "LCD_BLUE")
	(net 276 "LCD_RED")
	(net 277 "LCD_GREEN")
	(net 278 "RGB_EN")
	(net 279 "Net-(Q503-Pad4)")
	(net 280 "Net-(Q504-Pad2)")
	(net 281 "BATT+")
	(net 282 "BATT-")
	(net 283 "Net-(CC104-Pad1)")
	(net 284 "+5VP")
	(net 285 "VCC")
	(net 286 "+5VL")
	(net 287 "PWR2")
	(net 288 "PWR4")
	(net 289 "PWR")
	(net 290 "unconnected-(T500-Pad6)")
	(net 291 "Net-(C501-Pad1)")
	(footprint "A-PCENGINE:Strengthening_Via"
		(layer "F.Cu")
		(at 195.25 68.95)
		(property "Reference" "SV4"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 282 "BATT-")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2.8mm"
		(layer "F.Cu")
		(at 182.05 128.5)
		(property "Reference" "G3"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 177.125 93.425)
		(property "Reference" "TP40"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 186 "Net-(IC700-K6)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "F.Cu")
		(at 118.1608 141.1963 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D208"
			(at -4.3537 0.0642 180)
			(layer "F.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 189 "EXT_BRIGHT")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 189 "EXT_BRIGHT")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "LCD_SYNC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Strengthening_Via"
		(layer "F.Cu")
		(at 190.7 70.425)
		(property "Reference" "SV3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 282 "BATT-")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 175.5902 122.8598)
		(property "Reference" "TP13"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "AR10")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 185.2422 120.3706)
		(property "Reference" "TP6"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "AR3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Strengthening_Via"
		(layer "F.Cu")
		(at 190.7 73.2)
		(property "Reference" "SV2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 281 "BATT+")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 185.7502 115.1636)
		(property "Reference" "TP5"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "AR2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 186.963 117.7798 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R708"
			(at -0.8452 5.187 180)
			(layer "F.SilkS")
		)
		(property "Value" "4x18"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "unconnected-(R708-R1.1-Pad1)")
			(pinfunction "R1.1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "A2")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "A1")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "A0")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "AR0")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "AR1")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "AR2")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "unconnected-(R708-R1.2-Pad8)")
			(pinfunction "R1.2")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:PicoFuse"
		(layer "F.Cu")
		(at 190.85 58.95 180)
		(property "Reference" "F500"
			(at 13.75 4.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1A 125V"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 271 "Net-(D500-A)")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "2" thru_hole circle
			(at 12.75 0 180)
			(size 1.6 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 193 "Net-(SW500-A)")
			(pintype "passive")
			(clearance 0.3)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2.8mm"
		(layer "F.Cu")
		(at 182.25 62.5)
		(property "Reference" "G8"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "F.Cu")
		(at 136.4742 133.0198 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D206"
			(at 2.0742 -3.3302 180)
			(layer "F.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 2.4 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 180)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 181 "Net-(R203-R4.1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 180)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "VIDEOB")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 180)
			(size 1.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 172 "Net-(D206-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 183.6928 118.7958)
		(property "Reference" "TP8"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "AR5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 113.4302 140.1682 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R204"
			(at -3.3318 -0.1052 180)
			(layer "F.SilkS")
		)
		(property "Value" "4x100K"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 189 "EXT_BRIGHT")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 181 "Net-(R203-R4.1)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 179 "Net-(R203-R3.1)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 180 "Net-(R203-R2.1)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 163.9316 120.3706)
		(property "Reference" "TP23"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "AR20")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 175.1 93.425)
		(property "Reference" "TP41"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "Net-(IC700-O0)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 170.5102 124.4346)
		(property "Reference" "TP18"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "AR15")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "F.Cu")
		(at 179.45 90.3875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R723"
			(at -4.4125 2.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "N/P"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 186 "Net-(IC700-K6)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_10x2.5mm"
		(layer "F.Cu")
		(at 119.275 48.6)
		(property "Reference" "CC500"
			(at 6.75 2.325 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 16V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -7.3 0.775 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 0)
			(size 4 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 214 "Net-(C500-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1 0)
			(size 4 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Inductor_8mm"
		(layer "F.Cu")
		(at 120.725 57.525 180)
		(property "Reference" "L900"
			(at -3.425 -7.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uH"
			(at 0 7.25 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 8.75 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0 180)
			(size 3 8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 210 "Net-(L900-Pad1)")
			(pinfunction "1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 2.5 0 180)
			(size 3 8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 216 "BLH")
			(pinfunction "2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 167.2908 125.9696 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R712"
			(at -3.5054 -2.4908 180)
			(layer "F.SilkS")
		)
		(property "Value" "4x100"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "A18")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "A17")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "A16")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "A15")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "AR15")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "AR16")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "AR17")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "AR18")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Oscillator-3_Pin"
		(layer "F.Cu")
		(at 168.5036 90.3478)
		(property "Reference" "X700"
			(at -5.9036 -4.0978 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "21.4772 MHz"
			(at 0 3.81 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Oscillator*DIP*14*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 5.31 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 1.4 1.4)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
			(clearance 0.4)
		)
		(pad "2" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(clearance 0.2)
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.4 1.4)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 166 "Net-(X700-OUT)")
			(pinfunction "OUT")
			(pintype "output")
			(clearance 0.4)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:D_1206"
		(layer "F.Cu")
		(at 140.575 61.9 180)
		(descr "Diode SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "ZD501"
			(at -6.775 -1.275 180)
			(layer "F.SilkS")
		)
		(property "Value" "?"
			(at 0 1.82 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 268 "Net-(ZD501-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.6 0 180)
			(size 1.25 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_6.2x1.6mm"
		(layer "F.Cu")
		(at 177.125 71.1 -90)
		(property "Reference" "CC102"
			(at -0.575 3.425 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33uF 10V"
			(at 0 5.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.75 0.875 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.8 0 270)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 247 "Net-(CC102-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.8 0 270)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2mm"
		(layer "F.Cu")
		(at 126.25 95.55)
		(property "Reference" "G10"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2mm"
		(layer "F.Cu")
		(at 182 90.45)
		(property "Reference" "G11"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 108.525 137.1 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C204"
			(at 2.8 -0.325 0)
			(layer "F.SilkS")
		)
		(property "Value" "33pF"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 189 "EXT_BRIGHT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 122.275 114.2)
		(property "Reference" "CC503"
			(at 6.025 -2.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF 35V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -6.3 -0.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 272 "PWR3")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 174.5488 124.4346)
		(property "Reference" "TP14"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "AR11")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 132.975 126.025 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C709"
			(at -2.35 4 180)
			(layer "F.SilkS")
		)
		(property "Value" "33pF"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 141.025 56.825)
		(property "Reference" "CC502"
			(at 6.25 -2.65 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF 50V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.55 -2.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 198 "Net-(D501-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 182.725 97.5)
		(property "Reference" "TP37"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 183 "Net-(IC700-K1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_T500"
		(layer "F.Cu")
		(at 131.45 56.3)
		(property "Reference" "T500"
			(at -0.225 6.275 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "?"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at 0 -4.2)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 0 4.2)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -3.5 -2.35)
			(size 2.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 214 "Net-(C500-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -3.5 0)
			(size 2.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 200 "Net-(Q500-C)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -3.5 2.35)
			(size 2.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 194 "Net-(D501-A-Pad1)")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 3.5 2.35)
			(size 2.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 291 "Net-(C501-Pad1)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 3.5 0.8)
			(size 2.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 202 "unconnected-(T500-Pad5)")
			(pintype "passive+no_connect")
		)
		(pad "6" smd roundrect
			(at 3.5 -0.8)
			(size 2.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 290 "unconnected-(T500-Pad6)")
			(pintype "passive+no_connect")
		)
		(pad "7" smd roundrect
			(at 3.5 -2.35)
			(size 2.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 179.125 93.45)
		(property "Reference" "TP39"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 185 "Net-(IC700-K3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 173.5328 122.9106)
		(property "Reference" "TP15"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "AR12")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 170.5102 136.525)
		(property "Reference" "TP28"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "D6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 176.625 87.35)
		(property "Reference" "TP82"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 283 "Net-(CC104-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:CP_6.2x1.6mm"
		(layer "F.Cu")
		(at 174.075 78.125 90)
		(property "Reference" "CC101"
			(at -0.325 -3.175 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33uF 10V"
			(at 0 5.7 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.075 0.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.8 0 90)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 244 "Net-(CC101-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.8 0 90)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:CP_6.2x1.6mm"
		(layer "F.Cu")
		(at 120.775 86)
		(property "Reference" "CC901"
			(at 2.375 3.625 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "22uF 6.3V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.225 0.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 222 "Net-(D900-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin1"
		(layer "F.Cu")
		(at 122.1994 141.1963 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q507"
			(at 1.1713 4.9756 180)
			(layer "F.SilkS")
		)
		(property "Value" "12 51"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 220 "SLEEP")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "PWR2")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "PWR4")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 158.3182 101.9988 -90)
		(property "Reference" "CC703"
			(at 7.6012 1.8182 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 6.3V"
			(at 0 5.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -6.8738 0.7182 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0 270)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 71 "AGND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0 270)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:HUC62xx"
		(layer "F.Cu")
		(at 179.6072 108.775 90)
		(descr "EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "EQFP QFP")
		(property "Reference" "IC700"
			(at -0.3688 -17.8092 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HUC6280A"
			(at 0.55 9.22 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "41"
			(at 10.604 -17.7838 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "64"
			(at -10.732 -16.8948 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "40"
			(at 12.3312 -15.1676 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.85 11.15 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -8.54 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "AR5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -7.74 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "AR4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -6.94 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "AR3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -6.14 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "AR2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -5.34 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "AR1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -4.54 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "AR0")
			(pinfunction "A0")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -3.74 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS1")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.94 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "+5VL")
			(pinfunction "VAA")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -2.14 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "unconnected-(IC700-N{slash}C-Pad9)")
			(pinfunction "N/C")
			(pintype "no_connect")
		)
		(pad "10" smd roundrect
			(at -1.34 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(IC700-OSC)")
			(pinfunction "OSC")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -0.54 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "~{RST-OSC}")
			(pinfunction "RST")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 0.26 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "RDY")
			(pinfunction "RDY")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 1.06 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "unconnected-(IC700-SX-Pad13)")
			(pinfunction "SX")
			(pintype "input+no_connect")
		)
		(pad "14" smd roundrect
			(at 1.86 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "HSM")
			(pinfunction "HSM")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 2.66 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "+5VL")
			(pinfunction "VPPD")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 3.46 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS5")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at 4.26 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "AUDIO-L")
			(pinfunction "LOUT")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 5.06 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "AUDIO-R")
			(pinfunction "ROUT")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at 5.86 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "+5VL")
			(pinfunction "VPPA")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 6.66 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "AGND")
			(pinfunction "AGND")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 7.46 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSSA")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 8.26 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 182 "Net-(IC700-K0)")
			(pinfunction "K0")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 9.06 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "unconnected-(IC700-N{slash}C-Pad23)")
			(pinfunction "N/C")
			(pintype "no_connect")
		)
		(pad "24" smd roundrect
			(at 9.86 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 183 "Net-(IC700-K1)")
			(pinfunction "K1")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 12.89 -0.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 184 "Net-(IC700-K2)")
			(pinfunction "K2")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 12.89 -0.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 185 "Net-(IC700-K3)")
			(pinfunction "K3")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 12.89 -1.63 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "unconnected-(IC700-K4-Pad27)")
			(pinfunction "K4")
			(pintype "input+no_connect")
		)
		(pad "28" smd roundrect
			(at 12.89 -2.43 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "unconnected-(IC700-K5-Pad28)")
			(pinfunction "K5")
			(pintype "input+no_connect")
		)
		(pad "29" smd roundrect
			(at 12.89 -3.23 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 186 "Net-(IC700-K6)")
			(pinfunction "K6")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at 12.89 -4.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "XB")
			(pinfunction "K7")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at 12.89 -4.83 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(IC700-O0)")
			(pinfunction "O0")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at 12.89 -5.63 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(IC700-O1)")
			(pinfunction "O1")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at 12.89 -6.43 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "unconnected-(IC700-O2-Pad33)")
			(pinfunction "O2")
			(pintype "input+no_connect")
		)
		(pad "34" smd roundrect
			(at 12.89 -7.23 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "unconnected-(IC700-O3-Pad34)")
			(pinfunction "O3")
			(pintype "input+no_connect")
		)
		(pad "35" smd roundrect
			(at 12.89 -8.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "unconnected-(IC700-O4-Pad35)")
			(pinfunction "O4")
			(pintype "input+no_connect")
		)
		(pad "36" smd roundrect
			(at 12.89 -8.83 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "unconnected-(IC700-O5-Pad36)")
			(pinfunction "O5")
			(pintype "input+no_connect")
		)
		(pad "37" smd roundrect
			(at 12.89 -9.63 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "unconnected-(IC700-O6-Pad37)")
			(pinfunction "O6")
			(pintype "input+no_connect")
		)
		(pad "38" smd roundrect
			(at 12.89 -10.43 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "unconnected-(IC700-O7-Pad38)")
			(pinfunction "O7")
			(pintype "input+no_connect")
		)
		(pad "39" smd roundrect
			(at 12.89 -11.23 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "unconnected-(IC700-ERT-Pad39)")
			(pinfunction "ERT")
			(pintype "input+no_connect")
		)
		(pad "40" smd roundrect
			(at 12.89 -12.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "unconnected-(IC700-ER3-Pad40)")
			(pinfunction "ER3")
			(pintype "input+no_connect")
		)
		(pad "41" smd roundrect
			(at 9.86 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "unconnected-(IC700-ER2-Pad41)")
			(pinfunction "ER2")
			(pintype "input+no_connect")
		)
		(pad "42" smd roundrect
			(at 9.06 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "unconnected-(IC700-ER1-Pad42)")
			(pinfunction "ER1")
			(pintype "input+no_connect")
		)
		(pad "43" smd roundrect
			(at 8.26 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "~{XIRQ2}")
			(pinfunction "IRQ2")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at 7.46 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "~{IRQ+PUP}")
			(pinfunction "IRQ1")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at 6.66 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "+5VL")
			(pinfunction "NMI")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at 5.86 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "unconnected-(IC700-SYNC-Pad46)")
			(pinfunction "SYNC")
			(pintype "input+no_connect")
		)
		(pad "47" smd roundrect
			(at 5.06 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "+5VL")
			(pinfunction "VDD")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at 4.26 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS4")
			(pintype "input")
		)
		(pad "49" smd roundrect
			(at 3.46 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "50" smd roundrect
			(at 2.66 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "51" smd roundrect
			(at 1.86 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at 1.06 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at 0.26 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at -0.54 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at -1.34 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at -2.14 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at -2.94 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "+5VL")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "58" smd roundrect
			(at -3.74 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS3")
			(pintype "input")
		)
		(pad "59" smd roundrect
			(at -4.54 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "~{CEK}")
			(pinfunction "CEK")
			(pintype "input")
		)
		(pad "60" smd roundrect
			(at -5.34 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "~{CE7}")
			(pinfunction "CE7")
			(pintype "input")
		)
		(pad "61" smd roundrect
			(at -6.14 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "~{CER}")
			(pinfunction "CER")
			(pintype "input")
		)
		(pad "62" smd roundrect
			(at -6.94 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "Net-(IC700-RD)")
			(pinfunction "RD")
			(pintype "output")
		)
		(pad "63" smd roundrect
			(at -7.74 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 163 "Net-(IC700-WR)")
			(pinfunction "WR")
			(pintype "output")
		)
		(pad "64" smd roundrect
			(at -8.54 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 161 "AR20")
			(pinfunction "A20")
			(pintype "output")
		)
		(pad "65" smd roundrect
			(at -11.54 -12.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "AR19")
			(pinfunction "A19")
			(pintype "output")
		)
		(pad "66" smd roundrect
			(at -11.54 -11.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "AR18")
			(pinfunction "A18")
			(pintype "output")
		)
		(pad "67" smd roundrect
			(at -11.54 -10.43 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "AR17")
			(pinfunction "A17")
			(pintype "output")
		)
		(pad "68" smd roundrect
			(at -11.54 -9.63 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "AR16")
			(pinfunction "A16")
			(pintype "output")
		)
		(pad "69" smd roundrect
			(at -11.54 -8.83 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "AR15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "70" smd roundrect
			(at -11.54 -8.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "AR14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "71" smd roundrect
			(at -11.54 -7.23 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "AR13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "72" smd roundrect
			(at -11.54 -6.43 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "AR12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "73" smd roundrect
			(at -11.54 -5.63 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "AR11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "74" smd roundrect
			(at -11.54 -4.83 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "AR10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "75" smd roundrect
			(at -11.54 -4.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS2")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at -11.54 -3.23 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "+5VL")
			(pinfunction "VBB")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at -11.54 -2.43 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "AR9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "78" smd roundrect
			(at -11.54 -1.63 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "AR8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "79" smd roundrect
			(at -11.54 -0.83 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "AR7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "80" smd roundrect
			(at -11.54 -0.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "AR6")
			(pinfunction "A6")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "F.Cu")
		(at 177.4 90.3875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R719"
			(at -6.0125 4.775 0)
			(layer "F.SilkS")
		)
		(property "Value" "820"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 67 "SEL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 69 "Net-(IC700-O0)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 167.4622 123.4186)
		(property "Reference" "TP20"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "AR17")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 172.5168 124.4346)
		(property "Reference" "TP16"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 155 "AR13")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 108.525 129.775 -90)
		(property "Reference" "CC504"
			(at 6.1 2.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 6.3V"
			(at 0 5.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.325 -3.425 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0 270)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0 270)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 124.825 118.825)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R502"
			(at 5.275 -3.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.7K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 272 "PWR3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 254 "Net-(R502-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 173.3 93.425)
		(property "Reference" "TP42"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "Net-(IC700-O1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "F.Cu")
		(at 175.35 90.3875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R720"
			(at -4.1625 3.125 0)
			(layer "F.SilkS")
		)
		(property "Value" "820"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 68 "CLR")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 70 "Net-(IC700-O1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_10x2.5mm"
		(layer "F.Cu")
		(at 185.85 69.175 -90)
		(property "Reference" "CC100"
			(at -4 6.325 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 16V"
			(at 0 5.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -7.475 0.9 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 284 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 171.5516 122.9106)
		(property "Reference" "TP17"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "AR14")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 139.8586 138.1362 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R201"
			(at -3.2388 -0.9836 180)
			(layer "F.SilkS")
		)
		(property "Value" "4x5.6K"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 277 "LCD_GREEN")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 276 "LCD_RED")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 275 "LCD_BLUE")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "LCD_SYNC")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 176.6062 124.4346)
		(property "Reference" "TP12"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "AR9")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:VR_5P"
		(layer "F.Cu")
		(at 191.325 103.725)
		(property "Reference" "VR100"
			(at -0.1 -10.475 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Volume"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(fp_text user "2"
			(at -5.825 0.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -5.825 -3.4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at -5.825 4.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -5.825 2.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -5.825 -1.4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -4.5 -4)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 238 "VOL_IN_R")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -4.5 -2)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 239 "VOL_IN_L")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -4.5 0)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 224 "Net-(J100-Pin_5)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -4.5 2)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 227 "Net-(IC100A-+)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -4.5 4)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 6.9 -5.5)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 6.9 5.4)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 146.4 137.075 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R200"
			(at -7.2662 -5.9568 180)
			(layer "F.SilkS")
		)
		(property "Value" "4x5.6K"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "unconnected-(R200-R4.1-Pad4)")
			(pinfunction "R4.1")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "unconnected-(R200-R4.2-Pad5)")
			(pinfunction "R4.2")
			(pintype "passive+no_connect")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "Net-(D205-K)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "Net-(D204-K)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "Net-(D206-K)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 171.1125 56.8)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R506"
			(at 4.0875 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 197 "Net-(R506-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 172.3644 126.9492 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R711"
			(at -5.8008 -2.8394 180)
			(layer "F.SilkS")
		)
		(property "Value" "4x100"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "A14")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "A13")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "A12")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "A11")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "AR11")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "AR12")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 155 "AR13")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "AR14")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:HUC62xx"
		(layer "F.Cu")
		(at 135.5768 76.9952 -90)
		(descr "EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "EQFP QFP")
		(property "Reference" "IC701"
			(at 1.2368 5.7574 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HUC6270"
			(at 0.55 9.22 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "41"
			(at 10.965 -17.1534 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at 16.4548 1.2518 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at 10.8048 7.9268 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "64"
			(at -7.7548 -17.0518 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -7.5262 5.8844 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at -11.7426 3.319 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "65"
			(at -11.2092 -12.3274 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "40"
			(at 16.553 -11.032 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.85 11.15 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -8.54 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "~{CE7}")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -7.74 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "~{WR}")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -6.94 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "~{RD}")
			(pinfunction "RD")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -6.14 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "unconnected-(IC701-D15-Pad4)")
			(pinfunction "D15")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -5.34 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "unconnected-(IC701-D14-Pad5)")
			(pinfunction "D14")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" smd roundrect
			(at -4.54 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "unconnected-(IC701-D13-Pad6)")
			(pinfunction "D13")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" smd roundrect
			(at -3.74 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "unconnected-(IC701-D12-Pad7)")
			(pinfunction "D12")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" smd roundrect
			(at -2.94 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "unconnected-(IC701-D11-Pad8)")
			(pinfunction "D11")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd roundrect
			(at -2.14 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "unconnected-(IC701-D10-Pad9)")
			(pinfunction "D10")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" smd roundrect
			(at -1.34 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "unconnected-(IC701-D9-Pad10)")
			(pinfunction "D9")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd roundrect
			(at -0.54 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS1")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 0.26 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "unconnected-(IC701-D8-Pad12)")
			(pinfunction "D8")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" smd roundrect
			(at 1.06 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 1.86 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 2.66 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 3.46 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 4.26 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 5.06 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VDD1")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at 5.86 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 6.66 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 7.46 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 8.26 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "8/16")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 9.06 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "DCK")
			(pinfunction "CK")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 9.86 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "~{RST-OSC}")
			(pinfunction "RST")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 12.89 -0.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "XVSYNC")
			(pinfunction "VSYN")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 12.89 -0.83 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "XHSYNC")
			(pinfunction "HSYN")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 12.89 -1.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "unconnected-(IC701-DISP-Pad27)")
			(pinfunction "DISP")
			(pintype "output+no_connect")
		)
		(pad "28" smd roundrect
			(at 12.89 -2.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "VD8")
			(pinfunction "SPGB")
			(pintype "output")
		)
		(pad "29" smd roundrect
			(at 12.89 -3.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "VD7")
			(pinfunction "VD7")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 12.89 -4.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "VD6")
			(pinfunction "VD6")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 12.89 -4.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "VD5")
			(pinfunction "VD5")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 12.89 -5.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VDD2")
			(pintype "power_in")
		)
		(pad "33" smd roundrect
			(at 12.89 -6.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS2")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at 12.89 -7.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "VD4")
			(pinfunction "VD4")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 12.89 -8.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "VD3")
			(pinfunction "VD3")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at 12.89 -8.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "VD2")
			(pinfunction "VD2")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at 12.89 -9.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "VD1")
			(pinfunction "VD1")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 12.89 -10.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "VD0")
			(pinfunction "VD0")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 12.89 -11.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(IC701-MWR)")
			(pinfunction "MWR")
			(pintype "output")
		)
		(pad "40" smd roundrect
			(at 12.89 -12.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Net-(IC701-MRD)")
			(pinfunction "MRD")
			(pintype "output")
		)
		(pad "41" smd roundrect
			(at 9.86 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/VDC/MD0")
			(pinfunction "MD0")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 9.06 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/VDC/MD1")
			(pinfunction "MD1")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at 8.26 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/VDC/MD2")
			(pinfunction "MD2")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 7.46 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/VDC/MD3")
			(pinfunction "MD3")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at 6.66 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/VDC/MD4")
			(pinfunction "MD4")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at 5.86 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/VDC/MD5")
			(pinfunction "MD5")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 5.06 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VDD3")
			(pintype "power_in")
		)
		(pad "48" smd roundrect
			(at 4.26 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/VDC/MD6")
			(pinfunction "MD6")
			(pintype "bidirectional")
		)
		(pad "49" smd roundrect
			(at 3.46 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/VDC/MD7")
			(pinfunction "MD7")
			(pintype "bidirectional")
		)
		(pad "50" smd roundrect
			(at 2.66 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/VDC/MD8")
			(pinfunction "MD8")
			(pintype "bidirectional")
		)
		(pad "51" smd roundrect
			(at 1.86 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/VDC/MD9")
			(pinfunction "MD9")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at 1.06 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/VDC/MD10")
			(pinfunction "MD10")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at 0.26 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "/VDC/MD11")
			(pinfunction "MD11")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at -0.54 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/VDC/MD12")
			(pinfunction "MD12")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at -1.34 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS3")
			(pintype "input")
		)
		(pad "56" smd roundrect
			(at -2.14 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/VDC/MD13")
			(pinfunction "MD13")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at -2.94 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/VDC/MD14")
			(pinfunction "MD14")
			(pintype "bidirectional")
		)
		(pad "58" smd roundrect
			(at -3.74 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/VDC/MD15")
			(pinfunction "MD15")
			(pintype "bidirectional")
		)
		(pad "59" smd roundrect
			(at -4.54 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/VDC/MA0")
			(pinfunction "MA0")
			(pintype "output")
		)
		(pad "60" smd roundrect
			(at -5.34 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "/VDC/MA1")
			(pinfunction "MA1")
			(pintype "output")
		)
		(pad "61" smd roundrect
			(at -6.14 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "/VDC/MA2")
			(pinfunction "MA2")
			(pintype "output")
		)
		(pad "62" smd roundrect
			(at -6.94 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "/VDC/MA3")
			(pinfunction "MA3")
			(pintype "output")
		)
		(pad "63" smd roundrect
			(at -7.74 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "/VDC/MA4")
			(pinfunction "MA4")
			(pintype "output")
		)
		(pad "64" smd roundrect
			(at -8.54 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "/VDC/MA5")
			(pinfunction "MA5")
			(pintype "output")
		)
		(pad "65" smd roundrect
			(at -11.54 -12.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "/VDC/MA6")
			(pinfunction "MA6")
			(pintype "output")
		)
		(pad "66" smd roundrect
			(at -11.54 -11.23 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "/VDC/MA7")
			(pinfunction "MA7")
			(pintype "output")
		)
		(pad "67" smd roundrect
			(at -11.54 -10.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "/VDC/MA8")
			(pinfunction "MA8")
			(pintype "output")
		)
		(pad "68" smd roundrect
			(at -11.54 -9.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "/VDC/MA9")
			(pinfunction "MA9")
			(pintype "output")
		)
		(pad "69" smd roundrect
			(at -11.54 -8.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "/VDC/MA10")
			(pinfunction "MA10")
			(pintype "output")
		)
		(pad "70" smd roundrect
			(at -11.54 -8.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "/VDC/MA11")
			(pinfunction "MA11")
			(pintype "output")
		)
		(pad "71" smd roundrect
			(at -11.54 -7.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS4")
			(pintype "input")
		)
		(pad "72" smd roundrect
			(at -11.54 -6.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VDD4")
			(pintype "power_in")
		)
		(pad "73" smd roundrect
			(at -11.54 -5.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/VDC/MA12")
			(pinfunction "MA12")
			(pintype "output")
		)
		(pad "74" smd roundrect
			(at -11.54 -4.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "/VDC/MA13")
			(pinfunction "MA13")
			(pintype "output")
		)
		(pad "75" smd roundrect
			(at -11.54 -4.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/VDC/MA14")
			(pinfunction "MA14")
			(pintype "output")
		)
		(pad "76" smd roundrect
			(at -11.54 -3.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/VDC/MA15")
			(pinfunction "MA15")
			(pintype "output")
		)
		(pad "77" smd roundrect
			(at -11.54 -2.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "~{IRQ+PUP}")
			(pinfunction "IRQ")
			(pintype "input")
		)
		(pad "78" smd roundrect
			(at -11.54 -1.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "RDY")
			(pinfunction "BUSY")
			(pintype "input")
		)
		(pad "79" smd roundrect
			(at -11.54 -0.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "80" smd roundrect
			(at -11.54 -0.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 152.2222 126.492)
		(property "Reference" "TP2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "VIDEOG")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:CP_6.2x1.6mm"
		(layer "F.Cu")
		(at 148.2344 130.0734 -90)
		(property "Reference" "CC704"
			(at -3.1234 -5.7406 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF 16V"
			(at 0 5.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.4234 0.7094 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.8 0 270)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 4 "Net-(IC702-RGB-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.8 0 270)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "F.Cu")
		(at 123.775 144.75)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C511"
			(at 5.475 0.725 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2173913043)
			(net 287 "PWR2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2173913043)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 180.5 85.25)
		(property "Reference" "CC104"
			(at 4.05 4.7 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 6.3V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.925 -1.175 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 283 "Net-(CC104-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 249 "Net-(CC104-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 125.875 44.55)
		(property "Reference" "TP51"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 199 "Net-(D502-common)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2mm"
		(layer "F.Cu")
		(at 182.075 92.9)
		(property "Reference" "G12"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin2+3"
		(layer "F.Cu")
		(at 128.925 46.1125 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D502"
			(at -3.5625 2.55 180)
			(layer "F.SilkS")
		)
		(property "Value" "?"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 272 "PWR3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 199 "Net-(D502-common)")
			(pinfunction "common")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2mm"
		(layer "F.Cu")
		(at 128.825 95.525)
		(property "Reference" "G9"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:C_P7.50mm"
		(layer "F.Cu")
		(at 109.45 97.275 90)
		(descr "C, Rect series, Radial, pin pitch=7.50mm, , length*width=9*2.5mm^2, Capacitor, https://en.tdk.eu/inf/20/20/db/fc_2009/MKT_B32560_564.pdf")
		(tags "C Rect series Radial pin pitch 7.50mm  length 9mm width 2.5mm Capacitor")
		(property "Reference" "C901"
			(at 4.075 2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "33pF"
			(at 3.75 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 212 "Net-(CN900-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 211 "Net-(C901-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L9.0mm_W2.5mm_P7.50mm_MKT.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 159.875 91.425)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C723"
			(at -4.625 -0.575 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.5uF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_10x2.5mm"
		(layer "F.Cu")
		(at 112.125 57.2425 -90)
		(property "Reference" "CC900"
			(at -6.1175 1.675 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 16V"
			(at 0 5.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -6.5175 -1.2 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 216 "BLH")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1 0 270)
			(size 4 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2.8mm"
		(layer "F.Cu")
		(at 126.275 128.45)
		(property "Reference" "G1"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2.8mm"
		(layer "F.Cu")
		(at 128.9 65.1)
		(property "Reference" "G7"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 110.575 123.925 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C510"
			(at 4.25 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 121.25 118.825 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C506"
			(at 3.95 2.075 270)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 272 "PWR3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 188.7982 113.665)
		(property "Reference" "TP3"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "AR0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:VR_4P"
		(layer "F.Cu")
		(at 191.325 126.8)
		(property "Reference" "VR502"
			(at 1 9.375 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Brightness"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(fp_text user "1"
			(at -5.75 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -5.75 1.675 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at -5.75 3.675 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -4.5 -1)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 191 "Net-(VR502-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -4.5 1)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 288 "PWR4")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -4.5 3)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 288 "PWR4")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -4.5 -3)
			(size 2 1.6)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 192 "unconnected-(VR502-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole circle
			(at 6.9 -3.7)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 6.9 4.5)
			(size 2 2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 163.4236 122.936 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R714"
			(at -1.814 -2.3986 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 42 "A20")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 161 "AR20")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:HUC62xx"
		(layer "F.Cu")
		(at 135.5006 109.975 -90)
		(descr "EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "EQFP QFP")
		(property "Reference" "IC702"
			(at -3.2696 5.6304 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HUC6260"
			(at 0.55 9.22 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "80"
			(at -12.3628 3.5984 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at 10.275 6.9506 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at 13.6214 2.557 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "65"
			(at -13.4042 -11.1336 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -9.2894 5.7828 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "41"
			(at 10.294 -17.509 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "40"
			(at 13.1134 -12.9116 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "64"
			(at -9.2894 -15.7056 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0.85 11.15 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -8.54 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -7.74 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(IC702-OSC)")
			(pinfunction "OSC")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -6.94 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -6.14 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "unconnected-(IC702-D8-Pad4)")
			(pinfunction "D8")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -5.34 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -4.54 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.74 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -2.94 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -2.14 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -1.34 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -0.54 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 0.26 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 1.06 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at 1.86 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 2.66 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 3.46 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "17" smd roundrect
			(at 4.26 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 256 "unconnected-(IC702-BRT--Pad17)")
			(pinfunction "BRT-")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 5.06 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 257 "unconnected-(IC702-BRTC-Pad18)")
			(pinfunction "BRTC")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at 5.86 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at 6.66 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 258 "unconnected-(IC702-BURS-Pad20)")
			(pinfunction "BURS")
			(pintype "output+no_connect")
		)
		(pad "21" smd roundrect
			(at 7.46 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AVCC")
			(pintype "power_in")
		)
		(pad "22" smd roundrect
			(at 8.26 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "BRT+")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 9.06 3.19 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "unconnected-(IC702-B-Y--Pad23)")
			(pinfunction "B-Y-")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 9.86 3.19 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 260 "unconnected-(IC702-B-YC-Pad24)")
			(pinfunction "B-YC")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 12.89 -0.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "26" smd roundrect
			(at 12.89 -0.83 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "unconnected-(IC702-B-Y-Pad26)")
			(pinfunction "B-Y")
			(pintype "output+no_connect")
		)
		(pad "27" smd roundrect
			(at 12.89 -1.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AVCC")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at 12.89 -2.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "B-Y-+")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at 12.89 -3.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "30" smd roundrect
			(at 12.89 -4.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "unconnected-(IC702-R-Y--Pad30)")
			(pinfunction "R-Y-")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at 12.89 -4.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "unconnected-(IC702-R-YC-Pad31)")
			(pinfunction "R-YC")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at 12.89 -5.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "33" smd roundrect
			(at 12.89 -6.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "unconnected-(IC702-R-Y-Pad33)")
			(pinfunction "R-Y")
			(pintype "output+no_connect")
		)
		(pad "34" smd roundrect
			(at 12.89 -7.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AVCC")
			(pintype "power_in")
		)
		(pad "35" smd roundrect
			(at 12.89 -8.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "R-Y+")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at 12.89 -8.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AVCC")
			(pintype "power_in")
		)
		(pad "37" smd roundrect
			(at 12.89 -9.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 265 "unconnected-(IC702-Y--Pad37)")
			(pinfunction "Y-")
			(pintype "input")
		)
		(pad "38" smd roundrect
			(at 12.89 -10.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "unconnected-(IC702-YC-Pad38)")
			(pinfunction "YC")
			(pintype "input")
		)
		(pad "39" smd roundrect
			(at 12.89 -11.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "40" smd roundrect
			(at 12.89 -12.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "unconnected-(IC702-Y-Pad40)")
			(pinfunction "Y")
			(pintype "output+no_connect")
		)
		(pad "41" smd roundrect
			(at 9.86 -15.35 90)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AVCC")
			(pintype "power_in")
		)
		(pad "42" smd roundrect
			(at 9.06 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "Y+")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at 8.26 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(IC702-RGB-)")
			(pinfunction "SYN-")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at 7.46 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "SYNCV")
			(pinfunction "SYNC")
			(pintype "output")
		)
		(pad "45" smd roundrect
			(at 6.66 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "SYN+")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at 5.86 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(IC702-RGB-)")
			(pinfunction "RGB-")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at 5.06 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "VIDEOG")
			(pinfunction "G")
			(pintype "output")
		)
		(pad "48" smd roundrect
			(at 4.26 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "49" smd roundrect
			(at 3.46 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "VIDEOR")
			(pinfunction "R")
			(pintype "output")
		)
		(pad "50" smd roundrect
			(at 2.66 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "AVCC")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at 1.86 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "VIDEOB")
			(pinfunction "B")
			(pintype "output")
		)
		(pad "52" smd roundrect
			(at 1.06 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "RGB+")
			(pintype "input")
		)
		(pad "53" smd roundrect
			(at 0.26 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "54" smd roundrect
			(at -0.54 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "55" smd roundrect
			(at -1.34 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "56" smd roundrect
			(at -2.14 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" smd roundrect
			(at -2.94 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "58" smd roundrect
			(at -3.74 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "unconnected-(IC702-TEST1-Pad58)")
			(pinfunction "TEST1")
			(pintype "output+no_connect")
		)
		(pad "59" smd roundrect
			(at -4.54 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "unconnected-(IC702-TEST2-Pad59)")
			(pinfunction "TEST2")
			(pintype "output+no_connect")
		)
		(pad "60" smd roundrect
			(at -5.34 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "unconnected-(IC702-TEST3-Pad60)")
			(pinfunction "TEST3")
			(pintype "output+no_connect")
		)
		(pad "61" smd roundrect
			(at -6.14 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "CESEL")
			(pinfunction "SEL")
			(pintype "input")
		)
		(pad "62" smd roundrect
			(at -6.94 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "VD0")
			(pinfunction "VD0")
			(pintype "bidirectional")
		)
		(pad "63" smd roundrect
			(at -7.74 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "VD1")
			(pinfunction "VD1")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at -8.54 -15.35 270)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "VD2")
			(pinfunction "VD2")
			(pintype "bidirectional")
		)
		(pad "65" smd roundrect
			(at -11.54 -12.03 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "VD3")
			(pinfunction "VD3")
			(pintype "bidirectional")
		)
		(pad "66" smd roundrect
			(at -11.54 -11.23 180)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "VD4")
			(pinfunction "VD4")
			(pintype "bidirectional")
		)
		(pad "67" smd roundrect
			(at -11.54 -10.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "VD5")
			(pinfunction "VD5")
			(pintype "bidirectional")
		)
		(pad "68" smd roundrect
			(at -11.54 -9.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "VD6")
			(pinfunction "VD6")
			(pintype "bidirectional")
		)
		(pad "69" smd roundrect
			(at -11.54 -8.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "VD7")
			(pinfunction "VD7")
			(pintype "bidirectional")
		)
		(pad "70" smd roundrect
			(at -11.54 -8.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "VD8")
			(pinfunction "VD8")
			(pintype "bidirectional")
		)
		(pad "71" smd roundrect
			(at -11.54 -7.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "XHSYNC")
			(pinfunction "HSYN")
			(pintype "input")
		)
		(pad "72" smd roundrect
			(at -11.54 -6.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "XVSYNC")
			(pinfunction "VSYN")
			(pintype "input")
		)
		(pad "73" smd roundrect
			(at -11.54 -5.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "DCK")
			(pinfunction "CK")
			(pintype "input")
		)
		(pad "74" smd roundrect
			(at -11.54 -4.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "75" smd roundrect
			(at -11.54 -4.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at -11.54 -3.23)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at -11.54 -2.43)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "~{WR}")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "78" smd roundrect
			(at -11.54 -1.63)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "~{RD}")
			(pinfunction "RD")
			(pintype "input")
		)
		(pad "79" smd roundrect
			(at -11.54 -0.83)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "~{CEK}")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "80" smd roundrect
			(at -11.54 -0.03)
			(size 0.415 2.77875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "8/16")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 182.2196 118.7958)
		(property "Reference" "TP7"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "AR4")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 171.5262 134.493)
		(property "Reference" "TP26"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "A20")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "F.Cu")
		(at 142.5679 131.5466 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D204"
			(at -0.9071 4.5716 180)
			(layer "F.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 2.4 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 180)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 179 "Net-(R203-R3.1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 180)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "VIDEOR")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 180)
			(size 1.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 170 "Net-(D204-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 180.5 77.575)
		(property "Reference" "CC103"
			(at 5.7 -2.025 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 6.3V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.7 2.475 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 245 "Net-(CC103-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 246 "Net-(CC103-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-89-3"
		(layer "F.Cu")
		(at 119.5125 41.525 180)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "Q500"
			(at -0.0125 3.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "BU OY"
			(at 0 3.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 -1.5 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 201 "Net-(Q500-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2 0 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 200 "Net-(Q500-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.2 0 180)
			(size 3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 200 "Net-(Q500-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5 0 180)
			(size 1.5 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 200 "Net-(Q500-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2 1.5 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 120.725 131.075 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C203"
			(at 4.375 0.95 270)
			(layer "F.SilkS")
		)
		(property "Value" "82pF"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 178 "EXT_BLUE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 126.325 123.475)
		(property "Reference" "CC700"
			(at 5.275 7.025 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 6.3V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.975 2.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 163.9062 125.476)
		(property "Reference" "TP25"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "A20")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 159.875 88.875)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C703"
			(at -4.6 0.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "33pF"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 178.4414 126.9602 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R710"
			(at -7.2648 -1.5914 180)
			(layer "F.SilkS")
		)
		(property "Value" "4x100"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "A10")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "A9")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "A8")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "A7")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "AR7")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "AR8")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "AR9")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "AR10")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:GT_Power_SW"
		(layer "F.Cu")
		(at 190.8 53.325)
		(property "Reference" "SW500"
			(at 0 -4.75 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Power"
			(at 0 5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 6.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -6 -3)
			(size 1.9 1.9)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at -6 3)
			(size 1.9 1.9)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 6 -3)
			(size 1.9 1.9)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 6 3)
			(size 1.9 1.9)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -4 -1.25)
			(size 1.9 1.9)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 193 "Net-(SW500-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at -4 1.25)
			(size 1.9 1.9)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 193 "Net-(SW500-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -1.25)
			(size 1.9 1.9)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 285 "VCC")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.25)
			(size 1.9 1.9)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 285 "VCC")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 4 -1.25)
			(size 1.9 1.9)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 270 "N{slash}C")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 4 1.25)
			(size 1.9 1.9)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 270 "N{slash}C")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2mm"
		(layer "F.Cu")
		(at 126.3 65.1)
		(property "Reference" "G6"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:EMI_Dual_coil_small_pads"
		(layer "F.Cu")
		(at 195.625 72.025 -90)
		(property "Reference" "X500"
			(at 4.075 6.125 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Filter"
			(at 0 0.9 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L_* L_CommonMode*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -5 -3.7 270)
			(size 1.5 1.5)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 242 "Net-(J500-Pad2)")
			(pinfunction "1")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "2" thru_hole circle
			(at 5 -3.7 270)
			(size 1.5 1.5)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "3" thru_hole circle
			(at -5 3.7 270)
			(size 1.5 1.5)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 241 "Net-(J500-Pad1)")
			(pinfunction "3")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "4" thru_hole circle
			(at 5 3.7 270)
			(size 1.5 1.5)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 240 "Net-(D500-K)")
			(pinfunction "4")
			(pintype "passive")
			(clearance 0.3)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 125.85 76.1 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R515"
			(at -4.3 -1.375 270)
			(layer "F.SilkS")
		)
		(property "Value" "150K"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 204 "Net-(D503-A-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 287 "PWR2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:GT_VR"
		(layer "F.Cu")
		(at 119.725 108.7 90)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "VR500"
			(at 0.675 -3 90)
			(layer "F.SilkS")
		)
		(property "Value" "47K"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3 -0.95 90)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 254 "Net-(R502-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.3 0.95 90)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 255 "HPOS")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6 0 90)
			(size 1.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 255 "HPOS")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2.8mm"
		(layer "F.Cu")
		(at 128.85 130.975)
		(property "Reference" "G2"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Power_Jack"
		(layer "F.Cu")
		(at 191.425 62.675)
		(property "Reference" "J500"
			(at 7.9 -5.35 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "DC IN"
			(at 0 9.25 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "2"
			(at 6.425 -3.3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at 2.925 -4.35 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -1.35 2.125 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 10.75 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 0)
			(size 2 3.3)
			(drill oval 1.25 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 241 "Net-(J500-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5 0)
			(size 2 3.3)
			(drill oval 1.25 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 242 "Net-(J500-Pad2)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 2.5 -2.75 90)
			(size 2 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 243 "Net-(J500-Pad3)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "F.Cu")
		(at 150.275 136.625 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D205"
			(at 2.0516 7.2344 180)
			(layer "F.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 180 "Net-(R203-R2.1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "VIDEOG")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(D205-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:GT_Backlight_Connector"
		(layer "F.Cu")
		(at 105.975 89.525 90)
		(property "Reference" "CN900"
			(at -6.675 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -5.925 3 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 3.65 3.825 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 4.4 1.175 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -4.775 4.55 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at -5.15 0.975 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.25 0 90)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 212 "Net-(CN900-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.25 0 90)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:CP_Radial_P2.50mm"
		(layer "F.Cu")
		(at 197.925 114.15 -90)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "CC702"
			(at 1.25 -2 270)
			(layer "F.SilkS")
		)
		(property "Value" "470uF 6.3V"
			(at 1.25 3.75 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at -3 0.75 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 286 "+5VL")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:GT_Ear"
		(layer "F.Cu")
		(at 192.9 84.65)
		(property "Reference" "J100"
			(at 0.3 8.6 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Ear"
			(at 0 8.3 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center -5 -5)
			(end -4.4 -5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center -5 5)
			(end -4.4 5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 0 0)
			(end 0.6 0)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 5 -5)
			(end 5.6 -5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 5 5)
			(end 5.6 5)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "10"
			(at -1.25 -1.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "11"
			(at -1.25 3.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "6"
			(at -6 -1.25 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at -1.25 5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -1.25 -4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4"
			(at -6 4 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at -6 1.25 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 3.7 0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 9.8 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 228 "Net-(J100-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 229 "Net-(J100-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "3" thru_hole circle
			(at 0 5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 230 "Net-(J100-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "4" thru_hole circle
			(at -5 2.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 227 "Net-(IC100A-+)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 224 "Net-(J100-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -5 -2.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 248 "Net-(IC100B-+)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 -2.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 223 "EAR1")
			(pinfunction "Pin_10")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "11" thru_hole circle
			(at 0 2.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 231 "Net-(J100-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
			(clearance 0.3)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_VR"
		(layer "F.Cu")
		(at 167.025 58.525 90)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "VR501"
			(at -4.75 0.725 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3 -0.95 90)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 195 "Net-(C507-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.3 0.95 90)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 197 "Net-(R506-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6 0 90)
			(size 1.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 195 "Net-(C507-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 187.8076 115.189)
		(property "Reference" "TP4"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "AR1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 123.275 131.075 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C202"
			(at 4.275 -1.375 270)
			(layer "F.SilkS")
		)
		(property "Value" "33pF"
			(at 0 1.65 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 177 "EXT_RED")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 119.725 104.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R503"
			(at -0.15 -2.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "47K"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 255 "HPOS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 185.775 95.325 180)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R718"
			(at -3.625 1.75 270)
			(layer "F.SilkS")
		)
		(property "Value" "4x820"
			(at 0 2.8 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 180)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "DI0")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 180)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "DI1")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 180)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "DI2")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 180)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "DI3")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 180)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 185 "Net-(IC700-K3)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 180)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 184 "Net-(IC700-K2)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 180)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 183 "Net-(IC700-K1)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 180)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 182 "Net-(IC700-K0)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 181.1528 125.4252)
		(property "Reference" "TP9"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "AR6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 181.2 96.475)
		(property "Reference" "TP38"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 184 "Net-(IC700-K2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-89-3"
		(layer "F.Cu")
		(at 115.3 122.9 180)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "Q506"
			(at -0.95 -5.075 270)
			(layer "F.SilkS")
		)
		(property "Value" "BC 0M"
			(at 0 3.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 -1.5 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 188 "Net-(Q506-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2 0 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.2 0 180)
			(size 3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5 0 180)
			(size 1.5 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2 1.5 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 287 "PWR2")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 165.9636 122.4026)
		(property "Reference" "TP21"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "AR18")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2.8mm"
		(layer "F.Cu")
		(at 172.025 59.95)
		(property "Reference" "G5"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2.8 2.8)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Strengthening_Via"
		(layer "F.Cu")
		(at 195.25 74.525)
		(property "Reference" "SV1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.2 1.2)
			(drill 0.8)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 281 "BATT+")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "F.Cu")
		(at 120.225 122.9 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R513"
			(at -4.45 -1.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "10K"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 188 "Net-(Q506-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902439)
			(net 287 "PWR2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 169.5196 122.9106)
		(property "Reference" "TP19"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "AR16")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 173.0502 135.509)
		(property "Reference" "TP27"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "D7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Ground_Pad_2mm"
		(layer "F.Cu")
		(at 182.05 131)
		(property "Reference" "G4"
			(at 0 -6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Ground"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 185.275 98.05)
		(property "Reference" "TP36"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 182 "Net-(IC700-K0)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 168.025 61.5)
		(property "Reference" "TP50"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 197 "Net-(R506-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_T900"
		(layer "F.Cu")
		(at 114.25 72.025)
		(property "Reference" "T900"
			(at 1.2 10.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "?"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr through_hole)
		(fp_text user "NC"
			(at -4.925 -2.35 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "4"
			(at 4.075 6.775 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "7"
			(at -4.9 3.675 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "3"
			(at 3.75 3.675 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 3.7 0.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at -4.925 -5.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 3.625 -5.425 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "6"
			(at 3.7 -2.4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "0" thru_hole circle
			(at -8.5 -4.5)
			(size 2 2)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at -8.5 6.1)
			(size 2 2)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 8.5 -4.5)
			(size 2 2)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "0" thru_hole circle
			(at 8.5 4.6)
			(size 2 2)
			(drill 1.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "CASE")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 6.5 -6)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 217 "Net-(Q900-C)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 210 "Net-(L900-Pad1)")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 6.5 3)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 215 "Net-(Q901-C)")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 6.5 6)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 208 "Net-(Q901-B)")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -6.5 -6)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 207 "Net-(Q900-B)")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 6.5 -3)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -6.5 3)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 211 "Net-(C901-Pad2)")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -6.5 -3)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 209 "unconnected-(T900-Pad8)")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "F.Cu")
		(at 197.4 93.95 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "L105"
			(at -0.375 2.5 270)
			(layer "F.SilkS")
		)
		(property "Value" "?H"
			(at 0 1.85 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2173913043)
			(net 228 "Net-(J100-Pin_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2173913043)
			(net 253 "Net-(L102-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 126.825 116.775)
		(property "Reference" "TP86"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 254 "Net-(R502-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 160.3756 132.0292)
		(property "Reference" "TP29"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "F.Cu")
		(at 182.353 121.3756 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R709"
			(at -12.6994 4.922 90)
			(layer "F.SilkS")
		)
		(property "Value" "4x100"
			(at 0 2.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "A6")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "A4")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "A5")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "A3")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "AR3")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "AR5")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "AR4")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "AR6")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:CP_6.2x1.6mm"
		(layer "F.Cu")
		(at 126.925 41.525)
		(property "Reference" "CC501"
			(at 1.3 -3.225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF 50V"
			(at 0 5.7 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -3.25 -2.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 200 "Net-(Q500-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 199 "Net-(D502-common)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 189.23 138.0744)
		(property "Reference" "TP30"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "HSM")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 179.1208 123.9012)
		(property "Reference" "TP10"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "AR7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:HSRM20256LM"
		(layer "F.Cu")
		(at 163.28605 75.4478 -90)
		(descr "EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "EQFP QFP")
		(property "Reference" "IC704"
			(at -1.8386 7.63485 90)
			(layer "F.SilkS")
		)
		(property "Value" "M20256"
			(at 0.55 9.22 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.85 11.15 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -7.96 5.5 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/VDC/MA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -6.69 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/VDC/MA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.42 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "/VDC/MA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -4.15 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "/VDC/MA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.88 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "/VDC/MA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -1.61 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "/VDC/MA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -0.34 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "/VDC/MA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 0.93 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "/VDC/MA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.2 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "/VDC/MA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 3.47 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/VDC/MA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 4.74 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/VDC/MD0")
			(pinfunction "I/O1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 6.01 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/VDC/MD1")
			(pinfunction "I/O2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 7.28 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/VDC/MD2")
			(pinfunction "I/O3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 8.55 5.50125 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 8.55 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/VDC/MD3")
			(pinfunction "I/O4")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 7.28 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/VDC/MD4")
			(pinfunction "I/O5")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 6.01 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/VDC/MD5")
			(pinfunction "I/O6")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.74 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/VDC/MD6")
			(pinfunction "I/O7")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 3.47 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/VDC/MD7")
			(pinfunction "I/O8")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 2.2 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/VDC/MA15")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 0.93 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "/VDC/MA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -0.34 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Net-(IC701-MRD)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -1.61 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "/VDC/MA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -2.88 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "/VDC/MA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -4.15 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "/VDC/MA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at -5.42 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "/VDC/MA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at -6.69 -5.59875 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(IC701-MWR)")
			(pinfunction "WE")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at -7.96 -5.6 270)
			(size 0.57 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 177.6222 122.8852)
		(property "Reference" "TP11"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "AR8")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:CP_8.4x1.7mm"
		(layer "F.Cu")
		(at 146.675 143.725 -90)
		(property "Reference" "CC505"
			(at 1.025 -4.325 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF 6.3V"
			(at 0 5.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.05 -2.4 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 7.2 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6 0 270)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 288 "PWR4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.6 0 270)
			(size 3.2 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 174.5488 132.4864)
		(property "Reference" "TP24"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "A10")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:FFC_Connector_40P"
		(layer "F.Cu")
		(at 173.5502 144.2212 180)
		(property "Reference" "CN0"
			(at 0 -4 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HuCard FFC"
			(at 0 4.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -19.1342 2.8702 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "40"
			(at 19.4992 2.8194 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 6 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -19.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -18.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "~{XIRQ2}")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -17.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "~{RST-OSC}")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at -16.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "HSM")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at -15.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "~{WR}")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at -14.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "A18")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -13.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "A17")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at -12.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "A14")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd roundrect
			(at -11.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "A13")
			(pinfunction "Pin_9")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd roundrect
			(at -10.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "A8")
			(pinfunction "Pin_10")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd roundrect
			(at -9.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "A9")
			(pinfunction "Pin_11")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "12" smd roundrect
			(at -8.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "A11")
			(pinfunction "Pin_12")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "13" smd roundrect
			(at -7.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "~{RD}")
			(pinfunction "Pin_13")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "14" smd roundrect
			(at -6.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "A10")
			(pinfunction "Pin_14")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "15" smd roundrect
			(at -5.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "A20")
			(pinfunction "Pin_15")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "16" smd roundrect
			(at -4.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "D7")
			(pinfunction "Pin_16")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "17" smd roundrect
			(at -3.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "D6")
			(pinfunction "Pin_17")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "18" smd roundrect
			(at -2.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D5")
			(pinfunction "Pin_18")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "19" smd roundrect
			(at -1.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "D4")
			(pinfunction "Pin_19")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "20" smd roundrect
			(at -0.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D3")
			(pinfunction "Pin_20")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "21" smd roundrect
			(at 0.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 167 "Net-(CN0-Pin_21)")
			(pinfunction "Pin_21")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "22" smd roundrect
			(at 1.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 237 "HUCARD_AUDIO")
			(pinfunction "Pin_22")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "23" smd roundrect
			(at 2.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "A19")
			(pinfunction "Pin_23")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "24" smd roundrect
			(at 3.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "A16")
			(pinfunction "Pin_24")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "25" smd roundrect
			(at 4.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "A15")
			(pinfunction "Pin_25")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "26" smd roundrect
			(at 5.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "A12")
			(pinfunction "Pin_26")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "27" smd roundrect
			(at 6.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "A7")
			(pinfunction "Pin_27")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "28" smd roundrect
			(at 7.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "A6")
			(pinfunction "Pin_28")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "29" smd roundrect
			(at 8.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "A5")
			(pinfunction "Pin_29")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "30" smd roundrect
			(at 9.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "A4")
			(pinfunction "Pin_30")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "31" smd roundrect
			(at 10.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "A3")
			(pinfunction "Pin_31")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "32" smd roundrect
			(at 11.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "A2")
			(pinfunction "Pin_32")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "33" smd roundrect
			(at 12.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "A1")
			(pinfunction "Pin_33")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "34" smd roundrect
			(at 13.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "A0")
			(pinfunction "Pin_34")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "35" smd roundrect
			(at 14.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "D0")
			(pinfunction "Pin_35")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "36" smd roundrect
			(at 15.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D1")
			(pinfunction "Pin_36")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "37" smd roundrect
			(at 16.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "D2")
			(pinfunction "Pin_37")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "38" smd roundrect
			(at 17.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_38")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "39" smd roundrect
			(at 18.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_39")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "40" smd roundrect
			(at 19.5 0 270)
			(size 3 0.625)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_40")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "F.Cu")
		(at 151.257 123.444)
		(property "Reference" "TP1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(IC702-RGB-)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "F.Cu")
		(at 117.2625 92.25 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D902"
			(at -0.0125 -3.275 180)
			(layer "F.SilkS")
		)
		(property "Value" "D3E"
			(at 0 2.4 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 180)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "PWR2")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 180)
			(size 1.2 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "PWR2")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 180)
			(size 1.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "Net-(D900-A)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 184.125 86.3 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R107"
			(at -2.35 12.35 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 248 "Net-(IC100B-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 174.498 96.4946 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C705"
			(at -0.0696 -2.877 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 7 "OSC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 6 "Net-(IC700-OSC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "B.Cu")
		(at 194.25 108.075 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D700"
			(at 7 -1.55 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "~{RST-OSC}")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "~{RST-OSC}")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 180)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 197.825 87.825 180)
		(property "Reference" "TP67"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 228 "Net-(J100-Pin_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 118.25 80.225 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C902"
			(at 1 -2.275 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 207 "Net-(Q900-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 218 "Net-(D901-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 120.75 55.875 180)
		(property "Reference" "TP52"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 203 "Net-(D503-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 115.175 81.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R903"
			(at -4.3 -2.925 180)
			(layer "B.SilkS")
		)
		(property "Value" "12K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 218 "Net-(D901-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 106.05 96.85 180)
		(property "Reference" "TP900"
			(at -3.75 1.225 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 212 "Net-(CN900-Pin_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 195.325 66.05 180)
		(property "Reference" "TP509"
			(at -3.475 0.775 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 282 "BATT-")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 134.95 80.725 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C714"
			(at -0.2 2.7 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.5uF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:L_1008"
		(layer "B.Cu")
		(at 188.775 67.05 90)
		(descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L501"
			(at -1.225 4.85 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1uH?"
			(at 0 -2.05 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.1 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 282 "BATT-")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -1.075 0 90)
			(size 1.25 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 282 "BATT-")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.075 0 90)
			(size 1.25 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 243 "Net-(J500-Pad3)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.1 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 243 "Net-(J500-Pad3)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 169.475 62.55 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C719"
			(at 4.925 0.05 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "270nF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:HSRM20256LM"
		(layer "B.Cu")
		(at 163.35815 75.524 -90)
		(descr "EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "EQFP QFP")
		(property "Reference" "IC705"
			(at -5.9026 -7.86325 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "M20256"
			(at 0.55 -9.22 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.85 -11.15 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -7.96 -5.5 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/VDC/MA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -6.69 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/VDC/MA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.42 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 125 "/VDC/MA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -4.15 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 124 "/VDC/MA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.88 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 123 "/VDC/MA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -1.61 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 122 "/VDC/MA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -0.34 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 121 "/VDC/MA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 0.93 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 120 "/VDC/MA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.2 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 119 "/VDC/MA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 3.47 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/VDC/MA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 4.74 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/VDC/MD8")
			(pinfunction "I/O1")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 6.01 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/VDC/MD9")
			(pinfunction "I/O2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 7.28 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/VDC/MD10")
			(pinfunction "I/O3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 8.55 -5.50125 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 8.55 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 113 "/VDC/MD11")
			(pinfunction "I/O4")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 7.28 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/VDC/MD12")
			(pinfunction "I/O5")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 6.01 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/VDC/MD13")
			(pinfunction "I/O6")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.74 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/VDC/MD14")
			(pinfunction "I/O7")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 3.47 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/VDC/MD15")
			(pinfunction "I/O8")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 2.2 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/VDC/MA15")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 0.93 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 128 "/VDC/MA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -0.34 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 101 "Net-(IC701-MRD)")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -1.61 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 129 "/VDC/MA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -2.88 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "/VDC/MA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -4.15 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 126 "/VDC/MA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at -5.42 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 131 "/VDC/MA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at -6.69 5.59875 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(IC701-MWR)")
			(pinfunction "WE")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at -7.96 5.6 270)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 158.1912 115.2652)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R176"
			(at -0.0412 2.8098 180)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 30 "~{RD}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 162 "Net-(IC700-RD)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 194.775 111.125)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R701"
			(at -1.1 7.45 180)
			(layer "B.SilkS")
		)
		(property "Value" "470K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 1 "~{RST-OSC}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 131.2926 140.589 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C513"
			(at 4.014 -0.0176 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 273 "LCD_BRIGHT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 195.775 97.45 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R111"
			(at -4.2 3.375 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 252 "Net-(L102-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 112.625 85.85 180)
		(property "Reference" "TP60"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 218 "Net-(D901-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "B.Cu")
		(at 188.225 94.45 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C102"
			(at 10.325 -0.675 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 234 "Net-(R101-R1.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 235 "Net-(C102-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 132.325 102.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C716"
			(at 0.375 -2.65 180)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 114.625 92.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R905"
			(at -5.625 0.15 0)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 219 "Net-(D901-A-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 220 "SLEEP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 179.025 97 180)
		(property "Reference" "TP75"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 232 "Net-(R101-R3.2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 164.4396 131.0621 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R713"
			(at 2.3121 -3.0146 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 60 "A19")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 160 "AR19")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_1206_GT_Narrow"
		(layer "B.Cu")
		(at 177.292 64.008 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R102"
			(at 0.233 -3.642 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 284 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 285 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 125.85 50.75 180)
		(property "Reference" "TP54"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 206 "Net-(C501-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 141.575 62.025)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R508"
			(at 7.075 -7.425 180)
			(layer "B.SilkS")
		)
		(property "Value" "10K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 285 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 196 "Net-(Q502-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 117.15 92.5 180)
		(property "Reference" "TP61"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 221 "Net-(D900-common)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 159.2478 100.5586)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C712"
			(at -5.6978 0.0164 180)
			(layer "B.SilkS")
		)
		(property "Value" "1.5uF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 286 "+5VL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 189.7 100 180)
		(property "Reference" "TP63"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 224 "Net-(J100-Pin_5)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "B.Cu")
		(at 164.327 99.8664 180)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R707"
			(at 3.127 -3.4336 0)
			(layer "B.SilkS")
		)
		(property "Value" "4x5.6K"
			(at 0 -2.8 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.9 1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 164 "unconnected-(R707-R1.1-Pad1)")
			(pinfunction "R1.1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -0.9 0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 87 "~{IRQ+PUP}")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 -0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 44 "~{XIRQ2}")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 -1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "RDY")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 -1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 286 "+5VL")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 -0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 286 "+5VL")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 286 "+5VL")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 165 "unconnected-(R707-R1.2-Pad8)")
			(pinfunction "R1.2")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 185.1 115.725 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C711"
			(at -0.025 2.775 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.5uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 286 "+5VL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_1206_GT_Phat"
		(layer "B.Cu")
		(at 123.875 40.125 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "L500"
			(at 0 2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "?H"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.75 0 180)
			(size 1.7 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173911765)
			(net 285 "VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.75 0 180)
			(size 1.7 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173911765)
			(net 214 "Net-(C500-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 183.65 76.175 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R109"
			(at -6.625 6.025 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 246 "Net-(CC103-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 190.225 84.75 180)
		(property "Reference" "TP70"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 231 "Net-(J100-Pin_11)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 121.7 62.55 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C504"
			(at 2.9 -1.425 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1nF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 255 "HPOS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 180.5875 87.325)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R108"
			(at -4.2625 -0.8 180)
			(layer "B.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 227 "Net-(IC100A-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 174.9704 103.5304)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C707"
			(at -1.3704 2.3446 180)
			(layer "B.SilkS")
		)
		(property "Value" "10nF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 71 "AGND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 8 "AUDIO-L")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 150.6 110.675 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C715"
			(at 0.7 -2.775 0)
			(layer "B.SilkS")
		)
		(property "Value" "270nF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 174.4726 93.4212)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C704"
			(at -5.2476 -4.7462 180)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 7 "OSC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 134.475 65.075)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C503"
			(at -1.125 2.475 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 198 "Net-(D501-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 118.225 70.15 180)
		(property "Reference" "TP58"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 217 "Net-(Q900-C)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:FFC_Connector_8P_Flip"
		(layer "B.Cu")
		(at 109.4232 126.5856 90)
		(property "Reference" "CN200"
			(at -8.0894 -3.4482 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "AV IN"
			(at 0 -9.1 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -5.6144 -1.0232 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "8"
			(at 6.0856 -1.0732 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -10.6 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 289 "PWR")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -2.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 189 "EXT_BRIGHT")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at -1.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 178 "EXT_BLUE")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at -0.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 177 "EXT_RED")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 0.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 174 "EXT_GREEN")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 1.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 287 "PWR2")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at 2.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 173 "EXT_AUDIO")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at 3.5 0)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 189.725 74.6 180)
		(property "Reference" "TP81"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 240 "Net-(D500-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:FFC_Connector_8P"
		(layer "B.Cu")
		(at 138.6666 138.2522 180)
		(property "Reference" "CN201"
			(at -0.4834 -5.8978 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "LCD"
			(at 0 -9.1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "8"
			(at -5.4584 -1.1728 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at 4.3666 1.0772 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -10.6 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 3.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 2.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 273 "LCD_BRIGHT")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 1.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 272 "PWR3")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 0.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 274 "LCD_SYNC")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at -0.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 275 "LCD_BLUE")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at -1.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 276 "LCD_RED")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -2.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 277 "LCD_GREEN")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at -3.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 288 "PWR4")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 115.175 74.675 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C904"
			(at 4.1 0.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 213 "Net-(Q903-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 117.125 116.825 180)
		(property "Reference" "TP501"
			(at 0 2 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 272 "PWR3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-23-5-Reversed"
		(layer "B.Cu")
		(at 114.625 124.5375 90)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q504"
			(at -2.9625 7.45 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "XN1211"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 190 "Net-(Q504-Pad1)")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 280 "Net-(Q504-Pad2)")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 173 "EXT_AUDIO")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 280 "Net-(Q504-Pad2)")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin1"
		(layer "B.Cu")
		(at 115.175 78.2 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q903"
			(at 0.875 -4.375 0)
			(layer "B.SilkS")
		)
		(property "Value" "BR E"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 218 "Net-(D901-K)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 213 "Net-(Q903-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 110.65 69.15 180)
		(property "Reference" "TP57"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 207 "Net-(Q900-B)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 191.75 94.95 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "L101"
			(at -5.625 -6.55 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "?H"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 249 "Net-(CC104-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 250 "Net-(L101-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 149.5552 138.0998)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C512"
			(at 4.2448 3.8252 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 288 "PWR4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 183.6 100 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R103"
			(at -10.65 0.625 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "3.9K"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 238 "VOL_IN_R")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 235 "Net-(C102-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 139 67.125 180)
		(property "Reference" "TP48"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 279 "Net-(Q503-Pad4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 126.325 75.675 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R514"
			(at -4.25 -0.125 0)
			(layer "B.SilkS")
		)
		(property "Value" "47K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 272 "PWR3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 204 "Net-(D503-A-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 116.2 72.675 180)
		(property "Reference" "TP55"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 213 "Net-(Q903-E)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 110.675 65.125 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R900"
			(at 0.8 -3.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 207 "Net-(Q900-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 216 "BLH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 197.325 93.85 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "L102"
			(at 4.1 -0.95 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "?H"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 252 "Net-(L102-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 253 "Net-(L102-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 157.734 98.044)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R704"
			(at -4.359 -1.669 180)
			(layer "B.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 286 "+5VL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 71 "AGND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 145.575 59.5 180)
		(property "Reference" "TP49"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 196 "Net-(Q502-B)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 177.0126 90.932 180)
		(property "Reference" "TP32"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "OSC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 117.725 87.35 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C903"
			(at -0.575 -2.45 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 218 "Net-(D901-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 221 "Net-(D900-common)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "B.Cu")
		(at 194.775 103.525 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C702"
			(at 9 -4.9 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 1 "~{RST-OSC}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "B.Cu")
		(at 114.625 88.95 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D901"
			(at 0.9 -4.125 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 219 "Net-(D901-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 219 "Net-(D901-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 218 "Net-(D901-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 190.225 98.475 180)
		(property "Reference" "TP83"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 250 "Net-(L101-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 139.9032 130.0226 90)
		(property "Reference" "TP34"
			(at 0 0.5 270)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 278 "RGB_EN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 174.9704 101.0412)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C708"
			(at -4.5704 -1.4912 180)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 71 "AGND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 46 "AUDIO-R")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 117.825 49.725 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C500"
			(at 1.525 -3.375 0)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 214 "Net-(C500-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 187.675 97.575 180)
		(property "Reference" "TP74"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 235 "Net-(C102-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 134.8 59.9 180)
		(property "Reference" "TP500"
			(at 3.1 1.425 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 198 "Net-(D501-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 118.175 134.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C201"
			(at 4.1 1.05 180)
			(layer "B.SilkS")
		)
		(property "Value" "82pF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 174 "EXT_GREEN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:TO-252"
		(layer "B.Cu")
		(at 153.275 60)
		(descr "TO-252/DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
		(tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
		(property "Reference" "Q502"
			(at 2.175 -5.225 180)
			(layer "B.SilkS")
		)
		(property "Value" "B1182"
			(at 0 -4.5 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -5.04 2.28)
			(size 3.2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2083327778)
			(net 196 "Net-(Q502-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 6 6)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.043103)
			(net 287 "PWR2")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -5.04 -2.28)
			(size 3.2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2083327778)
			(net 285 "VCC")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:FFC_Connector_2P"
		(layer "B.Cu")
		(at 193.975 72.075 -90)
		(property "Reference" "CN500"
			(at 11.5 -1.875 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Battery"
			(at 0 -9.1 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_circle
			(center -2.3 -3.1)
			(end -1.6 -3.1)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 2.3 -3.1)
			(end 3 -3.1)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -10.6 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 1 0)
			(size 4 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 281 "BATT+")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at -1 0)
			(size 4 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 282 "BATT-")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 116.6 127.975 180)
		(property "Reference" "TP45"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 280 "Net-(Q504-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 193.25 114.175 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R706"
			(at -0.65 -2.325 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "000"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 286 "+5VL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 185.175 72.1 180)
		(property "Reference" "TP84"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 251 "Net-(L100-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 138 62.025)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R504"
			(at -5.125 0.45 180)
			(layer "B.SilkS")
		)
		(property "Value" "100K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 198 "Net-(D501-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 268 "Net-(ZD501-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 187.6 115.725 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C710"
			(at -3.425 -1.525 180)
			(layer "B.SilkS")
		)
		(property "Value" "330nF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 286 "+5VL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_1206_GT_Narrow"
		(layer "B.Cu")
		(at 179.578 64.008 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R112"
			(at 6.533 -4.228 180)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 284 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 90)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 285 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:HSRM20256LM"
		(layer "B.Cu")
		(at 170.3226 114.56455 180)
		(descr "EQFP, 144 Pin (https://www.intel.com/content/dam/www/programmable/us/en/pdfs/literature/packaging/04r00476-02.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "EQFP QFP")
		(property "Reference" "IC703"
			(at -3.1848 -7.73645 0)
			(layer "B.SilkS")
		)
		(property "Value" "M2264"
			(at 0.55 -9.22 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.85 -11.15 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -7.96 -5.5 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 138 "unconnected-(IC703-N{slash}C-Pad1)")
			(pinfunction "N/C")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -6.69 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.42 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 39 "A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -4.15 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 58 "A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.88 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -1.61 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 57 "A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -0.34 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 0.93 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "A2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at 2.2 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "A1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 3.47 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "A0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 4.74 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 54 "D0")
			(pinfunction "I/O3")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at 6.01 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D1")
			(pinfunction "I/O2")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 7.28 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "D2")
			(pinfunction "I/O1")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 8.55 -5.50125 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 8.55 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D3")
			(pinfunction "I/O4")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 7.28 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "D4")
			(pinfunction "I/O5")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 6.01 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D5")
			(pinfunction "I/O6")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 4.74 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "D6")
			(pinfunction "I/O7")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 3.47 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 31 "D7")
			(pinfunction "I/O8")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 2.2 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 90 "~{CER}")
			(pinfunction "CS1")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 0.93 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -0.34 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "~{RD}")
			(pinfunction "OE")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -1.61 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 50 "A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -2.88 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -4.15 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at -5.42 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at -6.69 5.59875 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "~{WR}")
			(pinfunction "WE")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at -7.96 5.6 180)
			(size 0.57 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/EQFP-144-1EP_20x20mm_P0.5mm_EP5x5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-6-Reversed"
		(layer "B.Cu")
		(at 123.825 54.8125 -90)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q501"
			(at -0.5875 4.125 180)
			(layer "B.SilkS")
		)
		(property "Value" "5H O.H"
			(at 0 -2.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 201 "Net-(Q500-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(D503-K)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 201 "Net-(Q500-B)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 255 "HPOS")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 205 "Net-(ZD500-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 194.35 57.4 180)
		(property "Reference" "TP507"
			(at 1.175 7.425 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 271 "Net-(D500-A)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 128.4 47.7 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C501"
			(at -3.025 -2.375 0)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 291 "Net-(C501-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 206 "Net-(C501-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "B.Cu")
		(at 185.65 94.45 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C103"
			(at -4.375 1.725 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 233 "Net-(R101-R2.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 236 "Net-(C103-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 167.375 95.525 180)
		(property "Reference" "TP22"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 269 "Net-(Q700-B)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 146.5072 138.6078 180)
		(property "Reference" "TP504"
			(at 2.6572 -7.3922 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 273 "LCD_BRIGHT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 147.5486 141.1224 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R512"
			(at 1.1486 -2.4776 0)
			(layer "B.SilkS")
		)
		(property "Value" "12K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 191 "Net-(VR502-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 273 "LCD_BRIGHT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 124.85 47.7 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R501"
			(at -2.025 -6.4 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 206 "Net-(C501-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 201 "Net-(Q500-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 143.0122 98.552 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C706"
			(at 0.0372 2.702 0)
			(layer "B.SilkS")
		)
		(property "Value" "220pF"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 7 "OSC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 5 "Net-(IC702-OSC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin2+3"
		(layer "B.Cu")
		(at 115.625 96.025 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D900"
			(at -0.125 4.75 0)
			(layer "B.SilkS")
		)
		(property "Value" "K S1"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 222 "Net-(D900-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 222 "Net-(D900-A)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 221 "Net-(D900-common)")
			(pinfunction "common")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 159.75 95.025 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R703"
			(at -4.45 -0.05 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "13K"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 269 "Net-(Q700-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 286 "+5VL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 167.875 104.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C718"
			(at 1.525 3.075 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.5uF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 163.8 94.475 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R705"
			(at -4.4 -0.075 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "6.8K"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 269 "Net-(Q700-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 155.2702 68.6054 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C721"
			(at 4.2196 -0.1048 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 146.675 64.625)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C507"
			(at 3.225 1.625 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 195 "Net-(C507-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 287 "PWR2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-5-Reversed"
		(layer "B.Cu")
		(at 113.675 71.125 90)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q902"
			(at -0.325 -4.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "9L O.5"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 208 "Net-(Q901-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 207 "Net-(Q900-B)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 220 "SLEEP")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 213 "Net-(Q903-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "B.Cu")
		(at 138.025 57.4 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D501"
			(at 1.275 3.175 0)
			(layer "B.SilkS")
		)
		(property "Value" "?"
			(at 0 -2.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 194 "Net-(D501-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 194 "Net-(D501-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 180)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 198 "Net-(D501-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "B.Cu")
		(at 181.575 96.125 180)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R101"
			(at 1.975 4.45 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4x5.6K"
			(at 0 -2.8 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.9 1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 234 "Net-(R101-R1.1)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.9 0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 233 "Net-(R101-R2.1)")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 -0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 233 "Net-(R101-R2.1)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 -1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 234 "Net-(R101-R1.1)")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 -1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 232 "Net-(R101-R3.2)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 -0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 232 "Net-(R101-R3.2)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 0.4 180)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "AUDIO-L")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 1.275 180)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "AUDIO-R")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-6-Reversed"
		(layer "B.Cu")
		(at 136.375 132.2875 -90)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q201"
			(at -0.6125 4.75 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "5C O.H"
			(at 0 -2.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 278 "RGB_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 187 "Net-(C200-Pad2)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 274 "LCD_SYNC")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 172 "Net-(D206-K)")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 270)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 275 "LCD_BLUE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 123.725 84.3 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R516"
			(at -3.625 -2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "6.8K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 198 "Net-(D501-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 289 "PWR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "B.Cu")
		(at 149.5552 134.5923 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D207"
			(at 5.3673 -0.7552 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "D3E"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 288 "PWR4")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 288 "PWR4")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 278 "RGB_EN")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 131.975 47.2 180)
		(property "Reference" "TP505"
			(at 0.45 4.625 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 118.25 75.225 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R904"
			(at -4.675 -9.3 180)
			(layer "B.SilkS")
		)
		(property "Value" "3.6K"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 213 "Net-(Q903-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 222 "Net-(D900-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 152.7302 68.6054 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C722"
			(at 4.2196 0.4552 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.5uF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 138 65.075 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R505"
			(at 0.125 -3.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "390"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 279 "Net-(Q503-Pad4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 113.6 120.325 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R510"
			(at 0.775 8.6 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "6.8K"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 280 "Net-(Q504-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 287 "PWR2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 185.65 91.325 180)
		(property "Reference" "TP72"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 233 "Net-(R101-R2.1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 116.675 84.3 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R902"
			(at 6.125 -0.675 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "91K?"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 222 "Net-(D900-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 218 "Net-(D901-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 123.25 73.175 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C900"
			(at 0.175 5.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 215 "Net-(Q901-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 217 "Net-(Q900-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:FFC_Connector_12P"
		(layer "B.Cu")
		(at 119.375 140.8 180)
		(property "Reference" "CN700"
			(at -0.9 -5.675 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Controller"
			(at 0 -9.1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "12"
			(at -9.3 -0.575 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at 6.525 -0.425 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -10.6 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 5.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 287 "PWR2")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd roundrect
			(at 4.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 63 "DI0")
			(pinfunction "Pin_2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd roundrect
			(at 3.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 64 "DI1")
			(pinfunction "Pin_3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd roundrect
			(at 2.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "DI2")
			(pinfunction "Pin_4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 1.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 66 "DI3")
			(pinfunction "Pin_5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd roundrect
			(at 0.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 67 "SEL")
			(pinfunction "Pin_6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd roundrect
			(at -0.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 68 "CLR")
			(pinfunction "Pin_7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd roundrect
			(at -1.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 220 "SLEEP")
			(pinfunction "Pin_8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd roundrect
			(at -2.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "Pin_9")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd roundrect
			(at -3.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd roundrect
			(at -4.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 223 "EAR1")
			(pinfunction "Pin_11")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "12" smd roundrect
			(at -5.5 0 270)
			(size 3 0.625)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 188.275 58.95 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R517"
			(at -5.7 4.675 180)
			(layer "B.SilkS")
		)
		(property "Value" "330"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 271 "Net-(D500-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 281 "BATT+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "B.Cu")
		(at 126.4125 58.975 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "ZD500"
			(at -2.1125 4.9 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "6.2L"
			(at 0 -2.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 272 "PWR3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 272 "PWR3")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 180)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 205 "Net-(ZD500-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 192.6 58.15 180)
		(property "Reference" "TP508"
			(at 10.675 9.6 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 241 "Net-(J500-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-89-3"
		(layer "B.Cu")
		(at 114.675 63.675 90)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "Q900"
			(at 1.9 -4.75 0)
			(layer "B.SilkS")
		)
		(property "Value" "2SD1898"
			(at 0 -3.5 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 1.5 90)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 207 "Net-(Q900-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2 0 90)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 217 "Net-(Q900-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.2 0 90)
			(size 3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 217 "Net-(Q900-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5 0 90)
			(size 1.5 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 217 "Net-(Q900-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2 -1.5 90)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 192.25 99.475 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R110"
			(at -4.175 0.425 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 249 "Net-(CC104-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 176.525 77.675 180)
		(property "Reference" "TP66"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 226 "Net-(IC100A--)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:GT_Solder_Jumper"
		(layer "B.Cu")
		(at 118.35 40.65 -90)
		(descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "R999"
			(at 0 2.05 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "000"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd rect
			(at -0.65 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 285 "VCC")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.65 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 216 "BLH")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 179.075 67.6 180)
		(property "Reference" "TP80"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 284 "+5VP")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 144.05 80.725 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C713"
			(at 2.05 -2.875 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "270nF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-5-Reversed"
		(layer "B.Cu")
		(at 142.575 66.0875 90)
		(descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q503"
			(at -3.7625 0.125 0)
			(layer "B.SilkS")
		)
		(property "Value" "5R O.O"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 196 "Net-(Q502-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 285 "VCC")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 195 "Net-(C507-Pad1)")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 279 "Net-(Q503-Pad4)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 268 "Net-(ZD501-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 181.575 103.55 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R100"
			(at 4.325 0.2 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "2.7K"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 232 "Net-(R101-R3.2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 237 "HUCARD_AUDIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 164.8 104.5 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C717"
			(at -1.1 -3.725 0)
			(layer "B.SilkS")
		)
		(property "Value" "270nF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 194.775 84.75 180)
		(property "Reference" "TP69"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 230 "Net-(J100-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "B.Cu")
		(at 192.775 92.4)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "L104"
			(at -2.7 -3.525 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "?H"
			(at 0 -1.85 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 250 "Net-(L101-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 230 "Net-(J100-Pin_3)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 183.6 103.55 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R104"
			(at 4.1 0.8 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "3.9K"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 236 "Net-(C103-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 239 "VOL_IN_L")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 197.8152 119.7864 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C701"
			(at -4.2886 -1.5402 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 237 "HUCARD_AUDIO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 166.925 62.55 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C720"
			(at 4.925 0.05 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.5uF"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/VDC/")
		(sheetfile "vdc.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 195.825 79.65 180)
		(property "Reference" "TP68"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 229 "Net-(J100-Pin_2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 196.94 59.96 180)
		(property "Reference" "TP510"
			(at -2.4 0.025 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 242 "Net-(J500-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 181.65 71.65)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C101"
			(at 6.425 -0.7 180)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 284 "+5VP")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 190.7032 136.017 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R700"
			(at 0.092 2.6218 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Connectors/")
		(sheetfile "connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 167 "Net-(CN0-Pin_21)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 3 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 199.85 96.45 180)
		(property "Reference" "TP85"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 252 "Net-(L102-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 118.2 72.125 180)
		(property "Reference" "TP59"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 215 "Net-(Q901-C)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOIC-8_P1.27mm"
		(layer "B.Cu")
		(at 179.55 81.835 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC100"
			(at 5.225 0.335 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "NJM2073"
			(at 0 -3.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.25 1.905 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 245 "Net-(CC103-Pad1)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -3.25 0.635 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 284 "+5VP")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -3.25 -0.635 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 283 "Net-(CC104-Pad1)")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -3.25 -1.905 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 3.25 -1.905 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 225 "Net-(IC100B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 3.25 -0.635 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 248 "Net-(IC100B-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 3.25 0.635 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 227 "Net-(IC100A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 3.25 1.905 180)
			(size 1.5 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 226 "Net-(IC100A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 180.6 76.175 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R106"
			(at 6.6 -5.05 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "820"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 225 "Net-(IC100B--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 247 "Net-(CC102-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 138.425 127.475 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R202"
			(at -4.25 -0.05 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "3.3K"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 61 "SYNCV")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 187 "Net-(C200-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 198.775 128.475 90)
		(property "Reference" "TP100"
			(at -1.325 -3.85 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 223 "EAR1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 106.05 82.625 180)
		(property "Reference" "TP901"
			(at -0.725 2.225 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 171.9834 88.8746 180)
		(property "Reference" "TP31"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 166 "Net-(X700-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 117.65 120.9 180)
		(property "Reference" "TP44"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 190 "Net-(Q504-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 118.3 43.7 180)
		(property "Reference" "TP902"
			(at 1.125 -2.475 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 216 "BLH")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 174.4726 90.932 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R702"
			(at -1.6024 2.282 0)
			(layer "B.SilkS")
		)
		(property "Value" "120"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 7 "OSC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 166 "Net-(X700-OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 126.95 44.15)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C502"
			(at -1.05 -1.725 180)
			(layer "B.SilkS")
		)
		(property "Value" "1nF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 200 "Net-(Q500-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 185.65 97.575 180)
		(property "Reference" "TP73"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 236 "Net-(C103-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:R_Array_4x0603"
		(layer "B.Cu")
		(at 113.9 133.525 90)
		(descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
		(tags "resistor array")
		(property "Reference" "R203"
			(at 2.75 6.325 0)
			(layer "B.SilkS")
		)
		(property "Value" "4x150"
			(at 0 -2.8 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.9 1.275 90)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 175 "unconnected-(R203-R1.1-Pad1)")
			(pinfunction "R1.1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -0.9 0.4 90)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 180 "Net-(R203-R2.1)")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 179 "Net-(R203-R3.1)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 181 "Net-(R203-R4.1)")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.9 -1.275 90)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 178 "EXT_BLUE")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.9 -0.4 90)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 177 "EXT_RED")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.9 0.4 90)
			(size 0.8 0.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 174 "EXT_GREEN")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.9 1.275 90)
			(size 0.8 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 176 "unconnected-(R203-R1.2-Pad8)")
			(pinfunction "R1.2")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "B.Cu")
		(at 179.575 100.5 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C100"
			(at 1.2 -6.125 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 232 "Net-(R101-R3.2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 173 "EXT_AUDIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 114.775 52.25 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R901"
			(at 4.45 1.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 208 "Net-(Q901-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 216 "BLH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin1"
		(layer "B.Cu")
		(at 169.925 95.45 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q700"
			(at 3.3 -0.75 0)
			(layer "B.SilkS")
		)
		(property "Value" "FR 46"
			(at 0 -2.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 269 "Net-(Q700-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 90)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 71 "AGND")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 90)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 117.175 89.95 180)
		(property "Reference" "TP62"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 219 "Net-(D901-A-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 182.1 85.55 180)
		(property "Reference" "TP65"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 248 "Net-(IC100B-+)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 158.1912 112.2172 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R175"
			(at 0.0912 2.5922 0)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/CPU/")
		(sheetfile "cpu.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 163 "Net-(IC700-WR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 28 "~{WR}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:L_1008"
		(layer "B.Cu")
		(at 186.725 62.55 180)
		(descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L502"
			(at 2.025 4.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uH?"
			(at 0 -2.05 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 90)
			(size 1.1 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 281 "BATT+")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at -1.075 0 180)
			(size 1.25 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 281 "BATT+")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.075 0 180)
			(size 1.25 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 271 "Net-(D500-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 90)
			(size 1.1 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2)
			(net 271 "Net-(D500-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 133.325 127.45 180)
		(property "Reference" "TP43"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 187 "Net-(C200-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 178.55 76.175 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R105"
			(at 0.55 -3.525 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "820"
			(at 0 -1.65 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 226 "Net-(IC100A--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 244 "Net-(CC101-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 135.9 127.475 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C200"
			(at -4.3 -0.15 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 61 "SYNCV")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 187 "Net-(C200-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-Box-Pin3"
		(layer "B.Cu")
		(at 121.7375 58.975 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D503"
			(at 3.4125 0.15 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "?"
			(at 0 -2.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV70_SER.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 204 "Net-(D503-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 180)
			(size 1.2 0.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 204 "Net-(D503-A-Pad1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.125 0 180)
			(size 1.2 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(D503-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-89-3"
		(layer "B.Cu")
		(at 113.875 56.375 180)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "Q901"
			(at 3.95 -1.225 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "2SD1898"
			(at 0 -3.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 1.5 180)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 208 "Net-(Q901-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2 0 180)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 215 "Net-(Q901-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.2 0 180)
			(size 3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 215 "Net-(Q901-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5 0 180)
			(size 1.5 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 215 "Net-(Q901-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2 -1.5 180)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 186.7625 74.6 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "L100"
			(at -1.3125 2.125 0)
			(layer "B.SilkS")
		)
		(property "Value" "?H"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 251 "Net-(L100-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 246 "Net-(CC103-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805_Narrow"
		(layer "B.Cu")
		(at 146.675 67.1 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R507"
			(at -1.175 -2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 287 "PWR2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 195 "Net-(C507-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 115.075 130.5 180)
		(property "Reference" "TP35"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 174 "EXT_GREEN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 127.95 80.65 180)
		(property "Reference" "TP502"
			(at -1.475 -2.5 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 287 "PWR2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 180.1 78.725 180)
		(property "Reference" "TP64"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 225 "Net-(IC100B--)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 142.1 56.85)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C505"
			(at 1.25 -2.675 180)
			(layer "B.SilkS")
		)
		(property "Value" "180nF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 268 "Net-(ZD501-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 115.775 49.7 180)
		(property "Reference" "TP56"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 208 "Net-(Q901-B)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SOT-89-3"
		(layer "B.Cu")
		(at 183.675 66.825 90)
		(descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
		(tags "SOT-89-3")
		(property "Reference" "D500"
			(at 8.5 -2.45 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "SI H"
			(at 0 -3.5 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 250.5 -116.85 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 250.5 -116.85 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.2 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2 1.5 90)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 240 "Net-(D500-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2 0 90)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 271 "Net-(D500-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.2 0 90)
			(size 3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 271 "Net-(D500-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5 0 90)
			(size 1.5 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 271 "Net-(D500-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2 -1.5 90)
			(size 1.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SOT-23-6-Reversed"
		(layer "B.Cu")
		(at 143.5 132.525 180)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q200"
			(at -1.575 5.375 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "5H O.H"
			(at 0 -2.4 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 278 "RGB_EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(D205-K)")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 277 "LCD_GREEN")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 278 "RGB_EN")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 170 "Net-(D204-K)")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 276 "LCD_RED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 117.65 123.4375 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R511"
			(at 0.0375 -2.6 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "680"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 190 "Net-(Q504-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 188 "Net-(Q506-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 185.65 89.375 180)
		(property "Reference" "TP71"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 234 "Net-(R101-R1.1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 121.2625 47.7 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R500"
			(at -0.6875 -2.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "6.8K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 201 "Net-(Q500-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 214 "Net-(C500-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 123.725 81.725 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R509"
			(at -0.35 2.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "6.8K"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 198 "Net-(D501-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 289 "PWR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 125.325 61.525 180)
		(property "Reference" "TP53"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 205 "Net-(ZD500-K)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:Test_Point_1.3mm_Callout"
		(layer "B.Cu")
		(at 173.6 54.35 180)
		(property "Reference" "TP503"
			(at -4 0.15 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 285 "VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "A-PCENGINE:SMD_0805"
		(layer "B.Cu")
		(at 194.8 77.15)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "C509"
			(at -2.025 -2.35 180)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 240 "Net-(D500-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902439)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:SMD_1206_GT"
		(layer "B.Cu")
		(at 188.225 77.15 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "L103"
			(at -1.875 -3.65 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "?H"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 229 "Net-(J100-Pin_2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2173913043)
			(net 251 "Net-(L100-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "A-PCENGINE:Test_Point_1mm"
		(layer "B.Cu")
		(at 184.6 106.575 180)
		(property "Reference" "TP76"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Video/")
		(sheetfile "video.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 239 "VOL_IN_L")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_arc
		(start 139.0904 52.6796)
		(mid 136.2399 51.3899)
		(end 134.9502 48.5394)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.925 48.05)
		(end 134.9502 48.5394)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.4542 118.2116)
		(mid 103.60299 117.85239)
		(end 103.9622 117.7036)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.2238 99.7204)
		(end 103.7082 99.7204)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200 148.775)
		(end 104.3949 148.7678)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 105.791 145.7198)
		(end 107.1626 145.6182)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.4551 147.828)
		(end 103.4542 118.2116)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.3574 36.2204)
		(end 129.3114 36.2204)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 185.8772 45.3898)
		(end 185.8772 46.8122)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.325 47.65)
		(end 201.3204 77.597)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.3204 77.597)
		(end 199.5932 79.3242)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 107.3404 61.849)
		(mid 107.184171 62.226171)
		(end 106.807 62.3824)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 107.3404 61.849)
		(end 107.3404 48.641)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 114.681 117.3226)
		(mid 114.569408 117.592008)
		(end 114.3 117.7036)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 186.3344 47.2694)
		(mid 186.011111 47.135489)
		(end 185.8772 46.8122)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.9072 47.9806)
		(mid 170.530895 51.303295)
		(end 167.2082 52.6796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 108.3818 47.5996)
		(end 110.8964 47.5996)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.9072 47.9806)
		(end 171.9072 45.3898)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.9622 117.7036)
		(end 114.3 117.7036)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.7082 99.7204)
		(mid 103.420832 99.601368)
		(end 103.3018 99.314)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 103.3018 62.738)
		(mid 103.405953 62.486553)
		(end 103.6574 62.3824)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.3018 99.314)
		(end 103.3018 62.738)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 129.3114 36.220401)
		(mid 129.892759 36.335542)
		(end 130.374094 36.681305)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 185.2422 44.7548)
		(mid 185.691213 44.940787)
		(end 185.8772 45.3898)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.2442 147.5232)
		(end 200 148.775)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 103.6574 62.3824)
		(end 106.807 62.3824)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.5932 90.1954)
		(end 201.225 91.825)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.3949 148.7678)
		(end 103.4551 147.828)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.9248 41.7322)
		(end 134.925 48.05)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.9072 45.3898)
		(mid 172.093187 44.940787)
		(end 172.5422 44.7548)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 139.0904 52.6796)
		(end 167.2082 52.6796)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 200.944 47.269)
		(mid 201.213408 47.380592)
		(end 201.325 47.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 134.644597 40.945455)
		(mid 134.852658 41.314623)
		(end 134.9248 41.7322)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.8748 42.6212)
		(mid 114.41666 46.14146)
		(end 110.8964 47.5996)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.5422 44.7548)
		(end 185.2422 44.7548)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.8748 42.6212)
		(end 115.8748 36.703)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 186.3344 47.2694)
		(end 200.944 47.269)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.225 91.825)
		(end 201.2442 147.5232)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 130.3782 36.6776)
		(end 134.6454 40.9448)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 107.3404 48.641)
		(mid 107.645419 47.904619)
		(end 108.3818 47.5996)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.681 117.3226)
		(end 114.681 100.1776)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 198.7042 145.7198)
		(end 200.0758 145.6182)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 114.2238 99.7204)
		(mid 114.547089 99.854311)
		(end 114.681 100.1776)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 177.3682 50.6984)
		(end 178.7398 50.5968)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.8748 36.703)
		(mid 116.01615 36.36175)
		(end 116.3574 36.2204)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 199.5932 79.3242)
		(end 199.5932 90.1954)
		(layer "Edge.Cuts")
	)
	(image
		(at 152.45 90.68)
		(layer "User.1")
		(scale 4)
	)
	(image
		(at 152.4 92.075)
		(layer "User.2")
	)
	(image
		(at 152.4 92.075)
		(layer "User.3")
	)
	(image
		(at 152.679 91.4638)
		(layer "User.4")
		(scale 4)
	)
	(gr_text "COSAM       COSAM       COSAM       COSAM       COSAM       COSAM       COSAM       COSAM       COSAM"
		(at 149.95 148.575 0)
		(layer "In1.Cu")
	)
	(gr_text "CN"
		(at 174.5488 141.3002 0)
		(layer "F.SilkS")
	)
	(gr_text "USA"
		(at 150.6 58.125 0)
		(layer "F.SilkS")
	)
	(gr_text "Z"
		(at 171.8564 137.9982 0)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 165.425 86.775 0)
		(layer "F.SilkS")
	)
	(gr_text "..."
		(at 177.3682 140.9446 0)
		(layer "F.SilkS")
	)
	(gr_text "28"
		(at 170.075 68.1 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 155.525 68.125 0)
		(layer "F.SilkS")
	)
	(gr_text "1A"
		(at 180.95 54.7 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 156.5 86.8 0)
		(layer "F.SilkS")
	)
	(gr_text "707V"
		(at 174.3202 138.5316 0)
		(layer "F.SilkS")
	)
	(gr_text "JPN"
		(at 150.95 61.725 0)
		(layer "F.SilkS")
	)
	(gr_text "A"
		(at 159.825 58.125 0)
		(layer "F.SilkS")
	)
	(gr_text "2023        2023        2023        2023        2023        2023        2023        2023        2023"
		(at 154.94 148.59 0)
		(layer "In2.Cu")
	)
	(gr_text "JLCJLCJLCJLC"
		(at 137.35 147.4 0)
		(layer "B.SilkS")
	)
	(gr_text "REPRO v1.1 BY COSAM 2024"
		(at 190.4 147.425 0)
		(layer "B.SilkS")
	)
	(gr_text "BLH"
		(at 123.5 43.625 0)
		(layer "B.SilkS")
	)
	(gr_text "060"
		(at 172.225 144.45 0)
		(layer "B.SilkS")
	)
	(gr_text "7610"
		(at 180.8 144.45 0)
		(layer "B.SilkS")
	)
	(zone
		(net 287)
		(net_name "PWR2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 56)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.65 118.35) (xy 117.65 119.85) (xy 118.175 120.375) (xy 118.175 121.425) (xy 116.65 121.425)
				(xy 116.65 120.85) (xy 115.625 119.925) (xy 115.625 119.075) (xy 116.425 118.275) (xy 117.575 118.275)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 92)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.7 61.975) (xy 115.7 59.9) (xy 115.225 59.375) (xy 109.475 59.375) (xy 109.125 59.725) (xy 109.125 62.4)
				(xy 109.675 62.95) (xy 116.675 62.95)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 61)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.325 95.775) (xy 125.325 97.475) (xy 127.3 99.45) (xy 128.1 99.45) (xy 128.425 99.125) (xy 128.425 98.925)
				(xy 129 98.35) (xy 129.225 98.35) (xy 129.375 98.275) (xy 129.525 98.175) (xy 129.675 98) (xy 129.725 97.825)
				(xy 129.775 97.575) (xy 131.4 95.95) (xy 131.4 95) (xy 128.875 92.475) (xy 127.325 92.475) (xy 125.35 94.475)
			)
		)
	)
	(zone
		(net 272)
		(net_name "PWR3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 57)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120.35 118.825) (xy 118.7 118.825) (xy 118.7 116.925) (xy 119.5 116.125) (xy 123.225 116.125)
				(xy 124.075 115.275) (xy 124.325 115.275) (xy 124.325 118.1) (xy 123.5 118.1) (xy 122.675 117.275)
				(xy 121.325 117.275) (xy 120.35 118.25)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.8656 75.438) (xy 143.8656 75.819) (xy 145.0848 77.216) (xy 146.431 77.216) (xy 146.431 77.5208)
				(xy 143.637 80.3148) (xy 143.637 82.7532) (xy 142.621 83.7692) (xy 142.621 85.2424) (xy 141.986 85.8774)
				(xy 141.986 86.5378) (xy 141.605 86.0806) (xy 141.605 83.7184) (xy 140.5636 82.677) (xy 140.5636 78.74)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 91)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.525 63.95) (xy 105.025 63.45) (xy 105.6 63.45) (xy 105.8 63.675) (xy 105.8 72.775) (xy 105.05 73.525)
				(xy 105.05 76.65) (xy 105.95 77.55) (xy 105.95 78.575) (xy 105.525 79) (xy 105.525 81.075) (xy 106.5 81.075)
				(xy 106.5 87.275) (xy 105.05 87.275) (xy 104.525 86.75)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.021 67.4624) (xy 168.021 65.6082) (xy 168.9862 65.4304) (xy 169.037 65.532) (xy 169.037 67.4624)
			)
		)
	)
	(zone
		(net 270)
		(net_name "N{slash}C")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 193.85 52.05) (xy 193.85 54.55) (xy 195.75 54.55) (xy 195.75 52.05)
			)
		)
	)
	(zone
		(net 214)
		(net_name "Net-(C500-Pad2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 106)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.725 48.275) (xy 117.725 51.6) (xy 118.3 52.175) (xy 127.35 52.175) (xy 128.875 53.7) (xy 128.875 54.025)
				(xy 126.85 54.025) (xy 126 53.175) (xy 116.75 53.175) (xy 116.225 52.65) (xy 116.225 48.275)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 36)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 134.475 122.9) (xy 134.475 123.45) (xy 135.5 123.45) (xy 135.5 124.175) (xy 134.775 124.175)
				(xy 132.975 125.975) (xy 131.975 125.975) (xy 130.95 127) (xy 130.95 127.25) (xy 130.725 127.5)
				(xy 130.1 127.5) (xy 129.85 127.25) (xy 129.85 127) (xy 129.3 126.5) (xy 123.75 126.5) (xy 121.975 128.275)
				(xy 114.925 128.275) (xy 114.675 128.025) (xy 113.625 128.025) (xy 112.675 128.975) (xy 108.75 128.975)
				(xy 108.5 128.725) (xy 108.5 128.025) (xy 110.1 128.025) (xy 110.1 127) (xy 108.825 127) (xy 108.825 126)
				(xy 112.65 126) (xy 113.175 125.475) (xy 113.175 124.45) (xy 111.55 124.45) (xy 111.55 123.45) (xy 113.075 123.45)
				(xy 113.075 122) (xy 113.2 121.875) (xy 114.55 121.875) (xy 114.65 121.975) (xy 114.65 125) (xy 116.625 126.975)
				(xy 119.25 126.975) (xy 122.175 124.05) (xy 122.175 122.925) (xy 122.45 122.65) (xy 125.025 122.65)
				(xy 125.3 122.925) (xy 125.3 123.925) (xy 126.075 124.7) (xy 130.725 124.7) (xy 131.95 123.475)
				(xy 132.85 123.475) (xy 133.425 122.9)
			)
		)
	)
	(zone
		(net 286)
		(net_name "+5VL")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 65)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.075 108.75) (xy 167 107.675) (xy 167 110.55) (xy 168.075 109.475) (xy 177.15 109.475) (xy 179.4 111.725)
				(xy 181.325 111.725) (xy 180.3 110.7) (xy 179.775 110.7) (xy 179 109.925) (xy 179 107.575) (xy 180.525 106.05)
				(xy 178.925 106.05) (xy 177.05 104.175) (xy 177.05 102.225) (xy 177.55 101.725) (xy 179.05 101.725)
				(xy 178.475 101.15) (xy 176.7 101.15) (xy 176.225 101.625) (xy 176.225 108.15) (xy 175.625 108.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 43)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 193.9 146.175) (xy 195.725 146.175) (xy 195.725 146.45) (xy 193.9 146.45)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 71)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 200.425 114.925) (xy 198.95 114.925) (xy 198.95 113.175) (xy 198.425 112.65) (xy 196.35 112.65)
				(xy 195.45 111.675) (xy 194.875 111.675) (xy 194.425 111.225) (xy 194.425 109.15) (xy 195.4 108.175)
				(xy 196.15 108.175) (xy 196.15 108.725) (xy 197.925 108.725) (xy 197.925 109.725) (xy 197.075 109.725)
				(xy 197.075 109.975) (xy 197.55 110.525) (xy 199.2 110.525) (xy 199.775 109.95) (xy 199.775 109.725)
				(xy 198.55 109.725) (xy 198.55 108.725) (xy 199.775 108.725) (xy 199.775 108.475) (xy 199.225 107.925)
				(xy 200.425 107.925)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 70)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 195.775 122.7) (xy 197.075 122.7) (xy 197.075 122.425) (xy 197.625 121.875) (xy 199.2 121.875)
				(xy 199.725 122.475) (xy 199.725 122.7) (xy 200.425 122.7) (xy 200.425 114.925) (xy 198.95 114.925)
				(xy 198.95 115.05) (xy 197.85 116.025) (xy 197.85 116.55) (xy 199.15 116.55) (xy 199.15 117.15)
				(xy 198.475 117.825) (xy 197.075 117.825) (xy 196.925 117.975) (xy 196.925 121.55)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 74)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198.35 99.775) (xy 198.35 101.725) (xy 195.4 101.725) (xy 193.825 100.125) (xy 193.825 96.425)
				(xy 195.325 96.425) (xy 196.05 97.15) (xy 197.475 97.15) (xy 197.65 97.3) (xy 197.65 98.1) (xy 196.95 98.1)
				(xy 196.95 98.875) (xy 197.9 98.875) (xy 197.9 99.775)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 109)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.6662 76.3778) (xy 149.1996 75.8444) (xy 149.6822 75.8444) (xy 149.6822 75.4634) (xy 148.7678 75.4634)
				(xy 148.3868 75.8444) (xy 148.3868 76.3778)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.5702 69.4944) (xy 143.8402 70.7644) (xy 143.8402 68.5546) (xy 142.5702 67.2846)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 78)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 155.25 118.875) (xy 155.775 118.35) (xy 155.775 116.8) (xy 156.275 116.3) (xy 156.275 109.575)
				(xy 152.8 109.575) (xy 152.8 110.2) (xy 153.225 110.625) (xy 153.225 110.8) (xy 153.3 110.95) (xy 153.425 111.1)
				(xy 153.6 111.2) (xy 153.8 111.225) (xy 153.85 111.225) (xy 155.2 112.575) (xy 155.2 118.875)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 35)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130.9 128) (xy 130.9 129.575) (xy 132.5 127.975) (xy 135.425 127.975) (xy 136.95 129.5) (xy 140.3 129.5)
				(xy 142.3 127.5) (xy 143.875 127.5) (xy 145.425 129.05) (xy 145.425 130.775) (xy 147.625 132.975)
				(xy 148.075 132.975) (xy 148.075 130.875) (xy 146.9 129.7) (xy 146.9 127.8) (xy 145.875 126.775)
				(xy 142.1 126.775) (xy 140.85 128.025) (xy 140.1 128.025) (xy 139.5 127.425) (xy 139.5 126.475)
				(xy 140.525 125.45) (xy 140.525 124.725) (xy 135.225 124.725) (xy 133.475 126.475) (xy 132.425 126.475)
				(xy 131.025 127.875)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.1)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.7122 99.1108) (xy 135.7122 102.1588) (xy 135.255 102.616) (xy 135.001 102.616) (xy 134.0104 101.6254)
				(xy 133.3754 101.6254) (xy 133.3754 101.2698) (xy 135.5344 99.1108)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 99)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.1 50.8) (xy 177.375 53.425) (xy 172.825 53.425) (xy 172.525 53.725) (xy 169.05 53.725) (xy 169.05 55.275)
				(xy 171.025 55.275) (xy 171.275 55.5) (xy 171.275 56.35) (xy 183.525 56.35) (xy 183.525 55.65) (xy 184.025 55.15)
				(xy 184.775 55.175) (xy 184.775 51.575) (xy 184.025 51.575) (xy 183.575 51.125) (xy 183.575 50.8)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.1)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 180.6702 128.5748) (xy 180.6702 127.7874) (xy 181.4322 127.0254) (xy 183.769 127.0254) (xy 184.2008 127.4572)
				(xy 184.2008 131.1402) (xy 183.1594 132.1816) (xy 183.1594 133.0198) (xy 182.6768 133.5024) (xy 181.1782 133.5024)
				(xy 180.6702 132.9944) (xy 180.6702 131.4704) (xy 180.1622 130.9624) (xy 180.1622 129.0828)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 80)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.55 103.3) (xy 160.025 103.3) (xy 161.525 104.6) (xy 160.9 104.6) (xy 160.475 105.025) (xy 158.55 105.025)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.1 143.175) (xy 114.775 141.85) (xy 111.525 141.85) (xy 108.9 139.225) (xy 108.9 138.825)
				(xy 107.025 138.825) (xy 107.025 138.125) (xy 108.175 138.125) (xy 108.175 137.75) (xy 107.05 136.625)
				(xy 107.05 135.6) (xy 107.575 135.075) (xy 109.05 135.075) (xy 110.575 133.55) (xy 113.625 133.55)
				(xy 115.025 132.15) (xy 115.025 131.825) (xy 108.45 131.825) (xy 108.45 133.025) (xy 104.475 133.025)
				(xy 104.475 142.675) (xy 104.975 143.175)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.161 67.3608) (xy 145.161 67.564) (xy 145.669 68.072) (xy 145.669 72.0598) (xy 146.177 72.5678)
				(xy 146.177 74.0918) (xy 145.7198 74.4982) (xy 145.7198 74.676) (xy 146.6596 74.676) (xy 148.717 72.6186)
				(xy 148.717 68.8594) (xy 147.2184 67.3608)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 98)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.375 48.2) (xy 196.375 49) (xy 196.025 49) (xy 195.55 49.475) (xy 195.55 49.9) (xy 186 49.9)
				(xy 186 49.3) (xy 185.5 48.925) (xy 185.275 48.925) (xy 185.275 50.225) (xy 184.3 50.225) (xy 184.3 48.95)
				(xy 184.075 48.95) (xy 183.525 49.5) (xy 183.525 49.875) (xy 184.175 49.875) (xy 184.175 50.8) (xy 180.1 50.8)
				(xy 180.125 47.3) (xy 181.25 46.175) (xy 184.5 46.175) (xy 185.2 46.875) (xy 185.2 48.225)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 86)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.9 70.575) (xy 125.35 70.575) (xy 125.875 70.05) (xy 125.875 65.225) (xy 125.35 65.225) (xy 125.35 61.475)
				(xy 125.85 60.975) (xy 128.5 60.975) (xy 129.45 60.025) (xy 131.175 60.025) (xy 131.175 61.025)
				(xy 130.125 61.025) (xy 130.125 61.325) (xy 130.775 61.9) (xy 131.45 61.9) (xy 131.45 67.55) (xy 130.875 67.55)
				(xy 129.9 68.525)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 101)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.125 55.3) (xy 144.65 55.3) (xy 144.65 53.725) (xy 138.7 53.725) (xy 138.225 53.65) (xy 137.8 53.475)
				(xy 137.45 53.325) (xy 137.125 53.15) (xy 136.5 52.7) (xy 136.125 52.375) (xy 135.75 51.975) (xy 135.425 51.575)
				(xy 135.15 51.15) (xy 134.875 50.625) (xy 134.625 50.025) (xy 134.5 49.55) (xy 134.4 49.025) (xy 134.325 48.375)
				(xy 134.325 45.85) (xy 131 45.85) (xy 131 47.1) (xy 129.9 47.1) (xy 129.9 47.75) (xy 131 47.75)
				(xy 131 48.1) (xy 133.2 48.1) (xy 133.2 53.2) (xy 134.025 53.2) (xy 135.05 54.225) (xy 136.475 54.225)
				(xy 137.55 55.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 60)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.3 104.425) (xy 123 104.425) (xy 123 103.625) (xy 120.275 103.625) (xy 120.275 90.375) (xy 121.3 89.35)
				(xy 124.275 89.35) (xy 124.75 89.825) (xy 124.75 90.45) (xy 122.25 92.95) (xy 122.25 98.95) (xy 123.3 100)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 93)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.45 67.55) (xy 131.975 67.025) (xy 131.975 65.55) (xy 132.5 65.025) (xy 133.975 65.025) (xy 134.475 64.525)
				(xy 134.475 64.05) (xy 134.825 63.7) (xy 141.2 63.7) (xy 139.425 61.925) (xy 138.875 61.925) (xy 138.875 62.5)
				(xy 137.525 62.5) (xy 137.525 60.7) (xy 136.775 59.95) (xy 133.975 59.95) (xy 131.7 57.65) (xy 131.375 57.65)
				(xy 131.375 58.1) (xy 129.45 60.025) (xy 130.125 60.025) (xy 130.125 59.85) (xy 130.75 59.225) (xy 132.175 59.225)
				(xy 132.775 59.825) (xy 132.775 61.325) (xy 132.2 61.9) (xy 131.45 61.9)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 87)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.1 80.1) (xy 170.1 84.525) (xy 170.1 86.3) (xy 174.05 86.3) (xy 176.65 83.7) (xy 178.175 83.7)
				(xy 180.175 81.7) (xy 181.225 81.7) (xy 183.225 83.7) (xy 185.75 83.7) (xy 186.475 82.975) (xy 186.475 81.825)
				(xy 186.85 81.4) (xy 186.85 78.525) (xy 186.55 78.525) (xy 186.55 79.9) (xy 186.25 80.25) (xy 186.25 81.525)
				(xy 185.575 82.2) (xy 184.7 82.2) (xy 182.8 80.3) (xy 175.95 80.3) (xy 175.625 80.625) (xy 175.625 81.675)
				(xy 175.125 82.175) (xy 173.025 82.175) (xy 172.475 81.625) (xy 172.475 80.1)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193.7512 141.5542) (xy 193.7512 142.621) (xy 193.1162 143.256) (xy 193.1162 141.5542)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.85 52.075) (xy 189.85 54.575) (xy 191.75 54.575) (xy 191.75 52.075)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 90)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 197.025 78.25) (xy 198.325 76.95) (xy 198.325 76.375) (xy 198.7 76) (xy 198.7 75.9) (xy 198.525 75.725)
				(xy 194.3 75.725) (xy 193.1 74.525) (xy 190.15 74.525) (xy 189.175 73.55) (xy 187.275 73.55) (xy 187.275 75.65)
				(xy 184.825 75.65) (xy 184.825 76.175) (xy 186.3 77.65) (xy 186.3 78.275) (xy 186.55 78.525) (xy 186.85 78.525)
				(xy 186.85 79.1) (xy 187.425 78.525) (xy 188.7 78.525) (xy 189.325 79.25) (xy 189.325 78.25)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.9954 88.0618) (xy 140.5128 87.5792) (xy 140.5128 86.9696) (xy 139.9794 86.4362) (xy 139.9794 84.4804)
				(xy 139.0904 83.5914) (xy 139.0904 77.8764) (xy 143.129 73.8632) (xy 143.129 75.1586) (xy 140.081 78.2066)
				(xy 140.081 82.7532) (xy 141.0716 83.7438) (xy 141.0716 88.0618)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 59)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.8 108.525) (xy 121.8 105.9) (xy 120.475 104.575) (xy 120.475 104.425) (xy 123.3 104.425)
				(xy 123.3 108.525)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 100)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.05 53.725) (xy 169.05 55.275) (xy 166 55.275) (xy 165.45 55.825) (xy 165.45 57.925) (xy 162.925 60.45)
				(xy 146.175 60.45) (xy 145.7 59.975) (xy 142.225 59.975) (xy 141.625 59.325) (xy 141.625 55.3) (xy 143.125 55.3)
				(xy 143.125 58.425) (xy 144.65 58.425) (xy 144.65 53.725)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.1)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.6662 101.6) (xy 148.1328 101.6) (xy 146.177 103.5558) (xy 146.177 108.1532) (xy 147.193 109.1692)
				(xy 147.193 117.3734) (xy 145.1864 119.38) (xy 136.0678 119.38) (xy 135.4836 118.7958) (xy 135.4836 112.6998)
				(xy 134.9756 112.141) (xy 134.9756 111.0234) (xy 134.7978 110.8202) (xy 134.2136 110.8202) (xy 134.1628 110.8964)
				(xy 134.1628 120.3706) (xy 133.4262 121.1072) (xy 133.425 122.9) (xy 134.475 122.9) (xy 134.475 122.5)
				(xy 135.6868 122.5042) (xy 135.6868 121.1326) (xy 135.9154 120.904) (xy 147.1676 120.904) (xy 147.6756 120.396)
				(xy 147.6756 118.0338) (xy 148.717 116.9924)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.891 73.3552) (xy 144.8816 74.3458) (xy 144.653 74.3458) (xy 143.891 75.1078)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 104)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131 48.1) (xy 133.2 48.1) (xy 133.2 52.025) (xy 132.8 52.025) (xy 132.8 51.325) (xy 132.275 50.8)
				(xy 131.95 50.8) (xy 131.95 51.925) (xy 130.95 51.925) (xy 130.95 50.8) (xy 130.725 50.8) (xy 130.15 51.375)
				(xy 130.15 52.825) (xy 130.725 53.4) (xy 132.3 53.4) (xy 132.8 52.9) (xy 132.8 52.4) (xy 133.2 52.4)
				(xy 133.2 53.2) (xy 133 53.2) (xy 131.2 55) (xy 127.7 51.525) (xy 127.7 51.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 79)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 152.8 109.575) (xy 152.8 103.8) (xy 153.775 102.825) (xy 156.775 102.825) (xy 156.775 105.125)
				(xy 158.3 105.125) (xy 158.3 106.125) (xy 156.275 108.15) (xy 156.275 109.575)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 95)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.85 73.575) (xy 175.55 73.575) (xy 175.55 72.6) (xy 176.525 72.6) (xy 176.525 71.825) (xy 175.6 70.9)
				(xy 175.6 67.625) (xy 176.175 67.05) (xy 177.675 67.05) (xy 179.125 68.5) (xy 180.175 68.5) (xy 180.725 69.05)
				(xy 180.725 68.1) (xy 180.175 67.55) (xy 180.175 66.6) (xy 180.725 66.05) (xy 183.225 66.05) (xy 183.825 65.45)
				(xy 183.825 64.125) (xy 183.725 64.025) (xy 183.5 64.025) (xy 183 64.375) (xy 181.45 64.375) (xy 180.375 63.3)
				(xy 180.375 61.65) (xy 181.4 60.625) (xy 183.05 60.625) (xy 183.55 60.95) (xy 183.75 60.95) (xy 183.875 60.825)
				(xy 183.875 59.275) (xy 184.8 58.35) (xy 184.8 56.45) (xy 183.95 56.45) (xy 183.95 57.075) (xy 183.85 57.325)
				(xy 183.7 57.325) (xy 183.525 57.075) (xy 183.525 56.35) (xy 176.15 56.35) (xy 176.15 60.975) (xy 169.1 60.975)
				(xy 171.85 63.725)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 34)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.225 132.475) (xy 124.8 134.05) (xy 130.3 134.05) (xy 130.9 133.45) (xy 130.9 128) (xy 129.9 128)
				(xy 128.95 127.05) (xy 128.125 127.05) (xy 127.95 127.225) (xy 126.3 127.225) (xy 126.3 128.275)
				(xy 128.275 128.275) (xy 128.3 129.175) (xy 127 130.475) (xy 125.95 130.475) (xy 126.725 129.35)
				(xy 125.475 129.35)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 73)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 199.425 98.35) (xy 199.425 98.6) (xy 199.6 98.775) (xy 199.6 101.725) (xy 198.35 101.725) (xy 198.35 99.775)
				(xy 198.825 99.775) (xy 199.025 99.575) (xy 199.025 99.525) (xy 198.175 98.675) (xy 198.45 98.35)
			)
		)
	)
	(zone
		(net 286)
		(net_name "+5VL")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 63)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 179.125 116.4) (xy 178.725 116.4) (xy 176.575 118.55) (xy 178.85 118.55) (xy 179.125 118.275)
			)
		)
	)
	(zone
		(net 287)
		(net_name "PWR2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.475 87.85) (xy 124.65 86.3) (xy 125.275 86.3) (xy 125.275 88.075) (xy 123.475 88.075)
			)
		)
	)
	(zone
		(net 193)
		(net_name "Net-(SW500-A)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 185.85 52.075) (xy 185.85 54.575) (xy 187.75 54.575) (xy 187.75 52.075)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 94)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.1 80.1) (xy 172.475 80.1) (xy 172.475 78.2) (xy 175.975 74.675) (xy 177.175 74.675) (xy 178.675 76.175)
				(xy 184.825 76.175) (xy 184.825 75.65) (xy 185.775 75.65) (xy 185.775 73.125) (xy 183.225 73.125)
				(xy 183.225 71.6) (xy 184.75 71.6) (xy 183.725 70.575) (xy 183.725 68.55) (xy 183.2 68.1) (xy 180.725 68.1)
				(xy 180.725 70.075) (xy 179.1 71.7) (xy 178.625 71.7) (xy 178.625 73.575) (xy 171.85 73.575) (xy 172.6 74.325)
				(xy 172.6 75.9) (xy 170.1 78.4)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 64)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 175.475 118.175) (xy 175.475 115.5) (xy 176.7 114.275) (xy 176.7 113.125) (xy 176.175 112.6)
				(xy 174.975 112.6) (xy 174.525 113.05) (xy 166.825 113.05) (xy 166.2 112.425) (xy 167.375 112.425)
				(xy 168.05 111.75) (xy 168.05 110.725) (xy 168.55 110.225) (xy 176.475 110.225) (xy 178.475 112.425)
				(xy 180.975 112.425) (xy 180.975 112.8) (xy 180.65 113.125) (xy 180.65 113.375) (xy 180.325 113.7)
				(xy 179.6 113.7) (xy 179.075 113.175) (xy 177.975 113.175) (xy 177.5 113.65) (xy 177.5 116.15)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 69)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 200.425 131.875) (xy 198.825 131.875) (xy 198.825 130.9) (xy 199.75 130.9) (xy 199.75 130.625)
				(xy 199.2 130.075) (xy 197.625 130.075) (xy 197 130.8) (xy 196.775 130.8) (xy 194.425 128.45) (xy 194.1 128.45)
				(xy 193.825 128.175) (xy 193.825 125.85) (xy 195.4 124.275) (xy 195.4 123.075) (xy 195.775 122.7)
				(xy 197.725 122.7) (xy 197.725 123.675) (xy 197.075 123.675) (xy 197.075 123.9) (xy 197.55 124.45)
				(xy 199.175 124.45) (xy 199.725 123.9) (xy 199.725 123.675) (xy 198.725 123.675) (xy 198.725 122.7)
				(xy 200.425 122.7)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.1)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.749 119.888) (xy 150.749 121.2088) (xy 150.876 121.6152) (xy 151.6634 121.6152) (xy 151.765 121.158)
				(xy 151.765 119.888)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.275 137.1) (xy 127.85 142.675) (xy 127.85 143.925) (xy 128.175 144.25) (xy 141.575 144.25)
				(xy 145.125 140.7) (xy 145.125 139.65) (xy 145.825 138.95) (xy 145.825 138.775) (xy 142.9 138.775)
				(xy 141.975 139.7) (xy 137.45 139.7) (xy 137 140.15) (xy 126.75 140.15) (xy 123.7 137.1)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 43)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 193.9 143.45) (xy 195.725 143.45) (xy 195.725 143.725) (xy 193.9 143.725)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 72)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 195.4 108.175) (xy 196.15 108.175) (xy 196.15 108.725) (xy 197.05 108.725) (xy 197.05 108.525)
				(xy 197.675 107.9) (xy 199.2 107.9) (xy 199.225 107.925) (xy 200.425 107.925) (xy 200.425 97.3)
				(xy 199.925 96.8) (xy 199.325 96.8) (xy 199.2 96.925) (xy 199.2 97.225) (xy 198.35 98.075) (xy 198.625 98.35)
				(xy 199.425 98.35) (xy 199.75 98.025) (xy 199.8 98.025) (xy 199.9 98.125) (xy 199.9 98.675) (xy 199.8 98.775)
				(xy 199.6 98.775) (xy 199.6 101.725) (xy 195.4 101.725)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 82)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.725 91.775) (xy 148.725 90.35) (xy 149.175 89.9) (xy 151.225 89.9) (xy 153.275 87.85) (xy 158 87.85)
				(xy 158 89.9) (xy 159.15 89.9) (xy 159.15 90.425) (xy 158 90.425) (xy 158 91.775)
			)
		)
	)
	(zone
		(net 216)
		(net_name "BLH")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 107)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.425 55.3) (xy 117.425 59.175) (xy 117.05 59.175) (xy 113.575 55.7) (xy 109.45 55.7) (xy 109.125 55.375)
				(xy 109.125 52.45) (xy 109.4 52.175) (xy 113.225 52.175) (xy 116.35 55.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 67)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.275 101.15) (xy 185.075 101.15) (xy 185.425 101.5) (xy 185.425 106) (xy 186.575 107.15)
				(xy 188.225 107.15) (xy 189.325 106.05) (xy 189.325 103.55) (xy 190.3 102.575) (xy 191.35 102.575)
				(xy 191.85 103.075) (xy 191.85 104.45) (xy 191.25 105.05) (xy 190.85 105.025) (xy 190.775 105.125)
				(xy 190.775 107.8) (xy 190.45 108.125) (xy 190.3 108.125) (xy 189.825 108.6) (xy 186.85 108.6) (xy 184.525 106.25)
				(xy 184.525 101.725) (xy 184.275 101.475)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 96)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.1 60.975) (xy 169.1 59.9) (xy 171.275 57.725) (xy 171.275 56.35) (xy 172.225 56.35) (xy 172.225 57.375)
				(xy 173.1 57.375) (xy 173.1 56.35) (xy 176.15 56.35) (xy 176.15 60.975)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 102)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131 45.85) (xy 134.325 45.85) (xy 134.325 41.625) (xy 129.775 37.075) (xy 117.675 37.075) (xy 116.925 37.825)
				(xy 116.925 39.125) (xy 117.8 40) (xy 118.95 40) (xy 119.325 40.375) (xy 121.275 40.375) (xy 121.275 39.65)
				(xy 120.625 39.65) (xy 120.625 38.95) (xy 122.3 38.95) (xy 122.3 39.95) (xy 121.95 39.95) (xy 121.95 40.375)
				(xy 123 40.375) (xy 123.375 40) (xy 129.975 40) (xy 131 41.05)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 76)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 172.05 103.525) (xy 174 101.575) (xy 175.1 101.575) (xy 175.575 102.05) (xy 175.575 107.625)
				(xy 175.1 108.1) (xy 168.575 108.1) (xy 168.075 107.6) (xy 168.075 102.525) (xy 168.55 102.05) (xy 170.975 102.05)
				(xy 170.975 104.65) (xy 169.975 105.525) (xy 169.975 106.525) (xy 170.475 107.1) (xy 171.475 107.1)
				(xy 172.05 106.525)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 68)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 197.925 131.975) (xy 197.925 132.725) (xy 197.5 132.725) (xy 197.425 132.8) (xy 197.425 134.475)
				(xy 197.925 134.975) (xy 199.875 134.975) (xy 200.425 134.425) (xy 200.425 131.875) (xy 199.75 131.875)
				(xy 199.75 132.125) (xy 199.15 132.725) (xy 198.8 132.725) (xy 198.8 131.975)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 85)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.825 70.575) (xy 123.3 70.05) (xy 123.3 67.65) (xy 122 67.65) (xy 120.6 69.05) (xy 120.6 69.525)
				(xy 122.05 70.775) (xy 122.05 76.45) (xy 122.75 76.45) (xy 123.825 77.525) (xy 123.825 73.125) (xy 124.4 72.55)
				(xy 125.975 72.55) (xy 127.4 73.975) (xy 127.4 77.8) (xy 127.475 77.875) (xy 127.65 77.875) (xy 129.9 75.625)
				(xy 129.9 70.575)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 39)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.4 138.525) (xy 131.4 138.525) (xy 135.45 134.475) (xy 136.525 134.475) (xy 137.575 135.525)
				(xy 137.575 137.675) (xy 136.05 139.2) (xy 127.725 139.2) (xy 124.7 136.175) (xy 119.8 136.175)
				(xy 119.3 136.675) (xy 119.1 136.475) (xy 119.65 135.925) (xy 124.8 135.925)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 58)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.8 119.525) (xy 121.8 121.35) (xy 122.375 121.925) (xy 126.85 121.925) (xy 127.375 122.45)
				(xy 127.375 123) (xy 130.4 123) (xy 130.4 111.675) (xy 129.85 111.125) (xy 125.875 111.1) (xy 123.3 108.525)
				(xy 121.8 108.525) (xy 121.8 110.625) (xy 123.4 112.225) (xy 127.1 112.225) (xy 127.875 113) (xy 127.875 119.325)
				(xy 126.8 120.4) (xy 123.175 120.4) (xy 122.4 119.525)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 77)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.975 102.05) (xy 170.975 99.55) (xy 172.625 97.9) (xy 167.3 97.9) (xy 166.45 97.05) (xy 162.925 97.05)
				(xy 162.925 97.6) (xy 163.325 98) (xy 165.425 98) (xy 166.45 99.025) (xy 169.05 99.025) (xy 170.55 100.525)
				(xy 170.55 101.5) (xy 170 102.05)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 66)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 181.45 101.375) (xy 180.85 100.775) (xy 180.85 98.2) (xy 180.475 97.825) (xy 173.55 97.825)
				(xy 173.55 98.15) (xy 173.75 98.15) (xy 174.1 98.5) (xy 174.1 99.025) (xy 174.6 99.525) (xy 178.625 99.525)
				(xy 180.475 101.375)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 37)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.65 139.675) (xy 147.875 138.9) (xy 151.525 138.9) (xy 152.225 138.2) (xy 153.1 139.075)
				(xy 153.375 139.075) (xy 153.725 139.425) (xy 153.725 142.075) (xy 152.725 142.075) (xy 152.725 143.45)
				(xy 154.05 143.45) (xy 154.05 143.725) (xy 152.725 143.725) (xy 152.725 146.175) (xy 153.9 146.175)
				(xy 153.9 146.45) (xy 152.725 146.45) (xy 152.725 147.3) (xy 152.15 147.875) (xy 109.575 147.875)
				(xy 109.075 147.375) (xy 109.075 144.75) (xy 107.525 143.175) (xy 119.95 143.175) (xy 120.225 142.9)
				(xy 120.35 142.9) (xy 120.35 143.625) (xy 119.65 144.225) (xy 111.575 144.25) (xy 111.1 144.725)
				(xy 111.1 145.775) (xy 111.575 146.25) (xy 143.125 146.25) (xy 145.675 143.7) (xy 149.7 143.7) (xy 152.675 140.725)
				(xy 152.675 139.875) (xy 152.475 139.675)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 97)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.8 56.35) (xy 196.8 57.275) (xy 199.975 57.275) (xy 200.425 56.825) (xy 200.425 48.575) (xy 200 48.2)
				(xy 196.375 48.2) (xy 196.375 50.4) (xy 197.3 50.4) (xy 197.3 49) (xy 197.65 49) (xy 198.175 49.525)
				(xy 198.175 49.825) (xy 197.35 49.825) (xy 197.35 50.825) (xy 198.15 50.825) (xy 198.15 51.1) (xy 197.6 51.65)
				(xy 196.825 51.65) (xy 196.825 55.1) (xy 197.75 55.1) (xy 198.325 55.675) (xy 198.325 56.35)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 42)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.475 133.025) (xy 104.475 118.8) (xy 104.8 118.475) (xy 112.3 118.475) (xy 112.625 118.8)
				(xy 112.625 121.825) (xy 112.05 122.4) (xy 109.125 122.4) (xy 108.55 122.975) (xy 108.55 123.475)
				(xy 109.45 123.475) (xy 109.45 124.425) (xy 108.125 124.425) (xy 107.025 125.525) (xy 107.025 129.5)
				(xy 108.425 130.9) (xy 108.425 131.5) (xy 106.525 131.5) (xy 106.525 133.025)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 83)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.35 97.05) (xy 166.45 97.05) (xy 166.45 94.55) (xy 167.05 93.95) (xy 171.425 93.95) (xy 173.525 91.85)
				(xy 173.525 88.525) (xy 174.05 88.075) (xy 174.05 86.3) (xy 170.1 86.3) (xy 170.1 84.525) (xy 169.35 85.275)
				(xy 168.25 85.275) (xy 168.025 85.5) (xy 168.025 86.85) (xy 167.45 87.35) (xy 165.45 87.35) (xy 161.95 90.875)
				(xy 161.95 91.875) (xy 161.275 92.55) (xy 164.35 92.55)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 81)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 153.775 102.825) (xy 156.775 102.825) (xy 156.775 104.05) (xy 158.125 104.05) (xy 158.125 103.225)
				(xy 156.825 101.925) (xy 156.825 98) (xy 157.825 97) (xy 160.375 97) (xy 160.85 96.525) (xy 160.85 95.05)
				(xy 161.4 94.5) (xy 162.4 94.5) (xy 162.95 95.05) (xy 162.925 97.05) (xy 164.35 97.05) (xy 164.35 92.55)
				(xy 159.925 92.55) (xy 159.05 91.675) (xy 158.8 91.675) (xy 158.8 92.45) (xy 158 92.45) (xy 158 91.775)
				(xy 155.5 91.775) (xy 155.5 94.175) (xy 153.075 94.175) (xy 153.075 91.775) (xy 148.725 91.775)
				(xy 148.725 93.475) (xy 151.8 96.55) (xy 151.8 98.075) (xy 153.775 100.05)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 89)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 194.2 89.65) (xy 194.2 79.65) (xy 191.6 79.65) (xy 191.6 78.25) (xy 197.025 78.25) (xy 196.175 79.1)
				(xy 196.175 83.7) (xy 194.85 85.05) (xy 194.85 89.65)
			)
		)
	)
	(zone
		(net 288)
		(net_name "PWR4")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 38)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.15 139.525) (xy 123.95 139.525) (xy 127.375 142.95) (xy 127.375 144.275) (xy 127.85 144.75)
				(xy 142.35 144.75) (xy 146.25 140.825) (xy 146.25 142.15) (xy 142.75 145.65) (xy 127.6 145.65) (xy 126.65 144.7)
				(xy 126.65 143.375) (xy 123.5 140.225) (xy 122.15 140.225)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 84)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.45 93.925) (xy 181.45 94.925) (xy 182.45 94.925) (xy 184.175 93.2) (xy 184.175 89.875) (xy 182.7 88.4)
				(xy 181.2 88.4) (xy 180.45 89.15)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.828 110.0328) (xy 147.828 110.2614) (xy 145.1102 110.2614) (xy 144.5514 109.7026) (xy 144.5514 101.0158)
				(xy 145.1356 100.4316) (xy 147.7264 100.4316) (xy 147.7264 100.6856) (xy 145.2118 100.6856) (xy 144.78 101.1174)
				(xy 144.78 109.601) (xy 145.2118 110.0328)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123 80.8) (xy 122.675 81.125) (xy 112 81.125) (xy 111.65 81.475) (xy 111.65 85.75) (xy 112.15 86.25)
				(xy 115.15 86.25) (xy 118.65 82.725) (xy 119.825 82.725) (xy 120.75 83.65) (xy 120.75 84.9) (xy 121.475 85.7)
				(xy 123.225 85.7) (xy 123.225 80.8)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 88)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193.825 96.425) (xy 192.375 94.975) (xy 192.375 93.975) (xy 189.325 90.95) (xy 189.325 78.25)
				(xy 191.6 78.25) (xy 191.6 89.65) (xy 194.85 89.65) (xy 194.85 96.425)
			)
		)
	)
	(zone
		(net 214)
		(net_name "Net-(C500-Pad2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 105)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.275 44.6) (xy 120 44.6) (xy 120.325 44.925) (xy 120.325 45.575) (xy 119.85 46.05) (xy 118.75 46.05)
				(xy 117.725 47.075) (xy 117.725 48.275) (xy 116.225 48.275) (xy 116.225 46.65)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 75)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193.825 100.125) (xy 190.2 96.5) (xy 190.2 94.5) (xy 188.025 92.325) (xy 186.1 92.325) (xy 185.65 91.875)
				(xy 185.65 88.4) (xy 184.175 86.925) (xy 181.2 86.925) (xy 181.125 86.85) (xy 181.125 86.8) (xy 181.2 86.725)
				(xy 184.25 86.725) (xy 185.85 88.325) (xy 185.85 91.8) (xy 186.175 92.125) (xy 188.125 92.125) (xy 190.425 94.425)
				(xy 190.425 96.425) (xy 193.825 99.825)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 103)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.25 50.925) (xy 124.25 49.125) (xy 120.8 49.125) (xy 120.8 50.925)
			)
		)
	)
	(zone
		(net 287)
		(net_name "PWR2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 149)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.95 143.05) (xy 121.975 144.025) (xy 123.15 144.025) (xy 123.15 143.05)
			)
		)
	)
	(zone
		(net 230)
		(net_name "Net-(J100-Pin_3)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 110)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 194.375 88.724417) (xy 194.575 88.849417) (xy 194.75 89.049417) (xy 194.825 89.274417) (xy 194.85 89.474417)
				(xy 194.85 89.774417) (xy 194.8 90.049417) (xy 194.725 90.249417) (xy 194.575 90.449417) (xy 194.4 90.574417)
				(xy 194.15 90.649417) (xy 191.699988 90.650583) (xy 191.449988 90.575583) (xy 191.249988 90.450583)
				(xy 191.074988 90.250583) (xy 190.999988 90.025583) (xy 190.974988 89.825583) (xy 190.974988 89.525583)
				(xy 191.024988 89.250583) (xy 191.099988 89.050583) (xy 191.249988 88.850583) (xy 191.424988 88.725583)
				(xy 191.674988 88.650583) (xy 194.125 88.649417)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 156.6 66.425) (xy 156.6 67.6) (xy 157.6 67.6) (xy 157.6 66.425)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130.775 136.575) (xy 129.225 138.125) (xy 127.025 138.125) (xy 127.025 138.35) (xy 128.775 140.1)
				(xy 130.775 140.1) (xy 130.775 138.6) (xy 131.8 138.6) (xy 131.8 140.1) (xy 132.325 140.1) (xy 132.775 140.55)
				(xy 132.775 140.875) (xy 133.05 141.15) (xy 133.8 141.15) (xy 135.3 139.65) (xy 135.3 136.95) (xy 134.925 136.575)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 25)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 199.775 130.475) (xy 197.9 130.475) (xy 193.75 134.625) (xy 193.75 138.525) (xy 197.3 134.975)
				(xy 199.8 134.975) (xy 200.3 134.475) (xy 200.3 131)
			)
		)
	)
	(zone
		(net 282)
		(net_name "BATT-")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 119)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.325 70.725) (xy 195.825 70.725) (xy 195.825 67.925) (xy 195 67.925) (xy 194.15 68.775) (xy 195.325 68.775)
			)
		)
	)
	(zone
		(net 273)
		(net_name "LCD_BRIGHT")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 136.1186 141.478) (xy 135.3566 142.24) (xy 136.8806 142.24)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198.15 49.85) (xy 197.05 49.85) (xy 197.05 48.875) (xy 197.425 48.875) (xy 198.15 49.5)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 128)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.175 72.675) (xy 155.725 71.125) (xy 155.725 69.175) (xy 150.675 69.175) (xy 148.025 71.825)
				(xy 148.025 72.075) (xy 148.75 72.675)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 137)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.375 55.6) (xy 196.375 51.7) (xy 195.375 50.7) (xy 191.375 50.7) (xy 189 48.325) (xy 189 48.15)
				(xy 189.125 48.025) (xy 199.725 48.025) (xy 200.675 48.975) (xy 200.675 56.6) (xy 200 57.275) (xy 196.825 57.275)
				(xy 196.4 56.85)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 198.152558 50.802967) (xy 197.052558 50.802967) (xy 197.052558 51.777967) (xy 197.427558 51.777967)
				(xy 198.152558 51.152967)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 114)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.5 82.25) (xy 141.95 82.25) (xy 142.525 81.675) (xy 142.525 80.7) (xy 143.05 80.175) (xy 143.05 78.75)
				(xy 144.375 78.75) (xy 144.375 80.05) (xy 144.725 80.05) (xy 145.075 79.7) (xy 145.075 77.275) (xy 143.525 75.725)
				(xy 139.025 75.725) (xy 137.475 74.175)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 30)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 182.075 122.975) (xy 182.1 116.725) (xy 179.575 114.2) (xy 179.575 112.725) (xy 180.6 112.725)
				(xy 184.125 116.25) (xy 198.325 116.25) (xy 198.325 118.55) (xy 197.325 118.55) (xy 197.325 118.275)
				(xy 195.775 118.275) (xy 195.775 119.275) (xy 195.25 119.275) (xy 194.75 119.775) (xy 194.775 128.075)
				(xy 194.375 128.475) (xy 194.15 128.475) (xy 190.975 131.65) (xy 190.775 131.65) (xy 190.75 118.275)
				(xy 189.7 117.225) (xy 188.725 117.225) (xy 188.125 117.775) (xy 187.675 117.775) (xy 187.675 117.025)
				(xy 187.15 117.025) (xy 187.15 117.775) (xy 185.65 117.775) (xy 185.65 117.075) (xy 184.625 117.075)
				(xy 184.625 121.525) (xy 182.575 123.575) (xy 182.575 122.975)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 28)
		(connect_pads no
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 147.45 121.45) (xy 147.15 121.75) (xy 147.15 122.475) (xy 149.1 124.425) (xy 153.625 124.425)
				(xy 158.225 119.825) (xy 161.975 119.825) (xy 161.975 119.025) (xy 161.825 118.875) (xy 152.725 118.875)
				(xy 152.2 119.325) (xy 152.2 121.925) (xy 151.65 122.475) (xy 150.575 122.475) (xy 149.55 121.45)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 33)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.6 118.725) (xy 119.725 115.825) (xy 119.725 102.075) (xy 120.725 101.075) (xy 123.7 101.075)
				(xy 123.7 109.25) (xy 126.225 111.775) (xy 134.35 111.775) (xy 135.3 112.725) (xy 137.3 112.725)
				(xy 137.825 112.2) (xy 137.825 109.225) (xy 138.475 108.575) (xy 144.025 108.575) (xy 144.025 108.775)
				(xy 138.5 108.775) (xy 138 109.275) (xy 138 112.275) (xy 136.575 113.7) (xy 132.9 113.7) (xy 131.85 114.75)
				(xy 131.85 118.275) (xy 131.4 118.725)
			)
		)
	)
	(zone
		(net 278)
		(net_name "RGB_EN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.5 130.9) (xy 142.7 130.1) (xy 144.3 130.1)
			)
		)
	)
	(zone
		(net 287)
		(net_name "PWR2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 135)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.75 64.55) (xy 151.75 63.1) (xy 150.2 63.1) (xy 149.2 64.1) (xy 147.95 64.1) (xy 147.95 66.85)
				(xy 145.625 69.175) (xy 132.925 69.175) (xy 129.925 72.175) (xy 129.925 77.675) (xy 125.775 81.825)
				(xy 125.775 85.1) (xy 123.775 87.1) (xy 123.775 87.9) (xy 124.25 88.375) (xy 125.075 88.375) (xy 125.3 88.125)
				(xy 125.3 87.975) (xy 127.275 86) (xy 127.275 82.325) (xy 131.35 78.275) (xy 131.35 73.2) (xy 133.9 70.65)
				(xy 146.075 70.65) (xy 148.6 68.125) (xy 148.6 67.15) (xy 151.2 64.55)
			)
		)
	)
	(zone
		(net 223)
		(net_name "EAR1")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 110)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 194.375012 81.224417) (xy 194.575012 81.349417) (xy 194.750012 81.549417) (xy 194.825012 81.774417)
				(xy 194.850012 81.974417) (xy 194.850012 82.274417) (xy 194.800012 82.549417) (xy 194.725012 82.749417)
				(xy 194.575012 82.949417) (xy 194.400012 83.074417) (xy 194.150012 83.149417) (xy 191.7 83.150583)
				(xy 191.45 83.075583) (xy 191.25 82.950583) (xy 191.075 82.750583) (xy 191 82.525583) (xy 190.975 82.325583)
				(xy 190.975 82.025583) (xy 191.025 81.750583) (xy 191.1 81.550583) (xy 191.25 81.350583) (xy 191.425 81.225583)
				(xy 191.675 81.150583) (xy 194.125012 81.149417)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 116)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 195.475 76.85) (xy 195.475 76.525) (xy 196.35 75.65) (xy 197.9 75.65) (xy 198.4 75.15) (xy 200.05 75.15)
				(xy 200.325 75.425) (xy 200.325 76.7) (xy 199.875 77.15) (xy 199.45 77.15) (xy 199.45 75.8) (xy 199.075 75.8)
				(xy 198.925 75.925) (xy 199.325 76.6) (xy 198.925 76.875) (xy 198.5 76.225) (xy 198.3 76.375) (xy 198.3 76.85)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 50)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.525 65.625) (xy 137.3 65.625) (xy 137.3 64.45) (xy 135.525 62.675)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 31)
		(connect_pads no
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.625 117.775) (xy 184.625 121.525) (xy 184.825 121.325) (xy 185.625 121.325) (xy 186.65 120.3)
				(xy 187.125 120.3) (xy 188.125 119.3) (xy 188.125 117.775)
			)
		)
	)
	(zone
		(net 211)
		(net_name "Net-(C901-Pad2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 139)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 109.275 87.2) (xy 110.425 88.35) (xy 110.425 89.825) (xy 110.35 90) (xy 110.25 90.125) (xy 109.95 90.4)
				(xy 109.275 90.4)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 143)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.6 74.175) (xy 109.525 71.075) (xy 108.95 71.075) (xy 108.075 70.2) (xy 107.05 70.2) (xy 106.525 69.675)
				(xy 106.525 65.15) (xy 107.1 64.575) (xy 108.575 64.575) (xy 110.05 63.1) (xy 110.05 59.85) (xy 109.725 59.525)
				(xy 109.225 59.525) (xy 108.275 60.475) (xy 108.275 62.275) (xy 108.25 62.525) (xy 108.15 62.7)
				(xy 108.025 62.875) (xy 107.85 63.05) (xy 107.575 63.225) (xy 107.275 63.325) (xy 106.9 63.375)
				(xy 104.9 63.375) (xy 104.2 64.075) (xy 104.2 75.975) (xy 105.025 75.975) (xy 105.025 73.95) (xy 106.6 72.375)
				(xy 108.975 72.375) (xy 111.7 75.1) (xy 112.6 75.1)
			)
		)
	)
	(zone
		(net 288)
		(net_name "PWR4")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.175 137.15) (xy 142.175 138.575) (xy 145 138.6) (xy 145.95 137.65) (xy 147.075 137.65) (xy 147.575 138.15)
				(xy 147.575 139.65) (xy 148 140.075) (xy 149.725 140.075) (xy 150.725 141.075) (xy 151.75 141.075)
				(xy 151.75 140.8) (xy 150.1 139.15) (xy 149.6 139.15) (xy 149.05 138.6) (xy 149.05 136.575) (xy 150.075 136.575)
				(xy 150.45 136.2) (xy 150.45 135.6) (xy 148.15 135.6) (xy 147.675 136.075) (xy 145.55 136.075) (xy 144.725 136.9)
				(xy 144.25 136.9) (xy 144 137.15)
			)
		)
	)
	(zone
		(net 282)
		(net_name "BATT-")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 120)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 193.825 68.575) (xy 188.275 68.575) (xy 188.275 69.625) (xy 188.425 69.775) (xy 189.475 69.775)
				(xy 191.225 71.525) (xy 193.825 71.525)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 124)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.25 77.7) (xy 172.475 77.7) (xy 173.475 76.7) (xy 173.475 73.6) (xy 172 72.125) (xy 172 66.6)
				(xy 169.95 64.55) (xy 169.95 63.125) (xy 166.375 63.125) (xy 166.375 63.95) (xy 167.9 65.475) (xy 167.9 65.775)
				(xy 168.2 66.075) (xy 169.975 66.075) (xy 171 67.1) (xy 171 72.625) (xy 172.525 74.15) (xy 172.525 76.15)
				(xy 171.25 77.425)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 138)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.275 51.8) (xy 119.35 51.8) (xy 119.35 50.225) (xy 120.175 50.225) (xy 120.75 50.8) (xy 120.75 54.325)
				(xy 119.175 55.9) (xy 117.275 54)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 178.525 86.825) (xy 179.3 86.825) (xy 179.3 87.85) (xy 178.525 87.85)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 152.225 70.675) (xy 153.225 70.675) (xy 153.225 69.875) (xy 152.225 69.875)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.3634 89.8398) (xy 164.3634 90.043) (xy 156.6418 90.043) (xy 149.6568 97.028) (xy 141.5034 97.028)
				(xy 140.5128 98.0186) (xy 137.414 98.0186) (xy 135.9408 96.5454) (xy 135.9662 95.0722) (xy 134.4168 93.5228)
				(xy 134.4168 88.392) (xy 135.9154 86.8934) (xy 136.4234 86.8934) (xy 136.4234 87.9094) (xy 136.9314 88.4174)
				(xy 136.906 94.996) (xy 138.4554 96.5454) (xy 139.5222 96.5454) (xy 139.9794 96.0882) (xy 139.9794 95.0468)
				(xy 138.0236 93.091) (xy 138.0236 88.8746) (xy 138.4808 88.4174) (xy 140.4874 88.4174) (xy 142.5194 90.4494)
				(xy 146.5326 90.4748) (xy 148.082 92.0242) (xy 152.7048 92.0242) (xy 154.8892 89.8398)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.5 60.525) (xy 168.5 61.475) (xy 169.45 61.475) (xy 169.45 60.525)
			)
		)
	)
	(zone
		(net 71)
		(net_name "AGND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 108)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.225 96.525) (xy 166.225 97.4) (xy 168.875 100.05) (xy 169.9 100.05) (xy 173.85 103.975)
				(xy 174.025 103.975) (xy 174.025 100.6) (xy 172.225 100.6) (xy 169.05 97.425) (xy 169.05 96.525)
			)
		)
	)
	(zone
		(net 214)
		(net_name "Net-(C500-Pad2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 146)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.85 40.825) (xy 121.35 40.825) (xy 119.575 42.6) (xy 119.575 46.525) (xy 117.75 48.35) (xy 117.725 49.125)
				(xy 119.725 49.125) (xy 120.75 48.1) (xy 120.75 43.625) (xy 122.85 41.525)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 134)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.775 64.325) (xy 119.275 64.825) (xy 120.775 64.825) (xy 121.175 64.4) (xy 121.175 63.025)
				(xy 120.75 63.025) (xy 120.75 63.725) (xy 120.025 63.725) (xy 120.025 62.025) (xy 118.775 60.775)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 22)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.575 143.975) (xy 125.025 139.425) (xy 124.7 139.425) (xy 124.7 140.875) (xy 125.725 140.875)
				(xy 125.725 143.2) (xy 125.1 143.2) (xy 124.3 144.125) (xy 123.7 144.125) (xy 123.7 144.4) (xy 123.975 144.675)
				(xy 129.575 144.675)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 122)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145.7 89.9) (xy 145.7 88.45) (xy 147.575 88.45) (xy 149.15 90.025) (xy 152.15 90.025) (xy 154.25 87.925)
				(xy 167.85 87.925) (xy 167.85 89.375) (xy 154.675 89.425) (xy 152.675 91.425) (xy 148.675 91.425)
				(xy 147.15 89.9)
			)
		)
	)
	(zone
		(net 228)
		(net_name "Net-(J100-Pin_1)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 110)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.974405 83.150012) (xy 197.099405 82.950012) (xy 197.299405 82.775012) (xy 197.524405 82.700012)
				(xy 197.724405 82.675012) (xy 198.024405 82.675012) (xy 198.299405 82.725012) (xy 198.499405 82.800012)
				(xy 198.699405 82.950012) (xy 198.824405 83.125012) (xy 198.899405 83.375012) (xy 198.900571 85.825024)
				(xy 198.825571 86.075024) (xy 198.700571 86.275024) (xy 198.500571 86.450024) (xy 198.275571 86.525024)
				(xy 198.075571 86.550024) (xy 197.775571 86.550024) (xy 197.500571 86.500024) (xy 197.300571 86.425024)
				(xy 197.100571 86.275024) (xy 196.975571 86.100024) (xy 196.900571 85.850024) (xy 196.899405 83.400012)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 29)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 182.575 125.125) (xy 184.325 126.875) (xy 184.325 130.2) (xy 184.1 130.425) (xy 183.5 130.425)
				(xy 183.5 131.5) (xy 182.55 132.45) (xy 181.85 132.45) (xy 181.025 131.625) (xy 181.025 130.875)
				(xy 180.8 130.65) (xy 180.8 130.05) (xy 180.5 129.75) (xy 180.5 128.3) (xy 179.125 126.925) (xy 179.125 125.925)
				(xy 182.075 122.975) (xy 182.575 122.975)
			)
		)
	)
	(zone
		(net 211)
		(net_name "Net-(C901-Pad2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 142)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.2 74.425) (xy 109.5 75.725) (xy 109.5 77.075) (xy 108.75 77.075) (xy 107.3 75.625) (xy 107.3 75.325)
			)
		)
	)
	(zone
		(net 229)
		(net_name "Net-(J100-Pin_2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 110)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 194.324988 78.724441) (xy 194.524988 78.849441) (xy 194.699988 79.049441) (xy 194.774988 79.274441)
				(xy 194.799988 79.474441) (xy 194.799988 79.774441) (xy 194.749988 80.049441) (xy 194.674988 80.249441)
				(xy 194.524988 80.449441) (xy 194.349988 80.574441) (xy 194.099988 80.649441) (xy 191.649976 80.650607)
				(xy 191.399976 80.575607) (xy 191.199976 80.450607) (xy 191.024976 80.250607) (xy 190.949976 80.025607)
				(xy 190.924976 79.825607) (xy 190.924976 79.525607) (xy 190.974976 79.250607) (xy 191.049976 79.050607)
				(xy 191.199976 78.850607) (xy 191.374976 78.725607) (xy 191.624976 78.650607) (xy 194.074988 78.649441)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 55)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 192.225 112.875) (xy 192.225 108.625) (xy 192.7 108.15) (xy 193.525 108.15) (xy 193.525 108.8)
				(xy 193.25 109.075) (xy 193.25 112.875)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 147)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.225 57.55) (xy 112.175 60.6) (xy 112.175 65.7) (xy 112.6 66.125) (xy 113.4 66.125) (xy 113.4 65)
				(xy 113.125 64.725) (xy 113.125 61.1) (xy 113.7 60.525) (xy 115.175 60.525) (xy 115.725 59.975)
				(xy 115.725 58.975) (xy 116.375 58.325) (xy 116.375 57.55)
			)
		)
	)
	(zone
		(net 208)
		(net_name "Net-(Q901-B)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 52)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.95 70.175) (xy 115.925 70.175) (xy 116.8 69.3) (xy 116.8 71.025)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads no
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.575 124.625) (xy 124.575 124.2) (xy 127.85 120.925) (xy 131.375 120.9) (xy 132.925 119.35)
				(xy 132.925 115.8) (xy 133.9 114.825) (xy 137.4 114.825) (xy 138.95 113.275) (xy 138.95 110.125)
				(xy 139.3 109.775) (xy 142.15 109.775) (xy 142.15 111.15) (xy 141.025 111.15) (xy 140.425 111.75)
				(xy 140.425 112.7) (xy 143.15 115.425) (xy 143.15 115.725) (xy 136.975 115.725) (xy 135.375 117.325)
				(xy 135.375 119.9) (xy 139.975 124.5) (xy 139.975 124.9) (xy 134.4 124.9) (xy 133.85 125.45) (xy 129.325 125.45)
				(xy 129.325 124.625)
			)
		)
	)
	(zone
		(net 198)
		(net_name "Net-(D501-K)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 49)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.525 57.6) (xy 137.525 62.05) (xy 136.95 62.05) (xy 135.45 60.55) (xy 134.3 60.55) (xy 134.3 59.7)
				(xy 136.4 57.6)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 127)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174 83.7) (xy 172.875 83.7) (xy 172.875 88.75) (xy 173.475 89.35) (xy 177.25 89.35) (xy 178.275 90.275)
				(xy 178.275 91.875) (xy 176.4 93.75) (xy 176.4 95.675) (xy 176.875 95.675) (xy 178.6 93.95) (xy 182.85 93.925)
				(xy 183.45 93.325) (xy 183.45 92.05) (xy 184.1 91.4) (xy 184.1 89.1) (xy 183.65 88.65) (xy 180.85 88.65)
				(xy 180.025 87.825) (xy 180.025 86.8) (xy 179.075 85.85) (xy 174.55 85.85) (xy 174 85.3)
			)
		)
	)
	(zone
		(net 271)
		(net_name "Net-(D500-A)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.025 62.05) (xy 184.025 63) (xy 184.25 63) (xy 182.725 64.525) (xy 182.725 66) (xy 184.65 66)
				(xy 184.65 64.575) (xy 185.775 63.45) (xy 185.775 62.05)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 113)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.3 88.4) (xy 133.4 83.3) (xy 133.4 81.175) (xy 134.5 80.075) (xy 134.5 79.4) (xy 134.4 79.4)
				(xy 134.4 78.725) (xy 135.475 78.725) (xy 135.475 80.175) (xy 135.95 80.175) (xy 136.5 80.725) (xy 136.5 81.75)
				(xy 137 82.25) (xy 137.5 82.25) (xy 137.475 71.675) (xy 136.975 71.175) (xy 133.95 71.175) (xy 131.925 73.2)
				(xy 131.925 78.7) (xy 127.85 82.775) (xy 127.85 86.35) (xy 125.8 88.4)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 111)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 148.125 103.05) (xy 148.125 104.05) (xy 147.15 105.025) (xy 138.925 105.025) (xy 137.4 103.5)
				(xy 136.15 103.525) (xy 135.925 103.3) (xy 135.925 103.025) (xy 133.2 103.025) (xy 133.2 102.325)
				(xy 130.4 99.525) (xy 130.375 94) (xy 128.875 92.5) (xy 128.875 90.3) (xy 130.325 90.3) (xy 130.325 91.975)
				(xy 131.825 93.475) (xy 131.825 98.55) (xy 134.925 101.65) (xy 137.4 101.65) (xy 138.8 103.05)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 112)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.7 101.075) (xy 123.7 100.575) (xy 124.225 100.05) (xy 125.25 100.05) (xy 128.725 103.525)
				(xy 131.4 103.525) (xy 131.4 101.675) (xy 129.8 100.075) (xy 129.8 93.975) (xy 128.3 92.475) (xy 128.3 88.4)
				(xy 125.8 88.4) (xy 125.25 88.95) (xy 123.775 88.95) (xy 123.25 89.475) (xy 123.25 91.475) (xy 120.725 94)
				(xy 120.725 101.075)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.8526 83.2866) (xy 167.3606 83.7946) (xy 167.3606 84.8614) (xy 169.1894 84.8614) (xy 169.1894 85.8266)
				(xy 168.656 86.36) (xy 164.338 86.36) (xy 163.83 85.852) (xy 163.83 83.6168) (xy 164.1602 83.2866)
			)
		)
	)
	(zone
		(net 287)
		(net_name "PWR2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 23)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114 141.15) (xy 111.05 141.15) (xy 104.875 134.975) (xy 104.875 137.825) (xy 111.75 144.7) (xy 111.75 145.2)
				(xy 112.525 145.2) (xy 112.525 143.7) (xy 114 142.225)
			)
		)
	)
	(zone
		(net 231)
		(net_name "Net-(J100-Pin_11)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 110)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 194.374988 86.224417) (xy 194.574988 86.349417) (xy 194.749988 86.549417) (xy 194.824988 86.774417)
				(xy 194.849988 86.974417) (xy 194.849988 87.274417) (xy 194.799988 87.549417) (xy 194.724988 87.749417)
				(xy 194.574988 87.949417) (xy 194.399988 88.074417) (xy 194.149988 88.149417) (xy 191.699976 88.150583)
				(xy 191.449976 88.075583) (xy 191.249976 87.950583) (xy 191.074976 87.750583) (xy 190.999976 87.525583)
				(xy 190.974976 87.325583) (xy 190.974976 87.025583) (xy 191.024976 86.750583) (xy 191.099976 86.550583)
				(xy 191.249976 86.350583) (xy 191.424976 86.225583) (xy 191.674976 86.150583) (xy 194.124988 86.149417)
			)
		)
	)
	(zone
		(net 281)
		(net_name "BATT+")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 47)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.425 62.05) (xy 189.425 63) (xy 187.9 63) (xy 187.9 62.05)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 123)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 167.85 89.375) (xy 167.85 87.925) (xy 169.425 87.925) (xy 171.25 86.1) (xy 171.25 77.7) (xy 172.475 77.7)
				(xy 172.475 86.85) (xy 169.95 89.375)
			)
		)
	)
	(zone
		(net 285)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 131)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 146.75 54.675) (xy 146.75 57.25) (xy 149.675 57.25) (xy 149.675 54.675)
			)
		)
	)
	(zone
		(net 281)
		(net_name "BATT+")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 118)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 189.875 73.25) (xy 191.7 75.075) (xy 195.525 75.075) (xy 195.8 74.8) (xy 195.8 73.5) (xy 194.85 73.5)
				(xy 194.85 74.125) (xy 193.25 74.125) (xy 193.25 73.25)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 136)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 176.025 61.475) (xy 178.6 61.475) (xy 180.625 59.45) (xy 178.15 59.45) (xy 177.6 59) (xy 177.4 58.1)
				(xy 182.75 52.75) (xy 184.95 52.75) (xy 185.2 52.5) (xy 185.2 49.7) (xy 183.775 48.275) (xy 180.9 48.275)
				(xy 180.1 49.075) (xy 180.1 50.7) (xy 177.4 53.425) (xy 175.65 53.45) (xy 175.15 53.95) (xy 175.15 55.3)
				(xy 174.575 55.875) (xy 176.05 55.875)
			)
		)
	)
	(zone
		(net 212)
		(net_name "Net-(CN900-Pin_1)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 140)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 109.4 96.6) (xy 107.5 96.6) (xy 106.975 96.075) (xy 106.975 92.05) (xy 106.55 91.625) (xy 105.4 91.625)
				(xy 105 92.025) (xy 105 97.975) (xy 105.525 98.5) (xy 109.35 98.5) (xy 110 97.85) (xy 110 97.225)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 115)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 197.225 109.1) (xy 199.225 109.1) (xy 199.225 103.525) (xy 196.225 100.525) (xy 193.55 100.525)
				(xy 193.05 100.025) (xy 192.625 100.025) (xy 192.625 100.775) (xy 192.8 100.775) (xy 192.8 101.525)
				(xy 191.7 101.525) (xy 191.7 100.025) (xy 191.525 100.025) (xy 190.725 100.825) (xy 190.725 102.575)
				(xy 190.4 102.575) (xy 189.875 103.1) (xy 189.875 104.375) (xy 190.525 104.95) (xy 191.275 104.95)
				(xy 193.75 102.475) (xy 195.725 102.475) (xy 197.225 103.975)
			)
		)
	)
	(zone
		(net 285)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 145)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.85 39.675) (xy 117.85 37.625) (xy 118.275 37.2) (xy 129.275 37.2) (xy 134.025 41.95) (xy 134.025 52.25)
				(xy 133 51.225) (xy 133 42.4) (xy 129.175 38.575) (xy 119.35 38.575) (xy 118.25 39.675)
			)
		)
	)
	(zone
		(net 194)
		(net_name "Net-(D501-A-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 132)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.55 55.75) (xy 139.175 55.375) (xy 138.875 55.375) (xy 138.875 58.425) (xy 139.55 58.425)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 24)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.525 120.4) (xy 106.05 120.875) (xy 106.05 122) (xy 106.525 122.4) (xy 111.55 122.4) (xy 112.05 121.9)
				(xy 112.05 120.925) (xy 111.525 120.4)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 133)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.65 65.1) (xy 129.65 62.85) (xy 128.375 61.575) (xy 126.575 61.575) (xy 124.35 63.8) (xy 124.35 65.5)
				(xy 127.475 68.6) (xy 128.85 68.6) (xy 129.325 68.125) (xy 129.625 68.125) (xy 129.9 67.825) (xy 129.9 66.95)
				(xy 129.75 66.8) (xy 129.75 65.2)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 121)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.875 90.3) (xy 130.325 90.3) (xy 130.325 89.4) (xy 135.425 84.3) (xy 139.95 84.3) (xy 140.5 84.85)
				(xy 140.5 87.45) (xy 142.95 89.9) (xy 145.7 89.9) (xy 145.7 88.45) (xy 143.525 88.45) (xy 142 86.925)
				(xy 142 85.3) (xy 143.525 83.775) (xy 145 83.775) (xy 146.65 82.125) (xy 146.65 81.725) (xy 143.55 81.725)
				(xy 143.55 82.325) (xy 143.075 82.8) (xy 135 82.8) (xy 128.875 88.925)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 48)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.225 59.45) (xy 183.375 56.3) (xy 183.375 56.875) (xy 183.45 57.075) (xy 183.575 57.275)
				(xy 183.7 57.425) (xy 183.75 57.475) (xy 184.9 56.325) (xy 185.575 56.875) (xy 185.275 57.275) (xy 184.2 58.35)
				(xy 184.2 58.925) (xy 183.675 59.45)
			)
		)
	)
	(zone
		(net 240)
		(net_name "Net-(D500-K)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 117)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193.925 76.15) (xy 191.9 76.15) (xy 191.9 77.175) (xy 193.925 77.175)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 54)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177.1 106.875) (xy 177.975 106.875) (xy 178.975 107.875) (xy 178.975 109.1) (xy 179.55 109.1)
				(xy 179.55 110.1) (xy 178.875 110.1) (xy 178.425 109.65) (xy 178.425 108.275) (xy 177.1 106.95)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 32)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.15 111.15) (xy 146.1 111.15) (xy 150.2 115.25) (xy 154.65 115.25) (xy 155.2 114.675) (xy 155.2 110.175)
				(xy 154.7 109.675) (xy 151.8 109.675) (xy 151.8 110.7) (xy 152.65 110.7) (xy 152.65 111.775) (xy 151.125 111.775)
				(xy 150.675 112.225) (xy 149.025 112.225) (xy 148.1 111.3) (xy 147.025 111.3) (xy 145.975 110.25)
				(xy 144.975 110.25) (xy 144.5 109.775) (xy 142.15 109.775)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.475 60.525) (xy 167.4 60.525) (xy 167.4 61.375) (xy 166.475 61.375)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 125)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.45 62.05) (xy 165.4 62.05) (xy 164.95 61.6) (xy 164.95 55.875) (xy 165.45 55.375) (xy 172.55 55.375)
				(xy 173.05 55.875) (xy 176.05 55.875) (xy 176 66.6) (xy 172.525 66.6) (xy 172.525 66.125) (xy 171 64.6)
				(xy 171 62.6)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 163.83 105.1052) (xy 167.513 105.1052) (xy 167.513 105.8164) (xy 149.9108 105.8164) (xy 148.971 104.8766)
				(xy 148.971 104.648) (xy 163.3728 104.648)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 53)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 185.425 109.475) (xy 181.45 105.525) (xy 181.375 105.525) (xy 181.3 105.6) (xy 181.3 105.675)
				(xy 185.3 109.7) (xy 188.725 109.7) (xy 190.3 108.125) (xy 190.45 108.1) (xy 190.625 108) (xy 190.75 107.85)
				(xy 190.775 107.6) (xy 190.75 107.325) (xy 190.85 107.225) (xy 191.25 107.225) (xy 193.375 105.1)
				(xy 193.375 105.025) (xy 193.3 104.95) (xy 193.225 104.95) (xy 191.175 107) (xy 190.6 107) (xy 190.525 107.075)
				(xy 190.05 107.075) (xy 189.825 107.225) (xy 189.7 107.425) (xy 189.7 107.725) (xy 189.8 107.95)
				(xy 190 108.1) (xy 188.625 109.475)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 141)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.75 78.125) (xy 106.75 87) (xy 106.625 87.125) (xy 106.625 87.275) (xy 105.975 87.925) (xy 105 87.925)
				(xy 104.2 87.125) (xy 104.2 75.975) (xy 105.025 75.975) (xy 105.025 76.15) (xy 106.35 77.475) (xy 106.35 78.125)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 126)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 172.525 66.6) (xy 172.525 71.575) (xy 174.05 73.1) (xy 174.05 77.2) (xy 172.9 78.35) (xy 172.875 83.7)
				(xy 174 83.7) (xy 174 81.7) (xy 175 80.7) (xy 175 79.2) (xy 175.475 78.725) (xy 175.475 75.125)
				(xy 176.5 74.1) (xy 178.025 74.1) (xy 178.55 73.575) (xy 178.55 69.15) (xy 176 66.6)
			)
		)
	)
	(zone
		(net 216)
		(net_name "BLH")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 148)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.625 64.3) (xy 110.625 58.95) (xy 109.125 57.45) (xy 109.125 52.55) (xy 109.425 52.25) (xy 112.225 52.25)
				(xy 112.7 51.775) (xy 112.7 49.25) (xy 117.325 44.625) (xy 117.325 41.75) (xy 117.725 41.35) (xy 118.825 41.35)
				(xy 118.825 45.15) (xy 114.2 49.775) (xy 114.2 53.35) (xy 113.75 53.8) (xy 111.65 53.8) (xy 111.15 54.3)
				(xy 111.15 58) (xy 111.6 58.45) (xy 111.6 64.05) (xy 111.35 64.3)
			)
		)
	)
	(zone
		(net 286)
		(net_name "+5VL")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.1)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.4932 99.314) (xy 162.306 99.314) (xy 162.306 101.4476) (xy 162.179 101.5746) (xy 161.5694 101.5746)
				(xy 161.036 101.0412) (xy 160.3248 101.0412) (xy 160.3248 100.1014) (xy 160.7058 100.1014)
			)
		)
	)
	(zone
		(net 278)
		(net_name "RGB_EN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 146.3 130.25) (xy 149.55 133.5) (xy 149.55 132.4) (xy 147.4 130.25)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 150)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.35 39.85) (xy 126.35 38) (xy 124.875 38) (xy 124.875 39.85)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 129)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 153.225 67.625) (xy 155.7 65.15) (xy 158.375 65.15) (xy 158.75 65.525) (xy 158.75 67.125) (xy 158.175 67.7)
				(xy 156.725 67.7) (xy 156.35 68.075) (xy 153.225 68.075)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 144)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.3 44.55) (xy 131.15 45.4) (xy 131.15 51.825) (xy 131.9 51.825) (xy 131.9 44.925) (xy 131.275 44.3)
				(xy 130.3 44.3)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads no
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.825 128.15) (xy 128.825 129.95) (xy 130.025 130.925) (xy 130.75 130.925) (xy 130.75 130.375)
				(xy 131.15 130.375) (xy 132.275 131.5) (xy 132.275 134.025) (xy 131.775 134.525) (xy 124.2 134.525)
				(xy 123.7 134.025) (xy 123.7 131.475) (xy 122.6 130.375) (xy 122.6 118.725) (xy 131.4 118.725) (xy 130.25 119.875)
				(xy 126.725 119.875) (xy 122.775 123.825) (xy 122.775 128.65) (xy 123.35 129.225) (xy 124.05 129.225)
				(xy 124.575 128.7) (xy 124.575 124.625) (xy 129.325 124.625) (xy 129.325 125.45) (xy 128.825 125.95)
			)
		)
	)
	(zone
		(net 287)
		(net_name "PWR2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 130)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.75 55.55) (xy 151.925 55.375) (xy 164.25 55.375) (xy 164.4 55.525) (xy 164.4 64.425) (xy 164.275 64.55)
				(xy 151.75 64.55)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 14)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.434 93.4974) (xy 170.434 94.361) (xy 170.2816 94.5134) (xy 168.8338 94.5134) (xy 164.846 94.5388)
				(xy 164.338 94.0308) (xy 162.8394 94.0308) (xy 162.1028 93.2942) (xy 158.6992 93.2688) (xy 158.4198 93.5482)
				(xy 158.4198 94.361) (xy 155.956 96.8248) (xy 155.956 98.8314) (xy 153.6446 101.1428) (xy 148.5392 101.1428)
				(xy 147.9804 100.584) (xy 147.9804 99.568) (xy 148.5646 98.9838) (xy 149.5806 98.9838) (xy 157.7086 90.8558)
				(xy 163.9062 90.8558) (xy 164.9984 91.948) (xy 171.196 91.948) (xy 172.5676 93.3196) (xy 172.5676 98.044)
				(xy 172.3644 98.044) (xy 172.3644 93.3704) (xy 171.1198 92.1512) (xy 164.8714 92.1512) (xy 163.8046 91.059)
				(xy 157.8102 91.059) (xy 149.6822 99.187) (xy 148.6662 99.187) (xy 148.209 99.6442) (xy 148.209 100.5078)
				(xy 148.6408 100.9396) (xy 149.7584 100.9396) (xy 158.8008 91.8972) (xy 163.0426 91.8972) (xy 164.211 93.0656)
				(xy 170.0022 93.0656)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 154)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 161.163 94.742) (xy 161.417 94.996) (xy 161.417 104.902) (xy 159.385 106.934) (xy 158.369 106.934)
				(xy 156.591 108.712) (xy 156.591 116.713) (xy 155.575 117.729) (xy 155.575 121.158) (xy 154.559 122.174)
				(xy 154.559 130.048) (xy 152.4 132.207) (xy 152.4 137.414) (xy 156.845 141.859) (xy 156.845 146.812)
				(xy 200.533 146.812) (xy 200.533 136.017) (xy 200.025 135.509) (xy 197.739 135.509) (xy 196.85 134.62)
				(xy 196.85 131.572) (xy 193.294 128.016) (xy 193.294 125.73) (xy 194.818 124.206) (xy 194.818 123.063)
				(xy 196.342 121.539) (xy 196.342 113.792) (xy 194.056 111.506) (xy 194.056 108.966) (xy 195.072 107.95)
				(xy 195.072 101.854) (xy 193.548 100.33) (xy 193.548 96.647) (xy 192.024 95.123) (xy 192.024 94.107)
				(xy 189.23 91.313) (xy 187.833 91.313) (xy 186.563 90.043) (xy 186.563 85.217) (xy 185.547 84.201)
				(xy 176.53 84.201) (xy 174.625 86.106) (xy 174.625 88.392) (xy 173.99 89.027) (xy 173.99 91.948)
				(xy 171.45 94.488) (xy 167.005 94.488) (xy 166.751 94.234) (xy 166.497 94.488) (xy 161.417 94.488)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 151)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.14 119.888) (xy 104.14 146.812) (xy 156.337 146.812) (xy 156.337 141.986) (xy 151.892 137.541)
				(xy 151.892 132.08) (xy 154.051 129.921) (xy 154.051 122.047) (xy 155.067 121.031) (xy 155.067 113.03)
				(xy 153.67 111.633) (xy 148.717 111.633) (xy 148.336 112.014) (xy 148.336 117.983) (xy 146.939 119.38)
				(xy 135.128 119.38) (xy 132.334 122.174) (xy 132.334 123.063) (xy 130.683 124.714) (xy 126.746 124.714)
				(xy 126.111 124.079) (xy 126.111 122.809) (xy 125.603 122.301) (xy 115.57 122.301) (xy 114.808 121.539)
				(xy 114.808 119.888)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 153)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.658 46.482) (xy 186.182 48.006) (xy 199.771 48.006) (xy 200.66 48.895) (xy 200.66 77.343)
				(xy 198.882 79.121) (xy 198.882 90.424) (xy 200.533 92.075) (xy 200.533 134.239) (xy 199.771 135.001)
				(xy 197.866 135.001) (xy 197.358 134.493) (xy 197.358 131.445) (xy 193.802 127.762) (xy 193.802 125.857)
				(xy 195.326 124.333) (xy 195.326 123.19) (xy 196.85 121.666) (xy 196.85 113.792) (xy 194.945 111.887)
				(xy 194.437 111.379) (xy 194.437 109.093) (xy 195.453 108.077) (xy 195.453 101.727) (xy 193.929 100.203)
				(xy 193.929 96.52) (xy 192.405 94.996) (xy 192.405 93.98) (xy 189.357 90.932) (xy 187.96 90.932)
				(xy 186.944 89.916) (xy 186.944 85.09) (xy 185.547 83.693) (xy 176.403 83.693) (xy 174.117 85.979)
				(xy 174.117 88.265) (xy 173.482 88.9) (xy 173.482 91.821) (xy 171.323 93.98) (xy 167.005 93.98)
				(xy 166.497 94.488) (xy 161.417 94.488) (xy 160.909 94.996) (xy 160.909 104.775) (xy 159.258 106.426)
				(xy 158.242 106.426) (xy 156.083 108.585) (xy 156.083 116.586) (xy 155.067 117.602) (xy 155.067 113.03)
				(xy 153.67 111.633) (xy 152.273 111.633) (xy 153.035 110.871) (xy 153.035 104.013) (xy 154.432 102.616)
				(xy 156.972 102.616) (xy 156.972 100.076) (xy 154.432 100.076) (xy 152.273 97.917) (xy 152.273 96.393)
				(xy 149.225 93.345) (xy 149.225 90.424) (xy 149.352 90.297) (xy 151.384 90.297) (xy 153.543 88.138)
				(xy 163.957 88.138) (xy 164.465 87.63) (xy 166.751 87.63) (xy 167.767 86.741) (xy 167.767 85.344)
				(xy 168.021 85.09) (xy 169.545 85.09) (xy 170.561 84.074) (xy 170.561 78.486) (xy 173.101 75.946)
				(xy 173.101 74.295) (xy 172.339 73.533) (xy 172.339 63.627) (xy 170.688 61.976) (xy 170.688 58.801)
				(xy 170.434 58.547) (xy 171.323 57.658) (xy 171.323 53.721) (xy 172.212 53.721) (xy 172.974 52.959)
				(xy 172.974 47.625) (xy 174.117 46.482)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 152)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.316 119.888) (xy 115.316 121.285) (xy 115.824 121.793) (xy 125.603 121.793) (xy 126.619 122.809)
				(xy 126.619 123.952) (xy 126.873 124.206) (xy 130.556 124.206) (xy 131.826 122.936) (xy 131.826 122.047)
				(xy 135.001 118.872) (xy 146.685 118.872) (xy 147.828 117.729) (xy 147.828 111.887) (xy 148.59 111.125)
				(xy 152.146 111.125) (xy 152.527 110.744) (xy 152.527 103.886) (xy 154.305 102.108) (xy 156.464 102.108)
				(xy 156.464 100.584) (xy 154.305 100.584) (xy 151.765 98.044) (xy 151.765 96.52) (xy 148.717 93.472)
				(xy 148.717 90.297) (xy 149.225 89.789) (xy 151.257 89.789) (xy 153.416 87.63) (xy 163.83 87.63)
				(xy 164.338 87.122) (xy 166.624 87.122) (xy 167.259 86.614) (xy 167.259 85.217) (xy 167.894 84.582)
				(xy 169.418 84.582) (xy 170.053 83.947) (xy 170.053 78.359) (xy 172.593 75.819) (xy 172.593 74.422)
				(xy 171.831 73.66) (xy 171.831 63.754) (xy 170.18 62.103) (xy 170.18 58.801) (xy 171.323 57.658)
				(xy 171.323 53.721) (xy 138.43 53.721) (xy 136.144 52.451) (xy 134.62 50.038) (xy 134.366 47.752)
				(xy 134.366 41.656) (xy 129.794 37.084) (xy 117.602 37.084) (xy 117.602 42.037) (xy 117.094 45.466)
				(xy 115.062 48.26) (xy 111.887 49.784) (xy 109.22 49.784) (xy 109.22 54.102) (xy 124.46 54.102)
				(xy 124.46 77.851) (xy 122.936 79.375) (xy 119.38 79.375) (xy 119.38 90.932) (xy 119.126 90.932)
				(xy 116.332 93.726) (xy 116.332 119.888)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 161)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.46 70.358) (xy 124.46 77.851) (xy 122.936 79.375) (xy 119.38 79.375) (xy 119.38 90.678)
				(xy 117.094 92.964) (xy 117.094 99.695) (xy 116.332 100.457) (xy 116.332 117.602) (xy 119.507 120.777)
				(xy 119.507 131.826) (xy 120.523 132.842) (xy 120.523 134.493) (xy 122.047 136.017) (xy 124.46 136.017)
				(xy 136.906 136.017) (xy 137.033 135.89) (xy 137.033 135.382) (xy 136.906 135.255) (xy 132.969 135.255)
				(xy 132.207 134.493) (xy 124.46 134.493) (xy 123.19 133.223) (xy 123.19 131.699) (xy 122.174 130.683)
				(xy 122.174 118.745) (xy 119.253 115.951) (xy 119.253 101.6) (xy 120.269 100.584) (xy 120.269 93.853)
				(xy 122.682 91.44) (xy 122.682 89.281) (xy 123.571 88.392) (xy 124.968 88.392) (xy 127.381 85.979)
				(xy 127.381 82.423) (xy 131.318 78.486) (xy 131.318 73.279) (xy 134.239 70.358)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 152)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.682 118.745) (xy 122.682 123.952) (xy 123.19 124.46) (xy 134.493 124.46) (xy 152.527 124.46)
				(xy 152.527 101.219) (xy 148.971 101.219) (xy 148.336 100.584) (xy 148.336 99.568) (xy 148.844 99.06)
				(xy 149.479 99.06) (xy 157.861 90.678) (xy 163.957 90.678) (xy 165.1 91.821) (xy 171.323 91.821)
				(xy 172.847 93.345) (xy 172.847 98.679) (xy 175.768 98.679) (xy 176.911 98.679) (xy 176.911 95.504)
				(xy 177.292 95.123) (xy 177.292 90.678) (xy 173.482 86.995) (xy 173.482 73.66) (xy 171.831 72.009)
				(xy 171.831 66.421) (xy 170.18 64.77) (xy 170.18 58.801) (xy 171.323 57.658) (xy 171.323 53.721)
				(xy 151.384 53.721) (xy 151.384 64.897) (xy 148.844 67.437) (xy 148.844 68.453) (xy 146.431 70.866)
				(xy 134.493 70.866) (xy 131.953 73.406) (xy 131.826 78.74) (xy 127.889 82.677) (xy 127.889 86.106)
				(xy 125.095 88.9) (xy 123.825 88.9) (xy 123.19 89.535) (xy 123.19 91.567) (xy 120.777 93.98) (xy 120.777 100.965)
				(xy 119.761 101.981) (xy 119.761 115.824)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 157)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.5 108.712) (xy 191.262 107.95) (xy 191.262 107.696) (xy 194.564 104.394) (xy 195.199 104.394)
				(xy 196.088 105.283) (xy 196.088 110.871) (xy 198.501 113.284) (xy 198.501 119.38) (xy 196.596 119.38)
				(xy 195.961 120.015) (xy 195.961 128.778) (xy 190.5 134.239)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 155)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.14 138.938) (xy 104.14 119.888) (xy 117.729 119.888) (xy 118.872 121.031) (xy 118.872 132.334)
				(xy 119.761 133.223) (xy 119.761 138.938)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 158)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.323 53.721) (xy 172.212 53.721) (xy 172.974 52.959) (xy 172.974 47.625) (xy 174.117 46.482)
				(xy 184.658 46.482) (xy 186.182 48.006) (xy 199.771 48.006) (xy 200.66 48.895) (xy 200.66 77.343)
				(xy 198.882 79.121) (xy 198.882 90.424) (xy 200.533 92.075) (xy 200.533 137.287) (xy 193.421 137.287)
				(xy 191.897 137.287) (xy 191.897 133.731) (xy 196.469 129.159) (xy 196.469 120.142) (xy 196.723 119.888)
				(xy 199.009 119.888) (xy 199.009 113.03) (xy 196.596 110.617) (xy 196.596 105.156) (xy 195.326 103.886)
				(xy 194.437 103.886) (xy 190.754 107.569) (xy 190.754 107.823) (xy 190.373 108.204) (xy 190.246 108.204)
				(xy 189.103 109.347) (xy 185.293 109.347) (xy 180.213 104.267) (xy 173.99 104.267) (xy 169.418 99.695)
				(xy 168.402 99.695) (xy 165.862 97.155) (xy 162.56 97.155) (xy 161.544 98.171) (xy 160.782 98.171)
				(xy 160.401 98.552) (xy 155.956 98.552) (xy 153.797 100.711) (xy 150.114 100.711) (xy 149.733 100.33)
				(xy 149.733 99.568) (xy 158.115 91.186) (xy 163.576 91.186) (xy 164.719 92.329) (xy 170.815 92.329)
				(xy 172.212 93.726) (xy 172.212 99.314) (xy 172.593 99.695) (xy 173.355 99.695) (xy 173.863 99.187)
				(xy 176.911 99.187) (xy 177.292 98.806) (xy 177.292 95.631) (xy 177.673 95.25) (xy 177.673 90.551)
				(xy 176.276 89.154) (xy 173.99 86.868) (xy 173.99 73.533) (xy 172.339 71.882) (xy 172.339 66.294)
				(xy 170.688 64.643) (xy 170.688 58.801) (xy 170.434 58.547) (xy 171.323 57.658)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 156)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.275 100.203) (xy 169.291 100.203) (xy 173.863 104.775) (xy 180.086 104.775) (xy 185.166 109.855)
				(xy 189.357 109.855) (xy 189.611 109.601) (xy 190.5 109.601) (xy 190.5 136.906) (xy 187.833 139.573)
				(xy 173.482 139.573) (xy 172.72 138.811) (xy 170.942 138.811) (xy 169.418 140.335) (xy 155.575 140.335)
				(xy 154.178 138.938) (xy 152.908 138.938) (xy 151.257 137.287) (xy 151.257 133.858) (xy 151.892 133.223)
				(xy 151.892 130.175) (xy 150.241 128.524) (xy 144.78 128.524) (xy 140.716 124.46) (xy 152.527 124.46)
				(xy 152.527 101.219) (xy 153.924 101.219) (xy 156.083 99.06) (xy 160.401 99.06) (xy 160.909 98.552)
				(xy 161.798 98.552) (xy 162.687 97.663) (xy 165.735 97.663)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 159)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 191.897 137.287) (xy 193.421 137.287) (xy 200.533 137.287) (xy 200.533 146.812) (xy 104.14 146.812)
				(xy 104.14 138.938) (xy 119.761 138.938) (xy 119.761 134.366) (xy 121.92 136.525) (xy 137.541 136.525)
				(xy 137.541 135.128) (xy 137.16 134.747) (xy 133.096 134.747) (xy 132.334 133.985) (xy 124.587 133.985)
				(xy 123.698 133.096) (xy 123.698 131.572) (xy 122.682 130.556) (xy 122.682 125.476) (xy 123.19 124.968)
				(xy 140.716 124.968) (xy 144.78 129.032) (xy 150.114 129.032) (xy 151.384 130.302) (xy 151.384 132.969)
				(xy 150.749 133.604) (xy 150.749 137.414) (xy 152.781 139.446) (xy 154.051 139.446) (xy 155.448 140.843)
				(xy 169.545 140.843) (xy 170.688 139.7) (xy 172.339 139.7) (xy 172.72 140.081) (xy 188.087 140.081)
				(xy 189.992 138.176) (xy 191.008 138.176)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 160)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 151.384 53.721) (xy 138.43 53.721) (xy 136.144 52.451) (xy 134.62 50.038) (xy 134.366 47.752)
				(xy 134.366 41.656) (xy 129.794 37.084) (xy 117.602 37.084) (xy 117.602 42.037) (xy 117.094 45.466)
				(xy 115.062 48.26) (xy 111.887 49.784) (xy 109.22 49.784) (xy 109.22 54.102) (xy 124.46 54.102)
				(xy 124.46 70.358) (xy 146.304 70.358) (xy 148.336 68.326) (xy 148.336 67.31) (xy 151.13 64.516)
				(xy 151.384 64.516)
			)
		)
	)
	(embedded_fonts no)
)
