(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "MiniNDP")
		(date "2026-09-03")
		(rev "T512_12")
		(company "Brian K. White - b.kenyon.w@gmail.com")
		(comment 1 "github.com/bkw777/NODE_DATAPAC")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Blue")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Blue")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 121.95 86.025)
		(grid_origin 151.95 115.025)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VMEM")
	(net 3 "VBUS")
	(net 4 "/AD0")
	(net 5 "/AD1")
	(net 6 "/AD2")
	(net 7 "/AD3")
	(net 8 "/AD4")
	(net 9 "/AD5")
	(net 10 "/AD6")
	(net 11 "/AD7")
	(net 12 "/A8")
	(net 13 "/A9")
	(net 14 "/A10")
	(net 15 "/A11")
	(net 16 "/A12")
	(net 17 "/A13")
	(net 18 "/A14")
	(net 19 "/A15")
	(net 20 "/~{RD}")
	(net 21 "/RAMRST")
	(net 22 "/~{Y0}")
	(net 23 "/(A)")
	(net 24 "unconnected-(J1-Pin_39-Pad39)")
	(net 25 "unconnected-(J1-Pin_40-Pad40)")
	(net 26 "unconnected-(J1-Pin_30-Pad30)")
	(net 27 "unconnected-(J1-Pin_31-Pad31)")
	(net 28 "unconnected-(J1-Pin_37-Pad37)")
	(net 29 "unconnected-(J1-Pin_15-Pad15)")
	(net 30 "/~{CE}")
	(net 31 "/A18_CE2")
	(net 32 "unconnected-(U1-Y1-Pad14)")
	(net 33 "/BUS_A10")
	(net 34 "unconnected-(U1-Y7-Pad7)")
	(net 35 "unconnected-(U1-Y0-Pad15)")
	(net 36 "unconnected-(U1-Y2-Pad13)")
	(net 37 "/A5")
	(net 38 "/A6")
	(net 39 "unconnected-(U1-Y3-Pad12)")
	(net 40 "unconnected-(U1-Y5-Pad10)")
	(net 41 "/A7")
	(net 42 "+BATT")
	(net 43 "/BUS_A8")
	(net 44 "/BUS_A9")
	(net 45 "/A16")
	(net 46 "/A17")
	(net 47 "/A3")
	(net 48 "/BYTE")
	(net 49 "unconnected-(U2-Q11-Pad1)")
	(net 50 "unconnected-(J1-Pin_17-Pad17)")
	(net 51 "unconnected-(J1-Pin_18-Pad18)")
	(net 52 "unconnected-(J1-Pin_19-Pad19)")
	(net 53 "unconnected-(J1-Pin_20-Pad20)")
	(net 54 "unconnected-(J1-Pin_25-Pad25)")
	(net 55 "unconnected-(J1-Pin_26-Pad26)")
	(net 56 "unconnected-(J1-Pin_27-Pad27)")
	(net 57 "unconnected-(J1-Pin_28-Pad28)")
	(net 58 "unconnected-(J1-Pin_33-Pad33)")
	(net 59 "unconnected-(J1-Pin_34-Pad34)")
	(net 60 "unconnected-(U2-Q10-Pad15)")
	(net 61 "/~{WR}")
	(net 62 "/BLOCK")
	(net 63 "/A0")
	(net 64 "/A2")
	(net 65 "/A4")
	(net 66 "/A1")
	(net 67 "Net-(U6-Pad6)")
	(footprint "000_LOCAL:TSSOP-16"
		(layer "F.Cu")
		(at 155.1 108.25 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U1"
			(at -1.25 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC238"
			(at 1 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/HC238.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC DECODER/DEMUX 1 X 3:8 16SO"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC238PW,118"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/BUS_A9")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/BUS_A8")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{E1}")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/(A)")
			(pinfunction "~{E2}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/~{Y0}")
			(pinfunction "E3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "unconnected-(U1-Y7-Pad7)")
			(pinfunction "Y7")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/BYTE")
			(pinfunction "Y6")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U1-Y5-Pad10)")
			(pinfunction "Y5")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "Y4")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(U1-Y3-Pad12)")
			(pinfunction "Y3")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "unconnected-(U1-Y2-Pad13)")
			(pinfunction "Y2")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "unconnected-(U1-Y1-Pad14)")
			(pinfunction "Y1")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "unconnected-(U1-Y0-Pad15)")
			(pinfunction "Y0")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_1206"
		(layer "F.Cu")
		(at 157.7 92.124999 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -0.000001 1.3 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47u"
			(at -1.218275 1.31639 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/TDK_MLCC_Cxxxx.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 47UF 25V X5R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C3216X5R1E476M160DC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475001 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475001 0 90)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 179.95 88.025 180)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2.000001 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2.000001 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0 180)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSOP32-dual"
		(layer "F.Cu")
		(at 149.199 92.925 180)
		(descr "Module CMS TSOP 32 pins")
		(tags "CMS TSOP")
		(property "Reference" "U4"
			(at -0.05 -1.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AS6C4008"
			(at -0.05 1.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/AS6C4008.pdf"
			(at 3.05 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC SRAM 512Kx8 PARALLEL STSOP-32"
			(at 3.05 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AS6C4008-55STIN"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*11.305x20.495mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -6.500001 -3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/A1")
			(pinfunction "A11")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -6.5 -3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/A2")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -6.5 -2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/A3")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -6.5 -2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/A6")
			(pinfunction "A13")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -6.5 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/~{WR}")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -6.500001 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/A18_CE2")
			(pinfunction "A17")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -6.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/A4")
			(pinfunction "A15")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -6.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -6.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/A17")
			(pinfunction "A18")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -6.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/A5")
			(pinfunction "A16")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -6.500001 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/A9")
			(pinfunction "A14")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -6.5 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/A7")
			(pinfunction "A12")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -6.5 2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A8")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -6.5 2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/A12")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -6.5 3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/A11")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -6.500001 3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/A10")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 6.500001 3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 13 3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 6.5 3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 13 3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 6.5 2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 13 2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 6.5 2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/A16")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 13 2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/A16")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 6.5 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 13 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 6.500001 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 13 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 6.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 13 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 6.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 13 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 6.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 13 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 6.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 13 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 6.500001 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 13 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 6.5 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 13 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 6.5 -2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 13 -2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 6.5 -2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/~{CE}")
			(pinfunction "~{CE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 13 -2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/~{CE}")
			(pinfunction "~{CE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 6.5 -3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A0")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 13 -3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A0")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 6.500001 -3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/~{RD}")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 13 -3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/~{RD}")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP32_8x14.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP32_8X20.step"
			(offset
				(xyz 3.25 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP-I-32_11.8x8mm_P0.5mm.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP-I-32_18.4x8mm_P0.5mm.step"
			(hide yes)
			(offset
				(xyz 3.25 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 123.95 88.025)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 146.225 104.25 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at -1.8 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CE2"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(zone_connect 1)
		(attr smd exclude_from_pos_files exclude_from_bom dnp allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 48 "/BYTE")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 31 "/A18_CE2")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/Solder_Bridge_1.5x2.3.step"
			(offset
				(xyz -1.15 -0.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "000_LOCAL:C_1206"
		(layer "F.Cu")
		(at 144.175 101.175)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -2.95 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47u"
			(at 0 -1.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/TDK_MLCC_Cxxxx.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 47UF 25V X5R 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C3216X5R1E476M160DC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 139.000001 101.175 180)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R2"
			(at 0.000001 2.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47k"
			(at 0.000001 1.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/sei-rmcf_rmcp.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RES 47K OHM 1% 1/8W 0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RMCF0805FT47K0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 21 "/RAMRST")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:MiniNDP_Cover_THIN"
		(layer "F.Cu")
		(at 151.95 103.025)
		(property "Reference" "N1"
			(at 0 -0.381 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "MiniNDP_Cover_THIN"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "../COVER/MiniNDP_Cover.scad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Snap cover for MiniNDP, thin version for CR2016"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MiniNDP_Cover_THIN.stl"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Enclosure* Housing*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/MiniNDP_Cover_THIN.step"
			(offset
				(xyz 0 0 -1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 123.95 118.025)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSSOP-16"
		(layer "F.Cu")
		(at 152.6 100.6 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at -1.25 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC4040"
			(at 1 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/4040.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC BINARY COUNTER 12-BIT 16SO"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC4040PW,118"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16* SO*16*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U2-Q11-Pad1)")
			(pinfunction "Q11")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/A5")
			(pinfunction "Q5")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/A4")
			(pinfunction "Q4")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/A6")
			(pinfunction "Q6")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/A3")
			(pinfunction "Q3")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/A2")
			(pinfunction "Q2")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/A1")
			(pinfunction "Q1")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A0")
			(pinfunction "Q0")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/BYTE")
			(pinfunction "CLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "Reset")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A8")
			(pinfunction "Q8")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/A7")
			(pinfunction "Q7")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/A9")
			(pinfunction "Q9")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "unconnected-(U2-Q10-Pad15)")
			(pinfunction "Q10")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 125.725 92.375 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C3"
			(at -0.85 1.075 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0.5 1.075 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSSOP-20"
		(layer "F.Cu")
		(at 130.275 94.575 90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at -1.25 -1.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC573"
			(at 1 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/HC573.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-bit Latch 3-state outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC573PW,118"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "D0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "D1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "D2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 -0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "D3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "D4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "D5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "D6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -2.9 2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "D7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -2.9 2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "LE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/A17")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/A16")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 2.9 -0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/A12")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 2.9 -1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/A11")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 2.9 -2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/A10")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 2.9 -2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-20.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 179.95 118.025 90)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2.000001 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2.000001 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0 90)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSSOP-8_3x3mm_P0.65mm"
		(layer "F.Cu")
		(at 141.825 104.25)
		(descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
		(tags "SSOP 0.65")
		(property "Reference" "U6"
			(at 0 0.515 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2G00"
			(at 0 2.55 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/2G00.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP* VSSOP*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(clearance 0.2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.875 -0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RAMRST")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.875 -0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RAMRST")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.875 0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/~{CE}")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.875 0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 1.875 0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/BYTE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 1.875 0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U6-Pad6)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 1.875 -0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U6-Pad6)")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 1.875 -0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-8.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 137.425 104.25 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 1.8 0.001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~{CE1}"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(zone_connect 1)
		(attr smd exclude_from_pos_files exclude_from_bom dnp allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 21 "/RAMRST")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "/~{CE}")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/Solder_Bridge_1.5x2.3.step"
			(offset
				(xyz -1.15 -0.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 149.95 109.625 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C2"
			(at 2.05 0.55 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.05 -0.65 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 146.87 109.375 -90)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U5"
			(at 0.04 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1G79"
			(at 2 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/LVC1G79.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC FF D-TYPE SNGL 1BIT 5TSSOP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74LVC1G79GW,125"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT* SG*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/BUS_A10")
			(pinfunction "D")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -0.949999 0 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "C")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/A18_CE2")
			(pinfunction "Q")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-353_SC-70-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 151.1 104.375)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C4"
			(at 3.85 -0.005239 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.6 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(zone_connect 0)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Keystone_3028_3034_bkw"
		(layer "F.Cu")
		(at 170.225 99.475 90)
		(descr "Keystone 3034 SMD battery holder for 2020, 2025 and 2032 coincell batteries. http://www.keyelco.com/product-pdf.cfm?p=798")
		(tags "Keystone type 3034 coin cell retainer")
		(property "Reference" "BT1"
			(at -8.75 -5.6 135)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Keystone_3028"
			(at 9.65 0.55 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/Keystone_3034.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "BATTERY RETAINER COIN 20MM x 1.6MM SMT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "Keystone_3028"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(zone_connect 2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -11.275 -2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -11.275 0)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -11.275 0 90)
			(size 1.85 7.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -11.275 2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 -2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 0)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at 11.275 0 90)
			(size 1.85 7.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -9.007825 -3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -9.007825 3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -3.731163 -9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -3.731163 9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd circle
			(at 0 0 90)
			(size 18 18)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 3.731163 -9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 3.731163 9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 9.007825 -3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 9.007825 3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_holder_Keystone_3034.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_holder_BAT-HLD-002-SMT.STEP"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_holder_Keystone_3028.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_blank.step"
			(offset
				(xyz 0 0 1.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_blank.step"
			(hide yes)
			(offset
				(xyz 0 0 1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_blank.step"
			(hide yes)
			(offset
				(xyz 0 0 3.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SOT-23"
		(layer "F.Cu")
		(at 160.65 88.875 -90)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "DA1"
			(at 0.025 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BAV70"
			(at -1.125 1.7 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/BAV70.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DIODE ARRAY GP 75V 150MA SOT23-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "BAV70-7-F"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -6.15 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "+BATT")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 1.15 0 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:IDC-Header_2x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 127.82 113.755 -90)
		(descr "Through hole IDC box header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x20 2.54mm double row")
		(property "Reference" "J1"
			(at -0.42 2.61 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x20_Odd_Even"
			(at 1.27 -24.003 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "datasheets/2x20_male_boxed.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CONN HEADER VERT 40POS 2.54MM"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "302-S401"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.905 -24.13 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 3 "VBUS")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VBUS")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at 2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/AD1")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at 2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/AD0")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/AD3")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at 2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/AD2")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/AD5")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 2.54 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/AD4")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 0 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/AD7")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at 2.54 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/AD6")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 0 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/BUS_A9")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at 2.54 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/BUS_A8")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 0 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(J1-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 2.54 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/BUS_A10")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 0 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(J1-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at 2.54 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(J1-Pin_18-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at 0 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(J1-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at 2.54 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(J1-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole circle
			(at 0 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole circle
			(at 2.54 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole circle
			(at 0 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/~{WR}")
			(pinfunction "Pin_23")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole circle
			(at 2.54 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/~{RD}")
			(pinfunction "Pin_24")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole circle
			(at 0 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(J1-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole circle
			(at 2.54 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J1-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole circle
			(at 0 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(J1-Pin_27-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole circle
			(at 2.54 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J1-Pin_28-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" thru_hole circle
			(at 0 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/~{Y0}")
			(pinfunction "Pin_29")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" thru_hole circle
			(at 2.54 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J1-Pin_30-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" thru_hole circle
			(at 0 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J1-Pin_31-Pad31)")
			(pinfunction "Pin_31")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" thru_hole circle
			(at 2.54 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/(A)")
			(pinfunction "Pin_32")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" thru_hole circle
			(at 0 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(J1-Pin_33-Pad33)")
			(pinfunction "Pin_33")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" thru_hole circle
			(at 2.54 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(J1-Pin_34-Pad34)")
			(pinfunction "Pin_34")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" thru_hole circle
			(at 0 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_35")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" thru_hole circle
			(at 2.54 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_36")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" thru_hole circle
			(at 0 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J1-Pin_37-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" thru_hole circle
			(at 2.54 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/RAMRST")
			(pinfunction "Pin_38")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" thru_hole circle
			(at 0 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J1-Pin_39-Pad39)")
			(pinfunction "Pin_39")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" thru_hole circle
			(at 2.54 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(J1-Pin_40-Pad40)")
			(pinfunction "Pin_40")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/IDC-Header_2x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 121.95 88.025)
		(mid 122.535786 86.610786)
		(end 123.95 86.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.95 118.025)
		(end 121.95 88.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.95 86.025)
		(end 179.95 86.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.95 120.025001)
		(mid 122.535786 119.439214)
		(end 121.949999 118.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.95 86.024999)
		(mid 181.364214 86.610786)
		(end 181.950001 88.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.95 120.025)
		(end 123.95 120.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.95 88.025)
		(end 181.95 118.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.950001 118.025)
		(mid 181.364214 119.439214)
		(end 179.95 120.025001)
		(layer "Edge.Cuts")
	)
	(gr_text "128k 256k:\nDNP U5 U6\nClose JP1 JP2"
		(at 123.275 99.275 0)
		(layer "F.SilkS")
	)
	(gr_text "512k:\nPopulate U5 U6\nOpen JP1 JP2"
		(at 123.275 103.875 0)
		(layer "F.SilkS")
	)
	(gr_text "CR2016 / CR2012"
		(at 180.9 99.475 90)
		(layer "F.SilkS")
	)
	(gr_text "${TITLE} - ${REVISION} - RAM DISK for TANDY 102/200"
		(at 151.95 118.575 0)
		(layer "F.SilkS")
	)
	(gr_text "128k"
		(at 126.875 110.15 0)
		(layer "F.SilkS")
	)
	(gr_text "256k"
		(at 133.675 110.15 0)
		(layer "F.SilkS")
	)
	(gr_text "512k"
		(at 140.475 110.15 0)
		(layer "F.SilkS")
	)
	(gr_text "BASIC to bootstrap RAMxxx.CO previously saved as the first file in bank 0"
		(at 151.95 95.086 0)
		(layer "B.SilkS")
	)
	(gr_text "128k 256k 512k\nRAM DISK for\nTANDY 102/200"
		(at 132.519 88.863 0)
		(layer "B.SilkS")
	)
	(gr_text "BATTERY\nCR2016\nCR2012"
		(at 181.45 109.525 90)
		(layer "B.SilkS")
	)
	(gr_text "${COMMENT1} - ${REVISION}"
		(at 151.95 92.775 0)
		(layer "B.SilkS")
	)
	(gr_text "${TITLE}"
		(at 151.95 88.863 0)
		(layer "B.SilkS")
	)
	(gr_text "bank 0:P=129  1:P=133\nblock 0-255: OUT P,N\nread byte:   D=INP(131)\nwrite byte:  OUT 131,D"
		(at 181.18 88.915 0)
		(layer "B.SilkS")
	)
	(gr_text "100 1 CLEAR0,61558:T=61558:E=62957:OUT129,2\n200 1 CLEAR0,59715:T=59715:E=61101:OUT129,2\n    2 FORA=0TO15:N=INP(131):NEXT:FORA=TTOE\n    3 POKEA,INP(131):IFA=T+1007THENOUT129,1\n    4 ?{dblquote}.{dblquote};:NEXT:SAVEM{dblquote}RAMDSK{dblquote},T,E,T"
		(at 180.6 97.175 0)
		(layer "B.SilkS")
	)
	(gr_text "Use ENIG copper finish\nfor gold battery contact.\n"
		(at 169.7 85.025 0)
		(layer "Eco1.User")
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 91.075) (xy 136.713185 91.077179) (xy 136.618197 91.077612) (xy 136.577507 91.063237)
				(xy 136.552701 91.030709) (xy 136.198 91.175) (xy 136.552701 91.319291) (xy 136.58249 91.283776)
				(xy 136.641061 91.270071) (xy 136.713185 91.272822) (xy 136.749 91.275)
			)
		)
	)
	(zone
		(net 65)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.699263 101.621127) (xy 154.733118 101.62543) (xy 154.848578 101.646893) (xy 154.895588 101.671959)
				(xy 154.917952 101.712884) (xy 155.500959 101.575281) (xy 154.9875 101.4) (xy 154.946698 101.43587)
				(xy 154.87992 101.446877) (xy 154.781302 101.433979) (xy 154.755609 101.429229)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.927935 96.754322) (xy 129.92392 96.775362) (xy 129.904068 96.842448) (xy 129.879411 96.868523)
				(xy 129.838052 96.879863) (xy 129.949761 97.47597) (xy 130.125 96.9625) (xy 130.10568 96.943163)
				(xy 130.096257 96.921202) (xy 130.099831 96.867491) (xy 130.112581 96.830168) (xy 130.122122 96.802187)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30157)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.70965 95.824994) (xy 135.730355 95.816164) (xy 135.806578 95.791228) (xy 135.844266 95.796066)
				(xy 135.874 95.825) (xy 136.199866 95.6745) (xy 135.805513 95.570094) (xy 135.786145 95.601003)
				(xy 135.725323 95.625647) (xy 135.669027 95.637729) (xy 135.609651 95.65179)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.333214 112.247847) (xy 137.398623 112.341158) (xy 137.446349 112.426975) (xy 137.476045 112.500419)
				(xy 137.493374 112.569499) (xy 137.496249 112.696142) (xy 137.461851 112.827437) (xy 137.362604 113.032639)
				(xy 137.243159 113.27607) (xy 137.189262 113.421896) (xy 137.146333 113.589173) (xy 137.980608 113.755793)
				(xy 138.452235 113.048251) (xy 138.082372 112.789707) (xy 137.95939 112.687203) (xy 137.853291 112.580834)
				(xy 137.648144 112.329911) (xy 137.559414 112.214253) (xy 137.491885 112.126096)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.804766 109.870651) (xy 158.747751 109.853665) (xy 158.647697 109.821345) (xy 158.610899 109.797487)
				(xy 158.595703 109.765902) (xy 157.9991 109.874567) (xy 157.99307 110.05) (xy 158.127645 110.02075)
				(xy 158.254568 110.002958) (xy 158.373371 109.996003) (xy 158.482987 109.999316) (xy 158.580861 110.011939)
				(xy 158.668467 110.033252) (xy 158.71799 110.050844)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.789388 107.843879) (xy 158.755309 107.84157) (xy 158.635621 107.826422) (xy 158.584233 107.803422)
				(xy 158.554828 107.76257) (xy 157.999013 107.924844) (xy 158.545985 108.093339) (xy 158.558725 108.069096)
				(xy 158.577764 108.052076) (xy 158.636512 108.034337) (xy 158.737959 108.039087) (xy 158.758093 108.041415)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.65 92.45) (xy 132.649499 92.424648) (xy 132.655524 92.306364) (xy 132.676166 92.253302)
				(xy 132.718339 92.220985) (xy 132.55 91.674) (xy 132.381661 92.220985) (xy 132.423649 92.253029)
				(xy 132.446245 92.315788) (xy 132.450501 92.424647) (xy 132.45 92.45)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 95.575) (xy 136.713185 95.577179) (xy 136.618197 95.577612) (xy 136.577507 95.563237)
				(xy 136.552701 95.530709) (xy 136.198 95.675) (xy 136.552701 95.819291) (xy 136.58249 95.783776)
				(xy 136.641061 95.770071) (xy 136.713185 95.772822) (xy 136.749 95.775)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.62713 96.724603) (xy 128.622978 96.749363) (xy 128.601868 96.833113) (xy 128.576673 96.866145)
				(xy 128.53513 96.880444) (xy 128.649793 97.475978) (xy 128.825 96.9625) (xy 128.796776 96.922019)
				(xy 128.797046 96.860665) (xy 128.813128 96.800258) (xy 128.822759 96.766186)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 96.575) (xy 136.713185 96.577179) (xy 136.618197 96.577612) (xy 136.577507 96.563237)
				(xy 136.552701 96.530709) (xy 136.198 96.675) (xy 136.552701 96.819291) (xy 136.58249 96.783776)
				(xy 136.641061 96.770071) (xy 136.713185 96.772822) (xy 136.749 96.775)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.145196 98.875) (xy 149.065664 98.870332) (xy 149.005069 98.857658) (xy 148.902813 98.809439)
				(xy 148.821184 98.766714) (xy 148.698773 98.729804) (xy 148.649 98.975) (xy 148.698773 99.220196)
				(xy 148.835415 99.176905) (xy 148.902813 99.140561) (xy 148.997709 99.094647) (xy 149.060872 99.080319)
				(xy 149.145196 99.075)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.621945 90.882555) (xy 128.616918 90.91522) (xy 128.593893 91.021782) (xy 128.568467 91.064052)
				(xy 128.527824 91.082456) (xy 128.649793 91.675978) (xy 128.825 91.1625) (xy 128.795211 91.12279)
				(xy 128.790354 91.05533) (xy 128.809221 90.959635) (xy 128.817574 90.924137)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 96.775) (xy 142.184814 96.772822) (xy 142.279802 96.772388) (xy 142.320492 96.786763)
				(xy 142.345298 96.819291) (xy 142.699999 96.675) (xy 142.345298 96.530709) (xy 142.31551 96.566224)
				(xy 142.25694 96.579929) (xy 142.184814 96.577179) (xy 142.148999 96.575)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30160)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.759156 93.789486) (xy 135.775369 93.784624) (xy 135.811925 93.77869) (xy 135.829822 93.790038)
				(xy 135.845299 93.819291) (xy 136.199991 93.67487) (xy 135.835577 93.537204) (xy 135.823555 93.566429)
				(xy 135.807072 93.582958) (xy 135.76635 93.59173) (xy 135.754273 93.591215) (xy 135.733054 93.591197)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 94.075) (xy 136.713185 94.077179) (xy 136.618197 94.077612) (xy 136.577507 94.063237)
				(xy 136.552701 94.030709) (xy 136.198 94.175) (xy 136.552701 94.319291) (xy 136.58249 94.283776)
				(xy 136.641061 94.270071) (xy 136.713185 94.272822) (xy 136.749 94.275)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.914103 90.877595) (xy 129.90884 90.912697) (xy 129.885888 91.023127) (xy 129.860746 91.067226)
				(xy 129.82065 91.087249) (xy 129.949742 91.675965) (xy 130.125 91.1625) (xy 130.091931 91.122299)
				(xy 130.084122 91.055926) (xy 130.100868 90.958414) (xy 130.107287 90.929361)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 90.275) (xy 135.684815 90.272822) (xy 135.779803 90.272388) (xy 135.820493 90.286763)
				(xy 135.845299 90.319291) (xy 136.2 90.175) (xy 135.845299 90.030709) (xy 135.815511 90.066224)
				(xy 135.756941 90.079929) (xy 135.684815 90.077179) (xy 135.649 90.075)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 99.525) (xy 150.449647 99.525501) (xy 150.331363 99.519476) (xy 150.278301 99.498834)
				(xy 150.245985 99.456661) (xy 149.699 99.625) (xy 150.245985 99.793339) (xy 150.278029 99.751351)
				(xy 150.340788 99.728755) (xy 150.449648 99.724499) (xy 150.475 99.725)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.35 98.25) (xy 131.349499 98.224648) (xy 131.355524 98.106364) (xy 131.376166 98.053302)
				(xy 131.418339 98.020985) (xy 131.25 97.474) (xy 131.081661 98.020985) (xy 131.123649 98.053029)
				(xy 131.146245 98.115788) (xy 131.150501 98.224647) (xy 131.15 98.25)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.425 106.125) (xy 151.491579 106.115878) (xy 151.604554 106.103745) (xy 151.653453 106.115592)
				(xy 151.6875 106.15) (xy 152.201 105.975) (xy 151.6875 105.8) (xy 151.649436 105.836332) (xy 151.585856 105.846559)
				(xy 151.491579 105.834122) (xy 151.425 105.825)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.65 98.25) (xy 132.649499 98.224648) (xy 132.655524 98.106364) (xy 132.676166 98.053302)
				(xy 132.718339 98.020985) (xy 132.55 97.474) (xy 132.381661 98.020985) (xy 132.423649 98.053029)
				(xy 132.446245 98.115788) (xy 132.450501 98.224647) (xy 132.45 98.25)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.260325 90.878569) (xy 129.256297 90.910165) (xy 129.234946 91.022415) (xy 129.209609 91.067952)
				(xy 129.16803 91.089) (xy 129.299761 91.67597) (xy 129.475 91.1625) (xy 129.442141 91.122121) (xy 129.433735 91.054439)
				(xy 129.448299 90.958366) (xy 129.454512 90.926432)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.551037 90.871728) (xy 130.546224 90.907951) (xy 130.524262 91.024625) (xy 130.499412 91.072025)
				(xy 130.45928 91.094846) (xy 130.599691 91.675951) (xy 130.775 91.1625) (xy 130.737224 91.121482)
				(xy 130.724814 91.055468) (xy 130.737292 90.954703) (xy 130.741246 90.933532)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 91.575) (xy 136.713185 91.577179) (xy 136.618197 91.577612) (xy 136.577507 91.563237)
				(xy 136.552701 91.530709) (xy 136.198 91.675) (xy 136.552701 91.819291) (xy 136.58249 91.783776)
				(xy 136.641061 91.770071) (xy 136.713185 91.772822) (xy 136.749 91.775)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.857517 96.666538) (xy 131.849729 96.710724) (xy 131.82425 96.825832) (xy 131.799627 96.871387)
				(xy 131.762269 96.892849) (xy 131.899618 97.475923) (xy 132.075 96.9625) (xy 132.035419 96.921458)
				(xy 132.023247 96.858153) (xy 132.039074 96.756659) (xy 132.042291 96.743076)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30148)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.85 103.525) (xy 139.848438 103.579833) (xy 139.8375 103.645963) (xy 139.807813 103.701611)
				(xy 139.783008 103.718699) (xy 139.75 103.725) (xy 139.95 103.926) (xy 140.15 103.725) (xy 140.121082 103.720289)
				(xy 140.098357 103.707312) (xy 140.066791 103.659045) (xy 140.051263 103.575467) (xy 140.05 103.525)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 94.775) (xy 142.184815 94.772822) (xy 142.279803 94.772388) (xy 142.320493 94.786763)
				(xy 142.345299 94.819291) (xy 142.7 94.675) (xy 142.345299 94.530709) (xy 142.315511 94.566224)
				(xy 142.256941 94.579929) (xy 142.184815 94.577179) (xy 142.149 94.575)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.703392 102.271617) (xy 154.735956 102.275558) (xy 154.849349 102.296209) (xy 154.895598 102.321153)
				(xy 154.91761 102.362372) (xy 155.50097 102.225239) (xy 154.9875 102.05) (xy 154.946878 102.084997)
				(xy 154.87937 102.095611) (xy 154.779428 102.082537) (xy 154.751252 102.077429)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.794454 92.806282) (xy 158.65055 92.921079) (xy 158.559685 92.973781) (xy 158.458497 93.020193)
				(xy 158.353155 93.05702) (xy 158.240445 93.084859) (xy 158.130082 93.101276) (xy 158.01505 93.107311)
				(xy 157.905071 93.102541) (xy 157.792427 93.086776) (xy 157.686133 93.061451) (xy 157.578613 93.025)
				(xy 157.699293 93.600707) (xy 158.6 93.828975) (xy 158.618666 93.754957) (xy 158.682411 93.663497)
				(xy 158.811987 93.543077) (xy 159.006531 93.396994) (xy 159.126809 93.308517) (xy 159.218718 93.230546)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.272175 96.792462) (xy 129.269719 96.806705) (xy 129.253701 96.853996) (xy 129.22964 96.871999)
				(xy 129.18678 96.880116) (xy 129.299778 97.475974) (xy 129.475 96.9625) (xy 129.45412 96.941465)
				(xy 129.445353 96.919986) (xy 129.452104 96.87532) (xy 129.458493 96.860071) (xy 129.46716 96.836967)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 96.075) (xy 136.713185 96.077179) (xy 136.618197 96.077612) (xy 136.577507 96.063237)
				(xy 136.552701 96.030709) (xy 136.198 96.175) (xy 136.552701 96.319291) (xy 136.58249 96.283776)
				(xy 136.641061 96.270071) (xy 136.713185 96.272822) (xy 136.749 96.275)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.7 102.870284) (xy 137.67999 102.950224) (xy 137.653541 102.993081) (xy 137.616104 103.032594)
				(xy 137.572421 103.063067) (xy 137.519604 103.085852) (xy 137.464191 103.097859) (xy 137.401353 103.100012)
				(xy 137.401111 103.1) (xy 137.425 103.601) (xy 137.925924 103.172459) (xy 137.90057 103.142481)
				(xy 137.889309 103.067471) (xy 137.895563 102.941431) (xy 137.9 102.870284)
			)
		)
	)
	(zone
		(net 42)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.629437 88.025) (xy 169.686573 88.029847) (xy 169.729039 88.043773) (xy 169.776648 88.088042)
				(xy 169.804283 88.164276) (xy 169.81299 88.205253) (xy 169.838633 88.309633) (xy 169.892412 88.422228)
				(xy 170.226 88.2) (xy 170.447228 87.867412) (xy 170.260683 87.724246) (xy 170.168865 87.639944)
				(xy 170.069222 87.550559) (xy 169.96338 87.482872) (xy 169.900036 87.458135) (xy 169.825424 87.439985)
				(xy 169.629437 87.425)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.246923 93.325) (xy 156.362866 93.344604) (xy 156.432807 93.371798) (xy 156.503527 93.410127)
				(xy 156.572175 93.458987) (xy 156.63643 93.5181) (xy 156.689385 93.581107) (xy 156.734455 93.652122)
				(xy 156.766613 93.722598) (xy 156.789314 93.799078) (xy 156.802262 93.936373) (xy 157.701 93.6)
				(xy 157.78331 93.025) (xy 157.485926 93.053336) (xy 157.080535 93.056091) (xy 156.661597 93.039381)
				(xy 156.246923 93.025)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30145)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.05 103.675) (xy 140.051563 103.620167) (xy 140.0625 103.554037) (xy 140.092188 103.498389)
				(xy 140.116992 103.481301) (xy 140.15 103.475) (xy 139.95 103.274) (xy 139.75 103.475) (xy 139.778918 103.479711)
				(xy 139.801643 103.492688) (xy 139.833209 103.540955) (xy 139.848737 103.624533) (xy 139.85 103.675)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 96.275) (xy 142.184815 96.272822) (xy 142.279803 96.272388) (xy 142.320493 96.286763)
				(xy 142.345299 96.319291) (xy 142.7 96.175) (xy 142.345299 96.030709) (xy 142.315511 96.066224)
				(xy 142.256941 96.079929) (xy 142.184815 96.077179) (xy 142.149 96.075)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30120)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 89.275) (xy 135.684815 89.272822) (xy 135.779803 89.272388) (xy 135.820493 89.286763)
				(xy 135.845299 89.319291) (xy 136.2 89.175) (xy 135.845299 89.030709) (xy 135.815511 89.066224)
				(xy 135.756941 89.079929) (xy 135.684815 89.077179) (xy 135.649 89.075)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.595569 115.11823) (xy 146.54227 115.212007) (xy 146.488081 115.286669) (xy 146.437351 115.339966)
				(xy 146.385152 115.380553) (xy 146.276726 115.429387) (xy 146.145393 115.447516) (xy 145.954793 115.440847)
				(xy 145.717187 115.432204) (xy 145.581909 115.439538) (xy 145.434173 115.461333) (xy 145.599546 116.29589)
				(xy 146.433667 116.460827) (xy 146.5056 116.030791) (xy 146.534645 115.84478) (xy 146.575975 115.6713)
				(xy 146.649159 115.472127) (xy 146.773767 115.209032)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.8 103.35) (xy 149.816778 103.638598) (xy 149.838829 104.035057) (xy 149.831195 104.234007)
				(xy 149.8 104.419343) (xy 150.2 104.376) (xy 150.472225 103.75) (xy 150.416971 103.745199) (xy 150.367869 103.731595)
				(xy 150.283973 103.680139) (xy 150.216906 103.596487) (xy 150.169171 103.481111) (xy 150.15 103.35)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.888773 90.863897) (xy 131.871153 90.923389) (xy 131.838126 91.026786) (xy 131.814189 91.06491)
				(xy 131.78288 91.080892) (xy 131.8995 91.675866) (xy 132.075 91.1625) (xy 132.051223 91.144507)
				(xy 132.036901 91.122345) (xy 132.030642 91.065405) (xy 132.058459 90.972567) (xy 132.061977 90.963897)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.6 99.030764) (xy 150.595292 99.113989) (xy 150.582338 99.179514) (xy 150.537978 99.27831)
				(xy 150.511952 99.318409) (xy 150.4538 99.416663) (xy 150.427548 99.482406) (xy 150.405764 99.566473)
				(xy 150.7 99.626) (xy 150.994236 99.566473) (xy 150.973493 99.485601) (xy 150.948581 99.421727)
				(xy 150.888048 99.318409) (xy 150.854617 99.265883) (xy 150.826536 99.206776) (xy 150.8072 99.131574)
				(xy 150.8 99.030764)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 90.575) (xy 136.713185 90.577179) (xy 136.618197 90.577612) (xy 136.577507 90.563237)
				(xy 136.552701 90.530709) (xy 136.198 90.675) (xy 136.552701 90.819291) (xy 136.58249 90.783776)
				(xy 136.641061 90.770071) (xy 136.713185 90.772822) (xy 136.749 90.775)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30121)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 90.775) (xy 155.184815 90.772822) (xy 155.279803 90.772388) (xy 155.320493 90.786763)
				(xy 155.345299 90.819291) (xy 155.7 90.675) (xy 155.345299 90.530709) (xy 155.315511 90.566224)
				(xy 155.256941 90.579929) (xy 155.184815 90.577179) (xy 155.149 90.575)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.976621 96.683719) (xy 127.971757 96.71513) (xy 127.948537 96.821044) (xy 127.922802 96.863066)
				(xy 127.881635 96.881139) (xy 127.999805 97.47598) (xy 128.175 96.9625) (xy 128.14694 96.922972)
				(xy 128.143751 96.854907) (xy 128.163325 96.761843) (xy 128.172777 96.722737)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.726233 115.209032) (xy 131.827416 115.418599) (xy 131.895461 115.585078) (xy 131.933667 115.70484)
				(xy 131.960003 115.816811) (xy 131.994399 116.030789) (xy 132.066333 116.460827) (xy 132.900454 116.29589)
				(xy 133.065827 115.461333) (xy 132.841017 115.433977) (xy 132.605491 115.437067) (xy 132.545207 115.440847)
				(xy 132.354794 115.447522) (xy 132.269461 115.439547) (xy 132.189473 115.41842) (xy 132.113904 115.379933)
				(xy 132.041825 115.319878) (xy 131.97231 115.234046) (xy 131.904431 115.11823)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.488969 106.953484) (xy 153.553536 106.848907) (xy 153.594085 106.768607) (xy 153.619204 106.710078)
				(xy 153.665606 106.607292) (xy 153.749441 106.466671) (xy 153.500555 106.299169) (xy 153.205764 106.358527)
				(xy 153.2466 106.491945) (xy 153.25882 106.521497) (xy 153.282693 106.583353) (xy 153.293117 106.642293)
				(xy 153.28157 106.707164) (xy 153.239529 106.786814)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30122)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 92.275) (xy 155.184815 92.272822) (xy 155.279803 92.272388) (xy 155.320493 92.286763)
				(xy 155.345299 92.319291) (xy 155.7 92.175) (xy 155.345299 92.030709) (xy 155.315511 92.066224)
				(xy 155.256941 92.079929) (xy 155.184815 92.077179) (xy 155.149 92.075)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30123)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 90.275) (xy 142.184815 90.272822) (xy 142.279803 90.272388) (xy 142.320493 90.286763)
				(xy 142.345299 90.319291) (xy 142.7 90.175) (xy 142.345299 90.030709) (xy 142.315511 90.066224)
				(xy 142.256941 90.079929) (xy 142.184815 90.077179) (xy 142.149 90.075)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.75 96.929804) (xy 154.745332 97.009336) (xy 154.732658 97.069931) (xy 154.684439 97.172186)
				(xy 154.641714 97.253815) (xy 154.604804 97.376227) (xy 154.85 97.426) (xy 155.095196 97.376227)
				(xy 155.051905 97.239584) (xy 155.015561 97.172187) (xy 154.969647 97.077291) (xy 154.955319 97.014128)
				(xy 154.95 96.929804)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.231596 99.480167) (xy 156.217154 99.483703) (xy 156.16607 99.495096) (xy 156.107889 99.500321)
				(xy 156.053176 99.488811) (xy 156.0125 99.45) (xy 155.499077 99.625382) (xy 156.08348 99.760739)
				(xy 156.105593 99.72257) (xy 156.166112 99.69331) (xy 156.263708 99.673007) (xy 156.308132 99.664942)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30124)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 91.275) (xy 142.184815 91.272822) (xy 142.279803 91.272388) (xy 142.320493 91.286763)
				(xy 142.345299 91.319291) (xy 142.7 91.175) (xy 142.345299 91.030709) (xy 142.315511 91.066224)
				(xy 142.256941 91.079929) (xy 142.184815 91.077179) (xy 142.149 91.075)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.902771 107.864095) (xy 146.890987 107.89596) (xy 146.833226 108.029525) (xy 146.791234 108.083246)
				(xy 146.766457 108.099594) (xy 146.738969 108.106173) (xy 146.869501 108.425867) (xy 147.07 108.446848)
				(xy 147.033134 108.319015) (xy 147.028346 108.174028) (xy 147.056659 108.020865) (xy 147.075975 107.964094)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.95 103.35) (xy 149.95018 103.379317) (xy 149.94891 103.497759) (xy 149.933912 103.630577)
				(xy 149.91684 103.691443) (xy 149.891026 103.742782) (xy 149.854699 103.780221) (xy 149.80609 103.799385)
				(xy 150.2 104.376) (xy 150.556016 103.759698) (xy 150.509439 103.75385) (xy 150.468679 103.739338)
				(xy 150.40048 103.686093) (xy 150.347047 103.597982) (xy 150.311061 103.472322) (xy 150.3 103.35)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.270867 91.654446) (xy 148.21793 91.594908) (xy 148.184045 91.543098) (xy 148.145835 91.436696)
				(xy 148.118326 91.348765) (xy 148.057867 91.236107) (xy 147.849293 91.374293) (xy 147.711107 91.582867)
				(xy 147.838338 91.648876) (xy 147.911696 91.670835) (xy 148.011264 91.705471) (xy 148.066059 91.740002)
				(xy 148.129446 91.795867)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30161)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.764206 91.789011) (xy 135.779546 91.784215) (xy 135.813426 91.778631) (xy 135.830266 91.790085)
				(xy 135.845299 91.819291) (xy 136.199991 91.67487) (xy 135.835958 91.53695) (xy 135.823695 91.56695)
				(xy 135.807252 91.583478) (xy 135.76788 91.591354) (xy 135.75835 91.590845) (xy 135.738105 91.590723)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.258757 112.635178) (xy 139.367208 112.750627) (xy 139.450509 112.854626) (xy 139.506487 112.940241)
				(xy 139.547915 113.021526) (xy 139.597111 113.178917) (xy 139.621684 113.378589) (xy 139.6259 113.436078)
				(xy 139.644556 113.651371) (xy 139.686333 113.920827) (xy 140.520707 113.755707) (xy 140.685827 112.921333)
				(xy 140.374143 112.875087) (xy 140.201078 112.8609) (xy 139.997533 112.841454) (xy 139.905092 112.823329)
				(xy 139.814338 112.794438) (xy 139.721869 112.750908) (xy 139.624287 112.688867) (xy 139.51819 112.604441)
				(xy 139.400178 112.493757)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.797923 112.363521) (xy 132.803423 112.469203) (xy 132.797979 112.558809) (xy 132.784001 112.629462)
				(xy 132.762179 112.6903) (xy 132.696913 112.791282) (xy 132.590077 112.89052) (xy 132.536581 112.932552)
				(xy 132.3691 113.073141) (xy 132.281061 113.166317) (xy 132.193251 113.282765) (xy 132.900098 113.755995)
				(xy 133.606749 113.282765) (xy 133.460094 113.093278) (xy 133.291299 112.927773) (xy 133.185983 112.827279)
				(xy 133.099963 112.714588) (xy 133.06506 112.645176) (xy 133.036026 112.562525) (xy 133.013209 112.463238)
				(xy 132.996959 112.343917)
			)
		)
	)
	(zone
		(net 47)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.241124 100.133942) (xy 156.221359 100.137768) (xy 156.108128 100.150448) (xy 156.052865 100.137889)
				(xy 156.0125 100.1) (xy 155.499049 100.275309) (xy 156.080067 100.415848) (xy 156.103046 100.375936)
				(xy 156.162394 100.347577) (xy 156.265295 100.329364) (xy 156.302927 100.324152)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.553363 103.922572) (xy 140.529956 103.916097) (xy 140.41167 103.87428) (xy 140.363215 103.837659)
				(xy 140.348238 103.81394) (xy 140.341933 103.786051) (xy 139.949041 103.924719) (xy 140.25 104.125)
				(xy 140.292867 104.09043) (xy 140.359951 104.082717) (xy 140.480394 104.109431) (xy 140.497017 104.11447)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30125)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149001 91.775) (xy 155.184816 91.772822) (xy 155.279804 91.772388) (xy 155.320494 91.786763)
				(xy 155.3453 91.819291) (xy 155.700001 91.675) (xy 155.3453 91.530709) (xy 155.315512 91.566224)
				(xy 155.256942 91.579929) (xy 155.184816 91.577179) (xy 155.149001 91.575)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30126)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 95.275) (xy 142.184815 95.272822) (xy 142.279803 95.272388) (xy 142.320493 95.286763)
				(xy 142.345299 95.319291) (xy 142.7 95.175) (xy 142.345299 95.030709) (xy 142.315511 95.066224)
				(xy 142.256941 95.079929) (xy 142.184815 95.077179) (xy 142.149 95.075)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.030967 112.127185) (xy 163.066701 112.239644) (xy 163.088232 112.34027) (xy 163.096696 112.425958)
				(xy 163.094685 112.503643) (xy 163.063528 112.640288) (xy 162.996112 112.771695) (xy 162.877673 112.93136)
				(xy 162.782286 113.055714) (xy 162.689101 113.199672) (xy 162.607367 113.373927) (xy 162.546333 113.589173)
				(xy 163.380342 113.755939) (xy 164.086749 113.282765) (xy 163.887755 113.015076) (xy 163.672596 112.782951)
				(xy 163.551763 112.656848) (xy 163.439654 112.514582) (xy 163.330593 112.325459) (xy 163.218905 112.058785)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30127)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 95.775) (xy 142.184815 95.772822) (xy 142.279803 95.772388) (xy 142.320493 95.786763)
				(xy 142.345299 95.819291) (xy 142.7 95.675) (xy 142.345299 95.530709) (xy 142.315511 95.566224)
				(xy 142.256941 95.579929) (xy 142.184815 95.577179) (xy 142.149 95.575)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.425 103.825) (xy 138.33057 103.804242) (xy 138.280369 103.777598) (xy 138.234538 103.739362)
				(xy 138.203806 103.699256) (xy 138.181836 103.650781) (xy 138.170722 103.579595) (xy 137.424 103.6)
				(xy 138.175 104.1) (xy 138.179739 104.077678) (xy 138.192914 104.06019) (xy 138.245854 104.035383)
				(xy 138.348604 104.024532) (xy 138.402557 104.024744) (xy 138.425 104.025)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.209935 90.866506) (xy 131.202273 90.909832) (xy 131.176621 91.024863) (xy 131.151799 91.070365)
				(xy 131.114145 91.091595) (xy 131.249618 91.675923) (xy 131.425 91.1625) (xy 131.386322 91.121545)
				(xy 131.374938 91.058144) (xy 131.391059 90.958368) (xy 131.394711 90.943038)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30128)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 90.775) (xy 135.684815 90.772822) (xy 135.779803 90.772388) (xy 135.820493 90.786763)
				(xy 135.845299 90.819291) (xy 136.2 90.675) (xy 135.845299 90.530709) (xy 135.815511 90.566224)
				(xy 135.756941 90.579929) (xy 135.684815 90.577179) (xy 135.649 90.575)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.465132 108.986535) (xy 147.481172 108.949424) (xy 147.545236 108.818896) (xy 147.588584 108.767479)
				(xy 147.613223 108.752041) (xy 147.63989 108.746043) (xy 147.520555 108.424169) (xy 147.32 108.39935)
				(xy 147.353862 108.527854) (xy 147.354641 108.670534) (xy 147.32179 108.817809) (xy 147.298838 108.875424)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.348942 105.325) (xy 145.448194 105.319115) (xy 145.619077 105.311352) (xy 145.694919 105.319506)
				(xy 145.750516 105.342805) (xy 146.226 104.9) (xy 145.479278 104.91009) (xy 145.49252 104.958203)
				(xy 145.494311 104.999478) (xy 145.47144 105.062846) (xy 145.420021 105.106378) (xy 145.348942 105.125)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/~{WR}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.66 112.071333) (xy 155.655052 112.229654) (xy 155.640415 112.362095) (xy 155.619459 112.462216)
				(xy 155.591276 112.548987) (xy 155.514771 112.695066) (xy 155.390958 112.853631) (xy 155.353288 112.897263)
				(xy 155.214244 113.06269) (xy 155.053251 113.282765) (xy 155.76 113.756) (xy 156.466749 113.282765)
				(xy 156.279056 113.029671) (xy 156.166712 112.897263) (xy 156.036535 112.739586) (xy 155.983985 112.661403)
				(xy 155.940242 112.576801) (xy 155.905637 112.480636) (xy 155.880506 112.367765) (xy 155.865182 112.233045)
				(xy 155.86 112.071333)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.925 99.075) (xy 148.950352 99.074499) (xy 149.068637 99.080524) (xy 149.121699 99.101166)
				(xy 149.154015 99.143339) (xy 149.701 98.975) (xy 149.154015 98.806661) (xy 149.121972 98.848649)
				(xy 149.059213 98.871245) (xy 148.950353 98.875501) (xy 148.925 98.875)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30129)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 91.775) (xy 142.184814 91.772822) (xy 142.279802 91.772388) (xy 142.320492 91.786763)
				(xy 142.345298 91.819291) (xy 142.699999 91.675) (xy 142.345298 91.530709) (xy 142.31551 91.566224)
				(xy 142.25694 91.579929) (xy 142.184814 91.577179) (xy 142.148999 91.575)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.105764 99.725) (xy 150.188989 99.729708) (xy 150.254514 99.742662) (xy 150.35331 99.787022)
				(xy 150.393409 99.813048) (xy 150.491663 99.8712) (xy 150.557406 99.897452) (xy 150.641473 99.919236)
				(xy 150.701 99.625) (xy 150.641473 99.330764) (xy 150.560601 99.351507) (xy 150.496727 99.376418)
				(xy 150.393409 99.436952) (xy 150.340883 99.470383) (xy 150.281776 99.498464) (xy 150.206574 99.5178)
				(xy 150.105764 99.525)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.3 105.125) (xy 144.292347 105.12501) (xy 144.226067 105.123681) (xy 144.149126 105.113665)
				(xy 144.080275 105.086223) (xy 144.054744 105.063235) (xy 144.038268 105.032612) (xy 143.699 105.225)
				(xy 144.038268 105.417388) (xy 144.072351 105.369506) (xy 144.138819 105.338862) (xy 144.244553 105.325508)
				(xy 144.292347 105.32499) (xy 144.3 105.325)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30130)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 89.775) (xy 142.184815 89.772822) (xy 142.279803 89.772388) (xy 142.320493 89.786763)
				(xy 142.345299 89.819291) (xy 142.7 89.675) (xy 142.345299 89.530709) (xy 142.315511 89.566224)
				(xy 142.256941 89.579929) (xy 142.184815 89.577179) (xy 142.149 89.575)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30131)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 90.275) (xy 155.184815 90.272822) (xy 155.279803 90.272388) (xy 155.320493 90.286763)
				(xy 155.345299 90.319291) (xy 155.7 90.175) (xy 155.345299 90.030709) (xy 155.315511 90.066224)
				(xy 155.256941 90.079929) (xy 155.184815 90.077179) (xy 155.149 90.075)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.425 90.675) (xy 125.435067 90.76466) (xy 125.447994 90.867352) (xy 125.445942 90.968009)
				(xy 125.433682 91.010682) (xy 125.410936 91.044576) (xy 125.375458 91.066935) (xy 125.325 91.075)
				(xy 125.725 91.476) (xy 126.125 91.075) (xy 126.084931 91.070206) (xy 126.053957 91.056651) (xy 126.016133 91.010261)
				(xy 126.000373 90.931465) (xy 126.009133 90.804439) (xy 126.014933 90.76466) (xy 126.025 90.675)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.929041 98.135776) (xy 148.98882 98.175964) (xy 149.068157 98.229666) (xy 149.093928 98.258164)
				(xy 149.1 98.286799) (xy 149.700755 98.325654) (xy 149.730816 98.15) (xy 149.598922 98.150997) (xy 149.476592 98.142104)
				(xy 149.367528 98.124414) (xy 149.269322 98.098288) (xy 149.187351 98.066298) (xy 149.116583 98.027598)
				(xy 149.060013 97.984626)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.75 98.25) (xy 128.749499 98.224648) (xy 128.755524 98.106364) (xy 128.776166 98.053302)
				(xy 128.818339 98.020985) (xy 128.65 97.474) (xy 128.481661 98.020985) (xy 128.523649 98.053029)
				(xy 128.546245 98.115788) (xy 128.550501 98.224647) (xy 128.55 98.25)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.55 101.275) (xy 141.673071 101.294413) (xy 141.754577 101.322505) (xy 141.837959 101.362109)
				(xy 141.915651 101.410429) (xy 141.986748 101.468164) (xy 142.039133 101.524425) (xy 142.081201 101.586726)
				(xy 142.106841 101.643832) (xy 142.121759 101.70476) (xy 142.125 101.75) (xy 142.701 101.175) (xy 142.125 100.6)
				(xy 142.106327 100.707634) (xy 142.05014 100.811329) (xy 141.953542 100.910817) (xy 141.816625 100.999121)
				(xy 141.656801 101.059915) (xy 141.55 101.075)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30132)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 92.275) (xy 142.184815 92.272822) (xy 142.279803 92.272388) (xy 142.320493 92.286763)
				(xy 142.345299 92.319291) (xy 142.7 92.175) (xy 142.345299 92.030709) (xy 142.315511 92.066224)
				(xy 142.256941 92.079929) (xy 142.184815 92.077179) (xy 142.149 92.075)
			)
		)
	)
	(zone
		(net 42)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.55 88.025) (xy 165.73273 88.045492) (xy 165.843943 88.073463) (xy 165.959109 88.113852)
				(xy 166.06268 88.161435) (xy 166.162034 88.219853) (xy 166.241233 88.278856) (xy 166.312487 88.346274)
				(xy 166.366069 88.411643) (xy 166.410559 88.483612) (xy 166.441497 88.553783) (xy 166.462932 88.629451)
				(xy 166.475 88.748724) (xy 170.226 88.2) (xy 166.70625 87.275) (xy 166.65534 87.332629) (xy 166.559547 87.380585)
				(xy 166.3989 87.417065) (xy 166.149188 87.435815) (xy 165.739077 87.429876) (xy 165.55 87.425)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.172396 115.034336) (xy 144.095605 114.863725) (xy 144.04099 114.718357) (xy 144.006104 114.598568)
				(xy 143.984039 114.490689) (xy 143.9638 114.269075) (xy 143.961275 114.202989) (xy 143.946205 113.942863)
				(xy 143.926874 113.781142) (xy 143.893667 113.589173) (xy 143.059567 113.7541) (xy 142.587765 114.461749)
				(xy 142.780483 114.56864) (xy 142.972483 114.63483) (xy 143.179142 114.670676) (xy 143.305873 114.682174)
				(xy 143.501583 114.703933) (xy 143.592664 114.725507) (xy 143.679625 114.760237) (xy 143.762763 114.812642)
				(xy 143.842374 114.887243) (xy 143.918755 114.98856) (xy 143.992202 115.121112)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.414617 104.648842) (xy 136.464282 104.659071) (xy 136.520288 104.680999) (xy 136.573644 104.713213)
				(xy 136.62092 104.756716) (xy 136.649746 104.7985) (xy 136.668671 104.847412) (xy 136.675 104.9)
				(xy 137.425984 104.900173) (xy 136.675 104.4) (xy 136.670275 104.422791) (xy 136.657201 104.439441)
				(xy 136.607526 104.458522) (xy 136.513043 104.458924) (xy 136.469484 104.45419) (xy 136.449347 104.451882)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30133)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 89.275) (xy 142.184814 89.272822) (xy 142.279802 89.272388) (xy 142.320492 89.286763)
				(xy 142.345298 89.319291) (xy 142.699999 89.175) (xy 142.345298 89.030709) (xy 142.31551 89.066224)
				(xy 142.25694 89.079929) (xy 142.184814 89.077179) (xy 142.148999 89.075)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30134)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 94.275) (xy 142.184814 94.272822) (xy 142.279802 94.272388) (xy 142.320492 94.286763)
				(xy 142.345298 94.319291) (xy 142.699999 94.175) (xy 142.345298 94.030709) (xy 142.31551 94.066224)
				(xy 142.25694 94.079929) (xy 142.184814 94.077179) (xy 142.148999 94.075)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.1 98.25) (xy 128.099499 98.224648) (xy 128.105524 98.106364) (xy 128.126166 98.053302) (xy 128.168339 98.020985)
				(xy 128 97.474) (xy 127.831661 98.020985) (xy 127.873649 98.053029) (xy 127.896245 98.115788) (xy 127.900501 98.224647)
				(xy 127.9 98.25)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/BUS_A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.802641 109.198699) (xy 158.758787 109.18971) (xy 158.651147 109.162771) (xy 158.609624 109.138028)
				(xy 158.591558 109.10135) (xy 157.999061 109.224658) (xy 158.5125 109.4) (xy 158.552499 109.36574)
				(xy 158.615323 109.358996) (xy 158.712904 109.380511) (xy 158.734239 109.386637)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.9 102.119236) (xy 143.904761 101.984041) (xy 143.918092 101.889009) (xy 143.943901 101.788694)
				(xy 143.994236 101.583527) (xy 143.7 101.524) (xy 143.405764 101.583527) (xy 143.456099 101.788696)
				(xy 143.488028 101.922951) (xy 143.5 102.119236)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.75 91.3) (xy 126.616315 91.291799) (xy 126.537262 91.277946) (xy 126.459477 91.254392) (xy 126.400528 91.225504)
				(xy 126.351525 91.18675) (xy 126.323892 91.150557) (xy 126.305814 91.107501) (xy 126.300615 91.08109)
				(xy 125.724 91.475) (xy 126.300615 91.86891) (xy 126.328894 91.791392) (xy 126.390176 91.731158)
				(xy 126.489656 91.684974) (xy 126.631565 91.656394) (xy 126.75 91.65)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30135)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 90.775) (xy 142.184815 90.772822) (xy 142.279803 90.772388) (xy 142.320493 90.786763)
				(xy 142.345299 90.819291) (xy 142.7 90.675) (xy 142.345299 90.530709) (xy 142.315511 90.566224)
				(xy 142.256941 90.579929) (xy 142.184815 90.577179) (xy 142.149 90.575)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 93.575) (xy 136.713185 93.577179) (xy 136.618197 93.577612) (xy 136.577507 93.563237)
				(xy 136.552701 93.530709) (xy 136.198 93.675) (xy 136.552701 93.819291) (xy 136.58249 93.783776)
				(xy 136.641061 93.770071) (xy 136.713185 93.772822) (xy 136.749 93.775)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.101058 105.125) (xy 147.064582 105.11979) (xy 147.024341 105.103318) (xy 146.991508 105.078271)
				(xy 146.966785 105.042494) (xy 146.956561 105.007161) (xy 146.956561 104.964573) (xy 146.970722 104.91009)
				(xy 146.224 104.9) (xy 146.699483 105.342805) (xy 146.759815 105.318511) (xy 146.877242 105.311381)
				(xy 147.001806 105.319115) (xy 147.101058 105.325)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_track$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.210957 110.876175) (xy 151.268334 110.817745) (xy 151.340875 110.7476) (xy 151.447225 110.670507)
				(xy 151.350707 110.524293) (xy 151.204493 110.427775) (xy 151.1274 110.534123) (xy 151.057258 110.606662)
				(xy 150.998825 110.664043)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30152)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.203723 94.299548) (xy 155.220994 94.294715) (xy 155.302347 94.280368) (xy 155.342651 94.290851)
				(xy 155.374001 94.325) (xy 155.699867 94.1745) (xy 155.318279 94.050991) (xy 155.295477 94.082997)
				(xy 155.232101 94.106117) (xy 155.159097 94.117529) (xy 155.103724 94.126345)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.7 98.25) (xy 130.699499 98.224648) (xy 130.705524 98.106364) (xy 130.726166 98.053302) (xy 130.768339 98.020985)
				(xy 130.6 97.474) (xy 130.431661 98.020985) (xy 130.473649 98.053029) (xy 130.496245 98.115788)
				(xy 130.500501 98.224647) (xy 130.5 98.25)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.806233 115.209032) (xy 136.907416 115.418599) (xy 136.975461 115.585078) (xy 137.013667 115.70484)
				(xy 137.040003 115.816811) (xy 137.074399 116.030789) (xy 137.146333 116.460827) (xy 137.980454 116.29589)
				(xy 138.145827 115.461333) (xy 137.921017 115.433977) (xy 137.685491 115.437067) (xy 137.625207 115.440847)
				(xy 137.434794 115.447522) (xy 137.349461 115.439547) (xy 137.269473 115.41842) (xy 137.193904 115.379933)
				(xy 137.121825 115.319878) (xy 137.05231 115.234046) (xy 136.984431 115.11823)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.9 102.175) (xy 137.9197 102.076656) (xy 137.947009 102.017182) (xy 137.985624 101.959218)
				(xy 138.03023 101.911358) (xy 138.083684 101.871236) (xy 138.136125 101.845441) (xy 138.194704 101.829451)
				(xy 138.248164 101.825) (xy 138.050002 101.174) (xy 137.700002 101.130953) (xy 137.72093 101.397413)
				(xy 137.715941 101.75908) (xy 137.709588 101.897112) (xy 137.7 102.175)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 94.575) (xy 136.713185 94.577179) (xy 136.618197 94.577612) (xy 136.577507 94.563237)
				(xy 136.552701 94.530709) (xy 136.198 94.675) (xy 136.552701 94.819291) (xy 136.58249 94.783776)
				(xy 136.641061 94.770071) (xy 136.713185 94.772822) (xy 136.749 94.775)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30151)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.284092 96.1251) (xy 156.236422 96.119275) (xy 156.138064 96.10373) (xy 156.099963 96.08514)
				(xy 156.081863 96.054196) (xy 155.698077 96.174618) (xy 156.024 96.325) (xy 156.040516 96.304437)
				(xy 156.061468 96.29252) (xy 156.118993 96.288844) (xy 156.180326 96.302827) (xy 156.207556 96.309875)
			)
		)
	)
	(zone
		(net 67)
		(net_name "Net-(U6-Pad6)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30149)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.6 104.175) (xy 143.598438 104.229833) (xy 143.5875 104.295963) (xy 143.557813 104.351611)
				(xy 143.533008 104.368699) (xy 143.5 104.375) (xy 143.7 104.576) (xy 143.9 104.375) (xy 143.871082 104.370289)
				(xy 143.848357 104.357312) (xy 143.816791 104.309045) (xy 143.801263 104.225467) (xy 143.8 104.175)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.97241 90.923968) (xy 127.968603 90.948333) (xy 127.948196 91.032972) (xy 127.923126 91.066522)
				(xy 127.881386 91.081189) (xy 127.999805 91.67598) (xy 128.175 91.1625) (xy 128.145638 91.121851)
				(xy 128.144363 91.059795) (xy 128.159735 90.996555) (xy 128.168566 90.962986)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.449261 110.35) (xy 151.327701 110.355029) (xy 151.234947 110.370233) (xy 151.173175 110.390583)
				(xy 151.118964 110.418088) (xy 151.002992 110.501465) (xy 150.833329 110.625559) (xy 150.999 110.875)
				(xy 151.249441 111.041671) (xy 151.291848 110.948696) (xy 151.310269 110.85039) (xy 151.320194 110.790361)
				(xy 151.339588 110.742723) (xy 151.379071 110.711322) (xy 151.449261 110.7)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30159)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.741542 93.291061) (xy 135.760778 93.285952) (xy 135.806688 93.278867) (xy 135.828279 93.289879)
				(xy 135.845299 93.319291) (xy 136.199991 93.17487) (xy 135.834402 93.037989) (xy 135.823083 93.064885)
				(xy 135.806516 93.081248) (xy 135.76153 93.092666) (xy 135.740195 93.092428) (xy 135.71544 93.092773)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.12 109.8) (xy 146.12001 109.807653) (xy 146.118681 109.873933) (xy 146.108665 109.950874)
				(xy 146.081223 110.019725) (xy 146.058235 110.045256) (xy 146.027612 110.061732) (xy 146.22 110.326)
				(xy 146.412388 110.061732) (xy 146.364506 110.027649) (xy 146.333862 109.961181) (xy 146.320508 109.855447)
				(xy 146.31999 109.807653) (xy 146.32 109.8)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 100.175) (xy 150.449647 100.175501) (xy 150.331363 100.169476) (xy 150.278301 100.148834)
				(xy 150.245985 100.106661) (xy 149.699 100.275) (xy 150.245985 100.443339) (xy 150.278029 100.401351)
				(xy 150.340788 100.378755) (xy 150.449648 100.374499) (xy 150.475 100.375)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30136)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 93.775) (xy 142.184815 93.772822) (xy 142.279803 93.772388) (xy 142.320493 93.786763)
				(xy 142.345299 93.819291) (xy 142.7 93.675) (xy 142.345299 93.530709) (xy 142.315511 93.566224)
				(xy 142.256941 93.579929) (xy 142.184815 93.577179) (xy 142.149 93.575)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30137)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 92.775) (xy 155.184815 92.772822) (xy 155.279803 92.772388) (xy 155.320493 92.786763)
				(xy 155.345299 92.819291) (xy 155.7 92.675) (xy 155.345299 92.530709) (xy 155.315511 92.566224)
				(xy 155.256941 92.579929) (xy 155.184815 92.577179) (xy 155.149 92.575)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30138)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 89.775) (xy 155.184815 89.772822) (xy 155.279803 89.772388) (xy 155.320493 89.786763)
				(xy 155.345299 89.819291) (xy 155.7 89.675) (xy 155.345299 89.530709) (xy 155.315511 89.566224)
				(xy 155.256941 89.579929) (xy 155.184815 89.577179) (xy 155.149 89.575)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30150)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.85 103.525) (xy 139.848438 103.579833) (xy 139.8375 103.645963) (xy 139.807813 103.701611)
				(xy 139.783008 103.718699) (xy 139.75 103.725) (xy 139.95 103.926) (xy 140.15 103.725) (xy 140.121082 103.720289)
				(xy 140.098357 103.707312) (xy 140.066791 103.659045) (xy 140.051263 103.575467) (xy 140.05 103.525)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.854592 105.682866) (xy 148.775335 105.651909) (xy 148.720106 105.618549) (xy 148.659315 105.549538)
				(xy 148.625439 105.488665) (xy 148.549441 105.358329) (xy 148.299049 105.524691) (xy 148.241473 105.819236)
				(xy 148.449297 105.865977) (xy 148.596662 105.912714) (xy 148.605143 105.915623) (xy 148.76189 105.968183)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30139)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149001 89.275) (xy 155.184816 89.272822) (xy 155.279804 89.272388) (xy 155.320494 89.286763)
				(xy 155.3453 89.319291) (xy 155.700001 89.175) (xy 155.3453 89.030709) (xy 155.315512 89.066224)
				(xy 155.256942 89.079929) (xy 155.184816 89.077179) (xy 155.149001 89.075)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.925 110.525) (xy 149.012498 110.53121) (xy 149.116159 110.554683) (xy 149.181704 110.582079)
				(xy 149.240509 110.621392) (xy 149.276623 110.65927) (xy 149.304087 110.705481) (xy 149.31918 110.752469)
				(xy 149.324977 110.806676) (xy 149.325 110.810501) (xy 149.951 110.525) (xy 149.989621 110.125)
				(xy 149.809936 110.160161) (xy 149.575028 110.168906) (xy 149.212493 110.144175) (xy 148.925 110.125)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.354804 91.475) (xy 133.434336 91.479668) (xy 133.494931 91.492342) (xy 133.597187 91.540561)
				(xy 133.678815 91.583285) (xy 133.801227 91.620196) (xy 133.851 91.375) (xy 133.801227 91.129804)
				(xy 133.664585 91.173094) (xy 133.597186 91.209439) (xy 133.50229 91.255353) (xy 133.439128 91.269681)
				(xy 133.354804 91.275)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.211103 98.813023) (xy 156.202433 98.816541) (xy 156.157478 98.833425) (xy 156.104188 98.844892)
				(xy 156.052536 98.838048) (xy 156.030443 98.82373) (xy 156.0125 98.8) (xy 155.499134 98.9755) (xy 156.094107 99.092119)
				(xy 156.113439 99.057797) (xy 156.175524 99.026029) (xy 156.25161 99.003847) (xy 156.311103 98.986227)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.45 92.179804) (xy 132.445332 92.259336) (xy 132.432658 92.319931) (xy 132.384439 92.422186)
				(xy 132.341714 92.503815) (xy 132.304804 92.626227) (xy 132.55 92.676) (xy 132.795196 92.626227)
				(xy 132.751905 92.489584) (xy 132.715561 92.422187) (xy 132.669647 92.327291) (xy 132.655319 92.264128)
				(xy 132.65 92.179804)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30140)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 91.275) (xy 155.184815 91.272822) (xy 155.279803 91.272388) (xy 155.320493 91.286763)
				(xy 155.345299 91.319291) (xy 155.7 91.175) (xy 155.345299 91.030709) (xy 155.315511 91.066224)
				(xy 155.256941 91.079929) (xy 155.184815 91.077179) (xy 155.149 91.075)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.4 98.25) (xy 129.399499 98.224648) (xy 129.405524 98.106364) (xy 129.426166 98.053302) (xy 129.468339 98.020985)
				(xy 129.3 97.474) (xy 129.131661 98.020985) (xy 129.173649 98.053029) (xy 129.196245 98.115788)
				(xy 129.200501 98.224647) (xy 129.2 98.25)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.35 104.675) (xy 139.357653 104.67499) (xy 139.423933 104.676319) (xy 139.500874 104.686335)
				(xy 139.569725 104.713777) (xy 139.595256 104.736765) (xy 139.611732 104.767388) (xy 139.951 104.575)
				(xy 139.611732 104.382612) (xy 139.577649 104.430494) (xy 139.511181 104.461138) (xy 139.405447 104.474492)
				(xy 139.357653 104.47501) (xy 139.35 104.475)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.425 107.375) (xy 151.450352 107.374499) (xy 151.568637 107.380524) (xy 151.621699 107.401166)
				(xy 151.654015 107.443339) (xy 152.201 107.275) (xy 151.654015 107.106661) (xy 151.621972 107.148649)
				(xy 151.559213 107.171245) (xy 151.450353 107.175501) (xy 151.425 107.175)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.056284 112.134548) (xy 135.092676 112.248815) (xy 135.114743 112.350905) (xy 135.12363 112.4377)
				(xy 135.122006 112.516358) (xy 135.091574 112.654994) (xy 135.024745 112.789647) (xy 134.918441 112.940986)
				(xy 134.829392 113.064375) (xy 134.742077 113.206824) (xy 134.664918 113.378402) (xy 134.606333 113.589173)
				(xy 135.440342 113.755939) (xy 136.146749 113.282765) (xy 135.95702 113.029557) (xy 135.772774 112.835499)
				(xy 135.708446 112.774871) (xy 135.583987 112.654209) (xy 135.468064 112.515777) (xy 135.356277 112.329711)
				(xy 135.244223 112.066146)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30146)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.05 103.675) (xy 140.051563 103.620167) (xy 140.0625 103.554037) (xy 140.092188 103.498389)
				(xy 140.116992 103.481301) (xy 140.15 103.475) (xy 139.95 103.274) (xy 139.75 103.475) (xy 139.778918 103.479711)
				(xy 139.801643 103.492688) (xy 139.833209 103.540955) (xy 139.848737 103.624533) (xy 139.85 103.675)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 89.575) (xy 136.713185 89.577179) (xy 136.618197 89.577612) (xy 136.577507 89.563237)
				(xy 136.552701 89.530709) (xy 136.198 89.675) (xy 136.552701 89.819291) (xy 136.58249 89.783776)
				(xy 136.641061 89.770071) (xy 136.713185 89.772822) (xy 136.749 89.775)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.425 104.475) (xy 138.402557 104.475256) (xy 138.259762 104.467675) (xy 138.199675 104.445214)
				(xy 138.181604 104.425934) (xy 138.175 104.4) (xy 137.424 104.9) (xy 138.170722 104.920404) (xy 138.189906 104.827638)
				(xy 138.24113 104.753958) (xy 138.321009 104.699915) (xy 138.415635 104.675259) (xy 138.425 104.675)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/BUS_A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.321243 117.414822) (xy 144.212792 117.299373) (xy 144.129491 117.195373) (xy 144.073513 117.109758)
				(xy 144.032085 117.028473) (xy 143.982888 116.871082) (xy 143.958315 116.671411) (xy 143.954099 116.613921)
				(xy 143.935444 116.398628) (xy 143.893667 116.129173) (xy 143.059293 116.294293) (xy 142.894173 117.128667)
				(xy 143.205856 117.174912) (xy 143.378921 117.189099) (xy 143.582466 117.208545) (xy 143.674907 117.22667)
				(xy 143.765661 117.255561) (xy 143.85813 117.299091) (xy 143.955712 117.361133) (xy 144.061809 117.445559)
				(xy 144.179822 117.556243)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.05 98.25) (xy 130.049499 98.224648) (xy 130.055524 98.106364) (xy 130.076166 98.053302)
				(xy 130.118339 98.020985) (xy 129.95 97.474) (xy 129.781661 98.020985) (xy 129.823649 98.053029)
				(xy 129.846245 98.115788) (xy 129.850501 98.224647) (xy 129.85 98.25)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.215305 96.673634) (xy 131.208621 96.712951) (xy 131.184041 96.823788) (xy 131.159094 96.867553)
				(xy 131.120479 96.887364) (xy 131.249691 97.475951) (xy 131.425 96.9625) (xy 131.390343 96.922194)
				(xy 131.381964 96.857487) (xy 131.399778 96.759238) (xy 131.405516 96.735435)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 93.075) (xy 136.713185 93.077179) (xy 136.618197 93.077612) (xy 136.577507 93.063237)
				(xy 136.552701 93.030709) (xy 136.198 93.175) (xy 136.552701 93.319291) (xy 136.58249 93.283776)
				(xy 136.641061 93.270071) (xy 136.713185 93.272822) (xy 136.749 93.275)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.35 104.025) (xy 139.357653 104.02499) (xy 139.423933 104.026319) (xy 139.500874 104.036335)
				(xy 139.569725 104.063777) (xy 139.595256 104.086765) (xy 139.611732 104.117388) (xy 139.951 103.925)
				(xy 139.611732 103.732612) (xy 139.577649 103.780494) (xy 139.511181 103.811138) (xy 139.405447 103.824492)
				(xy 139.357653 103.82501) (xy 139.35 103.825)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.761514 105.345945) (xy 147.828022 105.364131) (xy 147.876325 105.388053) (xy 147.931083 105.445382)
				(xy 147.968949 105.528172) (xy 148.000927 105.603847) (xy 148.050559 105.691671) (xy 148.30098 105.525195)
				(xy 148.358527 105.230764) (xy 148.199951 105.20351) (xy 148.089717 105.191217) (xy 148.079519 105.190274)
				(xy 147.965478 105.177908) (xy 147.800529 105.149789)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.65 101.075) (xy 140.527841 101.054337) (xy 140.457297 101.027182) (xy 140.39157 100.988108)
				(xy 140.349993 100.95044) (xy 140.319051 100.905471) (xy 140.304992 100.867343) (xy 140.3 100.825)
				(xy 139.949 101.175) (xy 140.3 101.525) (xy 140.318279 101.446081) (xy 140.371712 101.377997) (xy 140.463266 101.320032)
				(xy 140.587188 101.281284) (xy 140.65 101.275)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30156)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.288557 96.650756) (xy 156.229179 96.636855) (xy 156.13891 96.614397) (xy 156.105984 96.595837)
				(xy 156.091952 96.569294) (xy 155.698135 96.6745) (xy 156.024001 96.825) (xy 156.040519 96.804145)
				(xy 156.060721 96.793246) (xy 156.11188 96.794381) (xy 156.168034 96.81532) (xy 156.188558 96.82396)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 95.075) (xy 136.713185 95.077179) (xy 136.618197 95.077612) (xy 136.577507 95.063237)
				(xy 136.552701 95.030709) (xy 136.198 95.175) (xy 136.552701 95.319291) (xy 136.58249 95.283776)
				(xy 136.641061 95.270071) (xy 136.713185 95.272822) (xy 136.749 95.275)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30154)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.692092 95.324868) (xy 135.723109 95.314997) (xy 135.805784 95.294183) (xy 135.844625 95.299211)
				(xy 135.874 95.325) (xy 136.199923 95.174618) (xy 135.808768 95.065223) (xy 135.788583 95.099504)
				(xy 135.731566 95.122173) (xy 135.662926 95.132841) (xy 135.615561 95.140092)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30141)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 93.275) (xy 142.184815 93.272822) (xy 142.279803 93.272388) (xy 142.320493 93.286763)
				(xy 142.345299 93.319291) (xy 142.7 93.175) (xy 142.345299 93.030709) (xy 142.315511 93.066224)
				(xy 142.256941 93.079929) (xy 142.184815 93.077179) (xy 142.149 93.075)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.909176 107.067376) (xy 152.706725 107.118009) (xy 152.587277 107.133912) (xy 152.456016 107.137542)
				(xy 152.345557 107.128956) (xy 152.228179 107.108023) (xy 152.195405 107.1) (xy 152.199077 107.275382)
				(xy 152.792374 107.397428) (xy 152.798073 107.379591) (xy 152.811856 107.366948) (xy 152.867979 107.352472)
				(xy 152.940093 107.350323) (xy 153.023982 107.344538)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30143)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.676784 94.312866) (xy 135.712206 94.305007) (xy 135.802312 94.290189) (xy 135.843723 94.297765)
				(xy 135.874 94.325) (xy 136.199965 94.174742) (xy 135.816734 94.053301) (xy 135.794485 94.089265)
				(xy 135.738483 94.109546) (xy 135.665805 94.116431) (xy 135.625019 94.119682)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30153)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.682742 94.818424) (xy 135.716844 94.809586) (xy 135.803885 94.792223) (xy 135.844167 94.798623)
				(xy 135.874 94.825) (xy 136.199951 94.674691) (xy 135.813325 94.558403) (xy 135.791961 94.593808)
				(xy 135.735675 94.615062) (xy 135.664039 94.623562) (xy 135.620939 94.628214)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.420178 117.556243) (xy 172.535627 117.447792) (xy 172.639626 117.364491) (xy 172.725241 117.308513)
				(xy 172.806526 117.267085) (xy 172.963917 117.217888) (xy 173.163588 117.193315) (xy 173.221079 117.189099)
				(xy 173.436371 117.170444) (xy 173.705827 117.128667) (xy 173.540707 116.294293) (xy 172.706333 116.129173)
				(xy 172.660087 116.440856) (xy 172.6459 116.613922) (xy 172.626454 116.817466) (xy 172.608329 116.909907)
				(xy 172.579438 117.000662) (xy 172.535908 117.09313) (xy 172.473866 117.190712) (xy 172.38944 117.29681)
				(xy 172.278757 117.414822)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30158)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.55 91.275) (xy 133.479349 91.290603) (xy 133.408305 91.307556) (xy 133.384228 91.30671)
				(xy 133.375 91.294362) (xy 133.199 91.675) (xy 133.375 91.754782) (xy 133.379752 91.683695) (xy 133.393017 91.623272)
				(xy 133.413525 91.572948) (xy 133.439661 91.533189) (xy 133.470244 91.503579) (xy 133.503435 91.484457)
				(xy 133.55 91.475)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.99676 92.575) (xy 154.797004 92.563963) (xy 154.674909 92.557242) (xy 154.501227 92.579804)
				(xy 154.549 92.825) (xy 154.688893 93.032867) (xy 154.767862 92.960571) (xy 154.814825 92.888213)
				(xy 154.842171 92.84372) (xy 154.875579 92.807781) (xy 154.924095 92.783755) (xy 154.99676 92.775)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.65511 115.009669) (xy 154.730489 115.177341) (xy 154.784173 115.320737) (xy 154.81856 115.439583)
				(xy 154.840175 115.546631) (xy 154.859003 115.764585) (xy 154.861164 115.839273) (xy 154.874151 116.102476)
				(xy 154.892956 116.266208) (xy 154.926333 116.460827) (xy 155.760433 116.2959) (xy 156.232235 115.588251)
				(xy 156.03862 115.480734) (xy 155.845808 115.413908) (xy 155.63795 115.377125) (xy 155.519296 115.365511)
				(xy 155.32434 115.34222) (xy 155.233636 115.31999) (xy 155.14703 115.2847) (xy 155.064208 115.231848)
				(xy 154.984855 115.156931) (xy 154.908658 115.055447) (xy 154.835303 114.922892)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30142)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 89.775) (xy 135.684815 89.772822) (xy 135.779803 89.772388) (xy 135.820493 89.786763)
				(xy 135.845299 89.819291) (xy 136.2 89.675) (xy 135.845299 89.530709) (xy 135.815511 89.566224)
				(xy 135.756941 89.579929) (xy 135.684815 89.577179) (xy 135.649 89.575)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132 98.25) (xy 131.999499 98.224648) (xy 132.005524 98.106364) (xy 132.026166 98.053302) (xy 132.068339 98.020985)
				(xy 131.9 97.474) (xy 131.731661 98.020985) (xy 131.773649 98.053029) (xy 131.796245 98.115788)
				(xy 131.800501 98.224647) (xy 131.8 98.25)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 90.075) (xy 136.713185 90.077179) (xy 136.618197 90.077612) (xy 136.577507 90.063237)
				(xy 136.552701 90.030709) (xy 136.198 90.175) (xy 136.552701 90.319291) (xy 136.58249 90.283776)
				(xy 136.641061 90.270071) (xy 136.713185 90.272822) (xy 136.749 90.275)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 89.075) (xy 136.713185 89.077179) (xy 136.618197 89.077612) (xy 136.577507 89.063237)
				(xy 136.552701 89.030709) (xy 136.198 89.175) (xy 136.552701 89.319291) (xy 136.58249 89.283776)
				(xy 136.641061 89.270071) (xy 136.713185 89.272822) (xy 136.749 89.275)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30144)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.681748 91.294739) (xy 135.709607 91.289791) (xy 135.800088 91.280496) (xy 135.842602 91.292181)
				(xy 135.874 91.325) (xy 136.199991 91.17487) (xy 135.832769 91.03908) (xy 135.806009 91.075646)
				(xy 135.749622 91.092301) (xy 135.694314 91.094794) (xy 135.655653 91.09645)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.449261 110.35) (xy 151.399826 110.345173) (xy 151.364795 110.331385) (xy 151.329308 110.288326)
				(xy 151.310269 110.199609) (xy 151.293433 110.107009) (xy 151.276401 110.057861) (xy 151.249441 110.008329)
				(xy 150.999 110.175) (xy 150.833329 110.424441) (xy 151.002993 110.548535) (xy 151.092999 110.615453)
				(xy 151.181291 110.662713) (xy 151.292001 110.690751) (xy 151.449261 110.7)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.576087 96.679001) (xy 130.569205 96.716607) (xy 130.544059 96.82247) (xy 130.518896 96.863729)
				(xy 130.480199 96.881425) (xy 130.599742 97.475965) (xy 130.775 96.9625) (xy 130.744343 96.922898)
				(xy 130.739792 96.857596) (xy 130.761083 96.761243) (xy 130.769272 96.730764)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_track$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.998825 110.385957) (xy 151.057256 110.443336) (xy 151.1274 110.515875) (xy 151.204493 110.622225)
				(xy 151.350707 110.525707) (xy 151.447225 110.379493) (xy 151.340875 110.3024) (xy 151.268336 110.232256)
				(xy 151.210957 110.173825)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.266233 115.209032) (xy 134.367416 115.418599) (xy 134.435461 115.585078) (xy 134.473667 115.70484)
				(xy 134.500003 115.816811) (xy 134.534399 116.030789) (xy 134.606333 116.460827) (xy 135.440454 116.29589)
				(xy 135.605827 115.461333) (xy 135.381017 115.433977) (xy 135.145491 115.437067) (xy 135.085207 115.440847)
				(xy 134.894794 115.447522) (xy 134.809461 115.439547) (xy 134.729473 115.41842) (xy 134.653904 115.379933)
				(xy 134.581825 115.319878) (xy 134.51231 115.234046) (xy 134.444431 115.11823)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.346233 115.209032) (xy 139.447416 115.418599) (xy 139.515461 115.585078) (xy 139.553667 115.70484)
				(xy 139.580003 115.816811) (xy 139.614399 116.030789) (xy 139.686333 116.460827) (xy 140.520454 116.29589)
				(xy 140.685827 115.461333) (xy 140.461017 115.433977) (xy 140.225491 115.437067) (xy 140.165207 115.440847)
				(xy 139.974794 115.447522) (xy 139.889461 115.439547) (xy 139.809473 115.41842) (xy 139.733904 115.379933)
				(xy 139.661825 115.319878) (xy 139.59231 115.234046) (xy 139.524431 115.11823)
			)
		)
	)
	(zone
		(net 65)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30155)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.198955 93.793639) (xy 155.224879 93.788846) (xy 155.305744 93.780533) (xy 155.344291 93.792447)
				(xy 155.374 93.825) (xy 155.699991 93.67487) (xy 155.333248 93.53876) (xy 155.322919 93.561527)
				(xy 155.306192 93.576981) (xy 155.252651 93.592539) (xy 155.207316 93.594086) (xy 155.172853 93.59535)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 92.075) (xy 136.713185 92.077179) (xy 136.618197 92.077612) (xy 136.577507 92.063237)
				(xy 136.552701 92.030709) (xy 136.198 92.175) (xy 136.552701 92.319291) (xy 136.58249 92.283776)
				(xy 136.641061 92.270071) (xy 136.713185 92.272822) (xy 136.749 92.275)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.249 96.075) (xy 143.213185 96.077179) (xy 143.118197 96.077612) (xy 143.077507 96.063237)
				(xy 143.052701 96.030709) (xy 142.698 96.175) (xy 143.052701 96.319291) (xy 143.08249 96.283776)
				(xy 143.141061 96.270071) (xy 143.213185 96.272822) (xy 143.249 96.275)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.32 109.795196) (xy 146.324668 109.715664) (xy 146.337342 109.655069) (xy 146.385561 109.552813)
				(xy 146.428285 109.471184) (xy 146.465196 109.348773) (xy 146.22 109.299) (xy 145.974804 109.348773)
				(xy 146.018094 109.485415) (xy 146.054439 109.552813) (xy 146.100353 109.647709) (xy 146.114681 109.710872)
				(xy 146.12 109.795196)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.538773 96.663897) (xy 132.521153 96.723389) (xy 132.488126 96.826786) (xy 132.464189 96.86491)
				(xy 132.43288 96.880892) (xy 132.5495 97.475866) (xy 132.725 96.9625) (xy 132.701223 96.944507)
				(xy 132.686901 96.922345) (xy 132.680642 96.865405) (xy 132.708459 96.772567) (xy 132.711977 96.763897)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.764404 107.178039) (xy 158.740838 107.178206) (xy 158.628188 107.170586) (xy 158.57741 107.14924)
				(xy 158.545985 107.106661) (xy 157.999013 107.274844) (xy 158.545985 107.443339) (xy 158.559485 107.416578)
				(xy 158.578956 107.397622) (xy 158.636504 107.376787) (xy 158.713564 107.374931) (xy 158.73311 107.375575)
			)
		)
	)
	(zone
		(net 67)
		(net_name "Net-(U6-Pad6)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30147)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.8 104.325) (xy 143.801563 104.270167) (xy 143.8125 104.204037) (xy 143.842188 104.148389)
				(xy 143.866992 104.131301) (xy 143.9 104.125) (xy 143.7 103.924) (xy 143.5 104.125) (xy 143.528918 104.129711)
				(xy 143.551643 104.142688) (xy 143.583209 104.190955) (xy 143.598737 104.274533) (xy 143.6 104.325)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 101.475) (xy 150.449647 101.475501) (xy 150.331363 101.469476) (xy 150.278301 101.448834)
				(xy 150.245985 101.406661) (xy 149.699 101.575) (xy 150.245985 101.743339) (xy 150.278029 101.701351)
				(xy 150.340788 101.678755) (xy 150.449648 101.674499) (xy 150.475 101.675)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 100.825) (xy 150.449647 100.825501) (xy 150.331363 100.819476) (xy 150.278301 100.798834)
				(xy 150.245985 100.756661) (xy 149.699 100.925) (xy 150.245985 101.093339) (xy 150.278029 101.051351)
				(xy 150.340788 101.028755) (xy 150.449648 101.024499) (xy 150.475 101.025)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.74323 115.299431) (xy 164.837007 115.35273) (xy 164.911669 115.406919) (xy 164.964966 115.457649)
				(xy 165.005553 115.509847) (xy 165.054387 115.618273) (xy 165.072516 115.749606) (xy 165.065847 115.940207)
				(xy 165.057204 116.177813) (xy 165.064538 116.313091) (xy 165.086333 116.460827) (xy 165.92089 116.295454)
				(xy 166.085827 115.461333) (xy 165.655789 115.389399) (xy 165.469778 115.360354) (xy 165.2963 115.319024)
				(xy 165.097126 115.24584) (xy 164.834032 115.121233)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.2)
			(smoothing fillet)
			(radius 0.1)
		)
		(polygon
			(pts
				(xy 181.95 120.025) (xy 181.95 86.025) (xy 121.95 86.025) (xy 121.95 120.025)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.125 103.104804) (xy 146.120332 103.184336) (xy 146.107658 103.244931) (xy 146.059439 103.347186)
				(xy 146.016714 103.428815) (xy 145.979804 103.551227) (xy 146.225 103.601) (xy 146.470196 103.551227)
				(xy 146.426905 103.414584) (xy 146.390561 103.347187) (xy 146.344647 103.252291) (xy 146.330319 103.189128)
				(xy 146.325 103.104804)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.354804 91.475) (xy 147.434336 91.479668) (xy 147.494931 91.492342) (xy 147.597187 91.540561)
				(xy 147.678815 91.583285) (xy 147.801227 91.620196) (xy 147.851 91.375) (xy 147.801227 91.129804)
				(xy 147.664585 91.173094) (xy 147.597186 91.209439) (xy 147.50229 91.255353) (xy 147.439128 91.269681)
				(xy 147.354804 91.275)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.4 105.705764) (xy 153.395292 105.788989) (xy 153.382338 105.854514) (xy 153.337978 105.95331)
				(xy 153.311952 105.993409) (xy 153.2538 106.091663) (xy 153.227548 106.157406) (xy 153.205764 106.241473)
				(xy 153.5 106.301) (xy 153.794236 106.241473) (xy 153.773493 106.160601) (xy 153.748581 106.096727)
				(xy 153.688048 105.993409) (xy 153.654617 105.940883) (xy 153.626536 105.881776) (xy 153.6072 105.806574)
				(xy 153.6 105.705764)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.10324 92.775) (xy 154.159218 92.77978) (xy 154.200934 92.793239) (xy 154.253251 92.837471)
				(xy 154.285174 92.888212) (xy 154.3318 92.960144) (xy 154.411107 93.032867) (xy 154.551 92.825)
				(xy 154.598773 92.579804) (xy 154.479987 92.560977) (xy 154.394257 92.557144) (xy 154.302995 92.563963)
				(xy 154.10324 92.575)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.12 108.804804) (xy 146.115332 108.884336) (xy 146.102658 108.944931) (xy 146.054439 109.047186)
				(xy 146.011714 109.128815) (xy 145.974804 109.251227) (xy 146.22 109.301) (xy 146.465196 109.251227)
				(xy 146.421905 109.114584) (xy 146.385561 109.047187) (xy 146.339647 108.952291) (xy 146.325319 108.889128)
				(xy 146.32 108.804804)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.2 104.930764) (xy 148.195292 105.013989) (xy 148.182338 105.079514) (xy 148.137978 105.17831)
				(xy 148.111952 105.218409) (xy 148.0538 105.316663) (xy 148.027548 105.382406) (xy 148.005764 105.466473)
				(xy 148.3 105.526) (xy 148.594236 105.466473) (xy 148.573493 105.385601) (xy 148.548581 105.321727)
				(xy 148.488048 105.218409) (xy 148.454617 105.165883) (xy 148.426536 105.106776) (xy 148.4072 105.031574)
				(xy 148.4 104.930764)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.32 104.095196) (xy 146.324671 104.017097) (xy 146.337371 103.957368) (xy 146.380596 103.865739)
				(xy 146.387899 103.853699) (xy 146.432343 103.771959) (xy 146.470196 103.648773) (xy 146.225 103.599)
				(xy 145.979804 103.648773) (xy 146.023439 103.787907) (xy 146.05677 103.85184) (xy 146.101092 103.947354)
				(xy 146.114885 104.010703) (xy 146.12 104.095196)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.190898 99.974477) (xy 151.135378 99.912299) (xy 151.098205 99.856806) (xy 151.059712 99.755579)
				(xy 151.049761 99.708821) (xy 151.021405 99.598226) (xy 150.993481 99.533176) (xy 150.949441 99.458329)
				(xy 150.699293 99.624293) (xy 150.533329 99.874441) (xy 150.605181 99.916958) (xy 150.667962 99.944509)
				(xy 150.783821 99.974761) (xy 150.844602 99.988263) (xy 150.906253 100.010202) (xy 150.973102 100.049705)
				(xy 151.049477 100.115898)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.345196 91.275) (xy 134.265664 91.270332) (xy 134.205069 91.257658) (xy 134.102813 91.209439)
				(xy 134.021184 91.166714) (xy 133.898773 91.129804) (xy 133.849 91.375) (xy 133.898773 91.620196)
				(xy 134.035415 91.576905) (xy 134.102813 91.540561) (xy 134.197709 91.494647) (xy 134.260872 91.480319)
				(xy 134.345196 91.475)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.474916 99.427635) (xy 148.506806 99.363293) (xy 148.539818 99.319778) (xy 148.608253 99.272975)
				(xy 148.647292 99.256094) (xy 148.711308 99.227689) (xy 148.788893 99.182867) (xy 148.650382 98.974077)
				(xy 148.404804 98.926227) (xy 148.382744 99.043355) (xy 148.353481 99.179529) (xy 148.290146 99.351085)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.354804 97.525) (xy 154.434336 97.529668) (xy 154.494931 97.542342) (xy 154.597187 97.590561)
				(xy 154.678815 97.633285) (xy 154.801227 97.670196) (xy 154.851 97.425) (xy 154.801227 97.179804)
				(xy 154.664585 97.223094) (xy 154.597186 97.259439) (xy 154.50229 97.305353) (xy 154.439128 97.319681)
				(xy 154.354804 97.325)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.045196 92.575) (xy 132.965664 92.570332) (xy 132.905069 92.557658) (xy 132.802813 92.509439)
				(xy 132.721184 92.466714) (xy 132.598773 92.429804) (xy 132.549 92.675) (xy 132.598773 92.920196)
				(xy 132.735415 92.876905) (xy 132.802813 92.840561) (xy 132.897709 92.794647) (xy 132.960872 92.780319)
				(xy 133.045196 92.775)
			)
		)
	)
	(embedded_fonts yes)
	(embedded_files
		(file
			(name "ProggyVector.ttf")
			(type font)
		)
	)
)
