(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.5422)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1999)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.9906)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.1999)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-In)")
	(net 2 "GND")
	(net 3 "Net-(J3-In)")
	(net 4 "Net-(J5-In)")
	(net 5 "Net-(J7-In)")
	(net 6 "Net-(J10-In)")
	(net 7 "Net-(J11-In)")
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 76.093 107.9875 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J7-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 69.08116 106.268)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J7"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(J7-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 69.08116 74.302)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J3"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(J3-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 76.1485 100.614)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J7-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J7-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 204.857 107.9895 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J7-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 211.955966 122.251 180)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J10"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0 180)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J10-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.047 55.492 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 99.275 124.704 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J10-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 211.955966 74.359 180)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J4"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0 180)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(J3-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 69.08116 138.234)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J11"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J11-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 181.659 92.1385 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J5-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 211.955966 90.285 180)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J6"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0 180)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(J5-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 181.368 124.7435 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J10-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 99.334 140.2525 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J11-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 99.435 92.0545 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J5-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.096 76.0025 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J3-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 69.08116 90.285)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J5"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(J5-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 204.9835 100.583)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J7-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J7-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 156.163 76.0325 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J3-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.1281 68.7331)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J3-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J3-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 211.955966 138.234 180)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J12"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0 180)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J11-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 69.08116 58.319)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J1"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(J1-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 181.482 140.1975 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C19"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J11-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 156.2145 68.651)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J3-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J3-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 211.955966 58.319 180)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J2"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0 180)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(J1-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 99.4215 84.639)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J5-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J5-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 156.323 55.4935 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 181.748 84.611)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J5-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J5-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 99.4265 132.917)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J11-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J11-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 211.955966 106.268 180)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J8"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0 180)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(J7-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38 180)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38 180)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38 180)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 181.4055 132.832)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J11-In)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J11-In)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Molex_73251-1153_EdgeMount_Horizontal"
		(layer "F.Cu")
		(at 69.08116 122.251)
		(descr "Molex SMA RF Connectors, Edge Mount, https://tools.molex.com/pdm_docs/sd/732511150_sd.pdf")
		(tags "sma edge")
		(property "Reference" "J9"
			(at -1.5 7 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_Coaxial"
			(at -1.72 -7.11 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "t-coil2.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -1.5 7 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.72 0)
			(size 5.08 2.29)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J10-In)")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 -4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.72 4.38)
			(size 5.08 2.42)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 -4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.27 4.38)
			(size 0.95 0.46)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 -4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 1.72 4.38)
			(size 0.97 0.97)
			(drill 0.46)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Molex_73251-1153_EdgeMount_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 64.321 48.746)
		(end 216.721 150.346)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 215.741 50.839) (xy 214.029 148.661) (xy 66.765 148.959) (xy 65.311 50.352) (xy 65.311 50.35)
			)
		)
		(polygon
			(pts
				(xy 96.83 138.6665) (xy 101.83 138.6665) (xy 101.83 133.6665) (xy 96.83 133.6665)
			)
		)
		(polygon
			(pts
				(xy 178.982 138.6315) (xy 183.982 138.6315) (xy 183.982 133.6315) (xy 178.982 133.6315)
			)
		)
		(polygon
			(pts
				(xy 202.391 106.4125) (xy 207.391 106.4125) (xy 207.391 101.4125) (xy 202.391 101.4125)
			)
		)
		(polygon
			(pts
				(xy 73.594 106.3885) (xy 78.594 106.3885) (xy 78.594 101.3885) (xy 73.594 101.3885)
			)
		)
		(polygon
			(pts
				(xy 96.923 90.4555) (xy 101.923 90.4555) (xy 101.923 85.4555) (xy 96.923 85.4555)
			)
		)
		(polygon
			(pts
				(xy 179.154 85.425) (xy 179.154 90.425) (xy 184.154 90.425) (xy 184.154 85.425)
			)
		)
		(polygon
			(pts
				(xy 153.699 74.4765) (xy 158.699 74.4765) (xy 158.699 69.4765) (xy 153.699 69.4765)
			)
		)
		(polygon
			(pts
				(xy 121.592 74.456) (xy 126.592 74.456) (xy 126.592 69.456) (xy 121.592 69.456)
			)
		)
	)
	(embedded_fonts no)
)
