(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(R1-Pad2)")
	(net 3 "/In")
	(net 4 "/Out")
	(footprint "Symbol:qr"
		(layer "F.Cu")
		(at 146.267513 95.7586)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 144.85 98.3)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.05 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "5pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "probe.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/In")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/Out")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 144.8 95)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0.1475 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "2pF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "probe.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/In")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/Out")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 149.05 92)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.5MΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "probe.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "/Out")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount"
		(layer "F.Cu")
		(at 138.6 95 180)
		(descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
		(tags "SMA Straight Samtec Edge Mount")
		(property "Reference" "J1"
			(at 0 -5.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "To circuit"
			(at -3.4 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "probe.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 270)
			(size 1.27 3.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1968503937)
			(net 3 "/In")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 -2.825 270)
			(size 1.35 3.7)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 -2.825 270)
			(size 1.35 3.7)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 2.825 270)
			(size 1.35 3.7)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 2.825 270)
			(size 1.35 3.7)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Trimmer_Sprague-Goodman_SGC3"
		(layer "F.Cu")
		(at 148.659429 97.230414 -90)
		(descr "trimmer capacitor SMD horizontal, http://media.wix.com/ugd/d86717_38d9821e12823a7aa9cef38c6c2a73cc.pdf")
		(tags " Sprague Goodman SGC3")
		(property "Reference" "C3"
			(at 2.9 -2.990571 180)
			(layer "F.SilkS")
		)
		(property "Value" "8-30pF"
			(at 0 2.85 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/430/SCG3S_Series_Spec_2020.pdf?_gl=1*1cjebp5*_up*MQ..*_gs*MQ..&gclid=Cj0KCQiAr5nKBhCpARIsACa_NiOp8v-3Qg6VxRsadesvz1OIcx9M1SlvFwP3e9yqGBqAxM4DujWyJmgaArtFEALw_wcB&gclsrc=aw.ds&gbraid=0AAAAADrbLlhdecwtFDHIKXDcL_djQaT_V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Trimmable capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "https://www.digikey.com/en/products/detail/ew-electronics/SGC3S300NM/11689290"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "probe.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.8375 0 270)
			(size 1.075 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/Out")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.8375 0 270)
			(size 1.075 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Trimmer_Sprague-Goodman_SGC3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 144.85 92)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.5MΩ"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "probe.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "/In")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 2 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Coaxial:SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount"
		(layer "F.Cu")
		(at 154.9 95)
		(descr "Connector SMA, 0Hz to 20GHz, 50Ohm, Edge Mount (http://suddendocs.samtec.com/prints/sma-j-p-x-st-em1-mkt.pdf)")
		(tags "SMA Straight Samtec Edge Mount")
		(property "Reference" "J2"
			(at 0 -4.75 180)
			(layer "F.SilkS")
		)
		(property "Value" "To scope"
			(at -3.4 0.5 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*BNC* *SMA* *SMB* *SMC* *Cinch* *LEMO* *UMRF* *MCX* *U.FL*")
		(sheetname "/")
		(sheetfile "probe.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 2.6 0 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 0 0 90)
			(size 1.27 3.2)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1968503937)
			(net 4 "/Out")
			(pinfunction "In")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 -2.825 90)
			(size 1.35 3.7)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 -2.825 90)
			(size 1.35 3.7)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 2.825 90)
			(size 1.35 3.7)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.25 2.825 90)
			(size 1.35 3.7)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.1851851852)
			(net 1 "GND")
			(pinfunction "Ext")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Samtec_SMA-J-P-H-ST-EM1_EdgeMount.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 157.5 99.5)
		(mid 156.914214 100.914214)
		(end 155.5 101.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155.5 88.500014)
		(end 138 88.500014)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 138 101.5)
		(mid 136.585786 100.914214)
		(end 136 99.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 155.5 88.500014)
		(mid 156.914204 89.085796)
		(end 157.499986 90.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136 99.5)
		(end 136 90.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 136 90.5)
		(mid 136.585786 89.085786)
		(end 138 88.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155.5 101.5)
		(end 138 101.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.499986 90.5)
		(end 157.499986 99.492517)
		(layer "Edge.Cuts")
	)
	(gr_text "To scope\n"
		(at 151.6 90.6 90)
		(layer "B.SilkS")
	)
	(gr_text "To circuit"
		(at 141.85 100.05 270)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.5 87.5) (xy 135 87.5) (xy 135 102) (xy 158.5 102)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/In")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 138.6125 96.6) (xy 138.45 96.4375) (xy 138.45 93.503125) (xy 138.603125 93.35) (xy 140.805213 93.35)
				(xy 142 92.542257) (xy 142 92.012148) (xy 142.262148 91.75) (xy 144.060064 91.75) (xy 144.050144 98.6)
				(xy 142.095238 98.6) (xy 142.05 97.65) (xy 141 96.6)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/Out")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.9 96.65) (xy 155.15 96.316667) (xy 155.15 93.716666) (xy 154.9 93.3) (xy 152.25 93.3) (xy 151.567707 92.57506)
				(xy 151.52346 91.887681) (xy 151.347122 91.75) (xy 149.8 91.75) (xy 149.8 93) (xy 149.64 93.2) (xy 147.936207 93.2)
				(xy 146.85 94.7) (xy 145.45 94.75) (xy 145.502277 98.102277) (xy 145.9 98.5) (xy 149.67442 98.5)
				(xy 150.348291 97.092098) (xy 151.960348 97.047606) (xy 152.413563 96.687673)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.5 87.5) (xy 158.5 102) (xy 135 102) (xy 135 87.5)
			)
		)
	)
	(embedded_fonts no)
)
