(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x0001000_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "GNDA")
	(net 3 "+5V")
	(net 4 "/V_IN")
	(net 5 "+5VA")
	(net 6 "Net-(Q1-E)")
	(net 7 "/EXT_24V")
	(net 8 "Net-(Q2-E)")
	(net 9 "Net-(R2-Pad2)")
	(net 10 "/V_OFFSET")
	(net 11 "Net-(R10-Pad1)")
	(net 12 "unconnected-(U5-NC-Pad3)")
	(net 13 "unconnected-(U5-Pad6)")
	(net 14 "Net-(U3B--)")
	(net 15 "Net-(U6A-+)")
	(net 16 "Net-(Q4-E)")
	(net 17 "Net-(D1-A)")
	(net 18 "Net-(U2B-+)")
	(net 19 "Net-(U2A--)")
	(net 20 "Net-(J4-Pad1)")
	(net 21 "Net-(Q4-B)")
	(net 22 "Net-(Q3-C-Pad2)")
	(net 23 "Net-(Q1-B)")
	(net 24 "Net-(Q3-B)")
	(net 25 "Net-(U3A--)")
	(net 26 "Net-(U3A-+)")
	(net 27 "Net-(U3B-+)")
	(net 28 "Net-(R11-Pad1)")
	(net 29 "Net-(R13-Pad1)")
	(net 30 "Net-(R15-Pad1)")
	(net 31 "unconnected-(U1-Pad5)")
	(net 32 "Net-(U4-Pad2)")
	(net 33 "unconnected-(U4-NC-Pad3)")
	(net 34 "unconnected-(U4-Pad6)")
	(net 35 "Net-(U6A--)")
	(net 36 "Net-(D2-A)")
	(net 37 "Net-(C4-Pad1)")
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 131.9825 74.21 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 4.1725 -0.02 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 5 "+5VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 2 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(at 101.57 68.92)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "4N25"
			(at 3.81 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83725/4n25.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 30V, CTR 20%, Viso 2500V, DIP6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 11 "Net-(R10-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 32 "Net-(U4-Pad2)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 33 "unconnected-(U4-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 15 "Net-(U6A-+)")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 5 "+5VA")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 34 "unconnected-(U4-Pad6)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 142.03 81.25 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at -3.36 1.87 0)
			(layer "F.SilkS")
		)
		(property "Value" "45p"
			(at 0 1.85 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 21 "Net-(Q4-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 16 "Net-(Q4-E)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 79.8125 74.21 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 3.8625 -0.02 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.85 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 150.615 99.91625)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "Q4"
			(at 0 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BCP56"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://cache.nxp.com/documents/data_sheet/BCP56_BCX56_BC56PA.pdf?pspll=1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.15 0)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J4-Pad1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.15 0)
			(size 2 3.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "Net-(J4-Pad1)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(Q4-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 105.34 99.91625)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "Q3"
			(at 0 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "BCP56"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://cache.nxp.com/documents/data_sheet/BCP56_BCX56_BC56PA.pdf?pspll=1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?223*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.15 0)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(Q3-C-Pad2)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.15 0)
			(size 2 3.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(Q3-C-Pad2)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 88.913333 103.1975)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 78.9 81.315)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U3"
			(at 0 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP6002-xP"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1MHz, Low-Power Op Amp, DIP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U3B-+)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U3A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U3A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U3B-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(U3B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "Net-(C4-Pad1)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical"
		(layer "F.Cu")
		(at 59.7 106.76)
		(descr "Potentiometer, vertical, Bourns 3299W, https://www.bourns.com/pdfs/3299.pdf")
		(tags "Potentiometer vertical Bourns 3299W")
		(property "Reference" "RV2"
			(at -2.54 -3.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.54 5.44 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.175 1.14 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 18 "Net-(U2B-+)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.08 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3299W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:Term_Block_1x2_P5.08MM"
		(layer "F.Cu")
		(at 76.338 120.56)
		(descr "http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf")
		(property "Reference" "J2"
			(at 8.932 -3.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "OSTTC022162"
			(at 2.032 5.09 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:Term_Block_1x2_P5.08MM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2P SIDE ENT 5.08MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "ED2609-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "OSTTC022162"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors, Interconnects"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Terminal Blocks - Wire to Board"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-shore-technology-inc/OSTTC022162/ED2609-ND/614558"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "On Shore Technology Inc."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 2.3 2.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 90.539791 77.87)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.998 0)
			(layer "F.SilkS")
		)
		(property "Value" "DRIVE"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 37 "Net-(C4-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 131.07 81.315)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U6"
			(at 0 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP6002-xP"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1MHz, Low-Power Op Amp, DIP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U6A--)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U6A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U6A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GNDA")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U6A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "Net-(Q4-E)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(Q4-B)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "+5VA")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 69.81 89.557622)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at -4.03 0.002378 360)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 2.28 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 25 "Net-(U3A--)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 147.635 81.25 -90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at 0 -2.28 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 30 "Net-(R15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 16 "Net-(Q4-E)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 153.67 74.21 -90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -2.28 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 2 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 29 "Net-(R13-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical"
		(layer "F.Cu")
		(at 59.7 96.8175)
		(descr "Potentiometer, vertical, Bourns 3299W, https://www.bourns.com/pdfs/3299.pdf")
		(tags "Potentiometer vertical Bourns 3299W")
		(property "Reference" "RV1"
			(at -2.54 -3.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "5k"
			(at -2.54 5.44 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.175 1.14 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 9 "Net-(R2-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "Net-(Q2-E)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.08 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 8 "Net-(Q2-E)")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3299W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 137.825 86.14)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at -3.035 0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "V-R"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 16 "Net-(Q4-E)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "digikey-footprints:Term_Block_1x2_P5.08MM"
		(layer "F.Cu")
		(at 156.262 120.56 180)
		(descr "http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf")
		(property "Reference" "J4"
			(at -3.738 3.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "OSTTC022162"
			(at 2.032 5.09 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:Term_Block_1x2_P5.08MM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2P SIDE ENT 5.08MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "ED2609-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "OSTTC022162"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors, Interconnects"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Terminal Blocks - Wire to Board"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-shore-technology-inc/OSTTC022162/ED2609-ND/614558"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "TERM BLK 2P SIDE ENT 5.08MM PCB"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "On Shore Technology Inc."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 2.2 2.2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 20 "Net-(J4-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 2.3 2.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "/EXT_24V")
			(pintype "passive")
		)
	)
	(footprint "my_footprints:DIN_Rail_adapter"
		(layer "F.Cu")
		(at 45.48 76.32)
		(property "Reference" "M1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 36.83 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "my_footprints:DIN_Rail_adapter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(clearance 1)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0.09 6.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "" np_thru_hole circle
			(at 0 18.85)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0.09 6.35)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0.09 31.55)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 153.67 81.25 -90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -2.28 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 29 "Net-(R13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 16 "Net-(Q4-E)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "my_footprints:DIN_Rail_adapter"
		(layer "F.Cu")
		(at 164.23 75.93)
		(property "Reference" "M2"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 36.83 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "my_footprints:DIN_Rail_adapter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(clearance 1)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.09 6.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 18.85)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0.09 6.35)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
		(pad "" np_thru_hole circle
			(at 0.09 31.55)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 117.7 120.56)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.82 360)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 2 "GNDA")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4875 0)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 36 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 69.81 80.040184)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at -4.03 -0.020184 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 25 "Net-(U3A--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 27 "Net-(U3B-+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "F.Cu")
		(at 69.81 96.70506 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -2.3 360)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 2.3 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 26 "Net-(U3A-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 118.875 81.95)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 -1.998 0)
			(layer "F.SilkS")
		)
		(property "Value" "SEC-FEED"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 15 "Net-(U6A-+)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 147.635 74.21 -90)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 -2.28 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 2 "GNDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 30 "Net-(R15-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 78.9 89.557622)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -2.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 26 "Net-(U3A-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 10 "/V_OFFSET")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "F.Cu")
		(at 98.956666 89.557622 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -2.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 2.3 180)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 14 "Net-(U3B--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:Term_Block_1x2_P5.08MM"
		(layer "F.Cu")
		(at 54.588 120.56)
		(descr "http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf")
		(property "Reference" "J1"
			(at 9.192 -3.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "OSTTC022162"
			(at 2.032 5.09 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:Term_Block_1x2_P5.08MM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2P SIDE ENT 5.08MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "ED2609-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "OSTTC022162"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors, Interconnects"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Terminal Blocks - Wire to Board"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-shore-technology-inc/OSTTC022162/ED2609-ND/614558"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "On Shore Technology Inc."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 2.3 2.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 4 "/V_IN")
			(pintype "passive")
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(at 101.57 78.99)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U5"
			(at 3.81 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "4N25"
			(at 3.81 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83725/4n25.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 30V, CTR 20%, Viso 2500V, DIP6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 32 "Net-(U4-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 22 "Net-(Q3-C-Pad2)")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 12 "unconnected-(U5-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 14 "Net-(U3B--)")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 13 "unconnected-(U5-Pad6)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 109 89.557622 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 4.14 -1.432378 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 14 "Net-(U3B--)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 88.913333 89.557622 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "45p"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 37 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.188679)
			(net 14 "Net-(U3B--)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 78.9 105.1025)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at 0 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "MCP6002-xP"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1MHz, Low-Power Op Amp, DIP-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U2A--)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U2A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/V_IN")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U2B-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/V_OFFSET")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "/V_OFFSET")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 109 93.67)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 1.78 2.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "PRI-FEED"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 14 "Net-(U3B--)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 88.913333 96.56)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -2.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 37 "Net-(C4-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 24 "Net-(Q3-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "F.Cu")
		(at 78.9 96.70506 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -2.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 2.28 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 19 "Net-(U2A--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.192308)
			(net 26 "Net-(U3A-+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical"
		(layer "F.Cu")
		(at 131.55 96.8175)
		(descr "Potentiometer, vertical, Bourns 3299W, https://www.bourns.com/pdfs/3299.pdf")
		(tags "Potentiometer vertical Bourns 3299W")
		(property "Reference" "RV3"
			(at -2.54 -3.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.54 5.44 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Potentiometer_THT:Potentiometer_Bourns_3299W_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Potentiometer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.175 1.14 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 28 "Net-(R11-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GNDA")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -5.08 0)
			(size 1.44 1.44)
			(drill 0.8)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GNDA")
			(pinfunction "3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3299W_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:Term_Block_1x2_P5.08MM"
		(layer "F.Cu")
		(at 132.308 120.56)
		(descr "http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf")
		(property "Reference" "J3"
			(at 8.862 -3.17 0)
			(layer "F.SilkS")
		)
		(property "Value" "OSTTC022162"
			(at 2.032 5.09 0)
			(layer "F.Fab")
		)
		(property "Footprint" "digikey-footprints:Term_Block_1x2_P5.08MM"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "TERM BLK 2P SIDE ENT 5.08MM PCB"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "ED2609-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "OSTTC022162"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Category" "Connectors, Interconnects"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Family" "Terminal Blocks - Wire to Board"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.on-shore.com/wp-content/uploads/OSTTCXX2162.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-shore-technology-inc/OSTTC022162/ED2609-ND/614558"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "On Shore Technology Inc."
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 2.2 2.2)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 2 "GNDA")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 2.3 2.3)
			(drill 1.3)
			(layers "*.Cu" "*.Mask" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
				"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
				"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
				"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
				"In29.Cu" "In30.Cu"
			)
			(remove_unused_layers no)
			(net 7 "/EXT_24V")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 84.100416 89.557622)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -1.998 0)
			(layer "F.SilkS")
		)
		(property "Value" "OFFSET"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 10 "/V_OFFSET")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 71.36 74.21)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.998 0)
			(layer "F.SilkS")
		)
		(property "Value" "TARGET"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
			(net 27 "Net-(U3B-+)")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 108.9775 120.56 180)
		(descr "LED SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.82 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric_Pad1.42x1.75mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4875 0 180)
			(size 1.425 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.175439)
			(net 17 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "B.Cu")
		(at 63.98 85.5 180)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0 3.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "LT1009"
			(at 0 -3.4 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "2" smd roundrect
			(at -2.475 0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "3" smd roundrect
			(at -2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(Q1-E)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 2.475 -1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 31 "unconnected-(U1-Pad5)")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 2.475 -0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "7" smd roundrect
			(at 2.475 0.635 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "8" smd roundrect
			(at 2.475 1.905 180)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 66.26 104.65 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 2.28 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -2.28 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 18 "Net-(U2B-+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 66.26 99.53 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 2.28 0)
			(layer "B.SilkS")
		)
		(property "Value" "2k2"
			(at 0 -2.28 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 9 "Net-(R2-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(at 63.625833 76.5775 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0 2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "MMBT3906"
			(at 0 -2.4 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3906-D.PDF"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(Q1-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(Q1-B)")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 100.83 120.56)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 2.28 360)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -2.28 360)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 3 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 17 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 60.5975 69.01)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 2.28 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -2.28 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 23 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 125.41 120.56 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R17"
			(at 0 2.28 0)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -2.28 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 5 "+5VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 36 "Net-(D2-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 120.4375 100)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 2.3 180)
			(layer "B.SilkS")
		)
		(property "Value" "10u"
			(at 0 -2.3 180)
			(layer "B.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.188679)
			(net 15 "Net-(U6A-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.188679)
			(net 2 "GNDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 92.97 69.01 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 2.28 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -2.28 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 11 "Net-(R10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 3 "+5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
		(layer "B.Cu")
		(at 120.38 92.81 180)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 2.28 0)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -2.28 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_1210_3225Metric_Pad1.30x2.65mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 28 "Net-(R11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 2.65)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.192308)
			(net 15 "Net-(U6A-+)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "digikey-footprints:TO-252-3"
		(layer "B.Cu")
		(at 141.468 112.27)
		(descr "http://www.digikey.com/products/en?keywords=MC7805BDTRKGOSCT-ND")
		(property "Reference" "U7"
			(at 0 5.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "MC7805BDTRKG"
			(at 0 -5.1 0)
			(layer "B.Fab")
		)
		(property "Footprint" "digikey-footprints:TO-252-3"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MC7800-D.PDF"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "IC REG LINEAR 5V 1A DPAK"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Digi-Key_PN" "MC7805BDTRKGOSCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "MC7805BDTRKG"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Category" "Integrated Circuits (ICs)"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Family" "PMIC - Voltage Regulators - Linear"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DK_Datasheet_Link" "http://www.onsemi.com/pub/Collateral/MC7800-D.PDF"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DK_Detail_Page" "/product-detail/en/on-semiconductor/MC7805BDTRKG/MC7805BDTRKGOSCT-ND/1139742"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "ON Semiconductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Status" "Active"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.03 0.12 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -4.08 2.285 180)
			(size 3 1.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 7 "/EXT_24V")
			(pinfunction "IN")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -4.08 -2.285 180)
			(size 3 1.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 5 "+5VA")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "4" smd rect
			(at 3.09 0 180)
			(size 6.2 5.8)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GNDA")
			(pinfunction "GND")
			(pintype "power_in")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "B.Cu")
		(at 59.668 113.445 180)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.998 0)
			(layer "B.SilkS")
		)
		(property "Value" "IN"
			(at 0 -2.05 0)
			(layer "B.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 2 2)
			(layers "B.Cu" "B.Mask")
			(net 4 "/V_IN")
			(pinfunction "1")
			(pintype "passive")
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(at 56.2225 76.5775 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 2.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "MMBT3906"
			(at 0 -2.4 0)
			(layer "B.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3906-D.PDF"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "152_4_20mA_transmitter_V5_OSHPARK.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(Q2-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/V_IN")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 40 65)
		(end 170 125)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "152"
		(at 157.03 68.37 0)
		(layer "B.SilkS")
	)
	(gr_text "EXT 24V PS"
		(at 127.927144 112.08 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "PWR\nISO"
		(at 114.91 118.36 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OUT"
		(at 148.739143 115.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "R13-16\n100Ω"
		(at 145.34 88.13 0)
		(layer "F.SilkS")
	)
	(gr_text "RES"
		(at 57.225143 115.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "4-20mA Isolated Transmitter \nfor Tap-changer indication\n2025-09 az"
		(at 89 113.01 0)
		(layer "F.SilkS")
	)
	(gr_text "PWR"
		(at 106.44 118.36 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5V"
		(at 79.760858 115.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "+V"
		(at 135.516572 115.57 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OFFSET"
		(at 62.045 111.07 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "4-20mA"
		(at 148.74 112.08 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GAIN"
		(at 62.045 101.1275 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "0V"
		(at 130.650858 115.62 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Input: 0-3200 Ohm"
		(at 53.006667 68.89 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "0V"
		(at 52.930858 115.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "IN"
		(at 154.819143 115.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Output: 4-20mA"
		(at 114.04 68.89 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "0V"
		(at 74.680858 115.48 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "ADJ"
		(at 133.895 101.1275 0)
		(layer "F.SilkS" knockout)
	)
	(zone
		(net 2)
		(net_name "GNDA")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106 76) (xy 114 76) (xy 114 125) (xy 170 125) (xy 170 65) (xy 106 65)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113 125) (xy 113 77) (xy 105 77) (xy 105 65) (xy 95 65) (xy 40 65) (xy 40 125)
			)
		)
	)
)
