(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 86.233 87.249)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "main-bd-837-8952-gerbers/")
		)
	)
	(net 0 "")
	(net 1 "Net-(BT1-+)")
	(net 2 "GND")
	(net 3 "Net-(IC6-CT)")
	(net 4 "VCC2")
	(net 5 "Net-(IC16-VCC)")
	(net 6 "LRCKB")
	(net 7 "25M")
	(net 8 "CDCK")
	(net 9 "Net-(CN1-Pin_2)")
	(net 10 "Net-(CN1-Pin_3)")
	(net 11 "Net-(CN1-Pin_5)")
	(net 12 "Net-(CN1-Pin_6)")
	(net 13 "Net-(CN1-Pin_7)")
	(net 14 "Net-(CN1-Pin_8)")
	(net 15 "Net-(CN1-Pin_9)")
	(net 16 "Net-(CN1-Pin_10)")
	(net 17 "BCLK")
	(net 18 "SDATA")
	(net 19 "LRCK")
	(net 20 "DFCK")
	(net 21 "unconnected-(CN1-Pin_15-Pad15)")
	(net 22 "unconnected-(CN1-Pin_16-Pad16)")
	(net 23 "Net-(CN1-Pin_17)")
	(net 24 "SBSO")
	(net 25 "unconnected-(CN1-Pin_19-Pad19)")
	(net 26 "SCOR")
	(net 27 "WFCK")
	(net 28 "M.VCC")
	(net 29 "M.GND")
	(net 30 "Net-(CN3-Pin_19)")
	(net 31 "~{ERES}")
	(net 32 "BCLKB")
	(net 33 "DFCKB")
	(net 34 "DDATA")
	(net 35 "ATT")
	(net 36 "SHFT")
	(net 37 "LATCH")
	(net 38 "VCC")
	(net 39 "PDATA")
	(net 40 "PWCLK")
	(net 41 "PBCLK")
	(net 42 "PLRCK")
	(net 43 "SL2")
	(net 44 "SR2")
	(net 45 "12M")
	(net 46 "Net-(IC2-12M)")
	(net 47 "50M")
	(net 48 "Net-(IC2-25M)")
	(net 49 "D4")
	(net 50 "D3")
	(net 51 "D2")
	(net 52 "D1")
	(net 53 "D0")
	(net 54 "~{AS}")
	(net 55 "~{UDS}")
	(net 56 "~{LDS}")
	(net 57 "R{slash}~{W}")
	(net 58 "~{DTAK}")
	(net 59 "unconnected-(IC1-BG-Pad11)")
	(net 60 "unconnected-(IC1-NC-Pad18)")
	(net 61 "~{HALT}")
	(net 62 "~{RES}")
	(net 63 "unconnected-(IC1-VMA-Pad21)")
	(net 64 "~{VPA}")
	(net 65 "unconnected-(IC1-FC2-Pad28)")
	(net 66 "FC1")
	(net 67 "FC0")
	(net 68 "unconnected-(IC1-NC-Pad31)")
	(net 69 "A1")
	(net 70 "A2")
	(net 71 "A3")
	(net 72 "A4")
	(net 73 "A5")
	(net 74 "A6")
	(net 75 "A7")
	(net 76 "A8")
	(net 77 "A9")
	(net 78 "A10")
	(net 79 "A11")
	(net 80 "A12")
	(net 81 "A13")
	(net 82 "A14")
	(net 83 "A15")
	(net 84 "A16")
	(net 85 "A17")
	(net 86 "A18")
	(net 87 "A19")
	(net 88 "unconnected-(IC1-A20-Pad51)")
	(net 89 "unconnected-(IC1-A21-Pad53)")
	(net 90 "unconnected-(IC1-A22-Pad54)")
	(net 91 "unconnected-(IC1-A23-Pad55)")
	(net 92 "D15")
	(net 93 "D14")
	(net 94 "D13")
	(net 95 "D12")
	(net 96 "D11")
	(net 97 "D10")
	(net 98 "D9")
	(net 99 "D8")
	(net 100 "D7")
	(net 101 "D6")
	(net 102 "D5")
	(net 103 "~{BRAM}")
	(net 104 "~{BROM}")
	(net 105 "~{ROM}")
	(net 106 "~{CAS0}")
	(net 107 "~{LWR}")
	(net 108 "~{UWR}")
	(net 109 "~{ASEL}")
	(net 110 "~{CAS2}")
	(net 111 "~{FDC}")
	(net 112 "FRES")
	(net 113 "Net-(IC2-EAD0)")
	(net 114 "Net-(IC2-EAD1)")
	(net 115 "Net-(IC2-EAD2)")
	(net 116 "Net-(IC2-EAD3)")
	(net 117 "Net-(IC2-EAD4)")
	(net 118 "Net-(IC2-EAD5)")
	(net 119 "Net-(IC2-EAD6)")
	(net 120 "Net-(IC2-EAD7)")
	(net 121 "Net-(IC2-ED8)")
	(net 122 "Net-(IC2-ED9)")
	(net 123 "Net-(IC2-ED10)")
	(net 124 "Net-(IC2-ED11)")
	(net 125 "Net-(IC2-ED12)")
	(net 126 "Net-(IC2-ED13)")
	(net 127 "Net-(IC2-ED14)")
	(net 128 "Net-(IC2-ED15)")
	(net 129 "~{ERAS}")
	(net 130 "~{ECAS}")
	(net 131 "~{EOE}")
	(net 132 "~{ORAS}")
	(net 133 "~{OCAS}")
	(net 134 "~{OOE}")
	(net 135 "~{OWE}")
	(net 136 "Net-(IC2-OAD0)")
	(net 137 "Net-(IC2-OAD1)")
	(net 138 "Net-(IC2-OAD2)")
	(net 139 "Net-(IC2-OAD3)")
	(net 140 "Net-(IC2-OAD4)")
	(net 141 "Net-(IC2-OAD5)")
	(net 142 "Net-(IC2-OAD6)")
	(net 143 "Net-(IC2-OAD7)")
	(net 144 "Net-(IC2-OD8)")
	(net 145 "Net-(IC2-OD9)")
	(net 146 "Net-(IC2-OD10)")
	(net 147 "Net-(IC2-OD11)")
	(net 148 "Net-(IC2-OD12)")
	(net 149 "Net-(IC2-OD13)")
	(net 150 "Net-(IC2-OD14)")
	(net 151 "Net-(IC2-OD15)")
	(net 152 "Net-(IC2-LEDR)")
	(net 153 "Net-(IC2-LEDG)")
	(net 154 "WFCKD")
	(net 155 "SCORB")
	(net 156 "SBSOB")
	(net 157 "SDATAB")
	(net 158 "CDCKD")
	(net 159 "~{PCM}")
	(net 160 "~{DTEN}")
	(net 161 "~{WAIT}")
	(net 162 "~{HRD}")
	(net 163 "~{INT}")
	(net 164 "~{CDC}")
	(net 165 "~{COE}")
	(net 166 "C2LR")
	(net 167 "PA8")
	(net 168 "PA7")
	(net 169 "PA6")
	(net 170 "PA5")
	(net 171 "PA4")
	(net 172 "PA3")
	(net 173 "PA2")
	(net 174 "PA1")
	(net 175 "PA0")
	(net 176 "~{PRAS}")
	(net 177 "~{PCAS}")
	(net 178 "~{CUWE}")
	(net 179 "VA1")
	(net 180 "VA2")
	(net 181 "VA3")
	(net 182 "VA4")
	(net 183 "VA5")
	(net 184 "VA6")
	(net 185 "VA7")
	(net 186 "VA8")
	(net 187 "VA9")
	(net 188 "VA10")
	(net 189 "VA11")
	(net 190 "VA12")
	(net 191 "VA13")
	(net 192 "VA14")
	(net 193 "VA15")
	(net 194 "VA16")
	(net 195 "VA17")
	(net 196 "VD0")
	(net 197 "VD1")
	(net 198 "VD2")
	(net 199 "VD3")
	(net 200 "VD4")
	(net 201 "VD5")
	(net 202 "VD6")
	(net 203 "VD7")
	(net 204 "VD8")
	(net 205 "VD9")
	(net 206 "VD10")
	(net 207 "VD11")
	(net 208 "VD12")
	(net 209 "VD13")
	(net 210 "VD14")
	(net 211 "VD15")
	(net 212 "unconnected-(IC3-N.C.-Pad11)")
	(net 213 "unconnected-(IC3-N.C.-Pad20)")
	(net 214 "unconnected-(IC3-SHL-Pad29)")
	(net 215 "unconnected-(IC3-SHR-Pad30)")
	(net 216 "unconnected-(IC3-DAC7-Pad31)")
	(net 217 "unconnected-(IC3-DAC6-Pad32)")
	(net 218 "unconnected-(IC3-DAC5-Pad33)")
	(net 219 "unconnected-(IC3-DAC4-Pad34)")
	(net 220 "unconnected-(IC3-DAC3-Pad37)")
	(net 221 "unconnected-(IC3-DAC7L-Pad38)")
	(net 222 "unconnected-(IC3-DAC7R-Pad39)")
	(net 223 "unconnected-(IC3-RAMAX-Pad42)")
	(net 224 "/WD7")
	(net 225 "/WD6")
	(net 226 "/WD4")
	(net 227 "/WD2")
	(net 228 "/WD1")
	(net 229 "/WD0")
	(net 230 "/RA14")
	(net 231 "/RA13")
	(net 232 "/RA12")
	(net 233 "/RA11")
	(net 234 "/RA10")
	(net 235 "/RA9")
	(net 236 "/RA8")
	(net 237 "~{RAS2X}")
	(net 238 "~{CLWEX}")
	(net 239 "~{RCS1X}")
	(net 240 "Net-(IC10-~{WE})")
	(net 241 "/RA7")
	(net 242 "/RA6")
	(net 243 "/RA5")
	(net 244 "/RA4")
	(net 245 "unconnected-(IC3-XOUT-Pad71)")
	(net 246 "/RA3")
	(net 247 "/RA2")
	(net 248 "/RA1")
	(net 249 "/RA0")
	(net 250 "unconnected-(IC6-N.C.-Pad1)")
	(net 251 "unconnected-(IC6-VBAT1-Pad2)")
	(net 252 "unconnected-(IC6-~{ALARM1}-Pad6)")
	(net 253 "unconnected-(IC6-~{ALARM2}-Pad7)")
	(net 254 "unconnected-(IC6-RESET-Pad9)")
	(net 255 "~{EWE}")
	(net 256 "/RAA6")
	(net 257 "/RAA7")
	(net 258 "/RAA8")
	(net 259 "/RAA9")
	(net 260 "/RAA10")
	(net 261 "/RAA11")
	(net 262 "/RAA12")
	(net 263 "Net-(IC16-CS2)")
	(net 264 "unconnected-(IC6-VSENSE-Pad12)")
	(net 265 "unconnected-(IC6-N.C.-Pad15)")
	(net 266 "unconnected-(IC7-N.C.-Pad1)")
	(net 267 "unconnected-(IC7-N.C.-Pad20)")
	(net 268 "/CD7")
	(net 269 "/CD6")
	(net 270 "/CD5")
	(net 271 "/CD4")
	(net 272 "/CD3")
	(net 273 "/CD2")
	(net 274 "/CD1")
	(net 275 "/CD0")
	(net 276 "unconnected-(IC7-N.C.-Pad31)")
	(net 277 "unconnected-(IC7-N.C.-Pad32)")
	(net 278 "unconnected-(IC7-N.C.-Pad37)")
	(net 279 "unconnected-(IC8-N.C.-Pad1)")
	(net 280 "unconnected-(IC8-N.C.-Pad20)")
	(net 281 "unconnected-(IC8-N.C.-Pad31)")
	(net 282 "/RAA0")
	(net 283 "/RAA1")
	(net 284 "/RAA2")
	(net 285 "/RAA3")
	(net 286 "/RAA4")
	(net 287 "/RAA5")
	(net 288 "Net-(LD1-K)")
	(net 289 "Net-(LD1-A)")
	(net 290 "Net-(LD2-K)")
	(net 291 "Net-(LD2-A)")
	(net 292 "unconnected-(OSC1-EN-Pad1)")
	(net 293 "Net-(TR2-B)")
	(net 294 "Net-(TR1-B)")
	(net 295 "unconnected-(CN2-Pin_a27-Pada27)")
	(net 296 "unconnected-(CN2-Pin_a28-Pada28)")
	(net 297 "unconnected-(CN2-Pin_b24-Padb24)")
	(net 298 "unconnected-(CN2-Pin_b25-Padb25)")
	(net 299 "unconnected-(CN2-Pin_b27-Padb27)")
	(net 300 "unconnected-(CN2-Pin_b28-Padb28)")
	(net 301 "~{RCS2X}")
	(net 302 "~{ROE}")
	(net 303 "~{RAACS1}")
	(net 304 "BCK")
	(net 305 "~{RAACS2}")
	(net 306 "unconnected-(IC8-N.C.-Pad32)")
	(net 307 "unconnected-(IC8-N.C.-Pad37)")
	(net 308 "E")
	(net 309 "~{IPL2}")
	(net 310 "~{IPL1}")
	(net 311 "~{IPL0}")
	(net 312 "unconnected-(IC12-Pad11)")
	(net 313 "unconnected-(IC13-RA14-Pad10)")
	(net 314 "unconnected-(IC13-RA15-Pad11)")
	(net 315 "Net-(IC13-~{RWE})")
	(net 316 "Net-(IC13-~{ROE})")
	(net 317 "unconnected-(IC13-ERA-Pad15)")
	(net 318 "unconnected-(IC13-XTAL-Pad26)")
	(net 319 "unconnected-(IC13-MCK-Pad37)")
	(net 320 "unconnected-(IC13-~{STEN}-Pad60)")
	(net 321 "unconnected-(IC13-~{EOP}-Pad61)")
	(net 322 "Net-(IC13-~{RCS})")
	(net 323 "unconnected-(IC13-~{HDE}-Pad63)")
	(net 324 "unconnected-(IC14-N.C.-Pad1)")
	(net 325 "Net-(OSC1-OUT)")
	(net 326 "~{RAS2}")
	(net 327 "~{CLWE}")
	(net 328 "unconnected-(IC15-N.C.-Pad1)")
	(net 329 "unconnected-(IC16-N.C.-Pad1)")
	(net 330 "unconnected-(IC17B-~{Q}-Pad8)")
	(net 331 "unconnected-(IC17B-Q-Pad9)")
	(net 332 "unconnected-(IC5-N.C.-Pad11)")
	(net 333 "unconnected-(IC5-N.C.-Pad15)")
	(net 334 "unconnected-(IC5-N.C.-Pad29)")
	(net 335 "unconnected-(IC5-N.C.-Pad30)")
	(net 336 "LRCKBF")
	(net 337 "WD3")
	(net 338 "RAS2")
	(net 339 "PBCLKF")
	(net 340 "~{CLWEY}")
	(net 341 "BCLKBF")
	(net 342 "DFCKBF")
	(net 343 "WD5F")
	(net 344 "WD5")
	(net 345 "unconnected-(CN2-Pin_a2-Pada2)")
	(net 346 "VCC2C")
	(net 347 "VCC2B")
	(footprint "Oscillator:Oscillator_DIP-14"
		(layer "F.Cu")
		(at 187.071 76.6318)
		(descr "Oscillator, DIP14, http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
		(tags "oscillator")
		(property "Reference" "OSC1"
			(at 16.3576 3.9624 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50MHz"
			(at 7.62 3.74 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 -3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 292 "unconnected-(OSC1-EN-Pad1)")
			(pinfunction "EN")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole circle
			(at 15.24 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "Net-(OSC1-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "14" thru_hole circle
			(at 0 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_DIP-14.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:ZIP-40"
		(layer "F.Cu")
		(at 216.281 122.301 180)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC7"
			(at 5.207 27.3812 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TC511664BZ"
			(at 1.27 52.07 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 266 "unconnected-(IC7-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" thru_hole oval
			(at 2.54 1.27 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "Net-(IC2-ED8)")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "Net-(IC2-ED9)")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 2.54 3.81 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "Net-(IC2-ED10)")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "Net-(IC2-ED11)")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 2.54 6.35 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "Net-(IC2-ED12)")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(IC2-ED13)")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 2.54 8.89 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "Net-(IC2-ED14)")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(IC2-ED15)")
			(pinfunction "D15")
			(pintype "tri_state")
		)
		(pad "10" thru_hole oval
			(at 2.54 11.43 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 0 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "Net-(IC2-EAD0)")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 2.54 13.97 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "Net-(IC2-EAD1)")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 0 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at 2.54 16.51 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "Net-(IC2-EAD2)")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 0 17.78 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "Net-(IC2-EAD3)")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 2.54 19.05 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "Net-(IC2-EAD4)")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 0 20.32 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "Net-(IC2-EAD5)")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 2.54 21.59 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "Net-(IC2-EAD6)")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 0 22.86 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "Net-(IC2-EAD7)")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 2.54 24.13 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 267 "unconnected-(IC7-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "21" thru_hole oval
			(at 0 25.4 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "22" thru_hole oval
			(at 2.54 26.67 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 255 "~{EWE}")
			(pinfunction "~{UWE}")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 0 27.94 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 255 "~{EWE}")
			(pinfunction "~{LWE}")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 2.54 29.21 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "~{ERAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 0 30.48 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "Net-(IC2-EAD0)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 2.54 31.75 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "Net-(IC2-EAD1)")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 0 33.02 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "Net-(IC2-EAD2)")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 2.54 34.29 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "Net-(IC2-EAD3)")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "29" thru_hole oval
			(at 0 35.56 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "Net-(IC2-EAD4)")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "30" thru_hole oval
			(at 2.54 36.83 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole oval
			(at 0 38.1 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "unconnected-(IC7-N.C.-Pad31)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "32" thru_hole oval
			(at 2.54 39.37 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 277 "unconnected-(IC7-N.C.-Pad32)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "33" thru_hole oval
			(at 0 40.64 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" thru_hole oval
			(at 2.54 41.91 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "Net-(IC2-EAD5)")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "35" thru_hole oval
			(at 0 43.18 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "Net-(IC2-EAD6)")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "36" thru_hole oval
			(at 2.54 44.45 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "Net-(IC2-EAD7)")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "37" thru_hole oval
			(at 0 45.72 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 278 "unconnected-(IC7-N.C.-Pad37)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "38" thru_hole oval
			(at 2.54 46.99 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "~{EOE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "39" thru_hole oval
			(at 0 48.26 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "~{ECAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "40" thru_hole oval
			(at 2.54 49.53 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P7.00mm"
		(layer "F.Cu")
		(at 175.895 79.756)
		(property "Reference" "FB3"
			(at 4.445 -4.318 0)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "12M")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 7 0)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(IC2-12M)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:EM_Filter_Flipped"
		(layer "F.Cu")
		(at 162.433 115.57 90)
		(property "Reference" "EM2"
			(at 5.969 2.54 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "EMI filter, single capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 347 "VCC2B")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:FB_P7.00mm"
		(layer "F.Cu")
		(at 151.0642 110.871)
		(property "Reference" "FB14"
			(at 4.9172 -5.9436 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "DFCKB")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 7 0)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 342 "DFCKBF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 117.475 77.216 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C47"
			(at -0.9652 -3.1242 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.191 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 154.178 77.905 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C41"
			(at 0.4096 3.0734 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -3.375 3.302 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 346 "VCC2C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:EM_Filter"
		(layer "F.Cu")
		(at 156.083 85.471 -90)
		(property "Reference" "EM1"
			(at 6.7564 1.6764 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "EMI filter, single capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0 270)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 346 "VCC2C")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SOIC-14W_5.3mm_P1.27mm"
		(layer "F.Cu")
		(at 201.676 59.823 90)
		(descr "16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "IC17"
			(at 7.753 -3.302 180)
			(layer "F.SilkS")
		)
		(property "Value" "74AC74"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual D Flip-flop, Set & Reset"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0.895 0.127 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -0.762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{R}")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 237 "~{RAS2X}")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "50M")
			(pinfunction "C")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{S}")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 326 "~{RAS2}")
			(pinfunction "Q")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 338 "RAS2")
			(pinfunction "~{Q}")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 3.556 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 330 "unconnected-(IC17B-~{Q}-Pad8)")
			(pinfunction "~{Q}")
			(pintype "output+no_connect")
		)
		(pad "9" smd rect
			(at 3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 331 "unconnected-(IC17B-Q-Pad9)")
			(pinfunction "Q")
			(pintype "output+no_connect")
		)
		(pad "10" smd rect
			(at 3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{S}")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "C")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{R}")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_5.3x10.2mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P9.00mm"
		(layer "F.Cu")
		(at 118.618 100.821 90)
		(property "Reference" "FB15"
			(at 1.634 -3.81 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "PBCLK")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 9 0 90)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 339 "PBCLKF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-14W_5.3mm_P1.27mm"
		(layer "F.Cu")
		(at 88.9 66.554 90)
		(descr "16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "IC12"
			(at 7.8546 -1.4478 180)
			(layer "F.SilkS")
		)
		(property "Value" "74HC86"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad 2-input XOR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 327 "~{CLWE}")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 340 "~{CLWEY}")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "~{RAACS1}")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 305 "~{RAACS2}")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 3.556 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 304 "BCK")
			(pintype "output")
		)
		(pad "9" smd rect
			(at 3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 341 "BCLKBF")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 312 "unconnected-(IC12-Pad11)")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at 3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_5.3x10.2mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CON-25P-ANGLE"
		(layer "F.Cu")
		(at 108.758 128.651)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "CN1"
			(at 17.3022 -4.2672 0)
			(layer "F.SilkS")
		)
		(property "Value" "CON 25P ANGLE"
			(at 19.05 2.54 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x25, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "24"
			(at 29.672 -4.572 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at 29.672 -3.175 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -4.1354 0.8128 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -4.1354 -1.016 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 2.54 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "CDCK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 1.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 9 "Net-(CN1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 2.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 10 "Net-(CN1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole roundrect
			(at 3.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 31 "~{ERES}")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at 5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 11 "Net-(CN1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole roundrect
			(at 6.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 12 "Net-(CN1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole roundrect
			(at 7.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 13 "Net-(CN1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole roundrect
			(at 8.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 14 "Net-(CN1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole roundrect
			(at 10 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 15 "Net-(CN1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole roundrect
			(at 11.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 16 "Net-(CN1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole roundrect
			(at 12.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 17 "BCLK")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole roundrect
			(at 13.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 18 "SDATA")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole roundrect
			(at 15 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 19 "LRCK")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole roundrect
			(at 16.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 20 "DFCK")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole roundrect
			(at 17.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 21 "unconnected-(CN1-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole roundrect
			(at 18.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 22 "unconnected-(CN1-Pin_16-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
		)
		(pad "17" thru_hole roundrect
			(at 20 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 23 "Net-(CN1-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole roundrect
			(at 21.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 24 "SBSO")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole roundrect
			(at 22.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 25 "unconnected-(CN1-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole roundrect
			(at 23.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 26 "SCOR")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole roundrect
			(at 25 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole roundrect
			(at 26.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 27 "WFCK")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole roundrect
			(at 27.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole roundrect
			(at 28.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 28 "M.VCC")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole roundrect
			(at 30 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 29 "M.GND")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P7.00mm"
		(layer "F.Cu")
		(at 172.6946 123.8354 -90)
		(property "Reference" "FB1"
			(at -2.0424 -1.778 180)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(IC2-25M)")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 7 0 270)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "25M")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 173.863 67.31 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC16"
			(at 6.223 -11.938 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB8464A-10L"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 329 "unconnected-(IC16-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "A13")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "A8")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "A7")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "A6")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "A5")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "A4")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "A3")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "A2")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "A1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "~{BRAM}")
			(pinfunction "~{CS1}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "A11")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "~{COE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "A12")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "A10")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "A9")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "Net-(IC16-CS2)")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 327 "~{CLWE}")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(IC16-VCC)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P7.00mm"
		(layer "F.Cu")
		(at 151.0642 117.2718)
		(property "Reference" "FB12"
			(at 4.9172 -10.8712 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "BCLKB")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 7 0)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 341 "BCLKBF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOJ-40-Export"
		(layer "F.Cu")
		(at 122.428 120.396 90)
		(property "Reference" "IC5"
			(at 9.9822 -1.8542 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HM514270"
			(at 6.223 27.686 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 5.715 13.335 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 5.842 13.081 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0.635 1.27 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0.635 2.54 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at 0.635 3.81 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at 0.635 5.08 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "5" smd rect
			(at 0.635 6.35 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "6" smd rect
			(at 0.635 7.62 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "7" smd rect
			(at 0.635 8.89 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "8" smd rect
			(at 0.635 10.16 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "9" smd rect
			(at 0.635 11.43 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "10" smd rect
			(at 0.635 12.7 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "11" smd rect
			(at 0.635 13.97 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 332 "unconnected-(IC5-N.C.-Pad11)")
			(pinfunction "N.C.")
			(pintype "no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "12" smd rect
			(at 0.635 15.24 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 327 "~{CLWE}")
			(pinfunction "~{LWE}")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "13" smd rect
			(at 0.635 16.51 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 178 "~{CUWE}")
			(pinfunction "~{UWE}")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "14" smd rect
			(at 0.635 17.78 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 176 "~{PRAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "15" smd rect
			(at 0.635 19.05 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 333 "unconnected-(IC5-N.C.-Pad15)")
			(pinfunction "N.C.")
			(pintype "no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "16" smd rect
			(at 0.635 20.32 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 175 "PA0")
			(pinfunction "A0")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "17" smd rect
			(at 0.635 21.59 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 174 "PA1")
			(pinfunction "A1")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "18" smd rect
			(at 0.635 22.86 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 173 "PA2")
			(pinfunction "A2")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "19" smd rect
			(at 0.635 24.13 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "PA3")
			(pinfunction "A3")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "20" smd rect
			(at 0.635 25.4 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "21" smd rect
			(at 10.795 25.4 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "22" smd rect
			(at 10.795 24.13 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "PA4")
			(pinfunction "A4")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "23" smd rect
			(at 10.795 22.86 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "PA5")
			(pinfunction "A5")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "24" smd rect
			(at 10.795 21.59 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "PA6")
			(pinfunction "A6")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "25" smd rect
			(at 10.795 20.32 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "PA7")
			(pinfunction "A7")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "26" smd rect
			(at 10.795 19.05 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 167 "PA8")
			(pinfunction "A7")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "27" smd rect
			(at 10.795 17.78 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "~{COE}")
			(pinfunction "~{OE}")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "28" smd rect
			(at 10.795 16.51 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 177 "~{PCAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
			(thermal_bridge_angle 45)
		)
		(pad "29" smd rect
			(at 10.795 15.24 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 334 "unconnected-(IC5-N.C.-Pad29)")
			(pinfunction "N.C.")
			(pintype "no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "30" smd rect
			(at 10.795 13.97 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 335 "unconnected-(IC5-N.C.-Pad30)")
			(pinfunction "N.C.")
			(pintype "no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "31" smd rect
			(at 10.795 12.7 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "D8")
			(pinfunction "D8")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "32" smd rect
			(at 10.795 11.43 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "D9")
			(pinfunction "D9")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "33" smd rect
			(at 10.795 10.16 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "D10")
			(pinfunction "D10")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "34" smd rect
			(at 10.795 8.89 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "D11")
			(pinfunction "D11")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "35" smd rect
			(at 10.795 7.62 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(pad "36" smd rect
			(at 10.795 6.35 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "D12")
			(pinfunction "D12")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "37" smd rect
			(at 10.795 5.08 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "D13")
			(pinfunction "D13")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "38" smd rect
			(at 10.795 3.81 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "D14")
			(pinfunction "D14")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "39" smd rect
			(at 10.795 2.54 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "D15")
			(pinfunction "D15")
			(pintype "tri_state")
			(thermal_bridge_angle 45)
		)
		(pad "40" smd rect
			(at 10.795 1.27 90)
			(size 2.667 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:EM_Filter"
		(layer "F.Cu")
		(at 89.535 128.671)
		(property "Reference" "EM3"
			(at -6.7564 -0.8836 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "EMI filter, single capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 0)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.8 1.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:FB_P7.00mm"
		(layer "F.Cu")
		(at 97.409 64.897 -90)
		(property "Reference" "FB16"
			(at -3.9116 0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 344 "WD5")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 7 0 270)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 343 "WD5F")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P5.00mm"
		(layer "F.Cu")
		(at 55.245 80.471 -90)
		(property "Reference" "FB17"
			(at 2.3584 3.2512 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 2.5 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pintype "passive")
			(clearance 0.2)
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(CN3-Pin_19)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P7.00mm"
		(layer "F.Cu")
		(at 180.213 130.825 90)
		(property "Reference" "FB13"
			(at 9.159 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 2.5 2.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "LRCKB")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 7 0 90)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 336 "LRCKBF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:C_Radial_5mm"
		(layer "F.Cu")
		(at 55.245 73.366 -90)
		(property "Reference" "C52"
			(at -5.4718 2.54 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at 2.707 -0.381 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 2.5 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -2.5 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SOIC-20W_7.5x12.8mm_P1.27mm_narrowed"
		(layer "F.Cu")
		(at 157.2768 126.238 90)
		(descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC9"
			(at -5.2578 8.4074 0)
			(layer "F.SilkS")
		)
		(property "Value" "74HC245"
			(at 0 7.35 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.683 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.683 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "SDATAB")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -3.683 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "DFCKB")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -3.683 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "LRCKB")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -3.683 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "BCLKB")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -3.683 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "SBSOB")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -3.683 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "SCORB")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -3.683 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "WFCKD")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -3.683 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "CDCKD")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -3.683 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 3.683 5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "CDCK")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 3.683 4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "WFCK")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 3.683 3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "SCOR")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 3.683 1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "SBSO")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 3.683 0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "BCLK")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 3.683 -0.635 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "LRCK")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 3.683 -1.905 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "DFCK")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 3.683 -3.175 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "SDATA")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 3.683 -4.445 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 3.683 -5.715 90)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 347 "VCC2B")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:ZIP-40"
		(layer "F.Cu")
		(at 223.266 122.301 180)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC8"
			(at -3.175 25.8064 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TC511664BZ"
			(at 1.27 52.07 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 279 "unconnected-(IC8-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" thru_hole oval
			(at 2.54 1.27 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 144 "Net-(IC2-OD8)")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 145 "Net-(IC2-OD9)")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 2.54 3.81 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 146 "Net-(IC2-OD10)")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 147 "Net-(IC2-OD11)")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 2.54 6.35 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 148 "Net-(IC2-OD12)")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "Net-(IC2-OD13)")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 2.54 8.89 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 150 "Net-(IC2-OD14)")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 151 "Net-(IC2-OD15)")
			(pinfunction "D15")
			(pintype "tri_state")
		)
		(pad "10" thru_hole oval
			(at 2.54 11.43 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 0 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "Net-(IC2-OAD0)")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 2.54 13.97 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(IC2-OAD1)")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 0 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at 2.54 16.51 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Net-(IC2-OAD2)")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 0 17.78 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(IC2-OAD3)")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 2.54 19.05 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(IC2-OAD4)")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 0 20.32 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(IC2-OAD5)")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 2.54 21.59 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "Net-(IC2-OAD6)")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 0 22.86 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 143 "Net-(IC2-OAD7)")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 2.54 24.13 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 280 "unconnected-(IC8-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "21" thru_hole oval
			(at 0 25.4 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "22" thru_hole oval
			(at 2.54 26.67 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "~{OWE}")
			(pinfunction "~{UWE}")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 0 27.94 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "~{OWE}")
			(pinfunction "~{LWE}")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 2.54 29.21 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "~{ORAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 0 30.48 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "Net-(IC2-OAD0)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 2.54 31.75 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(IC2-OAD1)")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 0 33.02 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Net-(IC2-OAD2)")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 2.54 34.29 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(IC2-OAD3)")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "29" thru_hole oval
			(at 0 35.56 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(IC2-OAD4)")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "30" thru_hole oval
			(at 2.54 36.83 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole oval
			(at 0 38.1 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 281 "unconnected-(IC8-N.C.-Pad31)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "32" thru_hole oval
			(at 2.54 39.37 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 306 "unconnected-(IC8-N.C.-Pad32)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "33" thru_hole oval
			(at 0 40.64 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" thru_hole oval
			(at 2.54 41.91 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(IC2-OAD5)")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "35" thru_hole oval
			(at 0 43.18 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "Net-(IC2-OAD6)")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "36" thru_hole oval
			(at 2.54 44.45 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 143 "Net-(IC2-OAD7)")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "37" thru_hole oval
			(at 0 45.72 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "unconnected-(IC8-N.C.-Pad37)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "38" thru_hole oval
			(at 2.54 46.99 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "~{OOE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "39" thru_hole oval
			(at 0 48.26 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "~{OCAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "40" thru_hole oval
			(at 2.54 49.53 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PQFP-80_14x20mm_P0.8mm_long_pads"
		(layer "F.Cu")
		(at 99.695 111.664 90)
		(descr "PQFP80 14x20 / QIP80E CASE 122BS (see ON Semiconductor 122BS.PDF)")
		(tags "QFP 0.8")
		(property "Reference" "IC13"
			(at -11.907 -12.573 180)
			(layer "F.SilkS")
		)
		(property "Value" "LC8951"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "25"
			(at -10.764 14.351 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "•"
			(at 10.2616 5.4102 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at -8.351 -16.51 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "64"
			(at 11.461 -11.938 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "40"
			(at 8.286 15.113 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "65"
			(at 6.836 -16.503 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -13.304 -8.636 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at -12.542 10.668 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "41"
			(at 11.334 8.763 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at -9.142 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.146 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at -9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 256 "/RAA6")
			(pinfunction "RA6")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 257 "/RAA7")
			(pinfunction "RA7")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 258 "/RAA8")
			(pinfunction "RA8")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 259 "/RAA9")
			(pinfunction "RA9")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 260 "/RAA10")
			(pinfunction "RA10")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 261 "/RAA11")
			(pinfunction "RA11")
			(pintype "output")
		)
		(pad "8" smd rect
			(at -9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 262 "/RAA12")
			(pinfunction "RA12")
			(pintype "output")
		)
		(pad "9" smd rect
			(at -9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "~{RAACS1}")
			(pinfunction "RA13")
			(pintype "output")
		)
		(pad "10" smd rect
			(at -9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 313 "unconnected-(IC13-RA14-Pad10)")
			(pinfunction "RA14")
			(pintype "output+no_connect")
		)
		(pad "11" smd rect
			(at -9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 314 "unconnected-(IC13-RA15-Pad11)")
			(pinfunction "RA15")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at -9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 315 "Net-(IC13-~{RWE})")
			(pinfunction "~{RWE}")
			(pintype "output")
		)
		(pad "13" smd rect
			(at -9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at -9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 316 "Net-(IC13-~{ROE})")
			(pinfunction "~{ROE}")
			(pintype "output")
		)
		(pad "15" smd rect
			(at -9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 317 "unconnected-(IC13-ERA-Pad15)")
			(pinfunction "ERA")
			(pintype "passive+no_connect")
		)
		(pad "16" smd rect
			(at -9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 268 "/CD7")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -9.017 3.58 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 269 "/CD6")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 270 "/CD5")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at -9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 271 "/CD4")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 272 "/CD3")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at -9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 273 "/CD2")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at -9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "/CD1")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at -9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 275 "/CD0")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at -9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "25" smd rect
			(at -6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "25M")
			(pinfunction "XTALCK")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 318 "unconnected-(IC13-XTAL-Pad26)")
			(pinfunction "XTAL")
			(pintype "input+no_connect")
		)
		(pad "27" smd rect
			(at -4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST1")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at -3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST2")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CSEL")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "LMSEL")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "32" smd rect
			(at -0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 336 "LRCKBF")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "33" smd rect
			(at 0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "SDATAB")
			(pinfunction "SDATA")
			(pintype "input")
		)
		(pad "34" smd rect
			(at 1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 304 "BCK")
			(pinfunction "BCK")
			(pintype "input")
		)
		(pad "35" smd rect
			(at 2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "36" smd rect
			(at 2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "C2LR")
			(pinfunction "C2PO")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 319 "unconnected-(IC13-MCK-Pad37)")
			(pinfunction "MCK")
			(pintype "input+no_connect")
		)
		(pad "38" smd rect
			(at 4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "40" smd rect
			(at 6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at 9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "42" smd rect
			(at 9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "43" smd rect
			(at 9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "44" smd rect
			(at 9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "45" smd rect
			(at 9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "46" smd rect
			(at 9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "47" smd rect
			(at 9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "A1")
			(pinfunction "RS")
			(pintype "input")
		)
		(pad "48" smd rect
			(at 9.017 3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "~{COE}")
			(pinfunction "~{RD}")
			(pintype "input")
		)
		(pad "49" smd rect
			(at 9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 327 "~{CLWE}")
			(pinfunction "~{WR}")
			(pintype "input")
		)
		(pad "50" smd rect
			(at 9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "~{CDC}")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "51" smd rect
			(at 9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "~{INT}")
			(pinfunction "~{INT}")
			(pintype "input")
		)
		(pad "52" smd rect
			(at 9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "~{ERES}")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "54" smd rect
			(at 9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "~{ENABLE}")
			(pintype "input")
		)
		(pad "55" smd rect
			(at 9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{HWR}")
			(pintype "input")
		)
		(pad "56" smd rect
			(at 9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "~{HRD}")
			(pinfunction "~{HRD}")
			(pintype "input")
		)
		(pad "57" smd rect
			(at 9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{CMD}")
			(pintype "input")
		)
		(pad "58" smd rect
			(at 9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "~{WAIT}")
			(pinfunction "~{WAIT}")
			(pintype "input")
		)
		(pad "59" smd rect
			(at 9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "~{DTEN}")
			(pinfunction "~{DTEN}")
			(pintype "input")
		)
		(pad "60" smd rect
			(at 9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 320 "unconnected-(IC13-~{STEN}-Pad60)")
			(pinfunction "~{STEN}")
			(pintype "input+no_connect")
		)
		(pad "61" smd rect
			(at 9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 321 "unconnected-(IC13-~{EOP}-Pad61)")
			(pinfunction "~{EOP}")
			(pintype "input+no_connect")
		)
		(pad "62" smd rect
			(at 9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 322 "Net-(IC13-~{RCS})")
			(pinfunction "~{RCS}")
			(pintype "output")
		)
		(pad "63" smd rect
			(at 9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 323 "unconnected-(IC13-~{HDE}-Pad63)")
			(pinfunction "~{HDE}")
			(pintype "input+no_connect")
		)
		(pad "64" smd rect
			(at 9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "65" smd rect
			(at 6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "PA7")
			(pinfunction "HD7")
			(pintype "bidirectional")
		)
		(pad "66" smd rect
			(at 5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "PA6")
			(pinfunction "HD6")
			(pintype "bidirectional")
		)
		(pad "67" smd rect
			(at 4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "PA5")
			(pinfunction "HD5")
			(pintype "bidirectional")
		)
		(pad "68" smd rect
			(at 3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "PA4")
			(pinfunction "HD4")
			(pintype "bidirectional")
		)
		(pad "69" smd rect
			(at 2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "PA3")
			(pinfunction "HD3")
			(pintype "bidirectional")
		)
		(pad "70" smd rect
			(at 2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 173 "PA2")
			(pinfunction "HD2")
			(pintype "bidirectional")
		)
		(pad "71" smd rect
			(at 1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 174 "PA1")
			(pinfunction "HD1")
			(pintype "bidirectional")
		)
		(pad "72" smd rect
			(at 0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 175 "PA0")
			(pinfunction "HD0")
			(pintype "bidirectional")
		)
		(pad "73" smd rect
			(at -0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "74" smd rect
			(at -1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "SELDRQ")
			(pintype "input")
		)
		(pad "75" smd rect
			(at -2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 282 "/RAA0")
			(pinfunction "RA0")
			(pintype "output")
		)
		(pad "76" smd rect
			(at -2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 283 "/RAA1")
			(pinfunction "RA1")
			(pintype "output")
		)
		(pad "77" smd rect
			(at -3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 284 "/RAA2")
			(pinfunction "RA2")
			(pintype "output")
		)
		(pad "78" smd rect
			(at -4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 285 "/RAA3")
			(pinfunction "RA3")
			(pintype "output")
		)
		(pad "79" smd rect
			(at -5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 286 "/RAA4")
			(pinfunction "RA4")
			(pintype "output")
		)
		(pad "80" smd rect
			(at -6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 287 "/RAA5")
			(pinfunction "RA5")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-80_14x20mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CON-21P"
		(layer "F.Cu")
		(at 57.15 91.279 -90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "CN3"
			(at 11.1084 2.8194 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CON 21P"
			(at 19.05 2.54 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x21, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "21"
			(at 28.609 0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -3.903 0.508 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -3.903 -2.032 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at 28.609 -1.778 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 1.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 30 "Net-(CN3-Pin_19)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 2.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 31 "~{ERES}")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole roundrect
			(at 3.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 341 "BCLKBF")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at 5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 336 "LRCKBF")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole roundrect
			(at 6.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 342 "DFCKBF")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole roundrect
			(at 7.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 34 "DDATA")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole roundrect
			(at 8.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 35 "ATT")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole roundrect
			(at 10 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 36 "SHFT")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole roundrect
			(at 11.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 37 "LATCH")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole roundrect
			(at 12.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 38 "VCC")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole roundrect
			(at 13.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole roundrect
			(at 15 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 39 "PDATA")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole roundrect
			(at 16.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 40 "PWCLK")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole roundrect
			(at 17.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 41 "PBCLK")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole roundrect
			(at 18.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 42 "PLRCK")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole roundrect
			(at 20 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 43 "SL2")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole roundrect
			(at 21.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 44 "SR2")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole roundrect
			(at 22.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 30 "Net-(CN3-Pin_19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole roundrect
			(at 23.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 28 "M.VCC")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole roundrect
			(at 25 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 29 "M.GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 118.691 119.888 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C42"
			(at 0.327 -2.921 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Enable" "0"
			(at 237.382 239.776 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -3.229 4.318 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOT-23-Wide"
		(layer "F.Cu")
		(at 202.311 128.651 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "TR1"
			(at 4.0132 0.508 180)
			(layer "F.SilkS")
		)
		(property "Value" "C1623"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 330.962 -73.66 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=B 2=E 3=C"
			(at 330.962 -73.66 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 330.962 -73.66 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "C"
			(at 1.2192 -4.1148 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B"
			(at -2.0828 -3.9116 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.016 -0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 294 "Net-(TR1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.016 0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "open_emitter")
		)
		(pad "3" smd roundrect
			(at 1.016 0 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "Net-(LD1-K)")
			(pinfunction "C")
			(pintype "open_collector")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Battery_no_symbols"
		(layer "F.Cu")
		(at 208.8134 59.4614)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "BT1"
			(at 0.4064 7.874 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AL2032"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 20.32 7.62 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 -5.08 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "1" thru_hole oval
			(at 0 5.08 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
			(clearance 0.3)
		)
		(pad "2" thru_hole oval
			(at 15.24 0 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 17.78 0 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 72.39 117.983 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC14"
			(at -7.493 -11.557 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB8464A-90L"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 324 "unconnected-(IC14-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "/RAA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 257 "/RAA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 256 "/RAA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "/RAA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/RAA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/RAA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/RAA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 283 "/RAA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 282 "/RAA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 275 "/CD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/CD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 273 "/CD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 272 "/CD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "/CD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 270 "/CD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 269 "/CD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "/CD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 322 "Net-(IC13-~{RCS})")
			(pinfunction "~{CS1}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 260 "/RAA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 316 "Net-(IC13-~{ROE})")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "/RAA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/RAA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 258 "/RAA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 303 "~{RAACS1}")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 315 "Net-(IC13-~{RWE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 72.39 68.453 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC10"
			(at 9.3472 -6.5786 180)
			(layer "F.SilkS")
		)
		(property "Value" "65256BLFP-10T"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "/RA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 232 "/RA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 241 "/RA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "/RA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "/RA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "/RA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "/RA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 247 "/RA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "/RA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 249 "/RA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 229 "/WD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "/WD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 227 "/WD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 337 "WD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "/WD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 344 "WD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "/WD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 239 "~{RCS1X}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/RA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 302 "~{ROE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/RA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "/RA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "/RA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "/RA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 240 "Net-(IC10-~{WE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 72.39 100.711 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC15"
			(at -0.127 -10.287 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MB8464A-90L"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 328 "unconnected-(IC15-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "/RAA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 257 "/RAA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 256 "/RAA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "/RAA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/RAA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/RAA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/RAA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 283 "/RAA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 282 "/RAA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 275 "/CD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/CD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 273 "/CD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 272 "/CD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "/CD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 270 "/CD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 269 "/CD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "/CD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 322 "Net-(IC13-~{RCS})")
			(pinfunction "~{CS1}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 260 "/RAA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 316 "Net-(IC13-~{ROE})")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "/RAA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "/RAA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 258 "/RAA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 305 "~{RAACS2}")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 315 "Net-(IC13-~{RWE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:EDGE-60P"
		(layer "F.Cu")
		(at 120.65 50.8)
		(property "Reference" "CN2"
			(at -30.099 5.588 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EDGE 60P"
			(at 10.16 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x30, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "B30"
			(at -38.354 6.096 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B1"
			(at 37.338 7.366 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A1"
			(at 38.989 6.985 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "A30"
			(at -35.941 5.842 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -10.16 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "a1" smd rect
			(at 36.83 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Pin_a1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a2" smd rect
			(at 34.29 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 345 "unconnected-(CN2-Pin_a2-Pada2)")
			(pinfunction "Pin_a2")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "a3" smd rect
			(at 31.75 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 106 "~{CAS0}")
			(pinfunction "Pin_a3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a4" smd rect
			(at 29.21 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 196 "VD0")
			(pinfunction "Pin_a4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a5" smd rect
			(at 26.67 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 197 "VD1")
			(pinfunction "Pin_a5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a6" smd rect
			(at 24.13 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 198 "VD2")
			(pinfunction "Pin_a6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a7" smd rect
			(at 21.59 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 199 "VD3")
			(pinfunction "Pin_a7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a8" smd rect
			(at 19.05 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 200 "VD4")
			(pinfunction "Pin_a8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a9" smd rect
			(at 16.51 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 201 "VD5")
			(pinfunction "Pin_a9")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a10" smd rect
			(at 13.97 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 202 "VD6")
			(pinfunction "Pin_a10")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a11" smd rect
			(at 11.43 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 203 "VD7")
			(pinfunction "Pin_a11")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a12" smd rect
			(at 8.89 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Pin_a12")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a13" smd rect
			(at 6.35 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 204 "VD8")
			(pinfunction "Pin_a13")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a14" smd rect
			(at 3.81 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 205 "VD9")
			(pinfunction "Pin_a14")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a15" smd rect
			(at 1.27 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 206 "VD10")
			(pinfunction "Pin_a15")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a16" smd rect
			(at -1.27 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 207 "VD11")
			(pinfunction "Pin_a16")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a17" smd rect
			(at -3.81 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 208 "VD12")
			(pinfunction "Pin_a17")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a18" smd rect
			(at -6.35 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 209 "VD13")
			(pinfunction "Pin_a18")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a19" smd rect
			(at -8.89 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 210 "VD14")
			(pinfunction "Pin_a19")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a20" smd rect
			(at -11.43 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 211 "VD15")
			(pinfunction "Pin_a20")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a21" smd rect
			(at -13.97 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 105 "~{ROM}")
			(pinfunction "Pin_a21")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a22" smd rect
			(at -16.51 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 109 "~{ASEL}")
			(pinfunction "Pin_a22")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a23" smd rect
			(at -19.05 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 237 "~{RAS2X}")
			(pinfunction "Pin_a23")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a24" smd rect
			(at -21.59 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 111 "~{FDC}")
			(pinfunction "Pin_a24")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a25" smd rect
			(at -24.13 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 112 "FRES")
			(pinfunction "Pin_a25")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a26" smd rect
			(at -26.67 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 38 "VCC")
			(pinfunction "Pin_a26")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a27" smd rect
			(at -29.21 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 295 "unconnected-(CN2-Pin_a27-Pada27)")
			(pinfunction "Pin_a27")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "a28" smd rect
			(at -31.75 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 296 "unconnected-(CN2-Pin_a28-Pada28)")
			(pinfunction "Pin_a28")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "a29" smd rect
			(at -34.29 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 44 "SR2")
			(pinfunction "Pin_a29")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a30" smd rect
			(at -36.83 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Pin_a30")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b1" smd rect
			(at 36.83 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b2" smd rect
			(at 34.29 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b3" smd rect
			(at 31.75 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 179 "VA1")
			(pinfunction "Pin_b3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b4" smd rect
			(at 29.21 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 180 "VA2")
			(pinfunction "Pin_b4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b5" smd rect
			(at 26.67 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 181 "VA3")
			(pinfunction "Pin_b5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b6" smd rect
			(at 24.13 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 182 "VA4")
			(pinfunction "Pin_b6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b7" smd rect
			(at 21.59 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 183 "VA5")
			(pinfunction "Pin_b7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b8" smd rect
			(at 19.05 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 184 "VA6")
			(pinfunction "Pin_b8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b9" smd rect
			(at 16.51 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 185 "VA7")
			(pinfunction "Pin_b9")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b10" smd rect
			(at 13.97 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 186 "VA8")
			(pinfunction "Pin_b10")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b11" smd rect
			(at 11.43 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 187 "VA9")
			(pinfunction "Pin_b11")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b12" smd rect
			(at 8.89 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b12")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b13" smd rect
			(at 6.35 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 188 "VA10")
			(pinfunction "Pin_b13")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b14" smd rect
			(at 3.81 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 189 "VA11")
			(pinfunction "Pin_b14")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b15" smd rect
			(at 1.27 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 190 "VA12")
			(pinfunction "Pin_b15")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b16" smd rect
			(at -1.27 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 191 "VA13")
			(pinfunction "Pin_b16")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b17" smd rect
			(at -3.81 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 192 "VA14")
			(pinfunction "Pin_b17")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b18" smd rect
			(at -6.35 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 193 "VA15")
			(pinfunction "Pin_b18")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b19" smd rect
			(at -8.89 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 194 "VA16")
			(pinfunction "Pin_b19")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b20" smd rect
			(at -11.43 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 195 "VA17")
			(pinfunction "Pin_b20")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b21" smd rect
			(at -13.97 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 107 "~{LWR}")
			(pinfunction "Pin_b21")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b22" smd rect
			(at -16.51 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 108 "~{UWR}")
			(pinfunction "Pin_b22")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b23" smd rect
			(at -19.05 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 110 "~{CAS2}")
			(pinfunction "Pin_b23")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b24" smd rect
			(at -21.59 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 297 "unconnected-(CN2-Pin_b24-Padb24)")
			(pinfunction "Pin_b24")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b25" smd rect
			(at -24.13 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 298 "unconnected-(CN2-Pin_b25-Padb25)")
			(pinfunction "Pin_b25")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b26" smd rect
			(at -26.67 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 38 "VCC")
			(pinfunction "Pin_b26")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b27" smd rect
			(at -29.21 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 299 "unconnected-(CN2-Pin_b27-Padb27)")
			(pinfunction "Pin_b27")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b28" smd rect
			(at -31.75 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 300 "unconnected-(CN2-Pin_b28-Padb28)")
			(pinfunction "Pin_b28")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b29" smd rect
			(at -34.29 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 43 "SL2")
			(pinfunction "Pin_b29")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b30" smd rect
			(at -36.83 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b30")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SOIC-16W_5.3x10.2mm_P1.27mm"
		(layer "F.Cu")
		(at 188.976 59.823 90)
		(descr "16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "IC6"
			(at 7.1688 -0.2286 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB3790"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 250 "unconnected-(IC6-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 251 "unconnected-(IC6-VBAT1-Pad2)")
			(pinfunction "VBAT1")
			(pintype "power_in+no_connect")
		)
		(pad "3" smd rect
			(at -3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(IC16-VCC)")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(pad "4" smd rect
			(at -3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(IC16-VCC)")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(pad "5" smd rect
			(at -3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(BT1-+)")
			(pinfunction "VBAT2")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at -3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 252 "unconnected-(IC6-~{ALARM1}-Pad6)")
			(pinfunction "~{ALARM1}")
			(pintype "output+no_connect")
		)
		(pad "7" smd rect
			(at -3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 253 "unconnected-(IC6-~{ALARM2}-Pad7)")
			(pinfunction "~{ALARM2}")
			(pintype "output+no_connect")
		)
		(pad "8" smd rect
			(at -3.55 4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 3.55 4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 254 "unconnected-(IC6-RESET-Pad9)")
			(pinfunction "RESET")
			(pintype "input+no_connect")
		)
		(pad "10" smd rect
			(at 3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 263 "Net-(IC16-CS2)")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(IC6-CT)")
			(pinfunction "CT")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 264 "unconnected-(IC6-VSENSE-Pad12)")
			(pinfunction "VSENSE")
			(pintype "input+no_connect")
		)
		(pad "13" smd rect
			(at 3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 265 "unconnected-(IC6-N.C.-Pad15)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "16" smd rect
			(at 3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CONTROL")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_5.3x10.2mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOT-23-Wide"
		(layer "F.Cu")
		(at 208.0514 128.651 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "TR2"
			(at 4.1148 0.1524 180)
			(layer "F.SilkS")
		)
		(property "Value" "C1623"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 336.7024 -79.4004 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=B 2=E 3=C"
			(at 336.7024 -79.4004 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 336.7024 -79.4004 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "C"
			(at 0.6096 2.9972 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "E"
			(at -2.794 3.2004 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.016 -0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 293 "Net-(TR2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.016 0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "open_emitter")
		)
		(pad "3" smd roundrect
			(at 1.016 0 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 290 "Net-(LD2-K)")
			(pinfunction "C")
			(pintype "open_collector")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 171.25 81.026 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C43"
			(at 1.705 3.048 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -2.74 4.191 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:C_Radial_5mm"
		(layer "F.Cu")
		(at 146.558 127.341 -90)
		(property "Reference" "C51"
			(at -3.77 3.3274 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at 2.7832 2.8702 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 2.5 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -2.5 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 99.622 128.651 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C50"
			(at 0.435 2.9972 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.2386 3.5052 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 215.065 126.746 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C45"
			(at -0.073 -3.2258 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.01 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PQFP-80_14x20mm_P0.8mm_long_pads"
		(layer "F.Cu")
		(at 99.695 86.264 90)
		(descr "PQFP80 14x20 / QIP80E CASE 122BS (see ON Semiconductor 122BS.PDF)")
		(tags "QFP 0.8")
		(property "Reference" "IC3"
			(at -11.907 -14.859 180)
			(layer "F.SilkS")
		)
		(property "Value" "315-5476A"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "25"
			(at -7.716 14.097 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "64"
			(at 11.08 -11.43 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -12.192 -10.668 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "65"
			(at 7.016 -16.51 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "40"
			(at 4.603 15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at -12.192 8.763 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "41"
			(at 11.08 8.255 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at -7.589 -15.621 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "•"
			(at 10.2616 5.4102 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at -9.142 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.146 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at -9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "9" smd rect
			(at -9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "A2")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd rect
			(at -9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "A1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd rect
			(at -9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 212 "unconnected-(IC3-N.C.-Pad11)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "12" smd rect
			(at -9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "~{COE}")
			(pinfunction "~{RD}")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 238 "~{CLWEX}")
			(pinfunction "~{WR}")
			(pintype "input")
		)
		(pad "15" smd rect
			(at -9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST1")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at -9.017 3.58 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST2")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at -9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST3")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at -9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "20" smd rect
			(at -9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 213 "unconnected-(IC3-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "21" smd rect
			(at -9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at -9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at -9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at -9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at -6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at -5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at -4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at -3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at -2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 214 "unconnected-(IC3-SHL-Pad29)")
			(pinfunction "SHL")
			(pintype "passive+no_connect")
		)
		(pad "30" smd rect
			(at -2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 215 "unconnected-(IC3-SHR-Pad30)")
			(pinfunction "SHR")
			(pintype "passive+no_connect")
		)
		(pad "31" smd rect
			(at -1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 216 "unconnected-(IC3-DAC7-Pad31)")
			(pinfunction "DAC7")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" smd rect
			(at -0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 217 "unconnected-(IC3-DAC6-Pad32)")
			(pinfunction "DAC6")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" smd rect
			(at 0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 218 "unconnected-(IC3-DAC5-Pad33)")
			(pinfunction "DAC5")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" smd rect
			(at 1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 219 "unconnected-(IC3-DAC4-Pad34)")
			(pinfunction "DAC4")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" smd rect
			(at 2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 339 "PBCLKF")
			(pinfunction "BCLK")
			(pintype "input")
		)
		(pad "36" smd rect
			(at 2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "PDATA")
			(pinfunction "DATA")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 220 "unconnected-(IC3-DAC3-Pad37)")
			(pinfunction "DAC3")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" smd rect
			(at 4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 221 "unconnected-(IC3-DAC7L-Pad38)")
			(pinfunction "DAC7L")
			(pintype "passive+no_connect")
		)
		(pad "39" smd rect
			(at 5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 222 "unconnected-(IC3-DAC7R-Pad39)")
			(pinfunction "DAC7R")
			(pintype "passive+no_connect")
		)
		(pad "40" smd rect
			(at 6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "PLRCK")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "41" smd rect
			(at 9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "PWCLK")
			(pinfunction "WCLK1")
			(pintype "input")
		)
		(pad "42" smd rect
			(at 9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 223 "unconnected-(IC3-RAMAX-Pad42)")
			(pinfunction "RAMAX")
			(pintype "output+no_connect")
		)
		(pad "43" smd rect
			(at 9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "44" smd rect
			(at 9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 224 "/WD7")
			(pinfunction "RAMAD7")
			(pintype "bidirectional")
		)
		(pad "45" smd rect
			(at 9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 225 "/WD6")
			(pinfunction "RAMAD6")
			(pintype "bidirectional")
		)
		(pad "46" smd rect
			(at 9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 343 "WD5F")
			(pinfunction "RAMAD5")
			(pintype "bidirectional")
		)
		(pad "47" smd rect
			(at 9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 226 "/WD4")
			(pinfunction "RAMAD4")
			(pintype "bidirectional")
		)
		(pad "48" smd rect
			(at 9.017 3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 337 "WD3")
			(pinfunction "RAMAD3")
			(pintype "bidirectional")
		)
		(pad "49" smd rect
			(at 9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 227 "/WD2")
			(pinfunction "RAMAD2")
			(pintype "bidirectional")
		)
		(pad "50" smd rect
			(at 9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "/WD1")
			(pinfunction "RAMAD1")
			(pintype "bidirectional")
		)
		(pad "51" smd rect
			(at 9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "/WD0")
			(pinfunction "RAMAD0")
			(pintype "bidirectional")
		)
		(pad "52" smd rect
			(at 9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 230 "/RA14")
			(pinfunction "RAMA14")
			(pintype "output")
		)
		(pad "54" smd rect
			(at 9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 231 "/RA13")
			(pinfunction "RAMA13")
			(pintype "output")
		)
		(pad "55" smd rect
			(at 9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 232 "/RA12")
			(pinfunction "RAMA12")
			(pintype "output")
		)
		(pad "56" smd rect
			(at 9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 233 "/RA11")
			(pinfunction "RAMA11")
			(pintype "output")
		)
		(pad "57" smd rect
			(at 9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 234 "/RA10")
			(pinfunction "RAMA10")
			(pintype "output")
		)
		(pad "58" smd rect
			(at 9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 235 "/RA9")
			(pinfunction "RAMA9")
			(pintype "output")
		)
		(pad "59" smd rect
			(at 9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 236 "/RA8")
			(pinfunction "RAMA8")
			(pintype "output")
		)
		(pad "60" smd rect
			(at 9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 239 "~{RCS1X}")
			(pinfunction "~{RCS1}")
			(pintype "input")
		)
		(pad "61" smd rect
			(at 9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 301 "~{RCS2X}")
			(pinfunction "~{RCS2}")
			(pintype "input")
		)
		(pad "62" smd rect
			(at 9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 302 "~{ROE}")
			(pinfunction "~{RDE}")
			(pintype "input")
		)
		(pad "63" smd rect
			(at 9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 240 "Net-(IC10-~{WE})")
			(pinfunction "~{RWE}")
			(pintype "input")
		)
		(pad "64" smd rect
			(at 9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "~{ERES}")
			(pinfunction "~{RES}")
			(pintype "input")
		)
		(pad "65" smd rect
			(at 6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 241 "/RA7")
			(pinfunction "RAMA7")
			(pintype "output")
		)
		(pad "66" smd rect
			(at 5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 242 "/RA6")
			(pinfunction "RAMA6")
			(pintype "output")
		)
		(pad "67" smd rect
			(at 4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 243 "/RA5")
			(pinfunction "RAMA5")
			(pintype "output")
		)
		(pad "68" smd rect
			(at 3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 244 "/RA4")
			(pinfunction "RAMA4")
			(pintype "output")
		)
		(pad "69" smd rect
			(at 2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "70" smd rect
			(at 2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "12M")
			(pinfunction "XIN")
			(pintype "input")
		)
		(pad "71" smd rect
			(at 1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 245 "unconnected-(IC3-XOUT-Pad71)")
			(pinfunction "XOUT")
			(pintype "output+no_connect")
		)
		(pad "72" smd rect
			(at 0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "73" smd rect
			(at -0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 246 "/RA3")
			(pinfunction "RAMA3")
			(pintype "output")
		)
		(pad "74" smd rect
			(at -1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 247 "/RA2")
			(pinfunction "RAMA2")
			(pintype "output")
		)
		(pad "75" smd rect
			(at -2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 248 "/RA1")
			(pinfunction "RAMA1")
			(pintype "output")
		)
		(pad "76" smd rect
			(at -2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 249 "/RA0")
			(pinfunction "RAMA0")
			(pintype "output")
		)
		(pad "77" smd rect
			(at -3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "~{PCM}")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "78" smd rect
			(at -4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "A13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "79" smd rect
			(at -5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "80" smd rect
			(at -6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-80_14x20mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PLCC-68-Longer_Pads"
		(layer "F.Cu")
		(at 137.668 90.043 90)
		(descr "PLCC, 68 pins, surface mount")
		(tags "plcc smt")
		(property "Reference" "IC1"
			(at 2.413 -15.367 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "68HC000"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microprocessor, 16-bit bus"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "61"
			(at 12.446 -16.51 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "27"
			(at -9.525 14.605 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "9"
			(at -12.192 -15.113 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "43"
			(at 13.5382 13.2334 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at -13.843 -13.589 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "26"
			(at -14.859 10.16 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -13.462 13.462)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 13.462 -13.462)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at 0 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -1.27 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -2.54 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -3.81 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -5.08 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -6.35 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "~{AS}")
			(pinfunction "AS")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -7.62 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "~{UDS}")
			(pinfunction "UDS")
			(pintype "output")
		)
		(pad "8" smd rect
			(at -8.89 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "~{LDS}")
			(pinfunction "LDS")
			(pintype "output")
		)
		(pad "9" smd rect
			(at -10.16 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "R{slash}~{W}")
			(pinfunction "R/W")
			(pintype "output")
		)
		(pad "10" smd rect
			(at -11.938 -10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "~{DTAK}")
			(pinfunction "DTACK")
			(pintype "input")
		)
		(pad "11" smd rect
			(at -11.938 -8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "unconnected-(IC1-BG-Pad11)")
			(pinfunction "BG")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at -11.938 -7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 346 "VCC2C")
			(pinfunction "BGACK")
			(pintype "input")
		)
		(pad "13" smd rect
			(at -11.938 -6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 346 "VCC2C")
			(pinfunction "BR")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -11.938 -5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 346 "VCC2C")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at -11.938 -3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "12M")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "16" smd rect
			(at -11.938 -2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at -11.938 -1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at -11.938 0 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "unconnected-(IC1-NC-Pad18)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "19" smd rect
			(at -11.938 1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "~{HALT}")
			(pinfunction "HALT")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -11.938 2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "~{RES}")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "21" smd rect
			(at -11.938 3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "unconnected-(IC1-VMA-Pad21)")
			(pinfunction "VMA")
			(pintype "output+no_connect")
		)
		(pad "22" smd rect
			(at -11.938 5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 308 "E")
			(pinfunction "E")
			(pintype "output")
		)
		(pad "23" smd rect
			(at -11.938 6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "~{VPA}")
			(pinfunction "VPA")
			(pintype "input")
		)
		(pad "24" smd rect
			(at -11.938 7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 346 "VCC2C")
			(pinfunction "BERR")
			(pintype "input")
		)
		(pad "25" smd rect
			(at -11.938 8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 309 "~{IPL2}")
			(pinfunction "IPL2")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -11.938 10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 310 "~{IPL1}")
			(pinfunction "IPL1")
			(pintype "input")
		)
		(pad "27" smd rect
			(at -10.16 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 311 "~{IPL0}")
			(pinfunction "IPL0")
			(pintype "input")
		)
		(pad "28" smd rect
			(at -8.89 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "unconnected-(IC1-FC2-Pad28)")
			(pinfunction "FC2")
			(pintype "output+no_connect")
		)
		(pad "29" smd rect
			(at -7.62 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "FC1")
			(pinfunction "FC1")
			(pintype "output")
		)
		(pad "30" smd rect
			(at -6.35 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "FC0")
			(pinfunction "FC0")
			(pintype "output")
		)
		(pad "31" smd rect
			(at -5.08 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "unconnected-(IC1-NC-Pad31)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "32" smd rect
			(at -3.81 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "A1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "33" smd rect
			(at -2.54 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "A2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "34" smd rect
			(at -1.27 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "A3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "35" smd rect
			(at 0 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "A4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "36" smd rect
			(at 1.27 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "A5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "37" smd rect
			(at 2.54 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "A6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "38" smd rect
			(at 3.81 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "A7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "39" smd rect
			(at 5.08 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "A8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "40" smd rect
			(at 6.35 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "A9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "41" smd rect
			(at 7.62 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "A10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "42" smd rect
			(at 8.89 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "A11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "43" smd rect
			(at 10.16 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "A12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "44" smd rect
			(at 11.938 10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "A13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "45" smd rect
			(at 11.938 8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "A14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "46" smd rect
			(at 11.938 7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "A15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "47" smd rect
			(at 11.938 6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "A16")
			(pinfunction "A16")
			(pintype "output")
		)
		(pad "48" smd rect
			(at 11.938 5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "A17")
			(pinfunction "A17")
			(pintype "output")
		)
		(pad "49" smd rect
			(at 11.938 3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "A18")
			(pinfunction "A18")
			(pintype "output")
		)
		(pad "50" smd rect
			(at 11.938 2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "A19")
			(pinfunction "A19")
			(pintype "output")
		)
		(pad "51" smd rect
			(at 11.938 1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(IC1-A20-Pad51)")
			(pinfunction "A20")
			(pintype "output+no_connect")
		)
		(pad "52" smd rect
			(at 11.938 0 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 346 "VCC2C")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 11.938 -1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "unconnected-(IC1-A21-Pad53)")
			(pinfunction "A21")
			(pintype "output+no_connect")
		)
		(pad "54" smd rect
			(at 11.938 -2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "unconnected-(IC1-A22-Pad54)")
			(pinfunction "A22")
			(pintype "output+no_connect")
		)
		(pad "55" smd rect
			(at 11.938 -3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "unconnected-(IC1-A23-Pad55)")
			(pinfunction "A23")
			(pintype "output+no_connect")
		)
		(pad "56" smd rect
			(at 11.938 -5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" smd rect
			(at 11.938 -6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "58" smd rect
			(at 11.938 -7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "D15")
			(pinfunction "D15")
			(pintype "bidirectional")
		)
		(pad "59" smd rect
			(at 11.938 -8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "D14")
			(pinfunction "D14")
			(pintype "bidirectional")
		)
		(pad "60" smd rect
			(at 11.938 -10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "D13")
			(pinfunction "D13")
			(pintype "bidirectional")
		)
		(pad "61" smd rect
			(at 10.16 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "D12")
			(pinfunction "D12")
			(pintype "bidirectional")
		)
		(pad "62" smd rect
			(at 8.89 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "D11")
			(pinfunction "D11")
			(pintype "bidirectional")
		)
		(pad "63" smd rect
			(at 7.62 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "D10")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "64" smd rect
			(at 6.35 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "D9")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "65" smd rect
			(at 5.08 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "D8")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "66" smd rect
			(at 3.81 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "67" smd rect
			(at 2.54 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "68" smd rect
			(at 1.27 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_LCC.3dshapes/PLCC-68.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 222.069 126.746 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C46"
			(at 0.4032 -3.1242 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.118 3.048 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P7.00mm"
		(layer "F.Cu")
		(at 208.534 70.358 -90)
		(property "Reference" "FB2"
			(at 10.6934 -0.0254 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 2.5 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 325 "Net-(OSC1-OUT)")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 7 0 270)
			(size 1.3 1.3)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "50M")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:DIP-40_W15.24mm_Socket"
		(layer "F.Cu")
		(at 104.14 72.644 90)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
		(property "Reference" "IC4"
			(at -0.127 52.832 180)
			(layer "F.SilkS")
		)
		(property "Value" "27C1024"
			(at 7.62 50.59 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VPP")
			(pintype "power_in")
		)
		(pad "2" thru_hole roundrect
			(at 0 2.54 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 104 "~{BROM}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 0 5.08 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 211 "VD15")
			(pinfunction "D15")
			(pintype "tri_state")
		)
		(pad "4" thru_hole roundrect
			(at 0 7.62 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 210 "VD14")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "5" thru_hole roundrect
			(at 0 10.16 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 209 "VD13")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "6" thru_hole roundrect
			(at 0 12.7 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 208 "VD12")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "7" thru_hole roundrect
			(at 0 15.24 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 207 "VD11")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "8" thru_hole roundrect
			(at 0 17.78 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 206 "VD10")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "9" thru_hole roundrect
			(at 0 20.32 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 205 "VD9")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "10" thru_hole roundrect
			(at 0 22.86 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 204 "VD8")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "11" thru_hole roundrect
			(at 0 25.4 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole roundrect
			(at 0 27.94 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 203 "VD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "13" thru_hole roundrect
			(at 0 30.48 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 202 "VD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "14" thru_hole roundrect
			(at 0 33.02 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 201 "VD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "15" thru_hole roundrect
			(at 0 35.56 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 200 "VD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "16" thru_hole roundrect
			(at 0 38.1 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 199 "VD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "17" thru_hole roundrect
			(at 0 40.64 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 198 "VD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "18" thru_hole roundrect
			(at 0 43.18 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 197 "VD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "19" thru_hole roundrect
			(at 0 45.72 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 196 "VD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "20" thru_hole roundrect
			(at 0 48.26 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 106 "~{CAS0}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "21" thru_hole roundrect
			(at 15.24 48.26 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 179 "VA1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "22" thru_hole roundrect
			(at 15.24 45.72 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 180 "VA2")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "23" thru_hole roundrect
			(at 15.24 43.18 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 181 "VA3")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "24" thru_hole roundrect
			(at 15.24 40.64 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 182 "VA4")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "25" thru_hole roundrect
			(at 15.24 38.1 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 183 "VA5")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "26" thru_hole roundrect
			(at 15.24 35.56 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 184 "VA6")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "27" thru_hole roundrect
			(at 15.24 33.02 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 185 "VA7")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "28" thru_hole roundrect
			(at 15.24 30.48 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 186 "VA8")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole roundrect
			(at 15.24 27.94 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 187 "VA9")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "30" thru_hole roundrect
			(at 15.24 25.4 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "31" thru_hole roundrect
			(at 15.24 22.86 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 188 "VA10")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "32" thru_hole roundrect
			(at 15.24 20.32 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 189 "VA11")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "33" thru_hole roundrect
			(at 15.24 17.78 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 190 "VA12")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "34" thru_hole roundrect
			(at 15.24 15.24 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 191 "VA13")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "35" thru_hole roundrect
			(at 15.24 12.7 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 192 "VA14")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "36" thru_hole roundrect
			(at 15.24 10.16 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 193 "VA15")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "37" thru_hole roundrect
			(at 15.24 7.62 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 194 "VA16")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "38" thru_hole roundrect
			(at 15.24 5.08 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "D.C.")
			(pintype "power_in")
		)
		(pad "39" thru_hole roundrect
			(at 15.24 2.54 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "~{PGM}")
			(pintype "input")
		)
		(pad "40" thru_hole roundrect
			(at 15.24 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PQFP-208_28x28mm_P0.5mm_Wider"
		(layer "F.Cu")
		(at 184.664 102.031 90)
		(descr "PQFP, 208 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "IC2"
			(at -19.508 5.6582 180)
			(layer "F.SilkS")
		)
		(property "Value" "315-5548/315-5632"
			(at 0.025 11.6 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -18.8942 -14.2762 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "157"
			(at 11.861 -20.961 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "105"
			(at 18.084 13.583 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "208"
			(at -14.301 -19.437 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "53"
			(at -11.55 18.225 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "156"
			(at 17.703 -16.135 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "52"
			(at -19.2498 12.694 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "104"
			(at 12.242 17.393 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -15.875 -15.875)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at -15.875 15.875)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 15.853 -15.851)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 15.853 15.875)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd roundrect
			(at -15.5 -12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(IC2-25M)")
			(pinfunction "25M")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -15.5 -12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "~{BRAM}")
			(pinfunction "~{BRAM}")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -15.5 -11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -15.5 -11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "~{BROM}")
			(pinfunction "~{BROM}")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -15.5 -10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "~{ROM}")
			(pinfunction "~{ROM}")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -15.5 -10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "~{CAS0}")
			(pinfunction "~{CAS0}")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -15.5 -9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "~{LWR}")
			(pinfunction "~{LWR}")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -15.5 -9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "~{UWR}")
			(pinfunction "~{UWR}")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at -15.5 -8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "~{ASEL}")
			(pinfunction "~{ASEL}")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -15.5 -8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -15.5 -7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 326 "~{RAS2}")
			(pinfunction "~{RAS2}")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at -15.5 -7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "~{CAS2}")
			(pinfunction "~{CAS2}")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at -15.5 -6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "~{FDC}")
			(pinfunction "~{FDC}")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at -15.5 -6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "FRES")
			(pinfunction "FRES")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at -15.5 -5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -15.5 -5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "~{ERES}")
			(pinfunction "~{ERES}")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at -15.5 -4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "Net-(IC2-EAD0)")
			(pinfunction "EAD0")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at -15.5 -4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "Net-(IC2-EAD1)")
			(pinfunction "EAD1")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at -15.5 -3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "Net-(IC2-EAD2)")
			(pinfunction "EAD2")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -15.5 -3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "Net-(IC2-EAD3)")
			(pinfunction "EAD3")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -15.5 -2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Net-(IC2-EAD4)")
			(pinfunction "EAD4")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -15.5 -2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "Net-(IC2-EAD5)")
			(pinfunction "EAD5")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -15.5 -1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "Net-(IC2-EAD6)")
			(pinfunction "EAD6")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -15.5 -1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "Net-(IC2-EAD7)")
			(pinfunction "EAD7")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -15.5 -0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Net-(IC2-ED8)")
			(pinfunction "ED8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at -15.5 -0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "27" smd roundrect
			(at -15.5 0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at -15.5 0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "Net-(IC2-ED9)")
			(pinfunction "ED9")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at -15.5 1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "Net-(IC2-ED10)")
			(pinfunction "ED10")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at -15.5 1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "Net-(IC2-ED11)")
			(pinfunction "ED11")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at -15.5 2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "Net-(IC2-ED12)")
			(pinfunction "ED12")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at -15.5 2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "Net-(IC2-ED13)")
			(pinfunction "ED13")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at -15.5 3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "Net-(IC2-ED14)")
			(pinfunction "ED14")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at -15.5 3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "Net-(IC2-ED15)")
			(pinfunction "ED15")
			(pintype "input")
		)
		(pad "35" smd roundrect
			(at -15.5 4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "~{ERAS}")
			(pinfunction "~{ERAS}")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at -15.5 4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "~{ECAS}")
			(pinfunction "~{ECAS}")
			(pintype "input")
		)
		(pad "37" smd roundrect
			(at -15.5 5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "~{EOE}")
			(pinfunction "~{EOE}")
			(pintype "input")
		)
		(pad "38" smd roundrect
			(at -15.5 5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "39" smd roundrect
			(at -15.5 6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 255 "~{EWE}")
			(pinfunction "~{EWE}")
			(pintype "input")
		)
		(pad "40" smd roundrect
			(at -15.5 6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "~{ORAS}")
			(pinfunction "~{ORAS}")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at -15.5 7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "~{OCAS}")
			(pinfunction "~{OCAS}")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at -15.5 7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "~{OOE}")
			(pinfunction "~{OOE}")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at -15.5 8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "44" smd roundrect
			(at -15.5 8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "~{OWE}")
			(pinfunction "~{OWE}")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at -15.5 9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "Net-(IC2-OAD0)")
			(pinfunction "OAD0")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at -15.5 9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "Net-(IC2-OAD1)")
			(pinfunction "OAD1")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at -15.5 10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "Net-(IC2-OAD2)")
			(pinfunction "OAD2")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at -15.5 10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Net-(IC2-OAD3)")
			(pinfunction "OAD3")
			(pintype "input")
		)
		(pad "49" smd roundrect
			(at -15.5 11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Net-(IC2-OAD4)")
			(pinfunction "OAD4")
			(pintype "input")
		)
		(pad "50" smd roundrect
			(at -15.5 11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at -15.5 12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "Net-(IC2-OAD5)")
			(pinfunction "OAD5")
			(pintype "input")
		)
		(pad "52" smd roundrect
			(at -15.5 12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Net-(IC2-OAD6)")
			(pinfunction "OAD6")
			(pintype "input")
		)
		(pad "53" smd roundrect
			(at -12.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Net-(IC2-OAD7)")
			(pinfunction "OAD7")
			(pintype "input")
		)
		(pad "54" smd roundrect
			(at -12.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Net-(IC2-OD8)")
			(pinfunction "OD8")
			(pintype "input")
		)
		(pad "55" smd roundrect
			(at -11.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Net-(IC2-OD9)")
			(pinfunction "OD9")
			(pintype "input")
		)
		(pad "56" smd roundrect
			(at -11.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Net-(IC2-OD10)")
			(pinfunction "OD10")
			(pintype "input")
		)
		(pad "57" smd roundrect
			(at -10.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(IC2-OD11)")
			(pinfunction "OD11")
			(pintype "input")
		)
		(pad "58" smd roundrect
			(at -10.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "Net-(IC2-OD12)")
			(pinfunction "OD12")
			(pintype "input")
		)
		(pad "59" smd roundrect
			(at -9.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Net-(IC2-OD13)")
			(pinfunction "OD13")
			(pintype "input")
		)
		(pad "60" smd roundrect
			(at -9.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "61" smd roundrect
			(at -8.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "62" smd roundrect
			(at -8.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "Net-(IC2-OD14)")
			(pinfunction "OD14")
			(pintype "input")
		)
		(pad "63" smd roundrect
			(at -7.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "Net-(IC2-OD15)")
			(pinfunction "OD15")
			(pintype "input")
		)
		(pad "64" smd roundrect
			(at -7.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Net-(IC2-LEDR)")
			(pinfunction "LEDR")
			(pintype "output")
		)
		(pad "65" smd roundrect
			(at -6.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "Net-(IC2-LEDG)")
			(pinfunction "LEDG")
			(pintype "output")
		)
		(pad "66" smd roundrect
			(at -6.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "LATCH")
			(pinfunction "LATCH")
			(pintype "output")
		)
		(pad "67" smd roundrect
			(at -5.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "SHFT")
			(pinfunction "SHFT")
			(pintype "output")
		)
		(pad "68" smd roundrect
			(at -5.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "ATT")
			(pinfunction "AT")
			(pintype "output")
		)
		(pad "69" smd roundrect
			(at -4.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "DDATA")
			(pinfunction "DTM")
			(pintype "output")
		)
		(pad "70" smd roundrect
			(at -4.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "WFCKD")
			(pinfunction "WFCK")
			(pintype "input")
		)
		(pad "71" smd roundrect
			(at -3.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "SCORB")
			(pinfunction "SCOA")
			(pintype "input")
		)
		(pad "72" smd roundrect
			(at -3.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "73" smd roundrect
			(at -2.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "SBSOB")
			(pinfunction "SBSO")
			(pintype "input")
		)
		(pad "74" smd roundrect
			(at -2.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(CN1-Pin_17)")
			(pinfunction "EXCK")
			(pintype "input")
		)
		(pad "75" smd roundrect
			(at -1.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 336 "LRCKBF")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at -1.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "SDATAB")
			(pinfunction "SDATA")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at -0.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(CN1-Pin_10)")
			(pinfunction "C2PO")
			(pintype "input")
		)
		(pad "78" smd roundrect
			(at -0.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(CN1-Pin_9)")
			(pinfunction "DB3")
			(pintype "input")
		)
		(pad "79" smd roundrect
			(at 0.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "80" smd roundrect
			(at 0.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(CN1-Pin_8)")
			(pinfunction "DB2")
			(pintype "input")
		)
		(pad "81" smd roundrect
			(at 1.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(CN1-Pin_7)")
			(pinfunction "DB1")
			(pintype "input")
		)
		(pad "82" smd roundrect
			(at 1.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(CN1-Pin_6)")
			(pinfunction "DB0")
			(pintype "input")
		)
		(pad "83" smd roundrect
			(at 2.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(CN1-Pin_5)")
			(pinfunction "HDCK")
			(pintype "input")
		)
		(pad "84" smd roundrect
			(at 2.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "50M")
			(pinfunction "50M")
			(pintype "output")
		)
		(pad "85" smd roundrect
			(at 3.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "86" smd roundrect
			(at 3.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(CN1-Pin_3)")
			(pinfunction "~{IRQ}")
			(pintype "input")
		)
		(pad "87" smd roundrect
			(at 4.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(CN1-Pin_2)")
			(pinfunction "D/M")
			(pintype "input")
		)
		(pad "88" smd roundrect
			(at 4.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "CDCKD")
			(pinfunction "CDCK")
			(pintype "input")
		)
		(pad "89" smd roundrect
			(at 5.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "~{PCM}")
			(pinfunction "~{PCM}")
			(pintype "output")
		)
		(pad "90" smd roundrect
			(at 5.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "~{DTEN}")
			(pinfunction "~{DTEN}")
			(pintype "output")
		)
		(pad "91" smd roundrect
			(at 6.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 161 "~{WAIT}")
			(pinfunction "~{WAIT}")
			(pintype "output")
		)
		(pad "92" smd roundrect
			(at 6.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "~{HRD}")
			(pinfunction "~{HRD}")
			(pintype "output")
		)
		(pad "93" smd roundrect
			(at 7.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 163 "~{INT}")
			(pinfunction "~{INT}")
			(pintype "output")
		)
		(pad "94" smd roundrect
			(at 7.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 164 "~{CDC}")
			(pinfunction "~{CDC}")
			(pintype "output")
		)
		(pad "95" smd roundrect
			(at 8.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "~{COE}")
			(pinfunction "~{COE}")
			(pintype "output")
		)
		(pad "96" smd roundrect
			(at 8.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "97" smd roundrect
			(at 9.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "98" smd roundrect
			(at 9.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 166 "C2LR")
			(pinfunction "C2LR")
			(pintype "output")
		)
		(pad "99" smd roundrect
			(at 10.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "A19")
			(pinfunction "A19")
			(pintype "output")
		)
		(pad "100" smd roundrect
			(at 10.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "A18")
			(pinfunction "A18")
			(pintype "output")
		)
		(pad "101" smd roundrect
			(at 11.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "A17")
			(pinfunction "A17")
			(pintype "output")
		)
		(pad "102" smd roundrect
			(at 11.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "A16")
			(pinfunction "A16")
			(pintype "output")
		)
		(pad "103" smd roundrect
			(at 12.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "A15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "104" smd roundrect
			(at 12.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "A14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "105" smd roundrect
			(at 15.5 12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "A13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "106" smd roundrect
			(at 15.5 12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "A12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "107" smd roundrect
			(at 15.5 11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "108" smd roundrect
			(at 15.5 11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "A11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "109" smd roundrect
			(at 15.5 10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "A10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "110" smd roundrect
			(at 15.5 10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "A9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "111" smd roundrect
			(at 15.5 9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "A8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "112" smd roundrect
			(at 15.5 9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "A7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "113" smd roundrect
			(at 15.5 8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "A6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "114" smd roundrect
			(at 15.5 8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "115" smd roundrect
			(at 15.5 7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "A5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "116" smd roundrect
			(at 15.5 7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "A4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "117" smd roundrect
			(at 15.5 6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "A3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "118" smd roundrect
			(at 15.5 6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "A2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "119" smd roundrect
			(at 15.5 5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "120" smd roundrect
			(at 15.5 5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "A1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "121" smd roundrect
			(at 15.5 4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "FC0")
			(pinfunction "FC0")
			(pintype "output")
		)
		(pad "122" smd roundrect
			(at 15.5 4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "FC1")
			(pinfunction "FC1")
			(pintype "output")
		)
		(pad "123" smd roundrect
			(at 15.5 3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 311 "~{IPL0}")
			(pinfunction "~{IPL0}")
			(pintype "output")
		)
		(pad "124" smd roundrect
			(at 15.5 3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 310 "~{IPL1}")
			(pinfunction "~{IPL1}")
			(pintype "output")
		)
		(pad "125" smd roundrect
			(at 15.5 2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 309 "~{IPL2}")
			(pinfunction "~{IPL2}")
			(pintype "output")
		)
		(pad "126" smd roundrect
			(at 15.5 2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "~{VPA}")
			(pinfunction "~{VPA}")
			(pintype "output")
		)
		(pad "127" smd roundrect
			(at 15.5 1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "~{RES}")
			(pinfunction "~{RESET}")
			(pintype "output")
		)
		(pad "128" smd roundrect
			(at 15.5 1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "~{HALT}")
			(pinfunction "~{HALT}")
			(pintype "output")
		)
		(pad "129" smd roundrect
			(at 15.5 0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "Net-(IC2-12M)")
			(pinfunction "12M")
			(pintype "output")
		)
		(pad "130" smd roundrect
			(at 15.5 0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "131" smd roundrect
			(at 15.5 -0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "132" smd roundrect
			(at 15.5 -0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "~{DTAK}")
			(pinfunction "~{DTAK}")
			(pintype "output")
		)
		(pad "133" smd roundrect
			(at 15.5 -1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "R{slash}~{W}")
			(pinfunction "R/~{W}")
			(pintype "output")
		)
		(pad "134" smd roundrect
			(at 15.5 -1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "~{LDS}")
			(pinfunction "~{LDS}")
			(pintype "output")
		)
		(pad "135" smd roundrect
			(at 15.5 -2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "~{UDS}")
			(pinfunction "~{UDS}")
			(pintype "output")
		)
		(pad "136" smd roundrect
			(at 15.5 -2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "~{AS}")
			(pinfunction "~{AS}")
			(pintype "output")
		)
		(pad "137" smd roundrect
			(at 15.5 -3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "138" smd roundrect
			(at 15.5 -3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "139" smd roundrect
			(at 15.5 -4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "140" smd roundrect
			(at 15.5 -4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "141" smd roundrect
			(at 15.5 -5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "142" smd roundrect
			(at 15.5 -5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "143" smd roundrect
			(at 15.5 -6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "144" smd roundrect
			(at 15.5 -6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "145" smd roundrect
			(at 15.5 -7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "146" smd roundrect
			(at 15.5 -7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "D8")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "147" smd roundrect
			(at 15.5 -8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "148" smd roundrect
			(at 15.5 -8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "D9")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "149" smd roundrect
			(at 15.5 -9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "D10")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "150" smd roundrect
			(at 15.5 -9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "D11")
			(pinfunction "D11")
			(pintype "bidirectional")
		)
		(pad "151" smd roundrect
			(at 15.5 -10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "D12")
			(pinfunction "D12")
			(pintype "bidirectional")
		)
		(pad "152" smd roundrect
			(at 15.5 -10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "D13")
			(pinfunction "D13")
			(pintype "bidirectional")
		)
		(pad "153" smd roundrect
			(at 15.5 -11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "D14")
			(pinfunction "D14")
			(pintype "bidirectional")
		)
		(pad "154" smd roundrect
			(at 15.5 -11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "155" smd roundrect
			(at 15.5 -12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "D15")
			(pinfunction "D15")
			(pintype "bidirectional")
		)
		(pad "156" smd roundrect
			(at 15.5 -12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 175 "PA0")
			(pinfunction "PA0")
			(pintype "power_in")
		)
		(pad "157" smd roundrect
			(at 12.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 174 "PA1")
			(pinfunction "PA1")
			(pintype "power_in")
		)
		(pad "158" smd roundrect
			(at 12.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 173 "PA2")
			(pinfunction "PA2")
			(pintype "power_in")
		)
		(pad "159" smd roundrect
			(at 11.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 172 "PA3")
			(pinfunction "PA3")
			(pintype "power_in")
		)
		(pad "160" smd roundrect
			(at 11.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "PA4")
			(pinfunction "PA4")
			(pintype "power_in")
		)
		(pad "161" smd roundrect
			(at 10.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 170 "PA5")
			(pinfunction "PA5")
			(pintype "power_in")
		)
		(pad "162" smd roundrect
			(at 10.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 169 "PA6")
			(pinfunction "PA6")
			(pintype "power_in")
		)
		(pad "163" smd roundrect
			(at 9.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "PA7")
			(pinfunction "PA7")
			(pintype "power_in")
		)
		(pad "164" smd roundrect
			(at 9.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "165" smd roundrect
			(at 8.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "166" smd roundrect
			(at 8.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 167 "PA8")
			(pinfunction "PA8")
			(pintype "power_in")
		)
		(pad "167" smd roundrect
			(at 7.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 176 "~{PRAS}")
			(pinfunction "~{PRAS}")
			(pintype "output")
		)
		(pad "168" smd roundrect
			(at 7.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 177 "~{PCAS}")
			(pinfunction "~{PCAS}")
			(pintype "output")
		)
		(pad "169" smd roundrect
			(at 6.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 178 "~{CUWE}")
			(pinfunction "~{CUWE}")
			(pintype "output")
		)
		(pad "170" smd roundrect
			(at 6.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 327 "~{CLWE}")
			(pinfunction "~{CLWE}")
			(pintype "output")
		)
		(pad "171" smd roundrect
			(at 5.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 179 "VA1")
			(pinfunction "VA1")
			(pintype "output")
		)
		(pad "172" smd roundrect
			(at 5.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 180 "VA2")
			(pinfunction "VA2")
			(pintype "output")
		)
		(pad "173" smd roundrect
			(at 4.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 181 "VA3")
			(pinfunction "VA3")
			(pintype "output")
		)
		(pad "174" smd roundrect
			(at 4.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 182 "VA4")
			(pinfunction "VA4")
			(pintype "output")
		)
		(pad "175" smd roundrect
			(at 3.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 183 "VA5")
			(pinfunction "VA5")
			(pintype "output")
		)
		(pad "176" smd roundrect
			(at 3.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "177" smd roundrect
			(at 2.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 184 "VA6")
			(pinfunction "VA6")
			(pintype "output")
		)
		(pad "178" smd roundrect
			(at 2.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 185 "VA7")
			(pinfunction "VA7")
			(pintype "output")
		)
		(pad "179" smd roundrect
			(at 1.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 186 "VA8")
			(pinfunction "VA8")
			(pintype "output")
		)
		(pad "180" smd roundrect
			(at 1.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 187 "VA9")
			(pinfunction "VA9")
			(pintype "output")
		)
		(pad "181" smd roundrect
			(at 0.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 188 "VA10")
			(pinfunction "VA10")
			(pintype "output")
		)
		(pad "182" smd roundrect
			(at 0.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 189 "VA11")
			(pinfunction "VA11")
			(pintype "output")
		)
		(pad "183" smd roundrect
			(at -0.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "184" smd roundrect
			(at -0.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "VA12")
			(pinfunction "VA12")
			(pintype "output")
		)
		(pad "185" smd roundrect
			(at -1.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 191 "VA13")
			(pinfunction "VA13")
			(pintype "output")
		)
		(pad "186" smd roundrect
			(at -1.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 192 "VA14")
			(pinfunction "VA14")
			(pintype "output")
		)
		(pad "187" smd roundrect
			(at -2.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 193 "VA15")
			(pinfunction "VA15")
			(pintype "output")
		)
		(pad "188" smd roundrect
			(at -2.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 194 "VA16")
			(pinfunction "VA16")
			(pintype "output")
		)
		(pad "189" smd roundrect
			(at -3.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "190" smd roundrect
			(at -3.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 195 "VA17")
			(pinfunction "VA17")
			(pintype "output")
		)
		(pad "191" smd roundrect
			(at -4.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "VD0")
			(pinfunction "VD0")
			(pintype "bidirectional")
		)
		(pad "192" smd roundrect
			(at -4.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "VD1")
			(pinfunction "VD1")
			(pintype "bidirectional")
		)
		(pad "193" smd roundrect
			(at -5.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "VD2")
			(pinfunction "VD2")
			(pintype "bidirectional")
		)
		(pad "194" smd roundrect
			(at -5.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 199 "VD3")
			(pinfunction "VD3")
			(pintype "bidirectional")
		)
		(pad "195" smd roundrect
			(at -6.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "VD4")
			(pinfunction "VD4")
			(pintype "bidirectional")
		)
		(pad "196" smd roundrect
			(at -6.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 201 "VD5")
			(pinfunction "VD5")
			(pintype "bidirectional")
		)
		(pad "197" smd roundrect
			(at -7.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "VD6")
			(pinfunction "VD6")
			(pintype "bidirectional")
		)
		(pad "198" smd roundrect
			(at -7.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "VD7")
			(pinfunction "VD7")
			(pintype "bidirectional")
		)
		(pad "199" smd roundrect
			(at -8.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "VD8")
			(pinfunction "VD8")
			(pintype "bidirectional")
		)
		(pad "200" smd roundrect
			(at -8.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "201" smd roundrect
			(at -9.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "202" smd roundrect
			(at -9.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 205 "VD9")
			(pinfunction "VD9")
			(pintype "bidirectional")
		)
		(pad "203" smd roundrect
			(at -10.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "VD10")
			(pinfunction "VD10")
			(pintype "bidirectional")
		)
		(pad "204" smd roundrect
			(at -10.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 207 "VD11")
			(pinfunction "VD11")
			(pintype "bidirectional")
		)
		(pad "205" smd roundrect
			(at -11.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "VD12")
			(pinfunction "VD12")
			(pintype "bidirectional")
		)
		(pad "206" smd roundrect
			(at -11.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 209 "VD13")
			(pinfunction "VD13")
			(pintype "bidirectional")
		)
		(pad "207" smd roundrect
			(at -12.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "VD14")
			(pinfunction "VD14")
			(pintype "bidirectional")
		)
		(pad "208" smd roundrect
			(at -12.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "VD15")
			(pinfunction "VD15")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-208_28x28mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 186.4836 128.0414 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C44"
			(at 0.1746 -3.1496 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.3974 2.8448 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 60.325 68.453 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C49"
			(at 0.508 -3.175 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.445 2.54 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 72.39 84.201 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC11"
			(at -0.3048 10.7442 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "65256BLFP-10T"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "/RA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 232 "/RA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 241 "/RA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "/RA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "/RA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "/RA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "/RA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 247 "/RA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "/RA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 249 "/RA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 229 "/WD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "/WD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 227 "/WD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 337 "WD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "/WD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 344 "WD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "/WD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 301 "~{RCS2X}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/RA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 302 "~{ROE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/RA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "/RA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "/RA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "/RA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 240 "Net-(IC10-~{WE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 60.452 80.391 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C48"
			(at 5.207 0.127 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.699 2.413 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 187.833 99.441 180)
		(property "Reference" "M13"
			(at 0.3048 -2.3368 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 62 "~{RES}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 100.5586 69.088 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C29"
			(at 0.7366 -2.4892 90)
			(layer "B.SilkS")
		)
		(property "Value" "50pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 343 "WD5F")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 185.293 99.441 180)
		(property "Reference" "M12"
			(at 1.27 -2.5908 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "~{HALT}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 227.0506 122.3772 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R6"
			(at 4.5466 -0.0508 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "160"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 291 "Net-(LD2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 204.3176 63.1698)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C31"
			(at 0.1778 2.6416 0)
			(layer "B.SilkS")
		)
		(property "Value" "133pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 338 "RAS2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 118.6688 116.6622 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0.1778 2.7432 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 115.1636 84.2518)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C34"
			(at -0.9398 7.5184 0)
			(layer "B.SilkS")
		)
		(property "Value" "82pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 45 "12M")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 161.7726 128.0922 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB9"
			(at -0.3048 -6.9596 90)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 158 "CDCKD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 158 "CDCKD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 138.9888 111.5822)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C22"
			(at 0 -2.54 0)
			(layer "B.SilkS")
		)
		(property "Value" "N/U"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 177 "~{PCAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 64.135 117.856 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at -3.3274 -2.4892 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 87.249 91.694 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R11"
			(at 0 2.413 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 238 "~{CLWEX}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 327 "~{CLWE}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 171.958 121.031 180)
		(property "Reference" "M9"
			(at 0.635 3.048 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 107 "~{LWR}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 200.533 96.901 180)
		(property "Reference" "M5"
			(at 0.127 -2.667 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 67 "FC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 102.2096 94.9706)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C53"
			(at -0.2794 2.6416 0)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 238 "~{CLWEX}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 132.588 121.666 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB8"
			(at 5.08 -0.127 90)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 26 "SCOR")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 26 "SCOR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_SMD_Large"
		(layer "B.Cu")
		(at 171.2722 80.391 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB18"
			(at 0.8128 3.2512 0)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5748 0 180)
			(size 1.4 2.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1428571429)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5748 0 180)
			(size 1.4 2.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1428571429)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 168.0464 72.6694 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R5"
			(at -4.191 -0.254 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 81 "A13")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 208.6356 91.1606 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C23"
			(at 4.4958 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 129 "~{ERAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_SMD_Large"
		(layer "B.Cu")
		(at 193.4718 125.3998 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB4"
			(at -0.2032 2.9972 0)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5748 0 180)
			(size 1.4 2.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1428571429)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5748 0 180)
			(size 1.4 2.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1428571429)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 107.2388 75.9714 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R9"
			(at 4.6228 -0.0508 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 40 "PWCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 40 "PWCLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 133.223 98.806 180)
		(property "Reference" "M7"
			(at 0.254 -2.9718 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 308 "E")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 174.498 121.031 180)
		(property "Reference" "M10"
			(at 0.127 3.048 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 108 "~{UWR}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 64.135 84.201 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at 3.048 -3.048 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 208.6356 96.3422 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C25"
			(at 4.5974 1.3208 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 255 "~{EWE}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 215.0364 126.3142 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0.1778 -2.54 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 176.4792 130.8354)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C33"
			(at -2.8702 -2.3368 0)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 7 "25M")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 107.2388 82.5754)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C38"
			(at 4.9022 -0.762 0)
			(layer "B.SilkS")
		)
		(property "Value" "133pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 337 "WD3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 192.913 96.901 180)
		(property "Reference" "M3"
			(at 2.921 0.127 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 310 "~{IPL1}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:LED"
		(layer "B.Cu")
		(at 226.949 86.106 90)
		(property "Reference" "LD1"
			(at 4.8514 0.254 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "RED"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 288 "Net-(LD1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 289 "Net-(LD1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 199.7964 56.261)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 5.1562 0.0508 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 107.823 60.579)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 4.2672 0.1016 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 163.068 64.516 180)
		(property "Reference" "M0"
			(at 0.254 -2.921 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 263 "Net-(IC16-CS2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 186.4868 124.841 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at -0.0762 -3.0988 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 112.268 78.5114)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C57"
			(at 4.6482 -1.1176 0)
			(layer "B.SilkS")
		)
		(property "Value" "N/U"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 42 "PLRCK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 188.1886 56.261)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -0.2032 -2.54 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 138.176 100.838 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R2"
			(at -0.0762 -2.4638 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 346 "VCC2C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 61 "~{HALT}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 177.038 121.031 180)
		(property "Reference" "M11"
			(at -1.016 3.048 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 110 "~{CAS2}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 143.383 100.838 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R1"
			(at 0.1524 -2.5654 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 346 "VCC2C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 62 "~{RES}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 99.5934 124.841 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 0.0508 -2.6924 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 107.2388 86.1822)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C35"
			(at -3.4798 2.54 0)
			(layer "B.SilkS")
		)
		(property "Value" "60pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 39 "PDATA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 174.4218 86.6902 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at -4.2164 -0.1524 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 125.6284 82.2706)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C21"
			(at -0.381 2.8448 0)
			(layer "B.SilkS")
		)
		(property "Value" "133pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 97 "D10")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 64.135 100.711 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 0.1016 -3.048 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 98.3488 59.3598)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C30"
			(at -5.1562 0.4064 0)
			(layer "B.SilkS")
		)
		(property "Value" "N/U"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 109 "~{ASEL}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 159.8246 128.0922 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB10"
			(at 0.254 -6.5356 90)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 154 "WFCKD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 154 "WFCKD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 202.3872 124.9426 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R4"
			(at 0.127 2.5908 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 152 "Net-(IC2-LEDR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 294 "Net-(TR1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 221.9452 126.3142 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 1.7018 -2.5908 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 126.2126 121.666 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB5"
			(at 5.3594 0.1016 90)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 20 "DFCK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 20 "DFCK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:LED"
		(layer "B.Cu")
		(at 226.949 128.778 90)
		(property "Reference" "LD2"
			(at -1.4986 -3.0988 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "GREEN"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 290 "Net-(LD2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 291 "Net-(LD2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 152.7048 80.2894)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at -0.1778 -2.5908 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 346 "VCC2C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 115.1636 86.6902 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C54"
			(at 0.9398 -7.0104 0)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 339 "PBCLKF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 157.353 122.9868 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C39"
			(at 0.0254 8.636 90)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 341 "BCLKBF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 154.813 122.9868 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C55"
			(at -0.381 -2.6924 90)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 342 "DFCKBF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 197.993 96.901 180)
		(property "Reference" "M6"
			(at 0 -2.667 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 66 "FC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 198.882 63.2206)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R10"
			(at -5.461 0.254 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 237 "~{RAS2X}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 326 "~{RAS2}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 86.2838 63.8556 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C19"
			(at 0.2794 -2.6416 90)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 64.008 68.199 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0.3048 -2.5654 90)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 184.2008 121.9454)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C56"
			(at -1.9558 -2.3876 0)
			(layer "B.SilkS")
		)
		(property "Value" "N/U"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 336 "LRCKBF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 192.913 99.441 180)
		(property "Reference" "M4"
			(at -0.6096 -2.5908 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 309 "~{IPL2}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 92.0242 75.4634)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C37"
			(at -0.1524 2.286 0)
			(layer "B.SilkS")
		)
		(property "Value" "200pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 302 "~{ROE}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 208.026 124.9426 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R3"
			(at 0.0254 2.5908 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 153 "Net-(IC2-LEDG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 293 "Net-(TR2-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 167.386 61.3918)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 4.3434 -0.1016 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 5 "Net-(IC16-VCC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 157.9626 128.0922 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB11"
			(at 0.254 -6.1976 90)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 156 "SBSOB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 156 "SBSOB")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 159.893 122.9868 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C40"
			(at 0.0254 7.8232 90)
			(layer "B.SilkS")
		)
		(property "Value" "200pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 154 "WFCKD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 117.3988 80.645 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at -2.8702 -2.3368 0)
			(layer "B.SilkS")
		)
		(property "Value" "22uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 107.2388 78.5114 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R8"
			(at 4.5974 0.3048 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 42 "PLRCK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 42 "PLRCK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 124.333 121.666 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB6"
			(at 5.334 -0.1524 90)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 19 "LRCK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 19 "LRCK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 208.6356 93.7006 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C26"
			(at 4.445 0.1524 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 132 "~{ORAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 163.068 61.214 180)
		(property "Reference" "M14"
			(at 4.1402 0.127 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "Net-(IC16-VCC)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 175.0314 107.1626 180)
		(property "Reference" "M8"
			(at -3.0988 0.762 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 195 "VA17")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 190.373 99.441 180)
		(property "Reference" "M1"
			(at -0.508 -2.54 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "~{VPA}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 195.453 96.901 180)
		(property "Reference" "M2"
			(at 0.381 2.286 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 311 "~{IPL0}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 208.6356 82.2706 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C27"
			(at 3.0734 -2.5908 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 133 "~{OCAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 122.428 121.666 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "FB7"
			(at 0.635 -2.413 90)
			(layer "B.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 17 "BCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 17 "BCLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 87.249 94.234 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R12"
			(at -4.9276 -0.8382 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 238 "~{CLWEX}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 340 "~{CLWEY}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 194.056 69.5706)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at -0.0762 2.794 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 140.208 118.5418)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C32"
			(at -0.2286 2.54 0)
			(layer "B.SilkS")
		)
		(property "Value" "N/U"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 176 "~{PRAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 154.5336 114.9858)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at -5.0546 -0.0508 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 347 "VCC2B")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 227.0506 92.5576 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R7"
			(at 4.2926 0.0508 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "360"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 289 "Net-(LD1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 193.929 56.261)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -0.2032 -2.54 0)
			(layer "B.SilkS")
		)
		(property "Value" "1000pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 3 "Net-(IC6-CT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 208.6356 79.7306 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C24"
			(at 3.0734 2.286 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 130 "~{ECAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 112.268 75.9714)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C58"
			(at 4.8006 -0.8636 0)
			(layer "B.SilkS")
		)
		(property "Value" "N/U"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 40 "PWCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 111.7092 111.9378)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C36"
			(at -0.2794 -2.6924 0)
			(layer "B.SilkS")
		)
		(property "Value" "?F"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 336 "LRCKBF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder"
		(layer "B.Cu")
		(at 208.6356 98.8822 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C28"
			(at 4.3942 0.1016 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 135 "~{OWE}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 45.72 45.72)
		(end 67.72 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 45.72)
		(end 234.62 57.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 57.72)
		(end 234.12 57.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.1 137.72)
		(end 212.1 136.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.22 56.72)
		(end 79.97 56.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 177.5968 50.597569)
		(end 179.2968 50.597569)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 63.6524 50.5968)
		(end 65.3524 50.5968)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.12 64.72)
		(end 234.62 64.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 124.309885)
		(end 233.20323 124.309885)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.87 46.72)
		(end 159.87 55.22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 81.47 46.72)
		(mid 81.762893 46.012893)
		(end 82.47 45.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 91.234515)
		(end 233.20323 91.234515)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45.72 45.72)
		(end 45.72 137.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 81.28)
		(end 233.20323 81.28)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 183.5912 50.5968)
		(end 185.1912 50.5968)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.62 55.22)
		(end 172.62 46.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.12 64.72)
		(mid 230.62 61.22)
		(end 234.12 57.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.088 130.6068)
		(end 195.1228 130.6068)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 196.088 130.6068)
		(mid 198.193698 132.753009)
		(end 196.0626 134.874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.62 45.72)
		(end 234.62 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.202 137.7188)
		(end 234.62 137.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 67.72 45.72)
		(mid 68.427107 46.012893)
		(end 68.72 46.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 161.37 56.72)
		(mid 160.30934 56.28066)
		(end 159.87 55.22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.0064 75.4888)
		(end 229.0064 77.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.37 56.72)
		(end 171.12 56.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 64.72)
		(end 234.62 75.4888)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 50.6984 132.6896)
		(end 52.7984 132.6896)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 57.658 50.5968)
		(end 59.258 50.5968)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212.1 136.65)
		(mid 215.651 133.095993)
		(end 219.202 136.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 77.72)
		(end 229.0064 77.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.0626 134.874)
		(end 195.0974 134.874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45.72 137.72)
		(end 212.1 137.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 77.72)
		(end 234.62 137.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.47 55.22)
		(end 81.47 46.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.22 56.72)
		(mid 69.15934 56.28066)
		(end 68.72 55.22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.202 137.7188)
		(end 219.202 136.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.62 55.22)
		(mid 172.18066 56.28066)
		(end 171.12 56.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.0064 75.4888)
		(end 234.62 75.4888)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 57.658 61.1632)
		(end 61.308 61.1632)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.72 46.72)
		(end 68.72 55.22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.62 46.72)
		(mid 172.912893 46.012893)
		(end 173.62 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.47 45.72)
		(end 158.87 45.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 195.0974 134.874)
		(mid 193.012518 132.727914)
		(end 195.1228 130.6068)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 81.47 55.22)
		(mid 81.03066 56.28066)
		(end 79.97 56.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 230.5812 107.7468)
		(end 232.2812 107.7468)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.87 45.72)
		(mid 159.577107 46.012893)
		(end 159.87 46.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 134.2644)
		(end 233.20323 134.2644)
		(fill no)
		(layer "Edge.Cuts")
	)
	(image
		(at 139.2682 90.2716)
		(layer "User.1")
	)
	(image
		(at 139.1666 92.2782)
		(layer "User.2")
	)
	(image
		(at 140.0048 91.694)
		(layer "User.3")
		(scale 4)
	)
	(image
		(at 139.9794 91.8972)
		(layer "User.4")
		(scale 4)
	)
	(image
		(at 140.335 91.6432)
		(layer "User.5")
		(scale 4)
	)
)
