(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 71.9 141)
    (grid_origin 71.9 141)
    (pcbplotparams
      (layerselection 0x0001000_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "3_3V_Pico")
  (net 2 "GND")
  (net 3 "do7")
  (net 4 "do0")
  (net 5 "do15")
  (net 6 "do8")
  (net 7 "do14")
  (net 8 "do6")
  (net 9 "do9")
  (net 10 "do1")
  (net 11 "do13")
  (net 12 "do5")
  (net 13 "do10")
  (net 14 "do2")
  (net 15 "do12")
  (net 16 "do4")
  (net 17 "do3")
  (net 18 "Net-(IC1A-A0)")
  (net 19 "unconnected-(U1-NC-Pad1)")
  (net 20 "Net-(U2-GPIO16)")
  (net 21 "unconnected-(U2-GPIO17-Pad22)")
  (net 22 "unconnected-(U2-GPIO18-Pad24)")
  (net 23 "unconnected-(U2-GPIO19-Pad25)")
  (net 24 "Net-(U2-GPIO20)")
  (net 25 "unconnected-(U2-GPIO21-Pad27)")
  (net 26 "unconnected-(U2-GPIO22-Pad29)")
  (net 27 "unconnected-(U2-GPIO26_ADC0-Pad31)")
  (net 28 "unconnected-(U2-GPIO27_ADC1-Pad32)")
  (net 29 "unconnected-(U2-GPIO28_ADC2-Pad34)")
  (net 30 "unconnected-(U2-ADC_VREF-Pad35)")
  (net 31 "unconnected-(U2-3V3_EN-Pad37)")
  (net 32 "unconnected-(U2-VSYS-Pad39)")
  (net 33 "unconnected-(U2-VBUS-Pad40)")
  (net 34 "unconnected-(U2-SWCLK-Pad41)")
  (net 35 "unconnected-(U2-SWDIO-Pad43)")
  (net 36 "unconnected-(U3-NC-Pad1)")
  (net 37 "unconnected-(JP1-B-Pad3)")
  (net 38 "Net-(JP1-C)")
  (net 39 "do11")
  (net 40 "Net-(J17-In)")
  (net 41 "Net-(J18-In)")
  (net 42 "Net-(IC1A-A2)")
  (net 43 "Net-(IC1A-A4)")
  (net 44 "Net-(IC1A-A6)")
  (net 45 "Net-(IC1A-B6)")
  (net 46 "Net-(IC1A-B4)")
  (net 47 "Net-(IC1A-B2)")
  (net 48 "Net-(IC1A-B0)")
  (net 49 "Net-(IC2A-A0)")
  (net 50 "Net-(IC2A-A2)")
  (net 51 "Net-(IC2A-A4)")
  (net 52 "Net-(IC2A-A6)")
  (net 53 "Net-(IC2A-B6)")
  (net 54 "Net-(IC2A-B4)")
  (net 55 "Net-(IC2A-B2)")
  (net 56 "Net-(IC2A-B0)")
  (net 57 "Net-(IC3A-A0)")
  (net 58 "Net-(IC3A-A2)")
  (net 59 "Net-(IC3A-A4)")
  (net 60 "Net-(IC3A-A6)")
  (net 61 "Net-(IC3A-B6)")
  (net 62 "Net-(IC3A-B4)")
  (net 63 "Net-(IC3A-B2)")
  (net 64 "Net-(IC3A-B0)")
  (net 65 "Net-(IC4A-A0)")
  (net 66 "Net-(IC4A-A2)")
  (net 67 "Net-(IC4A-A4)")
  (net 68 "Net-(IC4A-A6)")
  (net 69 "Net-(IC4A-B6)")
  (net 70 "Net-(IC4A-B4)")
  (net 71 "Net-(IC4A-B2)")
  (net 72 "Net-(IC4A-B0)")
  (net 73 "Net-(R12-Pad2)")
  (net 74 "Net-(R21-Pad2)")
  (net 75 "Power  Supply")
  (net 76 "Net-(J19-Pin_3)")
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 101.511)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 59 "Net-(IC3A-A4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 8 "do6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 137.7775 77.543 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at 3.523 -0.1975 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 86.699896 94.475)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized_sma_in_board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.85) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0.200104 2.045) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 81.944 105.215 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 41 "Net-(J18-In)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 119.201)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 68 "Net-(IC4A-A6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 17 "do3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 151.7 118.486)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized_sma_in_board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.85) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at 0.05 -1.436) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 134.2448 134.8278 -45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at 0 -1.65 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 72 "Net-(IC4A-B0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 144.281 137.7 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C10" (at -0.028 2.092 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 107.311)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 58 "Net-(IC3A-A2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 12 "do5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 177.897 101.511 180)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J10" (at -0.012 4.157) (layer "F.SilkS"))
    (fp_text value "do6" (at -5 -0.33 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 8 "do6") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 177.897 89.811 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J8" (at 4.504 0.163 180) (layer "F.SilkS"))
    (fp_text value "do8" (at 0 5 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 6 "do8") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 89.811)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 49 "Net-(IC2A-A0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 6 "do8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 177.897 113.311)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J12" (at 0.012 -4.307) (layer "F.SilkS"))
    (fp_text value "do4" (at 5 0.3 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 16 "do4") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 108.65 68.5 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J1" (at 4.68 0.08 180) (layer "F.SilkS"))
    (fp_text value "do15" (at 0 -5.22 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 5 "do15") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 125.8374 85.8312 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 47 "Net-(IC1A-B2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 74.7 102.48 180)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr smd)
    (fp_text reference "J18" (at 0.057 6.248 180) (layer "F.SilkS"))
    (fp_text value "Ext. Clk." (at 8.58 -2.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "Net-(J18-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_SL_171971-0002_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 84.14 73.5 90)
    (descr "Molex Stackable Linear Connector, 171971-0002 (compatible alternatives: 171971-0102, 171971-0202), 2 Pins per row (https://www.molex.com/pdm_docs/sd/1719710002_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex SL vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J20" (at 1.27 -3.75 90) (layer "F.SilkS"))
    (fp_text value "EXT PWR" (at 6.217 0.876) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.27 1.85 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 90) (size 1.74 1.74) (drill 1.09) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.1436781609)
      (net 76 "Net-(J19-Pin_3)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 90) (size 1.74 1.74) (drill 1.09) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_SL_171971-0002_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MCU_RaspberryPi_and_Boards:RPi_Pico_SMD" (layer "F.Cu")
    (at 110.394448 112.3375 180)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "Pico" (at 0 2.159) (layer "F.Fab"))
    (fp_text user "GP0" (at -6.293552 -24.4405 45) (layer "F.SilkS"))
    (fp_text user "3V3" (at 6.507448 -13.8235 45) (layer "F.SilkS"))
    (fp_text user "GP27" (at 6.192448 -3.2685 45) (layer "F.SilkS"))
    (fp_text user "GP12" (at -6.024177 13.343149 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 0 21.456572 90) (layer "F.SilkS"))
    (fp_text user "SWDIO" (at 2.4384 20.828 90) (layer "F.SilkS"))
    (fp_text user "GP5" (at -6.293552 -9.32704 45) (layer "F.SilkS"))
    (fp_text user "GP1" (at -6.293552 -21.92159 45) (layer "F.SilkS"))
    (fp_text user "GP8" (at -6.293552 0.7486 45) (layer "F.SilkS"))
    (fp_text user "AGND" (at 6.192449 -5.8185 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 6.434885 -18.5185 45) (layer "F.SilkS"))
    (fp_text user "GP21" (at 6.192448 9.4315 45) (layer "F.SilkS"))
    (fp_text user "GP13" (at -6.024177 15.862059 45) (layer "F.SilkS"))
    (fp_text user "GP3" (at -6.293552 -14.36486 45) (layer "F.SilkS"))
    (fp_text user "RUN" (at 6.421416 1.8015 45) (layer "F.SilkS"))
    (fp_text user "GP26" (at 6.192448 -0.7385 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.266614 -19.402681 45) (layer "F.SilkS"))
    (fp_text user "GP17" (at 6.192448 22.1215 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.266614 18.380969 45) (layer "F.SilkS"))
    (fp_text user "GP14" (at -6.024177 20.899879 45) (layer "F.SilkS"))
    (fp_text user "3V3_EN" (at 5.669448 -15.5895 45) (layer "F.SilkS"))
    (fp_text user "GP28" (at 6.192448 -8.6125 45) (layer "F.SilkS"))
    (fp_text user "GP18" (at 6.192448 17.0415 45) (layer "F.SilkS"))
    (fp_text user "GP16" (at 6.052448 24.1135 180) (layer "F.SilkS"))
    (fp_text user "GP9" (at -6.293552 3.26751 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.266614 5.786419 45) (layer "F.SilkS"))
    (fp_text user "GP6" (at -6.293552 -4.28922 45) (layer "F.SilkS"))
    (fp_text user "GP19" (at 6.192448 14.5015 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 6.434885 19.5815 45) (layer "F.SilkS"))
    (fp_text user "GP7" (at -6.293552 -1.77031 45) (layer "F.SilkS"))
    (fp_text user "VBUS" (at 6.205917 -23.6685 45) (layer "F.SilkS"))
    (fp_text user "GP10" (at -6.024177 8.305329 45) (layer "F.SilkS"))
    (fp_text user "GP4" (at -6.293552 -11.84595 45) (layer "F.SilkS"))
    (fp_text user "GP15" (at -6.024177 23.418789 45) (layer "F.SilkS"))
    (fp_text user "GP22" (at 6.192448 4.3415 45) (layer "F.SilkS"))
    (fp_text user "GP11" (at -6.024177 10.824239 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -6.266614 -6.808131 45) (layer "F.SilkS"))
    (fp_text user "GP2" (at -6.293552 -16.88377 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 6.434885 6.8815 45) (layer "F.SilkS"))
    (fp_text user "VSYS" (at 6.273261 -21.0585 45) (layer "F.SilkS"))
    (fp_text user "SWCLK" (at -2.5908 20.713714 90) (layer "F.SilkS"))
    (fp_text user "ADC_VREF" (at 5.249639 -10.0225 45) (layer "F.SilkS"))
    (fp_text user "GP20" (at 6.192448 11.9615 45) (layer "F.SilkS"))
    (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 -30.2) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -8.89 -24.13 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 72 "Net-(IC4A-B0)") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "2" smd rect (at -8.89 -21.59 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 71 "Net-(IC4A-B2)") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "3" smd rect (at -8.89 -19.05 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at -8.89 -16.51 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 70 "Net-(IC4A-B4)") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" smd rect (at -8.89 -13.97 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 69 "Net-(IC4A-B6)") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" smd rect (at -8.89 -11.43 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 64 "Net-(IC3A-B0)") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" smd rect (at -8.89 -8.89 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 63 "Net-(IC3A-B2)") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" smd rect (at -8.89 -6.35 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "9" smd rect (at -8.89 -3.81 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 62 "Net-(IC3A-B4)") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "10" smd rect (at -8.89 -1.27 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 61 "Net-(IC3A-B6)") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "11" smd rect (at -8.89 1.27 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 56 "Net-(IC2A-B0)") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" smd rect (at -8.89 3.81 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 55 "Net-(IC2A-B2)") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" smd rect (at -8.89 6.35 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "14" smd rect (at -8.89 8.89 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 54 "Net-(IC2A-B4)") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "15" smd rect (at -8.89 11.43 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 53 "Net-(IC2A-B6)") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "16" smd rect (at -8.89 13.97 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 48 "Net-(IC1A-B0)") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "17" smd rect (at -8.89 16.51 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 47 "Net-(IC1A-B2)") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "18" smd rect (at -8.89 19.05 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" smd rect (at -8.89 21.59 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 46 "Net-(IC1A-B4)") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "20" smd rect (at -8.89 24.13 180) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 45 "Net-(IC1A-B6)") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "21" smd rect (at 8.89 24.13 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 20 "Net-(U2-GPIO16)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "22" smd rect (at 8.89 21.59 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 21 "unconnected-(U2-GPIO17-Pad22)") (pinfunction "GPIO17") (pintype "bidirectional+no_connect"))
    (pad "23" smd rect (at 8.89 19.05 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "24" smd rect (at 8.89 16.51 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 22 "unconnected-(U2-GPIO18-Pad24)") (pinfunction "GPIO18") (pintype "bidirectional+no_connect"))
    (pad "25" smd rect (at 8.89 13.97 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 23 "unconnected-(U2-GPIO19-Pad25)") (pinfunction "GPIO19") (pintype "bidirectional+no_connect"))
    (pad "26" smd rect (at 8.89 11.43 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 24 "Net-(U2-GPIO20)") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "27" smd rect (at 8.89 8.89 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 25 "unconnected-(U2-GPIO21-Pad27)") (pinfunction "GPIO21") (pintype "bidirectional+no_connect"))
    (pad "28" smd rect (at 8.89 6.35 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "29" smd rect (at 8.89 3.81 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 26 "unconnected-(U2-GPIO22-Pad29)") (pinfunction "GPIO22") (pintype "bidirectional+no_connect"))
    (pad "30" smd rect (at 8.89 1.27 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 38 "Net-(JP1-C)") (pinfunction "RUN") (pintype "input"))
    (pad "31" smd rect (at 8.89 -1.27 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 27 "unconnected-(U2-GPIO26_ADC0-Pad31)") (pinfunction "GPIO26_ADC0") (pintype "bidirectional+no_connect"))
    (pad "32" smd rect (at 8.89 -3.81 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 28 "unconnected-(U2-GPIO27_ADC1-Pad32)") (pinfunction "GPIO27_ADC1") (pintype "bidirectional+no_connect"))
    (pad "33" smd rect (at 8.89 -6.35 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "AGND") (pintype "power_in"))
    (pad "34" smd rect (at 8.89 -8.89 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 29 "unconnected-(U2-GPIO28_ADC2-Pad34)") (pinfunction "GPIO28_ADC2") (pintype "bidirectional+no_connect"))
    (pad "35" smd rect (at 8.89 -11.43 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 30 "unconnected-(U2-ADC_VREF-Pad35)") (pinfunction "ADC_VREF") (pintype "unspecified+no_connect"))
    (pad "36" smd rect (at 8.89 -13.97 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 1 "3_3V_Pico") (pinfunction "3V3") (pintype "unspecified"))
    (pad "37" smd rect (at 8.89 -16.51 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 31 "unconnected-(U2-3V3_EN-Pad37)") (pinfunction "3V3_EN") (pintype "input+no_connect"))
    (pad "38" smd rect (at 8.89 -19.05 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "39" smd rect (at 8.89 -21.59 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 32 "unconnected-(U2-VSYS-Pad39)") (pinfunction "VSYS") (pintype "unspecified+no_connect"))
    (pad "40" smd rect (at 8.89 -24.13 180) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 33 "unconnected-(U2-VBUS-Pad40)") (pinfunction "VBUS") (pintype "unspecified+no_connect"))
    (pad "41" smd rect (at -2.54 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 34 "unconnected-(U2-SWCLK-Pad41)") (pinfunction "SWCLK") (pintype "input+no_connect"))
    (pad "42" smd rect (at 0 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "43" smd rect (at 2.54 23.9 270) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 35 "unconnected-(U2-SWDIO-Pad43)") (pinfunction "SWDIO") (pintype "bidirectional+no_connect"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 121.3002 83.2912)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 1.3868 1.4848) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 46 "Net-(IC1A-B4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 139.241 137.7 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 71.924)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 52 "Net-(IC2A-A6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 39 "do11") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 93.763 124.758 45)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "JR5" (at 0 -2.28 45) (layer "F.SilkS"))
    (fp_text value "0" (at 0 2.28 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0 45) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0 45) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 143.9 79.1764)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "JR3" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "0" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 77.841)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 51 "Net-(IC2A-A4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 13 "do10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 125.38 67.36 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at -1.515 -1.841 90) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 42 "Net-(IC1A-A2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 11 "do13") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICs:SOIC127P1032X265-20N" (layer "F.Cu")
    (at 143.9 128.0206 180)
    (descr "SO20")
    (tags "Integrated Circuit")
    (property "Description" "74LVT245 - 3.3 V octal transceiver with direction pin (3-state)@en-us")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC4" (at 0 0) (layer "F.SilkS"))
    (fp_text value "74LVT245D,118" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "DIR") (pintype "power_in"))
    (pad "2" smd rect (at -4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(IC4A-A0)") (pinfunction "A0") (pintype "output"))
    (pad "3" smd rect (at -4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "Net-(IC4A-A0)") (pinfunction "A1") (pintype "output"))
    (pad "4" smd rect (at -4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(IC4A-A2)") (pinfunction "A2") (pintype "output"))
    (pad "5" smd rect (at -4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(IC4A-A2)") (pinfunction "A3") (pintype "output"))
    (pad "6" smd rect (at -4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(IC4A-A4)") (pinfunction "A4") (pintype "output"))
    (pad "7" smd rect (at -4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(IC4A-A4)") (pinfunction "A5") (pintype "output"))
    (pad "8" smd rect (at -4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(IC4A-A6)") (pinfunction "A6") (pintype "output"))
    (pad "9" smd rect (at -4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(IC4A-A6)") (pinfunction "A7") (pintype "output"))
    (pad "10" smd rect (at -4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd rect (at 4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(IC4A-B6)") (pinfunction "B7") (pintype "input"))
    (pad "12" smd rect (at 4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "Net-(IC4A-B6)") (pinfunction "B6") (pintype "input"))
    (pad "13" smd rect (at 4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(IC4A-B4)") (pinfunction "B5") (pintype "input"))
    (pad "14" smd rect (at 4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(IC4A-B4)") (pinfunction "B4") (pintype "input"))
    (pad "15" smd rect (at 4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(IC4A-B2)") (pinfunction "B3") (pintype "input"))
    (pad "16" smd rect (at 4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "Net-(IC4A-B2)") (pinfunction "B2") (pintype "input"))
    (pad "17" smd rect (at 4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(IC4A-B0)") (pinfunction "B1") (pintype "input"))
    (pad "18" smd rect (at 4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "Net-(IC4A-B0)") (pinfunction "B0") (pintype "input"))
    (pad "19" smd rect (at 4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "~{OE}") (pintype "power_in"))
    (pad "20" smd rect (at 4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Power  Supply") (pinfunction "VCC") (pintype "power_in"))
    (model "74LVT245D,118.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 117.3 68.5 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -0.04 1.871) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 44 "Net-(IC1A-A6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 180) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 5 "do15") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 94.834 83.471)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "3_3V_Pico") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICs:SOIC127P1032X265-20N" (layer "F.Cu")
    (at 143.9 87.7616 180)
    (descr "SO20")
    (tags "Integrated Circuit")
    (property "Description" "74LVT245 - 3.3 V octal transceiver with direction pin (3-state)@en-us")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "74LVT245D,118" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "DIR") (pintype "power_in"))
    (pad "2" smd rect (at -4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(IC2A-A0)") (pinfunction "A0") (pintype "output"))
    (pad "3" smd rect (at -4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "Net-(IC2A-A0)") (pinfunction "A1") (pintype "output"))
    (pad "4" smd rect (at -4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(IC2A-A2)") (pinfunction "A2") (pintype "output"))
    (pad "5" smd rect (at -4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(IC2A-A2)") (pinfunction "A3") (pintype "output"))
    (pad "6" smd rect (at -4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(IC2A-A4)") (pinfunction "A4") (pintype "output"))
    (pad "7" smd rect (at -4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "Net-(IC2A-A4)") (pinfunction "A5") (pintype "output"))
    (pad "8" smd rect (at -4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(IC2A-A6)") (pinfunction "A6") (pintype "output"))
    (pad "9" smd rect (at -4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "Net-(IC2A-A6)") (pinfunction "A7") (pintype "output"))
    (pad "10" smd rect (at -4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd rect (at 4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(IC2A-B6)") (pinfunction "B7") (pintype "input"))
    (pad "12" smd rect (at 4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(IC2A-B6)") (pinfunction "B6") (pintype "input"))
    (pad "13" smd rect (at 4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(IC2A-B4)") (pinfunction "B5") (pintype "input"))
    (pad "14" smd rect (at 4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Net-(IC2A-B4)") (pinfunction "B4") (pintype "input"))
    (pad "15" smd rect (at 4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(IC2A-B2)") (pinfunction "B3") (pintype "input"))
    (pad "16" smd rect (at 4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Net-(IC2A-B2)") (pinfunction "B2") (pintype "input"))
    (pad "17" smd rect (at 4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(IC2A-B0)") (pinfunction "B1") (pintype "input"))
    (pad "18" smd rect (at 4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(IC2A-B0)") (pinfunction "B0") (pintype "input"))
    (pad "19" smd rect (at 4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "~{OE}") (pintype "power_in"))
    (pad "20" smd rect (at 4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Power  Supply") (pinfunction "VCC") (pintype "power_in"))
    (model "74LVT245D,118.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 95.35 113.6 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, both open")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "RESET" (at 0 7.41) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 38 "Net-(JP1-C)") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(JP1-B-Pad3)") (pinfunction "B") (pintype "passive+no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICs:SOIC127P1032X265-20N" (layer "F.Cu")
    (at 123.4752 76 -90)
    (descr "SO20")
    (tags "Integrated Circuit")
    (property "Description" "74LVT245 - 3.3 V octal transceiver with direction pin (3-state)@en-us")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC1" (at 0 0 90) (layer "F.SilkS"))
    (fp_text value "74LVT245D,118" (at 0 0 90) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -4.725 -5.715) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "DIR") (pintype "power_in"))
    (pad "2" smd rect (at -4.725 -4.445) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(IC1A-A0)") (pinfunction "A0") (pintype "output"))
    (pad "3" smd rect (at -4.725 -3.175) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(IC1A-A0)") (pinfunction "A1") (pintype "output"))
    (pad "4" smd rect (at -4.725 -1.905) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(IC1A-A2)") (pinfunction "A2") (pintype "output"))
    (pad "5" smd rect (at -4.725 -0.635) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "Net-(IC1A-A2)") (pinfunction "A3") (pintype "output"))
    (pad "6" smd rect (at -4.725 0.635) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(IC1A-A4)") (pinfunction "A4") (pintype "output"))
    (pad "7" smd rect (at -4.725 1.905) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(IC1A-A4)") (pinfunction "A5") (pintype "output"))
    (pad "8" smd rect (at -4.725 3.175) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(IC1A-A6)") (pinfunction "A6") (pintype "output"))
    (pad "9" smd rect (at -4.725 4.445) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(IC1A-A6)") (pinfunction "A7") (pintype "output"))
    (pad "10" smd rect (at -4.725 5.715) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd rect (at 4.725 5.715) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(IC1A-B6)") (pinfunction "B7") (pintype "input"))
    (pad "12" smd rect (at 4.725 4.445) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "Net-(IC1A-B6)") (pinfunction "B6") (pintype "input"))
    (pad "13" smd rect (at 4.725 3.175) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(IC1A-B4)") (pinfunction "B5") (pintype "input"))
    (pad "14" smd rect (at 4.725 1.905) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "Net-(IC1A-B4)") (pinfunction "B4") (pintype "input"))
    (pad "15" smd rect (at 4.725 0.635) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(IC1A-B2)") (pinfunction "B3") (pintype "input"))
    (pad "16" smd rect (at 4.725 -0.635) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "Net-(IC1A-B2)") (pinfunction "B2") (pintype "input"))
    (pad "17" smd rect (at 4.725 -1.905) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(IC1A-B0)") (pinfunction "B1") (pintype "input"))
    (pad "18" smd rect (at 4.725 -3.175) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "Net-(IC1A-B0)") (pinfunction "B0") (pintype "input"))
    (pad "19" smd rect (at 4.725 -4.445) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "~{OE}") (pintype "power_in"))
    (pad "20" smd rect (at 4.725 -5.715) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Power  Supply") (pinfunction "VCC") (pintype "power_in"))
    (model "74LVT245D,118.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 125.011)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 67 "Net-(IC4A-A4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 14 "do2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 83.494448 87.2375)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "470" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 40 "Net-(J17-In)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 73 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 126.6502 116.362 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 62 "Net-(IC3A-B4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 136.611)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R36" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 65 "Net-(IC4A-A0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 4 "do0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 144.137 119.499)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "JR2" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "0" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 83.67)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 50 "Net-(IC2A-A2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 9 "do9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 131.8826 107.7006 -45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at -0.162776 -1.853327 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 61 "Net-(IC3A-B6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 93.2715 78.54 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J19" (at 2.3895 2.795 90) (layer "F.SilkS"))
    (fp_text value "PWR SEL" (at 0 7.41) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "3_3V_Pico") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 75 "Power  Supply") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 76 "Net-(J19-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 141.761 137.7 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C8" (at 0.008 0.001 180) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 83.594448 99.9375)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "470" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 41 "Net-(J18-In)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 74 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 139.192 97.286 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_132289_EdgeMount" (layer "F.Cu")
    (at 74.7 87.2375 180)
    (descr "http://www.amphenolrf.com/132289.html")
    (tags "SMA")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr smd)
    (fp_text reference "J17" (at 0.057 6.2795 180) (layer "F.SilkS"))
    (fp_text value "Ext. Trig." (at 8.68 -1.7825) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.79 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at 0 0 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(J17-In)") (pinfunction "In") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 -4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" smd rect (at 0 4.25 270) (size 1.5 5.08) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_132289_EdgeMount.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 95.48 95.009 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.85 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 1 "3_3V_Pico") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 124.291 129.844 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 70 "Net-(IC4A-B4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 130.811)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R35" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 66 "Net-(IC4A-A2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 10 "do1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 129.495 125.3188 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 270) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 69 "Net-(IC4A-B6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 130.899 101.255 -45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.65 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 55 "Net-(IC2A-B2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICs:SOIC127P1032X265-20N" (layer "F.Cu")
    (at 143.9 108.869 180)
    (descr "SO20")
    (tags "Integrated Circuit")
    (property "Description" "74LVT245 - 3.3 V octal transceiver with direction pin (3-state)@en-us")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "IC3" (at 0 0) (layer "F.SilkS"))
    (fp_text value "74LVT245D,118" (at 0 0) (layer "F.SilkS") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "DIR") (pintype "power_in"))
    (pad "2" smd rect (at -4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(IC3A-A0)") (pinfunction "A0") (pintype "output"))
    (pad "3" smd rect (at -4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "Net-(IC3A-A0)") (pinfunction "A1") (pintype "output"))
    (pad "4" smd rect (at -4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(IC3A-A2)") (pinfunction "A2") (pintype "output"))
    (pad "5" smd rect (at -4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "Net-(IC3A-A2)") (pinfunction "A3") (pintype "output"))
    (pad "6" smd rect (at -4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(IC3A-A4)") (pinfunction "A4") (pintype "output"))
    (pad "7" smd rect (at -4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(IC3A-A4)") (pinfunction "A5") (pintype "output"))
    (pad "8" smd rect (at -4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(IC3A-A6)") (pinfunction "A6") (pintype "output"))
    (pad "9" smd rect (at -4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "Net-(IC3A-A6)") (pinfunction "A7") (pintype "output"))
    (pad "10" smd rect (at -4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd rect (at 4.725 5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(IC3A-B6)") (pinfunction "B7") (pintype "input"))
    (pad "12" smd rect (at 4.725 4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "Net-(IC3A-B6)") (pinfunction "B6") (pintype "input"))
    (pad "13" smd rect (at 4.725 3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(IC3A-B4)") (pinfunction "B5") (pintype "input"))
    (pad "14" smd rect (at 4.725 1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(IC3A-B4)") (pinfunction "B4") (pintype "input"))
    (pad "15" smd rect (at 4.725 0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(IC3A-B2)") (pinfunction "B3") (pintype "input"))
    (pad "16" smd rect (at 4.725 -0.635 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "Net-(IC3A-B2)") (pinfunction "B2") (pintype "input"))
    (pad "17" smd rect (at 4.725 -1.905 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(IC3A-B0)") (pinfunction "B1") (pintype "input"))
    (pad "18" smd rect (at 4.725 -3.175 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "Net-(IC3A-B0)") (pinfunction "B0") (pintype "input"))
    (pad "19" smd rect (at 4.725 -4.445 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "~{OE}") (pintype "power_in"))
    (pad "20" smd rect (at 4.725 -5.715 270) (size 0.7 1.95) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Power  Supply") (pinfunction "VCC") (pintype "power_in"))
    (model "74LVT245D,118.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 130.6634 120.4768 -45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 -1.65 135) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 64 "Net-(IC3A-B0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 164.897 95.511 180)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J9" (at -0.162 4.038) (layer "F.SilkS"))
    (fp_text value "do7" (at -5.03 -0.52 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 3 "do7") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 180) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (layer "F.Cu")
    (at 91.9 87.211)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Schmitt Buffer Gate, Low-Voltage CMOS")
    (property "ki_keywords" "Single Gate Buff Schmitt LVC CMOS")
    (attr smd)
    (fp_text reference "U1" (at -0.178 -2.409) (layer "F.SilkS"))
    (fp_text value "74LVC1G17" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(U1-NC-Pad1)") (pinfunction "NC") (pintype "free"))
    (pad "2" smd rect (at -1.35 0) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "Net-(R12-Pad2)") (pintype "input"))
    (pad "3" smd rect (at -1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at 1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(U2-GPIO16)") (pintype "output"))
    (pad "5" smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "3_3V_Pico") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 177.897 125.011)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J14" (at 0 -4.75) (layer "F.SilkS"))
    (fp_text value "do2" (at 5 0.17 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 14 "do2") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 139.706 68.5 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J4" (at 4.68 -0.176 180) (layer "F.SilkS"))
    (fp_text value "do12" (at 0 5 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 15 "do12") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 151.7 97.886)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized_sma_in_board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.85) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at -1.75 -2.466) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 118.5 60 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J2" (at 4.59 -0.1 180) (layer "F.SilkS"))
    (fp_text value "do14" (at 0 5 270) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 7 "do14") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 126.847107 97.043107 135)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.65 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 135) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 53 "Net-(IC2A-B6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 135) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 102.387 76 90)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "JR1" (at 0 -2.28 90) (layer "F.SilkS"))
    (fp_text value "0" (at 0 2.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0 90) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0 90) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 124.2118 120.2388 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0.0088 -1.3918 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 63 "Net-(IC3A-B2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 177.897 136.6)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J16" (at 0.086 -4.093) (layer "F.SilkS"))
    (fp_text value "do0" (at 5 0.38 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 4 "do0") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 126.29 102.684 -45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.65 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 54 "Net-(IC2A-B4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 315) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 81.887 92.338 -90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.82 90) (layer "F.SilkS"))
    (fp_text value "47k" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 40 "Net-(J17-In)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 270) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 130.01 60 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J3" (at 4.64 -0.19 180) (layer "F.SilkS"))
    (fp_text value "do13" (at 0 5 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 11 "do13") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 116.1854 84.104 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at 0.6014 1.802) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 45 "Net-(IC1A-B6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 180) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 164.897 71.932 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J5" (at 4.352 -0.119 180) (layer "F.SilkS"))
    (fp_text value "do11" (at 0 5.03 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 39 "do11") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 113.311)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 57 "Net-(IC3A-A0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 16 "do4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380" (layer "F.Cu")
    (at 86.699896 113.525)
    (descr "Mounting Hole 3.2mm, no annular, M3, ISO7380")
    (tags "mounting hole 3.2mm no annular m3 iso7380")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized_sma_in_board.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Mounting Hole without connection")
    (property "ki_keywords" "mounting hole")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.85) (layer "F.SilkS") hide)
    (fp_text value "MountingHole" (at -0.849896 2.975) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers "*.Cu" "*.Mask"))
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 157.897 95.511)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 60 "Net-(IC3A-A6)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 3 "do7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 127.3106 132.9228 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 71 "Net-(IC4A-B2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 177.897 77.841 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J6" (at 4.201 0.147 180) (layer "F.SilkS"))
    (fp_text value "do10" (at 0 5 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 13 "do10") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 164.897 119.201)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J13" (at 0 -4.087) (layer "F.SilkS"))
    (fp_text value "do3" (at 5.03 0.27 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 17 "do3") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 129.47 68.5)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.82) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 18 "Net-(IC1A-A0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 15 "do12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (layer "F.Cu")
    (at 91.9 99.9375)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Buffef Gate, Low-Voltage CMOS")
    (property "ki_keywords" "Single Gate Buff LVC CMOS")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.9) (layer "F.SilkS"))
    (fp_text value "74LVC1G34" (at 0 2.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "unconnected-(U3-NC-Pad1)") (pinfunction "NC") (pintype "free"))
    (pad "2" smd rect (at -1.35 0) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(R21-Pad2)") (pintype "input"))
    (pad "3" smd rect (at -1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect (at 1.35 0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(U2-GPIO20)") (pintype "output"))
    (pad "5" smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "3_3V_Pico") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 129.715 85.212)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 48 "Net-(IC1A-B0)") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 137.531 117.806)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.85) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 134.995 77.543 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at 3.523 -0.12 180) (layer "F.SilkS"))
    (fp_text value "1u" (at -3.717 -0.135 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 164.897 107.311)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J11" (at -0.018 -4.199) (layer "F.SilkS"))
    (fp_text value "do5" (at 5.03 0.29 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 12 "do5") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 164.897 83.662 90)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J7" (at 3.981 0.086 180) (layer "F.SilkS"))
    (fp_text value "do9" (at 0 5.03 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 9 "do9") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54 90) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 132.2125 77.543 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 3.523 -0.0425 180) (layer "F.SilkS"))
    (fp_text value "100n" (at -4.557 -0.1025 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 90) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 75 "Power  Supply") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (at 133.723 104.042 135)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at -0.345068 1.630588 135) (layer "F.SilkS"))
    (fp_text value "10k" (at 0 1.65 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1 0 135) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 135) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 56 "Net-(IC2A-B0)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Coaxial:SMA_Amphenol_901-144_Vertical" (layer "F.Cu")
    (at 164.897 130.811)
    (descr "https://www.amphenolrf.com/downloads/dl/file/id/7023/product/3103/901_144_customer_drawing.pdf")
    (tags "SMA THT Female Jack Vertical")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, LEMO, ...)")
    (property "ki_keywords" "BNC SMA SMB SMC LEMO coaxial connector CINCH RCA MCX MMCX U.FL UMRF")
    (attr through_hole)
    (fp_text reference "J15" (at -0.011 -4.07) (layer "F.SilkS"))
    (fp_text value "do1" (at 5.03 0.03 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 2.05 2.05) (drill 1.5) (layers "*.Cu" "*.Mask")
      (net 10 "do1") (pinfunction "In") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 -2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 2.54) (size 2.25 2.25) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Ext") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Coaxial.3dshapes/SMA_Amphenol_901-144_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder" (layer "F.Cu")
    (at 121.5702 67.36 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "PrawnDO_Breakout_Connectorized.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 1.627 1.8638 270 unlocked) (layer "F.SilkS"))
    (fp_text value "49.9" (at 0 1.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 43 "Net-(IC1A-A4)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.55 0 90) (size 1.3 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1923076923)
      (net 7 "do14") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_2010_5025Metric_Pad1.40x2.65mm_HandSolder" (layer "F.Cu")
    (at 144.63 100.384)
    (descr "Resistor SMD 2010 (5025 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "power_connections_prawn_DO.kicad_sch")
    (property "Sheetname" "Power connections")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "JR4" (at 0 -2.28) (layer "F.SilkS"))
    (fp_text value "0" (at 0 2.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.4 0) (size 1.4 2.65) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1785707143)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2010_5025Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 71.9 141) (end 71.9 54.2)
    (layer "Edge.Cuts"))
  (gr_line (start 115.9 138.8) (end 104.9 138.8)
    (layer "Edge.Cuts"))
  (gr_line (start 115.9 141) (end 115.9 138.8)
    (layer "Edge.Cuts"))
  (gr_line (start 71.9 141) (end 104.9 141)
    (layer "Edge.Cuts"))
  (gr_line (start 184.9 54.2) (end 71.9 54.2)
    (layer "Edge.Cuts"))
  (gr_line (start 184.9 141) (end 184.9 54.2)
    (layer "Edge.Cuts"))
  (gr_line (start 115.9 141) (end 184.9 141)
    (layer "Edge.Cuts"))
  (gr_line (start 104.9 138.8) (end 104.9 141)
    (layer "Edge.Cuts"))
  (gr_text "Ext Clk" (at 72.63 109.79) (layer "F.SilkS"))
  (gr_text "Ext Trg" (at 72.33 94.62) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0))
    (min_thickness 0.25) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 106.094448 123.5375)
        (xy 106.094448 137.6375)
        (xy 114.494448 137.6375)
        (xy 114.494448 123.5375)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 71.92 54.22)
        (xy 71.9 141.01)
        (xy 184.91 141.02)
        (xy 184.89 54.23)
      )
    )
  )
)
