(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 122.5 92.25 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 108.695 81.65)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "J1"
			(at 2.805 4.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x06"
			(at 0 15.08 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 6.35 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/CTS")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pin_3-Pad3)")
			(pinfunction "Pin_3_3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/TXD")
			(pinfunction "Pin_4_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/RXD")
			(pinfunction "Pin_5_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/RTS")
			(pinfunction "Pin_6_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 113 92.25 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R3"
			(at 2.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 120 92.25 90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "LED")
		(property "Reference" "D2"
			(at 2.5 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D2-K)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 90)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/TXD")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RVL:TACTILE_SWITCH_SMD_4.6X2.8MM"
		(layer "F.Cu")
		(at 114.75 81.55 180)
		(descr "<h3>Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm</h3>\n<p>Normally-open (NO) SPST momentary switches (buttons, pushbuttons).</p>\n<p><a href=\"http://www.ck-components.com/media/1479/kmr2.pdf\">Datasheet</a></p>")
		(property "Reference" "SW1"
			(at -2.95 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_Dual"
			(at 0 1.524 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, symbol, four pins"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "3" "2" "4")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -2.05 0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "1_1")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 2.05 0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 2.05 -0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/EN")
			(pinfunction "3_3")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at -2.05 -0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/EN")
			(pinfunction "4_4")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "RVL:CONN_532610001-SD_05_MOL"
		(layer "F.Cu")
		(at 128.6942 88 -90)
		(tags "532610571 ")
		(property "Reference" "J2"
			(at 0 2.9045 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "532610571"
			(at 0 2.9045 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.molex.com/en-us/products/part-detail-pdf/532610571?display=pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_532610001-SD_05_MOL")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.9045 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 2.5 2.9045 270)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "1_1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.25 2.9045 270)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/TXD")
			(pinfunction "2_2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 2.9045 270)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RXD")
			(pinfunction "3_3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at -1.25 2.9045 270)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/IO0")
			(pinfunction "4_4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -2.5 2.9045 270)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/EN")
			(pinfunction "5_5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -5.05 0.004501 270)
			(size 2.2098 3.0988)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "7" smd rect
			(at 5.05 0.004501 270)
			(size 2.2098 3.0988)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 127.9914 84.004699) (xy 126.188 84.004699) (xy 126.188 84.995299) (xy 127.9914 84.995299)
				)
			)
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 127.9914 91.004701) (xy 126.188 91.004701) (xy 126.188 91.995301) (xy 127.9914 91.995301)
				)
			)
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 131.191401 84.004699) (xy 129.388001 84.004699) (xy 129.388001 84.995299) (xy 131.191401 84.995299)
				)
			)
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 131.191401 91.004701) (xy 129.388001 91.004701) (xy 129.388001 91.995301) (xy 131.191401 91.995301)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0805_2012Metric"
		(layer "F.Cu")
		(at 115.75 92.25 -90)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "LED")
		(property "Reference" "D1"
			(at -2.5 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D1-K)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9375 0 270)
			(size 0.975 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/RXD")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RVL:TACTILE_SWITCH_SMD_4.6X2.8MM"
		(layer "F.Cu")
		(at 121.5 81.55 180)
		(descr "<h3>Momentary Switch (Pushbutton) - SPST - SMD, 4.6 x 2.8mm</h3>\n<p>Normally-open (NO) SPST momentary switches (buttons, pushbuttons).</p>\n<p><a href=\"http://www.ck-components.com/media/1479/kmr2.pdf\">Datasheet</a></p>")
		(property "Reference" "SW2"
			(at -3.15 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push_Dual"
			(at 0 1.524 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, symbol, four pins"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "3" "2" "4")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -2.05 0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "1_1")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at 2.05 0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at 2.05 -0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/IO0")
			(pinfunction "3_3")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at -2.05 -0.8 180)
			(size 0.9 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/IO0")
			(pinfunction "4_4")
			(pintype "passive")
			(solder_mask_margin 0.0635)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 114.5 84.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R1"
			(at -2.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/RTS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/EN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 121.0875 84.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R2"
			(at -2.5875 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "serial-adapter.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/CTS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/IO0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 106.75 79.75)
		(end 106.75 96.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 106.75 96.25)
		(end 131.25 96.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.25 79.75)
		(end 106.75 79.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.25 96.25)
		(end 131.25 79.75)
		(layer "Edge.Cuts")
	)
	(gr_text "RXD"
		(at 112.75 90.25 0)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 120 90.25 0)
		(layer "F.SilkS")
	)
	(gr_text "EN"
		(at 112 82.5 90)
		(layer "F.SilkS")
	)
	(gr_text "MOD"
		(at 118.75 83.25 90)
		(layer "F.SilkS")
	)
	(gr_text "RVL Programmer v1\n© Bryan Hughes"
		(at 128 95.5 270)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
