(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "unconnected-(1-Pad28)")
	(net 2 "unconnected-(1-A13{slash}27-Pad27)")
	(net 3 "unconnected-(1-Pad29)")
	(net 4 "unconnected-(1-Pad32)")
	(net 5 "unconnected-(1-Pad33)")
	(net 6 "unconnected-(1-A10{slash}24-Pad24)")
	(net 7 "unconnected-(1-A12{slash}26-Pad26)")
	(net 8 "unconnected-(1-A11{slash}25-Pad25)")
	(net 9 "unconnected-(1-Pad31)")
	(net 10 "unconnected-(1-Pad30)")
	(net 11 "GND")
	(net 12 "Net-(PS1-+VIN)")
	(net 13 "unconnected-(1-PadPROG)")
	(net 14 "unconnected-(1-VBAT-PadVBAT\\)")
	(net 15 "unconnected-(1-PadON{slash}OFF)")
	(net 16 "unconnected-(1-Pad3V3_LN)")
	(net 17 "unconnected-(J1-EXT_CLK-Pad17)")
	(net 18 "unconnected-(J1-GPIO1-Pad6)")
	(net 19 "unconnected-(J1-GPIO2-Pad12)")
	(net 20 "unconnected-(J1-SDA-Pad20)")
	(net 21 "unconnected-(J1-NC-Pad19)")
	(net 22 "unconnected-(J1-NC-Pad9)")
	(net 23 "unconnected-(J1-NC-Pad5)")
	(net 24 "unconnected-(J1-SCL-Pad16)")
	(net 25 "unconnected-(J1-GND-Pad10)")
	(net 26 "unconnected-(J1-NC{slash}START-Pad14)")
	(net 27 "unconnected-(J1-CLKSEL-Pad2)")
	(net 28 "unconnected-(J1-GND-Pad18)")
	(net 29 "+9V")
	(net 30 "Net-(J3-Pin_12)")
	(net 31 "Net-(J1-RESETB)")
	(net 32 "Net-(J1-DOUT)")
	(net 33 "Net-(1-1{slash}TX1)")
	(net 34 "Net-(J1-CLK)")
	(net 35 "Net-(1-17{slash}A3{slash}TX4)")
	(net 36 "Net-(J1-START{slash}CS)")
	(net 37 "Net-(1-7{slash}RX2)")
	(net 38 "Net-(1-0{slash}RX1)")
	(net 39 "Net-(J1-CS)")
	(net 40 "Net-(1-15{slash}A1{slash}RX3)")
	(net 41 "Net-(J1-DIN)")
	(net 42 "Net-(1-14{slash}A0{slash}TX3)")
	(net 43 "Net-(J3-Pin_4)")
	(net 44 "Net-(J1-DRDYB)")
	(net 45 "Net-(J3-Pin_11)")
	(net 46 "Net-(1-8{slash}TX2)")
	(net 47 "Net-(1-16{slash}A2{slash}RX4)")
	(net 48 "Net-(J4-Pin_5)")
	(net 49 "Net-(1-21{slash}A7{slash}RX5)")
	(net 50 "Net-(1-20{slash}A6{slash}TX5)")
	(net 51 "Net-(J4-Pin_8)")
	(net 52 "Net-(J4-Pin_9)")
	(net 53 "Net-(J4-Pin_4)")
	(net 54 "Net-(J4-Pin_3)")
	(net 55 "Net-(J4-Pin_1)")
	(net 56 "Net-(J5-Pin_1)")
	(net 57 "Net-(J6-Pin_1)")
	(net 58 "unconnected-(U1-CTS-Pad2)")
	(net 59 "unconnected-(U1-RTS-Pad6)")
	(net 60 "Net-(J8-Pin_1)")
	(footprint ""
		(layer "F.Cu")
		(at 128.0668 71.8058)
		(property "Reference" "5"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.6868 79.4258)
		(property "Reference" "40"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 206.9846 48.7934 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J8"
			(at -3.7846 1.2954 0)
			(layer "F.SilkS")
		)
		(property "Value" "DEBUG_PWR"
			(at -2.3368 1.0668 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(J8-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(J4-Pin_3)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 120.4468 71.8058)
		(property "Reference" "2"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.6868 81.9658)
		(property "Reference" "48"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 130.6068 74.3458)
		(property "Reference" "14"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 137.5664 97.663 -90)
		(property "Reference" "41"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 201.3204 65.6336)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 12.319 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "330 ohm"
			(at 17.145 -0.3048 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(1-16{slash}A2{slash}RX4)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(J5-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.6868 71.8058)
		(property "Reference" "8"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 125.5268 81.9658)
		(property "Reference" "44"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 147.7264 95.123 -90)
		(property "Reference" "31"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 145.1864 97.663 -90)
		(property "Reference" "17"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.0264 95.123 -90)
		(property "Reference" "73"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 137.5664 95.123 -90)
		(property "Reference" "72"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.6868 76.8858)
		(property "Reference" "24"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 132.4864 92.583 -90)
		(property "Reference" "26"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 132.4864 90.043 -90)
		(property "Reference" "63"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 147.7264 90.043 -90)
		(property "Reference" "64"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 147.7264 87.503 -90)
		(property "Reference" "58"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D7.5mm_P2.50mm"
		(layer "F.Cu")
		(at 141.8482 49.784)
		(descr "CP, Radial series, Radial, pin pitch=2.50mm, diameter=7.5mm, height=8mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.50mm diameter 7.5mm height 8mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at -2.707 5 0)
			(layer "F.SilkS")
		)
		(property "Value" "1 uF"
			(at 1.25 5 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 55 "Net-(J4-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D7.5mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 122.9868 79.4258)
		(property "Reference" "35"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 145.1864 90.043 -90)
		(property "Reference" "65"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 132.4864 97.663 -90)
		(property "Reference" ""
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 145.1864 92.583 -90)
		(property "Reference" "28"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 125.5268 71.8058)
		(property "Reference" "4"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 122.1512 93.2688)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**1"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 206.5528 73.279 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J5"
			(at -2.5696 1.0972 0)
			(layer "F.SilkS")
		)
		(property "Value" "PWR_LED"
			(at -4.2206 0.9194 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(J5-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 122.9868 81.9658)
		(property "Reference" "43"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D10.0mm_P5.00mm"
		(layer "F.Cu")
		(at 128.239123 60.4012)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, diameter=10mm, height=16mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm diameter 10mm height 16mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at -2.128123 6.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "220 uF"
			(at 2.5 6.25 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 29 "+9V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0_ABR_footprints:TEENSY_4.0_WITH_24-33"
		(layer "F.Cu")
		(at 183.6 59 -90)
		(descr "WNG - Added 24 - 33")
		(property "Reference" "1"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(fp_text user "PJRC.COM"
			(at -3.175 3.81 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "TEENSY\n4.0"
			(at 0.03175 -0.762 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "0/RX" thru_hole circle
			(at -13.97 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(1-0{slash}RX1)")
			(pinfunction "0/RX1")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "1/TX" thru_hole circle
			(at -11.43 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(1-1{slash}TX1)")
			(pinfunction "1/TX1")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "2" thru_hole circle
			(at -8.89 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J3-Pin_4)")
			(pinfunction "2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3" thru_hole circle
			(at -6.35 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J1-DRDYB)")
			(pinfunction "3")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3V3_LN" thru_hole circle
			(at 16.51 2.54 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(1-Pad3V3_LN)")
			(pinfunction "3V3_LN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "3V3_LO" thru_hole circle
			(at -11.43 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(J4-Pin_3)")
			(pinfunction "3V3_LO")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "4" thru_hole circle
			(at -3.81 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J1-START{slash}CS)")
			(pinfunction "4")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "5" thru_hole circle
			(at -1.27 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J1-CS)")
			(pinfunction "5")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "6" thru_hole circle
			(at 1.27 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J1-RESETB)")
			(pinfunction "6")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "7" thru_hole circle
			(at 3.81 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(1-7{slash}RX2)")
			(pinfunction "7/RX2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "8" thru_hole circle
			(at 6.35 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(1-8{slash}TX2)")
			(pinfunction "8/TX2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "9" thru_hole circle
			(at 8.89 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J3-Pin_11)")
			(pinfunction "9")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "10/CS" thru_hole circle
			(at 11.43 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J3-Pin_12)")
			(pinfunction "10/CS")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "11/MOSI" thru_hole circle
			(at 13.97 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J1-DIN)")
			(pinfunction "11/MOSI")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "12/MISO" thru_hole circle
			(at 16.51 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J1-DOUT)")
			(pinfunction "12/MISO")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "13/SCK" thru_hole circle
			(at 16.51 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J1-CLK)")
			(pinfunction "13/SCK")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "14/A0" thru_hole circle
			(at 13.97 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(1-14{slash}A0{slash}TX3)")
			(pinfunction "14/A0/TX3")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "15/A1" thru_hole circle
			(at 11.43 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(1-15{slash}A1{slash}RX3)")
			(pinfunction "15/A1/RX3")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "16/A2" thru_hole circle
			(at 8.89 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(1-16{slash}A2{slash}RX4)")
			(pinfunction "16/A2/RX4")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "17/A3" thru_hole circle
			(at 6.35 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(1-17{slash}A3{slash}TX4)")
			(pinfunction "17/A3/TX4")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "18/A4/SDA" thru_hole circle
			(at 3.81 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J4-Pin_9)")
			(pinfunction "18/A4/SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "19/A5/SCL" thru_hole circle
			(at 1.27 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J4-Pin_8)")
			(pinfunction "19/A5/SCL")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "20/A6" thru_hole circle
			(at -1.27 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(1-20{slash}A6{slash}TX5)")
			(pinfunction "20/A6/TX5")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "21/A7" thru_hole circle
			(at -3.81 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(1-21{slash}A7{slash}RX5)")
			(pinfunction "21/A7/RX5")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "22/A8" thru_hole circle
			(at -6.35 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J4-Pin_5)")
			(pinfunction "22/A8")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "23/A9" thru_hole circle
			(at -8.89 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J4-Pin_4)")
			(pinfunction "23/A9")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "24" thru_hole circle
			(at 11.43 -5.08 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(1-A10{slash}24-Pad24)")
			(pinfunction "A10/24")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "25" thru_hole circle
			(at 8.89 -5.08 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(1-A11{slash}25-Pad25)")
			(pinfunction "A11/25")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "26" thru_hole circle
			(at 11.43 -2.54 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(1-A12{slash}26-Pad26)")
			(pinfunction "A12/26")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "27" thru_hole circle
			(at 8.89 -2.54 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "unconnected-(1-A13{slash}27-Pad27)")
			(pinfunction "A13/27")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "28" thru_hole circle
			(at 11.43 0 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "unconnected-(1-Pad28)")
			(pinfunction "28")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "29" thru_hole circle
			(at 8.89 0 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "unconnected-(1-Pad29)")
			(pinfunction "29")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "30" thru_hole circle
			(at 11.43 2.54 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(1-Pad30)")
			(pinfunction "30")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "31" thru_hole circle
			(at 8.89 2.54 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(1-Pad31)")
			(pinfunction "31")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "32" thru_hole circle
			(at 11.43 5.08 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "unconnected-(1-Pad32)")
			(pinfunction "32")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "33" thru_hole circle
			(at 8.89 5.08 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "unconnected-(1-Pad33)")
			(pinfunction "33")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "GND" thru_hole circle
			(at -16.51 7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "GND")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "GND2" thru_hole circle
			(at -13.97 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "GND2")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "GND3" thru_hole circle
			(at 16.51 0 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "GND3")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "ON/OFF" thru_hole circle
			(at 16.51 -5.08 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(1-PadON{slash}OFF)")
			(pinfunction "ON/OFF")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "PROG" thru_hole circle
			(at 16.51 -2.54 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(1-PadPROG)")
			(pinfunction "PROG")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "VBAT\\" thru_hole circle
			(at 16.51 5.08 90)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(1-VBAT-PadVBAT\\)")
			(pinfunction "VBAT")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(pad "VIN" thru_hole circle
			(at -16.51 -7.62 270)
			(size 1.4732 1.4732)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(J4-Pin_1)")
			(pinfunction "VIN")
			(pintype "bidirectional")
			(solder_mask_margin 0.1016)
			(thermal_bridge_angle 0)
		)
		(embedded_fonts no)
	)
	(footprint "Inductor_THT:L_Axial_L9.5mm_D4.0mm_P15.24mm_Horizontal_Fastron_SMCC"
		(layer "F.Cu")
		(at 139.8016 60.4012)
		(descr "Inductor, Axial series, Axial, Horizontal, pin pitch=15.24mm, length*diameter=9.5*4mm^2, Fastron, SMCC, http://cdn-reichelt.de/documents/datenblatt/B400/DS_SMCC_NEU.pdf, http://cdn-reichelt.de/documents/datenblatt/B400/LEADEDINDUCTORS.pdf")
		(tags "Inductor Axial series Axial Horizontal pin pitch 15.24mm  length 9.5mm diameter 4mm Fastron SMCC")
		(property "Reference" "L1"
			(at 7.62 -3.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "10 uH"
			(at 7.62 3.12 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "+9V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 15.24 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(PS1-+VIN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/L_Axial_L9.5mm_D4.0mm_P15.24mm_Horizontal_Fastron_SMCC.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 145.1864 87.503 -90)
		(property "Reference" "59"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 125.5268 79.4258)
		(property "Reference" "36"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 130.6068 81.9658)
		(property "Reference" "46"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 122.9868 76.8858)
		(property "Reference" "19"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 132.4864 95.123 -90)
		(property "Reference" "30"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 138.2268 81.9658)
		(property "Reference" "41"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 133.1468 71.8058)
		(property "Reference" "7"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 130.6068 79.4258)
		(property "Reference" "38"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 145.1864 95.123 -90)
		(property "Reference" "32"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "0_ABR_footprints:Adafruit_CP2102N_Friend"
		(layer "F.Cu")
		(at 215.392 55.1688 -90)
		(descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x06 2.54mm single row")
		(property "Reference" "U1"
			(at -4.6482 6.0198 0)
			(layer "F.SilkS")
		)
		(property "Value" "Adafruit_CP2102N_Friend"
			(at -2.8448 5.8166 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Adafruit_CP2102N_Friend"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3 -4.4958 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(U1-CTS-Pad2)")
			(pinfunction "CTS")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(J8-Pin_1)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(1-0{slash}RX1)")
			(pinfunction "TX")
			(pintype "bidirectional")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(1-1{slash}TX1)")
			(pinfunction "RX")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(U1-RTS-Pad6)")
			(pinfunction "RTS")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 122.9868 74.3458)
		(property "Reference" "11"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.0264 90.043 -90)
		(property "Reference" "68"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 219.1512 36.2688)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 194.437 42.49)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x14 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Teensy_pins13+"
			(at 0 35.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(1-21{slash}A7{slash}RX5)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(1-20{slash}A6{slash}TX5)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(J4-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J4-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(1-17{slash}A3{slash}TX4)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(1-16{slash}A2{slash}RX4)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(1-15{slash}A1{slash}RX3)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(1-14{slash}A0{slash}TX3)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J1-CLK)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 128.0668 74.3458)
		(property "Reference" "13"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 125.5268 74.3458)
		(property "Reference" "12"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 161.8488 78.3082)
		(descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x04 2.54mm single row")
		(property "Reference" "J2"
			(at -0.0762 10.3378 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1299_breakout"
			(at 0 10.39 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J1-CS)")
			(pinfunction "CS")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J1-START{slash}CS)")
			(pinfunction "START")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J1-DRDYB)")
			(pinfunction "DRDY")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J1-RESETB)")
			(pinfunction "RESET")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 133.1468 74.3458)
		(property "Reference" "15"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.0264 92.583 -90)
		(property "Reference" "70"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 125.5268 76.8858)
		(property "Reference" "20"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 147.7264 92.583 -90)
		(property "Reference" "27"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 147.7264 97.663 -90)
		(property "Reference" "9"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 138.2268 76.8858)
		(property "Reference" "25"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 120.4468 81.9658)
		(property "Reference" "42"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 219.1512 93.2688)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.80mm"
		(layer "F.Cu")
		(at 142.748 40.410651 90)
		(descr "CP, Radial series, Radial, pin pitch=3.80mm, diameter=8mm, height=14mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 3.80mm diameter 8mm height 14mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at 7.085851 -3.018349 0)
			(layer "F.SilkS")
		)
		(property "Value" "100 uF"
			(at 7.085851 1.9812 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 12 "Net-(PS1-+VIN)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.8 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.80mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 133.1468 81.9658)
		(property "Reference" "47"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 120.4468 76.8858)
		(property "Reference" "18"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x14_P2.54mm_Vertical"
		(locked yes)
		(layer "F.Cu")
		(at 171.9834 42.49)
		(descr "Through hole straight pin header, 1x14, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x14 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Teensy_0-12"
			(at 0 35.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x12, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 16.51 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(1-0{slash}RX1)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(1-1{slash}TX1)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J1-DRDYB)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(J1-START{slash}CS)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J1-CS)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J1-RESETB)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(1-7{slash}RX2)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(1-8{slash}TX2)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J3-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J3-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J1-DIN)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J1-DOUT)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x14_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 128.0668 81.9658)
		(property "Reference" "45"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 130.6068 76.8858)
		(property "Reference" "22"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 122.9868 71.8058)
		(property "Reference" "3"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 207.9956 80.3148 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J7"
			(at -2.794 1.4986 0)
			(layer "F.SilkS")
		)
		(property "Value" "TRIG_IN"
			(at -4.2926 1.0922 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(1-14{slash}A0{slash}TX3)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 137.5664 92.583 -90)
		(property "Reference" "69"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 138.2268 74.3458)
		(property "Reference" "17"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 131.5296 48.4178 90)
		(descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH vertical")
		(property "Reference" "X1"
			(at 8.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "from MMB0"
			(at 6.6 0.4 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "poslabel" "+"
			(at -1.4 -5.8 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.5 -2.6 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 29 "+9V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 120.4468 79.4258)
		(property "Reference" "34"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 215.9 73.279 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J6"
			(at -2.5188 1.4224 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DATA_LED"
			(at -4.2418 1.3462 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.5908 1.0414 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(J6-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.6464 95.123 -90)
		(property "Reference" "71"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.6464 97.663 -90)
		(property "Reference" "25"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.0264 87.503 -90)
		(property "Reference" "62"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 122.1512 36.2688)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**2"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 128.0668 76.8858)
		(property "Reference" "21"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 133.1468 76.8858)
		(property "Reference" "23"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.6464 90.043 -90)
		(property "Reference" "66"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 120.4468 74.3458)
		(property "Reference" "10"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 132.4864 87.503 -90)
		(property "Reference" "57"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.6464 87.503 -90)
		(property "Reference" "60"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 137.5664 90.043 -90)
		(property "Reference" "67"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 128.0668 79.4258)
		(property "Reference" "37"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 142.6464 92.583 -90)
		(property "Reference" "29"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 130.6068 71.8058)
		(property "Reference" "6"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 137.5664 87.503 -90)
		(property "Reference" "61"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 201.3204 68.1736)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 12.2936 0.0508 0)
			(layer "F.SilkS")
		)
		(property "Value" "330 ohm"
			(at 17.2212 0.0762 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(1-15{slash}A1{slash}RX3)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 10.16 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(J6-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "0_ABR_footprints:CONV_R-78E5.0-0.5"
		(layer "F.Cu")
		(at 155.7126 44.4246 90)
		(property "Reference" "PS1"
			(at -2.54 -5.715 90)
			(layer "F.SilkS")
		)
		(property "Value" "R-78E5.0-0.5_Gbottom"
			(at 5.08 5.715 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "v4"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "10.40mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "RECOM"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -2.54 2.25 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(PS1-+VIN)")
			(pinfunction "+VIN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 2.25 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 2.54 2.25 90)
			(size 1.508 1.508)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(J4-Pin_1)")
			(pinfunction "+VOUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.6868 74.3458)
		(property "Reference" "16"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_IDC:IDC-Header_2x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 173.02 90.4 90)
		(descr "Through hole IDC box header, 2x10, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x10 2.54mm double row")
		(property "Reference" "J1"
			(at -5.612 4.0688 0)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1299_Devboard_J3"
			(at 1.27 28.96 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "ABR_device_compact.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3.3006 1.224 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 36 "Net-(J1-START{slash}CS)")
			(pinfunction "START/CS")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J1-CLKSEL-Pad2)")
			(pinfunction "CLKSEL")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(J1-CLK)")
			(pinfunction "CLK")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J1-NC-Pad5)")
			(pinfunction "NC")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J1-GPIO1-Pad6)")
			(pinfunction "GPIO1")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J1-CS)")
			(pinfunction "CS")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(J1-RESETB)")
			(pinfunction "RESETB")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J1-NC-Pad9)")
			(pinfunction "NC")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(J1-GND-Pad10)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J1-DIN)")
			(pinfunction "DIN")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J1-GPIO2-Pad12)")
			(pinfunction "GPIO2")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(J1-DOUT)")
			(pinfunction "DOUT")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J1-NC{slash}START-Pad14)")
			(pinfunction "NC/START")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J1-DRDYB)")
			(pinfunction "DRDYB")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J1-SCL-Pad16)")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J1-EXT_CLK-Pad17)")
			(pinfunction "EXT_CLK")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J1-GND-Pad18)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J1-NC-Pad19)")
			(pinfunction "NC")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J1-SDA-Pad20)")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint ""
		(layer "F.Cu")
		(at 135.0264 97.663 -90)
		(property "Reference" "49"
			(at -1.8288 -4.318 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 133.1468 79.4258)
		(property "Reference" "39"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 138.2268 71.8058)
		(property "Reference" "9"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint ""
		(layer "F.Cu")
		(at 138.2268 79.4258)
		(property "Reference" "33"
			(at -1.8288 -4.318 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ""
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 115.7134 27.94)
		(end 225.7134 102.94)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "+"
		(at 213.619 72.0598 0)
		(layer "F.SilkS")
	)
	(gr_text "0/RX"
		(at 169.545 45.03 0)
		(layer "F.SilkS")
	)
	(gr_text "9"
		(at 169.545 67.89 0)
		(layer "F.SilkS")
	)
	(gr_text "14"
		(at 197.993 73.152 0)
		(layer "F.SilkS")
	)
	(gr_text "15"
		(at 197.993 70.612 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 169.545 42.49 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 169.545 50.11 0)
		(layer "F.SilkS")
	)
	(gr_text "17"
		(at 197.993 65.532 0)
		(layer "F.SilkS")
	)
	(gr_text "8"
		(at 169.545 65.35 0)
		(layer "F.SilkS")
	)
	(gr_text "ADS DRDY"
		(at 159.1564 83.3882 0)
		(layer "F.SilkS")
	)
	(gr_text "11/PICO"
		(at 169.545 72.97 0)
		(layer "F.SilkS")
	)
	(gr_text "13/CLK"
		(at 199.921571 75.692 0)
		(layer "F.SilkS")
	)
	(gr_text "ADS START"
		(at 159.1564 80.8482 0)
		(layer "F.SilkS")
	)
	(gr_text "5"
		(at 169.545 57.73 0)
		(layer "F.SilkS")
	)
	(gr_text "Vin(5V)"
		(at 199.7202 42.672 0)
		(layer "F.SilkS")
	)
	(gr_text "10"
		(at 169.545 70.43 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 197.993 60.452 0)
		(layer "F.SilkS")
	)
	(gr_text "ADS CS"
		(at 159.1564 78.3082 0)
		(layer "F.SilkS")
	)
	(gr_text "3.3V"
		(at 198.374 47.7266 0)
		(layer "F.SilkS")
	)
	(gr_text "12/POCI"
		(at 169.545 75.51 0)
		(layer "F.SilkS")
	)
	(gr_text "18"
		(at 197.993 62.992 0)
		(layer "F.SilkS")
	)
	(gr_text "1/TX"
		(at 169.545 47.57 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 197.993 45.212 0)
		(layer "F.SilkS")
	)
	(gr_text "16"
		(at 197.993 68.072 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 205.5826 79.4512 0)
		(layer "F.SilkS")
	)
	(gr_text "21"
		(at 197.993 55.372 0)
		(layer "F.SilkS")
	)
	(gr_text "6"
		(at 169.545 60.27 0)
		(layer "F.SilkS")
	)
	(gr_text "22"
		(at 197.993 52.832 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 169.545 55.19 0)
		(layer "F.SilkS")
	)
	(gr_text "ADS RESET"
		(at 159.1564 85.9282 0)
		(layer "F.SilkS")
	)
	(gr_text "23"
		(at 197.993 50.292 0)
		(layer "F.SilkS")
	)
	(gr_text "7"
		(at 169.545 62.81 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 204.2668 72.1614 0)
		(layer "F.SilkS")
	)
	(gr_text "20"
		(at 197.993 57.912 0)
		(layer "F.SilkS")
	)
	(gr_text "ABR Device v2.0\n2026-03-24"
		(at 195.2244 36.2966 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 169.545 52.65 0)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
