(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "mems-rt-breakout-filter-v2-gerber/")
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "F.Cu")
		(at 129.757714 77.978 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL6"
			(at 0 -2.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL6-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "/X-")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 129.757714 73.5095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "50k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad8)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL6-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "F.Cu")
		(at 141.732 77.8745 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL2"
			(at 0 -2.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL2-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "/Y+")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 126.746 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 2.54 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL6-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/X-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "F.Cu")
		(at 147.828 77.978 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL4"
			(at 0 -2.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL4-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "/Y-")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 160 65)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "H2"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "1_1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 135.781143 73.5095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "50k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad10)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL8-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "F.Cu")
		(at 135.781143 77.978 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL8"
			(at 0 -2.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL8-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.24)
			(net "/X+")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 147.823715 73.5095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "50k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad6)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL4-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "_my_footprints:AMPHENOL_L77SDB25S1ACH4F"
		(layer "F.Cu")
		(at 137.9 87.2)
		(property "Reference" "J2"
			(at -23.468 -6.466 0)
			(layer "F.SilkS")
		)
		(property "Value" "DE9_Sockets_MountingHoles"
			(at -11.403 -4.576 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "25-pin D-SUB connector, socket (female), Mounting Hole"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Website" "https://www.digikey.com/en/products/detail/amphenol-cs-commercial-products/L77SDB25S1ACH4F/4888628"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "DSUB*Socket*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "14" "2" "15" "3" "16" "4" "17" "5" "18" "6" "19" "7" "20"
					"8" "21" "9" "22" "10" "23" "11" "24" "12" "25" "13" "SH"
				)
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "PCB EDGE"
			(at 22.1 9.8 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 16.62 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Y+GND")
			(pinfunction "1_1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 13.85 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 11.08 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "3_3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 8.31 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Y-GND")
			(pinfunction "4_4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 5.54 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "5_5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 2.77 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "6_6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 0 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/X-GND")
			(pinfunction "7_7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at -2.77 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "8_8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at -5.54 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "9_9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at -8.31 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/X+GND")
			(pinfunction "10_10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at -11.08 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "11_11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at -13.85 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "12_12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at -16.62 -1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "13_13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 15.235 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P14_14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 12.465 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Y+")
			(pinfunction "P15_15")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 9.695 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P16_16")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" thru_hole circle
			(at 6.925 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P17_17")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" thru_hole circle
			(at 4.155 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Y-")
			(pinfunction "P18_18")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "19" thru_hole circle
			(at 1.385 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P19_19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" thru_hole circle
			(at -1.385 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P20_20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "21" thru_hole circle
			(at -4.155 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/X-")
			(pinfunction "P21_21")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "22" thru_hole circle
			(at -6.925 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P22_22")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "23" thru_hole circle
			(at -9.695 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P23_23")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "24" thru_hole circle
			(at -12.465 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/X+")
			(pinfunction "P24_24")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "25" thru_hole circle
			(at -15.235 1.27)
			(size 1.725 1.725)
			(drill 1.15)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "P25_25")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH" thru_hole circle
			(at -23.52 0)
			(size 4.266 4.266)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "PAD_SH")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH" thru_hole circle
			(at 23.52 0)
			(size 4.266 4.266)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "PAD_SH")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/L77SDB25S1ACH4F.step"
			(offset
				(xyz 0 -11.5 7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -180 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 132.842 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 2.54 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL8-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/X+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 138.684 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 2.54 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL2-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/Y+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 141.732 73.406 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "50k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL2-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 144.78 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 2.54 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL4-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "/Y-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 115 65)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 DIN965")
		(property "Reference" "H1"
			(at 0 -3.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_Pad"
			(at 0 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(attr exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "1_1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "_my_footprints:CONN_3220-10-0100-00_CNC"
		(layer "B.Cu")
		(at 140 68.072 180)
		(tags "3220-10-0100-00 ")
		(property "Reference" "J1"
			(at 2.5 4.5 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "3220-10-0100-00"
			(at 2.54 0.635 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "3220-10-0100-00"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_3220-10-0100-00_CNC")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6" "7" "8" "9" "10")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 2.54 0.635 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad1)")
			(pinfunction "1_1")
			(pintype "unspecified+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 1.27 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J1-Pad2)")
			(pinfunction "2_2")
			(pintype "unspecified+no_connect")
		)
		(pad "3" thru_hole circle
			(at 1.27 0 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad3)")
			(pinfunction "3_3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 1.27 1.27 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad4)")
			(pinfunction "4_4")
			(pintype "unspecified")
		)
		(pad "5" thru_hole circle
			(at 2.54 0 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad5)")
			(pinfunction "5_5")
			(pintype "unspecified")
		)
		(pad "6" thru_hole circle
			(at 2.54 1.27 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad6)")
			(pinfunction "6_6")
			(pintype "unspecified")
		)
		(pad "7" thru_hole circle
			(at 3.81 0 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad7)")
			(pinfunction "7_7")
			(pintype "unspecified")
		)
		(pad "8" thru_hole circle
			(at 3.81 1.27 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad8)")
			(pinfunction "8_8")
			(pintype "unspecified")
		)
		(pad "9" thru_hole circle
			(at 5.08 0 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad9)")
			(pinfunction "9_9")
			(pintype "unspecified")
		)
		(pad "10" thru_hole circle
			(at 5.08 1.27 180)
			(size 1.1684 1.1684)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pad10)")
			(pinfunction "10_10")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3220-10-0100-00.STEP"
			(offset
				(xyz 2.5 0.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 129.685143 73.5095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "50k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad9)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL7-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "B.Cu")
		(at 141.732 77.8745 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL3"
			(at 0 2.5 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL3-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "/Y-GND")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 144.78 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 2.54 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL1-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "/Y+GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "B.Cu")
		(at 129.757714 77.978 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL7"
			(at 0 2.5 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL7-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "/X+GND")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 135.781143 73.5095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "50k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad7)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL5-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 147.755429 73.5095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "50k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL1-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 132.842 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 2.54 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL5-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "/X-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "B.Cu")
		(at 147.828 77.978 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL1"
			(at 0 2.5 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL1-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "/Y+GND")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Filter:Filter_Mini-Circuits_FV1206"
		(layer "B.Cu")
		(at 135.781143 77.978 -90)
		(descr "Mini-Circuits Filter SMD 1206 https://ww2.minicircuits.com/case_style/FV1206.pdf")
		(tags "Mini-Circuits Filter SMD 1206")
		(property "Reference" "FL5"
			(at 0 2.5 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LFCN-80"
			(at 0 -2.5 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.minicircuits.com/pdfs/LFCN-80+.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "80MHz 50 Ohm Passive Low Pass Filter, FV1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Filter*Mini?Circuits*FV1206*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "Net-(FL5-IN)")
			(pinfunction "IN_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.625 0 270)
			(size 1.04 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.24)
			(net "/X-GND")
			(pinfunction "OUT_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0 0.9275 270)
			(size 0.61 1.245)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 1.105 270)
			(size 0.61 0.61)
			(drill 0.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Filter.3dshapes/Filter_Mini-Circuits_FV1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 126.746 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 2.54 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL7-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "/X+GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 141.732 73.406 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 1.65 90)
			(layer "B.SilkS")
		)
		(property "Value" "50k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Stiffening resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J1-Pad5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL3-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 138.684 77.978 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 2.54 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 ohm"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Do not place"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "mems-rt-breakout-filter-v3-db25.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(FL3-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net "/Y-GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 110.49 58.928)
		(end 165.49 98.928)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "X+ = 24. X+G = 10\nX- = 21. X-G = 7\nY- = 18. Y-G = 4\nY+ = 15. Y+G = 1\nall others = GND\nmounting hole = GND"
		(at 119.5 67 0)
		(layer "F.SilkS")
	)
	(gr_text "13 . . . . 1\n 25 . . 14"
		(at 121.079 68.976 0)
		(layer "F.SilkS")
	)
	(gr_text "20260923\nto mines from dmqis\nmems driver\nto db25 female\nv3"
		(at 147.25 69.25 0)
		(layer "F.SilkS")
	)
	(gr_text "X+ X- Y- Y+ NC\nG   G  G   G  NC"
		(at 131.318 63.754 0)
		(layer "F.SilkS")
	)
	(gr_text "NC Y+ Y- X- X+\nNC G  G  G  G"
		(at 144.272 63.754 0)
		(layer "B.SilkS")
	)
	(zone
		(net "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 110.49 58.928) (xy 119.888 58.928) (xy 119.876105 76.25) (xy 156.038995 76.239294) (xy 156.035217 63.4788)
				(xy 119.126 63.246) (xy 119.126 58.928) (xy 165.608 58.928) (xy 165.608 99.06) (xy 110.236 99.06)
			)
		)
	)
	(embedded_fonts no)
)
