(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (footprint "Probe_holes:1.3mmProbeHole" (layer "F.Cu")
    (at 83.535 100)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "1.3mmProbeHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 1.3) (layers "F.Cu" "B.Mask")
      (solder_mask_margin 10) (clearance 1.1))
  )
  (footprint "Probe_holes:1.3mmProbeHole" (layer "F.Cu")
    (at 167.035 100)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**1" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "1.3mmProbeHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 1.3) (layers "F.Cu" "B.Mask")
      (solder_mask_margin 10) (clearance 1.1))
  )
  (footprint "Probe_holes:1.3mmProbeHole" (layer "F.Cu")
    (at 250.535 100)
    (descr "Mounting Hole 2.1mm, no annular")
    (tags "mounting hole 2.1mm no annular")
    (attr exclude_from_pos_files exclude_from_bom)
    (fp_text reference "REF**2" (at 0 -3.2) (layer "F.SilkS") hide)
    (fp_text value "1.3mmProbeHole" (at 0 3.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "" np_thru_hole circle (at 0 0) (size 2.1 2.1) (drill 1.3) (layers "F.Cu" "B.Mask")
      (solder_mask_margin 10) (clearance 1.1))
  )
  (gr_line locked (start 21.465 148.535) (end 285.535 148.535)
    (layer "Edge.Cuts"))
  (gr_line locked (start 167.035 51.465) (end 83.535 51.465)
    (layer "Edge.Cuts"))
  (gr_line locked (start 285.535 51.465) (end 167.035 51.465)
    (layer "Edge.Cuts"))
  (gr_line locked (start 83.535 51.465) (end 21.465 51.465)
    (layer "Edge.Cuts"))
  (gr_line locked (start 285.535 148.535) (end 285.535 100)
    (layer "Edge.Cuts"))
  (gr_line locked (start 21.465 51.465) (end 21.465 148.535)
    (layer "Edge.Cuts"))
  (gr_line locked (start 285.535 100) (end 285.535 51.465)
    (layer "Edge.Cuts"))
  (gr_text "Simulated RHCP Gain Pattern\nPeak Gain: 5.8 dB" (at 55.88 57.785) (layer "F.SilkS"))
  (gr_text "PENN STATE UNIVERSITY" (at 139.065 142.875) (layer "F.SilkS"))
  (dimension (type orthogonal) (layer "F.SilkS")
    (pts (xy 49.6 83.82) (xy 54.45 78.97))
    (height -14.675)
    (orientation 1)
    (gr_text "4.85 mm" (at 32.775 81.395 90) (layer "F.SilkS"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "F.SilkS")
    (pts (xy 67.575 121.035) (xy 151.075 121.035))
    (height 7.235)
    (orientation 0)
    (gr_text "83.5000 mm" (at 109.325 126.12) (layer "F.SilkS"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "F.SilkS")
    (pts (xy 91.035 78.965) (xy 48.965 83.815))
    (height -7.845)
    (orientation 0)
    (gr_text "42.07 mm" (at 70 68.97) (layer "F.SilkS"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 2))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "F.SilkS")
    (pts (xy 83.535 100) (xy 91.035 97.575))
    (height -7.29)
    (orientation 0)
    (gr_text "7.5 mm" (at 86.995 91.44) (layer "F.SilkS"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 4) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 2) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type orthogonal) (layer "F.SilkS")
    (pts (xy 91.035 78.965) (xy 86.185 121.035))
    (height -50.395)
    (orientation 1)
    (gr_text "42.07 mm" (at 38.49 100 90) (layer "F.SilkS"))
    (format (prefix "") (suffix "") (units 3) (units_format 1) (precision 2) suppress_zeroes)
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5) (island_removal_mode 1) (island_area_min 10))
    (polygon
      (pts
        (xy 21.465 51.465)
        (xy 285.535 51.465)
        (xy 285.535 100)
        (xy 285.535 148.535)
        (xy 167.035 148.535)
        (xy 83.535 148.535)
        (xy 21.465 148.535)
      )
    )
  )
)
