(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin yes)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.545 84.23 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P2"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P2-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P2-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.545 91.92 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P3"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P3-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P3-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.825 85.23 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.775 107.11 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P5"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P5-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P5-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 72.44)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J12"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND0"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 176.83 124.75)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.285 84.23)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0.06 2.78 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P2-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.305 122.3)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P7-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 118.51)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J15"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND3"
			(at 0.21625 -5.145 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.725 100.51 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P4-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.545 76.73 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P1-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P1-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.205 107.11)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J7"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S5"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J7-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 150.215 114.61)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J8-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.305 99.42)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P4-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 150.215 91.92)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J5-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.315 76.73)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J3"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S1"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J3-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.445 64.21)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R16"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J10-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J11-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.825 75.73 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.835 70.1025 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C0"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P0-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.725 106.11 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.305 114.61)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P6-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 87.94)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J13"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND1"
			(at -0.1 5.62 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.825 114.61 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P6"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P6-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P6-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.545 122.3 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P7"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P7-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P7-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 95.44)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J19"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND7"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 86.75 65.63)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.635 69.98 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P0-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.725 90.81 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 89.835 83.24)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J10"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "Laser_Signal"
			(at -0.76 5.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J10-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.615 75.73 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.315 68.93)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J2"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S0"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J2-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.205 91.92)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J5"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S3"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J5-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.725 85.23 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.545 69.04 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P0"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P0-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P0-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.735 106.11 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P5-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.395 76.73)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 102.94)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J14"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND2"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.735 115.71 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P6-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 150.215 107.11)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J7-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.395 84.23)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J4-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.735 121.31 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P7-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "bpw34s:BPW34SZ"
		(layer "F.Cu")
		(at 127.545 99.42 180)
		(descr "BPW34S-Z-2")
		(tags "LED")
		(property "Reference" "P4"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "BPW34S-Z"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.ph/fil/ProductDetail/ams-OSRAM/BPW34S-Z?qs=j%252BKdi43vpAhJ804RMgwweA%3D%3D&srsltid=AfmBOoqIfwy-AVM8EIZV_i-abD30HV-78fwzTMtJ8RFgWJ2BJkIzmVcp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Photodiode PIN Chip 850nm 0.62A/W Sensitivity 2-Pin DIL SMT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "ams OSRAM"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "BPW34S-Z"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/bpw34s-z/osram-opto-semiconductors"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.05 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P4-A)")
			(pinfunction "A_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 3.05 0 180)
			(size 1.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(P4-K)")
			(pinfunction "K_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BPW34S-Z.stp"
			(offset
				(xyz 0 0 1.20000003)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
		(model "${KIPRJMOD}/3d/BPW 34 S-Z.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 171.085 64.42)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J17"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND5"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 150.215 122.3)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P7-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J9-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.735 100.51 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P4-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.085 64.21)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J11"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "Laser Input"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J11-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.205 114.61)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J8"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S6"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J8-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 89.965 107.69)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J16"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND4"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.285 76.73)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.205 122.3)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J9"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S7"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J9-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.305 107.11)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P5-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 125.695)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J21"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND1"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 112.825 90.81 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.305 91.92)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P3-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 110.69)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J20"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND8"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.725 121.31 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P7-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.315 84.23)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J4"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S2"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J4-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 165.87 79.94)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J18"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND6"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 90.07 89.94)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J22"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND4"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J12-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.725 115.71 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0 -1.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J12-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 96.085 101.92 180)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J1"
			(at 0 -2.148 180)
			(layer "F.SilkS")
		)
		(property "Value" "V_bias"
			(at 0 2.25 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0 180)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J1-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 176.98 65.54)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 150.215 99.42)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P4-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J6-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 149.365 68.97)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(P0-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net "Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 86.55 124.75)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "REF**"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "mounting_hardware/mounting_hole"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 103.235 69.1)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R0"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(P0-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_2.5x2.5mm"
		(layer "F.Cu")
		(at 159.495 99.42)
		(descr "SMD rectangular pad as test Point, square 2.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "J6"
			(at 0 -2.148 0)
			(layer "F.SilkS")
		)
		(property "Value" "S4"
			(at 0 2.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "bpw34s.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1")
			)
		)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.15 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 2.5 2.5)
			(layers "F.Cu" "F.Mask")
			(net "Net-(J6-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 81.75 59.59)
		(end 181.75 129.59)
		(fill no)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
