(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/BATT+")
	(net 3 "/VCC")
	(net 4 "Net-(U1-BST)")
	(net 5 "Net-(U1-SW)")
	(net 6 "Net-(U1-PMID)")
	(net 7 "/8_IN")
	(net 8 "/6_SYS")
	(net 9 "/D-")
	(net 10 "/D+")
	(net 11 "Net-(J3-Pin_2)")
	(net 12 "/SDA")
	(net 13 "/SCL")
	(net 14 "Net-(U1-CSP)")
	(net 15 "Net-(U1-SCL)")
	(net 16 "Net-(U1-SDA)")
	(net 17 "Net-(U1-VRNTC)")
	(net 18 "/INT")
	(net 19 "unconnected-(U1-DM-Pad13)")
	(net 20 "unconnected-(U1-DP-Pad12)")
	(net 21 "Net-(U1-NTC)")
	(net 22 "unconnected-(J2-SBU2-PadB8)")
	(net 23 "unconnected-(J2-SBU1-PadA8)")
	(net 24 "Net-(J2-CC2)")
	(net 25 "Net-(J2-CC1)")
	(net 26 "Net-(J3-Pin_1)")
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 140.208 88.0364)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at -0.4572 -1.6256 0)
			(layer "F.SilkS")
		)
		(property "Value" "VRNTC"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 17 "Net-(U1-VRNTC)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 152.0444 93.1164 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.43 315)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 1.43 315)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 315)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.862501 0 315)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/BATT+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.862501 0 315)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 152.5524 97.028 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 2.4892 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.68 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 8 "/6_SYS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 153.2128 76.962)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 4.9784 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D-"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${NET_NAME(1)}"
			(at 2.6416 0.3556 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 9 "/D-")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 148.1328 86.614 -45)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.43 315)
			(layer "F.SilkS")
		)
		(property "Value" "10m Shunt"
			(at 0 1.43 315)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 315)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 315)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 315)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(J3-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 141.351 84.963 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 2.2606 -0.0762 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-NTC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 141.478 82.804)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at -1.8288 -0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "VCC"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${NET_NAME(1)}"
			(at -2.1844 1.1176 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "/VCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MP2696AGQ:QFN21_3MMx3MM_MNP"
		(layer "F.Cu")
		(at 146.499999 89.95)
		(tags "MP2696AGQ-0000-P ")
		(property "Reference" "U1"
			(at 1.531201 2.6076 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MP2696AGQ-0000-P"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN21_3MMx3MM_MNP")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.600001)
			(size 1.4986 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.05 -0.199999)
			(size 1.4986 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(U1-SW)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -1.05 0.2)
			(size 1.4986 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1-PMID)")
			(pinfunction "PMID")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -1.05 0.599999)
			(size 1.4986 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(U1-PMID)")
			(pinfunction "SMID")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -1.000001 1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/6_SYS")
			(pinfunction "SYS")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at -0.599999 1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/6_SYS")
			(pinfunction "SYS")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at -0.2 1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/8_IN")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 0.2 1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/8_IN")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 0.599999 1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(U1-CSP)")
			(pinfunction "CSP")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 1.000001 1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/BATT+")
			(pinfunction "BATT")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 1.45 0.800001)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at 1.45 0.399999)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(U1-DP-Pad12)")
			(pinfunction "DP")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" smd rect
			(at 1.45 0)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(U1-DM-Pad13)")
			(pinfunction "DM")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" smd rect
			(at 1.45 -0.399999)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/INT")
			(pinfunction "INT")
			(pintype "output")
		)
		(pad "15" smd rect
			(at 1.45 -0.800001)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(U1-SCL)")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 1.000001 -1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(U1-SDA)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 0.599999 -1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(J3-Pin_1)")
			(pinfunction "IB")
			(pintype "input")
		)
		(pad "18" smd rect
			(at 0.2 -1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(U1-NTC)")
			(pinfunction "NTC")
			(pintype "input")
		)
		(pad "19" smd rect
			(at -0.2 -1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/VCC")
			(pinfunction "VCC")
			(pintype "input")
		)
		(pad "20" smd rect
			(at -0.599999 -1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(U1-VRNTC)")
			(pinfunction "VRNTC")
			(pintype "output")
		)
		(pad "21" smd rect
			(at -1.000001 -1.45 90)
			(size 0.7112 0.2032)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(U1-BST)")
			(pinfunction "BST")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 155.0924 91.8464)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -2.6416 0)
			(layer "F.SilkS")
		)
		(property "Value" "BATT+"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${NET_NAME(1)}"
			(at 0.0508 -1.3208 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "/BATT+")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 145.669 84.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 2.544 0.431 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 158.9316 92.66)
		(descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x02 1.00mm single row")
		(property "Reference" "J4"
			(at -1.5532 2.1328 0)
			(layer "F.SilkS")
		)
		(property "Value" "breakout to batt"
			(at 0 2.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/BATT+")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 139.573 96.266)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.648 0)
			(layer "F.SilkS")
		)
		(property "Value" "INT"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${NET_NAME(1)}"
			(at 0 2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 18 "/INT")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 158.9316 95.99)
		(descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x02 1.00mm single row")
		(property "Reference" "N1"
			(at -1.5532 2.2572 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 2.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/6_SYS")
			(pinfunction "5V")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 0 1)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 158.9316 89.33)
		(descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x02 1.00mm single row")
		(property "Reference" "J1"
			(at -1.5532 1.9576 0)
			(layer "F.SilkS")
		)
		(property "Value" "I2C Breakout"
			(at 0 2.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/SDA")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/SCL")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 151.675001 90.5764)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -2.221401 0.1016 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(U1-SCL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 151.675001 89)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.170601 0.0016 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U1-SDA)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x02_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 158.9316 86)
		(descr "Through hole straight pin header, 1x02, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x02 1.00mm single row")
		(property "Reference" "J3"
			(at -1.5532 2.138 0)
			(layer "F.SilkS")
		)
		(property "Value" "breakout to header pin"
			(at 0 2.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x02_P1.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 139.827 91.059 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0.071842 1.185394 315)
			(layer "F.SilkS")
		)
		(property "Value" "0.47uF"
			(at 0 1.43 315)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 315)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 315)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.862501 0 315)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U1-BST)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.862501 0 315)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-SW)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 155.194 95.758 -90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 3.3528 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10m"
			(at 0 1.83 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 2 "/BATT+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 270)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 14 "Net-(U1-CSP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 153.2128 79.756)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 4.9784 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "GND"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${NET_NAME(1)}"
			(at 2.6416 0.3556 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 153.2128 82.296)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 4.9784 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "VBUS"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 7 "/8_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 142.5956 91.186 135)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -0.466973 -1.544604 135)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.679999 135)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 135)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "Net-(U1-PMID)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 135)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 142.8496 87.9602)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at -0.6096 -1.6002 0)
			(layer "F.SilkS")
		)
		(property "Value" "BST"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(U1-BST)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 152.5016 86.0044 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 11 "Net-(J3-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 144.018 85.217 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.0066 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(U1-VRNTC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-NTC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.5mm"
		(layer "F.Cu")
		(at 153.2128 74.168)
		(descr "SMD pad as test Point, diameter 1.5mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 4.9784 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D+"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${NET_NAME(1)}"
			(at 2.6416 0.3556 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -1.65 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 10 "/D+")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "IHLM2525CZER3R3M01:IND_IHLM-2525CZ_VIS"
		(layer "F.Cu")
		(at 145.5 97 180)
		(tags "IHLM2525CZER3R3M01 ")
		(property "Reference" "L1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "3.3uH"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.6543 0 270)
			(size 3.175 2.2352)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(U1-CSP)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.6543 0 270)
			(size 3.175 2.2352)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(U1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 146.9859 98.6383) (xy 144.0141 98.6383) (xy 144.0141 95.3617) (xy 146.9859 95.3617)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 149.0687 95.3617) (xy 141.9313 95.3617) (xy 141.9313 93.6853) (xy 149.0687 93.6853)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 149.0687 100.3147) (xy 141.9313 100.3147) (xy 141.9313 98.6383) (xy 149.0687 98.6383)
				)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Downloaded Symbols and Footprints/IHLM2525CZER3R3M01/IHLM2525.step"
			(offset
				(xyz -5.6 -2.5 -2.75)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "USB4105:GCT_USB4105-GF-A"
		(layer "F.Cu")
		(at 146.304 75.819 180)
		(property "Reference" "J2"
			(at 0 0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "USB4105-GF-A"
			(at 5.16 -7.135 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "PCB EDGE"
			(at 5.4 2.5 180)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -3.68 180)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -3.68 180)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1_B12" smd rect
			(at -3.2 -4.755 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "A4_B9" smd rect
			(at -2.4 -4.755 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 7 "/8_IN")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "A5" smd rect
			(at -1.25 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 25 "Net-(J2-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 10 "/D+")
			(pinfunction "DP1")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at 0.25 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 9 "/D-")
			(pinfunction "DN1")
			(pintype "bidirectional")
		)
		(pad "A8" smd rect
			(at 1.25 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 23 "unconnected-(J2-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional")
		)
		(pad "B1_A12" smd rect
			(at 3.2 -4.755 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
		)
		(pad "B4_A9" smd rect
			(at 2.4 -4.755 180)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net 7 "/8_IN")
			(pinfunction "VBUS__1")
			(pintype "power_in")
		)
		(pad "B5" smd rect
			(at 1.75 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 24 "Net-(J2-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 10 "/D+")
			(pinfunction "DP2")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at -0.75 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 9 "/D-")
			(pinfunction "DN2")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at -1.75 -4.755 180)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net 22 "unconnected-(J2-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional")
		)
		(pad "SH1" thru_hole oval
			(at -4.32 -4.18 180)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHELL_GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH2" thru_hole oval
			(at 4.32 -4.18 180)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHELL_GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH3" thru_hole oval
			(at -4.32 0 180)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHELL_GND__2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "SH4" thru_hole oval
			(at 4.32 0 180)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHELL_GND__3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Downloaded Symbols and Footprints/USB4105_GF_A/USB4105-GF-A.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 149 83.5 -45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 1.131371 -1.414214 135)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 135)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.862501 0 315)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/8_IN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.862501 0 315)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 144.272 80.645 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(J2-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 148.336 80.645 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NVG Monocular.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(J2-CC1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 144.8 94.9 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_line
		(start 140.7541 72.8519)
		(end 158.4993 72.8519)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.3822 75.7348)
		(end 161.3822 98.6028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.4993 101.4857)
		(end 140.7541 101.4857)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 161.3822 98.6028)
		(mid 160.537818 100.641318)
		(end 158.4993 101.4857)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 137.8712 75.7348)
		(mid 138.715582 73.696282)
		(end 140.7541 72.8519)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 140.7541 101.4857)
		(mid 138.715582 100.641318)
		(end 137.8712 98.6028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.8712 98.6028)
		(end 137.8712 75.7348)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.4993 72.8519)
		(mid 160.537818 73.696282)
		(end 161.3822 75.7348)
		(layer "Edge.Cuts")
	)
	(gr_text "-\n"
		(at 160.3248 94.234 90)
		(layer "F.SilkS")
	)
	(gr_text "CURR"
		(at 160.5788 87.63 90)
		(layer "F.SilkS")
	)
	(gr_text "+\n"
		(at 160.3756 96.3676 90)
		(layer "F.SilkS")
	)
	(gr_text "Vin\n"
		(at 155.9 82.3 0)
		(layer "F.SilkS")
	)
	(gr_text "BATT\n"
		(at 161.29 94.0308 90)
		(layer "F.SilkS")
	)
	(gr_text "-\n"
		(at 160.3756 97.536 90)
		(layer "F.SilkS")
	)
	(gr_text "SCL\n"
		(at 160.5788 91.6432 90)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 160.5788 89.8144 90)
		(layer "F.SilkS")
	)
	(gr_text "5VOUT\n\n"
		(at 162.2552 97.7392 90)
		(layer "F.SilkS")
	)
	(gr_text "+\n"
		(at 160.3248 93.0656 90)
		(layer "F.SilkS")
	)
	(gr_text "MP2696A Breakout V1\nMade with <3 by\nSiwen Long"
		(at 157 77 90)
		(layer "B.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 137.8712 87.1688) (xy 161.3822 87.1688)
		)
		(height 20.5312)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "925.6299"
			(at 149.6267 106.6 0)
			(layer "F.SilkS")
		)
	)
	(dimension
		(type orthogonal)
		(layer "F.SilkS")
		(pts
			(xy 158.4993 101.4857) (xy 158.4993 72.8519)
		)
		(height 9.2007)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "1127.315"
			(at 166.6 87.1688 90)
			(layer "F.SilkS")
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.8 72.6) (xy 161.6 72.6) (xy 161.7 102.1) (xy 137.5 102.1) (xy 137.8 72.5)
			)
		)
	)
	(embedded_fonts no)
)
