(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 0.8836)
		(legacy_teardrops no)
	)
	(paper "B")
	(title_block
		(title "STM DRIVER PCB")
		(date "2026-02-04")
		(company "Thomas Gokie")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" power)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0711)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 0.711)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0711)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 111.3 228.1)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+48V")
	(net 2 "GND")
	(net 3 "12VOUT")
	(net 4 "5VOUT")
	(net 5 "VCC")
	(net 6 "+3.3V")
	(net 7 "DIR")
	(net 8 "SCLK")
	(net 9 "MISO")
	(net 10 "MOSI")
	(net 11 "DIAG1")
	(net 12 "STEP")
	(net 13 "SS")
	(net 14 "DIAG0")
	(net 15 "Net-(Q1-G)")
	(net 16 "Net-(Q2-G)")
	(net 17 "Net-(Q3-G)")
	(net 18 "Net-(Q3-S)")
	(net 19 "Net-(Q4-G)")
	(net 20 "Net-(Q5-G)")
	(net 21 "Net-(Q6-G)")
	(net 22 "Net-(Q7-G)")
	(net 23 "Net-(Q7-S)")
	(net 24 "Net-(Q8-G)")
	(net 25 "Net-(U2-VCP)")
	(net 26 "Net-(U2-CB2)")
	(net 27 "Net-(U2-CB1)")
	(net 28 "Net-(U2-CPI)")
	(net 29 "Net-(U2-CPO)")
	(net 30 "Net-(U2-CA2)")
	(net 31 "Net-(U2-CA1)")
	(net 32 "Net-(U2-HB1)")
	(net 33 "Net-(U2-HB2)")
	(net 34 "Net-(U2-LB1)")
	(net 35 "Net-(U2-LB2)")
	(net 36 "Net-(U2-SRBH)")
	(net 37 "Net-(U2-SRBL)")
	(net 38 "Net-(U2-HA1)")
	(net 39 "Net-(U2-HA2)")
	(net 40 "Net-(U2-LA1)")
	(net 41 "Net-(U2-LA2)")
	(net 42 "Net-(U2-SRAH)")
	(net 43 "Net-(U2-SRAL)")
	(net 44 "unconnected-(U2-DCIN_CFG5-Pad24)")
	(net 45 "unconnected-(U2-DCEN_CFG4-Pad23)")
	(net 46 "unconnected-(U2-DCO_CFG6-Pad25)")
	(net 47 "unconnected-(U1-NC-Pad4)")
	(net 48 "/STM_B2")
	(net 49 "/STM_A1")
	(net 50 "/STM_A2")
	(net 51 "/STM_B1")
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 142.7 209.266667)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -0.1 -1.566667 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 38 "Net-(U2-HA1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 20 "Net-(Q5-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 161.9 201 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 4.1 -0.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OPT OUT CAP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/STM_A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_MaiXu_MX126-5.0-04P_1x04_P5.00mm"
		(layer "F.Cu")
		(at 195.6 207.65 90)
		(descr "terminal block MaiXu MX126-5.0-04P, 4 pins, pitch 5mm, size 20.5x7.8mm, drill diameter 1.3mm, pad diameter 2.8mm, https://www.lcsc.com/datasheet/lcsc_datasheet_2309150913_MAX-MX126-5-0-03P-GN01-Cu-S-A_C5188435.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_MaiXu")
		(tags "THT terminal block MaiXu MX126-5.0-04P pitch 5mm size 20.5x7.8mm drill 1.3mm pad 2.8mm")
		(property "Reference" "J2"
			(at 18.95 2.3325 180)
			(layer "F.SilkS")
		)
		(property "Value" "STM_OUT_LEFT"
			(at 7.25 4.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.25 2.65 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.089286)
			(net 50 "/STM_A2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "/STM_A1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10 0 90)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/STM_B2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15 0 90)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/STM_B1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_MaiXu_MX126-5.0-04P_1x04_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 182.1 208.9)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q8"
			(at 5.4 4.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(Q8-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/STM_A2")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(Q7-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric"
		(layer "F.Cu")
		(at 185.3 180.7)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 2.6 -2.8 0)
			(layer "F.SilkS")
		)
		(property "Value" ".075"
			(at 0 2.63 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CRA2512"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9625 0)
			(size 1.225 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.204082)
			(net 18 "Net-(Q3-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.9625 0)
			(size 1.225 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.204082)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 160.388889 190)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q4"
			(at 5.411111 -1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(Q4-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/STM_B2")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(Q3-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 193.9 186.5 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 1.3 2.7 180)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OPT OUT CAP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/STM_B1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 194.3 222.1)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "MH2"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 142.4875 199.1 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.7125 -0.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 16 "Net-(Q2-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 33 "Net-(U2-HB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 142.4875 197.1 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.5875 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 19 "Net-(Q4-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 35 "Net-(U2-LB2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 126.39 191.74 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 1.06 -2.01 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 4 "5VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 5 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 142.4875 195.1)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 34 "Net-(U2-LB1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 17 "Net-(Q3-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 174.9 222)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "47"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 43 "Net-(U2-SRAL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 138.7 206.7)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at -3.2 0.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U2-CA1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/STM_A1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 119.2 205.9 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at -1.9 1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 172.6 181.9)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 3 0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "47"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 36 "Net-(U2-SRBH)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 18 "Net-(Q3-S)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm"
		(layer "F.Cu")
		(at 125.5 202.9 -90)
		(descr "TQFP, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2100_datasheet_Rev1.08.pdf (page 45)), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TQFP QFP")
		(property "Reference" "U2"
			(at 0.2 -6 90)
			(layer "F.SilkS")
		)
		(property "Value" "TMC2160"
			(at 0 5.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2160A-datasheet_Rev1.06.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Standalone driver for two-phase bipolar stepper motor, 8-60V, external FETs, TQFP48"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*1EP?7x7mm*P0.5mm*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.875 -1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -1.875 -0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -1.875 0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -1.875 1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -0.625 -1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -0.625 -0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -0.625 0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -0.625 1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 0.625 -1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 0.625 -0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 0.625 0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 0.625 1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 1.875 -1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 1.875 -0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 1.875 0.625 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 1.875 1.875 270)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "1" smd roundrect
			(at -4.1625 -2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U2-HB1)")
			(pinfunction "HB1")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -4.1625 -2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-CB1)")
			(pinfunction "CB1")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -4.1625 -1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "12VOUT")
			(pinfunction "12VOUT")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -4.1625 -1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "12VOUT")
			(pinfunction "VSA")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -4.1625 -0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "5VOUT")
			(pinfunction "5VOUT")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at -4.1625 -0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GNDA")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -4.1625 0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "Net-(U2-SRAL)")
			(pinfunction "SRAL")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -4.1625 0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Net-(U2-SRAH)")
			(pinfunction "SRAH")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -4.1625 1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U2-SRBH)")
			(pinfunction "SRBH")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -4.1625 1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Net-(U2-SRBL)")
			(pinfunction "SRBL")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -4.1625 2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "TST_MODE")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -4.1625 2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -2.75 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "SS")
			(pinfunction "~{CS}_CFG3")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at -2.25 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "SCLK")
			(pinfunction "SCK_CFG2")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at -1.75 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "MOSI")
			(pinfunction "SDI_CFG1")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at -1.25 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "MISO")
			(pinfunction "SDO_CFG0")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at -0.75 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "STEP")
			(pinfunction "STEP")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at -0.25 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "DIR")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at 0.25 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GNDD")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at 0.75 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3.3V")
			(pinfunction "VCC_IO")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at 1.25 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3.3V")
			(pinfunction "VCC_IO")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 1.75 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+3.3V")
			(pinfunction "SPI_MODE")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 2.25 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(U2-DCEN_CFG4-Pad23)")
			(pinfunction "DCEN_CFG4")
			(pintype "input+no_connect")
		)
		(pad "24" smd roundrect
			(at 2.75 4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(U2-DCIN_CFG5-Pad24)")
			(pinfunction "DCIN_CFG5")
			(pintype "input+no_connect")
		)
		(pad "25" smd roundrect
			(at 4.1625 2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U2-DCO_CFG6-Pad25)")
			(pinfunction "DCO_CFG6")
			(pintype "output+no_connect")
		)
		(pad "26" smd roundrect
			(at 4.1625 2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "DIAG0")
			(pinfunction "DIAG0")
			(pintype "output")
		)
		(pad "27" smd roundrect
			(at 4.1625 1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "DIAG1")
			(pinfunction "DIAG1")
			(pintype "output")
		)
		(pad "28" smd roundrect
			(at 4.1625 1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "~{DRV_EN}")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at 4.1625 0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "30" smd roundrect
			(at 4.1625 0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GNDD")
			(pintype "passive")
		)
		(pad "31" smd roundrect
			(at 4.1625 -0.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U2-CPO)")
			(pinfunction "CPO")
			(pintype "passive")
		)
		(pad "32" smd roundrect
			(at 4.1625 -0.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U2-CPI)")
			(pinfunction "CPI")
			(pintype "passive")
		)
		(pad "33" smd roundrect
			(at 4.1625 -1.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+48V")
			(pinfunction "VS")
			(pintype "power_in")
		)
		(pad "34" smd roundrect
			(at 4.1625 -1.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U2-VCP)")
			(pinfunction "VCP")
			(pintype "passive")
		)
		(pad "35" smd roundrect
			(at 4.1625 -2.25 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U2-CA2)")
			(pinfunction "CA2")
			(pintype "passive")
		)
		(pad "36" smd roundrect
			(at 4.1625 -2.75 270)
			(size 1.475 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "Net-(U2-HA2)")
			(pinfunction "HA2")
			(pintype "output")
		)
		(pad "37" smd roundrect
			(at 2.75 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/STM_A2")
			(pinfunction "BMA2")
			(pintype "passive")
		)
		(pad "38" smd roundrect
			(at 2.25 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U2-LA2)")
			(pinfunction "LA2")
			(pintype "output")
		)
		(pad "39" smd roundrect
			(at 1.75 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(U2-LA1)")
			(pinfunction "LA1")
			(pintype "output")
		)
		(pad "40" smd roundrect
			(at 1.25 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/STM_A1")
			(pinfunction "BMA1")
			(pintype "passive")
		)
		(pad "41" smd roundrect
			(at 0.75 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "Net-(U2-HA1)")
			(pinfunction "HA1")
			(pintype "output")
		)
		(pad "42" smd roundrect
			(at 0.25 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U2-CA1)")
			(pinfunction "CA1")
			(pintype "output")
		)
		(pad "43" smd roundrect
			(at -0.25 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U2-CB2)")
			(pinfunction "CB2")
			(pintype "passive")
		)
		(pad "44" smd roundrect
			(at -0.75 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U2-HB2)")
			(pinfunction "HB2")
			(pintype "output")
		)
		(pad "45" smd roundrect
			(at -1.25 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/STM_B2")
			(pinfunction "BMB2")
			(pintype "passive")
		)
		(pad "46" smd roundrect
			(at -1.75 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Net-(U2-LB2)")
			(pinfunction "LB2")
			(pintype "output")
		)
		(pad "47" smd roundrect
			(at -2.25 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Net-(U2-LB1)")
			(pinfunction "LB1")
			(pintype "output")
		)
		(pad "48" smd roundrect
			(at -2.75 -4.1625 270)
			(size 0.3 1.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/STM_B1")
			(pinfunction "BMB1")
			(pintype "passive")
		)
		(pad "49" smd rect
			(at 0 0 270)
			(size 5 5)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-48-1EP_7x7mm_P0.5mm_EP5x5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock:TerminalBlock_MaiXu_MX126-5.0-02P_1x02_P5.00mm"
		(layer "F.Cu")
		(at 163.8 177.3 180)
		(descr "terminal block MaiXu MX126-5.0-02P, 2 pins, pitch 5mm, size 10.5x7.8mm, drill diameter 1.3mm, pad diameter 2.8mm, https://www.lcsc.com/datasheet/lcsc_datasheet_2309150913_MAX-MX126-5-0-03P-GN01-Cu-S-A_C5188435.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_MaiXu")
		(tags "THT terminal block MaiXu MX126-5.0-02P pitch 5mm size 10.5x7.8mm drill 1.3mm pad 2.8mm")
		(property "Reference" "J1"
			(at 5.65 -5.1675 0)
			(layer "F.SilkS")
		)
		(property "Value" "POWER_IN"
			(at 2.25 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.25 2.65 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.089286)
			(net 1 "+48V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2.8 2.8)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_MaiXu_MX126-5.0-02P_1x02_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm"
		(layer "F.Cu")
		(at 140 220.7 180)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, diameter=12.5mm, height=20mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm diameter 12.5mm height 20mm Electrolytic Capacitor")
		(property "Reference" "C14"
			(at 10.4 -3 0)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 2.5 7.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 1 "+48V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 117.3 178.6)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "MH4"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 194.3 178.6)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "MH1"
			(at 4.4 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 132.8 197.8)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-CB1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/STM_B1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 149.5 190)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q2"
			(at 5.4 -0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(Q2-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+48V")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/STM_B2")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 152.3 199 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OPT OUT CAP"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/STM_B2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 152.25 181.3 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 1.45 -1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "470n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+48V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric"
		(layer "F.Cu")
		(at 183.9 219.1)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0.3 -2.9 0)
			(layer "F.SilkS")
		)
		(property "Value" ".075"
			(at 0 2.63 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CRA2512"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9625 0)
			(size 1.225 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.204082)
			(net 23 "Net-(Q7-S)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.9625 0)
			(size 1.225 3.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.204082)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 138.1 211.7 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 21 "Net-(Q6-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 39 "Net-(U2-HA2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 142.4 205.3)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at -3.1 -1 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U2-CA2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/STM_A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad_Via"
		(layer "F.Cu")
		(at 117.3 222.1)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "MH3"
			(at 0 -4.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at -1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 -2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 0 2.4)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 -1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 1.697056 1.697056)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(pad "1" thru_hole circle
			(at 2.4 0)
			(size 0.8 0.8)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 123.6 190.74)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 3.4 -1.58 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "5VOUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 175 219.7)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "47"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 42 "Net-(U2-SRAH)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 23 "Net-(Q7-S)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 172.7 179.7)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 2.1 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "47"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 37 "Net-(U2-SRBL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 171.211111 208.9)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q6"
			(at 5.488889 -0.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(Q6-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+48V")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/STM_A2")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 113.4 193)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONTROL_IO"
			(at 0 25.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "SCLK")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "MOSI")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "MISO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "SS")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "DIR")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "STEP")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "DIAG0")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "DIAG1")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 138.2 209.3)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -3.1 0.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 40 "Net-(U2-LA1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 22 "Net-(Q7-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 127.5 210.2 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 2.5 -0.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n, 100V"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U2-VCP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+48V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 182.166667 190)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q3"
			(at 5.433333 -3.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(Q3-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "/STM_B1")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(Q3-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm"
		(layer "F.Cu")
		(at 137.9 180.3 180)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, diameter=12.5mm, height=20mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm diameter 12.5mm height 20mm Electrolytic Capacitor")
		(property "Reference" "C6"
			(at 9.8 3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "470uF"
			(at 2.5 7.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 1 "+48V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 142.7 211.3 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -0.9 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 24 "Net-(Q8-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 41 "Net-(U2-LA2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 137.3 195.6)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "15"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 32 "Net-(U2-HB1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 15 "Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 171.277778 190)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q1"
			(at 5.422222 -2.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+48V")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "/STM_B1")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 160.6 208.9)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q7"
			(at 5.3 -2.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(Q7-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "/STM_A1")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(Q7-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 120.59 191.4 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -1.1 2.19 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "12VOUT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 123.59 192.8 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0.59 -1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "470n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 147.7 219 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "470n"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+48V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 125.4 210.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0.5 1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "22n, 100V"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(U2-CPO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(U2-CPI)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 130.7 211.7 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0.4 1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+48V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:6-HSOP_S-1142D"
		(layer "F.Cu")
		(at 121.2 182.96)
		(descr "12V Voltage Regulator")
		(property "Reference" "U1"
			(at 5.6 2.04 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "S1142D"
			(at 2.3 1.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 2.3 3.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 5.28)
			(size 0.76 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "12VOUT")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(pad "2" smd rect
			(at 1.91 5.28)
			(size 2.03 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at 3.82 5.28)
			(size 0.76 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+48V")
			(pinfunction "ON/OFF")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 3.82 0)
			(size 0.76 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "unconnected-(U1-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd rect
			(at 1.91 0)
			(size 2.03 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at 0 0)
			(size 0.76 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+48V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 142.45 203)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -2.75 -0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U2-CB2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/STM_B2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 195.9 213.9 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 2.8 -1.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "1nF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OPT OUT CAP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/STM_A2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "stmdrivers:AOD444"
		(layer "F.Cu")
		(at 149.711111 208.9)
		(descr "AOD444-1")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q5"
			(at 5.388889 -4.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "AOD444"
			(at 0 0.242 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.aosmd.com/products/mosfets/medium-voltage-mosfets-40v-400v/aod444"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 60 V 4A (Ta), 12A (Tc) 2.1W (Ta), 20W (Tc) Surface Mount TO-252 (DPAK)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Alpha & Omega Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "AOD444"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/aod444/alpha-and-omega-semiconductor?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.242 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(Q5-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 -2.108)
			(size 6.25 6.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "+48V")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.286 4.492)
			(size 1.5 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "/STM_A1")
			(pinfunction "S")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "AOD444.stp"
			(offset
				(xyz 0 0.559999994 1.139999969)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 119.1 184.66 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0.24 2.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "capstonepcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "+48V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 111.3 176.6)
		(mid 112.471573 173.771573)
		(end 115.3 172.6)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 115.3 228.1)
		(mid 112.471573 226.928427)
		(end 111.3 224.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.3 224.1)
		(end 111.3 176.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200.3 176.6)
		(end 200.3 224.1)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 196.3 172.6)
		(mid 199.128427 173.771573)
		(end 200.3 176.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.3 228.1)
		(end 115.3 228.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 115.3 172.6)
		(end 196.3 172.6)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 200.3 224.1)
		(mid 199.128427 226.928427)
		(end 196.3 228.1)
		(layer "Edge.Cuts")
	)
	(gr_text "THOMAS GOKIE"
		(at 177.8 226.7 0)
		(layer "F.SilkS")
	)
	(gr_text "48VDC"
		(at 170.8 176 0)
		(layer "F.SilkS")
	)
	(gr_text "B2"
		(at 187.592857 198.766666 0)
		(layer "F.SilkS")
	)
	(gr_text "REV 1.0"
		(at 177.8 224.6 0)
		(layer "F.SilkS")
	)
	(gr_text "A1"
		(at 187.7 203.6 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 167.2 178.8 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 153.1 178.1775 0)
		(layer "F.SilkS")
	)
	(gr_text "+3.3V\nGND\nSCLK\nMOSI\nMISO\nSS\nDIR\nSTEP\nDIAG0\nDIAG1"
		(at 115.5 216.6 0)
		(layer "F.SilkS")
	)
	(gr_text "2.8A STM DRIVER"
		(at 146.6 226.7 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 148.2 176.2 0)
		(layer "F.SilkS")
	)
	(gr_text "A2"
		(at 187.7 208.433333 0)
		(layer "F.SilkS")
	)
	(gr_text "B1"
		(at 187.592857 193.933333 0)
		(layer "F.SilkS")
	)
	(gr_text "UNL SENIOR DESIGN CAPSTONE\n2026 GROUP 200"
		(at 188.7 192.1 0)
		(layer "B.SilkS")
	)
	(gr_text "LawnBa"
		(at 155.8 214.6 0)
		(layer "B.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.2 165) (xy 208.1 165.1) (xy 208.3 236.3) (xy 103.6 236.6)
			)
		)
	)
	(embedded_fonts no)
)
