(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(U1-1-Pad3)")
	(footprint "Testing:8737-SS_1"
		(layer "F.Cu")
		(at 106.28 58.166 90)
		(descr "8737-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U3"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8737"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.keyelco.com/product-pdf.cfm?p=1571"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test Plugs & Test Jacks Mini binding Post"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "534-8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/8737?qs=%2F%252BPMR94VuMZat15d7csBXA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Keystone Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "High Temperature Reverse Bias.kicad_sch")
		(attr through_hole)
		(fp_text user "M4"
			(at 6.066 1.42 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "" thru_hole rect
			(at 0 0.381 90)
			(size 2.2 1.819)
			(drill 1.2
				(offset 0.2 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole rect
			(at 2.54 0.381 90)
			(size 2.14 1.819)
			(drill 1.2
				(offset -0.17 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -5.08 0.4 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U1-1-Pad3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 5.08 0.4064 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "8737.stp"
			(offset
				(xyz 0 0 5.380000034)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Testing:8737-SS_1"
		(layer "F.Cu")
		(at 68.18 58.166 90)
		(descr "8737-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U4"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8737"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.keyelco.com/product-pdf.cfm?p=1571"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test Plugs & Test Jacks Mini binding Post"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "534-8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/8737?qs=%2F%252BPMR94VuMZat15d7csBXA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Keystone Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "High Temperature Reverse Bias.kicad_sch")
		(attr through_hole)
		(fp_text user "M1"
			(at -5.984 -0.73 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "" thru_hole rect
			(at 0 0.381 90)
			(size 2.2 1.819)
			(drill 1.2
				(offset 0.2 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole rect
			(at 2.54 0.381 90)
			(size 2.14 1.819)
			(drill 1.2
				(offset -0.17 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -5.08 0.4 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U1-1-Pad3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 5.08 0.4064 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "8737.stp"
			(offset
				(xyz 0 0 5.380000034)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 108.15 95.7)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 108.15 43.05)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 67 95.7)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Testing:8737-SS_1"
		(layer "F.Cu")
		(at 86.4362 45.339)
		(descr "8737-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8737"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.keyelco.com/product-pdf.cfm?p=1571"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test Plugs & Test Jacks Mini binding Post"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.9"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "534-8737"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/8737?qs=%2F%252BPMR94VuMZat15d7csBXA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Keystone Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "8737"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "High Temperature Reverse Bias.kicad_sch")
		(attr through_hole)
		(fp_text user "M3"
			(at -6.0862 -0.789 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "" thru_hole rect
			(at 0 0.381)
			(size 2.2 1.819)
			(drill 1.2
				(offset 0.2 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole rect
			(at 2.54 0.381)
			(size 2.14 1.819)
			(drill 1.2
				(offset -0.17 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -5.08 0.4)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U1-1-Pad3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 5.08 0.4064)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "8737.stp"
			(offset
				(xyz 0 0 5.380000034)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 67 43.05)
		(descr "Mounting Hole 2.2mm, M2, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2")
		(property "Reference" "REF**"
			(at 0 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_2.2mm_M2"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Testing:8737-VCC"
		(layer "F.Cu")
		(at 89 91.44 -90)
		(descr "8737-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U22"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8737"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.keyelco.com/product-pdf.cfm?p=1571"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test Plugs & Test Jacks Mini binding Post"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.9"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "534-8737"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/8737?qs=%2F%252BPMR94VuMZat15d7csBXA%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Keystone Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "8737"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "High Temperature Reverse Bias.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U1-1-Pad3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "8737.stp"
			(offset
				(xyz 0 0 5.380000034)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Testing:8737-SS_1"
		(layer "F.Cu")
		(at 106.28 81.166 90)
		(descr "8737-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U2"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8737"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.keyelco.com/product-pdf.cfm?p=1571"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test Plugs & Test Jacks Mini binding Post"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "534-8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/8737?qs=%2F%252BPMR94VuMZat15d7csBXA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Keystone Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "High Temperature Reverse Bias.kicad_sch")
		(attr through_hole)
		(fp_text user "M5"
			(at 5.666 1.52 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "" thru_hole rect
			(at 0 0.381 90)
			(size 2.2 1.819)
			(drill 1.2
				(offset 0.2 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole rect
			(at 2.54 0.381 90)
			(size 2.14 1.819)
			(drill 1.2
				(offset -0.17 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -5.08 0.4 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U1-1-Pad3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 5.08 0.4064 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "8737.stp"
			(offset
				(xyz 0 0 5.380000034)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Testing:8737-Drain"
		(layer "F.Cu")
		(at 86.2 91.44 -90)
		(descr "8737-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U23"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8737"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.keyelco.com/product-pdf.cfm?p=1571"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test Plugs & Test Jacks Mini binding Post"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.9"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "534-8737"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/8737?qs=%2F%252BPMR94VuMZat15d7csBXA%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Keystone Electronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "8737"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "High Temperature Reverse Bias.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "8737.stp"
			(offset
				(xyz 0 0 5.380000034)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Testing:8737-SS_1"
		(layer "F.Cu")
		(at 68.18 81.166 90)
		(descr "8737-1")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U21"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8737"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.keyelco.com/product-pdf.cfm?p=1571"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test Plugs & Test Jacks Mini binding Post"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "4.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "534-8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Keystone-Electronics/8737?qs=%2F%252BPMR94VuMZat15d7csBXA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Keystone Electronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "8737"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "High Temperature Reverse Bias.kicad_sch")
		(attr through_hole)
		(fp_text user "M0"
			(at -6.234 -0.73 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "" thru_hole rect
			(at 0 0.381 90)
			(size 2.2 1.819)
			(drill 1.2
				(offset 0.2 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "1" thru_hole rect
			(at 2.54 0.381 90)
			(size 2.14 1.819)
			(drill 1.2
				(offset -0.17 0.0095)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -5.08 0.4 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(U1-1-Pad3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at 5.08 0.4064 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "8737.stp"
			(offset
				(xyz 0 0 5.380000034)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 60.96 38.1)
		(end 114.16 100.68)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 60 37) (xy 115 37) (xy 115 102) (xy 60 102)
			)
		)
	)
	(embedded_fonts no)
)
