(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "EN")
	(net 3 "IO14")
	(net 4 "IO12")
	(net 5 "IO13")
	(net 6 "IO15")
	(net 7 "IO2")
	(net 8 "IO0")
	(net 9 "+3V3")
	(net 10 "IO16")
	(net 11 "TOUT")
	(net 12 "RST")
	(net 13 "IO5")
	(net 14 "TXD")
	(net 15 "RXD")
	(net 16 "IO4")
	(footprint "RF_Module:ESP-WROOM-02_MODIFIED"
		(layer "F.Cu")
		(at 144.78 95.758)
		(descr "https://www.espressif.com/sites/default/files/documentation/0c-esp-wroom-02_datasheet_en.pdf")
		(tags "ESP WROOM-02 espressif esp8266ex")
		(property "Reference" "U1"
			(at -10.5 5.13 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ESP-WROOM-02D"
			(at -0.18 -7.158 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -8.875 -6)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+3V3")
		)
		(pad "2" smd rect
			(at -8.875 -4.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "EN")
		)
		(pad "3" smd rect
			(at -8.875 -3)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "IO14")
		)
		(pad "4" smd rect
			(at -8.875 -1.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "IO12")
		)
		(pad "5" smd rect
			(at -8.875 0)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "IO13")
		)
		(pad "6" smd rect
			(at -8.875 1.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "IO15")
		)
		(pad "7" smd rect
			(at -8.875 3)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "IO2")
		)
		(pad "8" smd rect
			(at -8.875 4.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "IO0")
		)
		(pad "9" smd rect
			(at -8.875 6)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "10" smd rect
			(at 8.875 6)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "IO4")
		)
		(pad "11" smd rect
			(at 8.875 4.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "RXD")
		)
		(pad "12" smd rect
			(at 8.875 3)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "TXD")
		)
		(pad "13" smd rect
			(at 8.875 1.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "14" smd rect
			(at 8.875 0)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "IO5")
		)
		(pad "15" smd rect
			(at 8.875 -1.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "RST")
		)
		(pad "16" smd rect
			(at 8.875 -3)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "TOUT")
		)
		(pad "17" smd rect
			(at 8.875 -4.5)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "IO16")
		)
		(pad "18" smd rect
			(at 8.875 -6)
			(size 1.75 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(pad "19" smd rect
			(at 1.1 0.61)
			(size 4 4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/ESP-WROOM-02.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 138 128.76)
		(descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x09 2.54mm single row")
		(property "Reference" "J1"
			(at -0.2 3.24 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_1x09_P2.54mm_Vertical"
			(at -4.3 4.24 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -10.16 270)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3V3")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "EN")
		)
		(pad "3" thru_hole circle
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "IO14")
		)
		(pad "4" thru_hole circle
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "IO12")
		)
		(pad "5" thru_hole circle
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "IO13")
		)
		(pad "6" thru_hole circle
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "IO15")
		)
		(pad "7" thru_hole circle
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "IO2")
		)
		(pad "8" thru_hole circle
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "IO0")
		)
		(pad "9" thru_hole circle
			(at 0 -20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x09_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 151.5 128.76)
		(descr "Through hole straight pin header, 1x09, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x09 2.54mm single row")
		(property "Reference" "J2"
			(at -0.3 6.14 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PinHeader_1x09_P2.54mm_Vertical"
			(at 9.6 4.34 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -10.16 270)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "IO16")
		)
		(pad "3" thru_hole circle
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "TOUT")
		)
		(pad "4" thru_hole circle
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "RST")
		)
		(pad "5" thru_hole circle
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "IO5")
		)
		(pad "6" thru_hole circle
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "7" thru_hole circle
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "TXD")
		)
		(pad "8" thru_hole circle
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "RXD")
		)
		(pad "9" thru_hole circle
			(at 0 -20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "IO4")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x09_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 133.65 81.8) (xy 133.6 105) (xy 135.6 105) (xy 135.5 130.8) (xy 139.8 130.8) (xy 154 130.9) (xy 154 105)
			(xy 156 105) (xy 156.05 81.8)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "IO0"
		(at 139.75 111.65 0)
		(layer "F.SilkS")
	)
	(gr_text "RXD"
		(at 146.65 111.7 0)
		(layer "F.SilkS")
	)
	(gr_text "IO2"
		(at 139.75 114.2 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 146.65 116.75 0)
		(layer "F.SilkS")
	)
	(gr_text "IO15"
		(at 139.75 116.75 0)
		(layer "F.SilkS")
	)
	(gr_text "IO16"
		(at 146 126.9 0)
		(layer "F.SilkS")
	)
	(gr_text "IO13"
		(at 139.8 119.25 0)
		(layer "F.SilkS")
	)
	(gr_text "IO12"
		(at 139.75 121.85 0)
		(layer "F.SilkS")
	)
	(gr_text "TOUT"
		(at 146 124.3 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 139.55 109.05 0)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 146.9 114.2 0)
		(layer "F.SilkS")
	)
	(gr_text "EN"
		(at 139.75 126.9 0)
		(layer "F.SilkS")
	)
	(gr_text "IO5"
		(at 147.05 119.25 0)
		(layer "F.SilkS")
	)
	(gr_text "IO14"
		(at 139.8 124.35 0)
		(layer "F.SilkS")
	)
	(gr_text "RST"
		(at 146.9 121.8 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 146.5 129.45 0)
		(layer "F.SilkS")
	)
	(gr_text "IO4"
		(at 147.1 109.15 0)
		(layer "F.SilkS")
	)
	(gr_text "+3V3"
		(at 139.8 129.45 0)
		(layer "F.SilkS")
	)
	(gr_text "ESP-WROOM-02D \nBREAKOUT BOARD\n@doggiedoc\n12/25/2025"
		(at 144.78 95.758 0)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.2 89.2) (xy 154.45 89.25) (xy 154.45 103.35) (xy 153.6 103.4) (xy 153.5 130.35) (xy 136.1 130.15)
				(xy 136 103.6) (xy 135 103.55) (xy 135.05 89.2)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.15 89.3) (xy 154.45 89.3) (xy 154.35 103.4) (xy 153.5 103.4) (xy 153.5 130.45) (xy 135.95 130.4)
				(xy 136 103.6) (xy 135.2 103.6)
			)
		)
	)
	(embedded_fonts no)
)
