(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "Model T 8K RAM Module")
		(date "2026-05-30")
		(rev "012")
		(company "b.kenyon.w@gmail.com")
		(comment 1 "github.com/bkw777/Model_T_RAM")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "HAL lead-free")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.22)
		(allow_soldermask_bridges_in_footprints yes)
		(tenting front back)
		(grid_origin 147.32 99.06)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "/~{CS_C}")
	(net 2 "/~{CS_D}")
	(net 3 "GND")
	(net 4 "/~{CS_A}")
	(net 5 "/~{CS_B}")
	(net 6 "VCC")
	(net 7 "/CE2")
	(net 8 "/A11")
	(net 9 "/A12")
	(net 10 "Net-(U2-Pad3)")
	(net 11 "/A7")
	(net 12 "/A6")
	(net 13 "/A5")
	(net 14 "/AD3")
	(net 15 "/A4")
	(net 16 "/AD4")
	(net 17 "/A3")
	(net 18 "/AD5")
	(net 19 "/A2")
	(net 20 "/AD6")
	(net 21 "/A1")
	(net 22 "/AD7")
	(net 23 "/A0")
	(net 24 "/AD0")
	(net 25 "/A10")
	(net 26 "/AD1")
	(net 27 "/AD2")
	(net 28 "/~{WE}")
	(net 29 "/A9")
	(net 30 "/A8")
	(net 31 "/RAM_RST")
	(net 32 "unconnected-(U1-NC-Pad1)")
	(footprint "000_LOCAL:DIP28_725mils_pcb_pins"
		(layer "F.Cu")
		(at 147.32 99.06 90)
		(descr "28-lead though-hole mounted DIP package, row spacing 700mils")
		(tags "THT DIP DIL PDIP 2.54mm 700mil")
		(property "Reference" "J1"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "KC-85_RAM"
			(at -1.5 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Model_T_RAM.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.397 -17.78)
			(end 9.652 -17.78)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -9.652 -17.78)
			(end -1.397 -17.78)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -10.16 -17.272)
			(end -10.16 17.272)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 10.16 17.272)
			(end 10.16 -17.272)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -9.652 17.78)
			(end 9.652 17.78)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 9.652 -17.78)
			(mid 10.01121 -17.63121)
			(end 10.16 -17.272)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -1.397 -17.78)
			(mid -1.307197 -17.742803)
			(end -1.27 -17.653)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 1.27 -17.653)
			(mid 1.307197 -17.742803)
			(end 1.397 -17.78)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 1.27 -17.653)
			(mid 0 -16.383)
			(end -1.27 -17.653)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -10.16 -17.272)
			(mid -10.01121 -17.63121)
			(end -9.652 -17.78)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 10.16 17.272)
			(mid 10.01121 17.63121)
			(end 9.652 17.78)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -9.652 17.78)
			(mid -10.01121 17.63121)
			(end -10.16 17.272)
			(layer "Edge.Cuts")
		)
		(fp_text user "KEL ICC05-028-360TP"
			(at 2 0 180)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at -9.2075 -16.51 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.1)
			(net 11 "/A7")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -9.2075 -13.97 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/A6")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at -9.2075 -11.43 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/A5")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -9.2075 -8.89 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/A4")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at -9.2075 -6.35 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/A3")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at -9.2075 -3.81 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/A2")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at -9.2075 -1.27 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/A1")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at -9.2075 1.27 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/A0")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -9.2075 3.81 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/AD0")
			(pinfunction "AD0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at -9.2075 6.35 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "/AD1")
			(pinfunction "AD1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at -9.2075 8.89 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/AD2")
			(pinfunction "AD2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at -9.2075 11.43 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at -9.2075 13.97 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/~{CS_A}")
			(pinfunction "~{CS_A}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at -9.2075 16.51 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/~{CS_B}")
			(pinfunction "~{CS_B}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 9.2075 16.51 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/~{CS_C}")
			(pinfunction "~{CS_C}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 9.2075 13.97 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 9.2075 11.43 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/AD3")
			(pinfunction "AD3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at 9.2075 8.89 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/AD4")
			(pinfunction "AD4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at 9.2075 6.35 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/AD5")
			(pinfunction "AD5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at 9.2075 3.81 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/AD6")
			(pinfunction "AD6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole circle
			(at 9.2075 1.27 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/AD7")
			(pinfunction "AD7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole circle
			(at 9.2075 -1.27 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "/RAM_RST")
			(pinfunction "RAM_RST")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole circle
			(at 9.2075 -3.81 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/A10")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole circle
			(at 9.2075 -6.35 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/~{CS_D}")
			(pinfunction "~{CS_D}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole circle
			(at 9.2075 -8.89 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "/~{WE}")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole circle
			(at 9.2075 -11.43 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "/A9")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole circle
			(at 9.2075 -13.97 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/A8")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole circle
			(at 9.2075 -16.51 90)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/packages3d/Mill_Max_3121_1_14_2.54.step"
			(offset
				(xyz 9.2075 16.51 -1.7272)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 90)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/packages3d/Mill_Max_3121_1_14_2.54.step"
			(offset
				(xyz -9.2075 16.51 -1.7272)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 90)
			)
		)
	)
	(footprint "000_LOCAL:SOIC-14_4x9"
		(layer "F.Cu")
		(at 158.115 99.06)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at 0.762 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "HC86"
			(at -0.889 0 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC86"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC GATE XOR 4CH 2-INP 14SOIC"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MC74HC86ADR2G"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(sheetname "/")
		(sheetfile "Model_T_RAM.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.6655 -3.81)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/~{CS_D}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.6655 -2.54)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/~{CS_C}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.6655 -1.27)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U2-Pad3)")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.6655 0)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U2-Pad3)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.6655 1.27)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/A11")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.6655 2.54)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/CE2")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.6655 3.81)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 2.6655 3.81)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/A11")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.6655 2.54)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/~{CS_A}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.6655 1.27)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/~{CS_B}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.6655 0)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/A12")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.6655 -1.27)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/~{CS_A}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.6655 -2.54)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/~{CS_C}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.6655 -3.81)
			(size 1.524 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/packages3d/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 160.02 93.345 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "datasheets/885012207045.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 16V X7R 0805"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "885012207045"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Model_T_RAM.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/packages3d/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 132.08 93.98 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "datasheets/885012207045.pdf"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 16V X7R 0805"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "885012207045"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Model_T_RAM.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/packages3d/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SSOP-28"
		(layer "F.Cu")
		(at 142.875 99.06 90)
		(property "Reference" "U1"
			(at -0.9 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "6264"
			(at 1 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/Alliance-Memory_64K_AS6C6264v2.0July2017.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SRAM 8Kx8 Parallel 55ns 5v 28-SOP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AS6C6264-55SCN"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Model_T_RAM.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -5.4229 -8.255 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "unconnected-(U1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -5.4229 -6.985 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/A12")
			(pinfunction "A12")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -5.4229 -5.715 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/A7")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -5.4229 -4.445 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A6")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -5.4229 -3.175 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/A5")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -5.4229 -1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/A4")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -5.4229 -0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A3")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -5.4229 0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A2")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -5.4229 1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/A1")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -5.4229 3.175 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/A0")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -5.4229 4.445 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/AD0")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -5.4229 5.715 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/AD1")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -5.4229 6.985 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/AD2")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -5.4229 8.255 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 5.4229 8.255 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/AD3")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 5.4229 6.985 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/AD4")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 5.4229 5.715 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/AD5")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 5.4229 4.445 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/AD6")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 5.4229 3.175 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/AD7")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 5.4229 1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/RAM_RST")
			(pinfunction "~{CE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 5.4229 0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/A10")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 5.4229 -0.635 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 5.4229 -1.905 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/A11")
			(pinfunction "A11")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 5.4229 -3.175 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/A9")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 5.4229 -4.445 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/A8")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 5.4229 -5.715 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/CE2")
			(pinfunction "CE2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 5.4229 -6.985 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/~{WE}")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 5.4229 -8.255 90)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/packages3d/SOP-28_MIL330_ALL.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_text "${COMMENT1} v${REVISION}"
		(at 147.32 106.46 0)
		(layer "F.SilkS")
	)
	(gr_text "\"Model T\" 8K RAM"
		(at 147.32 91.76 0)
		(layer "F.SilkS")
	)
	(gr_text "Kyotronic KC-85\nTRS-80 Model 100\nNEC PC-8201 / PC-8300\nOlivetti M10"
		(at 147.32 99.06 0)
		(layer "B.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 163.83 108.2675) (xy 163.83 89.8525)
		)
		(height 3.81)
		(format
			(prefix "")
			(suffix "")
			(units 1)
			(units_format 1)
			(precision 0)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "725 mils"
			(at 166.49 99.06 90)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 29)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.801086 90.622165) (xy 136.705717 90.519747) (xy 136.637176 90.430144) (xy 136.596008 90.359966)
				(xy 136.567531 90.292417) (xy 136.534957 90.145938) (xy 136.523227 90.044979) (xy 136.506971 89.90647)
				(xy 136.478471 89.735446) (xy 135.889293 89.851793) (xy 135.772946 90.440971) (xy 136.047399 90.48195)
				(xy 136.082479 90.485727) (xy 136.231905 90.505066) (xy 136.363215 90.542739) (xy 136.498453 90.621371)
				(xy 136.659665 90.763586)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.686274 92.6735) (xy 151.538085 92.700459) (xy 151.437907 92.72175) (xy 151.404244 92.724648)
				(xy 151.389247 92.718493) (xy 151.129 93.6371) (xy 151.4094 93.717872) (xy 151.41432 93.485742)
				(xy 151.432557 93.279332) (xy 151.454612 93.156179) (xy 151.485636 93.051843) (xy 151.516134 92.986328)
				(xy 151.553006 92.934631) (xy 151.587965 92.903653) (xy 151.627701 92.883225) (xy 151.686274 92.8735)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.99725 92.303829) (xy 145.965685 92.465455) (xy 145.932784 92.556453) (xy 145.888633 92.639132)
				(xy 145.850934 92.686074) (xy 145.807788 92.719228) (xy 145.783283 92.729672) (xy 146.049293 93.637807)
				(xy 146.318766 92.732739) (xy 146.241545 92.689119) (xy 146.181436 92.614225) (xy 146.144161 92.513228)
				(xy 146.138671 92.44525)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/~{CS_C}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.93 91.040971) (xy 163.934985 90.901115) (xy 163.949877 90.78929) (xy 163.970391 90.710556)
				(xy 163.998019 90.642656) (xy 164.078562 90.516046) (xy 164.141656 90.436364) (xy 164.228102 90.326928)
				(xy 164.328882 90.185842) (xy 163.83 89.8515) (xy 163.331118 90.185842) (xy 163.496207 90.408886)
				(xy 163.518345 90.436365) (xy 163.61033 90.555699) (xy 163.676541 90.675188) (xy 163.716567 90.826416)
				(xy 163.73 91.040971)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(U2-Pad3)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.3495 98.46) (xy 155.344196 98.519337) (xy 155.327066 98.590584) (xy 155.300901 98.65331)
				(xy 155.26303 98.707847) (xy 155.229027 98.736735) (xy 155.188313 98.754951) (xy 155.1495 98.76)
				(xy 155.4495 99.061) (xy 155.7495 98.76) (xy 155.678542 98.741866) (xy 155.620875 98.689619) (xy 155.575123 98.600089)
				(xy 155.550402 98.482667) (xy 155.5495 98.46)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.41 92.3671) (xy 143.4043 92.448017) (xy 143.384398 92.544971) (xy 143.358315 92.615205)
				(xy 143.320654 92.676139) (xy 143.286999 92.70883) (xy 143.246474 92.730949) (xy 143.241234 92.732739)
				(xy 143.51 93.6381) (xy 143.778766 92.732739) (xy 143.714862 92.693173) (xy 143.662698 92.61733)
				(xy 143.624478 92.499905) (xy 143.61 92.3671)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.26 94.9071) (xy 137.2657 94.826183) (xy 137.285602 94.72923) (xy 137.311685 94.658995) (xy 137.349346 94.598061)
				(xy 137.383001 94.56537) (xy 137.423526 94.543251) (xy 137.428766 94.541461) (xy 137.16 93.6361)
				(xy 136.891234 94.541461) (xy 136.955138 94.581028) (xy 137.007302 94.656871) (xy 137.045522 94.774297)
				(xy 137.06 94.9071)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.7185 102.97) (xy 159.794042 102.975407) (xy 159.884604 102.993253) (xy 159.962191 103.019707)
				(xy 160.032152 103.058157) (xy 160.072289 103.093174) (xy 160.101618 103.135354) (xy 160.111097 103.158582)
				(xy 160.7815 102.87) (xy 160.111097 102.581418) (xy 160.070288 102.648983) (xy 159.992453 102.705967)
				(xy 159.872479 102.749855) (xy 159.7185 102.77)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.535483 92.303097) (xy 148.505193 92.463268) (xy 148.472823 92.554567) (xy 148.429131 92.63793)
				(xy 148.391432 92.685898) (xy 148.34816 92.720118) (xy 148.321984 92.731616) (xy 148.589293 93.637807)
				(xy 148.858766 92.732739) (xy 148.781366 92.689059) (xy 148.72073 92.613882) (xy 148.682782 92.512432)
				(xy 148.676903 92.444517)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/~{CS_B}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.73 107.079029) (xy 163.725015 107.218884) (xy 163.710123 107.330709) (xy 163.689609 107.409442)
				(xy 163.661981 107.477342) (xy 163.581438 107.603952) (xy 163.518345 107.683634) (xy 163.431899 107.793071)
				(xy 163.331118 107.934158) (xy 163.83 108.2685) (xy 164.328882 107.934158) (xy 164.163792 107.711113)
				(xy 164.141655 107.683635) (xy 164.04967 107.5643) (xy 163.983459 107.444812) (xy 163.943433 107.293584)
				(xy 163.93 107.079029)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.261086 90.622165) (xy 134.165717 90.519747) (xy 134.097176 90.430144) (xy 134.056008 90.359966)
				(xy 134.027531 90.292417) (xy 133.994957 90.145938) (xy 133.983227 90.044979) (xy 133.966971 89.90647)
				(xy 133.938471 89.735446) (xy 133.349293 89.851793) (xy 133.232946 90.440971) (xy 133.507399 90.48195)
				(xy 133.542479 90.485727) (xy 133.691905 90.505066) (xy 133.823215 90.542739) (xy 133.958453 90.621371)
				(xy 134.119665 90.763586)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.88 92.03) (xy 131.874087 92.127889) (xy 131.852697 92.247018) (xy 131.825367 92.3326) (xy 131.785718 92.411362)
				(xy 131.748716 92.459556) (xy 131.70372 92.497949) (xy 131.660817 92.520101) (xy 131.611805 92.532647)
				(xy 131.58 92.534972) (xy 132.08 93.031) (xy 132.58 92.534972) (xy 132.531388 92.52967) (xy 132.488118 92.515507)
				(xy 132.41368 92.462087) (xy 132.352269 92.372222) (xy 132.30575 92.240744) (xy 132.281498 92.077279)
				(xy 132.28 92.03)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/~{WE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.79 92.3671) (xy 135.7843 92.448017) (xy 135.764398 92.544971) (xy 135.738315 92.615205)
				(xy 135.700654 92.676139) (xy 135.666999 92.70883) (xy 135.626474 92.730949) (xy 135.621234 92.732739)
				(xy 135.89 93.6381) (xy 136.158766 92.732739) (xy 136.094862 92.693173) (xy 136.042698 92.61733)
				(xy 136.004478 92.499905) (xy 135.99 92.3671)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.88 105.7529) (xy 144.8857 105.671983) (xy 144.905602 105.57503) (xy 144.931685 105.504795)
				(xy 144.969346 105.443861) (xy 145.003001 105.41117) (xy 145.043526 105.389051) (xy 145.048766 105.387261)
				(xy 144.78 104.4819) (xy 144.511234 105.387261) (xy 144.575138 105.426828) (xy 144.627302 105.502671)
				(xy 144.665522 105.620097) (xy 144.68 105.7529)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.739665 107.356414) (xy 141.637247 107.451782) (xy 141.547644 107.520324) (xy 141.477466 107.561491)
				(xy 141.409917 107.589968) (xy 141.263437 107.622542) (xy 141.16248 107.634272) (xy 141.023971 107.650529)
				(xy 140.852946 107.679029) (xy 140.969293 108.268207) (xy 141.558471 108.384554) (xy 141.59945 108.110101)
				(xy 141.603227 108.075021) (xy 141.622566 107.925594) (xy 141.660239 107.794285) (xy 141.738871 107.659047)
				(xy 141.881086 107.497835)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.357239 92.43866) (xy 138.33773 92.541369) (xy 138.311185 92.600323) (xy 138.27307 92.655625)
				(xy 138.233217 92.694131) (xy 138.18534 92.723414) (xy 138.161234 92.732739) (xy 138.430707 93.637807)
				(xy 138.698766 92.732739) (xy 138.637312 92.693797) (xy 138.578654 92.611484) (xy 138.527149 92.477117)
				(xy 138.499204 92.315012) (xy 138.49866 92.297239)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/~{CS_C}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.7185 96.62) (xy 159.794042 96.625407) (xy 159.884604 96.643253) (xy 159.962191 96.669707)
				(xy 160.032152 96.708157) (xy 160.072289 96.743174) (xy 160.101618 96.785354) (xy 160.111097 96.808582)
				(xy 160.7815 96.52) (xy 160.111097 96.231418) (xy 160.070288 96.298983) (xy 159.992453 96.355967)
				(xy 159.872479 96.399855) (xy 159.7185 96.42)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.070696 98.96) (xy 159.991164 98.955332) (xy 159.930569 98.942658) (xy 159.828313 98.894439)
				(xy 159.746684 98.851714) (xy 159.624273 98.814804) (xy 159.5745 99.06) (xy 159.624273 99.305196)
				(xy 159.760915 99.261905) (xy 159.828313 99.225561) (xy 159.923209 99.179647) (xy 159.986372 99.165319)
				(xy 160.070696 99.16)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.279625 92.308955) (xy 147.265419 92.387647) (xy 147.237963 92.482347) (xy 147.201513 92.570089)
				(xy 147.154549 92.646706) (xy 147.117183 92.686106) (xy 147.075275 92.711589) (xy 147.062556 92.715793)
				(xy 147.319293 93.637807) (xy 147.588766 92.732739) (xy 147.512828 92.68955) (xy 147.456384 92.616628)
				(xy 147.423743 92.518767) (xy 147.421045 92.450375)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.138671 105.67475) (xy 146.152526 105.573774) (xy 146.175641 105.516583) (xy 146.210583 105.462793)
				(xy 146.247941 105.425558) (xy 146.293889 105.396964) (xy 146.318766 105.387261) (xy 146.049293 104.482193)
				(xy 145.783282 105.390327) (xy 145.845896 105.429002) (xy 145.907359 105.51171) (xy 145.963455 105.647181)
				(xy 145.996722 105.809117) (xy 145.99725 105.816171)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/~{CS_C}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.8425 96.42) (xy 161.766958 96.414593) (xy 161.676396 96.396747) (xy 161.59881 96.370293)
				(xy 161.528848 96.331843) (xy 161.488711 96.296825) (xy 161.459382 96.254646) (xy 161.449903 96.231418)
				(xy 160.7795 96.52) (xy 161.449903 96.808582) (xy 161.490712 96.741016) (xy 161.568548 96.684032)
				(xy 161.688523 96.640144) (xy 161.8425 96.62)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.3875 101.7) (xy 154.463042 101.705407) (xy 154.553604 101.723253) (xy 154.631191 101.749707)
				(xy 154.701152 101.788157) (xy 154.741289 101.823174) (xy 154.770618 101.865354) (xy 154.780097 101.888582)
				(xy 155.4505 101.6) (xy 154.780097 101.311418) (xy 154.739288 101.378983) (xy 154.661453 101.435967)
				(xy 154.541479 101.479855) (xy 154.3875 101.5)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.207446 105.813974) (xy 137.243067 105.64767) (xy 137.277534 105.5578) (xy 137.322989 105.477431)
				(xy 137.360618 105.433645) (xy 137.40331 105.403734) (xy 137.422783 105.396214) (xy 137.160707 104.482193)
				(xy 136.891234 105.387261) (xy 136.967911 105.430699) (xy 137.026443 105.504747) (xy 137.061717 105.604393)
				(xy 137.066026 105.672554)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.758914 107.497835) (xy 152.854282 107.600253) (xy 152.922824 107.689855) (xy 152.963991 107.760034)
				(xy 152.992468 107.827582) (xy 153.025042 107.974062) (xy 153.036772 108.07502) (xy 153.053029 108.213529)
				(xy 153.081529 108.384554) (xy 153.670707 108.268207) (xy 153.787054 107.679029) (xy 153.512601 107.638049)
				(xy 153.47752 107.634272) (xy 153.328093 107.614933) (xy 153.196784 107.57726) (xy 153.061547 107.498628)
				(xy 152.900335 107.356414)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.791797 90.551454) (xy 131.709059 90.461937) (xy 131.646049 90.379759) (xy 131.566588 90.232877)
				(xy 131.521675 90.079483) (xy 131.509523 90.020142) (xy 131.486855 89.9144) (xy 131.45281 89.798952)
				(xy 131.396962 89.668853) (xy 131.308882 89.519158) (xy 130.809293 89.851793) (xy 130.476658 90.351382)
				(xy 130.580345 90.415018) (xy 130.674325 90.462349) (xy 130.851414 90.524223) (xy 130.977642 90.552023)
				(xy 131.099205 90.579027) (xy 131.222507 90.622905) (xy 131.356204 90.701911) (xy 131.508954 90.834297)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.980335 90.763586) (xy 158.082753 90.668217) (xy 158.172355 90.599676) (xy 158.242534 90.558508)
				(xy 158.310082 90.530031) (xy 158.456561 90.497457) (xy 158.557521 90.485727) (xy 158.69603 90.469471)
				(xy 158.867054 90.440971) (xy 158.750707 89.851793) (xy 158.161529 89.735446) (xy 158.120549 90.009898)
				(xy 158.116772 90.04498) (xy 158.097433 90.194406) (xy 158.05976 90.325715) (xy 157.981128 90.460953)
				(xy 157.838914 90.622165)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/~{WE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.99 92.685196) (xy 135.994668 92.605664) (xy 136.007342 92.545069) (xy 136.055561 92.442813)
				(xy 136.098285 92.361184) (xy 136.135196 92.238773) (xy 135.89 92.189) (xy 135.644804 92.238773)
				(xy 135.688094 92.375415) (xy 135.724439 92.442813) (xy 135.770353 92.537709) (xy 135.784681 92.600872)
				(xy 135.79 92.685196)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.119665 107.356414) (xy 134.017247 107.451782) (xy 133.927644 107.520324) (xy 133.857466 107.561491)
				(xy 133.789917 107.589968) (xy 133.643437 107.622542) (xy 133.54248 107.634272) (xy 133.403971 107.650529)
				(xy 133.232946 107.679029) (xy 133.349293 108.268207) (xy 133.938471 108.384554) (xy 133.97945 108.110101)
				(xy 133.983227 108.075021) (xy 134.002566 107.925594) (xy 134.040239 107.794285) (xy 134.118871 107.659047)
				(xy 134.261086 107.497835)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.218914 107.497835) (xy 150.314282 107.600253) (xy 150.382824 107.689855) (xy 150.423991 107.760034)
				(xy 150.452468 107.827582) (xy 150.485042 107.974062) (xy 150.496772 108.07502) (xy 150.513029 108.213529)
				(xy 150.541529 108.384554) (xy 151.130707 108.268207) (xy 151.247054 107.679029) (xy 150.972601 107.638049)
				(xy 150.93752 107.634272) (xy 150.788093 107.614933) (xy 150.656784 107.57726) (xy 150.521547 107.498628)
				(xy 150.360335 107.356414)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/~{CS_A}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.7185 97.89) (xy 159.794042 97.895407) (xy 159.884604 97.913253) (xy 159.962191 97.939707)
				(xy 160.032152 97.978157) (xy 160.072289 98.013174) (xy 160.101618 98.055354) (xy 160.111097 98.078582)
				(xy 160.7815 97.79) (xy 160.111097 97.501418) (xy 160.070288 97.568983) (xy 159.992453 97.625967)
				(xy 159.872479 97.669855) (xy 159.7185 97.69)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.820335 90.763586) (xy 147.922753 90.668217) (xy 148.012355 90.599676) (xy 148.082534 90.558508)
				(xy 148.150082 90.530031) (xy 148.296561 90.497457) (xy 148.397521 90.485727) (xy 148.53603 90.469471)
				(xy 148.707054 90.440971) (xy 148.590707 89.851793) (xy 148.001529 89.735446) (xy 147.960549 90.009898)
				(xy 147.956772 90.04498) (xy 147.937433 90.194406) (xy 147.89976 90.325715) (xy 147.821128 90.460953)
				(xy 147.678914 90.622165)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/RAM_RST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.280335 90.763586) (xy 145.382753 90.668217) (xy 145.472355 90.599676) (xy 145.542534 90.558508)
				(xy 145.610082 90.530031) (xy 145.756561 90.497457) (xy 145.857521 90.485727) (xy 145.99603 90.469471)
				(xy 146.167054 90.440971) (xy 146.050707 89.851793) (xy 145.461529 89.735446) (xy 145.420549 90.009898)
				(xy 145.416772 90.04498) (xy 145.397433 90.194406) (xy 145.35976 90.325715) (xy 145.281128 90.460953)
				(xy 145.138914 90.622165)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/RAM_RST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.68 92.3671) (xy 144.6743 92.448017) (xy 144.654398 92.544971) (xy 144.628315 92.615205)
				(xy 144.590654 92.676139) (xy 144.556999 92.70883) (xy 144.516474 92.730949) (xy 144.511234 92.732739)
				(xy 144.78 93.6381) (xy 145.048766 92.732739) (xy 144.984862 92.693173) (xy 144.932698 92.61733)
				(xy 144.894478 92.499905) (xy 144.88 92.3671)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.61 91.040971) (xy 143.614985 90.901115) (xy 143.629877 90.78929) (xy 143.650391 90.710556)
				(xy 143.678019 90.642656) (xy 143.758562 90.516046) (xy 143.821656 90.436364) (xy 143.908102 90.326928)
				(xy 144.008882 90.185842) (xy 143.51 89.8515) (xy 143.011118 90.185842) (xy 143.176207 90.408886)
				(xy 143.198345 90.436365) (xy 143.29033 90.555699) (xy 143.356541 90.675188) (xy 143.396567 90.826416)
				(xy 143.41 91.040971)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.42 105.7529) (xy 147.4257 105.671983) (xy 147.445602 105.57503) (xy 147.471685 105.504795)
				(xy 147.509346 105.443861) (xy 147.543001 105.41117) (xy 147.583526 105.389051) (xy 147.588766 105.387261)
				(xy 147.32 104.4819) (xy 147.051234 105.387261) (xy 147.115138 105.426828) (xy 147.167302 105.502671)
				(xy 147.205522 105.620097) (xy 147.22 105.7529)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.728406 107.207673) (xy 131.578013 107.330642) (xy 131.34876 107.465508) (xy 131.21324 107.527768)
				(xy 131.071162 107.581492) (xy 130.934813 107.622061) (xy 130.798632 107.651018) (xy 130.681174 107.665329)
				(xy 130.568049 107.66776) (xy 130.561472 107.6675) (xy 130.809293 108.268207) (xy 131.41 108.516028)
				(xy 131.420319 108.319523) (xy 131.471093 108.085567) (xy 131.566048 107.826318) (xy 131.698198 107.57385)
				(xy 131.770004 107.467096) (xy 131.842613 107.377704) (xy 131.869827 107.349094)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/~{CS_A}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.7185 101.7) (xy 159.794042 101.705407) (xy 159.884604 101.723253) (xy 159.962191 101.749707)
				(xy 160.032152 101.788157) (xy 160.072289 101.823174) (xy 160.101618 101.865354) (xy 160.111097 101.888582)
				(xy 160.7815 101.6) (xy 160.111097 101.311418) (xy 160.070288 101.378983) (xy 159.992453 101.435967)
				(xy 159.872479 101.479855) (xy 159.7185 101.5)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.754517 105.816903) (xy 139.784807 105.656731) (xy 139.817177 105.565433) (xy 139.860868 105.48207)
				(xy 139.898568 105.434102) (xy 139.94184 105.399881) (xy 139.968015 105.388383) (xy 139.700707 104.482193)
				(xy 139.431234 105.387261) (xy 139.508634 105.430942) (xy 139.569271 105.506119) (xy 139.607218 105.607569)
				(xy 139.613097 105.675483)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.34 105.7529) (xy 142.3457 105.671983) (xy 142.365602 105.57503) (xy 142.391685 105.504795)
				(xy 142.429346 105.443861) (xy 142.463001 105.41117) (xy 142.503526 105.389051) (xy 142.508766 105.387261)
				(xy 142.24 104.4819) (xy 141.971234 105.387261) (xy 142.035138 105.426828) (xy 142.087302 105.502671)
				(xy 142.125522 105.620097) (xy 142.14 105.7529)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.77 94.65) (xy 160.766089 94.735446) (xy 160.74214 94.834285) (xy 160.716927 94.879185) (xy 160.679834 94.915982)
				(xy 160.628571 94.940859) (xy 160.560848 94.95) (xy 160.7805 95.251) (xy 161.189967 94.95) (xy 161.165822 94.945239)
				(xy 161.149461 94.931912) (xy 161.135588 94.884171) (xy 161.145422 94.787707) (xy 161.155493 94.738725)
				(xy 161.17 94.65)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.0612 93.23) (xy 134.105841 93.235046) (xy 134.148839 93.250369) (xy 134.188396 93.275436)
				(xy 134.224937 93.310769) (xy 134.286923 93.415259) (xy 134.328459 93.57179) (xy 134.3406 93.74517)
				(xy 134.621 93.6371) (xy 134.3406 92.920845) (xy 134.335846 92.93097) (xy 134.322571 92.932893)
				(xy 134.259148 92.910501) (xy 134.209386 92.886562) (xy 134.126756 92.848031) (xy 134.0612 92.83)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.676903 105.675483) (xy 148.691386 105.574321) (xy 148.714877 105.516937) (xy 148.750166 105.462981)
				(xy 148.787798 105.425603) (xy 148.83396 105.396928) (xy 148.858766 105.387261) (xy 148.589293 104.482193)
				(xy 148.321984 105.388383) (xy 148.384796 105.427515) (xy 148.446278 105.510665) (xy 148.502115 105.646409)
				(xy 148.534897 105.808514) (xy 148.535483 105.816903)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.199665 107.356414) (xy 139.097247 107.451782) (xy 139.007644 107.520324) (xy 138.937466 107.561491)
				(xy 138.869917 107.589968) (xy 138.723437 107.622542) (xy 138.62248 107.634272) (xy 138.483971 107.650529)
				(xy 138.312946 107.679029) (xy 138.429293 108.268207) (xy 139.018471 108.384554) (xy 139.05945 108.110101)
				(xy 139.063227 108.075021) (xy 139.082566 107.925594) (xy 139.120239 107.794285) (xy 139.198871 107.659047)
				(xy 139.341086 107.497835)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.79134 92.297239) (xy 149.769927 92.449734) (xy 149.74209 92.541763) (xy 149.702611 92.627349)
				(xy 149.666724 92.678784) (xy 149.624602 92.716612) (xy 149.591234 92.732739) (xy 149.859293 93.637807)
				(xy 150.128766 92.732739) (xy 150.049964 92.688589) (xy 149.985072 92.611141) (xy 149.941649 92.506029)
				(xy 149.932761 92.43866)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/~{CS_D}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.3875 95.35) (xy 154.463042 95.355407) (xy 154.553604 95.373253) (xy 154.631191 95.399707)
				(xy 154.701152 95.438157) (xy 154.741289 95.473174) (xy 154.770618 95.515354) (xy 154.780097 95.538582)
				(xy 155.4505 95.25) (xy 154.780097 94.961418) (xy 154.739288 95.028983) (xy 154.661453 95.085967)
				(xy 154.541479 95.129855) (xy 154.3875 95.15)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.02275 105.816171) (xy 141.054315 105.654545) (xy 141.087216 105.563547) (xy 141.131367 105.480867)
				(xy 141.169066 105.433924) (xy 141.212212 105.400769) (xy 141.236718 105.390324) (xy 140.970707 104.482193)
				(xy 140.701234 105.387261) (xy 140.778455 105.430882) (xy 140.838564 105.505777) (xy 140.875839 105.606773)
				(xy 140.881329 105.67475)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.138914 107.497835) (xy 145.234282 107.600253) (xy 145.302824 107.689855) (xy 145.343991 107.760034)
				(xy 145.372468 107.827582) (xy 145.405042 107.974062) (xy 145.416772 108.07502) (xy 145.433029 108.213529)
				(xy 145.461529 108.384554) (xy 146.050707 108.268207) (xy 146.167054 107.679029) (xy 145.892601 107.638049)
				(xy 145.85752 107.634272) (xy 145.708093 107.614933) (xy 145.576784 107.57726) (xy 145.441547 107.498628)
				(xy 145.280335 107.356414)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/~{CS_C}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.5115 96.42) (xy 156.435958 96.414593) (xy 156.345396 96.396747) (xy 156.26781 96.370293)
				(xy 156.197848 96.331843) (xy 156.157711 96.296825) (xy 156.128382 96.254646) (xy 156.118903 96.231418)
				(xy 155.4485 96.52) (xy 156.118903 96.808582) (xy 156.159712 96.741016) (xy 156.237548 96.684032)
				(xy 156.357523 96.640144) (xy 156.5115 96.62)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.900335 90.763586) (xy 153.002753 90.668217) (xy 153.092355 90.599676) (xy 153.162534 90.558508)
				(xy 153.230082 90.530031) (xy 153.376561 90.497457) (xy 153.477521 90.485727) (xy 153.61603 90.469471)
				(xy 153.787054 90.440971) (xy 153.670707 89.851793) (xy 153.081529 89.735446) (xy 153.040549 90.009898)
				(xy 153.036772 90.04498) (xy 153.017433 90.194406) (xy 152.97976 90.325715) (xy 152.901128 90.460953)
				(xy 152.758914 90.622165)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.7185 99.16) (xy 159.794042 99.165407) (xy 159.884604 99.183253) (xy 159.962191 99.209707)
				(xy 160.032152 99.248157) (xy 160.072289 99.283174) (xy 160.101618 99.325354) (xy 160.111097 99.348582)
				(xy 160.7815 99.06) (xy 160.111097 98.771418) (xy 160.070288 98.838983) (xy 159.992453 98.895967)
				(xy 159.872479 98.939855) (xy 159.7185 98.96)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.463304 105.808116) (xy 138.480378 105.725625) (xy 138.511905 105.626473) (xy 138.550144 105.541736)
				(xy 138.598267 105.469749) (xy 138.635166 105.434928) (xy 138.676079 105.413972) (xy 138.681991 105.412365)
				(xy 138.430707 104.482193) (xy 138.161234 105.387261) (xy 138.23642 105.430198) (xy 138.29079 105.501999)
				(xy 138.320842 105.598094) (xy 138.321884 105.666696)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.613097 92.444517) (xy 139.598614 92.545679) (xy 139.575123 92.603063) (xy 139.539834 92.657019)
				(xy 139.502203 92.694397) (xy 139.45604 92.723072) (xy 139.431234 92.732739) (xy 139.700707 93.637807)
				(xy 139.968015 92.731616) (xy 139.905204 92.692484) (xy 139.843722 92.609335) (xy 139.787885 92.473591)
				(xy 139.755103 92.311486) (xy 139.754517 92.303097)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.3875 100.43) (xy 154.463042 100.435407) (xy 154.553604 100.453253) (xy 154.631191 100.479707)
				(xy 154.701152 100.518157) (xy 154.741289 100.553174) (xy 154.770618 100.595354) (xy 154.780097 100.618582)
				(xy 155.4505 100.33) (xy 154.780097 100.041418) (xy 154.739288 100.108983) (xy 154.661453 100.165967)
				(xy 154.541479 100.209855) (xy 154.3875 100.23)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.41 107.079029) (xy 143.405015 107.218884) (xy 143.390123 107.330709) (xy 143.369609 107.409442)
				(xy 143.341981 107.477342) (xy 143.261438 107.603952) (xy 143.198345 107.683634) (xy 143.111899 107.793071)
				(xy 143.011118 107.934158) (xy 143.51 108.2685) (xy 144.008882 107.934158) (xy 143.843792 107.711113)
				(xy 143.821655 107.683635) (xy 143.72967 107.5643) (xy 143.663459 107.444812) (xy 143.623433 107.293584)
				(xy 143.61 107.079029)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.932761 105.68134) (xy 149.952269 105.578634) (xy 149.978813 105.51968) (xy 150.016927 105.464378)
				(xy 150.05678 105.425871) (xy 150.104657 105.396587) (xy 150.128766 105.387261) (xy 149.859293 104.482193)
				(xy 149.591234 105.387261) (xy 149.652689 105.426204) (xy 149.711346 105.508517) (xy 149.762851 105.642885)
				(xy 149.790796 105.80499) (xy 149.79134 105.822761)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.17 94.57) (xy 161.176332 94.438866) (xy 161.200659 94.280333) (xy 161.228726 94.178925)
				(xy 161.26903 94.084193) (xy 161.307231 94.023249) (xy 161.353745 93.972038) (xy 161.398024 93.939493)
				(xy 161.448662 93.916423) (xy 161.45097 93.915671) (xy 160.97 93.344) (xy 160.48903 93.915671) (xy 160.575687 93.96303)
				(xy 160.648481 94.045799) (xy 160.708288 94.170337) (xy 160.751066 94.341182) (xy 160.769681 94.541908)
				(xy 160.77 94.57)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(U2-Pad3)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.5495 98.39) (xy 155.554804 98.330663) (xy 155.571934 98.259416) (xy 155.598099 98.19669)
				(xy 155.63597 98.142153) (xy 155.669973 98.113265) (xy 155.710687 98.095049) (xy 155.7495 98.09)
				(xy 155.4495 97.789) (xy 155.1495 98.09) (xy 155.220458 98.108134) (xy 155.278125 98.160381) (xy 155.323877 98.249911)
				(xy 155.348598 98.367333) (xy 155.3495 98.39)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/~{CS_B}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.8425 100.23) (xy 161.766958 100.224593) (xy 161.676396 100.206747) (xy 161.59881 100.180293)
				(xy 161.528848 100.141843) (xy 161.488711 100.106825) (xy 161.459382 100.064646) (xy 161.449903 100.041418)
				(xy 160.7795 100.33) (xy 161.449903 100.618582) (xy 161.490712 100.551016) (xy 161.568548 100.494032)
				(xy 161.688523 100.450144) (xy 161.8425 100.43)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.61 105.7529) (xy 143.6157 105.671983) (xy 143.635602 105.57503) (xy 143.661685 105.504795)
				(xy 143.699346 105.443861) (xy 143.733001 105.41117) (xy 143.773526 105.389051) (xy 143.778766 105.387261)
				(xy 143.51 104.4819) (xy 143.241234 105.387261) (xy 143.305138 105.426828) (xy 143.357302 105.502671)
				(xy 143.395522 105.620097) (xy 143.41 105.7529)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.07 94.9071) (xy 141.0757 94.826183) (xy 141.095602 94.72923) (xy 141.121685 94.658995) (xy 141.159346 94.598061)
				(xy 141.193001 94.56537) (xy 141.233526 94.543251) (xy 141.238766 94.541461) (xy 140.97 93.6361)
				(xy 140.701234 94.541461) (xy 140.765138 94.581028) (xy 140.817302 94.656871) (xy 140.855522 94.774297)
				(xy 140.87 94.9071)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.298914 107.497835) (xy 155.394282 107.600253) (xy 155.462824 107.689855) (xy 155.503991 107.760034)
				(xy 155.532468 107.827582) (xy 155.565042 107.974062) (xy 155.576772 108.07502) (xy 155.593029 108.213529)
				(xy 155.621529 108.384554) (xy 156.210707 108.268207) (xy 156.327054 107.679029) (xy 156.052601 107.638049)
				(xy 156.01752 107.634272) (xy 155.868093 107.614933) (xy 155.736784 107.57726) (xy 155.601547 107.498628)
				(xy 155.440335 107.356414)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/~{CS_A}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.8425 101.5) (xy 161.766958 101.494593) (xy 161.676396 101.476747) (xy 161.59881 101.450293)
				(xy 161.528848 101.411843) (xy 161.488711 101.376825) (xy 161.459382 101.334646) (xy 161.449903 101.311418)
				(xy 160.7795 101.6) (xy 161.449903 101.888582) (xy 161.490712 101.821016) (xy 161.568548 101.764032)
				(xy 161.688523 101.720144) (xy 161.8425 101.7)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.659665 107.356414) (xy 136.557247 107.451782) (xy 136.467644 107.520324) (xy 136.397466 107.561491)
				(xy 136.329917 107.589968) (xy 136.183437 107.622542) (xy 136.08248 107.634272) (xy 135.943971 107.650529)
				(xy 135.772946 107.679029) (xy 135.889293 108.268207) (xy 136.478471 108.384554) (xy 136.51945 108.110101)
				(xy 136.523227 108.075021) (xy 136.542566 107.925594) (xy 136.580239 107.794285) (xy 136.658871 107.659047)
				(xy 136.801086 107.497835)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.305 92.83) (xy 133.173866 92.823668) (xy 133.015333 92.799341) (xy 132.913925 92.771274)
				(xy 132.819193 92.73097) (xy 132.758249 92.692769) (xy 132.707038 92.646255) (xy 132.674493 92.601976)
				(xy 132.651423 92.551338) (xy 132.650671 92.54903) (xy 132.079 93.03) (xy 132.650671 93.51097) (xy 132.69803 93.424313)
				(xy 132.780799 93.351519) (xy 132.905337 93.291712) (xy 133.076182 93.248934) (xy 133.276908 93.230319)
				(xy 133.305 93.23)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.99 103.428696) (xy 135.994668 103.349164) (xy 136.007342 103.288569) (xy 136.055561 103.186313)
				(xy 136.098285 103.104684) (xy 136.135196 102.982273) (xy 135.89 102.9325) (xy 135.644804 102.982273)
				(xy 135.688094 103.118915) (xy 135.724439 103.186313) (xy 135.770353 103.281209) (xy 135.784681 103.344372)
				(xy 135.79 103.428696)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/~{CS_D}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.705 90.777946) (xy 141.699889 90.522365) (xy 141.68411 90.3405) (xy 141.628252 90.057627)
				(xy 141.558471 89.735446) (xy 140.97 89.8515) (xy 140.636658 90.351382) (xy 140.773656 90.421348)
				(xy 140.929365 90.461439) (xy 141.136041 90.479259) (xy 141.282781 90.490519) (xy 141.345584 90.503899)
				(xy 141.399712 90.526769) (xy 141.443941 90.562367) (xy 141.477047 90.613936) (xy 141.497808 90.684715)
				(xy 141.505 90.777946)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.678914 107.497835) (xy 147.774282 107.600253) (xy 147.842824 107.689855) (xy 147.883991 107.760034)
				(xy 147.912468 107.827582) (xy 147.945042 107.974062) (xy 147.956772 108.07502) (xy 147.973029 108.213529)
				(xy 148.001529 108.384554) (xy 148.590707 108.268207) (xy 148.707054 107.679029) (xy 148.432601 107.638049)
				(xy 148.39752 107.634272) (xy 148.248093 107.614933) (xy 148.116784 107.57726) (xy 147.981547 107.498628)
				(xy 147.820335 107.356414)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.5115 100.23) (xy 156.435958 100.224593) (xy 156.345396 100.206747) (xy 156.26781 100.180293)
				(xy 156.197848 100.141843) (xy 156.157711 100.106825) (xy 156.128382 100.064646) (xy 156.118903 100.041418)
				(xy 155.4485 100.33) (xy 156.118903 100.618582) (xy 156.159712 100.551016) (xy 156.237548 100.494032)
				(xy 156.357523 100.450144) (xy 156.5115 100.43)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.79 103.2129) (xy 135.7843 103.293817) (xy 135.764398 103.390771) (xy 135.738315 103.461005)
				(xy 135.700654 103.521939) (xy 135.666999 103.55463) (xy 135.626474 103.576749) (xy 135.621234 103.578539)
				(xy 135.89 104.4839) (xy 136.158766 103.578539) (xy 136.094862 103.538973) (xy 136.042698 103.46313)
				(xy 136.004478 103.345705) (xy 135.99 103.2129)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.77 94.014804) (xy 160.764199 94.235863) (xy 160.727682 94.446762) (xy 160.724804 94.461227)
				(xy 160.97 94.511) (xy 161.215196 94.461227) (xy 161.21232 94.446776) (xy 161.175801 94.235867)
				(xy 161.17 94.014804)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.360335 90.763586) (xy 150.462753 90.668217) (xy 150.552355 90.599676) (xy 150.622534 90.558508)
				(xy 150.690082 90.530031) (xy 150.836561 90.497457) (xy 150.937521 90.485727) (xy 151.07603 90.469471)
				(xy 151.247054 90.440971) (xy 151.130707 89.851793) (xy 150.541529 89.735446) (xy 150.500549 90.009898)
				(xy 150.496772 90.04498) (xy 150.477433 90.194406) (xy 150.43976 90.325715) (xy 150.361128 90.460953)
				(xy 150.218914 90.622165)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.440335 90.763586) (xy 155.542753 90.668217) (xy 155.632355 90.599676) (xy 155.702534 90.558508)
				(xy 155.770082 90.530031) (xy 155.916561 90.497457) (xy 156.017521 90.485727) (xy 156.15603 90.469471)
				(xy 156.327054 90.440971) (xy 156.210707 89.851793) (xy 155.621529 89.735446) (xy 155.580549 90.009898)
				(xy 155.576772 90.04498) (xy 155.557433 90.194406) (xy 155.51976 90.325715) (xy 155.441128 90.460953)
				(xy 155.298914 90.622165)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.17 95.005196) (xy 161.175801 94.784133) (xy 161.21232 94.573224) (xy 161.215196 94.558773)
				(xy 160.97 94.509) (xy 160.724804 94.558773) (xy 160.727682 94.573238) (xy 160.764199 94.784136)
				(xy 160.77 95.005196)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/~{CS_A}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.059665 107.356414) (xy 161.957247 107.451782) (xy 161.867644 107.520324) (xy 161.797466 107.561491)
				(xy 161.729917 107.589968) (xy 161.583437 107.622542) (xy 161.48248 107.634272) (xy 161.343971 107.650529)
				(xy 161.172946 107.679029) (xy 161.289293 108.268207) (xy 161.878471 108.384554) (xy 161.91945 108.110101)
				(xy 161.923227 108.075021) (xy 161.942566 107.925594) (xy 161.980239 107.794285) (xy 162.058871 107.659047)
				(xy 162.201086 107.497835)
			)
		)
	)
	(zone
		(net 3)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.4)
			(smoothing fillet)
			(radius 0.2)
		)
		(polygon
			(pts
				(xy 165.1 88.9) (xy 165.1 109.22) (xy 129.54 109.22) (xy 129.54 88.9)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A12")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.080304 99.16) (xy 159.159836 99.164668) (xy 159.220431 99.177342) (xy 159.322687 99.225561)
				(xy 159.404315 99.268285) (xy 159.526727 99.305196) (xy 159.5765 99.06) (xy 159.526727 98.814804)
				(xy 159.390085 98.858094) (xy 159.322686 98.894439) (xy 159.22779 98.940353) (xy 159.164628 98.954681)
				(xy 159.080304 98.96)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/A12")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.169446 102.512633) (xy 136.109908 102.565569) (xy 136.058098 102.599454) (xy 135.951697 102.637664)
				(xy 135.863765 102.665174) (xy 135.751107 102.725633) (xy 135.889293 102.934207) (xy 136.097867 103.072393)
				(xy 136.163876 102.945162) (xy 136.185835 102.871804) (xy 136.22047 102.772236) (xy 136.255002 102.717441)
				(xy 136.310867 102.654054)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/~{WE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.186818 91.780944) (xy 136.126451 91.830166) (xy 136.073842 91.861442) (xy 135.976145 91.892785)
				(xy 135.962856 91.895592) (xy 135.869828 91.92037) (xy 135.751107 91.982133) (xy 135.889265 92.190677)
				(xy 136.097867 92.328893) (xy 136.16649 92.198673) (xy 136.186467 92.140171) (xy 136.22612 92.042283)
				(xy 136.263257 91.989319) (xy 136.322252 91.92811)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.474804 94.71) (xy 160.695867 94.715801) (xy 160.906776 94.75232) (xy 160.921227 94.755196)
				(xy 160.971 94.51) (xy 160.921227 94.264804) (xy 160.906762 94.267682) (xy 160.695863 94.304199)
				(xy 160.474804 94.31)
			)
		)
	)
	(zone
		(net 6)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.791797 90.551454) (xy 131.709059 90.461937) (xy 131.646049 90.379759) (xy 131.566588 90.232877)
				(xy 131.521675 90.079483) (xy 131.509523 90.020142) (xy 131.486855 89.9144) (xy 131.45281 89.798952)
				(xy 131.396962 89.668853) (xy 131.308882 89.519158) (xy 130.809293 89.851793) (xy 130.476658 90.351382)
				(xy 130.580345 90.415018) (xy 130.674325 90.462349) (xy 130.851414 90.524223) (xy 130.977642 90.552023)
				(xy 131.099205 90.579027) (xy 131.222507 90.622905) (xy 131.356204 90.701911) (xy 131.508954 90.834297)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/~{WE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.622831 90.731218) (xy 137.724371 90.64447) (xy 137.81356 90.582088) (xy 137.885544 90.54367)
				(xy 137.953928 90.51789) (xy 138.099387 90.49128) (xy 138.193875 90.484104) (xy 138.349844 90.471286)
				(xy 138.547054 90.440971) (xy 138.430735 89.851823) (xy 137.931118 89.519158) (xy 137.873816 89.61343)
				(xy 137.831288 89.70067) (xy 137.778203 89.867236) (xy 137.752736 90.043396) (xy 137.736008 90.171341)
				(xy 137.699743 90.299268) (xy 137.66794 90.365489) (xy 137.62364 90.434423) (xy 137.564305 90.506976)
				(xy 137.487398 90.584052)
			)
		)
	)
	(embedded_fonts no)
)
